Using KVM Dongle (CBL-0218L included with your chassis) to update the BIOS:

	1. Copy the contents of the zip file to a bootable USB pen drive
	2. Connect the KVM Dongle (CBL-0218L) to the front side of the blade in the KVM dongle connector
	3. Connect your bootable USB pen drive to one of the two USB slots on KVM dongle
	4. Boot to USB pen drive and go to appropriate directory to where you saved the contents of zip file
	5. Type, flash filename.rom (replace filename.rom by actual rom file name)

Using the USB ports on the CMM

	1. Copy the contents of the zip file to a bootable USB pen drive
	2. Connect your bootable USB pen drive to one of the two USB slots on CMM. CMM is found on the back side of blade.
	3. Boot to USB pen drive and go to appropriate directory to where you have saved the contents of the zip file
	4. Type, flash filename.rom (replace filename.rom by actual rom file name)

Using floppy image file (This has to be done remotely)
	
	1. Copy the image file from the zip file on your desktop.
	2. Use web browser or IPMIView to access your CMM remotely using IP Address
	3. Go to Virtual Media menu and select Floppy Image Upload
        4. Browse or Open to locate the .img file which is on your desktop. Select the .img file.
	5. Press the Upload button and wait for a few seconds for the image to upload to CMM.
	6. Once the upload finishes turn on your blade and press "del" to enter into the BIOS.
        7. Now bring the " USB LS120: PEPPCMM VIRTUAL DISC 1" to the top of the boot priority.
        8. Please exit saving chages. Now you will boot to the virtual media (floppy image) A:\> 
        9. Type, flash filename.rom (replace filename.rom by actual rom file name, Eg: B7DBE142.rom)

================================================
FOR <filename>.exe
================================================
	1. Run the <filename>.exe file under Windows to create the BIOS flash floppy disk.
	2. Insert the floppy into the system for which you wish to flash the BIOS.
	3. Boot up the system for which you wish to flash the BIOS.
	4. The BIOS utility will run automatically and begin flashing the BIOS WITHOUT any prompts.

	** Warning: Flashing the wrong BIOS file on your 
	motherboard can cause harm to your system. **

================================================
FOR <filename>.zip
================================================
	1. Boot to a DOS prompt and type flash.bat filename.rom
	

** If the BIOS flash failed, you can contact our RMA dept. to order a new bios chip.  
The RMA dept's email address is rma@supermicro.com
