IPMI Firmware Release Note
----------------------------

Filename: SMT_206.bin ver2.06 Date: 09-02-2010

Bug fixes:
1. X8SIT: Fix event log cannot catch CPU thermal trip event log (issueID=24349)
and modify sensor system temperature to read from RT1: Bank 2, Reg.50
2. H8DGU-LN4+: Fix sensor CPU temperature does not show medium/high (IssueID=24950)


======================================================================================
Filename: SMT_205.bin ver2.05 Date: 08-27-2010

Bug fixes:
1. X7SPA: Modify sensor name "Vnbcore" to "Vichcore"
2. H8DG6-F: Fix CPU temperature reports 'Low' eventhough 
CPU is overheating (issueID=24719) 
3. Fix SSH login with user/password: ADMIN/C0rbisSMAdmin 


======================================================================================
Filename: SMT_204.bin ver2.04 Date: 08-13-2010

Bug fixes:
1. X8SIL/X8SIE/X8SIA/X8SIU: Modify system temperature to read 
from RT1: Bank 2, Reg.50 (issueID=24254) 
2. Add Daylight Saving Time in web gui: Configuration->Date & Time
3. H8DGG-QF: Support Fermi GPU M2050 which can slowdown and 
shutdown GPU when overheat 


======================================================================================
Filename: SMT_203_0805.bin  ver2.03  Date: 08-05-2010

Bug fixes:
1. X8DTU-6F+: Add 100ms delay for sensor polling to fix issue
wrong sensor readings on SD3 client after overnight stress test (issueID=23803)


======================================================================================
Filename: SMT_203_0803.bin  ver2.03  Date: 08-03-2010

Bug fixes:
1. H8DG6: Remove GPU from sensor readings (issueID=24521)
2. X7SPE-HF-D525: Modify +12V sensor calculation 


=====================================================================================
Filename: SMT_202_0727.bin  ver2.02  Date: 07-27-2010

Bug fixes:
1. H8DGU-LN4F: set GPIO34 to high to fix BIOS hangs with 
post code '3E' or 'E1' (IssueID=24461)
2. Add SMTP sender's email (Web gui: Configuration -> SMTP)


=====================================================================================
Filename: SMT_201_0721.bin  ver2.01  Date: 07-21-2010

Bug fixes:
1. Fix Lan1 issue for all motherboards with Hartwell (82574) LAN chip
Description: Cannot connect to BMC use onboard LAN1 after upgrade to new FW.
Validation: With default setting "failover" or default for non-dedicate LAN MB, 
BMC connect with LAN1, SUT in OS (WS2008R2, RH5.4, or RH5.5).  Please upgrade FW 
from previous release version to this new version using web GUI and check whether 
BMC can connect again after FW flashing.


=====================================================================================
Filename: SMT_200_0720.bin  ver2.00  Date: 07-20-2010

Bug fixes:
1. X8DTU-LN4F+: Add +1.1V sensor (issueID=24334)
2. X8DTU-F: Add sensor CPU1 DIMM and CPU2 DIMM (issueID=24269)
3. X7SPA/X7SPE: Rename sensor name "1.05V" to "Vnbcore" to sync with BIOS
(issueID=23092)

