Supermicro Update Manager (for UEFI BIOS) 1.0.0 (2020/04/01) (UEFI)

Introduction
  The Supermicro Update Manager (SUM) UEFI can be used to manage the system BIOS
  and BMC firmware image update for X12/H12 and later platforms except H12 non-RoT
  systems under EFI shell.

The package includes:
  - SUM.efi
  - README.txt
  - ReleaseNote.txt

==============================================================================================================================
==============================================================================================================================

SYNOPSIS
  SUM.efi [OPTIONs] [COMMAND] [COMMAND ARGUMENTS]

Help Message
  SUM.efi (Shows help information)
  SUM.efi -h/H (Shows help information)
  SUM.efi -h/H -c <Command name> (Shows help information for each command)

OPTIONs
  -I        Redfish_HI
  -u        <BMC user ID>
  -p        <BMC user password>
  -c        <Command name>

COMMANDS
  UpdateBios, GetBiosInfo, UpdateBmc, GetBmcInfo
            
COMMAND ARGUMENTS
  Required and optional arguments of each commands. 
  For detail information of each command, please refer to section below.

------------------------------------------------------------------------------------------------------------------------------
UpdateBios command:

Description
  Updates BIOS.

Example
  FS0:\> SUM.efi -I Redfish_HI -u ADMIN -p ADMIN -c UpdateBios --file BIOS.rom --reboot [Optional Arguments]

Required Arguments
  --file        BIOS image file
  --reboot      Forces the managed system to reboot or power up after operation

Optional Arguments
  --flash_smbios        Overwrites the SMBIOS data
  --preserve_nv         Preserves the NVRAM region
  --preserve_mer        Preserves the ME firmware region

Note: flash_smbios and preserve_nv optional arguments cannot be used at the same time.

==============================================================================================================================

UpdateBmc command:

Description
  Updates BMC.

Example
  SUM.efi -I Redfish_HI -u ADMIN -p ADMIN -c UpdateBmc --file BMC.rom [Optional Arguments]

Required Arguments
  --file    BMC image file

Optional Arguments
  --overwrite_cfg        Overwrites the current BMC configuration using the factory default values in the given BMC image file
  --overwrite_sdr        Overwrites current BMC SDR data

==============================================================================================================================

GetBiosInfo command:

Description
  Gets system BIOS information of the managed system.

Example
  SUM.efi -I Redfish_HI -u ADMIN -p ADMIN -c GetBiosInfo

Required Arguments
  N/A

Optional Arguments
  N/A

==============================================================================================================================

GetBmcInfo command:

Description
  Gets system BMC information of the managed system.

Example
  SUM.efi -I Redfish_HI -u ADMIN -p ADMIN -c GetBmcInfo 

Required Arguments
  N/A

Optional Arguments
  N/A