
--------------------------------------------------------------------------------------------
 CPU Microcode                  | Option ROM/EFI driver                   | Intel RC/TXT/ME
--------------------------------------------------------------------------------------------
 CPUID FAMILY                   | Aspeed VBIOS Legacy       : 1.10.01     |RC Package :1524.D00
 50654 Skylake U0 : 2006906     | Intel SATA RAID Legacy    : 6.3.0.1005  |BIOS ACM : 20190712 (1.3.81)
 50655 Skylake U0 : 3000010     | Intel SATA RAID UEFI      : 6.3.0.1005  |SINIT ACM : 20170613 (1.3.1)
 50656 Skylake U0 : 4002F01     | Intel Giga                : 1.4.04      |
 50657 CascadeLake L1 : 5002F01 | Intel Giga                : 0.1.12      |
                                | Intel Giga UEFI driver    : 6.7.05      |ME : 11.12.79.1722
--------------------------------------------------------------------------------------------
 BIOS feature                   | Support
--------------------------------------------------------------------------------------------
OOB Flash BIOS                  | N
OOB Update Setting              | Y
OOB Change SMBIOS               | Y
InBand Flash BIOS               | Y
InBand Update Setting           | Y
InBand Change SMBIOS            | Y
InBand SMI E7h supported        | N
InBand SMI D9h supported        | Y
Hii to BMC supported            | Y
--------------------------------------------------------------------------------------------
 SW ECO Caused By               | Status
--------------------------------------------------------------------------------------------
BIOS/IPMI Customization         | N
HW Vendor Updates               | Y
BIOS/IPMI Workaround            | Y
BIOS/IPMI Vendor Updates        | Y
BIOS/IPMI Enhancements          | Y
BIOS/IPMI Bug fixes             | Y
--------------------------------------------------------------------------------------------
BIOS : X11SRA0.903   Release Date :  09/03/2020
BIOS revision: 2.2   BIOS Engineer : ChenXuan Huang
BIOS Checksum: 99a6fc90h SVN Revision : 554
BIOS Change:

1. [Fixes] Fixed when use AMIBCP to setting the LAN1 PXE as disable the setting can't work problem.
   Description: It's the duplicate item for LAN1 PXE setting
   Validation: a. Use AMIBCP to change the LAN1 PXE setting as disable.
	       b. Flash the BIOS into the MB.
	       c. Boot up system, and check the LAN1 PXE setting is enable or disable.

2. [Enhancements] Update ME corporate 11.12.79.1722 for INTEL-SA-00404 Security Advisory to address CVE-2020-8758(9.8, Critical) security issues.
   Description : Update ME corporate 11.12.79.1722 for INTEL-SA-00404 Security Advisory to address CVE-2020-8758(9.8, Critical) security issues.
   Validation  : a) Confirm that "ME firmware Version" is 11.12.79.1722 under BIOS setup menu.
                 b) Confirm that "ME firmware Mode" is "Normal Mode" under BIOS setup menu.
                 c) Confirm ME related functions.

3. [Fixes] Fixed the SUM cannot dump the setup items of Advanced/Chipset Configuration/North Bridge/IIO Configuration page.
   Description: Fixed the SUM cannot dump the setup items of Advanced/Chipset Configuration/North Bridge/IIO Configuration page.
   Validation: Execute SUM OOB command: "./sum -i <IP or host name> -u <username> -p <username> -c GetCurrentBiosCfg --file <FileName.xml>" 
               to confirm SUM can dump the setup items of Advanced/Chipset Configuration/North Bridge/IIO Configuration page.

4. [Enhancements] Enhancements the Above 4G policy, the Above 4G add auto item. User can select it as "Auto" "Enabled" and "Disabled".
   Description: Add "Auto" item in the Above 4G option. Default setting as "Auto".
   Validation: a) Boot up system and setting the Above 4G as "Auto".
               b) Plug in 3 VGA add on card in the system, and check the memory resource already running as above 4G or not.
	       c) Remove add on VGA, and setting the Above 4G as "Disabled".
	       d) Boot up system and check the memory resource is below 4G or not.
	       e) Plug in 1 VGA add on card in the system, and check the memory resouce running as below 4G or not.

5. [Fixes] Fix some items disappear in BIOS setup menu.
   Description: Fix some items disappear in BIOS setup menu.
   Validation:  1. Boot into BIOS setup menu. 
                2. Check the items of setup menu should match the BIOS Template.

6. [Enhancements] Change BIOS version to 2.2.
    Description: Change BIOS version to 2.2.
    Validation: Check the BIOS version is 2.2 or not. 		

7. [Enhancements] Update SecureBoot module to label 32 for AMI SA-50085 Grub Bootloader vulnerability to address CVE-2020-10713 (8.2, high)   security issue.
   Description: Update SecureBoot module to label 32 for AMI SA-50085 Grub Bootloader vulnerability to address CVE-2020-10713 (8.2, high)   security issue.
   Validation: Check Secure Boot feature can work or not.
   
--------------------------------------------------------------------------------------------
 CPU Microcode                  | Option ROM/EFI driver                   | Intel RC/TXT/ME
--------------------------------------------------------------------------------------------
 CPUID FAMILY                   | Aspeed VBIOS Legacy       : 1.10.01     |RC Package :1524.D00
 50654 Skylake U0 : 2006906     | Intel SATA RAID Legacy    : 6.3.0.1005  |BIOS ACM : 20190712 (1.3.81)
 50655 Skylake U0 : 3000010     | Intel SATA RAID UEFI      : 6.3.0.1005  |SINIT ACM : 20170613 (1.3.1)
 50656 Skylake U0 : 4002F01     | Intel Giga                : 1.4.04      |
 50657 CascadeLake L1 : 5002F01 | Intel Giga                : 0.1.12      |
                                | Intel Giga UEFI driver    : 6.7.05      |ME : 11.12.77.1664
--------------------------------------------------------------------------------------------
 BIOS feature                   | Support
--------------------------------------------------------------------------------------------
OOB Flash BIOS                  | N
OOB Update Setting              | Y
OOB Change SMBIOS               | Y
InBand Flash BIOS               | Y
InBand Update Setting           | Y
InBand Change SMBIOS            | Y
InBand SMI E7h supported        | N
InBand SMI D9h supported        | Y
Hii to BMC supported            | Y
--------------------------------------------------------------------------------------------
 SW ECO Caused By               | Status
--------------------------------------------------------------------------------------------
BIOS/IPMI Customization         | N
HW Vendor Updates               | Y
BIOS/IPMI Workaround            | Y
BIOS/IPMI Vendor Updates        | Y
BIOS/IPMI Enhancements          | Y
BIOS/IPMI Bug fixes             | Y
--------------------------------------------------------------------------------------------
BIOS : X11SRA0.622   Release Date :  06/22/2020
BIOS revision: 2.1   BIOS Engineer : Mike Tsai
BIOS Checksum: ed772ad0h SVN Revision : 506
BIOS Change:

1. [Enhancements] Update the BIOS version as 2.1.
   Description: Update the BIOS version as 2.1.
   Validation: Check BIOS version is 2.1 or not.

2. [Enhancements] Enhance support GlacierFlass WS Turbo Boost 3.0 feature.
   Description: Enhance support GlacierFlass WS Turbo Boost 3.0 feature. Only W-2245/W-2255/W-2265/W-2276/W-2296 support Intel Turbo Boost 3.0 feature.
   Validation: a. Boot up with the list CPU.
               b. Boot into Windows and check the device manager has "Intel(R) Turbo Boost Max Technology 3.0 Driver" device or not.

3. [Fixes] Fixed when plug in K80 system will no boot issue.
   Description: Since the K80 need big memory resource.
   Validation: a. plug in K80 in system.
               b. Boot up system, and check system can boot up or not.

4. [Fixes] Fixed manufacturing Date in Part number field 's tail (date :Year/Week) of SMBIOS Type 17.
   Description: Fixed the SMBIOS type 17 manufacturing date is empty problem.
   Validation: a. Boot up system into OS.
               b. Use RW tool to read the SMBIOS Type 17 manufacturing date has data or not.

5. [Fixes] Fixed when enabled EuP mode then clean CMOS then system will hang up.
   Description: Fixed when enabled EuP mode then clean CMOS then system will hang up.
   Validation: a. Boot up system to setup menu then enabled EuP mode.
               b. Boot up system into OS, then shutdown system.
	             c. Remove AC power then clean CMOS.
	             d. Power on system and check system can boot up or not.

6. [Fixes] Enhance the memory correctable threshold can't work problem.
   Description: Enhance the memory correctable threshold can't work problem.
   Validation: a. Use tool to setting the "Memory Corrected Error Threshold" as 10.
               b. Enable AER and MCE via http://10.135.15.110/enable_mce_aer/.
	             c. Boot into CentOS OS 7.0.
	             d. Use command to install einj driver. (modprobe einj param_extension=1")
	             e. Execute following command to ejection memory error.
	                e-1: echo 0x08 > /sys/kernel/debug/apei/einj/error_type
		              e-2: echo 0x3000 > /sys/kernel/debug/apei/einj/param1
		              e-3: echo $((-1 << 12)) > /sys/kernel/debug/apei/einj/param2
		              e-4: echo 1 > /sys/kernel/debug/apei/einj/error_inject
		              e-5: repact e-4 step 10 times to ejection 10 memory event log.
	            f. Check the SMBIOS and IPMI event log has 1 memory event log or not.

7. [Fixes] Fixed when test SUM TC: 210/304/408 will fail problem.
   Description: Fixed when test SUM TC: 210/304/408 will fail problem.
   Validation: a. Setup system with SUM.
               b. Test SUM TC: 210/304/408 can pass or not.

8. [Fixes] Fixed the BIOS Device value of LAN1 and LAN2 are both em1 under Linux.
   Description: Fixed the BIOS Device value of LAN1 and LAN2 are both em1 under Linux.
   Validation: a. Boot to RHEL 7.6 or Ubuntu.
               b. Run "sudo biosdevname -d".
               c. Check the value of "BIOS device" that should not be the same for each LAN device.

9. [Enhancements] Updated ME 11.12.77.1664. For INTEL-SA-00295 Security Advisory to address CVE-2020-0542(7.8, High), CVE-2020-0532(7.1, High), CVE-2020-0538(7.5, High), CVE-2020-0534(7.5, High), CVE-2020-0541(6.7, Medium), CVE-2020-0533(7.5, High), CVE-2020-0537(4.9, Medium), CVE-2020-0531(6.5, Medium), CVE-2020-0535(5.3, Medium), CVE-2020-0536(5.5, Medium), CVE-2020-0545(4.4, Medium), CVE-2020-0540(5.3, Medium), CVE-2020-0566(7.3, High), CVE-2020-0539(3.3, Low), CVE-2020-0586(7.3, High), CVE-2020-0594(9.8, Critical), CVE-2020-0595(9.8, Critical), CVE-2020-0596(7.5, High), CVE-2020-8674(4.3, Medium) and CVE-2020-0597(6.5, Medium). 
    Description : Updated ME corporate 11.12.77.1664.
    Validation  : a. Confirm ME version and ME status under BIOS setup menu. Version should be 11.12.77.1664, status should be Normal.
                  b. Make sure system could normally.

10. [Enhancements] Display "No memory DIMM detected, install memory DIMMs" strig, when there is not any dimm in slot.
   Description: When there is not any dimm in slot, screen should display "No memory DIMM detected, install memory DIMMs" strig during post.
   Validation: 1.Don't plugin any dimm in slot.
               2.Boot up.
	             3.Make sure the string display on screen.

11. [Fixes] Fix when plug in 5 VGA in the system include plug in the VGA in the PCH the system will hang up in CP: 3Bh problem.
   Description: Fix when plug in 5 VGA in the system include plug in the VGA in the PCH the system will hang up in CP: 3Bh problem.
   Validation: a. Setup system with 5 VGA add on cards include plug in one VGA in the PCH slot.
               b. Check system can boot up success or not.

12. [Fixes] Remove the "System Firmware Error(POST ERROR)" error log to BMC and "EFI 01030006" in BIOS event log.
   Description : GPU card may not have Option ROM, so will issue this error to BMC and BIOS event log. This is an unnecessary error log. So remove it.
   Validation  : 1. Plug in GPU card which does not has Option ROM( ex: NVIDIA : Quadro GPU-NVQP6000).
                 2. Please check event log from IPMI web page and event log in BIOS setup.
                 3. There is no "System Firmware Error(POST ERROR)" or "EFI 01030006" log event.  

13. [Enhancements] Update Skylake microcode MB750656_04002F01 MB750654_02006906. For INTEL-SA-00329 Security Advisory to address CVE-2020-0548(2.8, Low) and CVE-2020-0549(6.5, Medium) security issue.       
                  Update Cascadelake microcode MBF50657_05002F01. For INTEL-SA-00329 Security Advisory to address CVE-2020-0548(2.8, Low) and CVE-2020-0549(6.5, Medium) security issue.    
   Description : Update Skylake microcode MB750656_04002F01 MB750654_02006906. For INTEL-SA-00329 Security Advisory to address CVE-2020-0548(2.8, Low) and CVE-2020-0549(6.5, Medium) security issue.       
                  Update Cascadelake microcode MBF50657_05002F01. For INTEL-SA-00329 Security Advisory to address CVE-2020-0548(2.8, Low) and CVE-2020-0549(6.5, Medium) security issue.   
   Validation  : 1. Check Microcode version in BIOS setup for Skylake CPU and Cascadelake CPU.
                 2. Check CPU related functions including C-State, performance.

14. [Fixes] Fixed an issue that caused the DMI Type2 incorrect when the PCD product name length was less then the FRU1 product name length.
   Description: DMI Type2 product will show incorrect problem.
   Validation: a. Program the system's Board Product Name (BPN) as "BPN_1588734447". (ex: ipmicfg -fru1 BPN BPN_1588734447)
               b. Reboot system and check the DMI Type 2 Product data is the same as "BPN_1588734447" or not.

15. [Enhancements] Add back the "NVMe Configuration" items.
   Description: Add back the "NVMe Configuration" items.
   Validation: a. Boot up system into BIOS setup menu.
               b. Check "NVMe Configuration" in the Advanced page or not.

16. [Enhancements] Update Intel RSTe RAID Option ROM/UEFI Driver to 6.3.0.1005 and VMD to 6.1.0.1034.
   Description: Update the RSTe RAID Option ROM/UEFI Driver to 6.3.0.1005.
   Validation: a) Enable RAID option ROM or UEFI Driver then check the version is 6.3.0.1005 or not.
               b) Check build RAID function can work or not.
	             c) Check the VMD version is 6.2.0.1034, and check VMD function can work or not.

17. [Enhancements] Update RC code to 1524.D00 for GlacierFallsWS IPU 2020.1.
   Description: Based on Intel IPU 2020.1 update the GlacierFallsWS RC to 1524.D00
   Validation: a. Check PCH On/Off stress.
               b. Check NMI function can work or not.
	       c. Check VMD function can work or not.
	       d. Install Windows 10 and check it has blue screen or not.
	       e. Install RHEL OS and check dmesage has error message or not. 

18. [Fixes] Modify GPP_A7 for the i219 boot in PXE will very slow problem.
   Description: When use i219 boot up PXE, system will very slow.
   Validation: a. Boot up system and set LAN2 PXE enable.
               b. Boot into PXE server, and check it will slow or not.

--------------------------------------------------------------------------------------------
 CPU Microcode                  | Option ROM/EFI driver                   | Intel RC/TXT/ME
--------------------------------------------------------------------------------------------
 CPUID FAMILY                   | Aspeed VBIOS Legacy       : 1.10.01     |RC Package :2.0.44.50
 50654 Skylake U0 : 2000065     | Intel SATA RAID Legacy    : 6.2.0.1034  |BIOS ACM : 20190712 (1.3.81)
 50655 Skylake U0 : 3000010     | Intel SATA RAID UEFI      : 6.2.0.1034  |SINIT ACM : 20170613 (1.3.1)
 50656 Skylake U0 : 400002C     | Intel Giga                : 1.4.04      |
 50657 CascadeLake L1 : 500002C | Intel Giga                : 0.1.12      |
                                | Intel Giga UEFI driver    : 6.7.05      |ME : 11.12.0.1622
--------------------------------------------------------------------------------------------
 BIOS feature                   | Support
--------------------------------------------------------------------------------------------
OOB Flash BIOS                  | N
OOB Update Setting              | Y
OOB Change SMBIOS               | Y
InBand Flash BIOS               | Y
InBand Update Setting           | Y
InBand Change SMBIOS            | Y
InBand SMI E7h supported        | N
InBand SMI D9h supported        | Y
Hii to BMC supported            | Y
--------------------------------------------------------------------------------------------
 SW ECO Caused By               | Status
--------------------------------------------------------------------------------------------
BIOS/IPMI Customization         | N
HW Vendor Updates               | Y
BIOS/IPMI Workaround            | Y
BIOS/IPMI Vendor Updates        | Y
BIOS/IPMI Enhancements          | Y
BIOS/IPMI Bug fixes             | Y
--------------------------------------------------------------------------------------------
BIOS : X11SRA0.210 Release Date :  02/10/2020
BIOS revision: 2.0a  BIOS Engineer : Mike Tsai
BIOS Checksum: 7444E269h SVN Revision : 427
BIOS Change:

1. [Enhancements] Change BIOS version to 2.0a.
   Description : Change BIOS version to 2.0a.
   Validation  : Confirm BIOS version under BIOS setup.

2. [Fixes] Fixed when use X11SRA MB the FAN speed can't be setting problem.
   Description: Customization FAN speed control can't be worked.
   Validation: a. Boot up system enter BIOS setup menu -> System Health -> Fan Control
               b. Setting "Fan Speed Control Mode" as Customize.
	       c. Setting Fan speed as customize.

3. [Enhancements] Add limit the priory first VGA use under 4G resource function.
   Description : Add limit the priory first VGA use under 4G resource function.
   Validation  : a. Use Geforce GTX 780Ti as first priority output.
                 b. Enable above 4G.
                 c. Confirm if memory resource of this GPU is under 4G.

4. [Fixes] Fixed when plug in memory 64GB x 8 then the BIOS setup menu will show 256GB in the BIOS setup menu.
   Description: Since the 64GB size will DMI Type 17 ExtendedSize.
   Validation:  1. Boot into BIOS setup menu with 64GB x 8.
                2. Check  the Memory size is 512GB or not.

5. [Enhancements] Add ACS control item in Advanced/Chipset Configuration/North Bridge/IIO Configuration/Intel VT for Directed I/O (VT-d) page.
   Description: Add ACS control item in Advanced/Chipset Configuration/North Bridge/IIO Configuration/Intel VT for Directed I/O (VT-d) page.
   Validation:  1. Boot into BIOS setup menu.
                2. Check ACS control item in Advanced/Chipset Configuration/North Bridge/IIO Configuration/Intel VT for Directed I/O (VT-d) page.

6. [Fixes] Fix recovery page title would be "Main" and recovery page would disappear when move to another page under recovery mode.
   Description: Fix recovery page title would be "Main" and recovery page would disappear when move to another page under recovery mode.
   Validation: a. Let system enter recovery mode.
               b. Confirm if recovery page is "Recovery".
               c. Move to another page, confirm if recovery page still exist.

7. [Enhancements] Update GlacierFalls RC code to 2.0.44.50.
   Description: Update GlacierFalls RC code to 2.0.44.50.
   Validation: a. Check PCH On/Off stress.
               b. Check NMI function can work or not.
	       c. Check VMD function can work or not.
	       d. Install Windows 10 and check it has blue screen or not.
	       e. Install RHEL OS and check dmesage has error message or not.

8. [Enhancements] Add "NVMe FW Source" function.
   Description : Add "NVMe FW Source" function.
   Validation  : 1. Power on the system with M.2/U.2/PCIe NVMe device(Vendor driver is included) and boot to BIOS Setup.
                 2. Set "NVMe FW Source" to "AMI Native FW" or "Vendor Defined".
                 3. Verify it will load "AMI NVMe driver" when set to "AMI Native FW". (Shell CMD: drivers)
                 4. Verify it will load "Vendor NVMe driver" when set to "Vendor Defined". (Shell CMD: drivers)

--------------------------------------------------------------------------------------------
 CPU Microcode                  | Option ROM/EFI driver                   | Intel RC/TXT/ME
--------------------------------------------------------------------------------------------
 CPUID FAMILY                   | Aspeed VBIOS Legacy       : 1.10.01     |RC Package :2.0.32.20
 50654 Skylake U0 : 2000065     | Intel SATA RAID Legacy    : 6.2.0.1034  |BIOS ACM : 20190712 (1.3.81)
 50655 Skylake U0 : 3000010     | Intel SATA RAID UEFI      : 6.2.0.1034  |SINIT ACM : 20170613 (1.3.1)
 50656 Skylake U0 : 400002C     | Intel Giga                : 1.4.04      |
 50657 CascadeLake L1 : 500002C | Intel Giga                : 0.1.12      |
                                | Intel Giga UEFI driver    : 6.7.05      |ME : 11.12.0.1622
--------------------------------------------------------------------------------------------
 BIOS feature                   | Support
--------------------------------------------------------------------------------------------
OOB Flash BIOS                  | N
OOB Update Setting              | Y
OOB Change SMBIOS               | Y
InBand Flash BIOS               | Y
InBand Update Setting           | Y
InBand Change SMBIOS            | Y
InBand SMI E7h supported        | N
InBand SMI D9h supported        | Y
Hii to BMC supported            | Y
--------------------------------------------------------------------------------------------
 SW ECO Caused By               | Status
--------------------------------------------------------------------------------------------
BIOS/IPMI Customization         | N
HW Vendor Updates               | Y
BIOS/IPMI Workaround            | Y
BIOS/IPMI Vendor Updates        | Y
BIOS/IPMI Enhancements          | Y
BIOS/IPMI Bug fixes             | Y
--------------------------------------------------------------------------------------------
BIOS : X11SRA9.C11 Release Date :  12/11/2019
BIOS revision: 2.0  BIOS Engineer : Mike Tsai
BIOS Checksum: 90CDB71Ah SVN Revision : 368
BIOS Change:

1. [Enhancements] Support GlacierFalls CLX-W CPU.
   Description : Support GlacierFalls CLX-W CPU.
   Validation  : a. Flash BIOS from OLD ECO BIOS to ECO BIOS 2.0.
                 b. Make sure the system can power on success.
                 c. Change CPU to CLX-W CPU, and check it can boot up or not.
                 d. Check the CPU is running at correct speed or not.
                 e. Check AVL list memories can be detect can boot up success.
                 f. Also check memory speed is correct or not.
                 g. Check system can boot into Windows 10 and Linux OS success.
                 h. Check after boot into Windows 10 the system has blue screen or not.
                 i. Stress OS on/off test over 500 times.
                 j. Check CPU information is correct or not, and CPU can running to top speed.
                 k. Check CPU running speed is correct or not.
                 l. Stress CPU and check it will hang up or not.

2. [Enhancements] Update PCIe module in the GlacierFalls platform.
   Description : Update PCIe module in the project.
   Validation  : a. Check system onboard device can be work or not.
                 b. Use BIOS setup menu to disable onboard LAN device can be work or not.
                 c. Check onboard LAN device speed is correct or not.
                 d. Check support add on cards can be detect success or not in the system.
                 e. Check when plug in add on cards and the SMBIOS information can show correct or not.
                 f. Running the C-Burn test pass over 500 times.

3. [Enhancements] Update the USB module in the GlacierFalls platform.
   Description : Update the USB module in the GlacierFalls platform.
   Validation  : a. Check all USB port can detect USB device under DOS or OS.
                 b. Check the USB port speed is correct or not.
                 c. Check plug in and plug out function can work or not.
                 
4. [Enhancements] Update the TPM module in the GlacierFalls platform.
   Description : Update the TPM module in the GlacierFalls platform.
   Validation  : a. Check the TPM module can detect success or not.
                 b. Check TPM module can show success or not in the OS.
                 c. Check Windows 10 Bitlocker function can work or not.

5. [Enhancements] Update the ESA setup menu module in the GlacierFalls platform.
   Description : Update the ESA setup menu module in the GlacierFalls platform.
   Validation  : a. Boot up system, and boot into BIOS setup menu.
                 b. Check after boot into BIOS setup menu the mouse point is move smooth or not.
                 c. Check SuperFlash update BIOS can work or not.

6. [Enhancements] Update the console redirection module in the GlacierFalls platform.
   Description : Update the console redirection module in the GlacierFalls platform.
   Validation  : Check the console redirection function can work or not.

7. [Enhancements] Update the serial port function in the GlacierFalls platform.
   Description : Update the serial port function in the GlacierFalls platform.
   Validation  : Check the serial port function can work.

8. [Enhancements] Update the power policy setting in the GlacierFalls platform.
   Description : Update the power policy setting in the GlacierFalls platform.
   Validation  : Check power policy function can work or not.
   
9. [Enhancements] Update the SATA module function in the GlacierFalls platform.
   Description : Update the SATA module function in the GlacierFalls platform.
   Validation  : a. Check all of the SATA port can detect the SATA device.
                 b. Check the SATA HDD speed is running correct or not.
                 c. Stress SATA HDD.

10. [Fixes] Fixed when set BIOS setup menu CSM as disabled then system can't boot problem.
   Description: When setting BIOS setup menu CSM as disabled the Onboard VGA should setting as "EFI" mode.
   Validation: Boot up system then setting CSM as disabled, then check system can boot up or not.

11. [Enhancements] Add SMC Password style in the GlacierFalls Projects.
   Description: Follow newest SMC Password style to add in GlacierFalls projects.
   Validation: a) Boot up system and boot into Security Page.
               b) Check the "Password Description" has follow SMC password style or not.
	       c) Check the Minimum Length is 8.
	       d) Check when without enter Administrator Password the User Password can enter or not.
	       e) Check the "Password Check" function can work or not.

12. [Enhancements] Add AER and MCE items.
   Description : Add AER and MCE items.
   Validation  : 1. Power on this system with networking. (Make sure it has BMC IP)
                 2. Boot to any environments.
                 3. Active BMC product key via http://10.135.15.110/activate/.
                 4. Enable AER and MCE via http://10.135.15.110/enable_mce_aer/.
                 5. Restart the system and boot to any environments.
                 6. Verify "MCEON" and "AERON" strings will be displayed during POST.
		 
13. [Enhancements] Updated ME 11.12.00.1622.
    Description : Updated ME 11.12.00.1622.
    Validation  : a. Confirm ME version and ME status under BIOS setup menu. Version should be 11.12.00.1622, status should be Normal.
                  b. Make sure system could normally.

14. [Fixes] Fix when use AMI SCE tool to dump to BIOS setup items the "Storage Option ROM/UEFI Driver" will be mask.
   Description: When use AMI SCE tool to dump to BIOS setup items the "Storage Option ROM/UEFI Driver" will be mask.
   Validation: a) Boot up system and enter UEFI shell.
               b) run "amisce.efi /o /s aaa.txt".
	             c) Check the "Storage Option ROM/UEFI Driver" can be find or mask.

17. [Enhancements] Add "SMBIOS Preservation" Enabled/Disabled item for flash recovery.
   Description : Add "SMBIOS Preservation" Enabled/Disabled item for flash recovery.
   Validation  : a. Boot into shell and change SMIBIOS data by AMI shell tool, use "AMIDEEFIx64.efi /bp Test11".
                 b. Reboot system and flash BIOS, AC off system when system erase main block.
                 c. AC on system, system should enter recovery page.
                 d. Select "SMBIOS Preservation" then start recovery procedure.
                 e. After recovery is done, reboot system and boot to shell. Confirm DMI Type 2 board product is "Test11".
                 f. Repeat step b~c.
                 g. Do not select "SMBIOS Preservation" then start recovery procedure.
                 h. After recovery is done, reboot system and boot to shell. Confirm DMI Type 2 board project return to default value.

18. [Fixes] Fix when use AFU tool to clean event log will return not support problem.
   Description: When use AFU tool to clean event log will return not support problem.
   Validation: a. Boot up system into UEFI shell.
               b. Run "afuefi.efi /clnevnlog" then check return status is ok or not.

19. [Fixes] Fix the VGA priority can't change by SMC Option ROM control function.
   Description: Fix the VGA priority can't change by SMC Option ROM control function.
   Validation: Check the SMC Option ROM control function can work or not.

20. [Fixes] Fix when change VGA priority to Add on card will show the message in the onboard VGA output.
   Description: When change the VGA priority to add on card need show the message in the onbard VGA output.
   Validation: a. Plug in a VGA card in the PCIe slot.
               b. Boot up system then setup the VGA priority to PCie slot.
	       c. Save and exit, then check the onboard VGA output has message or not.

21. [Fixes] Add item "Storage Option ROM/UEFI Driver" of Advanced/SATA and RST Configuration page.
   Description: Add item "Storage Option ROM/UEFI Driver" of Advanced/SATA and RST Configuration page.
   Validation: Confirm if the item "Storage Option ROM/UEFI Driver" exist in Advanced/SATA and RST Configuration page.

22. [Fixes] Fix cannot load VMD driver when enable VMD ports under "Intel VMD Technology" menu.
   Description: The VMD function fail cause by the RSTeSataRaidEfi module has been removed.
   Validation: a. Plug in two NVMe devices on CPU PCIe slots.
               b. Boot up system and boot into BIOS setup menu.
               c. Setting the VMD enable and check each string of VMD port that should match HW silkscreen on Advanced-> Chipset Configuration-> North Bridge-> IIO Configuration-> Intel VMD technology page.
               d. Check the VMD driver can build NVMe device or not.

23. [Enhancements] Update VROC VMD driver, RSTe UEFI driver and Legacy ROM to 6.2.0.1034.
   Description: Update VROC VMD driver, RSTe UEFI driver and Legacy ROM to 6.2.0.1034.
   Validation: a. Enable RAID option ROM or UEFI Driver then check the version is 6.2.0.1034 or not.
               b. Check build RAID function can work or not.

24. [Enhancements] Implement prompt message at post screen when enter BIOS recovery mode for the platform support early video. 
   Description: Implement prompt message at post screen when enter BIOS recovery mode for the platform support early video.
   Validation: a) Reboot system and flash BIOS, AC off system when system erase main block.
               b) AC on system, system should enter recovery page.
               Check recovery error message when no BIOS image:
               c) Removing USB drive and waiting system enter recovery.
               d) Confirm error message. 
               Check prompt message at post screen
               e) Insert a USB device that contains SUPER.ROM.
               f) AC on system, system should enter recovery page.
               g) Confirm BIOS recovery message.

25. [Enhancements] Update Skylake microcode MB750654_02000065. For INTEL-SA-00271 Security Advisory to address CVE-2019-11139(5.8, Medium) security issue.       
                  Update Cascadelake microcode MBF50656_0400002C and MBF50657_0500002C. For INTEL-SA-00270 Security Advisory to address CVE-2019-11135(6.5, Medium) security issue.      
   Description : Update Skylake microcode MB750654_02000065. For INTEL-SA-00271 Security Advisory to address CVE-2019-11139(5.8, Medium) security issue.       
                 Update Cascadelake microcode MBF50656_0400002C and MBF50657_0500002C. For INTEL-SA-00270 Security Advisory to address CVE-2019-11135(6.5, Medium) security issue.      
   Validation  : 1. Check Microcode version in BIOS setup for Skylake CPU and Cascadelake CPU.
                 2. Check CPU related functions including C-State, performance.

26. [Enhancements] Updated Basin Falls BIOS ACM and SINIT ACM to PW singed version 1_3_81_20190712_KBL_PW_signed and BASINFALLS_SINIT_v1_3_1_20170613_KBL_PW_signed, respectively.
   Description: Updated Basin Falls BIOS ACM and SINIT ACM to PW version.
   Validation: a) Plug TPM 1.2 or TPM 2.0 to SUT.
               b) Using official release BIOS.
               c) Provision TPM.
               d) Enabled "TXT support" under "Advanced -> Trusted Computing" then "Save & Exit". 
               e) Boot to EFI shell.
               f) Execute "getsec64.efi -l SENTER".
               g) Check if the system prompts "GETSEC[SENTER] complete. System is now in TXT Environment".
               h) Execute "getsec64.efi -l SEXIT".
               i) Check if the system prompts ""GETSEC[SEXIT] complete. System has exited TXT Environment".

27. [Enhancements] Change the maximum value of Memory Frequency to 2933 in Memory page.
   Description : Change the maximum value of Memory Frequency to 2933 in Memory page.
   Validation  : 1. Power on the system and boot to BIOS Setup.
                 2. Enter Memory page.
                 3. Check the option of Memory Frequency that the maximum value should be 2933.

28. [Enhancements] Modify the IIO string in the BIOS setup menu.
   Description: Modify the IIO string in the BIOS setup menu.
   Validation: Check the BIOS setup menu VMD/IIO PCIe slot define string, it must match the MB define.

29. [Fixes] Fix that press "Enter" then can enter Setup Menu if ADMIN password is set.
   Description: Fix that press "Enter" then can enter Setup Menu if ADMIN password is set.
   Validation  : 1. Setup ADMIN password.
                 2. Re-boot to Setup Menu and verify it cannot enter to it with pressing "Enter" or incorrect password.

30. [Enhancements] Since the GPP_C12, GPP_C13, GPP_C14, GPP_C15, GPP_D5, GPP_D6, GPP_D7, GPP_D9, GPP_D10, GPP_D11, GPP_D12, GPP_D20, GPP_D21, GPP_D22, GPP_D23, GPP_G2, GPP_G3 and GPP_G6 are un-usage GPIO setting those GPIO as GPO low.
   Since the PP_C12, GPP_C13, GPP_C14, GPP_C15, GPP_D5, GPP_D6, GPP_D7, GPP_D9, GPP_D10, GPP_D11, GPP_D12, GPP_D20, GPP_D21, GPP_D22, GPP_D23, GPP_G2, GPP_G3 and GPP_G6 are un-usage GPIO setting those GPIO as GPO low.
   Validation: Check PP_C12, GPP_C13, GPP_C14, GPP_C15, GPP_D5, GPP_D6, GPP_D7, GPP_D9, GPP_D10, GPP_D11, GPP_D12, GPP_D20, GPP_D21, GPP_D22, GPP_D23, GPP_G2, GPP_G3 and GPP_G6 status is GPO low.

31. [Enhancements] Set IO port to 2F8h and IRQ to 3 for AST2500 Serial Port 2.
   Description: Set IO port to 2F8h and IRQ to 3 for AST2500 Serial Port 2.
   Validation: Check the serial port function.

32. [Enhancements] Add use BIOS setup item to change the Project Name font size.
   Description: Use BIOS Setup menu hidden item to change the project name font size.
   Validation: a) Use AMI BCP to setting "Project Name Font Size" from 20 ~ 40.
               b) Update the BIOS then check the BIOS setup menu's project name as change the font size or not.

33. [Fixes] [ESA] Fixed in the workstation non-IPMI project the BCLK will show incorrect speed problem.
   Description: The BCLK speed reading incorrect.
   Validation: Boot into BIOS setup menu and check the BCLK speed is correct or not.

34. [Fixes] Default enabled the PROCHOT pin as BIDIRECTIONAL to support processor hot feature.
   Description: When processor hot the CPU didn't trigger the PROCHOT pin.
   Validation: Setup system and check the PROCHOT feature can work or not.
   
35. [Fixes] Fix user password doesn't clear after clearing administrator password.
   Description: When clear administrator password the user password will be cleared as well.
   Validation: 1. Enter BIOS security menu then create administrator and user password.
               2. Change password check to "Always".
               3. Save and reboot system.
               4. Enter BIOS then clear the administrator password.
               5. Save and reboot system.
               6. Password check should not pop out to ask password.
               7. Check user password is cleared as well.

36. [Fixes] Fixed the early console redirection can't work in the SOL problem.
   Description: When system post the early console redirection can't work in the SOL.
   Validation: 1. Boot up system and connect the SOL.
               2. Check the SOL has early console redirection or not.

37. [Fixes] Add fixed when system boot into Windows OS will blue screen problem.
   Description: Add fixed when system boot into Windows OS will blue screen problem.
   Validation: 1. Power on and boot into Windows.
               2. There should doesn't occur BSOD when windows log in.

38. [Enhancements] Add use BIOS setup menu to enable/disable the LAN1/LAN2 function.
   Description: Use BIOS setup menu to enabled/disable the LAN1/LAN2 function.
   Validation: a. Boot into BIOS setup menu and disable the LAN1/LAN2 function.
               b. Reboot system and check the LAN1/LAN2 can be disable or not. 

39. [Fixes] Fix IPMI web setting didn't sync with BIOS IPMI page.
   Description: When you set IPMI "Share" to "Dedicate" on IPMI web, BIOS IPMI page will not sync with the setting.
   Validation: 1.Set IPMI from "Share" to "Dedicate" on IPMI web.
               2.Enter BIOS IPMI page.
	       3.Make sure IPMI LAN Selection is "Dedicate LAN".

40. [Fixes] Fixed when update BIOS with the ME IPMI has PCH temperature reading fail event log problem.
   Description: Fixed when update BIOS with the ME IPMI has PCH temperature reading fail event log problem.
   Validation: a. Setup system and check the sensor reading.
               b. Use flash package or SUM inband tool to update BIOS.
	       c. After finish update BIOS check the IPMI event log has PCH temperature reading fail or not.