*****************************************************************************
* ATEN Technology, Inc.                                                     *
*****************************************************************************
* FUNCTION   :  IPMI FIRMWARE UPDATE UTILITY                                *
* VERSION    :  1.15                                                        *
* BUILD DATE :  Jan 07 2010                                                 *
* USAGE      :                                                              *
*             (1)Update FIRMWARE : dUpdate.exe -f filename.bin [OPTION]     *
*             (2)Dump FIRMWARE : dUpdate.exe -d filename                    *
*****************************************************************************
* OPTION                                                                    *
*   -r Preserve Configuration(default is Preserve)                          *
*      n:No Preserve, reset to factory default settings                     *
*      y:Preserve, keep all of the settings                                 *
*****************************************************************************


1.Place the FW binary file & FW update utility into the same folder.
2.Excute the command line, and execute this utility.

1.12 add list:
(1) add preserve configuration.

1.14 add list:
(1) Add error handling.

1.15 add list:
(1) add dump flash feature
