
Firmware Version: 01.02.23
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220329_01.02.23_STDsp.bin
Production signed Firmware CRC: ED9D2CD5
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220329_01.02.23_STDsp.bin
Production signed eMMC Firmware CRC: F27653BE
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20220329_01.02.23_STDsp.bin
Production signed SPI NOR Firmware CRC: AD6FD973
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220329_01.02.23_STDsd.bin
Debug signed Firmware CRC: 5F5F7AFD
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220329_01.02.23_STDsd.bin
Debug signed eMMC Firmware CRC: 8134549F
Build Date: 03/29/2022
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: fix
   Description:
     [139021] - Keep running process if syslog status has not changed
   Infected Motherboard: All
   Affected functions: Redfish, Web
   Validation:
     1) Press save button on syslog page, make sure it returns 200 ok

2. Category: fix
   Description:
     [ENGINEERING] - Redfish automation test failed.
   Infected Motherboard: ALL
   Affected functions: Redfish automation
   Validation:
     1) Redfish automation

3. Category: fix
   Description:
     [137453] - When four AOC-STG-b2T cards are installed in SYS-220GQ-TNAR+, cburn onoff failed random sensors missing.
   Infected Motherboard: ALL
   Affected functions: AOC NIC
   Validation:
     1) Plug in four AOC-STG-b2T.
     2) run cburn.
     3) Check if sensor missing.

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.22
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220323_01.02.22_STDsp.bin
Production signed Firmware CRC: FC488ABC
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220323_01.02.22_STDsp.bin
Production signed eMMC Firmware CRC: 9CD4ADCD
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20220323_01.02.22_STDsp.bin
Production signed SPI NOR Firmware CRC: AD6FD973
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220323_01.02.22_STDsd.bin
Debug signed Firmware CRC: E0D5FE58
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220323_01.02.22_STDsd.bin
Debug signed eMMC Firmware CRC: 41C98820
Build Date: 03/23/2022
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1.Category: fix
  Description:
    [138931] - Modify user name or password will return oops error while Account Type is "SNMP".
    [138990] - SNMPv2/SNMPv3 buttons should be set "OFF" by default.
  Validation:
    1) Login BMC GUI Web -> Configuration -> Account Services -> Users page
    2) Click on "Add", pop up "Add New User" window
    3) Add new account with Account type "Redfish" and "SNMP" success
    4) Modify same account, enter new User name or New Password/ Confirm Password
    5) Click on Save and check result
       expected: save successfully.

2. Category: fix
   Description:
     [137826] – [Security] Wrong base64 caused 500 Internal error at redfish
   Infected Motherboard: ALL
   Affected functions: Security
   Validation:
     1) Webpage didn’t show 500 error.

3. Category: fix
   Description:
     [138455] - Can not change directory service to "LADP" & "Active Directory" & "RADIUS
     [138959] - "LDAP" is unable to submit while all filed is preserve default value.
   Infected Motherboard: ALL
   Affected functions: Web/Redfish
   Validation:
     1) Select "LADP", "Active Directory" or "RADIUS".
     2) Refresh the web page.
     3) The setting will be changed.
     4) Run SATC Radius is pass

4. Category: fix
   Description:
     [134718] - Redfish automation test failed.
     [136971] - Redfish automation test fail.
     [138220] - Redfish automation test failed.
     [138258] - Redfish automation testing failed.
     [138362] - There are 10 fail items when running SATC test
   Infected Motherboard: ALL
   Affected functions: Redfish automation
   Validation:
     1) Redfish automation

5. Category: feature
   Description:
     [ENGINEERING] - Support AOC P3IMB-M-P1, P3IMB-M-P2 sensor reading
   Infected Motherboard: ALL
   Affected functions:
   Validation:
     1) check AOC_ASIC1 Temp via ipmitool

6. Category: fix
   Description:
     [ENGINEERING] - OTP key management is ready.
     [ENGINEERING] - Please provide which version enable SPL recovery function
   Infected Motherboard: ALL
   Affected functions: ROT20
   Validation:
     1) Do ROT20 provision
     2) verify SPL recovery function.

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.21
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220311_01.02.21_STDsp.bin
Production signed Firmware CRC: 696894B0
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220311_01.02.21_STDsp.bin
Production signed eMMC Firmware CRC: 800416CB
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20220311_01.02.21_STDsp.bin
Production signed SPI NOR Firmware CRC: 54EBADDF
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220311_01.02.21_STDsd.bin
Debug signed Firmware CRC: D51FE934
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220311_01.02.21_STDsd.bin
Debug signed eMMC Firmware CRC: FDF33A46
Build Date: 03/11/2022
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: fix
   Description:
     [138548] - Couldn't turn on NTP Enable
   Infected Motherboard: ALL
   Affected functions: NTP
   Validation:
     1) verify NTP enable and disable through WEBUI

2. Category: fix
   Description:
     [138422] fix- Language Change title string not translated.
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) check Language Change string via web

3. Category: fix
   Description:
     [137839] - Task list filter Completed Time the string will be shifted
     [136835] - Dynamic DNS feature has different filter rule between H12 and X12
     [136298] - The link speed in physical view is displaying "drives link speed and also link not active"
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Task -> filter by completed time -> string will not shift
     3) Physical view with nvme -> if single link will only show single link not two links
     4) dynamic dns -> hostname no longer allows "@" and "+"

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.20
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220308_01.02.20_STDsp.bin
Production signed Firmware CRC: A108DAAF
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220308_01.02.20_STDsp.bin
Production signed eMMC Firmware CRC: BDCB19BC
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20220308_01.02.20_STDsp.bin
Production signed SPI NOR Firmware CRC: 54EBADDF
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220308_01.02.20_STDsd.bin
Debug signed Firmware CRC: 833125D6
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220308_01.02.20_STDsd.bin
Debug signed eMMC Firmware CRC: 5E72B7CC
Build Date: 03/08/2022
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: Fix
   Description:
     [138059] - Remove current settings and set user defaults to ADMIN/ADMIN does not work
   Infected Motherboard: ALL
   Affected functions: reset default
   Validation:
     1) reset default works as expected.

2. Category: fix
   Description:
     [137747] - The user account can be changed Enabled Status when the account logging in
   Infected Motherboard: ALL
   Affected functions: Redfish/Web
   Validation:
     1)Login SUT with ADMIN and create a new account in ID 3
     2)Login SUT with new account (id3) and different browser
     3)Used ADMIN to delete ID 3 and check BMC return the error(confirm ID 3 is logging)
     4)Edit ID 3 account with ADMIN
     5)Switch ID 3 account Enabled status from "enable" to "disable". It should not be changed.

3. Category: fix
   Description:
     [136834] - Server will escape original double quotes in json format when receive an empty value.
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) PATCH the property with an empty string will show the expected result.

4. Category: fix
   Description:
     [137916] fix - [RoT] RoT event log display Out of SPEC Definition 0x00/0x01
   Infected Motherboard: All
   Affected functions: Event
   Validation:
     1) update BMC/BIOS and under flashing to do ac cycle to trigger auto recover

5. Category: fix
   Description:
     [137453] - When four AOC-STG-b2T cards are installed in SYS-220GQ-TNAR+, cburn onoff failed random sensors missing
   Infected Motherboard: All
   Affected functions: sensor reading
   Validation:
     1) Installed 4XAOC-STG-b2T
     2) Power on and post complete
     3) The sensor is ready.

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.19
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220224_01.02.19_STDsp.bin
Production signed Firmware CRC: C3764C21
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220224_01.02.19_STDsp.bin
Production signed eMMC Firmware CRC: 3D1B4A75
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20220224_01.02.19_STDsp.bin
Production signed SPI NOR Firmware CRC: 521CB30E
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220224_01.02.19_STDsd.bin
Debug signed Firmware CRC: 14DEE5C0
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220224_01.02.19_STDsd.bin
Debug signed eMMC Firmware CRC: 2B33B29D
Build Date: 02/24/2022
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: fix
     Description:
       [137743] - System Crash Dump can be generated/download with wrong license(No key or OOB)
       [137760] - "Save" button is not appropriate for clear event log confirmation boxes
       [137775] - Add SNMP type user Not have * to inform Auth Key and Private Key are required items
       [137778] - Add SNMP type User not had error message When use not allowed characters
       [137830] - Mount *.img display wrong file type on Virtual Media page
     Infected Motherboard: ALL
     Affected functions: Web
     Validation:
       1) Log into web
       2) vm page -> upload .img floppy disk -> displays "There is an img file mounted"
       3) users page -> auth/private key have * meaning required, auth/private key
                        check correct symbols, characters
       4) MEL page -> clear MEL popup modal, buttons are "Close" and "Yes"

2. Category: Enhancement
   Description:
     [134674] - Unable to generate "NTP update" on the task list, while NTP Enable/Disable.
     [137841] - Unable to generate "NTP update" on the task list, while NTP setting.
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
      1) Patch /redfish/v1/Managers/1/Oem/Supermicro/NTP
      2) The configuration is handled by Task service

3. Category: fix
   Description:
     [137784] - Filter account type "Redfish/IPMI" or "SNMP" will stuck.
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Login -> Configuration -> Account Services -> click filter
     2) the filter function work normally

4. Category: fix
   Description:
     [136114] - [IPMI ECO 01.02.13] Automation tests Failure.
     [136456] - [BIOS ECO 1.2] Automation tests Failure.
     [133392] - Redfish Installation Test fail caused by incorrect BIOS preservation option.
   Infected Motherboard: ALL
   Affected functions: automation test
   Validation:
     1) automation test

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.18
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220218_01.02.18_STDsp.bin
Production signed Firmware CRC: 66BD98FB
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220218_01.02.18_STDsp.bin
Production signed eMMC Firmware CRC: 986E22B3
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20220218_01.02.18_STDsp.bin
Production signed SPI NOR Firmware CRC: 521CB30E
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220218_01.02.18_STDsd.bin
Debug signed Firmware CRC: 753DC29E
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220218_01.02.18_STDsd.bin
Debug signed eMMC Firmware CRC: 4A6E29DF
Build Date: 02/18/2022
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: fix
   Description:
     [137550] - IPMI Web gui storage monitoring battery/nvme capacity status.
   Infected Motherboard: ALL
   Affected functions: Storage
   Validation:
     1) Plug AOC-3808
     2) Log in Web
     3) Check AOC-3808 battery status. It should be "gray".

2. Category: fix
   Description:
     [136826] - [Security] SSH service supports weak MAC algorithms.
   Infected Motherboard: ALL
   Affected functions: Security
   Validation:
     1) Run scanning tool on port 22.
     2) See if show "hmac-sha1-96" in the report.

3. Category: Fix
   Description:
     [136996] - The DNS server ip changed back to "0.0.0.0"
   Infected Motherboards: ALL
   Affected Function: Network
   Validation:
     1) Login BMC web, and run power reset
     2) After BIOS POST, go to [Network] page, to check DNS setting is normal or not.

4. Category: Fix
   Description:
    [ENGINEERING] - Added a prompt to ask user if they want to reboot system after BIOS runtime update.
    [137380] - Flashing BIOS by "Immediate Update" not works under Web GUI.
   Infected Motherboard: ALL
   Affected functions: BIOS Firmware Update
   Validation:
    1) Update BIOS Immediately on Web GUI
    2) After update, a prompt will show up asking if user wants to reboot the system.
    3) Rebooting the system will show the new BIOS version

5. Category: Fix
   Description:
     [136702] - The Severity is incorrect when VBAT Battery fail
   Infected Motherboard: ALL
   Affected functions: SEL
   Validation:
     1) raw 0x04 0x02 0x04 0x29 0xff 0x6f 0xf1 0xff 0xff to check severity

6. Category: fix
   Description:
     [136217] - Fix The description about memory install/remove location in health event log is incorrect
   Infected Motherboard: ALL
   Affected functions: SEL
     Validation:
       1) raw 0x4 0x2 0x4 0xDC 0xFF 0x6F 0x20 0x00 0x00 on UP platform should get [COMP-0010] DIMM removed on DIMMA1
       2) raw 0x4 0x2 0x4 0xDC 0xFF 0x6F 0x20 0x00 0x00 on DP platform should get [COMP-0010] DIMM removed on P1-DIMMA1

7. Category: Fix
   Description:
     [136963] - The NTP time incorrect
   Infected Motherboard: All
   Affected functions: NTP
   Validation:
      1) Enable NTP service and reboot the host. After host is ready, the system time should be adjusted according to NTP.

8. Category: fix
   Description:
     [137065] - [DVT]WEB UI update 3808 FW failed
   Infected Motherboard: ALL
   Affected functions: Storage
   Validation:
     1) Plug AOC-3808
     2) Log in Web
     3) Update AOC-3808 fw.

9. Category: fix
   Description:
     [136800] - Redfish automation test failed.
     [137260] - [IPMI ECO 01.02.16] 31 tests failed will occur when executing redfish automation tool
     [136114] - [IPMI ECO 01.02.13] Automation tests Failure.
     [127406] - Redfish Automation Tool check fail.
     [136456] - [BIOS ECO 1.2] Automation tests Failure.
     [134718] - Redfish automation test failed.
     [136254] - Redfish automation test failed.
   Infected Motherboard: ALL
   Affected functions: Redfish automation test
   Validation:
     1) Redfish automation test

10.Category: Fix
  Description:
    [135987] - User list couldn't cancel session id after closed ikvm/html5 session
  Infected Motherboards: ALL
  Affected Function: HTML5
  Validation:
    1) Launch 3 or 4 HTML5 sessions
    2) Close some sessions.
    3) Check User List.

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.17
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220209_01.02.17_STDsp.bin
Production signed Firmware CRC: B94EAF9C
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220209_01.02.17_STDsp.bin
Production signed eMMC Firmware CRC: 98E6F569
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20220209_01.02.17_STDsp.bin
Production signed SPI NOR Firmware CRC: 521CB30E
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220209_01.02.17_STDsd.bin
Debug signed Firmware CRC: 6B066BED
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220209_01.02.17_STDsd.bin
Debug signed eMMC Firmware CRC: 8B2E6011
Build Date: 02/09/2022
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: fix
   Description:
     [136720] : [ECO] assertion:temp critical when Physically hot swapping NVMe
   Infected Motherboard: ALL
   Affected functions: Storage NVMe SEL
   Validation:
     1) Log in Web
     2) Plug in/out NVMe drive
     3) Check SEL

2. Category: enhancement
   Description:
     [ENGINEERING] Support BRCM 38xx, 39xx I2C mode and auto-switching to PCIe mode.
   Infected Motherboard: ALL
   Affected functions: Storage
   Validation:
     1) Plug in AOC-39XX.
     2) Boot to UEFI shell
     3) Use BRCM tool to set I2C mode.
        $storcli /c0 set oob mode=i2c maxpayloadsize=1024 maxpacketsize=64
     4) reboot Host
     5) Boot to UEFI shell
     6) Use BRCM tool to verify if I2C mode.
        $storcli /c0 show oob
     7) Reboot Host
     8) Boot to UEFI shell
     9) Use BRCM tool to verify if PCIe mode.
        $storcli /c0 show oob
     Note: For AOC-38XX, please refer to PB#133660 steps.

3. Category: Fix
   Description:
     [136961] - Unexpected events log after the system reboots
   Infected Motherboard: ALL
   Affected functions: SEL from Windows
   Validation:
     1) install Windows OS and power reset. BMC will disgard these unexpected event log

4. Category: Fix
   Description:
     [135983] - BMC will stay at FW update mode when upload invalid BMC FW
     [135183] - Web hang in loading after uploaded invalid BMC file
   Infected Motherboard: ALL
   Affected functions: BMC FW upload
   Validation:
     1) try to upload invalid BMC FW.

5. Category: Fix
   Description:
     [136798] - NIC Temp is N/A
   Infected Motherboard: X12DGQ-R
   Affected functions: AOM-PTG-I2T temp sensor
   Validation:
     1) Install AOM-PTG-I2T and check NIC Temp sensor reading

6. Category: fix
   Description:
     [137051] - IPMI ECO automation test failed.(TS-411 ,TS-412, TS-413)
   Infected Motherboard: All
   Affected functions: Web
   Validation:
     1) Run IPMIECO test case 411 412 413 should pass.

7. Category: Fix
   Description:
     [136800] - [Firmware v01.02.15 ECO] Redfish automation test failed.
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) run SATC Systems\EthernetInterface


--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.16
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220129_01.02.16_STDsp.bin
Production signed Firmware CRC: 512A3C74
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220129_01.02.16_STDsp.bin
Production signed eMMC Firmware CRC: 82E5A0C4
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20220129_01.02.16_STDsp.bin
Production signed SPI NOR Firmware CRC: 886144BB
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220129_01.02.16_STDsd.bin
Debug signed Firmware CRC: 4DCBAC9C
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220129_01.02.16_STDsd.bin
Debug signed eMMC Firmware CRC: 5F846125
Build Date: 01/29/2022
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: Enhance
   Description:
     [ENGINEERING] - Change all voltage sensor name based on Supermicro_BMC_Sensor_Naming_Guildeline_2.0 (DRAFT V06).xlsx
   Infected Motherboard: X13/B13
   Affected functions: voltage sensor
   Validation:
     1) follow Supermicro_BMC_Sensor_Naming_Guildeline_2.0 (DRAFT V06).xlsx
     2) check voltage sensor name

2. Category: fix
   Description:
     [ENGINEERING] - Support RMCP over IPv6.
   Infected Motherboard: ALL
   Affected functions: ipmitool over IPv6.
   Validation :
     1) through WEBUI to get the last IPB6 adddress in IPV6 list 
     2) SMCIPMITool ${BMC_IPv6} ADMIN ADMIN ipmi raw 6 1
     3) SMCIPMITool ${BMC_IPv4} ADMIN ADMIN ipmi raw 6 1

3. Category: fix
   Description:
     [135659] - The format of Maintenance Event Log page about the "Clear All
                the Event Logs" button and "Interface" ?"User" and "Category" are not matched
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web -> MEL
     2) Interface web is "Web" not "WEB"

3. Category: fix
   Description:
     [136219] - Unable to see NVMe Max Link Speed and Max Link Width on Storage Monitor
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web - > storage monitoring -> physical view
     2) Plug in NVME
     3) Show max link speed and max link width under dropdown of each nvme for intel,
        western digital, and kioxia

4. Category: fix
   Description:
     [134099] - IPMI Console Capture Video sometime freeze in progress
   Infected Motherboard: ALL
   Affected functions: console capture video
   Validation:
     1) Verify console capture video

5. Category: fix
   Description:
     [136626] - Storage Monitoring displaying additional nvme drive slots
   Infected Motherboard: X12DPG-QR
   Affected functions: storage physical view
   Validation:
     1) the storage NVME physical view should show 4 slots at most.


--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.15
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220124_01.02.15_STDsp.bin
Production signed Firmware CRC: 585A22AC
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220124_01.02.15_STDsp.bin
Production signed eMMC Firmware CRC: EF5EA6E8
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20220124_01.02.15_STDsp.bin
Production signed SPI NOR Firmware CRC: 886144BB
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220124_01.02.15_STDsd.bin
Debug signed Firmware CRC: 2F406F7B
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220124_01.02.15_STDsd.bin
Debug signed eMMC Firmware CRC: 59C4BA36
Build Date: 01/24/2022
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: fix
   Description:
     [135519] :[DVT SYS-620TP-HC9TR] WEB UI Storage monitoring function delay over 1 minute when executing create RAID/delete RAID.
     [135455] :[DVT]WEB UI Storage monitoring function delay over 1 minute when executing create RAID/delete RAID.
     [135305] :[DVT]WEB GUI RAID50/10 create failed it can't select span for RAID create.
   Infected Motherboard: ALL
   Affected functions: Storage
   Validation:
     1) Plug in AOC-3908 and 6/4 HDDs
     2) Create RAID50/RAID10
     3) Check if it is successfull and how long it takes
     4) Clear all configuration
     5) Check if it is successfull and how long it takes

2. Category: fix
   Description:
     [135939] - Out of Spec Definition Assertion Deassertion events logs when hotpluging PWS
   Infected Motherboard: ALL
   Affected functions: SEL
   Validation:
     1) hotplug psu
     2) check psu health event show correctly

3. Category: Fix
   Description:
     [136072] - When launch java plug-in under Remote Console , it will return to Web UI log in page.
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Login Web and Launch Console

4. Category: Fix
   Description:
     [135985] -  SMCIPMITool is able to setting primary server to localhost
   Infected Motherboard: ALL
   Affected functions: CMD
   Validation:
     1) SMCIPMITool $IP ADMIN ADMIN ipmi oem x10cfg ntp primary localhost

5. Category: fix
   Description:
     [ENGINEERING] - incorrect NVME event description in 01.02.13 if Drive slot defined in system SPEC
   Infected Motherboard: ALL
   Affected functions: NVME event
   Validation:
     1) BMC will have events like "Slot@<slot> description" if system spec defined drive slot order

6. Category: fix
   Description:
     [136090] - QYFQ has incorrect CT and NR temperature on IPMI
     [ENGINEERING] - CPU Temp sensor threshold cannot be adjusted in 01.02.13
   Infected Motherboard: ALL
   Affected functions: CPU sensor threshold
   Validation:
     1) power on and post complete.
     2) ipmitool raw 0x30 0x96 to get CPU Tjmax
     3) ipmitool sensor to check CPU Temp high threshold UC and UNR

7. Category: fix
   Description:
     [135044] - Power supply information missing/misplaced/failed to update in IPMI WebGUI
     [ENGINEERING] - Add appropriate id to power supply on web
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Install multiple power supplies
     2) Log into web
     3) Inventory page -> shows all power supplies numbered

8. Category: fix
   Description:
     [ENGINEERING] - SAS logical SEL description incorrect
   Infected Motherboard: ALL
   Affected functions: Storage
   Validation:
     1) Plug in AOC-3908 and 2 HDD
     2) Create RAID1; then plug out/in one HDD.
     3) Check System/Health Event Log

9. Category: Fix
   Description:
     [135847] - SYS-120TP-DC9TR (MBD-X12DPT-PT6-P Rev:1.01) BMC FW_01.02.12 not show AOC_SSD1 Temp
     [135624] - [DVT[AOC SAS Storage sensor spec issue of HDD Temp and HDD Status
     [135621] - [DVT[AOC SAS Storage sensor spec issue of Drive Status
     [135216] - [DVT]Broadcom3908 System sensor check issue
   Infected Motherboard: ALL
   Affected functions: Sensor
   Validation:
     1) Get sensor reading via ipmitool

10.Category: Fix
   Description:
     [ENGINEERING] - make BMC compatible to support special cable to fix NVME order reversed.
   Infected Motherboard: X12DPG-QR
   Affected functions: NVME
   Validation:
     1) without special cable, the nvme slot order will be reversed.
     2) with special cable, the nvme slot order will be normal.

11.Category: Fix
   Description:
     [135747] - [QCL AOC-SLG3-2SM2 / AOC-SLG3-2NM2] Sensor readings not show AOC_SSD*_Temp
   Infected Motherboard: ALL
   Affected functions: Sensor
   Validation:
     1) Get sensor reading via ipmitool

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.14
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220114_01.02.14_STDsp.bin
Production signed Firmware CRC: 5C81BCF1
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220114_01.02.14_STDsp.bin
Production signed eMMC Firmware CRC: 13A901C8
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20220114_01.02.14_STDsp.bin
Production signed SPI NOR Firmware CRC: 886144BB
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220114_01.02.14_STDsd.bin
Debug signed Firmware CRC: 5371426F
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220114_01.02.14_STDsd.bin
Debug signed eMMC Firmware CRC: DDD9AE5F
Build Date: 01/14/2022
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: fix
   Description:
     [135519] :[DVT SYS-620TP-HC9TR] WEB UI Storage monitoring function delay over 1 minute when executing create RAID/delete RAID.
     [135455] :[DVT]WEB UI Storage monitoring function delay over 1 minute when executing create RAID/delete RAID.
     [135305] :[DVT]WEB GUI RAID50/10 create failed it can't select span for RAID create.
   Infected Motherboard: ALL
   Affected functions: Storage
   Validation:
     1) Plug in AOC-3908 and 6/4 HDDs
     2) Create RAID50/RAID10
     3) Check if it is successfull and how long it takes
     4) Clear all configuration
     5) Check if it is successfull and how long it takes

2. Category: fix
   Description:
     [135939] - Out of Spec Definition Assertion Deassertion events logs when hotpluging PWS
   Infected Motherboard: ALL
   Affected functions: SEL
   Validation:
     1) hotplug psu
     2) check psu health event show correctly

3. Category: Fix
   Description:
     [136072] - When launch java plug-in under Remote Console , it will return to Web UI log in page.
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Login Web and Launch Console

4. Category: Fix
   Description:
     [135985] -  SMCIPMITool is able to setting primary server to localhost
   Infected Motherboard: ALL
   Affected functions: CMD
   Validation:
     1) SMCIPMITool $IP ADMIN ADMIN ipmi oem x10cfg ntp primary localhost

5. Category: fix
   Description:
     [ENGINEERING] - incorrect NVME event description in 01.02.13 if Drive slot defined in system SPEC
   Infected Motherboard: ALL
   Affected functions: NVME event
   Validation:
     1) BMC will have events like "Slot@<slot> description" if system spec defined drive slot order

6. Category: fix
   Description:
     [136090] - QYFQ has incorrect CT and NR temperature on IPMI
     [ENGINEERING] - CPU Temp sensor threshold cannot be adjusted in 01.02.13
   Infected Motherboard: ALL
   Affected functions: CPU sensor threshold
   Validation:
     1) power on and post complete.
     2) ipmitool raw 0x30 0x96 to get CPU Tjmax
     3) ipmitool sensor to check CPU Temp high threshold UC and UNR

7. Category: fix
   Description:
     [135044] - Power supply information missing/misplaced/failed to update in IPMI WebGUI
     [ENGINEERING] - Add appropriate id to power supply on web
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Install multiple power supplies
     2) Log into web
     3) Inventory page -> shows all power supplies numbered

8. Category: fix
   Description:
     [ENGINEERING] - SAS logical SEL description incorrect
   Infected Motherboard: ALL
   Affected functions: Storage
   Validation:
     1) Plug in AOC-3908 and 2 HDD
     2) Create RAID1; then plug out/in one HDD.
     3) Check System/Health Event Log

9. Category: Fix
   Description:
     [135847] - SYS-120TP-DC9TR (MBD-X12DPT-PT6-P Rev:1.01) BMC FW_01.02.12 not show AOC_SSD1 Temp
     [135624] - [DVT[AOC SAS Storage sensor spec issue of HDD Temp and HDD Status
     [135621] - [DVT[AOC SAS Storage sensor spec issue of Drive Status
     [135216] - [DVT]Broadcom3908 System sensor check issue
   Infected Motherboard: ALL
   Affected functions: Sensor
   Validation:
     1) Get sensor reading via ipmitool

10.Category: Fix
   Description:
     [ENGINEERING] - make BMC compatible to support special cable to fix NVME order reversed.
   Infected Motherboard: X12DPG-QR
   Affected functions: NVME
   Validation:
     1) without special cable, the nvme slot order will be reversed.
     2) with special cable, the nvme slot order will be normal.

11.Category: Fix
   Description:
     [135747] - [QCL AOC-SLG3-2SM2 / AOC-SLG3-2NM2] Sensor readings not show AOC_SSD*_Temp
   Infected Motherboard: ALL
   Affected functions: Sensor
   Validation:
     1) Get sensor reading via ipmitool

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.13
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220107_01.02.13_STDsp.bin
Production signed Firmware CRC: C7E54640
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220107_01.02.13_STDsp.bin
Production signed eMMC Firmware CRC: 94EA9D10
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20220107_01.02.13_STDsp.bin
Production signed SPI NOR Firmware CRC: 886144BB
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20220107_01.02.13_STDsd.bin
Debug signed Firmware CRC: 47071AD2
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20220107_01.02.13_STDsd.bin
Debug signed eMMC Firmware CRC: D588908B
Build Date: 01/07/2022
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: fix
   Description:
     [135157] - Network number mismatch during run system on/off test (Failover mode)
   Infected Motherboard: ALL
   Affected functions: Host Interface
   Validation:
     1) Run system on/off test

2. Category: fix
   Description:
     [ENGINEERING] - Show storage controller VPD information on Web GUI.
   Infected Motherboard: ALL
   Affected functions: Storage
   Validation:
     1) Plug in AOC-38XX
     2) Log in Web.
     3) Check Storage/Controller View

3. Category: fix
   Description:
     [135649] - There is no BMC User Guide link is workable in help page
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Help page has note at top mentioning general guide message

4. Category: fix
   Description:
     [135636] - The IPv6 address is out of bounds
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web with ipv6 address
     2) hover logout button, ipv6 address does not go off screen

5.Category: Fix
  Description:
    [135655] - The format of CPU page is incorrect.
  Infected Motherboards: ALL
  Affected Function: Component Info
  Validation:
    1)Login BMC WEB
    2)Check CPU page, the CPU ‘Model’ field should not include frequency.

6. Category: Fix
   Description:
    [ENGINEERING] - Host will not reboot automatically after BIOS runtime update.
   Infected Motherboard: ALL
   Affected functions: Firmware Update
   Validation:
    1) On a system that supports BIOS Runtime Update, update BIOS immediately.
    2) Host should not reboot afterwards.

7. Category: fix
   Description:
     [135391] -  WEB UI GPU Slot sequence will change after refresh
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web -> GPU page
     2) Refresh page, gpu should still be in order

8. Category: Fix
   Description:
     [135188] - Web ADMIN Can delete new create user when new user login
   Infected Motherboard: ALL
   Affected functions: Web & redfish
   Validation:
     1) Web ADMIN should not to delete new create user when new user login

9. Category: feature
   Description:
     [ENGINEERING] - implement SEL based on spec 1.34
   Infected Motherboard: ALL
   Affected functions: SEL
   Validation:
     1) Add SEL raw cmd: 0x4 0x2 0x4 0xXX 0xXX 0xXX 0xXX 0xXX 0xXX
     2) Check SEL match spec

10.Category: feature
   Description:
     [ENGINEERING] - implement MEL based on spec 1.04
   Infected Motherboard: ALL
   Affected functions: MEL
   Validation:
     1) Go to Website
     2) Change value
     3) Check MEL match spec

11.Category: fix
   Description:
     [127685] - IP Address can't support IPv6 format on "IP Access control" page.
   Infected Motherboard: ALL
   Affected functions: Web, IPMI, Redfish
   Validation:
     1) Add/Delete IP Access Control

12.Category: fix
   Description:
     [131149] - SOL fail to start in SMASH Console
   Infected Motherboard: All
   Affected functions: SMASH SOL
   Validation:
     1) boot into EFI shell.
     2) Connect to SMASH console.
     3) Executed "cd system1/sol1" and "start".
     4) Press any keys, the keys shall be effected on BIOS UEFI command line.

13.Category: new
   Description:
     [ENGINEERING] - support AOM-PTG-I2T
   Infected Motherboard: X12DGQ-R, X12DPG-QR
   Affected functions: Phy LED
   Validation:
     1) install AOM-PTG-I2T
     2) post complete then check Phy LED behavior
     3) then power off and reboot BMC then check Phy LED behavior after BMC ready.

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.12
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211231_01.02.12_STDsp.bin
Production signed Firmware CRC: 6BD70C51
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211231_01.02.12_STDsp.bin
Production signed eMMC Firmware CRC: DF50527F
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20211231_01.02.12_STDsp.bin
Production signed SPI NOR Firmware CRC: 886144BB
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211231_01.02.12_STDsd.bin
Debug signed Firmware CRC: 90987809
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211231_01.02.12_STDsd.bin
Debug signed eMMC Firmware CRC: E59F772E
Build Date: 12/31/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: Fix
   Description:
     [134950] - AOC-S25G-B2S-O is not display in WebGUI
   Infected Motherboard: ALL
   Affected functions: Redfsih
   Validation:
     1) install two LAN AOC cards and check network AOC in WEBUI.

2. Category: enhancement
   Description:
    [ENGINEERING] - the BIOS authorization enhancement
   Infected Motherboard: RoT20 projects
   Affected functions: BIOS upload and boot authenticate
   Validation:
    1) Update the latest BIOS firmware and it should pass the validation
    2) AC cycle the machine and host should boot up

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.11
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211230_01.02.11_STDsp.bin
Production signed Firmware CRC: 361A388A
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211230_01.02.11_STDsp.bin
Production signed eMMC Firmware CRC: AD2923C7
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20211230_01.02.11_STDsp.bin
Production signed SPI NOR Firmware CRC: 45069889
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211230_01.02.11_STDsd.bin
Debug signed Firmware CRC: BC4AA445
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211230_01.02.11_STDsd.bin
Debug signed eMMC Firmware CRC: E6F9EE01
Build Date: 12/30/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: fix
   Description:
     [133425] - Showing warning message when user try to add a duplicate rule
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Make sure warning message pops up when user try to add a duplicate rule

2. Category: Fix
   Description:
     [ENGINEERING] - SecureBoot API for new HII
   Infected Motherboard: B12/X12/X13
   Affected functions: Redfish new HII
   Validation:
      1) SecureBoot is passed in SATC

3. Category: fix
   Description:
     [134692] - display symbol of "Descending" ↓ as default? for task page
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Task page -> shows create time is sorted arrow descending

4. Category: fix
   Description:
     [134099] - IPMI Console Capture Video sometime freeze in progress
   Infected Motherboard: ALL
   Affected functions: Console Capture, HTML5, Java KVM
   Validation:
     1) Enable console capture video and set 'Record until POST ends'
     2) Run HTML5 client
     3) Do power reset on SUT
     4) After BIOS POST, check video file on console capture page

5. Category: fix
   Description:
     [ENGINEERING] - Fix BIOS UFFN version mismatch
   Infected Motherboard: All
   Affected functions: Redfish
   Validation:
     1) Update BIOS thenGet /redfish/v1/UpdateService/FirmwareInventory/BIOS to check UniqueFilename

6. Category: fix
   Description:
     [134083] - [LCS-AOC-S3908L-H8IR-16DD] There are extra labels for HDD operation in BMC WEB UI.
   Infected Motherboard: ALL
   Affected functions: Storage
   Validation:
     1) Log in Web.
     2) Select Storage/Physical View
     3) Select drive; then run "Disk Erase"
     4) Select drive; then run "Erase Abort"

7. Category: fix
   Description:
     [134699] - Used wrong information will return Oops! error while mount ISO (Virtual Media).
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) VM -> fail vm -> Incorrect user/pass error msg shows

8. Category: Fix
   Description:
     [132720] Fix #132720 STD --17198--1.02.02--Web Notification Alert
   Infected Motherboard: ALL
   Affected functions: SEL
   Validation:
     0) Setup Redfish event receiver
     1) raw 4 2 4 5 aa 8 0 ff ff f
        Check redfish can receive event

9. Category: fix
   Description:
     [134190] fix - Sensor readings not show all NVMe temp in BMC
   Infected Motherboard: All
   Affected functions: Sensor
   Validation:
     1) check sensor name via ipmitool

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.10
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211217_01.02.10_STDsp.bin
Production signed Firmware CRC: 7DFE478A
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211217_01.02.10_STDsp.bin
Production signed eMMC Firmware CRC: EE294494
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20211217_01.02.10_STDsp.bin
Production signed SPI NOR Firmware CRC: 45069889
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211217_01.02.10_STDsd.bin
Debug signed Firmware CRC: 89D7E0DB
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211217_01.02.10_STDsd.bin
Debug signed eMMC Firmware CRC: DB80B2CC
Build Date: 12/17/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: Fix
   Description:
     [134696] - AC cycle got Dedicated LAN Link Down event
     [133687] - Fan speed miss detect / LAN Link Up - Down - Up in BMC log
   Infected Motherboard: ALL
   Affected functions: BMC LAN
   Validation:
     Testcase 1:
       1) Clear SEL and reboot SUT
       2) Check SEL should contain only one Link up event
     Testcase 2:
       1) Change lan mode to failover.
       2) Check SEL should contain only one Link down up event

2. Category: fix
   Description:
     [ENGINEERING] - PSU Input voltage/Current/Power wording to support AC Input
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web -> PSU page
     2) If input voltage between 20V to 80V, text is DC Input..., else AC Input...

3. Category: fix
   Description:
     [133589] - Unable to login to BMC
   Infected Motherboard: ALL
   Affected functions: Web, Redfish
   Validation:
     1) Enable MEL, syslog, and then enable IP Access control.
     2) Make sure MEL of IP Access Control only create once.

4. Category: fix
   Description:
     [134402] - IPMI Web - System - Component Info - PSU - Fan2 shows 0 RPM
   Infected Motherboard: ALL
   Affected functions: PSU info
   Validation:
     1) Log in Web.
     2) Check system - Component Info - PSU info
        If FAN2 is exist, show xxx RPM.
        If FAN2 is not exist, show N/A.
        Model		Fan
        PWS-1K02A-1R	1
        PWS-1K22A-1R	1
        PWS-1K22F-1R	1
        PWS-1K24A-1R	1
        PWS-1K30D-1R	1
        PWS-1K31D-1R	1
        PWS-1K60D-1R	2
        PWS-1K62A-1R	1
        PWS-1K63A-1R	2
        PWS-1K66P-1R	2
        PWS-2K03P-1R	2
        PWS-2K04D-1R	2
        PWS-2K05A-1R	2
        PWS-2K06F-1R	2
        PWS-2K07F-1R	1
        PWS-2K08A-1R	1
        PWS-2K08F-1R	1
        PWS-2K63A-1R	2
        PWS-751P-1R	1
        PWS-901A-1R	1
        PWS-901F-1R	1
        PWS-902A-1R	1
        PWS-903A-1R	1
        PWS-903A-1R	1
        PWS-1K69P-1R	1
        PWS-1K64P-1R	1
        PWS-2K70A-1R	1
        PWS-2K70F-1R	1
        PWS-751F-1R	1

5. Category: fix
   Description:
     [134686] - It shouldn't sort by "Health Status" and "state" at same time
     [134692] - Default sorting task by "Create Time" (Descending) is more user friendly
     [134734] - "Update" and "Inventory" didn't translation to Chinese simplified and Japanese
     [134738] - "System Lockdown" didn't trasnlation to CHinese simplified and truncation
     [134749] - "Host Interface" and "System Lockdown" display incomplete and overlap (Japanese)
     [134748] - "System Lockdown" didn't translation to Chinese simplified and truncation.
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) firmware page -> "update" and "inventory" translated for all languages
     3) task page -> on load, sorted by latest created -> can order each column individually
     4) BMC configurations -> all tabs translated

6. Category: Fix
   Description:
     [134603] Fix - CPU Health severity is not correct on Dashboard(System) and Component Info
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     Testcase 1:
       1) Add sel 0x04 0x02 0x01 0x04 0xd4 0xff 0x6f 0xa5 0x00 0x81
       2) Check system status turn yellow
       3) Check cpu status turn yellow

7. Category: Fix
   Description:
    [ENGINEERING] Fix - Host now automatically powers on (if host is off) after BIOS Update Golden
   Infected Motherboard: ALL
   Affected functions: PFR
   Validation:
    1) Navigate to Maintenace -> Firmware Management -> Firmware Inventory on the Web GUI
    2) Execute BIOS Update Golden
    3) Host should automatically power on after recovery

8. Category: fix
   Description:
     [134365] - Some NVME information missing on IPMI webGUI.
   Infected Motherboard: X12DPG_QR
   Affected functions: Storage
   Validation:
     1) Log in Web.
     2) Check Storage/Physical View

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.09
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211210_01.02.09_STDsp.bin
Production signed Firmware CRC: 50C2582E
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211210_01.02.09_STDsp.bin
Production signed eMMC Firmware CRC: DC338A72
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20211210_01.02.09_STDsp.bin
Production signed SPI NOR Firmware CRC: 45069889
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211210_01.02.09_STDsd.bin
Debug signed Firmware CRC: C22FF756
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211210_01.02.09_STDsd.bin
Debug signed eMMC Firmware CRC: 8F5E7403
Build Date: 12/10/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: fix
   Description:
     [133906] - iKVM Record video function no display under HTML5 remote console
   Infected Motherboard: All
   Affected functions: HTML5 record video
   Validation:
     1) Run record function under HTML5 remote console
     2) Download video file and play video file

2. Category: fix
   Description:
     [134437] - Fail to Setup Time Zone
     [134559] - Time zone won't able to change under NTP server via WebGUI
     [134556] - BMC failed to set timezone
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web -> Date/Time Page
     2) Save configuration with time zone changed -> save successfully

3. Category: Fix
   Description:
     [133273] - User is able to delete itself while logged in.
   Infected Motherboard: ALL
   Affected functions: Web & Redfish
   Validation:
     1) Add the new User TestAdmin and login Web
     2) Using the Web interface to del the user TestAdmin. It Will pop the error message
        Unable to delete user [TestAdmin]. Please make sure the user is not logged in.

4. Category: fix
   Description:
     [134149] - User is able to enter 65 characters as Authentication Key and Encryption key when setting Alerts with SNMPv3
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Alerts-> edit alert -> SNMPv3 -> key error message is 8-65 characters

5. Category: Fix
   Description:
    [134605] - Should now be able to upload .ima files onto Floppy Disk on Web GUI
   Infected Motherboard: ALL
   Affected functions: Virtual Media
   Validation:
    1) Navigate to Configuration -> Virtual Media
    2) Upload Floppy Disk file with .ima extension

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.08
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211203_01.02.08_STDsp.bin
Production signed Firmware CRC: 8C2805FD
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211203_01.02.08_STDsp.bin
Production signed eMMC Firmware CRC: 21B5CF63
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20211203_01.02.08_STDsp.bin
Production signed SPI NOR Firmware CRC: E1BD5BE1
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211203_01.02.08_STDsd.bin
Debug signed Firmware CRC: B6B41B98
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211203_01.02.08_STDsd.bin
Debug signed eMMC Firmware CRC: DAA9800F
Build Date: 12/03/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: fix
   Description:
     [134086] -[LCS-AOC-S3908L-H8IR-16DD] Populate S3908L-H8IR-16DD without BBU but the BBU status is error.
   Infected Motherboard: ALL
   Affected functions: Storage
   Validation:
     1) Log in Web.
     2) Check storage info/BBU status

2.Category: Fix
    [132987] - IPMIECO TC 267 Mount ISO over IPv6 fail
  Infected Motherboard: ALL
  Affected Functions: IPv6
  Validation:
    1)Run IPMIECO TC267 Mount ISO over IPv6, it should pass
    2)Execute raw cmd 0x30 0x42 to load bmc default, then enable IPv6, IPv6 connection should be okay.

3. Category: fix
   Description:
     [134150] - User name and password requirement are inconsistent with tips/Help info
     [134149] - User is able to enter 65 characters as Authentication Key and Encryption key when setting Alerts with SNMPv3 protocol 
     [ENIGNEERING] - Task page update: remove ID
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Users Page -> type username that is not allowed -> tip message update 4-15 characters only
     3) notification page -> edit alert -> SNMPv3-> for auth key and private key no more than 64 characters
     4) Task page -> id is hidden

4. Category: fix
   Description:
     [133280] - [IPMI ECO 01.02.04] Automation tests Failure.
   Infected Motherboard: All
   Affected functions: Configuration
   Validation:
     1) FW update from 01.02.05 to the latest FW, web session should keep the same

5. Category: Fix
   Description:
    [134075] - [REDFISH] CPU SEL event triggers SEL itself to return 500
   Infected Motherboard: ALL
   Affected functions: SEL display
   Validation:
    1) Send ipmi raw 04 02 01 04 d4 ff 6f a5 00 81
    2) GET /redfish/v1/Systems/1/LogServices/Log1/Entries, should not get 500 error
    3) On WEB, Dashboard.Recent Log and System > Health Event Log pages, should be able to display SEL

6. Category: fix
   Description:
     [133934] - Upper right corner language no change in IPMI Web GUI
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Welcome back in upper right hand corner translate when changing languages

7. Category: Fix
   Description:
    [133069] Fix - PFR "Recover" button now greys out when DCMS license is unactivated.
   Infected Motherboard: ALL
   Affected functions: PFR
   Validation:
    1) When license activated is not DCMS, check Firmware Inventory PFR page.
    2) "Recover" button should exist, but be greyed out.
    3) "Recover" button should only be accessible with DCMS license activated.

8. Category: Fix
   Description:
    [132720] - Web Notification Alert issue -smtp alert
    [134148] - Unable to configure SMTP when setting Alerts
   Infected Motherboard: ALL
   Affected functions: SMTP
   Validation:
     1) Setup SMTP alert
     2) Check received mail while MEL created

9. Category: fix
   Description
     [ENGINEERING] - support BPN-NVME4-228N-S4
   Infected Motherboard: X12DPG-QR
   Affected functions: NVME
   Validation:
     1) install BPN-NVME4-228N-S4 and verify WEBUI storage page

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.07
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211122_01.02.07_STDsp.bin
Production signed Firmware CRC: FA85372D
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211122_01.02.07_STDsp.bin
Production signed eMMC Firmware CRC: 6DA420DF
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20211122_01.02.07_STDsp.bin
Production signed SPI NOR Firmware CRC: E1BD5BE1
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211122_01.02.07_STDsd.bin
Debug signed Firmware CRC: 464764DF
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211122_01.02.07_STDsd.bin
Debug signed eMMC Firmware CRC: 10E62224
Build Date: 11/22/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: fix
   Description:
     [133473] - SYS-220GQ-TNAR+ GPU S/N showing incorrectly or missing info on WebGUI
   Infected Motherboard: X12DPG-QR
   Affected functions: GPU info
   Validation:
     1) Install 4 GPU and check GPU info in webpage

2. Category: fix
   Description:
     [133642] - ME status shows "Recovery" after finishing update BIOS 1.1b fw by using the flashupdate tool
   Infected Motherboard: ALL
   Affected functions: BIOS update
   Validation:
     1) using the flashupdate tool, do BIOS update
     2) FlashUpdateAct.nsh BIOS_X12DGQ-R-1C37_20211101_1.1b_STDsp.bin /B /P /N /K /R /ME

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.06
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211119_01.02.06_STDsp.bin
Production signed Firmware CRC: 8DE668C7
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211119_01.02.06_STDsp.bin
Production signed eMMC Firmware CRC: 48F242BD
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20211119_01.02.06_STDsp.bin
Production signed SPI NOR Firmware CRC: E1BD5BE1
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211119_01.02.06_STDsd.bin
Debug signed Firmware CRC: 40F92383
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211119_01.02.06_STDsd.bin
Debug signed eMMC Firmware CRC: 446D58F0
Build Date: 11/19/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: new
   Description:
     [ENGINEERING] - new JAVA certificate
   Infected MotherBoard: ALL
   Affected Function: JAVA console
   Validation:
     1)Check Java Console certificate

2. Category: new
   Description:
     [ENGINEER] - Support BIOS rumtime update
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) update BIOS during power on via web

3. Category: fix
   Description:
     [133286] - Automation tests Failure.
   Infected Motherboard: ALL
   Affected functions: CMD
   Validation:
     1) sum -c KeyProductDeletion --key_name SFT-DCMS-SVC-KEY
     2) sum -c QueryProductKey

4. Category: Fix
   Description:
     [133282] - Set Initial value to object of subject.
   Infected MotherBoards: ALL
   Affected Function: Web page
   Validation:
     1) Login BMC web GUI -> Configuration -> Notification -> Alerts page
     2) Modify Alert, select Protocol : SMTP
     3) Check default value of "Subject" field

5. Category: Fix
   Description:
     [133321] - Modify title for the field
   Infected MotherBoards: ALL
   Affected Function: Web page
   Validation:
     1) Login BMC web GUI -> Configuration -> Notification -> Alerts page
     2) Modify Alert, select Protocol : Redfish
     3) Check all field

6. Category: Fix
   Description:
     [133338] - Modify title for fields
   Infected MotherBoards: ALL
   Affected Function: Web page
   Validation:
     1) Login BMC web GUI -> Configuration -> Notification -> Alerts page
     2) Modify Alert, select Protocol : SNMPv3
     3) Check Authentication key / Authentication Protocol /Encryption Key/Encryption Protocol fields

7. Category: Fix
   Description:
     [133335] - Set default 'checked' to Auth and Private protocol
   Infected MotherBoards: ALL
   Affected Function: Web page
   Validation:
     1) Login BMC web GUI -> Configuration -> Notification -> Alerts page
     2) Modify Alert, select Protocol : SNMPv3
     3) Check Authentication Protocol /Encryption Protocol fields

8. Category: Fix
   Description:
     [133334] - String Handling
   Infected MotherBoards: ALL
   Affected Function: Web page
   Validation:
     1) Login BMC web GUI -> Configuration -> Notification -> Alerts page
     2) Modify Alert, select Protocol : SNMPv3
     3) Check Authentication/Encryption key fields

9. Category: fix
   Description:
     [133381] - Upload wrong type of "IPMI Configuration" file should not allow to reload
     [133380] - Couldn't remove selected file due to "X" is out of frame
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) IPMI Config page -> upload non .bin file -> attempt to save configuration
     3) license active page -> upload file -> click x to remove file successfully

10.Category: Fix
   Description:
    [133394] - Update BIOS on Next Boot can now be triggered by "Power Reset"
   Infected Motherboard: ALL
   Affected functions: Firmware Update
   Validation:
    1) Upload BIOS on Web GUI
    2) Choose "Update on next boot"
    3) After BIOS firmware finishes uploading, "Power Reset" host.
    4) BIOS update should run

11. Category: fix
   Description:
     [131042] - Systemlockdown issue on the web
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Enable system lockdown mode
     3) Visit configuration directory page and troubleshooting page
     4) Go back to system lockdown page and disable successfully

12.Category: Fix
   Description:
     [ENGINEERING] - Backward compatible to support AOC-STG-b2T with PLDM or original thermal reading.
   Infected MotherBoard: AOC-STG-b2T
   Affected Function: AOC_NIC temperataure
   Validation:
     1)install AOC-STG-b2T with NCT6683, verify AOC_NIC temperataure reading.
     2)install AOC-STG-b2T enabled PLDM fw214(PLDM sensor number is 0x0003), verify AOC_NIC temperataure reading.
     3)install AOC-STG-b2T enabled PLDM newfw(PLDM sensor number is 0x012C), verify AOC_NIC temperataure reading.

13.Category: fix
   Description:
     [127638] - Enable autoconfig when IPv6 is enabled with stateless mode to fix TC267
   Infected Motherboard: ALL
   Affected functions: Web, IPMI
   Validation:
     1) On web page, the autoconfig switch should be "on" state and "disabled" when IPv6 is disabled
     2) Using IPMI command to enable IPv6 will also turn on autoconfig

14.Category: fix
   Description:
     [132970] - Domain Name Save Issue DDNS Page
   Infected Motherboard: ALL
   Affected functions: DDNS
   Validation:
     1) Go To Dynamic DNS page
     2) Input any valid domain to [Dynamic DNS Server Address] textfield, Click save
     3) The valid domain name should be saved and appear in the textfield after a successful save

15.Category: Fix
   Description:
     [132720] - Web Notification Alert
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
      1) Modify alert with Redfish setting.
         select target event type individually( like Resource added only)
      2) Trigger event
      3) Receive Redfish event based on the selected category

16.Category: Fix
   Description:
     [133273] - User is able to delete itself while logged in
   Infected Motherboard: ALL
   Affected functions: Redfish & Web
   Validation:
     Web:
     1) Login BMC web GUI ->go Configuration -> Account Services
     2) Go User page -> Add -> Add user account, example: TestAdmin (privilege: Administrator)
     3) Logout ADMIN
     4) Login TestAdmin->go Configuration -> Account Services
     5) Go User page -> Delete "TestAdmin"
     6) pop the "Some thing wrong message"
     Redfish
     1) Post /redfish/v1/AccountService/Accounts with Base auth: ADMIN
           {"UserName":"test123","Password":"abc12345!","RoleId":"Administrator"}
     2) POST DEL /redfish/v1/AccountService/Accounts/3 with Base auth: test123
           Got 400 bad request

17.Category: fix
   Description:
     [133243] - ikvm port becomes 0 after reloading configuration file
   Infected Motherboard: ALL
   Affected functions: KVM, KVM port number
   Validation:
     1) Login WebGUI
     2) Save current configuration file (Make sure ikvm port no changes)
     3) Reload the configuration with saved configuration file
     4) Check Port page

18.Category: fix
   Description:
     [131042] - Systemlockdown issue on the web
     [133277] - Close" button is out of the "Preference" page on IKVM(HTML5).
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Enable Lockdown -> go to troubleshooting page
     3) Go back to lockdown -> disable lockdown successfully
     4) open IKVM HTML5 -> Option -> Prefences -> Close button in frame for all tabs

19.Category: fix
   Description:
     [133078] - X12 Data Mismatch when Comparing Excel File with Web Event Log
   Infected Motherboard: ALL
   Affected functions: SEL
   Validation:
     Testcase 1:
       1) Add SEL 0x4 0x2 0x4 0x01 0x01 0x01 0x02 0x00 0x00
       2) Check https://$IP/redfish/v1/Systems/1/LogServices/Log1/Entries property Members > Message without additional space

20. Category: fix
   Description:
     [133473] - SYS-220GQ-TNAR+ GPU S/N showing incorrectly or missing info on WebGUI
   Infected Motherboard: X12DPG-QR
   Affected functions: GPU info
   Validation:
     1) Install 4 GPU and check GPU info in webpage

21.Category: Fix
   Description:
     [133532] The GPU location in the WebUI is not displayed clearly
   Infected MotherBoards: ALL
   Affected Function: GPU Info
   Validation:
     1) Insert GPU on MB
     2) Check GPU information page, the location data should show System Slot + slot number


--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.05
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211105_01.02.05_STDsp.bin
Production signed Firmware CRC: A9600EED
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211105_01.02.05_STDsp.bin
Production signed eMMC Firmware CRC: 76AD6F83
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20211105_01.02.05_STDsp.bin
Production signed SPI NOR Firmware CRC: 13F547D2
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211105_01.02.05_STDsd.bin
Debug signed Firmware CRC: 0B419A81
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211105_01.02.05_STDsd.bin
Debug signed eMMC Firmware CRC: 150CAAE6
Build Date: 11/05/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: Fix
   Description:
     [132844] [- Storage card controller 'create raid' button still enable when system lockdown disable.
   Infected Motherboard: ALL
   Affected functions: Web page "Broadcom Storage Controller".
   Validation:
     1) Install Broadcom raid card (ex: AOC-S3108L, SAS3908)
     2) Active BMC Product Key
     3) Login BMC web, go to "Storage Monitoring -> Controller View -> Broadcom Storage Controller" page.
     4) Web page will show Configuration buttons (ex: Create RAID, Import Foreign Configurations,
                                                 Clear Foreign Configurations, Clear all configurations ......)
     4) Enable system lock down
     5) Go to "Storage Monitoring -> Controller View -> Broadcom Storage Controller" page.
        All configuration buttons will be disabled.

2. Category: Feature
   Description:
     [ENGINEERING] – Intel Cscripts through redfish
   Infected Motherboard: B12, X12
   Affected functions: Redfish
   Validation:
     1) consult TS team
     2) Run Cscript python.exe .\startCscripts.py -a redfish -H $IP -U $username -P $password

3. Category: Fix
   Description:
    [ENGINEERING] - Redfish response inconsistence
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
    1) verify via SATC

4. Category: fix
   Description:
      [132860] - NTP primary server check for correct IP
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web -> Date/Time
     2) Try to save setting with NTP server 'localhost', fails
     3) Only allows correct formatted IP

5. Category: Fix
   Description:
     [132778] - FAN curve of SMART SPEED mode in incorrect
   Infected Motherboard: X12DPG-QR
   Affected functions: SMART SPEED
   Validation:
    1) verify FAN SMART SPEED fan curve. Verified


--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.04
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211027_01.02.04_STDsp.bin
Production signed Firmware CRC: E503B410
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211027_01.02.04_STDsp.bin
Production signed eMMC Firmware CRC: EC7AA6DC
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20211027_01.02.04_STDsp.bin
Production signed SPI NOR Firmware CRC: 13F547D2
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211027_01.02.04_STDsd.bin
Debug signed Firmware CRC: BEA0D6F6
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211027_01.02.04_STDsd.bin
Debug signed eMMC Firmware CRC: 76599533
Build Date: 10/27/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: Fix
   Description:
    [132775] - PFR Recover Action now only accessible with DCMS License on firmware inventory page
   Infected Motherboard: ALL
   Affected functions: PFR
   Validation:
    1) With OOB License activated, Navigate to Firmware Inventory page
    2) Select "Platform Resiliency Actions"
    3) "Recover" functions should not be shown

2. Category: Fix
   Description:
     [129850] - pminfo reading issues
   Infected Motherboard: ALL
   Affected functions: PMBUS STD PSU.
   Validation:
     1) Read pminfo: SMCIPMITool.exe BMCIP ADMIN ADMIN pminfo
     2) PWS Revision will display at console.

3.Category: Fix
  Description:
    [132501] - HTML5 concole keeps connecting when performing ikvm reset
  Infected Motherboard: ALL
  Affected Function: HTML5
  Validation:
    1) Launch HTML5 iKVM
    2) Perform reset iKVM
    3) HTML5 iKVM should be terminated.

4. Category: Fix
   Description:
     [132498] - Password requirement doesn’t match
   Infected Motherboard: ALL
   Affected functions: Account
   Validation:
     1)	use WEBUI/redfish create user with password(Aa34567890123456789) is successfully.
     2)	Use WEBUI/redfish create user with password(Aa345678901234567890) return fail.

5. Category: fix
   Description:
     [ENGINEERING] - RHEL 8.3 hang up issue.
   Infected Motherboard: ALL X12
   Affected functions: eSPI
   Validation:
     1) enable both COM1 and COM2/SOL and do serial stress
     2) per LAB testing result, it pass

6. Category: fix
   Description:
     [131892] - B12SPE NIC1 and NIC2 MAC addresses swapped (reported by Intel)
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Lan MAC Addresses information displayed correctly

7. Category: fix
   Description:
     [132047] - different drives are displaying on BMC Web Gui Issues
   Infected Motherboard: ALL
   Affected functions: NVMe Storage.
   Validation:
     1) Insert Samsung PM9A3 NVMe drive.
     1) Log in Web.
     2) Storage/Physical View
     3) Check if the NVMe drive "Disk Info#" and "Link Speed" are
        correct.

8. Category: fix
   Description:
     [127638] - IPv6 address list is not cleared
   Infected Motherboard: ALL
   Affected functions: IPMI
   Validation:
     1) Switch to failover mode. Add a new IPv6 address on web page, and then run cmd 0x30 0x42. Make sure IPv6 address list is cleared after reboot
     2) Switch to dedicated mode. Add a new IPv6 address on web page, and then run cmd 0x30 0x42. Make sure IPv6 address list is cleared after reboot
     3) Switch to shared mode. Add a new IPv6 address on web page, and then run cmd 0x30 0x42. Make sure IPv6 address list is cleared after reboot

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.03
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211018_01.02.03_STDsp.bin
Production signed Firmware CRC: 3B464533
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211018_01.02.03_STDsp.bin
Production signed eMMC Firmware CRC: 58650FE5
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20211018_01.02.03_STDsp.bin
Production signed SPI NOR Firmware CRC: 6B626D46
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211018_01.02.03_STDsd.bin
Debug signed Firmware CRC: C4F31355
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211018_01.02.03_STDsd.bin
Debug signed eMMC Firmware CRC: 6650088A
Build Date: 10/18/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1.Category: New
  Description:
    [ENGINEERING] - USB LAN between BMC and BIOS should work with all BIOS with USB LAN local MAC or USB LAN global MAC.
    [ENGINEERING] - Add new raw command 30 68 E1 to select host MAC for redfish host interface
  Infected Motherboard: ALL
  Affected Function: redfish host interface
  Validation:
    1) Check with BIOS engineer to get three BIOS: 
        one BIOS that does support ipmi raw 30 68 E1
        one BIOS that does not supported ipmi raw 30 68 E1, but use USB LAN local MAC
        one BIOS that does not supported ipmi raw 30 68 E1, but use USB LAN global MAC 
    2) Go to UEFI shell and run 'ifconfig -l -b'
    3) HOSTINTERFACE should have valid MAC and valid IP
    4) Do ac cycle/system reset/power onoff, HOSTINTERFACE should have valid MAC and valid IP

2. Category: fix
   Description:
     [ENGINEERING] - support Nvidia A16 and A2
   Infected Motherboard: ALL
   Affected functions: GPU
   Validation:
     1) GPU temperature and Info

3. Category: fix
   Description:
     [ENGINEERING] - support Intel GPU Artic Sound-P
   Infected Motherboard: ALL
   Affected functions: GPU
   Validation:
     1) GPU temperature and Info, only Model name is ready to read

4. Category: fix
   Description:
     [ENGINEERING] - AOC-A25G-i2SM temperature
   Infected Motherboard: ALL
   Affected functions: AIOM
   Validation:
     1) Check AIOM Temp and AOC network info. Info depends on VPD programming

5. Category: Fix
   Description:
     [128595] – Set Lock down Mode to yes but not work
   Infected Motherboard: B3ST1, BH12SSi
   Affected functions: OOBCmd
   Validation:
     1) ./sum -i bmcip -u ADMIN -p ADMIN -c setlockdownmode --lock yes --reboot
     2) ./sum -i bmcip -u ADMIN -p ADMIN -c Getlockdownmode
     3) ./sum -i bmcip -u ADMIN -p ADMIN -c setlockdownmode --lock no --reboot

6. Category: Fix
   Description:
     [131042] - System lockdown issue on the web
   Infected Motherboard: ALL
   Affected functions: Power sidebar, Marvell controller 'create raid' button.
   Validation:
     Create Read button:
     1.) Add Marvell raid card at system.
     2.) Power ON system, Login BMC and go to Configuration --> BMC Settings --> System Lockdown page.
     3.) Enable System Lockdown.
     4.) Go to Storage --> Controller View --> Marvell --> Create Read button disabled.
     Power sidebar:
     1.) Power ON system, Login BMC and go to Configuration --> BMC Settings page.
     2.) Check Power sidebar All options Enabled (Power Down - Immediate,  Graceful Shutdown, Power Cycle,  Power Reset).

7. Category: fix
   Description:
     [131075] - Web element isn't disabled when login with user privilege
   Infected Motherboard: ALL
   Affected functions: remote , console capture video
   Validation :
      1. Login IPMI Web GUI with User Privilege
      As "User" privilege, user only has "read-only" privilege for below items:
         1) Dashboard >> Switch 'UID' to [ON]
         2) Remote Control >> Launch Console >> Choose option 'HTML5'
         3) Maintenance >> Troubleshooting >> Console Capture >> Console Capture Video >> Swich 'Enable' to [ON]

8.Category: Fix
  Description:
    [130851] - Failed to run IPMIECO Automation test (TC401/402)
  Infected Motherboard: ALL
  Affected Function: User Management
  Validation:
    1) Get new version SMCIPMITool (SMCIPMITool_2.25.1_build.211001) or later.
    2) Run SMCIPMITool $IP $USER $PWD user add 6 test1 Test1234 0x4 to add user, user should be added successfully.
    3) Run SMCIPMITool $IP $USER $PWD user add 7 test1 Test1234 0x3 to add user, it should be failure because user name is duplicated, IPMI response code is 0x01
    4) Run SMCIPMITool $IP $USER $PWD user add 7 test2 test1234 0x3 to add user, it should be failure because user pwd check is fail, IPMI response code is 0x011
    5) Run SMCIPMITool $IP $USER $PWD user delete 6, the user should be deleted.

9. Category: fix
   Description:
     [Fix] Fix AOC-S25G-m2S no link status.
   Infected Motherboard: ALL
   Affected functions: Network AOC.
   Validation:
     1) Insert AOC-S25G-m2S
     2) Log in Web.
     3) System/Component Info/Network AOC
     4) Check AOC-S25G-m2S link status

10.Category: Fix
   Description:
     [ENGINEERING] - Directory Service support group only
   Infected Motherboard: ALL
   Affected functions: AD/LDAP
   Validation:
     TestCase1:
     1) config AD configuration with group normal
     2) login successfully

     TestCase2:
     1) config LDAP configuration with POSIX group
     2) login successfully

11.Category: fix
   Description:
     [132245] - [S3108-SAS] BMC fail to delete the Raid configuration
   Infected Motherboard: ALL
   Affected functions: SAS3108
   Validation:
     1) Let Raid configuration be in "Background initialization progress" ( OS mdoe).
     1) Log in Web.
     2) Storage/Logical View
     3) Check if the logical drive can be selected or not.

12.Category: Fix
   Description:
     [131966] - IPMICFG execute IPv6 command "-addrptl 2" failed
   Infected Motherboard: All
   Affected functions: IPMI IPv6 commands
   Validation:
     1) Issue below commands in-band on the OS and expect normal return code.
          ipmitool raw 0xc 1 1 0x33 0 (IPV6_ADDRESS_NOT_SUPPORT)
          ipmitool raw 0xc 1 1 0x33 1 (IPV6_ADDRESS_IPV6_ONLY)
          ipmitool raw 0xc 1 1 0x33 2 (IPV6_ADDRESS_IPV6_AND_IPV4)
     2) Issue below IPMICFG commands in-band on the OS and expect normal return code.
          ./IPMICFG.x86_64 -addrptl 1 (IPV6_ADDRESS_NOT_SUPPORT)
          ./IPMICFG.x86_64 -addrptl 2 (IPV6_ADDRESS_IPV6_ONLY)
          ./IPMICFG.x86_64 -addrptl 3 (IPV6_ADDRESS_IPV6_AND_IPV4)

13.Category: fix
   Description:
     [130770,130772,130774] STD -- 19146-- Latest Version – [Security] Buffer overflow in ipmi_lan ASF protocol
     [130776~130778]STD -- 19146 -- Latest Version – [Security] DoS BMC with incorrect IPMI operate packet
   Infected Motherboard: X12 H12 X11
   Affected functions: ASFMsgHandler, LAN_Recv, DecodeRMCPPlusIPMIPKG
   Validation :
     1) Custom security testing script

14.Category: fix
   Description:
      [ENGINEERING] default preserve boot option if update BIOS not set PreserveBOOTCONF
   Infected Motherboard: X12
   Affected functions: Redfish
   Validation:
     1) Post /redfish/v1/UpdateService/upload with UpdateParameters:
        {"@Redfish.OperationApplyTime" : "OnReset", "Oem" : {"Supermicro" : {"BIOS" : {"BackupBIOS" : false,"PreserveME" : false,"PreserveNVRAM" : false,"PreserveSMBIOS" : true}}},"Targets" : ["/redfish/v1/Systems/1/Bios"]}
     2) Post /redfish/v1/UpdateService/Oem/Supermicro/FirmwareInventory/BIOS/Actions/SmcFirmwareInventory.Update with {"PreserveSMBIOS":true,"BackupBIOS":false}

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.02
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211007_01.02.02_STDsp.bin
Production signed Firmware CRC: E96C1FFB
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211007_01.02.02_STDsp.bin
Production signed eMMC Firmware CRC: D394B9D5
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20211007_01.02.02_STDsp.bin
Production signed SPI NOR Firmware CRC: 6B626D46
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211007_01.02.02_STDsd.bin
Debug signed Firmware CRC: 838F1809
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211007_01.02.02_STDsd.bin
Debug signed eMMC Firmware CRC: 78F7EF2E
Build Date: 10/07/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: fix
   Description:
     [ENGINEERING] - Remove MouseMode, IKVM and Snooping license check
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) remove all license
     2) Get /redfish/v1/Managers/1/Oem/Supermicro/MouseMode
     3) Get /redfish/v1/Managers/1/Oem/Supermicro/IKVM
     4) Get /redfish/v1/Managers/1/Oem/Supermicro/Snooping

2. Category: Fix
   Description:
     [131139] - Fail to unlock the ADMIN account
   Infected Motherboard: ALL
   Affected functions: Account
   Validation:
     1) Reset to ADMIN/ADMIN, and add one Administrator user Tester001
     2) let ADMIN user locked
     3) Use Tester001 unlock ADMIN
        expecting: unlock ADMIN successfully

3. Category: fix
   Description:
     [ENGINEERING] - Fix OEMGetSetSmartCool 30 70 73 cmd response
   Infected Motherboard: ALL
   Affected functions: Cmd
   Validation:
     1) raw 0x30 0x070 0x73 0x00 return 0xCC

4. Category: fix
   Description:
     [131933] - [3108-SAS] Blink LED feature not working in logical view page and no option to delete Raid volume as well.
   Infected Motherboard: ALL
   Affected functions: BRCM Storage.
   Validation:
     1) Log in Web.
     2) Storage/Logical View
     3) Check if Blink/Unblik works w/o license

5. Category: fix
   Description:
     [131783] - multi function should grey out when login with user priv
   Infected Motherboard: ALL
   Affected functions: web
   Validation:
     1) login with user priv
     2) Maintenance -> Troubleshooting -> function should not work
     3) Remote Control -> all function should not work


--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.01
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211002_01.02.01_STDsp.bin
Production signed Firmware CRC: 5E3D7BD6
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211002_01.02.01_STDsp.bin
Production signed eMMC Firmware CRC: E06256B9
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20211002_01.02.01_STDsp.bin
Production signed SPI NOR Firmware CRC: 6B626D46
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20211002_01.02.01_STDsd.bin
Debug signed Firmware CRC: 26FC21A4
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20211002_01.02.01_STDsd.bin
Debug signed eMMC Firmware CRC: 59235DC2
Build Date: 10/02/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: Fix
   Description:
     [ENGINEERING] - somehow the firmware uploading is hanging in few cases.
   Infected Motherboard: ALL
   Affected functions: Firmware Uploading
   Validation:
     1) try to do any firmware update.

2.Category: New
    [ENGINEERING] - Add new raw command 0x30 0x68 0x39 to add/delete user account.
    [ENGINEERING] - SMCIPMItool automation test failure
  Infected Motherboard: ALL
  Affected Function: User Management
  Validation:
    1) Get latest version SMCIPMITool (SMCIPMITool_2.25.1_build.211001)
    2) Run SMCIPMITool $IP $USER $PWD user add 6 test1 Test1234 0x4 to add user, user should be added successfully.
    3) Run SMCIPMITool $IP $USER $PWD user add 7 test1 Test1234 0x3 to add user, it should be failure because user name is duplicated, IPMI response code is 0x01
    4) Run SMCIPMITool $IP $USER $PWD user add 7 test2 test1234 0x3 to add user, it should be failure because user pwd check is fail, IPMI response code is 0x011
    5) Run SMCIPMITool $IP $USER $PWD user delete 6, the user should be deleted.

3. Category: Fix
   Description:
     [131790] - Missing NVMe graphics
   Infected Motherboard: ALL
   Affected functions: storage WEBUI
   Validation:
     1) not install SAS controller, just install NVMe
     2) check storage summary WEBUI

4. Category: Fix
   Description:
     [131731] fix – After issue the DC28 of cmd then check BMC web found Description is incorrect
   Infected Motherboard: ALL
   Affected functions: SEL
   Validation:
     Testcase 1:
       1) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x00 0xFF 0xFF then get sel description should meet spec
       2) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x01 0xFF 0xFF then get sel description should meet spec
       3) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x02 0xFF 0xFF then get sel description should meet spec
       4) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x10 0xFF 0xFF then get sel description should meet spec
       5) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x11 0xFF 0xFF then get sel description should meet spec
       6) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x12 0xFF 0xFF then get sel description should meet spec
       7) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x20 0xFF 0xFF then get sel description should meet spec
       8) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x21 0xFF 0xFF then get sel description should meet spec
       9) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x22 0xFF 0xFF then get sel description should meet spec
       10) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x30 0xFF 0xFF then get sel description should meet spec
       11) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x31 0xFF 0xFF then get sel description should meet spec
       12) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x32 0xFF 0xFF then get sel description should meet spec
       13) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x40 0xFF 0xFF then get sel description should meet spec
       14) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x41 0xFF 0xFF then get sel description should meet spec
       15) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x42 0xFF 0xFF then get sel description should meet spec
       16) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x50 0x10 0x12 then get sel description should meet spec
       17) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x50 0x20 0x12 then get sel description should meet spec
       18) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x50 0x30 0x12 then get sel description should meet spec
       19) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x51 0x10 0x12 then get sel description should meet spec
       20) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x51 0x20 0x12 then get sel description should meet spec
       21) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x51 0x30 0x12 then get sel description should meet spec
       22) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x52 0x10 0x12 then get sel description should meet spec
       23) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x52 0x20 0x12 then get sel description should meet spec
       24) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x52 0x30 0x12 then get sel description should meet spec
       25) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x60 0x03 0x12 then get sel description should meet spec
       26) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x61 0x03 0x12 then get sel description should meet spec
       27) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x62 0x03 0x12 then get sel description should meet spec
       28) ipmitool -I lanplus -H 10.184.3.246 -U ADMIN -P ADMIN raw 0x04 0x02 0x04 0xDC 0xFF 0x6F 0x63 0x03 0x12 then get sel description should meet spec

5. Category: enhancement
   Description: Fix
     [ENGINEERING] -  Share LAN IP missing of AIOM w/o standby power.
   Infected Motherboard: X12DPT-B6
   Affected Functions: AIOM
   Validation:
     a) disconnect dedicated RJ45 cable. set Failover LAN mode, and dhcp ip
     1) power off system
     2) reboot BMC using UID
     3) wait for 2 minutes
     4) power on system
     5) ping BMC IP
     b) disconnect dedicated RJ45 cable. set Failover LAN mode, and static ip
       all 5 steps
     c) disconnect dedicated RJ45 cable. set Share LAN mode, and static ip
       all 5 steps
     d) disconnect dedicated RJ45 cable. set Share LAN mode, and dhcp ip
       all 5 steps

6. Category: fix
   Description:
      [ENGINEERING] - power consumption always 2W after stress cburn on/off
   Infected Motherboard: Twin Serial
   Affected functions: power reading
   Validation:
     1) overnight Cburn on/off, then check power consumption reading.

7. Category: Fix
   Description:
    [130891] Fix - Updating BIOS via /redfish/v1/UpdateService/Actions/UpdateService.SimpleUpdate now preserves SMBIOS
   Infected Motherboard: ALL
   Affected functions: Firmware Update
   Validation:
    1) Update BIOS via /redfish/v1/UpdateService/Actions/UpdateService.SimpleUpdate
    2) SMBIOS should be preserved

8. Category: Fix
   Description:
     [ENGINEERING] - network AOC no link status
   Infected Motherboard: ALL
   Affected functions: Network AOC
   Validation:
     1) Install AOC-S25G-m2S, plug in network cable; then power on.
     2) Log in web
     3) System/Component Info/Network AOC
     4) Check  AOC-S25G-m2S/link status

9. Category: fix
   Description:
     [ENGINEERING] - support NVME backplane 3003
   Infected Motherboard: X12DPG-QR
   Affected Functions: storage info
   Validation:
     1) in BIOS, change JS1 PCIE 4X4 to support 4 NVME
     2) check BMC storage NVME page

10. Description:
     [131001] - GPU sensor numbering does not match physical location
   Infected Motherboard: X12DPG-QR
   Affected functions: GPU temp
   Validation:
     1) GPU3 and GPU4 temperature should be higher then GPU1 and GPU2


--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.02.00
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210922_01.02.00_STDsp.bin
Production signed Firmware CRC: AD7E2A40
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210922_01.02.00_STDsp.bin
Production signed eMMC Firmware CRC: AC5FBD7F
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210922_01.02.00_STDsp.bin
Production signed SPI NOR Firmware CRC: 6B626D46
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210922_01.02.00_STDsd.bin
Debug signed Firmware CRC: 5EF296BF
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210922_01.02.00_STDsd.bin
Debug signed eMMC Firmware CRC: 9E535089
Build Date: 09/22/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: Fix
   Description:
    [130891] Fix - Updating BMC via /redfish/v1/UpdateService/Actions/UpdateService.SimpleUpdate now preserves configurations
   Infected Motherboard: ALL
   Affected functions: Firmware Update
   Validation:
    1) Update BMC via /redfish/v1/UpdateService/Actions/UpdateService.SimpleUpdate
    2) BMC configurations should be preserved after update.

2. Category: Fix
   Description:
    [130891] Fix - Updating BIOS via /redfish/v1/UpdateService/Actions/UpdateService.SimpleUpdate now prints to MEL
   Infected Motherboard: ALL
   Affected functions: Firmware Update
   Validation:
    1) Update BIOS via /redfish/v1/UpdateService/Actions/UpdateService.SimpleUpdate
    2) BIOS update completion message should print to MEL.

3. Category: enhancement
   Description: Fix
     [ENGINEERING] - network AOC FW version length cut
   Infected Motherboard: ALL
   Affected Functions: Network AOC
   Validation:
     1) Plug in network AOCs
     2) Log in web
     3) Choose System/Component Info/Network AOC and Check FW version

4 .Category: Fix
  Description:
    [129980] - Anonymous account or null value can be created on HW IPMI
  Infected Motherboard: ALL
  Affected Functions: User Management / Redfish
  Validation:
    1) Use ipmitool –I lan –H IP –U ADMIN –P ADMIN user set name 8 ‘’ to set user name, the request should be block when ID or Password is empty
    2) Use ipmitool –I lan –H IP –U ADMIN –P ADMIN user set password 8 ‘’ to set user pwd, the request should be block when ID or Password is empty
    3) Use ipmitool –I lan –H IP –U ADMIN –P ADMIN user priv 8 0x4 to set user privilege, the request should be block when ID or Password is empty
    4) Use ipmitool –I lan –H IP –U ADMIN –P ADMIN user enable 8  to enable user privilege, the request should be block when ID or Password is empty
    5) Use https://BMCIP/redfish/v1/AccountService/Accounts with POST body {"UserName":"SWQAADMIN1","Password":"","RoleId":"Administrator"} to create
       an invalid account, the request should be block.
    6) Downgrade to older BMC FW (such v01.01.13), and repeat step 1 to 4 the user can be created success, and use ipmitool to check user list.
    7) Upgrade to new FW with preserve setting, after upgrade FW, check user list from WEB, the invalid account should be shown on WEB and it should  be disabled.
    8) Use invalid account to access BMC, it should be rejected.

5. Category: Enhancement
   Description:
     [ENGINEERING] - Support EUI-48 Locally Administered MAC Address for Redfish host interface
     [ENGINEERING] - Host interface can get IP in client OS after reboot OS or remove/insert rndis driver.
   Infected Motherboard: All
   Affected functions: Redfish Host interface
   Validation:
     1) SUM used redfish host interface to access BMC in OS
     2) Go to UEFI shell and run 'ifconfig -l -b'
     3) Host Interface should have IP 169.254.3.1 and MAC BE:3A:F2:B6:05:9F
     4) Run PXE stress

6. Category: fix
   Description:
     [130652] - User with User-level permissions can attempt to change UID setting
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web -> user priviledge
     2) Component Info page -> UID button is disabled and greyed out

7. Category: Fix
   Description:
     [130682] - There is no NIC sensor reading.
   Infected Motherboard: All
   Affected functions: Redfish
   Validation:
      1) check Web does not display on-board LAN in X12/X13 and pass SATC for X12 platforms

8. Category: Feature
   Description:
     [ENGINEERING] - Add restore boot configuration during BIOS update
   Infected Motherboard: X12
   Affected functions: BIOS update
   Validation:
     1) web update bios shows Preserve BIOS Boot Options Configuration

9.Category: Fix
  Description:
    [127638] - IPMI ECO Automation test failed (for TC 506 only)
  Infected Motherboard: ROT 20
  Affected functions: multiple PFR actions on RoT20
  Validation:
    1) Queue action item of 'update BMC golden'
        $ sum -i $IP -u ADMIN -p ADMIN -c BmcRotManage --action Stage --stage_golden
    2) Queue action item of 'update BIOS golden'
        $ sum -i $IP -u ADMIN -p ADMIN -c BiosRotManage --action Stage --stage_golden
    3) Update BMC
        $ sum -i $IP -u ADMIN -p ADMIN -c UpdateBMC --file images/AST2600_all.dbg.signed.bin --boot_check
    4) Expected to see that they are all updated

10. Category: Fix
   Description:
     [131001] - GPU sensor numbering does not match physical location
   Infected Motherboard: X12DPG-QR
   Affected functions: GPU temp
   Validation:
     1) GPU3 and GPU4 temperature should be higher then GPU1 and GPU2

11. Category: fix
   Description:
     [130043] fix  - IPMI on/off via dedicated LAN failed after passing 578 cycles
   Infected Motherboard: ALL
   Affected functions: Memory leak.
   Validation:
     1) run LAB IPMI on/off script test.




--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.01.12
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210913_01.01.12_STDsp.bin
Production signed Firmware CRC: 2ED33DF1
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210913_01.01.12_STDsp.bin
Production signed eMMC Firmware CRC: 12EA3F26
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210913_01.01.12_STDsp.bin
Production signed SPI NOR Firmware CRC: 3B8BB73E
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210913_01.01.12_STDsd.bin
Debug signed Firmware CRC: 914BF42F
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210913_01.01.12_STDsd.bin
Debug signed eMMC Firmware CRC: 6CF2A7F1
Build Date: 09/13/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: Feature
   Description:
     [ENGINEER] Add BIOSVersion and BootBlockVersion property in StorageController
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) Get /redfish/v1/Systems/1/Storage/HA-RAID

2. Category: Fix
   Description:
     [130475] - Trying toGenerate Evidence & update FW at the same time behavior mismatch SPEC define.
   Infected Motherboard: ALL
   Affected functions: Evidencne generatioin & download
   Validation:
     1) Manually recover BIOS and generate evidence afterwards
     2) Try to update BMC or BIOS FW and expected to see the error message

3. Category: Enhancement
   Description:
     [ENGINEERING] - Rollback ID alert is now a tooltip
   Infected Motherboard: RoT
   Affected functions: Firmware Update WEBUI
   Validation:
     1) Hover cursor over "Allow Rollback ID To Be Updated"

4. Category: Enhancement
   Description:
     [ENGINEERING] - Rollback ID checkbox for Motherboard CPLD should now be disabled when license is unactivated.
   Infected Motherboard: RoT
   Affected functions: Firmware Update WEBUI
   Validation:
     1) Under Motherboard CPLD, "Allow Rollback ID To Be Updated" checkbox should be disabled when license is unactivated.

5. Category: fix
   Description:
     [124514] - Number of Drives Displaying issues on Overview and Physical View tabs on Storage monitoring
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Storage page displays correct number of drives on summary page for each chart

6. Category: Fix
   Description:
     [130655] - AOC card Thermal reading issue w/ AOC-SLG3-2H8M2 on ipmiweb
   Infected Motherboard: ALL
   Affected Function: sensor, storage
   Validation:
     1) Install AOC-SLG3-2H8M2 on MB
     2) Check related sensor reading on IPMI web
     3) Check related sensor names, should be "AOC_SAS" + system slot + " Temp"
        and "AOC_SSD" + system slot + "Temp"

7. Category: fix
   Description:
     [130398] - FW Inventory Page Loading Unnecessary Buttons
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Firmware inventory page -> only bmc and bios show while loading, then
        rest of buttons will appear


--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.01.12
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210912_01.01.12_STDsp.bin
Production signed Firmware CRC: 5778179F
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210912_01.01.12_STDsp.bin
Production signed eMMC Firmware CRC: 35B9A4A8
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210912_01.01.12_STDsp.bin
Production signed SPI NOR Firmware CRC: 3B8BB73E
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210912_01.01.12_STDsd.bin
Debug signed Firmware CRC: DF0E33AC
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210912_01.01.12_STDsd.bin
Debug signed eMMC Firmware CRC: 7C4FD192
Build Date: 09/12/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: Feature
   Description:
     [ENGINEER] Add BIOSVersion and BootBlockVersion property in StorageController
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) Get /redfish/v1/Systems/1/Storage/HA-RAID

2. Category: Fix
   Description:
     [130475] - Trying toGenerate Evidence & update FW at the same time behavior mismatch SPEC define.
   Infected Motherboard: ALL
   Affected functions: Evidencne generatioin & download
   Validation:
     1) Manually recover BIOS and generate evidence afterwards
     2) Try to update BMC or BIOS FW and expected to see the error message

3. Category: Enhancement
   Description:
     [ENGINEERING] - Rollback ID alert is now a tooltip
   Infected Motherboard: RoT
   Affected functions: Firmware Update WEBUI
   Validation:
     1) Hover cursor over "Allow Rollback ID To Be Updated"

4. Category: Enhancement
   Description:
     [ENGINEERING] - Rollback ID checkbox for Motherboard CPLD should now be disabled when license is unactivated.
   Infected Motherboard: RoT
   Affected functions: Firmware Update WEBUI
   Validation:
     1) Under Motherboard CPLD, "Allow Rollback ID To Be Updated" checkbox should be disabled when license is unactivated.

5. Category: fix
   Description:
     [124514] - Number of Drives Displaying issues on Overview and Physical View tabs on Storage monitoring
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Storage page displays correct number of drives on summary page for each chart

6. Category: Fix
   Description:
     [130655] - AOC card Thermal reading issue w/ AOC-SLG3-2H8M2 on ipmiweb
   Infected Motherboard: ALL
   Affected Function: sensor, storage
   Validation:
     1) Install AOC-SLG3-2H8M2 on MB
     2) Check related sensor reading on IPMI web
     3) Check related sensor names, should be "AOC_SAS" + system slot + " Temp"
        and "AOC_SSD" + system slot + "Temp"

7. Category: fix
   Description:
     [130398] - FW Inventory Page Loading Unnecessary Buttons
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Firmware inventory page -> only bmc and bios show while loading, then
        rest of buttons will appear


--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.01.11
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210903_01.01.11_STDsp.bin
Production signed Firmware CRC: 49375A59
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210903_01.01.11_STDsp.bin
Production signed eMMC Firmware CRC: C6F9D21E
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210903_01.01.11_STDsp.bin
Production signed SPI NOR Firmware CRC: 3B8BB73E
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210903_01.01.11_STDsd.bin
Debug signed Firmware CRC: A4EA0474
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210903_01.01.11_STDsd.bin
Debug signed eMMC Firmware CRC: EAA4DD3A
Build Date: 09/03/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: fix
   Description:
     [130409] - Fan mode selection
     [130408] - Enable PWM 3 for controlling PSU fan
     [ENGINEERING] - Set default fan mode Optimal, and change "Smart" to "Smart Speed"
   Infected Motherboard: X12DPG-QR
   Affected functions: Web/redfish
   Validation:
     1) check FAN mode and make selection

2. Category: fix
   Description:
     [130040] - IPMI HWM Testing Fail for Vcpu1VCCIO & Vcpu2VCCIO
   Infected Motherboard: X12DPG-QR
   Affected functions: Web/redfish
   Validation:
     1) verify voltage difference between BMC reading and real value

3. Category: fix
   Description:
     [130406] - All GPU related sensor should be displayed on web GUI
   Infected Motherboard: X12DPG-QR
   Affected functions: Web/redfish
   Validation:
     1) Log into web -> sensor page, GPU sensors have drop down containing sub GPU sensors
     2) Get /redfish/v1/Chassis/1/Thermal

4. Category: Enhancement
   Description:
     [ENGINEERING] - Added querying stored rollback ID
   Infected Motherboard: ALL
   Affected functions: Firmware Resiliency
   Validation:
     1) Query Stored BMC Rollback ID: raw 0x30 0x68 0x28 0x08 0x0 0x4
     2) Query Stored BIOS Rollback ID: raw 0x30 0x68 0x28 0x08 0x1 0x4

5. Category: fix
   Description:
     [130402] - Front Panel red LED does not light up when fans are removed
     [130401] - No IPMI event log when fans are removed
   Infected Motherboard: X12DPG-QR
   Affected functions: Fan fail
   Validation:
     1) Remove one fan, in aroud 10 more seconds, error led will be blinking.
     1) Install this fan back in slot, in aroud 10 more seconds, error led will be turned off

6. Category: fix
   Description:
     [129892] - Incorrect PWS information
   Infected Motherboard: X12DPG-QR
   Affected functions: pminfo
   Validation:
     1) SMCIPMITool pminfo

7. Category: fix
   Description:
     [ENGINEERING] - BRCM3808 HDD detection error
     [ENGINEERING] - HDD blink/unblink need DCMS license.
   Infected Motherboard: ALL
   Affected functions: BRCM Storage.
   Validation:
     1) Log in Web.
     2) Storage/Physical View
     3) Check if HDD exist
     4) Check if Blink/Unblik works w/o license

8. Category: Fix
   Description:
     [129023] [IPMI ECO 01.01.05] Redfish automation tool check is fail
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) Get /redfish/v1/UpdateService/Oem/Supermicro/FirmwareInventory/HARAIDController.0 to check "Updateable"

9. Category: Fix
   Description:
    Updating BMC/BIOS Golden does not require DCMS license. GETing Rollback ID doesn't require DCMS license.
   Infected Motherboard: ALL
   Affected functions: Firmware Resiliency
   Validation:
    1) Update BMC/BIOS Golden without DCMS License. Should be allowed.
    2) Recover BMC/BIOS Golden without DCMS License is not allowed.
    3) GET /redfish/v1/UpdateService/Oem/Supermicro/RollbackID without DCMS License. Should be allowed.
    4) PATCH /redfish/v1/UpdateService/Oem/Supermicro/RollbackID without DCMS LICENSE is not allowed.

10. Category: fix
   Description:
     [129870] fix  - [QCL NVMe M.2] IPMI has NO storage monitoring tab/ no AOC_SSD temp sensor reading with AOC-SLG3-2H8M2
   Infected Motherboard: ALL
   Affected functions: BRCM Storage.
   Validation:
     1) Log in Web.
     2) Storage/Physical View and "Sensor Readings"/Sensor
     3) Check if Physical drives and AOC_SAS Temp exist.

11. Category: Fix
   Description:
     [ENGINEERING] - Firmware update checkboxes now work correctly
   Infected Motherboard: ALL
   Affected functions: Firmware Update
   Validation:
     1) Perform firmware update while selecting any options for that component.
     2) Options should work correctly.

--------------------------------------------------------------------------------------------------------------------------------------

Firmware Version: 01.01.10
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210827_01.01.10_STDsp.bin
Production signed Firmware CRC: CE6DFD95
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210827_01.01.10_STDsp.bin
Production signed eMMC Firmware CRC: 8310CB87
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210827_01.01.10_STDsp.bin
Production signed SPI NOR Firmware CRC: 3B8BB73E
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210827_01.01.10_STDsd.bin
Debug signed Firmware CRC: 116C44F1
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210827_01.01.10_STDsd.bin
Debug signed eMMC Firmware CRC: 9D9123EA
Build Date: 08/27/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.

1. Category: fix
   Description:
     [ENIGINEERING] - missing redfish/v1/Chassis/1/PCIeDevices/NVMeSSD[nvme_ssd_num]
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Get https://${BMC_IP}/redfish/v1/Chassis/1/PCIeDevices/NVMeSSD1

2. Category: fix
   Description:
     [124514] - number of SATA drives on Broadcom rectangle sometimes incorrect
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web -> storage page
     2) Broadcom square always show correct SATA drives

3. Category: Fix
   Description:
     [129898] - IKVM becomes abnormal after changing language from English to ????
   Infected Motherboard: ALL
   Affected functions: HTML5 KVM
   Validation:
     1) Log into web, change language to Simplified Chinese
     2) Run HTML5 KVM

4. Category: fix
   Description:
     [122497] - [SYS-220BT-HNC9R] ROM update for RAID controller and see "Update Failed ...."
   Infected Motherboard: ALL
   Affected functions: BRCM Storage.
   Validation:
     1) Log in Web.
     2) Maintenance/Firmware Management
     3) Choose SAS 39XX

5. Category: fix
   Description:
     [129921] - Users feature has Cross-site scripting issue when use specific payload
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Add user with "<script>alert(" as username
     3) After adding, delete user and no alert box should appear

6. Category: fix
   Description:
     [129947] - ECO -18441 -- 01.01.09? web storage controller tab not correct
   Infected Motherboard: ALL
   Affected functions: Web Storage.
   Validation:
     1) Log in Web.
     2) Check Storage/Controller tab string.

7. Category: Fix
   Description:
     [129862] - unable to modify boot option order via PATCH bios attributes
   Infected Motherboard: All
   Affected functions: Redfish
   Validation:
     1) Modify boot option order via PATCH bios attributes and send GET SD api to confrim the chagnes applied.

8. Category: Fix
   Description:
     [129023] - Redfish automation tool check is fail
   Infected Motherboard: All
   Affected functions: Redfish
   Validation:
     1) Redfish automation

9. Category: Fix
   Description:
     [129870] [QCL NVMe M.2] IPMI has NO storage monitoring tab / no AOC_SSD temp sensor reading with AOC-SLG3-2H8M2
   Infected Motherboard: X12DPT-PT6
   Affected functions: Sensor
   Validation:
     1) Install AOC-SLG3-2H8M2 then check AOC_SAS Temp reading

10. Category: Fix
   Description:
     [130137] - FAN sensor quantity not matches M/B's FAN-header #.
     [130039] - IPMI HWM Testing Fail for the CMOS Battery Part of the Test
     [129906] - WebGUI, No GPU information or sensor reading
     [129847] - FAN status is not showing in X12DPG-QR IPMI GUI
   Infected Motherboard: X12DPG-QR
   Affected functions: sensor
   Validation:
     1) verify sensor reading

--------------------------------------------------------------------------------------------------------------------------------------

Firmware Version: 01.01.09
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210817_01.01.09_STDsp.bin
Production signed Firmware CRC: 6B5B6BD4
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210817_01.01.09_STDsp.bin
Production signed eMMC Firmware CRC: 16358403
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210817_01.01.09_STDsp.bin
Production signed SPI NOR Firmware CRC: 05DFC643
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210817_01.01.09_STDsd.bin
Debug signed Firmware CRC: C6008701
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210817_01.01.09_STDsd.bin
Debug signed eMMC Firmware CRC: 7AEE39DF
Build Date: 08/17/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.

1. Category: Fix
   Description:
     [129490] - Power Supplies Event Log doesn't include number
   Infected Motherboard: ALL
   Affected functions: SEL
   Validation:
     1) SEL can show sensor name with "Power Supply Failure detected", "Power Supply input lost (AC/DC)" and "Power Supply Installed"

2. Category: Fix
   Description:
     [129533] - IPv6 network address not present on WEBGUI Dashboard
   Infected Motherboard: ALL
   Affected functions: WEBUI
   Validation:
     1) Enable IPV6 mode.
     2) Check WEBUI Dashboard host section will show IPv6 address

3. Category: fix
   Description:
     [129509] - BMC Storage Monitoring doesn't show green circle for user role
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web with user privilege
     2) Go to storage monitoring
     3) Overview and physical page should be displayed properly

4. Category: fix
   Description:
     [129660] - BIOS version string inappropriate
     [129056] - BIOS firmware version string is inappropriate
     [126242] - Redfish and Thermal automation test cannot run
   Infected Motherboard: ALL
   Affected functions: Web/redfish
   Validation:
     1) Check firmware inventory

5. Category: fix
   Description:
     [129629] - Storage Monitoring Overview page will cause BMC hang when keep the overview page for 3-5 mins
     [129053] - no confirmation message after performs fd/unit reset from web
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Factory reset, confirmation message appear before reset
     3) Storage page no longer redraws charts

6. Category: Fix
   Description:
     [129192] - IPMI web power consumption data is not correct
   Infected Motherboard: ALL
   Affected functions: Web, bbptask
   Validation:
     Testcase 1:
       1) Last week should record power consumption every 12 hours

7. Category: Fix
   Description:
     [129225] - IPMI IP will be changed when executing IPMI ECO automation test
   Infected Motherboard: X12DPT-PT6
   Affected functions: Network
   Validation:
     1) IP keep after run IPMI ECO test.

8. Category: Fix
   Description:
     [120938] - Generate Evidence can't update BIOS firmware message not match Spec define
   Affected functions: Evidence generation & download
   Validation:
     1) Manual recover BMC and/or BIOS
     2) Should be able to generate and download evidence afterwards

9. Category: Fix
   Description:
     [127576] - BIOS ECO SUM fail
   Affected functions: Recovery function & log
   Validation:
     1) Update BMC golden or backup with FW containing the fix
     2) Recover BMC and expected to see the logs once it finishes
        e.g. "Recovering the current [BMC] image initiated." as MEL
        e.g. "[BMC] successfully recovered from golden image - Assertion" as SEL

10. Category: fix
   Description:
     [124514] - Number of Drives Displaying issues on Overview and Physical View tabs on Storage monitoring
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Number of drives correct on all pages of storage monitoring

11.Category: Fix
  Description:
    [129404] - IPMI BIOS Recovery fail
  Infected Motherboard: ROT2.0
  Affected functions:  Recover BIOS Backup/Golden Now Works
  Validation:
    1) Make sure BIOS Backup/Golden are ver 1.1
    2) Make sure BIOS Active is 1.1a
    3) Navigate to "Platform Resiliency Actions" in Firmware Management web page.
    4) Perform the BIOS Recover action
    5) Check BIOS Active version and Maintenance Event Log to see if the recover action was successful

12. Category: fix
   Description:
     [129732] - System Temp, Peripheral Temp and NIC Temp show N/A
     [129731] - Power supply information not shows up in WEBUI
     [129728] - Sensor reading are uncompeted
     [129704] - IPMI missing sensors
   Infected Motherboard: X12DPG-QR
   Affected functions: Sensor and PSU
   Validation:
     1) Check sensor and PSU info

--------------------------------------------------------------------------------------------------------------------------------------

Firmware Version: 01.01.08
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210806_01.01.08_STDsp.bin
Production signed Firmware CRC: 248FD6E8
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210806_01.01.08_STDsp.bin
Production signed eMMC Firmware CRC: 1A585886
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210806_01.01.08_STDsp.bin
Production signed SPI NOR Firmware CRC: 50E2F30C
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210806_01.01.08_STDsd.bin
Debug signed Firmware CRC: 9868415D
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210806_01.01.08_STDsd.bin
Debug signed eMMC Firmware CRC: 6A029E24
Build Date: 08/06/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_latest_08282020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.


1. Category: Fix
   Description:
     [ENGINEERING] - SMSTC IPMIECO TS#102 - Checking IPMI configuration
   Infected Motherboard: ALL
   Affected functions: PS
   Validation:
     Testcase 1:
     1) Downgrade to v01.01.05
        ./sum -i ${BMC_IP} -u ${BMC_USR} -p ${BMC_PW} -c UpdateBMC --file v010105.bin --overwrite_cfg --overwrite_sdr
     2) Modify SMTP setting
     3) Upgrade firmware with preserved configuration
        ./sum -i ${BMC_IP} -u ${BMC_USR} -p ${BMC_PW} -c UpdateBMC --file BMC_firmware.bin

2. Category: fix
   Description:
     [129316] - [AST2600 A3] IPMIECO automation test failed staring on TC#260
   Infected Motherboard: Projects with RoT 1.0 solution
   Affected functions: CPLD FW update
   Validation:
     1) Update CPLD FW:
        e.g. sum -i 172.31.35.63 -u ADMIN -p ADMIN -c updatecpld --file debug_signed_cpld.bin --reboot
     2) Expected to work normally instead of seeing error message 'Sending packets timeout'

3. Category: fix
   Description:
     [127816] - It's empty when switch on "Multi Node" page (User Privilege)
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web with user and go to multi node page
     2) All clickable are disabled

4. Category: Fix
   Description:
     [128914] - Power consumption curves of "last day" and "last week" doesn't match highest peak value in IPMI webGUI.
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     Testcase 1:
     1) Run cburn test and make sure peak value is meet between "System Board Power Consumption Graph" and "Historical Trends"
     2) x axis display from now to -55m in "last hour"
     3) x axis display from now to -23h in "last day"
     4) x axis display from now to -6.5d in "last week"
     5) all average data should between max and min value

5. Category: fix
   Description:
     [128247] - Some of function still configurable when using "User" Privilege.
     [127831] - Component Info no translation to Japanese and Chinese simplified
     [127794] - Some of functions still configurable when usign "User" Privilege
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Component Info all translates correctly
     3) All password locks hidden for User

6. Category: fix
   Description:
     [129309] - No IPMI SEL log for HDD smart error.
   Infected Motherboard: ALL
   Affected functions: BRCM storage.
   Validation:
     1) Plug in the HDD with smart error.
     2) Check if HDD error SEL generated.

7.Category: Fix
  Description:
    [127996] - BiosRotManage UpdateGolden should not throw "Sending packets timeout"
  Infected Motherboard: ALL
  Affected functions: PFR
  Validation:
    1) Run "sum.exe -i <ip> -u <username> -p <password> -c BiosRotManage --action UpdateGolden"
    2) Should not throw "Sending packets timeout" error

8.Category: Enhancement
  Description:
    [127996] - Prompt to reboot system will show after updating NICs and Broadcom firmware
  Infected Motherboard: ALL
  Affected functions: Firmware Update
  Validation:
    1) Navigate to "Firmware Management" page.
    2) Update a NIC or Broadcom firmware
    3) Prompt will show at completion asking whether if user wants to reboot system or not

9. Category: fix
   Description:
     [127737] - Some of function still configurable when using "Operator" priviledge
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web -> auto focuses on username on login page
     2) Date_Time/port/ssdp/license pages are completely disabled for operator

--------------------------------------------------------------------------------------------------------------------------------------

Firmware Version: 01.01.07
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210728_01.01.07_STDsp.bin
Production signed Firmware CRC: 38AECACF
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210728_01.01.07_STDsp.bin
Production signed eMMC Firmware CRC: 2CA591CC
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210728_01.01.07_STDsp.bin
Production signed SPI NOR Firmware CRC: 50E2F30C
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210728_01.01.07_STDsd.bin
Debug signed Firmware CRC: 43B7B334
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210728_01.01.07_STDsd.bin
Debug signed eMMC Firmware CRC: 9B01B920
Build Date: 07/28/2021
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_latest_06112020
Supported Platform: X12DGQ-R, X12DPG-QR
---------------------------------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3.

1. Category: fix
   Description:
     [129054] - failed to save radius configuration from the web
     [129053] - no confirmation message after performs fd/unit reset from web
     [127816] - It's empty when switch on "Multi Node" page (User Privilege).
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) RADIUS configuration requires user to input secret password to continue
     3) Unit reset page displays "restarting bmc..." upon restart
     4) ADMIN/operator privilege has full multi node, but User can only see current node

2. Category: fix
   Description:
     [126200] - SUM update CPLD failed.
   Infected Motherboard: B12
   Affected functions: CPLD update
   Validation:
     1) e.g. sum -i 172.31.52.215 -u ADMIN -p ADMIN -c Updatecpld --file
        B12DPE-6_R100_F10FB200_20210402Ad.bin --reboot
     2) Expected to set everything works normally

3.Category: Fix
  Description:
    [128047] Fix - WebGUI/SMCIPMITool pminfo/IPMITool sdr should now show correctly when hot swapping PSU with host on
  Infected Motherboard: ALL
  Affected functions: Sensor Reading
  Validation:
    1) Turn on system (power on host).
    2) Navigate to PSU section of Sensor Readings on the web GUI.
    3) Hotswap PSU and check to see if readings are expected.
    4) Check SMCIPMITool pminfo as well to see if readings are expected.
    5) Check SMCIPMITool ipmi sdr as well to see if readings are expected.

4. Category: Fix
   Description:
     [All]Fix SSDP is not working sometimes.
   Infected Motherboard: ALL
   Validation:
     1) Enable SSDP in web.
     2) Scan nodes by SSDP tool.

5. Category: feature
   Description:
     [ENGINEER] feature - Support UFFN via redfish
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) Get /redfish/v1/UpdateService/FirmwareInventory/BMC to check UniqueFilename
     2) Get /redfish/v1/UpdateService/FirmwareInventory/BIOS to check UniqueFilename

6. Category: Fix
   Description:
     [129056] - BIOS firmware version string is inapprotiate
   Infected Mother Board: ALL
   Affected Function: N/A
   Validation:
     1) verify BIOS version word

---------------------------------------------------------------------------------------------------------------------------

Firmware Version: 01.01.06
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210724_01.01.06_STDsd.bin
Debug signed Firmware CRC: AD7E74EE
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210724_01.01.06__STDsp.bin
Production signed Firmware CRC: CCAB618D
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210724_01.01.06__STDsd.bin
Debug signed eMMC Firmware CRC: FF75A382
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210724_01.01.06__STDsp.bin
Production signed eMMC Firmware CRC: 521DE7F6
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210724_01.01.06__STDsp.bin
Production signed SPI NOR Firmware CRC: 50E2F30C
Build date: 07/24/2021
Supported Platform: X12DGQ-R, X12DPG-QR
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_latest_06112020
-------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3

1. Category: Fix
   Description:
     [127710] - Turn On/Off the "System Lockdown Mode" icon will not sync status with difference user.
     [128281] - Turn On/Off the "System Lockdown Mode" icon will not sync status with difference user.
   Infected Motherboard: All
   Affected functions: Web system lockdown
   Validation:
     1) Launch two browser(A/B connection) and login BMC WEB. Current system lockdown is disabled.
     2) Enable system lockdown on browser-A, the system-lockdown indicator shall be displayed on left-bottom of sidebar menu.
     3) Click "Refresh" button on browser-B, the system-lockdown indicator shall be displayed and subpage shall be not configurable.
     4) Enable system lockdown, click logout button shall be normal displayed "Login" page.

2. Category: Fix
   Description:
     [128484] - Inconsistent behavior when setting user name and password to the same (Add and modify)
   Validation:
     1) Create user username and password are same as "Tester001"
     2) Expecting: can't create user

3. Category: Fix
   Description:
     [ENGINEERING] - IKVM remote console show 0x3F8 control code after load factory default
   Infected Motherboard: ALL
   Affected Function: IKVM/SOL
   Validation:
     1) Launch HTML5 IKVM console and run IPMICFG –fd3 under UEFI shell
     2) After BMC reboot, launch HTML5 IKVM console, and press any key, the 3F8 control code will not be shown

4. Category: fix
   Description:
     [ENGINEERING] - Storage Monitoring page didn't show correct data
     [128439] - Keep showing "Configured-driver is rebuilding" in physical view after raid status in logical view returns to "Optimal" and found 3(expect 1) "HDD is rebuilding" event logs in web.
   Infected Motherboard: ALL with BRCM 3108
   Affected functions: BRCM 3108
   Validation :
     1) Install BRCM 3108 and two HDD
     2) Create RAID1
     3) Check logical view page and physical view page
     4) Delete RAID1
     5) Check logical view page and physical view page

5. Category: Fix
   Description:
     [ENGINEERING] - SNMP range and special char
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) SNMPv3 user name only allow 0-9a-zA-Z, Patch {"Snmpv3Enabled": true, "AuthProtocol": "MD5", "PrivateProtocol": "DES", "AuthKey": "Auth1234", "PrivateKey": "Private1234", "UserName": "Test1234_"} on /redfish/v1/Managers/1/Oem/Supermicro/SNMP/SNMPv3
     2) SNMPv3 user name max is 32, Patch {"Snmpv3Enabled": true, "AuthProtocol": "MD5", "PrivateProtocol": "DES", "AuthKey": "Auth1234", "PrivateKey": "Private1234", "UserName": "Test123456789012345678901234567890"} on /redfish/v1/Managers/1/Oem/Supermicro/SNMP/SNMPv3
     3) SNMPv3 Auth Key only allow 0-9a-zA-Z and at leat one number, one lower and one upper, Patch {"Snmpv3Enabled": true, "AuthProtocol": "MD5", "PrivateProtocol": "DES", "AuthKey": "Auth1234", "PrivateKey": "Private1234", "UserName": "Test1234"} on /redfish/v1/Managers/1/Oem/Supermicro/SNMP/SNMPv3
     4) SNMPv3 Auth Key only allow 0-9a-zA-Z and at leat one number, one lower and one upper, Patch {"Snmpv3Enabled": true, "AuthProtocol": "MD5", "PrivateProtocol": "DES", "AuthKey": "auth1234", "PrivateKey": "Private1234", "UserName": "Test1234"} on /redfish/v1/Managers/1/Oem/Supermicro/SNMP/SNMPv3
     5) SNMPv3 Auth Key max is 64, Patch {"Snmpv3Enabled": true, "AuthProtocol": "MD5", "PrivateProtocol": "DES", "AuthKey": "Auth1234567890123456789012345678901234567890123456789012345678901", "PrivateKey": "Private1234", "UserName": "Test1234"} on /redfish/v1/Managers/1/Oem/Supermicro/SNMP/SNMPv3
     6) SNMPv3 Prive Key only allow 0-9a-zA-Z and at leat one number, one lower and one upper, Patch {"Snmpv3Enabled": true, "AuthProtocol": "MD5", "PrivateProtocol": "DES", "AuthKey": "Auth1234", "PrivateKey": "Private1234", "UserName": "Test1234"} on /redfish/v1/Managers/1/Oem/Supermicro/SNMP/SNMPv3
     7) SNMPv3 Prive Key only allow 0-9a-zA-Z and at leat one number, one lower and one upper, Patch {"Snmpv3Enabled": true, "AuthProtocol": "MD5", "PrivateProtocol": "DES", "AuthKey": "Auth1234", "PrivateKey": "private1234", "UserName": "Test1234"} on /redfish/v1/Managers/1/Oem/Supermicro/SNMP/SNMPv3
     8) SNMPv3 Prive Key max is 64, Patch {"Snmpv3Enabled": true, "AuthProtocol": "MD5", "PrivateProtocol": "DES", "AuthKey": "Auth1234", "PrivateKey": "Private123456789012345678901234567890123456789012345678901234567890", "UserName": "Test1234"} on /redfish/v1/Managers/1/Oem/Supermicro/SNMP/SNMPv3
     9) SNMPv3 user name only allow 0-9a-zA-Z, ipmi raw 30 68 19 01 01 0a 31 32 33 34 35 36 37 38 39 30
     10) SNMPv3 user name max is 32, ipmi raw 30 68 19 01 01 21 31 32 33 34 35 36 37 38 39 30 31 32 33 34 35 36 37 38 39 30 31 32 33 34 35 36 37 38 39 30 31 32 33
     11) SNMPv3 Auth Key only allow 0-9a-zA-Z and at leat one number, one lower and one upper, ipmi raw 30 68 19 01 04 16 31 32 33 34 35 36 37 38 39 30 31 32 33 34 35 36 37 38 39 30 41 62
     12) SNMPv3 Auth Key only allow 0-9a-zA-Z and at leat one number, one lower and one upper, ipmi raw 30 68 19 01 04 16 31 32 33 34 35 36 37 38 39 30 31 32 33 34 35 36 37 38 39 30 41 42
     13) SNMPv3 Auth Key max is 64, ipmi raw 30 68 19 01 04 41 31 32 33 34 35 36 37 38 39 30 31 32 33 34 35 36 37 38 39 30 31 32 33 34 35 36 37 38 39 30 31 32 33 34 35 36 37 38 39 30 31 32 33 34 35 36 37 38 39 30 31 32 33 34 35 36 37 38 39 30 41 42 43 44 45
     14) SNMPv3 Prive Key only allow 0-9a-zA-Z and at leat one number, one lower and one upper, ipmi raw 30 68 19 01 05 16 31 32 33 34 35 36 37 38 39 30 31 32 33 34 35 36 37 38 39 30 43 64
     15) SNMPv3 Prive Key only allow 0-9a-zA-Z and at leat one number, one lower and one upper, ipmi raw 30 68 19 01 05 16 31 32 33 34 35 36 37 38 39 30 31 32 33 34 35 36 37 38 39 30 43 44
     16) SNMPv3 Prive Key max is 64, ipmi raw 30 68 19 01 05 41 31 32 33 34 35 36 37 38 39 30 31 32 33 34 35 36 37 38 39 30 31 32 33 34 35 36 37 38 39 30 31 32 33 34 35 36 37 38 39 30 31 32 33 34 35 36 37 38 39 30 31 32 33 34 35 36 37 38 39 30 41 42 43 44 45

6. Category: Fix
   Description:
     [128999] - IPV4 static subnet mask format always failed
   Infected Motherboard: ALL
   Affected functions: WebUI Network config
   Validation :
     1) check IPV4 static subnet mask in WEBUI network configuration.

7. Category: Fix
   Description:
     [ENGINEERING] - 0x30 0x68 0x28 0x06 0x01 command can't get stage/backup/golden BIOS revision
   Infected Motherboard: All
   Affected functions: BIOS revision
   Validation :
     1) Run 0x30 0x68 0x28 0x06 0x01 0x00 to get stage BIOS revision
     2) Run 0x30 0x68 0x28 0x06 0x01 0x01 to get backup BIOS revision
     3) Run 0x30 0x68 0x28 0x06 0x01 0x02 to get golden BIOS revision

8. Category: Fix
   Description:
     [126644] - The vendor model name of GPU info page shows incorrect data.
   Infected Motherboard: ALL
   Affected Function: WEB
   Validation:
     1) Install GPU on system.
     2) Login BMC WEB -> [Component Info] -> [GPU] to check GPU information is correct or not.

9. Category: new
   Description:
     [ENGINEERING] - support network AOC FW update.
   Infected Motherboard: ALL
   Affected functions: Network AOC FW update.
   Validation:
     1) Update network AOC FW by redfish.

10. Category: fix
    Description:
      [128485] - "required" overlapped when mounting CD-ROM image
      [127848] - Tips in line feed for Japanese/Chinese not complete
      [124514] - Number of drives displaying issues on overview/physical incorrect
    Infected Motherboard: ALL
    Affected functions: Web
    Validation:
      1) Log into web -> go to VM
      2) click select file and cancel, then mount CD-ROM and required messaged should be hidden
      3) add new user in Japanese and Chinese same as English
      4) storage should load all drives, physical and logical drive

11.Category: Fix
   Description:
     [ENGINEERING] - Cannot get current rollback ID setting from BMC
   Infected Motherboard: ALL
   Affected Function: WEB
   Validation:
     1) Check all related items on [Firmware Management]-> [Update] page.

12.Category: Fix
   Description:
     [ENGINEERING] - The battery module has been plugged but the battery status is "Not Install".
   Infected Motherboard: All
   Affected functions: Storage BBU
   Validation:
     Current status is battery module plugged-in.
     1) AC off -> on, until it show "Not Install" or "Optimal" on Storage Monitoring\Controller\Broadcom Storage Controller page.
        Check BBU shall be no log displayed on Health Event log and BBU status is "Optimal".
     2) Please remove battery Module and AC ON.
        Check BBU shall be displayed "BBU DeAssertion" on Health Event log and BBU status is "Not Install".
     3) DC off->on
        Check BBU shall be no log displayed on Health Event log and BBU status is "Not Install".
     4) Please plug-in battery module and AC ON.
        Check BBU shall be displayed "BBU Assertion" on Health Event Log and BBU status is "Optimal".

13.Category: fix
   Description:
     [ENGINEERING] - enhancement BIOS golden update
   Infected Motherboard: Projects with RoT 1
   Affected functions: CPLD update
   Validation:
     1) Update BIOS golden through web page, should be ok

14.Category: fix
   Description:
     [127576] - BIOS ECO SUM fail
   Infected Motherboard: Projects with RoT 1
   Affected functions: CPLD update
   Validation:
     1) Update CPLD FW through web page, should be ok
     2) Update CPLD FW through in-band SUM when host is on, should be ok
     3) Update CPLD FW through in-band SUM when host is down, should be ok
     4) Update CPLD FW through out-band SUM when host is on, should be ok
     5) Update CPLD FW through out-band SUM when host is down, should be ok

15.Category: Fix
   Description:
     [128683] - Session timeout should not occur when failing multiple verifications.
   Infected Motherboard: ALL
   Affected functions: Firmware Update
   Validation:
     1) Navigate to Firmware Management page
     2) Upload an invalid BMC firmware
     3) Watch it fail multiple times. It should not cause session timeout.

16.Category: Fix
   Description:
     [ENGINEERING] - update raid controller by old method fail
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) install 3108 card
     2) Get redfish/v1/UpdateService/Oem/Supermicro/FirmwareInventory/HARAIDController.0
     3) Post /redfish/v1/UpdateService/Oem/Supermicro/FirmwareInventory/HARAIDController.0/Actions/SmcFirmwareInventory.EnterUpdateMode
     4) Post /redfish/v1/UpdateService/Oem/Supermicro/FirmwareInventory/HARAIDController.0/Actions/SmcFirmwareInventory.Upload
     5) Post /redfish/v1/UpdateService/Oem/Supermicro/FirmwareInventory/HARAIDController.0/Actions/SmcFirmwareInventory.Update
     6) Post /redfish/v1/UpdateService/Oem/Supermicro/FirmwareInventory/HARAIDController.0/Actions/SmcFirmwareInventory.Cancel

17.Category: enhancement
   Description:
     [ENGINEERING] - sometimes BMC WEBUI logout immediately after login BMC WEBUI
   Validation:
     1) login BMC WEBUI successfully. 

18.Category: new
   Description:
     [ENGINEERING] - support staged BIOS update
   Infected Motherboard: All with RoT
   Affected functions: BIOS update
   Validation :
     1) Log in WebUI. Go to the Firmware Management page.
     2) Choose BIOS.
     3) There is a option for users to select either "Update on next boot" or "Immediate Update"
     4) If users choose "Immediate Update", the following flow is as before.
       - system power off -> upload BIOS image -> Verify image -> Update
     5) If users choose "Update on next boot", the following flow is as below.
        upload BIOS image -> Verify image.
     6) After the Step 5, users can do one of the followings.
       - Cancel this update.
       - Perform a system reset(power cycle reset/power reset/warm reset) to trigger the BIOS update.
       - Do other FW update such as BMC,CPLD, etc.

19.Category: Fix
   Description:
     [ENGINEERING] - SATC AD test case fail
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) run Account Service on SATC

20.Category: Enhancement
   Description: 
     [ENGINEERING] - Upgrade dropbear to version 2019.78
   Infected Motherboard: X12
   Affected functions: SSH
   Validation:
      1) SSH to BMC and use command "cd" and "show"

21.Category: Fix
   Description:
     [128957] - PUE2 fan mode should be eliminated
   Infected MotherBoard: X12DGQ-R
   Affected Function: fan mode
   Validation:
     1) check fan mode.

----------------------------------------------------------------------------------------------------------

Firmware Version: 01.01.05
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210715_01.01.05_STDsd.bin
Debug signed Firmware CRC: 7439E13E
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210715_01.01.05_STDsp.bin
Production signed Firmware CRC: F373D47E
Debug signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210715_01.01.05_STDsd.bin
Debug signed eMMC Firmware CRC: 3C78A88D
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210715_01.01.05_STDsp.bin
Production signed eMMC Firmware CRC: 778FCCDA
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210715_01.01.05_STDsp.bin
Production signed SPI NOR Firmware CRC: 50E2F30C
Build date: 07/15/2021
Supported Platform: X12DGQ-R, X12DPG-QR
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_latest_06112020
-------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3

1. Category: fix
   Description:
     [ENGINEERING] - Fix BMC Web hang when get network AOC information issue
   Infected Mother Board: ALL
   Affected Function: AOC Network card information
   Validation:
     1) Plug AOC network LAN card on Riser
     2) Login BMC WEB and check AOC network information is correct.

2. Category: fix
   Description:
     [128678] - IPMI show N/A on AOC-card Temp reading
   Infected Motherboard: ALL
   Affected functions: AOC Network Temperature
   Validation :
     1) Login Webpage and check Components-> AOC Network Temperature reading.
     2) GET /redfish/v1/Chassis/1/Thermal and find odata.id of AOC temperature
     3) GET /redfish/v1/Chassis/1/PCIeDevices/NICx and check NIC information match the sensor name.

3. Category: fix
   Description:
     [128332] - Sensor reading can not be detected "AOC_NICI_Temp" when attach AOC-S25GC-i4S card
   Infected Motherboard: ALL
   Validation:
     1) Install AOC-S25GC-I4S and AOC-AH25G-m2S2TM
     2) Check sensor reading and Network AOC page

4. Category: fix
   Description:
     [ENGINEERING] - No AIOM Card BMC should not generate AION sensor
   Infected Motherboard: ALL
   Affected functions: AIOM Sensor
   Validation :
     1) no AIOM card, No AIOM Sensor

5. Category: fix
   Description:
     [127628] - Save Success Messages For Web UI Inconsistent
   Infected Motherboard: ALL
   Affected functions: WEBUI
   Validation:
     1) Log into web
     2) Save any function, save message consistent and same

6. Category: fix
   Description:
     [128243] - Some of function still configurable when using "Operator" Privilege
   Infected Motherboard: ALL
   Affected functions: WEBUI
   Validation:
     1) Log into web
     2) RADIUS/Syslog/SMTP/SSDP/Date_Time/License pages should not be clickable under Operator

7. Category: fix
   Description:
     [128439] - Keep showing "Configured-driver is rebuilding" in physical view after raid status
               in logical view returns to "Optimal" and found 3(expect 1) "HDD is rebuilding" event logs in web.
   Infected Motherboard: ALL
   Affected functions: BRCM storage rebuild SEL.
   Validation:
     1) Create RAID on slot0 and slot2. =>Power OFF system.
     2) Remove 1HDD -> Power ON system ->  Raid status shows "Degraded" in Logical view page -> Power OFF system.
     3) Re-plug in 1HDD -> System start rebuilding.
     4) After some time(3 hours),Raid status shows "Optimal" in Logical view page.
     5) Check Physical view status and event log.

8. Category: fix
   Description:
     [128249] - IPMI event log will null when event log add to 4096
   Infected Motherboard: ALL
   Affected functions: WEBUI
   Validation:
     Testcase 1:
       1) run  ipmitool.exe -I lanplus -H {{IP}} -U ADMIN -P ADMIN event 1 for 4096 times
       2) goto System > Health Event Log should show all 4096 records.

9. Category: fix
   Description:
     [126782] - page unresponsive when VM with bad file name
   Infected Motherboard: All
   Affected functions: WEBUI
   Validation:
     1) input VM with bad file name. page is alive still

10.Category: fix
   Description:
     [128321] - IPMIECO Automation test failed with 13 failures.
   Infected Motherboard: ALL
   Affected functions: SEL
       1) Run ipmieco testcase 124 pass

11.Category: fix
   Description:
     [128399] - Can not connect to IPMI Web using "http://IP:81 when web port 81 is ON.
   Infected Motherboard: ALL
   Affected functions: WEBUI
   Validation:
     1) change web port to 81
     2) case 1)  http://IP
        case 2)  http://IP:81
        case 3)  https://IP
        case 4)  https://IP:443
        case 5)  IP
        above cases, it should auto-redirect to https://IP successfully.

12.Category: fix
   Description:
     [ENGINEERING] - The Battery status shall be displayed "Prohibit" icon when RAID card does not support battery module.
     [128336] - Storage Monitoring - battery status error.
   Infected Motherboard: ALL
   Affected functions: Storage, BBU
   Validation:
     1) Check battery status on storage monitoring overview page
        3108 with battery module, here shall be according battery status to displayedn Green/Red icon, show Prohibit icon before controller stable.
        3108 w/o battery module, here shall be show Prohibit icon.
        3008 w/o battery module, here shall be show Prohibit icon.
     2) Check health event log
        Power-On and 3108 with battery, the battery status is Optimal.
        AC-OFF, remove the battery module and AC-ON, there shall be displayed Message "OEM BBU presence (StorageController 0) - DeAssertion".
        DC-OFF and DC-ON, there shall be no battery message displayed.
        AC-OFF, install the battery module, AC-ON, there shall be displayed Message "OEM BBU presence (StorageController 0) - Assertion".
        DC-OFF and DC-ON, there shall be no battery message displayed.

13.Category: fix
   Description:
     [ENGINEERING] - PFR Action Buttons Behavior Changed from show/hide to disable/enable
   Infected Motherboard: ALL
   Affected functions: PFR
   Validation:
     1) Navigate to Firmware Inventory page.
     2) Select "Platform Resiliency Actions"
     3) "Recover" and "Update" buttons are disabled by default
     4) Selecting BIOS or BMC will make "Recover" button enabled.
     5) Selecting BIOS Golden or BMC Golden will make "Update" button enabled.
     6) Unchecking image will disable buttons.

14.Category: fix
   Description:
     [127831] - Component information no translation to Japanese and Chinese simplified
     [127832] - DDNS/IPMI/License Activation "Select Files" button no translation to Japanese and Chinese simplified.
     [127811] - Help content no "Multi Node" related information.
   Infected Motherboard: ALL
   Affected functions: WEBUI
   Validation:
     1) Log into web
     2) go to all component info -> translate all pages
     3) go to all pages with "select file" -> should be translated
     4) help page has multi node information

15.Category: fix
   Description:
     [128423] - After disabling NTP, the NTP Enable switch position moves to On and the "On/Off" string disappears
   Infected Motherboard: All
   Affected functions: WEBUI
   Validation:
     1) disable NTP, and check NTP status when stress switching NTP webpage here and there

16.Category: fix
   Description:
     [128063] - change "System Lockdown" (either On to off or Off to On), the web page will be logged out.
   Infected Motherboard: All
   Affected functions: Web system lockdown
   Validation:
     1) Login BMC WEB by Chrome.
     2) Enable system lockdown.
     3) The dashboard page shall be displayed with indicator.
     4) Disable system lockdown.
     5) The dashboard page shall be displayed without indicator.

17.Category: fix
  Description:
    [ENGINEERING] - Filenames now should not affect verification
  Infected Motherboard: ALL
  Affected functions: Firmware Update
  Validation:
    1) Use an X12DPG-OA6 board, since this is where the issue was seen.
    2) POST /redfish/v1/UpdateService/Oem/Supermicro/FirmwareInventory/BMC/Actions/SmcFirmwareInventory.EnterUpdateMode
    3) POST /redfish/v1/UpdateService/Oem/Supermicro/FirmwareInventory/BMC/Actions/SmcFirmwareInventory.Upload
       Use BMC firmware: BMC_X12DPGOA6-ROT-6202MS_20210627_01.01.03_STDsd.bin
    4) This procedure should pass verification and go on to update successfully.

18.Category: fix
   Description:
     [ENGINEERING] - no health when no linkup with TAS
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) run TAS and unplug system lan port
     2) Get /redfish/v1/Systems/1/EthernetInterfaces/1

19.Category: fix
   Description:
     [ENGINEER] - NetworkDeviceFunctions collection count 0 and NetworkDeviceFunctions shows mac garbled
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) Get /redfish/v1/Chassis/1/NetworkAdapters/1/NetworkDeviceFunctions
     2) Get /redfish/v1/Chassis/1/NetworkAdapters/1/NetworkDeviceFunctions/1

20.Category: fix
   Description:
     [124397] - Test fail via smstc
   Infected Motherboard: All
   Affected functions: BIOS golden update
   Validation:
     1) Update BIOS golden through web page
     2) Expected to see system powering up automatically afterwards

21. Category: fix
   Description:
     [128004] - PSU Page Extended Info Will Automatically minimize
   Infected Motherboard: ALL
   Affected functions: WEBUI
   Validation:
     1) Log into web
     2) PSU page, open and close detail of PSU

22. Category: fix
   Description:
     [127163] - COM2 console redirection connect fail
   Infected MotherBoard: All
   Affected Functions: SOL
   Validation:
     1) Use latest BIOS BMC to verify this issue.
     2) Disable COM1 and Enable COM2 from BIOS setup menu
     3) Verify console redirection function.

23. Category: Fix
   Description:
     [ENGINEERING] initial X12DPG-QR 
   Infected Motherboard: X12DPG-QR
   Affected functions: N/A
   Validation :
      1) Check BMC info
      2) Check sensor

24. Category: fix
   Description:
     [ENGINEERING] - Rollback ID mechanism enhancement
   Infected Motherboard: RoT 20 Projects
   Affected functions: Rollback ID mechanism
   Validation:
     1) Remove or decrease rollback ID of BIOS
     2) Update BIOS
     3) Expected to see BMC reset and golden update

25. Category: fix
   Description:
     [ENGINEERING] - fix factory default issue & a few others
   Infected Motherboard: ROT 2.0
   Affected functions: upload, staging, inventory, datablk
   Validation:
     1) Try Update/update_w_back/generate_golden
     2) Expect to see the inventory reflecting the correct information
     3) verify UID to reset BMC.
     4) verify UID to reset default BMC

--------------------------------------------------------------------------------------------------------
Firmware Version: 01.01.04
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210702_01.01.04_STDsd.bin
Debug signed Firmware CRC: FD5A8FF1
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210702_01.01.04_STDsp.bin
Production signed Firmware CRC: 17479CEF
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210702_01.01.04_STDsp.bin
Production signed eMMC Firmware CRC: 989BD7AE
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210702_01.01.04_STDsp.bin
Production signed SPI NOR Firmware CRC: C1DCC285
Build date: 07/02/2021
Supported Platform: X12DGQ-R
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_latest_06112020
-------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3

1. Category: fix
   Description:
     [128081] - AIOM 1G(AOC-AG-i2M) should not has sensor
   Infected Motherboard: ALL
   Affected functions: Sensor reading.
   Validation:
     1) Install AIOM: AOC-AG-i2M Rev: 1.01*1
     2) Web log in system
     3) Check NO AIOM sensor on Web GUI

2. Category: fix
   Description:
     [125179] - IPMI WebUI is not responsive
     [127207] - After disabling the FIFO, I can still receive logs when the log is full (512 logs)
     [128249] - [IPMI_ECO_01.01.03] IPMI event log will null when event log add to 4096
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Add SEL until 4096 records
     2) Goto System > Health event log
     3) web should not hang

3. Category: fix
   Description:
     [128292] - Turn On "Virtual Media Port" first will return Opps error
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Cannot turn on "Virtual Media Port" first if "IKVM Server Port" is OFF.

4. Category: fix
   Description:
     [128228] - 1.01.03 won't able to enable Dynamic DNS in setting process.
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) enabled DDNS and save successfuly.

5. Category: fix
   Description:
     [128000] - Component Info Spelling Issues
   Infected Motherboard: ALL
   Affected functions: Component Info
   Validation:
     1) Check Components Network AOC Serial Number wording.
     2) Check Components FAN Thresholds wording.

6. Category: fix
   Description:
     [128261] - Using full-width characters when added or modify user name will return error
     [128264] - Input full-width characters at user password will return unmatch hit message
   Infected Motherboard: ALL
   Affected functions: WEBUI
   Validation:
     1) Using full-width characters to add user and password, you will check error message "Please use Half-Width characters"

7. Category: fix
   Description:
     [128255] - HDD rebuilding had too much log on web
   Infected Motherboard: ALL
   Affected functions: BRCM storage rebuild SEL.
   Validation:
     1) Create RAID on slot0 and slot2.
     2) Swap slot2 HDD with a another empty HDD.
     3) Check if rebuild SEL will keep creating or not.

8. Category: fix
   Description:
     [128213] - DNS Server2 IP default value is not correct
     [128212] - DNS Server IP / DNS Server2 IP couldn't configurable on Network page
     [ENGINEERING] - Enhance IPV4 static netmask input validation
   Infected Motherboard: ALL
   Affected functions:DNS
   Validation:
     1) IPv4 DNS Server IP / DNS Server2 IP can be configuarable if lockdown is not set
     2) IPv4 DNS Server2 IP default IP is empty
     3) Set IPv4 static netmask 255.255.255.0, WEBUI validation will be passed.
     4) Set IPv4 static netmask 1.2.3.4, WEBUI validation will be error.

9. Category: fix
   Description:
     [127576] - BIOS ECO SUM fail
   Infected Motherboard: PFR-ROT2.0 boards
   Affected functions: BIOS Update
   Validation:
     1) Use SUM to issue two times BIOS update when System power off.

10.Category: New
   Description:
    [ENGINEERING]- AntiRollback Feature
  Infected Motherboard: ROT 2.0
  Affected functions: AntiRollback
  Validation:
    1) Update BMC, BIOS, or Motherboard CPLD with a higher rollback ID.
       If rollback ID needs to be updated, BMC will reboot.
    2) Upload BMC, BIOS, or Motherboard CPLD file with a lower rollback
       ID. It should be blocked.
    3) Check the event log for rollback ID update success message.
---------------------------------------------------------------------------------------------------------------------

Firmware Version: 01.01.03
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210627_01.01.03_STDsd.bin
Debug signed Firmware CRC: 76962524
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210627_01.01.03_STDsp.bin
Production signed Firmware CRC: BAF8F85C
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210627_01.01.03_STDsp.bin
Production signed eMMC Firmware CRC: 5072E496
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210627_01.01.03_STDsp.bin
Production signed SPI NOR Firmware CRC: C1DCC285
Build date: 06/27/2021
Supported Platform: X12DGQ-R
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_latest_06112020
-------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3

1. Category: new
   Description:
     [ENGINEERING] - add one more byte in raw 0x30 0x68 0xE0 0x00
   Infected Motherboard: ALL
   Affected functions: SUM detect post complete
   Validation:
     1) ipmitool raw 0x30 0x68 0xE0 0x00 return 4 bytes.
        byte 1: complete code
        byte 2-3: set post status by BIOS if KCS enabled.
        byte 4: post complete GPIO pin status. 1 for bios post complete, 0 for not bios  post

2. Category: fix
   Description:
     [ENGINEERING] - update LCMC improvement
   Infected Motherboard: X12DPT-PT6
   Affected functions: LCMC update
   Validation:
     1) update LCMC FW via web

3. Category: fix
   Description:
     [127436] - IPMI event log will null when event log add to 4096
     [127523] - Health Event Log page will hang in reading process when create over then 4096 events.
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web -> SEL
     2) SEL Entries load quickly, and 50 entries or less shown
     3) Download excel will download all entries

4. Category: fix
   Description:
     [127935] - [ECO]event log error when rebuild HDD slot2.
   Infected Motherboard: ALL
   Affected functions: BRCM3108
   Validation:
     1) Create RAID on slot0 and slot2.
     2) Swap slot2 HDD with a another empty HDD.
     3) Check if SEL has a rebuild message on PD slot2.

5. Category: fix
   Description:
     [128000] - Component Info Spelling Issues
   Infected Motherboard: ALL
   Affected functions: Component Info
   Validation:
     1) Check Components Information Serial Number wording.
     2) Check Components Board Info Serial Number wording.
     3) Check Components Sensor Thresholds wording.

6. Category: fix
   Description:
     [ENGINEERING] - PSU status wrong error if system is powered off and PSU with power cord
   Infected Motherboard: ALL
   Affected functions: PSU and System status
   Validation:
     1) Power on system, the PSU with power cord should be status normal, the PSU without power cord should be status error
     2) Power off system, the PSU with power cord should be status normal, the PSU without power cord should be status error

7. Category: fix
   Description:
     [ENGINEERING] - support maximum 4 Mellanox card
   Infected Motherboard: ALL
   Affected functions: Mellanox card sensor
   Validation:
     1) install 4 Mellanox card and check sensor reading.

8. Category: fix
   Description:
     [127937] - Selected protocol (SHA96/AES128) will not save at SNMPv3(Alert)
   Infected Motherboard: All
   Affected functions: Web (Notifications - Alerts )
   Validation :
    1) Login BMC GUI Web and select sidebar: Configuration -> Notifications -> Alerts -> Modify Alert
    2) Protocol : SNMPv3, input below information and make selection:
      Destination Address: 10.132.160.93
      User Name: ErinC
      Authentication Key: AaBb1234567890
      Authentication Protocol: SHA96
      Encryption Key: Key: AaBb1234567890
      Encryption Protocol: AES128
    3) Click on Save
    4) Check result. Authentication protocol should be SHA96. Encryption Protocol should be AES128

9. Category: fix
   Description:
     [127940] - "Message" field not match on "Alerts" page when protocol is "Redfish".
   Infected Motherboard: All
   Affected functions: Web (Notifications - Alerts )
   Validation :
     1) Login BMC GUI Web and select sidebar: Configuration -> Notifications -> Alerts -> Modify Alert (Enable)
     2) Protocol : Redfish
     3) Destination Address field, typing https://smc.com:443
     4) Message field, input H12 Test Message
     5) Save and return to Alerts page
     6) Check the title of Alert info is "Message", not "Context"

10.Category: fix
   Description:
     [ENGINEERING] - SOL cannot be disabled issue.
   Infected Motherboard: ALL
   Affected functions: SOL
   Validation:
     1) Run OEM command 30 70 06 01 to disable SOL, then check SOL function.
     2) Run OEM command 30 70 06 03 to enable SOL, then check SOL function.

11.Category: Fix
   Description:
    [126848] - Chassis Intrusion status will be de-asserted automatically after it’s triggered
   Infected Motherboard: ALL
   Affected functions: Sensor
   Validation:
    1) Trigger chassis intrusion.
    2) Check sensor status on web, its status should be "Hardware Intrusion"
    3) Click [Intrusion Reset] button on WEB, it will be de-asserted.

12.Category: Fix
   Description:
     [126893] - Cannot find BBU status in IPMI storage monitoring overview page
   Infected Motherboard: H12SSFF-AN6
   Affected functions: Web system lockdown
   Validation:
     1) check battery status on storage monitoring overview page.
        Display status_red.png when battery status is "Missing", "Needs To Be Replaced" or "Voltage Low".
        Display status_green.png when battery status is "Charging", "Discharging" or "Optimal".
        Display status_grey.png when battery status does not exist.

13.Category: fix
   Description:
     [126803] - Web Session timeout fail.
   Infected Motherboard: X12 , H12
   Affected functions: Web
   Validation:
     1) IPMI Web -> Configuration -> BMC Settings -> Web Session
     2) Set Session Timeout Value to 1 and then save.
     3) After 1 minute, the system will logout automatically.
     4) Login and repeat 1)
     5) Set Session Timeout Value to 3 and then save.
     6) After 3 minutes, the system will logout automatically.

14.Category: fix
   Description:
     [127149] - PWS sensor reading
   Infected Motherboard: ALL
   Affected functions: WEBUI components
   Validation:
     1) Make PSU and FAN fail
     2) Check WEBUI components PSU status should show error, FAN status should show error, sensor status should show normal

15.Category: fix
   Description:
     [ENGINEERING] - no host interface after BMC factory default
   Infected Motherboard: All
   Affected functions: Host interface
   Validation:
     1) Run factory default
     2) AC on or reboot host
     3) Check BMC web if can show CPU information

16.Category: fix
   Description:
     [126860] - IP Access Control, DDNS, Syslog, Time Zone, and NTP Server can be edited after lockdown the system.
     [127336][127701] - Some of function still configurable at System lockdown Mode.
     [127737][127794] - Some of function still configurable when using "Operator" and "User" Privilege.
   Infected Motherboard: ALL
   Affected functions: Web system lockdown
   Validation:
     1) Enable IP Access Control, DDNS, Syslog, Time Zone, Virtual Media, SMTP and NTP Server, the functions shall be configurable.
     2) Lockdown system.
     3) Check the components shall be disabled on Radius user, update firmware, Virtual CD-ROM, Web port, Date and Time, DDNS, IP Access Control, Syslog pages.

17.Category: fix
   Description:
     [ENGINEERING] - Sometimes cannot got IP during lan interface switch from share to failover
   Infected Motherboard: X12DPT-PT6
   Affected functions: Lan Interface
   Validation:
     1) ipmi oem lani 1 switch to share then check connection
     2) ipmi oem lani 2 switch to failover then check connection

18.Category: fix
   Description:
     [127966] - Fail to enable SNMPv3 when special characters include username
   Infected Motherboard: ALL
   Affected functions: SNMP page
   Validation:
     1) change SNMPV3 username through WEBUI
     2) change SNMPv2 community through WEBUI
     3) use SMCIPMITool to change SNMPV3 username
     4) use SMCIPMITool to change SNMPV2 community

19.Category: fix
   Description:
     [ENGINEERING] - show output current as wrong small value on WEBUI PSU page if PSU output current is over 65A
   Infected Motherboard: X12, H12
   Affected functions: PSU page info
   Validation:
     1) make PSU output current is over 65A or more
     2) check PSU output current info in PSU WEBUI page

20.Category: fix
   Description:
     [127213] - The NTP time doesn't sync after updating the BIOS
   Infected Motherboard: All
   Affected functions: NTP/ME
   Validation:
     1) Sync time with NTP Server
     2) Update BIOS firmware
     3) Check system time should sync with NTP time

21.Category: fix
   Description:
     [ENGINEERING] -  wrong relative link on UpdateService/FirmwareInventory/Broadcom1
   Infected Motherboard: All
   Affected functions: Redfish
   Validation:
     1)  install 3216 card then Get /redfish/v1/UpdateService/FirmwareInventory/Broadcom1
     2) "Related Item" should be "/redfish/v1/Systems/1/Storage/HBA#/StorageControllers/0"

22.Category: fix
   Description:
     [127836] - IPMITool Factory Default Command raw 30 40 should not reset the network settings
   Infected Motherboard: X12, H12
   Affected functions: factor default
   Validation:
     1) SMCIPMITool ipmi raw 30 70 0c 01 00(to set dedicated LAN), then ipmi raw 30 40(to reset default and keep LAN config).
     2) after BMC boot up, SMCIPMITool ipmi raw 30 70 0c 00(to read lan mode) will return 00 (dedicated lan mode)
     3) SMCIPMIToolipmi raw 30 70 0c 01 00(to set dedicated LAN), then ipmi raw 30 42(to reset default and don't keep LAN config).
     4) after BMC boot up, SMCIPMITool ipmi raw 30 70 0c 00(to read lan mode) will return 02 (failover lan mode)

23.Category: fix
   Description:
     [127207] - After disabling the FIFO, I can still receive logs when the log is full (512 logs)
   Infected Motherboard: ALL
   Affected functions: SEL
   Validation:
     1) Add SEL number to 4096. Added SEL command is below.
        Ex: ipmitool -I lanplus -H BMCIP -U ADMIN -P ADMIN raw 0xa 0x44 0x01 0x00 0x02 0xea 0x91 0x12 0x56 0x20 0x00 0x04 0x13 0x00 0x6f 0x04 0x03 0x05
     2) Disable FIFO Event Log in web page
     3) Add SEL again and should not add successfully
     4) Enable FIFO Event Log in web page
     5) Add SEL again and should add successfully

24.Category: fix
   Description:
     [127680] - Display wrong information when "Virtual Media Port" is turn off.
     [127668] - "TSIG .key File" and "TSIG .private File" hit message is lost one, overlap and shift on DDNS page.
     [127628] - Save success messages for WEBUI inconsistent
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into WEBUI
     2) Turn off VM port -> go to VM page -> redirect msg to port page correct
     3) go to DDNS page -> tsig required messages correctly displayed
     4) save messages correct on syslog and host interface page

25.Category: new
   Description:
     [ENGINEERING] - BMC Unique Firmware Name
   Infected Motherboard: All
   Affected functions: BMC Firmware unified Name
   Validation:
     1)use sum_2.6.0_Linux_x86_64 tool with firmware binary file to check the string of BMC UFFN.
       CMD: ./sum_2.6.0_Linux_x86_64/sum -c GetBmcInfo --file ./BMC_H12AST2600-ROT20-4301MS_20210607_80.11.77_STDsd_.bin
       BMC UFFN shall be BMC_H12AST2600-ROT20-4301MS_20210607_80.11.77_STDsd.bin.

26.Category: fix
   Description:
     [127605] - BMC reset will have Voltage VcpuVCCIO Upper Critical event log in SEL
     [127583] - CPU2 VRMIO temp will randomly display -1C
   Infected Motherboard: X12DPT-PT6
   Affected functions: Sensor
   Validation:
     1) Idle over night then check abnormal VRM temp and voltage event


27.Category: fix
   Description:
     [126549] - MIB sensor Table check error
   Infected Motherboard: ALL
   Affected functions: SNMP
   Validation :
     1) Enable SNMP.
     2) Use SNMP management tools (like iReasoning) to get OEM OID's table values. OEM OID includes sensorTable, nicTable, selTable.
     3) Check there is no excessive rows and columns.

28.Category: fix
   Description:
     [127310] - CPU overheat abnormal
   Infected Motherboard: ALL
   Affected functions: Fan
   Validation:
     1) Boot to cburn-r78
     2) Let CPU overheat
     3) When the CPU temp is higher than upper critical threshold, check if FAN will not slow down.

29.Category: fix
   Description:
     [ENGINEERING] -  use system slot at "Location" in Network AOC tab
   Infected Motherboard: ALL
   Affected functions: Network AOC
   Validation:
     1) Log in Web
     2) System->Component Info->Network AOC

30.Category: Fix
   Description:
     [127700] - RADIUS Server Address Input issue
   Infected Motherboard: ALL
   Affected functions: Account service display
   Validation:
     1) enable RADIUS in account service in WEBUI
     2) config secret and RADIUS server IPv6 address, save and IPv6 address will show [], submit and IPv6 address will show [] too.
     3) config secret and RADIUS server IPv4 or domain name, save and address will not show [], submit and address will not show [] too.

31.Category: Fix
   Description:
     [ENGINEERING] - the system COM1 can not send any data out
   Infected Motherboard: X12
   Validation:
     1)run script rs232.nsh
     2)run UARTTest.efi -port 3F8 -loopback external -baudrate 115200

32.Category: fix
   Description:
     [127224] fix this - ipmi conifg and lic activation
     [127254]  Tips and hit message is overlap on Add new user window.
     [127274] "Auth key" and "Private key" hit message is overlap and not complete on SNMPv3 page.
     [127322] "Port" and "Time to live" hit message is overlap on SSDP page.
     [127324] Select Files..." hit message is overlap with button on IPMI Configuration page.
     [127666] Select Files..." hit message is overlap with button on IPMI Configuration page.
     [127657] Tips and hit message is overlap on "Add New User" window.
     [127665] "Port" and "Time to live" tips and hit message is overlap on SSDP page.
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Go to account page, SSDP, enter any values, no overlapping windows
     3) Go to ipmi config, license activation -> select file -> required
        error message no overlap
     4) SNMPv3 error message no overlap

-----------------------------------------------------------------------------------------------------------------

Firmware Version: 01.01.01
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210609_01.01.01_STDsd.bin
Debug signed Firmware CRC: A411D424
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210609_01.01.01_STDsp.bin
Production signed Firmware CRC: 5D80CBF8
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210609_01.01.01_STDsp.bin
Production signed eMMC Firmware CRC: 0A179A04
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210609_01.01.01_STDsp.bin
Production signed SPI NOR Firmware CRC: 7A9703C5
Build date: 06/09/2021
Supported Platform: X12DGQ-R
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_latest_06112020
-------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.
***note 3: BMC version 1.01.01 start supporting AST2600 A3

1. Category: Fix
   Description:
     [127300] - Account services issue
   Infected Motherboard: ALL
   Affected functions: Redfish, WebUI
   Validation:
    1) WebUI>Configuration>Account Service>Add button
       User Name: test3
       Network Privileges: Administrator

    2) WebUI>Configuration>Account Service>Advanced Settings
        Failed Login Attempt Lockout Threshold : 3
            Failed Login Counter Reset : 5m
            Account Lockout Duration : 5m
       click "Save" button.
       save settings successfully.

    3) use user "ADMIN" login WebUI.
       with 3 times failed password.
       expecting: ADMIN user locked

    4) use user "test3" login WebUI.
       WebUI>Configuration>Account Service
       expecting: ADMIN user is locked. and ADMIN user didn't have deleted button

    5) click ADMIN "unlock" button
       expecting: unlock successfully

2. Category: Fix
   Description:
     [ENGINEERING] Fix redfish liense check
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) run SATC Permission and License test case

3. Category: fix
   Description:
     [124591] - [IPMI Web GUI] Network AOC tab
   Infected Motherboard: ALL
   Affected functions: Network AOC
   Validation:
     1) Log in Web
     2) System->Component Info->Network AOC

4. Category: new
   Description:
     [ENGINEERING] - support AST2600A3
   Infected Motherboard: X12 H12 B12
   Validation:
     Verify on AST2600A3 and AST2600 A1/A2
     1) AC ON/OFF
     2) DC ON/OFF
     3) Power reset
     4) BMC reset cold
     5) Check COM port

-------------------------------------------------------------------------------------------------------

Firmware Version: 01.00.09
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210607_01.00.09_STDsd.bin
Debug signed Firmware CRC: 900A9BE5
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210607_01.00.09_STDsp.bin
Production signed Firmware CRC: A9105C66
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210607_01.00.09_STDsp.bin
Production signed eMMC Firmware CRC: 52E00D12
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210607_01.00.09_STDsp.bin
Production signed SPI NOR Firmware CRC: 359BC090
Build date: 06/07/2021
Supported Platform: X12DGQ-R
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_latest_06112020
-------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.

1. Category: fix
   Description:
     [ENGINEERING] fix - set default DC power cycle interval 10s
   Infected Motherboard: X12DGQ-R
   Affected functions: DC power cycle
   Validation:
     1) stress DC power cycle

2. Category: Fix
   Description:
     [126534] - IPMI Web SNMPv3 can't disabled.
   Infected Motherboard: ALL
   Affected functions: SNMPv3 Redfish
   Validation:
     Testcase 1:
       1) Disable snmpv3 on IPMI Web -> Configuration -> Notifications -> SNMP -> Enable SNMP -> Enabled SNMPv3

3. Category: Fix
    Description:
      [ENGINEERING] - Alert IP is not synchronized between OEM command and Redfish/Web.
    Infected Motherboard: All
    Validation:
      1)Set Alert IP by OEMGetSetAlert(30 68 0B).
      2)Send /redfish/v1/EventService/Subscriptions/{id} API to check the Destination.
      3)Navigate to Notification in Web to check the Destination Address.
      4)Change Destination Address in Web and get Alert IP by OEM command.
      5)Patch Destination by Redfish API and get Alert IP by OEM command.

4. Category: fix
   Description:
     [ENGINEERING] fix - missing sensor reading
   Infected Motherboard: ALL
   Affected functions: sensor reading
   Validation:
     1) host reset then check sensor reading
-----------------------------------------------------------------------------------------------------

Firmware Version: 01.00.08
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210603_01.00.08_STDsd.bin
Debug signed Firmware CRC: F206BA753
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210603_01.00.08_STDsp.bin
Production signed Firmware CRC: 3ABEA3D3
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210603_01.00.08_STDsp.bin
Production signed eMMC Firmware CRC: 023DE265
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210603_01.00.08_STDsp.bin
Production signed SPI NOR Firmware CRC: 359BC090
Build date: 06/03/2021
Supported Platform: X12DGQ-R
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_latest_06112020
-------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW 01.00.08 will be not allowed to downgrade.

1. Category: new
   Description:
     [ENGINEERING] - support AOC-S25GC-i4S
   Infected Motherboard: ALL
   Affected functions: AOC
   Validation:
     1) install AOC-S25GC-i4S
     2) check sensor reading

2. Category: fix
   Description:
     [ENGINEERING] - Fan threshold unify as 280.000   | 420.000   | 560.000   | 35420.000 | 35560.000 | 35700.000
   Infected Motherboard: motherboard without Backplane FAN
   Affected functions: FAN threshold
   Validation:
     1) verify Fan threshold on motherboard without Backplane FAN
        the threshold should be  280.000   | 420.000   | 560.000   | 35420.000 | 35560.000 | 35700.000

3. Category: Fix
   Description:
     [ENGINEERING] - redfish Driver property typo
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) Get /redfish/v1/Chassis/HA-RAID.0.StorageEnclosure.0/Drives/Disk.Bay.0

4. Category: fix
   Description:
     [ENGINEERING] - update BIOS version early in recovery flow as well
   Infected Motherboard: Projects with RoT 20 solution
   Affected functions: RoT 20 BIOS recovery
   Validation:
     1) Try to recover BIOS
     2) Check the inventory page and expect to see the version change

5 .Category: Fix
   Description:
     [ENGINEERING] - Trying to change Rollback ID setting on any license other than DCMS will show prompt.
   Infected Motherboard: PFR-CPLD
   Affected functions: AntiRollback
   Validation:
     1) Activate OOB License on system.
     2) Navigate to "Firmware Management" page on Web UI.
     3) Try changing Rollback ID setting to Manual.
     4) Prompt will pop up stating that DCMS license is required to set Manual setting and asking if user wants to go to License Activation page.

6. Category: fix
   Description:
     [127285] - Memory serial number doesn't show completely.
     [127256] - "Export to excel" string display is over the edge on HEL/MEL page.(Japanese)
     [127223] - Don't show error message when type in IPv4 format address at IPv6 DNS server
     [127214] - Language Dict Spelling Issues
     [126676] - Non-functioning Scroll Bar On Many Pages Of Web UI
     [126611] - Different format under PSU page is u "
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web -> memory page -> serial numbers fully visible
     2) SEL -> change to Japanese -> all buttons text only in buttons
     3) configuration network -> type in correct and incorrect ipv6 address
     4) psu and account services page removed unnecessary scroll bars
     5) psu all entries have border line in table

7. Category: Fix
   Description:
     [ENGINEERING] - redfish property mismatch by TSMC request
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) Get /redfish/v1/Managers/1/EthernetInterfaces/1 to check HostName
     2) Get /redfish/v1/Systems/1 to check SerialNumber
     3) Get /redfish/v1/Systems/1 to check ProcessorSummary HealthRoolup and MemorySummary HealthRoolup
     4) Get /redfish/v1/Managers/1/LogServices/Log1/Entries to check description
     5) Get /redfish/v1/Systems/1/LogServices/Log1/Entries to check description
     6) Get /redfish/v1/Managers/1/EthernetInterfaces/1 to check always show IPv4StaticAddresses if no in static mode
     7) Get /redfish/v1/Managers/1/EthernetInterfaces/1 to check NameServers include IPV6 DNS
     8) Get /redfish/v1/Managers/1/EthernetInterfaces/1 to check DHCPv4 and DHCPv6 property
     9) Get /redfish/v1/Managers/1/EthernetInterfaces/1 to check always show IPv6StaticAddresses if no in static mode
    10) Get /redfish/v1/Chassis/1/NetworkAdapters/1/NetworkPorts/1 to check Name and PhysicalPortNumber
    11) Get /redfish/v1/Chassis/1/Power to check PowerSupplies include InputRanges, PartNumber and Redundancy
    11) Get /redfish/v1/Chassis/1/Power to check Voltage remove UpperThresholdNonCritical, LowerThresholdNonCritical
    12) Get /redfish/v1/Chassis/1/Thermal to check Fan remove UpperThresholdNonCritical, LowerThresholdNonCritical and add SensorNumber
    13) Get /redfish/v1/Chassis/1/Thermal to check Termperature remove UpperThresholdNonCritical, LowerThresholdNonCritical and add SensorNumber

8. Category: Fix
   Description:
     [127225] - SMCIPMITOOL couldn't show IPv6 address after setting Network lan mode to dual
     [ENGINEERING] - IPMIECO TC #267 IPMIECO.SUM OOB Test.Test case 267 - OOB - Test SUM command "MountIsoImage" and "UnmountIsoImage" with IPv6
   Infected Motherboard: ALL
   Validation:
   Testcase1:
     Pre-condition: need have RA in network environment
     1) SMCIPMITOOL > ipmi raw 30 42
     2) SMCIPMITOOL > ipmi lan protocol 2
     3) SMCIPMITOOL > ipmi lan ipv6 list
        expecting: has one ipv6 address.

   Testcase2:
     1) SMCIPMITOOL > ipmi raw 30 42
     2) SMCIPMITOOL > ipmi lan protocol 2
     3) SMCIPMITOOL > ipmi lan ipv6 add 3 2021:db9::3 64
     4) SMCIPMITOOL > ipmi lan ipv6 list
        expecting: index 3 has added ipv6 address

9. Category: new
   Description:
     [ENGINEERING] - support AST2600A3
   Infected Motherboard: X12 H12
   Validation:
     Verify on AST2600A3 and AST2600 A1/A2
     1) AC ON/OFF
     2) DC ON/OFF
     3) Power reset
     4) BMC reset cold
     5) Check COM port
     6) Check SAS3808 sensor reading

10.Category: Fix
   Description:
     [122631] - SUMECO TC #315
   Infected Motherboard: B12SPE
   Validation:
     1)Run SUMECO TC #315 and it's passed.

11.Category: Fix
   Description:
     [126285] - BMC storage monitoring Logical view page only can show 1 JBOD device. 2 JBOD devices actually created in the system.
     [126970] - incorrect information showing in controller page
   Infected Motherboard: X12DPT-B6
   Affected functions: Storage
   Validation:
     1) Install AOC-SMG3-2M2-B on system.
     2) Create 2 JBOD volumes via Marvell in-band tool.
     3) Login BMC WEB
     4) Go to [System]->[Storage Monitoring]->[Logical View] page to check VD data.
     5) Go to [System]->[Storage Monitoring]->[Controller] page to check controller data.

12.Category: Fix
   Description:
     [121788] - Added longer delay as well as forcefully shutting down system if graceful shutdown doesn't work
   Infected Motherboard: ALL
   Affected functions: PFR
   Validation:
     1) Run sum.exe -i <ip> -u <username> -p <password> -c BiosRotManage --action 2 --reboot
     2) SUM should not encounter "Sending packets timeout..." error

13. Category: fix
    Description: 
      [127088] - MEM thermal trip event that will trigger CPU thermal trip.
    Infected Motherboard: X12DPT-PT6
    Affected functions: Event
    Validation :
      1) Heat up memory to shutdown then check only memory thermal trip event.

14. Category: Fix
    Description:
      [127085] - Time format not match
    Infected Motherboard: ALL
    Affected functions: Redfish
    Validation:
      1) Get redfish/v1/Managers/1/LogServices/Log1/Entries to check time format yyyy-mm-ddThh:mm:ssZ

15. Category: Fix
    Description:
      [126622] - User only can launch one HTML5 window after FD
    Infected Motherboard: ALL
    Affected functions: Web iKVM
    Validation:
      Check the iKVM interface can be launched four windows at the most.
      1) Login BMC WEB GUI
      2) Login Webgui
      3) Perform Factory default
      4) Launch console in HTML5 window and 2nd/3rd/4th windows.

16. Category: new
    Description:
     [ENGINEERING] - support mellanox AOC-653436A-HDAB 200GbE
    Infected Motherboard: ALL
    Affected functions: AIOM
    Validation:
      1) install AOC-653436A-HDAB
      2) check sensor reading

17. Category: Fix
    Description:
      [122125] - The latest event can not be marked as acknowledged.
    Infected Motherboard: ALL
    Affected functions: Redfish
    Validation:
      1) add HEL to 4096 by watch -n 0.5 ./SMCIPMITool 10.135.169.167 ADMIN ADMIN ipmi raw 4 02 01 4 c2 ff 6f a0 18 ff
      2) Get redfish/v1/Systems/1/LogServices/Log1/Entries/4096
      3) Patch {"Oem": {"Supermicro": {"MarkAsAcknowledged": true}}} on redfish/v1/Systems/1/LogServices/Log1/Entries/4096

18. Category: fix
    Description:
      [126781] - Virutal CD-ROM can import invalid symbol for input option
    Infected Motherboard: ALL
    Affected functions: Web
    Validation:
      1) Go to VM page -> cd ROM user/password will reject containina '\' '/'

19. Category: fix
    Description:
      [ENGINEERING] Fix wrong relative link on UpdateService/FirmwareInventory/Broadcom1
    Infected Motherboard: X12
    Affected functions: Redfish
    Validation:
      1)  install 3008 card then Get /redfish/v1/UpdateService/FirmwareInventory/Broadcom1
      2) "RelatedItem" should be "/redfish/v1/Systems/1/Storage/HBA#/StorageControllers/0"

20. Category: fix
    Description:
      [126637]	- System will not power up after flashed BIOS on IPMI web
      [127002]	- BMC Web gui can't login after running SATC auto testing.
    Infected Motherboard: ROT20
    Affected functions: update
    Validation:
      1) update BIOS and power on
      2) run SATC

----------------------------------------------------------------------------------------------------------

Firmware Version: 01.00.07
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210521_01.00.07_STDsd.bin
Debug signed Firmware CRC: 3B19C3E3
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210521_01.00.07_STDsp.bin
Production signed Firmware CRC: 9DB64DAA
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210521_01.00.07_STDsp.bin
Production signed eMMC Firmware CRC: 2C99175E
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210521_01.00.07_STDsp.bin
Production signed SPI NOR Firmware CRC: 12B24F2C
Build date: 05/21/2021
Supported Platform: X12DGQ-R
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_latest_06112020
-------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW and above will be not allowed to downgrad.

1. Category: fix
   Description:
     [126642] - Power consumption SC mode error...
     [126727] - Fix for user password validation on WebGUI
     [126600] - IPMI Web - Account info display format different in two platforms
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web -> change to SC
     2) x-axis in power graph correct
     3) Account info contains user/role/server separatly
     4) Add user with password "Tester001!@#$% succesfully

2. Category: Fix
   Description:
     [126757] - AOC-MCX566A-CDA AIOM sensor drop during cburn on/off
   Infected Motherboard: ALL
   Affected functions: AIOM
   Validation:
     1) verify AIOM sensor

3.Category: Fix
  Description:
    [ENGINEERING] - Yellow rbid notification now only shows on BMC or BIOS selected components
  Infected Motherboard: ALL
  Affected functions: Firmware Update
  Validation:
    1) Navigate to Firmware Management page on Web GUI
    2) When the "Allow Rollback ID To Be Updated" is checked, the yellow warning notification will appear.
    3) This notification should only appear for BMC and BIOS components, not Motherboard or Backplane CPLD, etc.

4. Category: Fix
   Description:
     [126328] Fix - AOC revision showing as rev 1.0 instead of 1.01
   Infected Motherboard: X12DPT-B6
   Affected functions: Storage
   Validation:
     1) Login BMC WEB
     2) Go to [System]->[Storage Monitoring]->[Controller] to check
        Marvell AOC version, its format should be X.YZ (such as: 1.01)

5.Category: fix
  Description:
    [ENGINEERING] - Disable GPIOS2 internal pull down to prevent PEWEAK voltage level be dropped.
  Infected Motherboard: X12MBs
  Affected functions: PEWEAK
  Validation:
    1)Measure PEWEAK pin voltage level.

6. Category: Fix
   Description:
     [ENGINEERING]- fix the PCIe Gen version in PCIeDevices instance API
   Infected Motherboard: X12
   Validation:
     1)Issue PCIeDevices API and check MaxPCIeType value.

7. Category: Fix
   Description:
     [126317] - The system got "PSU status power supply installed" event log when running idle stress while boot in cburn.
   Infected Motherboard: X12DPT-PT6
   Affected functions: EventLog
   Validation:
     1) Idle over night then check abnormal PSU or smart power event

8. Category: fix
   Description:
     [126469] - No Network AOC card sensor and info
     [126406] - no AOC NIC sensor reading
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) verify AOC threshold and sensor reading

9.Category: Enhancement
  Description:
    [ENGINEERING] - Update BIOS through SUM with BMC reboot now preserves BIOS settings
  Infected Motherboard: PFR-CPLD
  Affected functions: Firmware Update
  Validation:
    1) In SUM, run command -c GetCurrentBiosCfg
    2) Modify the downloaded BIOS config file
    3) In SUM, run command -c ChangeBiosCfg. Wait until after POST to go to step 4.
    4) In SUM, run command -c GetCurrentBiosCfg again, compare with previous config file. Should be same as modified config file.
    5) In SUM, run command -c UpdateBIOS with --preserve_setting
       Make sure that the firmware you are testing with will update the BIOS rollback ID and cause BMC to reboot.
    6) Power on BIOS (if it is off), wait until after POST and in SUM, run command -c GetCurrentBiosCfg. Should be the same as the modified config file.

10. Category: fix
   Description:
     [ENGINEERING] - TC 407/408
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web with no license -> SEL
     2) Check one red SEL, hover over "Clear Acknowledgments"
     3) Tooltip appears sending user to license activation page

11. Category: fix
   Description:
     [ENGINEERING] - greatly refine pfr_ast2600_log_events()
   Infected Motherboard: Projects with RoT 20 solution
   Affected functions: RoT 20 log
   Validation:
     1) Try BMC/BIOS update
     2) Try BMC/BIOS golden updage/recovery
     3) Try to trigger automatic recovery
     4) Expected to see everything works normally

12. Category: Fix
   Description:
     [126299] [IPMI ECO 01.00.03]SATC test fail; there are 10 fail items
     [123888] [Milan IPMI v01.26 ECO] SATC redfish automation test failed.
     [123263] [IPMI ECO 1.26]SATC test fail; there are 4 fail items.
     [120918] Redfish Automation API test failed with 23 failures
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) run full test on SATC then check result should all pass

13. Category: fix
   Description:
     [126614] - Abnormal behavior on Sensor page
     [126676] - non-functioning Scroll bar on many pages
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Sensor page -> Remove all filter change severity
     3) Entries in sensor grid will not comeback
     2) remove vertical scrollbar in MEL,CPU,GPU,memory,network aoc,power,psu,SEL

14. Category: fix
   Description:
     [126581] - SSDP port number 1-65535
     [126581] - Disable VM port at the first time
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Port page -> set settings -> check if correct
     3) SSDP page -> cannot enter 0 port number

15. Category: Enhancement
   Description:
      [#122284] fix - The snmp alerts can't be added by SMCIPMITool
   Infected Motherboard: ALL
   Affected functions: SNMP v1 Trap
   Validation:
     Testcase 1:
       1) .\SMCIPMITool.exe [IP] [Name] [Password] shell
       1-1) nm20 alert 1
       1-2) nm20 addpolicy 0 1 0 0 1 50 6000 50 3 1
       1-3) redfish eventService alert setSNMPv1 2 0 10.135.177.157 0
       2) Do OS power off and power on
       3) Should receive nm alert

16. Category: feature
   Description:
     [ENGINEERING] Fix Storage redfish API count
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) Get redfish/v1/Systems/1/ should shows Storage and SimpleStorage
     2) Get redfish/v1/Systems/1/SimpleStorage count is 0 for no storage controller
     3) Get redfish/v1/Systems/1/Storage count is 0 for no storage controller

17. Category: feature
   Description:
     [ENGINEERING] Add SensorNumber property in /Chassis/1/Thermal
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) Get redfish/v1/Chassis/1/Thermal to check SensorNumber of Fans

18. Category: Fix
   Description:
     [ENGINEERING] - fix the NIC is assigned to shared NIC when both dedicated and shared NICs are connected
   Infected Motherboard: ALL
   Affected functions: DHCP
   Validation:
     1.) Connect dedicated NIC and shared NIC to different dhcp server.
         The dhcp servers serve different ip range can help to recognize the using NIC.
     2) Confirm the dedicated NIC is using, and doing AC cycle. It includes two cases, host power on and host power off.
     3) After BMC booting up is completed, check the dedicated NIC is using.

19.Category: Fix
  Description:
    [ENGINEERING] - Completion message now stays for 15 seconds.
  Infected Motherboard: ALL
  Affected functions: Firmware Update with SUM
  Validation:
    1) Update BIOS through the Web GUI
    2) The completion message "System is rebooting!" stays for 15 seconds.

20. Category: fix
   Description:
     [ENGINEERING] - Correct power status displayed after BIOS update
   Infected Motherboard: ALL
   Affected functions: web bios update
   Validation:
     1) Log into web
     2) Update Bios
     3) System will turn on after completion and show correct power status

21.Category: Fix
  Description:
    [126574] - Generate Evidence function now works after auto recovery
  Infected Motherboard: ROT 2.0
  Affected functions: PFR
  Validation:
    1) Make sure there are valid BIOS images in backup and golden areas.
    2) Trigger BIOS auto recovery.
    3) Go to Firmware Inventory page and click on icon to bring up PFR actions.
    4) Generate Evidence button should be enabled.

22.Category: Fix
  Description:
    [ENGINEERING] - Rollback ID Alert doesn't show on Sentry and ROT 2.0 systems.
  Infected Motherboard: ROT 1.0 and ROT 2.0
  Affected functions: Firmware Update
  Validation:
    1) Navigate to "Firmware Management" page on the web GUI.
    2) The Rollback ID yellow notification will not be displayed on Sentry and ROT 2.0 systems.

23.Category: Fix
  Description:
    [ENGINEERING] - BMC auto recovery now prints to SEL
  Infected Motherboard: ROT 2.0
  Affected functions: PFR
  Validation:
    1) Make sure there are valid BMC images in backup and golden areas.
    2) Trigger BMC auto recovery.
    3) BMC successfully recovered message will show in SEL.

24.Category: Fix
  Description:
    [126283] - Red LED now lights up solid if BIOS auto recovery fails or the BIOS flash chip is removed
  Infected Motherboard: ROT 2.0
  Affected functions: PFR
  Validation:
    1) AC OFF
    2) Remove BIOS flash chip
    3) AC ON
    4) Verify that the red LED will light up solid

----------------------------------------------------------------------------------------------------------------

Firmware Version: 01.00.06
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210511_01.00.06_STDsd_8A19D623.bin
Debug signed Firmware CRC: 8A19D623
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210511_01.00.06_STDsp_764AC1A7.bin
Production signed Firmware CRC: 764AC1A7
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210511_01.00.06_STDsp_A9AA49BC.bin
Production signed eMMC Firmware CRC: A9AA49BC
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210511_01.00.06_STDsp_12B24F2C.bin
Production signed SPI NOR Firmware CRC: 12B24F2C
Build date: 05/11/2021
Supported Platform: X12DGQ-R
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_latest_06112020
-------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW and above will be not allowed to downgrad.

1. Category: Fix
   Description:
     [126390] - [ROT] BIOS recovery feature doesn't work when unauthorized BIOS image is detected
     [126387] - [ROT] BIOS doesn't recover when power loss during update
     [126283] - [ROT] BIOS failed LED behavior is incorrect
   Infected Motherboard: Projects with RoT 20
   Affected functions: BIOS recovery, CPLD update
   Validation:
     1) Destory BIOS flash and AC cycle. It's expected to see the successful recovery and log
     2) Remove BIOS flash and AC cycle. It's expected to see the failed recovery and log

2. Category: Fix
   Description:
     [126404] - [ROT] MEL for BMC manual recovery
   Infected Motherboard: Projects with RoT 20
   Affected functions: log of BMC recovery
   Validation:
     1) Perform BMC recovery
     2) Expected to see the corresponding log

3. Category: Fix
   Description:
     [126390] - [ROT] BIOS recovery feature doesn't work when unauthorized BIOS image is detected
   Infected Motherboard: Projects with RoT 20
   Affected functions: log of BIOS auto recovery
   Validation:
     1) Perform BIOS auto recovery
     2) Expected to see the corresponding log

4. Category: Fix
   Description:
     [126335] - [ROT] No event log for backup image updated
   Infected Motherboard: Projects with RoT 20
   Affected functions: log of BIOS update
   Validation:
     1) Perform BIOS backup & update
     2) Expected to see the corresponding log

5. Category: fix
   Description:
     [126475] - SSDP port number range from note box and alert message mismatch.
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web -> go to SSDP
     2) Enter 0 for por number -> error msg say 1-65535.

6. Category: fix
   Description:
     [126406] - No AOC NIC sensor reading
     [126291] - There is no temp sensor reading for AOC-S100G-i2C
     [126469] - No Network AOC cards sensor and info
     [ENGINEERING] - AOC tempeature name has unknown character in SMCIPMITool
   Infected Motherboard: ALL
   Affected functions: sensor
   Validation:
     1) verify AOC NIC temperature reading
     2) verify SMCIPMITool ipmi sensor name

7. Category: fix
   Description:
     [126042] - Wrong threshold settings on multiple sensors
   Infected Motherboard: X12DGQ-R
   Affected functions: sensor
   Validation:
     1) verify sensor threshold

8. Category: fix
   Description:
     [126266] - User able to set username with "@" error message fix
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web
     2) Add new user with username containing '@'

9. Category: fix
   Description:
     [ENGINEERING] - BIOS update finished but task status is EXCEPTION
   Infected Motherboard: All
   Affected functions: BIOS update
   Validation:
     1) Update BIOS and check task status

10. Category: Fix
   Description:
     [123310] - Incorrect WebUI behavior after enable system lockdown
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1.) Enable System Lockdown.
     2.) Click the thumbnail of iKVM preview on MainPage(DashBoard).
     3.) Check iKVM shall be not opened.

11. Category: fix
   Description:
     [ENGINEERING] - BIOS update finished but task status is EXCEPTION
   Infected Motherboard: All
   Affected functions: BIOS update
   Validation:
     1) Update BIOS and check task status

12. Category: Fix
   Description:
     [123310] - Incorrect WebUI behavior after enable system lockdown
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1.) Enable System Lockdown.
     2.) Click the thumbnail of iKVM preview on MainPage(DashBoard).
     3.) Check iKVM shall be not opened.

13. Category:
   Description: fix
     [ENGINEERING] - Replace BMC power into DCMI power reading for template work around
     [124855] - It got fail via smstc att on TC102 Reset/Load default IPMI "0 Watts"
   Infected Motherboard: ALL
   Affected functions: DCMI
   Validation :
    1) ipmitool -t 0x2c -b 0 raw 0x2c 0x02 0xdc 0x01 0x00 0x00 to check ME report 0 watt
    2) ipmitool raw 0x2c 0x02 0xdc 0x01 0x00 0x00 to check power reading

14. Category: Enhancement
   Description:
     [ENGINEERING] - when the operator delete the user though SMCIPMITool, it always shows “Clean user password failed”
   Infected Motherboard: ALL
   Affected functions: IPMI CMD
   Validation:
     Testcase 1:
       1) .\SMCIPMITool.exe [IP] ADMIN ADMIN user add 3 1234 1qaz@WSX 4
       2) .\SMCIPMITool.exe [IP] ADMIN ADMIN user delete 3
       3) Cmd should work successfully

15. Category: Fix
   Description:
    [ENGINEERING] - Added some delay for SUM to poll BIOS update progress
   Infected Motherboard: ALL
   Affected functions: Firmware Update
   Validation:
    1) Use SUM to update the BIOS
    2) SUM should not give an error pertaining to not being able to poll the update progress.

16. Category: fix
   Description:
     [125426] - Extra characters in warning error message for user
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web -> virtual media
     2) User input error message correct

17. Category:
   Description: fix
     [123848] IPMI Web - System - Component Info - CPU Speed value error.
   Infected Motherboard: ALL
   Affected functions: Web
   Validation :
     1) Login Web>Component Info>CPU to check

18. Category: Fix
   Description:
     [123865] After heating memory until OS shutdown, IPMI create event log is incorrect.
   Infected Motherboard: ALL
   Affected functions: HEL
   Validation:
     1) raw 0x4 0x02 0x01 0x4 0xc2 0xff 0x6f 0xa0 0x18 0xff
---------------------------------------------------------------------------------------------------

Firmware Version: 01.00.04
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210505_01.00.04_STDsd.bin
Debug signed Firmware CRC: F66A464B
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210505_01.00.04_STDsp.bin
Production signed Firmware CRC: 184D37AA
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210505_01.00.04_STDsp.bin
Production signed eMMC Firmware CRC: 7EC92FF6
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210505_01.00.04_STDsp.bin
Production signed SPI NOR Firmware CRC: 5A82B242
Build date: 05/05/2021
Supported Platform: X12DGQ-R
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_latest_06112020
-------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW and above will be not allowed to downgrad.

1. Category: fix
   Description:
     [ENGINEERING]  - [RoT 2] Update BIOS version early
   Infected Motherboard: Projects with RoT 2
   Affected functions: Inventory page
   Validation:
     1) Remove CPU and update BIOS
     2) Expected to see BIOS version changed without the help from BIOS

2. Category: fix
   Description:
     [ENGINEERING] - update crash dump 1.0.6
   Infected Motherboard: ALL
   Affected functions: Crashdump
   Validation:
     1) power on and post complete then crashdump
     2) check the crashdump version in dump file

3. Category: fix
   Description:
     [126116] fix - NVMe eject and insert fail
   Infected Motherboard: X12DGQ-R
   Affected functions: storage
   Validation:
     1) try to eject the NVMe
     2) try to insert the NVMe

4. Category: fix
   Description:
     [ENGINEERING]- Support the combination of 'erase' and 'update' commands
   Infected Motherboard: Projects with RoT
   Affected functions: Update/erase commands
   Validation:
     1) 0x30 0x68 0sx28 0x20 # update
     2) 0x30 0x68 0sx28 0x21 # erase

5. Category: new
   Description:
     [ENGINEERING] new - support bpn cpld update
   Infected Motherboard: X12DGQ-R
   Affected functions: bpn cpld
   Validation:
     1) update bpn cpld then check firmware version

6. Category: fix
   Description:
     [125362] - Golden Images Cannot Be Updated in WebGUI
     [126130] - [ROT] CPLD provision through IPMI raw command
     [126084] - [ROT] IPMI backup existing BIOS image failed
     [126048] - [ROT] BIOS golden image update failed
     [126126] - [ROT] IPMI web BMC recover feature doesn't work
   Infected Motherboard: ALL
   Affected functions: ROT
   Validation:
     1) update golden image through WEBUI
     2) CPLD provision through IPMI raw command
     3) do BIOS backup
     4) do recovery

---------------------------------------------------------------------------------------------------

Firmware Version: 01.00.03
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210430_01.00.03_STDsd.binn
Debug signed Firmware CRC: 736D8F4D
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210430_01.00.03_STDsp.bin
Production signed Firmware CRC: 1AEED529
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210430_01.00.03_STDsp.bin
Production signed eMMC Firmware CRC: BC24D76E
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210430_01.00.03_STDsp.bin
Production signed SPI NOR Firmware CRC: D09A94BB
Build date: 04/30/2021
Supported Platform: X12DGQ-R
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_latest_06112020
-------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: This FW and above will be not allowed to downgrad.

1. Category: fix
   Description:
     [126105] - No M.2 sensor reading
   Infected Motherboard: X12DGQ-R
   Affected functions: sensor
   Validation:
     1) verify M.2 sensor reading

2. Category: fix
   Description:
     [ENGINEERING] - Preserve NVRAM removed because unnecessary
   Infected Motherboard: ALL
   Affected functions: mntc fw update page
   Validation:
     1) Log into web -> firmware update -> bios
     2) preserve nvram hidden

3.  Category: Fix
    Description:
      [126083] - MEL severity is incorrect
    Infected Motherboard: ALL
    Affected functions: WebUI, Virtual Media
    Validation:
    Testcase 1:
      1) check Maintenance event log

4. Category: fix
   Description:
     [125725] - Inaccurate inlet temperature sensor reading to actual ambient
   Infected Motherboard: X12DGQ-R
   Affected functions: sensor
   Validation:
     1) verify Inlet Temp thermal and reading.

5. Category: fix
   Description:
     [126042] - Wrong threshold settings on multiple sensors
   Infected Motherboard: X12DGQ-R
   Affected functions: sensor
   Validation:
     1) verify sensor threshold

6. Category: fix
   Description:
     [125550] - Incorrect value chassis info shows after modify CT value.
     [125554] - Fail to remove invalid file under SSL Certification page
     [125551] - User cannot set password with 20 characters.
     [125176] - Fail to save valid SSDP port value
   Infected Motherboard: ALL
   Affected functions: web
   Validation:
     1) Under Compnent Info -> chassis type valid
     2) Remove invalid file on SSL certification page succesful
     3) Create new user with password of length 20 successful
     4) Hover SSDP port value, warning message is 1~65535

7.  Category: Fix
    Description:
        [#125547] Fix - User is able to set user name with special character which is not allowed
    Infected Motherboard: ALL
    Affected functions: IPMI CMD
    Validation:
      Testcase 1:
        1) Ipmitool -H {IP} -U {username} -P {password} user set name 3 #$#$# -> failed
        2) Any other name include Space, Tab, Double quote, Single quote, Colon, Comma, Hash, Minus, and Semicolon is not allowed

8. Category: fix
   Description:
     [123543] - fix 123543 - LAN Connection Failover fail
   Infected Motherboard: ALL
   Affected functions: HTML5 KVM
   Validation:
     0) Setup: Dedicated, Share NIC netowrk workable
     1) BMC Web > Configuration > Network > "Lan Interface" set to Failover
	check Configuration > Network > "Active Interface"
	expecting: Dedicated
     2) BMC Web > Remote Control
	Set "Current Interface": HTML5
	Click "Launch Console" Button
	expecting: launch HTML5 KVM key-in characters successfully.
	           and dont't close this windows.
     3) Plug-out Dedicated lan cable
	check Configuration > Network > "Active Interface"
	expecting: Share
     4) In HTML5 KVM windows key-in some characters
	expecting: work successfully

9. Category: fix
   Description:
     [ENGINEERING] - BMC/BIOS/CPLD update functions support
   Infected Motherboard: X12DGQ-R
   Affected functions: fw update
   Validation:
     1) update BMC/BIOS/CPLD
---------------------------------------------------------------------------------------------------

Firmware Version: 01.00.01
Debug signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210427_01.00.01_STDsd.bin
Debug signed Firmware CRC: 003224F4
Production signed Firmware Name: BMC_X12DGQR-ROT20-1301MS_20210427_01.00.01_STDsp.bin
Production signed Firmware CRC: B7FB4671
Production signed eMMC Firmware Name: BMC_X12DGQR-ROT20-1301MS-eMMC_20210427_01.00.01_STDsp.bin
Production signed eMMC Firmware CRC: F6FAF3BF
Production signed SPI NOR Firmware Name: BMC_X12DGQR-ROT20-1301MS-NOR_20210427_01.00.01_STDsp.bin
Production signed SPI NOR Firmware CRC: 4730F5F3
Build date: 04/27/2021
Supported Platform: X12DGQ-R
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_latest_06112020
-------------------------------------------------------------------------------
***note 1: If your board is running debug FW,  please cap JPFR2 jumper then update debug signed FW.
***note 2: 01.00.01 will be not allowed to downgrad.

1. Category: Fix
   Description:
     [125759] - IPMI sensoer missing VCPU and VDIMM
   Infected Motherboard: X12DGQ-R
   Affected functions: sensor
   Validation:
     1) verify sensor reading.

2. Category: Fix
   Description:
     [125548] - Error message will pop up when create Username with < >
   Infected Motherboard: ALL
   Affected functions: User
   Validation:
     1) Add user with name <test12345> should add successfully.

3.  Category: Fix
    Description:
      [ENGINEERING] - IPMIECO Testcase #267,#401,#402,#408,#409 WebUI test case
    Infected Motherboard: ALL
    Affected functions: WebUI, Virtual Media
    Validation:
    Testcase 1:
      1) IPMIECO WebUI
      2) Test case #401,#402,#407,#408,#409
      3) Test Case # 267 (Test SUM command "MountIsoImage" and "UnmountIsoImage" with IPv6)

    Testcase 2:
      1) Mount RHEL8.2.iso over HTTP (has 7.9G)
      2) Install OS. expecting: installed successfully.

4. Category:
   Description: fix
     [125714] [DVT]AOC-S100G-b2C sensor reading show NA in the IPMI GUI.
   Infected Motherboard: ALL
   Affected functions: Sensor
   Validation :
     1) install AOC-S100G-b2C then check reading

5. Category: fix
   Description:
     [125820] - [SK hynix PE810] IPMI show manufacturer's name is UNKNOWN
   Infected Motherboard: ALL
   Affected functions: NVME
   Validation:
     1) Install SK hynix PE810 and check NVME detail info

6.  Category: fix
    Description:
      [ENGINEERING] -IPMIECO Test case 124 - OEM command for Event of Call Home
    Infected Motherboard: ALL
    Affected functions: Sensor
    Validation:
      Testcase:
      1) IPMIECO
      2) Test case #124

7. Category: fix
   Description:
     [123604] - Virtual keyboard ikvm java cut short fix
   Infected Motherboard: ALL
   Affected functions: ikvm
   Validation:
     1) Open java ikvm -> check virtual keyboard is not cut short

8. Category: fix
   Description:
     [ENGINEERING] - kernel panic when remote install ESXi OS by httpfs mount
   Infected Motherboard: ALL
   Affected functions: VM
   Validation:
     1) mount VM CD ISO to install ESXi then check BMC should not disconnect

9. Category: fix
   Description:
     [124599] ECO -18441-- 01.00.12(03/12/2021)-- Fail to save and mount floppy image file
     [125557] OEM - Nvidia 19713 -- 00.01.33 - Fail to save & mount floppy image file
   Infected Motherboard: ALL
   Affected functions: Virtual Media
   Validation:
     1) Mount floppy through BMC virtual media page

10. Category: fix
   Description:
     [ENGINEERING] - host won't power up after BIOS update by tool
   Infected Motherboard: ALL
   Affected functions: BIOS update
   Validation:
     1) sum -i $IP -u ADMIN -p ADMIN -c updatebios --file your_bios --reboot
     2) host should power up after BIOS update

11.Category: Fix
  Description:
    [ENGINEERING] - Update Rollback ID Checkbox no longer interactable with Rollback ID Setting being Automatic
  Infected Motherboard: ALL
  Affected functions: Firmware Update
  Validation:
    1) Navigate to "Firmware Management" page on the web GUI
    2) Go to "Step 2"
    3) Click "Cancel"
    4) It should take you back to "Step 1" with "Update Rollback ID" checkbox still non-interactable.

12.Category: Fix
  Description:
    [ENGINEERING] - Disable Rollback ID setting change during Step 3
  Infected Motherboard: ALL
  Affected functions: Firmware Update
  Validation:
    1) Navigate to "Firmware Management" page on the web GUI
    2) Go to "Step 3"
    3) Try changing Rollback ID setting between Automatic and Manual. The radio buttons should not be interactable.

13. Category: Enhancement
   Description:
     [ENGINEERING] - go back to power off update BIOS
   Infected Motherboard: X12, B12
   Affected functions: WEBUI Update BIOS
   Validation:
     1) power off to update BIOS.

14. Category: Fix
   Description:
     [ENGINEERING] - The bios update percentage keep 0 if preserve BIOS NVRAM
   Infected Motherboard: ALL
   Affected functions: BIOS Update
   Validation:
     1) The bios update percentage should be normal if preserve BIOS NVRAM

15. Category: fix
   Description:
     [125174] - Abnormal behavior after return back to Alerts page from SNMP page
   Infected Motherboard: ALL
   Affected functions: web
   Validation:
     1) Log in -> alert page -> snmp page -> alert page
     2) Alert page looks correct with no issues

16. Category: Fix
   Description:
     [ENGINEERING] - "DateTime" zone format mismatch and MEL serverity format
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) Get redfish/v1/Systems/1/LogServices/Log1/
     2) Get redfish/v1/Systems/1/LogServices/Log1/Entries
     3) Get redfish/v1/Managers/1/LogServices/Log1/
     4) Get redfish/v1/Managers/1/LogServices/Log1/Entries

17. Category: fix
   Description:
     [ENGINEERING] - Web service may hang up when SEL are full and log in webUI with Chrome browser
   Infected Motherboard: ALL
   Affected functions: WebUI
   Validation :
     1) Add SEL to 4096.
     2) Login WebUI by the Chrome browser.
     3) Check website not hang up.
     4) Logout and Login WebUI three times.
     5) Check website not hang up.

18.Category: Fix
  Description:
    [123408] - If FW verification fails or system powers off on Firmware Management page, it will stay on Step 2.
  Infected Motherboard: ALL
  Affected functions: Firmware Update
  Validation:
    1) Navigate to "Firmware Management" page on web GUI
    2) Upload invalid firmware OR power off system IF there is prompt to power off system.
    3) It will stay on Step 2

19.Category: Fix
  Description:
    [123512] - First step: Choose component and options / Second step: Upload Firmware File
  Infected Motherboard: ALL
  Affected functions: Firmware Update
  Validation:
    1) Navigate to "Firmware Management" page on web GUI
    2) First step now consists of selecting component and options.
    3) Second step consists of uploading the firmware file.

20. Category: fix
   Description:
     [125426] - LANG Dictionary and Textfield Error Message Errors
   Infected Motherboard: ALL
   Affected functions: WEBUI network page and virtual media page
   Validation:
     1) Verify virtual media page user field and multi-language
     2) Verify network page IPv6 address field and multi-language
     3) Verify network page IPv6 DNS Server IP field and multi-language
     4) Verify network page IPv6 Prefix to Route field and multi-language
     5) Verify network page IPv6 Router Address field and multi-language

21. Category: Fix
   Description:
     [123888] - SATC redfish automation test failed.
   Infected Motherboard: ALL
   Affected functions: IPv6
   Validation:
     Testcase 1:
     1) Run SATC Manager->Ethernet Interface
     Testcase 2:
     1) PATCH /redfish/v1/Managers/1/EthernetInterfaces/1/ with {"IPv6StaticAddresses": [{"Address": "2001::8392:8392:8392:5", "PrefixLength": 64}]}
     2) PATCH /redfish/v1/Managers/1/EthernetInterfaces/1/ with {"IPv6StaticAddresses": [null]}
     3) GET /redfish/v1/Managers/1/EthernetInterfaces/1/ should not contain 2001::8392:8392:8392:5/64
     Testcase 3:
     1) PATCH /redfish/v1/Managers/1/EthernetInterfaces/1/ with {"IPv6StaticAddresses": [{"Address": "2001::8392:8392:8392:5", "PrefixLength": 64}]}
     2) Delete /redfish/v1/Managers/1/EthernetInterfaces/1/ with {"IPv6StaticAddresses":{"Address": "2001::8392:8392:8392:5/64", "PrefixLength": 64}} should not contain 2001::8392:8392:8392:5/64

22.Category: Enhancement
  Description:
    [ENGINEERING] - Added CPLD checking prior to performing rollback ID actions.
  Infected Motherboard: ALL
  Affected functions: Rollback ID
  Validation:
    1) Try performing rollback ID actions on a non-CPLD board.
    2) Rollback ID actions should not be allowed on non-CPLD board.

23. Category: Fix
  Description:
    [ENGINEERING] - Fixed bug where if user cancels BIOS update, the BIOS rollback ID from staging remains.
  Infected Motherboard: ALL
  Affected functions: BIOS Update
  Validation:
    1) Upload a BIOS firmware with a higher rollback ID than the one in CPLD.
    2) Cancel the update process.
    3) Try to manually update the BIOS rollback ID via raw 0x30 0x68 0x2a 0x2 0x1
    4) It should fail.
--------------------------------------------------------------------------------------------

Firmware Version: 00.00.08
Firmware Name: BMC_X12AST2600_ROT20_1301MS_20210412_00.00.08_TESsd.bin
Firmware CRC: 036C35E2
Firmware Name: BMC_X12AST2600_ROT20_1301MS-NOR_20210412_00.00.08_TESsd.bin
Firmware CRC: 2927E256
Firmware Name: BMC_X12AST2600_ROT20_1301MS-eMMC_20210412_00.00.08_TESsd.bin
Firmware CRC: C5DDA8B2
Build date: 04/12/2021
Supported Platform: X12DGQ-R
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_latest_06112020
-------------------------------------------------------------------------------

1. Category: Fix
   Description:
     [ENGINEERING] - BIOS cannot be update in 0.00.07
   Infected Motherboard: X12DGQ-R
   Affected functions: BIOS update
   Validation:
     1) BIOS update
-----------------------------------------------------------------------------------------------

Firmware Version: 00.00.07
Firmware Name: BMC_X12AST2600_ROT20_1301MS_20210410_00.00.07_TESsd.bin
Firmware CRC: 1375F13D
Firmware Name: BMC_X12AST2600_ROT20_1301MS-NOR_20210410_00.00.07_TESsd.bin
Firmware CRC: 2927E256
Firmware Name: BMC_X12AST2600_ROT20_1301MS-eMMC_20210410_00.00.07_TESsd.bin
Firmware CRC: 9C047D6A
Build date: 04/10/2021
Supported Platform: X12DGQ-R
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_latest_06112020
-------------------------------------------------------------------------------

1. Category: Fix
   Description:
     [124917] - Unavailable GPU thermal sensor reading on IPMI
   Infected Motherboard: X12DGQ-R
   Affected functions: GPU
   Validation:
     1) Check GPU sensor

2.Category: fix
  Description:
    [124334] - Intel P4610 NVMe no storage page on IPMI WEB
  Infected Motherboard: X12DGQ-R
  Affected functions: NVME
  Validation:
    1) verify storage WEBUI with Intel P4610 installed

3. Category: fix
   Description:
     [124873] - FAN speed not following Thermal Guideline
     [124916] - Fan RPM threshold does not match fan capability
   Infected Motherboard: X12DGQ-R
   Affected functions: FAN
   Validation:
     1) reset default and check Smart Power setting defaut enabled.

4. Category: Fix
   Description:
       [#123046] Fix - IPMI Web - Configuration - Network - IPv6 setting fail
   Infected Motherboard: ALL
   Affected functions: IPv6
   Validation:
   Testcase 1:
	1) Set Dhcp ipv6 mode to Disable and remove SLAAC ipaddr
	2) SLAAC IP address should be removed successfully.

5. Category: fix
   Description:
     [125176] - MEL lost after Filter and Severity are modified/changed...
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Log into web -> MEL -> change severity/filter freely

6. Category: fix
   Description:
     [125213] - IPMI Web CPU info tab doesn't match with X12 IPMI UI Spec
   Infected Motherboard: ALL
   Affected functions: CPU info
   Validation:
     1) Check CPU info tab "Max Speed" instead

7. Category: fix
   Description:
     [124648] - DNS_server2 default display correctly on web
   Infected Motherboard: ALL
   Affected functions: web
   Validation:
     1) log into web -> network
     2) Default server2 ip is 0.0.0.0

8. Category: fix
   Description: 
     [120019] HTML5 IKVM hotkey setting interface blank
   Infected Motherboard: ALL
   Affected functions: html5 ikvm
   Validation:
    1) Log into web -> remote -> html5 ikvm
    2) Go to options -> hotkey settings -> hotkey setting interface shows

9. Category: fix
   Description: 
     [ENGINEERING] Remove $(TAG_CS from health page after lockdown enable
   Infected Motherboard: ALL
   Affected functions: health_event page
   Validation:
    1) Log into web -> enable lockdown in bmc settings
    2) Go to health event log page
    3) Page looks ok with no extra text

10. Category: fix
   Description: 
     [123856] Memory page fix warning event
   Infected Motherboard: ALL
   Affected functions: memory web page
   Validation:
    1) Cause memory warning issue
    2) Log into web -> component info -> memory page
    3) Memory icon status is yellow cause of warning issue

11. Category: Fix
   Description:
     [124941] [SD5_5.11.0b1026] Product Key info not observed via command sdc.sh -pk but observed via smcipmitool w/ nodekey list comamnd
   Infected Motherboard: ALL
   Affected functions: License
   Validation:
     1) run SuperDoctor5 to check License

12. Category: fix
   Description:
     [124931] - Redfish SEL Health Server Status show "Failed to get SEL..."
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) get  redfish/v1/Systems/1/LogServices/Log1
     1) get  redfish/v1/managers/1/LogServices/Log1

13. Category: fix
   Description:
     [125006] - FD does not clear RADIUS server if RADIUS is disabled
   Infected Motherboard: ALL
   Affected functions: RADIUS
   Validation:
     1) configure RADIUS then do BMC reset default

14. Category: fix
   Description:
     [125008] - Cannot enable NTP using SMCIPMITool
   Infected Motherboard: ALL
   Affected functions: NTP
   Validation:
     1) SMCIPMITool ipmi oem x10cfg ntp state enable
     2) SMCIPMITool ipmi oem x10cfg ntp state.

15. Category: Fix
   Description:
     [ENGINEERING]Lock is now released after BIOS update completes.
   Infected Motherboard: ALL
   Affected functions: Firmware Update
   Validation:
     1) Update BIOS using EnterUpdateMode/Upload/Update method in Redfish
     2) Check TaskService for status of update.
     3) Once complete, the lock will automatically be released.

16. Category: Fix
   Description:
     [#124235] Fix - It got fail results via smstc att TC 137 IPMI Management - ipmi lan ipv6 - fail
   Infected Motherboard: ALL
   Affected functions: SMSTC TC137
   Validation:
     Testcase 1:
       1) Run TC137 pass

17. Category: Fix
   Description:
     [124939] [Smcipmitool_2.25.0b210326] not define the 0xDC events
   Infected Motherboard: ALL
   Affected functions: HEL
   Validation:
     1) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x00 0xff 0xff
     2) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x01 0xff 0xff
     3) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x02 0xff 0xff
     4) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x10 0xff 0xff
     5) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x11 0xff 0xff
     6) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x12 0xff 0xff
     7) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x20 0xff 0xff
     8) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x21 0xff 0xff
     9) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x22 0xff 0xff
     10) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x30 0xff 0xff
     11) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x31 0xff 0xff
     12) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x32 0xff 0xff
     13) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x40 0xff 0xff
     14) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x41 0xff 0xff
     15) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x42 0xff 0xff
     16) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x50 0xff 0xff
     17) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x51 0xff 0xff
     18) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x52 0xff 0xff
     19) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x60 0xff 0xff
     20) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x61 0xff 0xff
     21) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x62 0xff 0xff
     21) raw 0x4 0x02 0x01 0x4 0xdc 0xff 0x6f 0x63 0xff 0xff

18. Category: Fix
   Description:
     [123462] Redfish Automation Tool check fail.
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) Get redfish/v1/Chassis/1/PCIeSlots to check Lanes and ServiceLabel
     2) Get redfish/v1/Chassis/1/PCIeDevices/NIC1 to check PCIeInterface

19. Category: fix
   Description: 
     [124900] UI tables missing some info
   Infected Motherboard: ALL
   Affected functions: CPU, GPU, PSU, memory table
   Validation:
    1) Log into web -> go to CPU, GPU, PSU, memory page
    4) All info displayed no matter size of browser

20. Category: fix
   Description: 
     [124648] DNS server failed to save
   Infected Motherboard: ALL
   Affected functions: config_network
   Validation:
    1) Log into web -> configurations -> network
    2) Save new DNS server successfully

21. Category: Fix
   Description:
     [123362] - Session Timeout After Updating BIOS
   Infected Motherboard: ALL
   Affected functions: Firmware Update
   Validation:
     1) Update BIOS
     2) After completing the update, it should not bring user back to login page (or see session time out prompt).

22. Category: Fix
    Description:
      [ENGINEERING] fix - not support non 80 port of Mount Virtual Media function over http and MEL not send with event service
    Infected Motherboard: ALL
    Affected functions: Redfish and MEL
    Validation:
      Testcase 1:
        1) Go to Virtual Media website
        2) Input Share Host: http://{{IP}}:{{PORT}}
        3) Input Path to Image: ISO file path
        4) Input Username and Password if necessary
        5) Click Mount and Save
      Testcase 2:
        1) Set notification with protocol Redfish
        2) Clear health event log at System > Health Event Log page
        3) Check MEL is exist and receive MEL from redfish event service

23. Category: Fix
   Description:
     [124700] - BMC issue when run SUM with -scan rom option
   Infected Motherboard: ALL
   Affected functions: bios info
   Validation:
     1) raw 0x30 0x60 2 0 0 0 should show full data instead of hang

24. Category: fix
   Description: 
     [ENGINEERING] Web date/time turn ntp on fix/sync ssdp page
   Infected Motherboard: ALL
   Affected functions: date/time, ssdp page
   Validation:
    1) Log into web -> bmc settings -> set NTP enable successful
    2) Network -> SSDP -> set SSDP settings successful

25. Category: Fix
   Description:
     [123434] [DVT]BMC reset to Factory Default got Dedicated LAN Link Down / Link up event
   Infected Motherboard: All
   Affected functions: Event
   Validation:
     1) do factory default then check HEL should only one NIC Link Up event

26.Category: ENGINEERING
  Description:
    [ENGINEERING] - Support SFT-SDDC-SINGLE license activation.
  Infected Motherboard: ALL
  Affected Functions:   License Management
  Validation:
    1) Activate SDDC license via SUM activateproductkey command, it should work.
    2) Query SDDC license via SUM queryproductkey command, the SDDC license will be displayed.
    3) Deactivate SDDC license via SUM clearproductkey command, it should work
    4) Query license via SUM queryproductkey command, the SDDC license will be removed.
    4) Activate SDDC license from BMC WEB, it should work.

27.  Category: fix
    Description:
      [ENGINEERING] - Automated test fail - license permission fail
    Infected Motherboard: X12, H12, B12
    Affected functions: redfish
    Validation:
     1) No matter with or without product key.
       Try HTTP GET https://10.138.160.1/redfish/v1/UpdateService/Oem/Supermicro/SSLCert, it will succeed.

28. Category: Fix
   Description:
     [ENGINEERING] - BMC now picks up the correct IP based on the network interface and LAN mode being used.
   Infected Motherboard: ALL
   Affected functions: Network
   Validation:
     1) In one domain, plug ethernet into Shared LAN
     2) In another domain, plug ethernet into Dedicated Lan
     3) Update BMC without Preserve Configurations or Reset BMC to Default or Reset BMC
     4) Check "BMC Network Configurations" in BIOS to observe whether the "network link status" matches the IP
        obtained for that particular interface.

29. Category: Fix
   Description:
     [123947] [DVT]BMC Events for PSU Behavior different with X12 document "BMC_PSU_LAN_Plug_In_Out_Behavior_v1.3".
   Infected Motherboard: ALL
   Affected functions: PSU Event
   Validation:
     Follow test step in BMC_PSU_LAN_Plug_In_Out_Behavior_v1.3.docx

     Step:PSU Behavior:      Event log:                                             Power Fail LED:
     |---|------------------|------------------------------------------------------|--------------|
     |1.)|AC ON             |Info | Power Supply Installed – Assertion             |OFF           |
     |   |(PSU1             |                                                      |              |
     |   | & PSU2 Install)  |                                                      |              |
     |---|------------------|------------------------------------------------------|--------------|
     |2.)|Remove            |Warning | Power Supply Installed - Deassertion        |OFF           |
     |   |PSU1 Power Module |                                                      |              |
     |   |& Power Cord      |                                                      |              |
     |   |(at the same time)|                                                      |              |
     |---|------------------|------------------------------------------------------|--------------|
     |3.)|Install  PSU1     |Info | Power Supply Installed - Assertion             |Blink or Solid|
     |   |Power Module Only |Critical | Power Supply Failure detected – Assertion  |              |
     |   |                  |Critical | Power Supply Input lost (AC/DC) – Assertion|              |
     |---|------------------|------------------------------------------------------|--------------|
     |4.)|Install           |Info | Power Supply Failure detected – Deassertion    |OFF           |
     |   |PSU1 Power Cord   |Info | Power Supply Input lost (AC/DC) – Deassertion  |              |
     |---|------------------|------------------------------------------------------|--------------|
     |5.)|Remove PSU1       |Critical | Power Supply Failure detected – Assertion  |Blink or Solid|
     |   |Power Cord Only   |Critical | Power Supply Input lost (AC/DC) – Assertion|              |
     |---|------------------|------------------------------------------------------|--------------|
     |6.)|Remove PSU1       |Warning | Power Supply Installed – Deassertion        |OFF           |
     |   |Power Module      |Info | Power Supply Failure detected – Deassertion    |              |
     |   |                  |Info | Power Supply input lost (AC/DC) - Deassertion  |              |
     |---|------------------|------------------------------------------------------|--------------|
     |7.)|Install PSU1      |Info | Power Supply – Assertion                       |OFF           |
     |   |Power Module      |                                                      |              |
     |   |& Power Cord      |                                                      |              |
     |   |at the same time  |                                                      |              |
     |---|------------------|------------------------------------------------------|--------------|

30.  Category: Fix
    Description:
      [123122] Fix - Notifications alerts setting doesn't reload with IPMI configuration file. Copy Project Issue Link
    Infected Motherboard: ALL
    Affected functions: reload config
    Validation:
    Testcase 1:
	1) Modify settings in Notification>Alert page
	2) Download Config
	3) Reset to default
	4) Reload Config and compare with before settings

31. Category: Enhancement
   Description:
     [Enhancement]: Show the NVMe drive Temperature and PDLU;
   Infected Motherboard: all
   Affected functions: Storage.
   Validation:
     1) Install any NVMe drive which supports the NVMe-MI;
     2) Check the drive detail info on the storage physical view web page;
-----------------------------------------------------------------------------------------

Firmware Version: 00.00.06
Firmware Name: BMC_X12AST2600_ROT20_1301MS_202103174_00.00.06_TESsd.bin
Firmware CRC: 9B17AC4D
Firmware Name: BMC_X12AST2600_ROT20_1301MS-NOR_20210317_00.00.06_TESsd.bin
Firmware CRC: 951D7489
Firmware Name: BMC_X12AST2600_ROT20_1301MS-eMMC_20210317_00.00.06_TESsd.bin
Firmware CRC: 13D66FC2
Build date: 03/17/2021
Supported Platform: X12DGQ-R
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_latest_06112020
-------------------------------------------------------------------------------
1. Category: fix
   Description:
     [[ENGINEERING]] - AST2600-A2 support, fix sol issue
   Infected Motherboard: X12DGQ-R
   Affected functions: ALL
   Validation:
     1) SOL function

2. Category: fix
   Description: 
     [ENGINEERING] success message clickable after 1 sec
   Infected Motherboard: ALL
   Affected functions: all web
   Validation:
    1) Log into web -> change any configurations
    2) Green success message only clickable after 1 sec
 
3. Category: fix
   Description: 
     [ENGINEERING] Mntc event log mis colored severity
   Infected Motherboard: ALL
   Affected functions: mntc_fevent
   Validation:
    1) Log into web -> Check mel color severity correct

4. Category: fix
   Description:
     [ALL] fix - enable/disable button for maintenance event log on web page might
     not work properly after rebooting BMC
   Infected Motherboard: All
   Affected functions: Maintenance log enable/disable
   Validation:
     1) Enable or disable it
     2) Reboot BMC right away
     3) Expect to see the setting remains after BMC reboot

-----------------------------------------------------------------------------------------

Firmware Version: 00.00.05
Firmware Name: BMC_X12AST2600_ROT20_1301MS_20210204_00.00.05_TESsd.bin
Firmware CRC: 3EB46A79
Firmware Name: BMC_X12AST2600_ROT20_1301MS-NOR_20210204_00.00.05_TESsd.bin
Firmware CRC: 5CC76D50
Firmware Name: BMC_X12AST2600_ROT20_1301MS-eMMC_20210204_00.00.05_TESsd.bin
Firmware CRC: E8031BA3
Build date: 02/04/2021
Supported Platform: X12DGQ-R
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_latest_06112020
-------------------------------------------------------------------------------
1. Category: New
   Description: Enable GUI to support update BIOS without PCH reset

2. Category: New
   Description: Operate uboot env through TeeOS  

3. Category: Fix
   Description: Need to work with CPLD F2.04.08; add workaround for ast2600a1 
                integrity check random fail

-----------------------------------------------------------------------------------------

Firmware Version: 00.00.04
BMC Firmware Name: BMC_X12AST2600_ROT20_1301MS_20210127_00.00.04_TESsd.bin
BMC Firmware CRC: 11837558
NOR Firmware Name: BMC_X12AST2600_ROT20_1301MS-NOR_20210127_00.00.04_TESsd.bin
NOR Firmware CRC: 7A91084A
EMMC Firmware Name: BMC_X12AST2600_ROT20_1301MS-eMMC_20210127_00.00.04_TESsd.bin
EMMC Firmware CRC: 7953FD95
Build date: 01/27/2021
Supported Platform: X12DGQ-R
Redfish API : Redfish API : X12_Redfish_1_80_API_full_list_latest_06112020
-------------------------------------------------------------------------------

Firmware Version: 0.20.01
Firmware Name: BMC_X12AST2600-ROT20-1301MS__20201230_00.20.01_STDsd.bin
Firmware CRC: 9D0D48B4
BootLoader Name: BootLoader_X12AST2600-ROT20-NOR-1301MS_20201230_00.20.01_STDsd.bin
BootLoader CRC: D67B30D2
Build date: 12/30/2020
Redfish API : X12_Redfish_1_80_API_full_list_latest_06112020
TEE OS Version: 9999.01.05 CA: 05 Signtool: 07
Supported Platform: X12DGQ-R
------------------------------------------------------------------

1. Category: new
   Description:
     [[ENGINEERING]] - support X12DGQ-R
   Infected Motherboard: X12DGQ-R
   Affected functions: ALL
   Validation:
     1) ALL functions
--------------------------------------------------------------------------------------------