Supermicro Update Manager (for UEFI BIOS) 1.3.0 (2022/04/21) (UEFI)

Introduction
  The Supermicro Update Manager (SUM) UEFI can be used to manage the system BIOS
  and BMC firmware image update for X12/H12 and later platforms except H12 non-RoT
  systems under EFI shell.

The package includes:
  - SUM.efi
  - README.txt
  - ReleaseNote.txt

==============================================================================================================================
==============================================================================================================================

SYNOPSIS
  SUM.efi [OPTIONs] [COMMAND] [COMMAND ARGUMENTS]

Help Message
  SUM.efi (Shows help information)
  SUM.efi -h/H (Shows help information)
  SUM.efi -h/H -c <Command name> (Shows help information for each command)

OPTIONs
  -I        Redfish_HI
  -u        <BMC user ID>
  -p        <BMC user password>
  -c        <Command name>

COMMANDS
  UpdateBios, GetBiosInfo, BiosRotManage, UpdateBmc, GetBmcInfo, BmcRotManage
            
COMMAND ARGUMENTS
  Required and optional arguments of each commands. 
  For detail information of each command, please refer to section below.

------------------------------------------------------------------------------------------------------------------------------
UpdateBios command:

Description
  Updates BIOS.

Example
  FS0:\> SUM.efi -I Redfish_HI -u ADMIN -p ADMIN -c UpdateBios --file BIOS.rom --reboot [Optional Arguments]

Required Arguments
  --file        BIOS image file
  --reboot      Forces the managed system to reboot or power up after operation

Optional Arguments
  --flash_smbios         Overwrites the SMBIOS data
  --preserve_nv          Preserves the NVRAM region
  --preserve_mer         Preserves the ME firmware region
  --backup               Backups current running BMC image. (Only support for RoT systems)
  --forward              Confirms the Rollback ID forward (Only support X12/H12 and later platforms except the H12 non-RoT systems)

Node Product Key Required
  No

Note: flash_smbios and preserve_nv optional arguments cannot be used at the same time.

==============================================================================================================================

UpdateBmc command:

Description
  Updates BMC.

Example
  SUM.efi -I Redfish_HI -u ADMIN -p ADMIN -c UpdateBmc --file BMC.rom [Optional Arguments]

Required Arguments
  --file    BMC image file

Optional Arguments
  --overwrite_cfg        Overwrites the current BMC configuration using the factory default values in the given BMC image file
  --overwrite_sdr        Overwrites current BMC SDR data
  --backup               Backups current running BMC image. (Only support for RoT systems)
  --forward              Confirms the Rollback ID forward (Only support X12/H12 and later platforms except the H12 non-RoT systems)

Node Product Key Required
  No

==============================================================================================================================

GetBiosInfo command:

Description
  Gets system BIOS information of the managed system.

Example
  SUM.efi -I Redfish_HI -u ADMIN -p ADMIN -c GetBiosInfo

Required Arguments
  N/A

Optional Arguments
  N/A

Node Product Key Required
  No

==============================================================================================================================

GetBmcInfo command:

Description
  Gets system BMC information of the managed system.

Example
  SUM.efi -I Redfish_HI -u ADMIN -p ADMIN -c GetBmcInfo 

Required Arguments
  N/A

Optional Arguments
  N/A

Node Product Key Required
  No

==============================================================================================================================

BiosRotManage command:

Description
  Execute Rot relate actions.

Example
  SUM.efi -I Redfish_HI -u ADMIN -p ADMIN -c BiosRotManage --action UpdateGolden

Required Arguments
  --action
        Sets action to:
	    1 = GetInfo
	    2 = UpdateGolden
	    3 = Recover

Optional Arguments
  N/A

Node Product Key Required
  No
  SFT-DCMS-SINGLE for action recover
  
Note: UpdateGolden action will overwrite golden image with current BIOS firmware.

==============================================================================================================================

BmcRotManage command:

Description
  Execute Rot related actions.

Example
  SUM.efi -I Redfish_HI -u ADMIN -p ADMIN -c BmcRotManage --action UpdateGolden

Required Arguments
  --action
        Sets action to:
	    1 = GetInfo
	    2 = UpdateGolden
	    3 = Recover

Optional Arguments
  N/A

Node Product Key Required
  No
  SFT-DCMS-SINGLE for action recover
  
Note: UpdateGolden action will overwrite golden image with current BMC firmware.