Firmware Version: 2.09.01-18
Firmware Name: obmc_smci_fda_r12spd_v2.9.1-18_20220630.bin
Build date: 06/30/2022
Supported Platform: R12SPD
Intel commit source: https://github.com/Intel-BMC/openbmc
Intel commit number: 7cf0c1cd0ce835d1833509b7b911e8a97380278b 
-------------------------------------------------------------------------
Note #1: Please reference "R12SPD OpenBMC Software Functional Specification_v08.pdf"
Note #2: obmc_smci_fda_r12spd_v2.9.1-18_20220630.mtd.tar is update file for WebUI and Redfish
Note #3: obmc_smci_fda_r12spd_v2.9.1-18_20220630.bin can update by uboot tftp and burn tool directly
Note #4: Support Redfish-Service-Validator v2.1.6 and 2022.1 Redfish Schema

1. Category: fix
   Description:
   [142689] fix - DHCP switch static IP,SUT can not connect
   [141811] fix - The System can't access BMC WEB UI the BMC IP Subnet Mask needs help check
   [141189] fix - BMC Switching to Shared LAN Despite Dedicated LAN Being Active (Phy still marked up; has link)
   Infected Motherboard: ALL
   Affected functions: Riser Card
   Validation:
     1. keep bmc on dhcp mode
     2. do DC on/off
     3. wait entry uefi complete
     4. use office subnet to ping target unit on lab subnet

2. Category: fix
   Description:
   [141517] fix - After NVMe hot plug, NVMe information will be left in IPMI web
   Infected Motherboard: ALL
   Affected functions: NVMe
   Validation:
     1. Please rework HW first
     2. setup BPN-SAS3-LA26A-N12 + Riser RSC-D2-668G5 + RSC-D2-66G4 + AOC-S3816L-L16IT (RD environment)
     3. wait bios post complete
     4. plugout NVMe, please wait more than 12s to look at FRU and Temperature
     5. plugin NVMe in others slot, wait more than 12s to look at FRU and Temperature


=======================================================================================================
Firmware Version: 2.09.01-17
Firmware Name: obmc_smci_fda_r12spd_v2.9.1-17_20220623.bin
Build date: 06/23/2022
Supported Platform: R12SPD
Intel commit source: https://github.com/Intel-BMC/openbmc
Intel commit number: 7cf0c1cd0ce835d1833509b7b911e8a97380278b 
-------------------------------------------------------------------------
Note #1: Please reference "R12SPD OpenBMC Software Functional Specification_v08.pdf"
Note #2: obmc_smci_fda_r12spd_v2.9.1-17_20220623.mtd.tar is update file for WebUI and Redfish
Note #3: obmc_smci_fda_r12spd_v2.9.1-17_20220623.bin can update by uboot tftp and burn tool directly
Note #4: Support Redfish-Service-Validator v2.1.6 and 2022.1 Redfish Schema

1. Category: fix
   Description:
   [ENGINEER] fix - Insert the same riser card causes the service to automatically detect conflicts.
   Infected Motherboard: ALL
   Affected functions: Riser Card
   Validation:
     1. insert two RSC-D2-66G4 Riser in different PCIE slots
     2. insert AOC-LAN to different Riser Card
     3. check sensor list has AOC temperature sensor


=======================================================================================================
Firmware Version: 2.09.01-16
Firmware Name: obmc_smci_fda_r12spd_v2.9.1-16_20220621.bin
Build date: 06/21/2022
Supported Platform: R12SPD
Intel commit source: https://github.com/Intel-BMC/openbmc
Intel commit number: 7cf0c1cd0ce835d1833509b7b911e8a97380278b 
-------------------------------------------------------------------------
Note #1: Please reference "R12SPD OpenBMC Software Functional Specification_v08.pdf"
Note #2: obmc_smci_fda_r12spd_v2.9.1-16_20220621.mtd.tar is update file for WebUI and Redfish
Note #3: obmc_smci_fda_r12spd_v2.9.1-16_20220621.bin can update by uboot tftp and burn tool directly
Note #4: Support Redfish-Service-Validator v2.1.6 and 2022.1 Redfish Schema

1. Category: fix
   Description:
   [141189] fix - BMC Switching to Shared LAN Despite Dedicated LAN Being Active (Phy still marked up; has link)
   Infected Motherboard: ALL
   Affected functions: onboard share lan
   Validation:
     case 1: Check NCSI link status
        1. Plug in onboard share lan cable.
        2. Check eth0 is up.
        # cat /sys/class/net/eth0/carrier
          1
        3. plug out onboard share lan cable.
        4. Check eth0 is down.
        # cat /sys/class/net/eth0/carrier
          0
     case2: Check onboard share lan failover on different channels.
        1. Plug in cables into channel 0 and channel 1.
        2. Plug out channel 0 cable. Check link is switching to channel 1.
        3. Plug out channel 1 cable. Check the interface is link down.
        4. Plug in cables into channel 0 or channel 1.
        5. Check the interface is link up.
        6. Plug only one cable into channel 0 or channel 1.
        7. Do a AC cycle
        8. Check the interface is link up after BMC eady.
        9. Plug out this cable then plug into another channels
       10. Check the interface is link up again.

2. Category: fix
   Description:
   [140027] fix - Can't sensor GPU T4 and A100 sensor reading
   Infected Motherboard: ALL
   Affected functions: GPU
   Validation:
     1. insert 4 Nvidia T4 GPU cards
        - 2 MB PCIE solts + 2 RSC-D2-668G5 PCIE slots
     2. check sensor temperature on WebUI

3. Category: fix
   Description:
   [enhancement] change get thermal trip way 
   Infected Motherboard: ALL
   Affected functions: thermal trip
   Validation:
     1. please consult with HW to get the newest CPLD firmware
     2. run "stress-ng cpu 128" to burn cpu
     3. check thermal trip log


=======================================================================================================
Firmware Version: 2.09.01-15
Firmware Name: obmc_smci_fda_r12spd_v2.9.1-15_20220620.bin
Build date: 06/20/2022
Supported Platform: R12SPD
Intel commit source: https://github.com/Intel-BMC/openbmc
Intel commit number: 7cf0c1cd0ce835d1833509b7b911e8a97380278b 
-------------------------------------------------------------------------
Note #1: Please reference "R12SPD OpenBMC Software Functional Specification_v07.pdf"
Note #2: obmc_smci_fda_r12spd_v2.9.1-15_20220620.mtd.tar is update file for WebUI and Redfish
Note #3: obmc_smci_fda_r12spd_v2.9.1-15_20220620.bin can update by uboot tftp and burn tool directly
Note #4: Support Redfish-Service-Validator v2.1.6 and 2022.1 Redfish Schema

1. Category: fix
   Description:
   [141745] fix - After NVMe hot plug, NVMe information will be left in IPMI web Copy Project Issue Link
   Infected Motherboard: ALL
   Affected functions: NVMe
   Validation:
     1. ac power on
     2. wait system post complete
     3. plugout NVMe, please wait more than 14s to look at FRU and Temperature
     4. plugin NVMe in others slot, wait more than 14s to look at FRU and Temperature

2. Category: fix
   Description:
   [141022] fix - When trigger Power failed the BMC WEB UI Power module healthy still shows OK
   [141026] fix - sensor status behavior was different from other module sensors
   Infected Motherboard: ALL
   Affected functions: PSU sensor status
   Validation:
     1. ac/dc power on
     2. wait system post complete
     3. remove power module or power cable
     4. look at power healthy status and icon

3. Category: fix
   Description:
   [142294] fix - System will generate lots of event logs when installed riser RSC-X-6G4
   Infected Motherboard: ALL
   Affected functions: Event logs
   Validation:
     1. install RSC-X-6G4
     2. wait system post complete
     3. look at WebUI Logs -> Event logs


=======================================================================================================
Firmware Version: 2.09.01-14
Firmware Name: obmc_smci_fda_r12spd_v2.9.1-14_20220615.bin
Build date: 06/15/2022
Supported Platform: R12SPD
Intel commit source: https://github.com/Intel-BMC/openbmc
Intel commit number: 7cf0c1cd0ce835d1833509b7b911e8a97380278b 
-------------------------------------------------------------------------
Note #1: Please reference "R12SPD OpenBMC Software Functional Specification_v07.pdf"
Note #2: obmc_smci_fda_r12spd_v2.9.1-14_20220615.mtd.tar is update file for WebUI and Redfish
Note #3: obmc_smci_fda_r12spd_v2.9.1-14_20220615.bin can update by uboot tftp and burn tool directly
Note #4: Support Redfish-Service-Validator v2.1.6 and 2022.1 Redfish Schema

1. Category: fix
   Description:
   [141759] fix - No AOC NIC card sensor reading
   [140738] fix - There is no AOC_M.2 sensor when insert AOC-SLG3-2M2
   Infected Motherboard: ALL
   Affected functions: AOC NIC
   Validation:
     1. power on system and wait post complete
     2. check webui sensor: Hardware status -> Sensors -> "M.2 SSD X Temp"

2. Category: fix
   Description:
   [141630] fix - No U.2 NVME Device Temp in WEB UI Sensor 
   Infected Motherboard: ALL
   Affected functions: NVME
   Validation:
     1. power on system and wait post complete
     2. check webui sensor: Hardware status -> Sensors -> "NVMe X Temp"
     3. check nvme info: Hardware status -> "Inventory and LEDs" -> Chassis -> "NVMe_X"

3. Category: fix
   Description:
   [142068] fix - SDHM test fail
   Infected Motherboard: ALL
   Affected functions: host interface
   Validation:
     1. install arm base ipmitool and ipmicfg_.134.0_220615
     2. run ipmitool sdr on system OS
     3. run ipmicfg.arm64 -sdr on system OS

4. Category: enhancement
   Description:
   [ENGINEER] fix - unexpected Bios and PostCodes Actions api response.
   Infected Motherboard: ALL
   Affected functions: redfish
   Validation:
     1. /redfish/v1/Systems/system/Bios/Actions/Bios.ResetBios
        1. Send a post request
        2. Get 400 bad request
        3. Severity is Warning
     2. /redfish/v1/Systems/system/LogServices/PostCodes/Actions/LogService.ClearLog
        1. Send a post request
        2. Get 200 OK
        3. Response body should not be empty

5. Category: enhancement
   Description:
   [ENGINEER] fix - service validator on account service and OEM virtual media item
   /redfish/v1/AccountService
   /redfish/v1/Managers/bmc/VirtualMedia/<device>
   Need an odata.id for Oem/OpenBMC property to pass Redfish service validator
   Infected Motherboard: ALL
   Affected functions: redfish
   Validation:
     1. run Redfish service validator 2.1.6 with DSP8010_2022.1.
     2. not fails with:
        ERROR - OpenBMC: EntityType resource does not contain required
        @odata.id property, attempting default /OpenBMC


=======================================================================================================
Firmware Version: 2.09.01-13
Firmware Name: obmc_smci_fda_r12spd_v2.9.1-13_20220609.bin
Build date: 06/09/2022
Supported Platform: R12SPD
Intel commit source: https://github.com/Intel-BMC/openbmc
Intel commit number: 7cf0c1cd0ce835d1833509b7b911e8a97380278b 
-------------------------------------------------------------------------
Note #1: Please reference "R12SPD OpenBMC Software Functional Specification_v07.pdf"
Note #2: obmc_smci_fda_r12spd_v2.9.1-13_20220609.mtd.tar is update file for WebUI and Redfish
Note #3: obmc_smci_fda_r12spd_v2.9.1-13_20220609.bin can update by uboot tftp and burn tool directly

1. Category: fix
   Description:
   [ENGINEER] fix - modify default LED state of RTL8211F
   Infected Motherboard: ALL
   Affected functions: Dedicate LED
   Validation:
     1. ac power on
     2. wait system post ready
     3. Check the Link LED is solid and the Activity LED is blinking

2. Category: fix
   Description:
   [ENGINEER] fix - updated fan support capability
   Infected Motherboard: ALL
   Affected functions: fan control
   Validation:
     1. check capability: ipmitool raw 0x30 0x45 0x02
     2. R12SPD only support std and full speed mode

3. Category: enhancement
   Description:
   [ENGINEER] add get/set bios factory default - 0x3c 0x20 [option]
   Infected Motherboard: ALL
   Affected functions: bios
   Validation:
     1. get bios default
        ipmitool raw 0x3c 0x20 0
     2. enable bios default
        ipmitool raw 0x3c 0x20 1 1
     3. disable bios default
        ipmitool raw 0x3c 0x20 1 0

2. Category: fix
   Description:
   [ENGINEER] fix - match ipmi spec. for user control
   Infected Motherboard: ALL
   Affected functions: user
   Validation:
     Case 1:
        Check default root account is ID 2.
        1. ipmitool -H $BMC_IP -U root -P 0penBmc -I lanplus user list
     Case 2:
        Check new user is append from ID 3 with WebUI
        1. Login WebUI
        2. Security and access > User management > Add user
        3. ipmitool -H $BMC_IP -U root -P 0penBmc -I lanplus user list
        3. New user is ID 3.
    Case 3:
        Modify user id 3 of username by IPMI
        1. ipmitool -H $BMC_IP -U root -P 0penBmc -I lanplus user set name 3 smci3
        2. Login WebUI with smci3
    Case 4:
        Modify user id 3 of password by IPMI
        1. ipmitool -H $BMC_IP -U root -P 0penBmc -I lanplus user set password 3 Supermicro1993
        2. Login WebUI with smci3
        3. Test IPMI command with smci3
           ipmitool -H $BMC_IP -U smci3 -P Supermicro1993 -I lanplus raw 0x06 0x01
    Case 5:
        Add user at user id 16 by IPMI
        1. ipmitool -H $BMC_IP -U root -P 0penBmc -I lanplus user set name 16 smci16
        2. ipmitool -H $BMC_IP -U root -P 0penBmc -I lanplus user list
        3. Set password
            ipmitool -H $BMC_IP -U root -P 0penBmc -I lanplus raw 0x06 0x47 0x10 0x02 0x53 0x75 0x70 0x65 0x72 0x6d 0x69 0x63 0x72 0x6f 0x31 0x39 0x39 0x33 0x00 0x00
        4. Enable User ID 16
            ipmitool -H $BMC_IP -U root -P 0penBmc -I lanplus raw 0x06 0x47 0x10 0x01
        5. Set access privilege
            ipmitool -H $BMC_IP -U root -P 0penBmc -I lanplus channel setaccess 1 16 ipmi=on link=on privilege=2
        6. Test IPMI command
            ipmitool -H $BMC_IP -U smci16 -P Supermicro1993 -I lanplus -L USER raw 0x06 0x01
        7. Test WebUI Login
            smci16/Supermicro1993
    Case 6:
        Test permanent setting
        1. AC cycle
        2. Test IPMI command
            ipmitool -H $BMC_IP -U smci16 -P Supermicro1993 -I lanplus -L USER raw 0x06 0x01
        3. Test WebUI Login
    Case 7:
        User ID 1 protection (anonymous user)
        1. Should be disable to modify username
            ipmitool -H $BMC_IP -U root -P 0penBmc -I lanplus user set name 1 anonymous
        2. Should be disable to modify password
            ipmitool -H $BMC_IP -U root -P 0penBmc -I lanplus user set password 1 Supermicro1993
    Case 8:
        Max user count is 16 (anonymous + 15 users)
        1. Login WebUI
        2. Security and access > User management > Add user
        3. Should not be able to add 16th user at WebUI


=======================================================================================================
Firmware Version: 2.09.01-12
Firmware Name: obmc_smci_fda_r12spd_v2.9.1-12_20220606.bin
Build date: 06/06/2022
Supported Platform: R12SPD
Intel commit source: https://github.com/Intel-BMC/openbmc
Intel commit number: 7cf0c1cd0ce835d1833509b7b911e8a97380278b 
-------------------------------------------------------------------------
Note #1: Please reference "R12SPD OpenBMC Software Functional Specification_v07.pdf"
Note #2: obmc_smci_fda_r12spd_v2.9.1-12_20220606.mtd.tar is update file for WebUI and Redfish
Note #3: obmc_smci_fda_r12spd_v2.9.1-12_20220606.bin can update by uboot tftp and burn tool directly

1. Category: fix
   Description:
   [141743] fix - VBAT will display Warning under sensor reading
   Infected Motherboard: ALL
   Affected functions: sensor
   Validation:
     1. check VBAT sensor threshold
     2. change new BAT to look at the sensor status

2. Category: fix
   Description:
   [140751] fix - No CPU Thermal Trip event log
   Infected Motherboard: ALL
   Affected functions: thermal trip
   Validation:
     1. need to update CPLD to R12SPD_101_v5
     2. run stress tool: ex stress-ng cpu 128
     3. look at the event log

3. Category: enhancement
   Description:
   [ENGINEER] add "Set Front Panel LED Control" - 0x30 0x70 0x65 [option]
   Infected Motherboard: ALL
   Affected functions: LED
   Validation:
     1. led off
     ipmitool raw 0x30 0x70 0x65 0
     2. led on
     ipmitool raw 0x30 0x70 0x65 1
     3. fan fail
     ipmitool raw 0x30 0x70 0x65 2
     4. power fail
     ipmitool raw 0x30 0x70 0x65 3

4. Category: enhancement
   Description:
   [ENGINEER] add get/set fan mode - 0x30 0x45 [option]
   Infected Motherboard: ALL
   Affected functions: fan
   Validation:
     1. get fan mode
     ipmitool raw 0x30 0x45 0
     2. set fan mode
     ipmitool raw 0x30 0x45 1 0 //stand mode
     ipmitool raw 0x30 0x45 1 1 //full speed mode
     3. get fan mode capability
     ipmitool raw 0x30 0x45 2
     4. get fan zon pwm and value
     ipmitool raw 0x30 0x45 3

5. Category: enhancement
   Description:
   [ENGINEER] add get/set HID LED mode - 0x30 0x0c/0x0d/0x0e
   Infected Motherboard: ALL
   Affected functions: HID LED
   Validation:
     1. get HID status
     ipmitool raw 0x30 0x0c
     2. set HID LED on
     ipmitool raw 0x30 0x0d
     3. set HID LED off
     ipmitool raw 0x30 0x0e


=======================================================================================================
Firmware Version: 2.09.01-11
Firmware Name: obmc_smci_fda_r12spd_v2.9.1-11_20220527.bin
Build date: 05/27/2022
Supported Platform: R12SPD
Intel commit source: https://github.com/Intel-BMC/openbmc
Intel commit number: 7cf0c1cd0ce835d1833509b7b911e8a97380278b 
-------------------------------------------------------------------------
Note #1: Please reference "R12SPD OpenBMC Software Functional Specification_v07.pdf"
Note #2: obmc_smci_fda_r12spd_v2.9.1-11_20220527.mtd.tar is update file for WebUI and Redfish
Note #3: obmc_smci_fda_r12spd_v2.9.1-11_20220527.bin can update by uboot tftp and burn tool directly

1. Category: fix
   Description:
   [139200] fix - No tool to modify the system FRU data
   Infected Motherboard: ALL
   Affected functions: fru
   Validation:
     1. Write partial FRU info by smcipmitool
     SMCIPMITool <BMCIP> root 0penBmc ipmi fruw <field> <string>
     <field> can be: CP,CS,BM,BPN,BS,BP,PM,PN,PPM,PV,PS,PAT
     e.g.
     ./SMCIPMITool <BMCIP> root 0penBmc ipmi fruw PAT Test125433
     2. Reboot BMC or AC power cycle
     3. Check FRU data is kept.
     4. Write whole FRU data by ipmitool. Check function is working.
     >> ipmitool fru write 0 R12_test_FRU.bin
     5. Get whole FRU data by ipmitool. Check function is working.
     >> ipmitool fru read 0 R12_test_FRU.bin

2. Category: fix
   Description:
   [138641] fix - FAN curve incorrect when system
   [136678] fix - The FAN6 connector is no function
   Infected Motherboard: ALL
   Affected functions: fan control
   Validation:
     ipmitool raw 0x30 0x70 0x066 [option][zone][duty]
	 option: 0:get, 1:set, 2:disable smart fan, 4:recover smart fan
     1. Get zone 0 pwm: ipmitool raw 0x30 0x70 0x66 0 0
     2. Get zone 1 pwm: ipmitool raw 0x30 0x70 0x66 0 1
     3. Get zone 2 pwm: ipmitool raw 0x30 0x70 0x66 0 2
     4. Get zone 3 pwm: ipmitool raw 0x30 0x70 0x66 0 3
	 5. Disable smart fan: ipmitool raw 0x30 0x70 0x66 2
	 6. Set zone 0 fan duty 100: ipmitool raw 0x30 0x70 0x66 1 0 0x64
	 7. Set zone 1 fan duty 100: ipmitool raw 0x30 0x70 0x66 1 1 0x64
	 8. Set zone 2 fan duty 100: ipmitool raw 0x30 0x70 0x66 1 2 0x64
	 9. Set zone 3 fan duty 100: ipmitool raw 0x30 0x70 0x66 1 3 0x64
	 10.Recover smart fan: ipmitool raw 0x30 0x70 0x66 4

3. Category: fix
   Description:
   [138656] fix - No chassis intrusion event log in the IPMI GUI.
   Infected Motherboard: ALL
   Affected functions: intrusion log
   Validation:
     1. HW v1.01 support
     2. short the chassis intrusion jumper
	 3. plug out jumper
	 4. check event log

=======================================================================================================
Firmware Version: 2.09.01-10
Firmware Name: obmc_smci_fda_r12spd_v2.9.1-10_20220524.bin
Build date: 05/24/2022
Supported Platform: R12SPD
Intel commit source: https://github.com/Intel-BMC/openbmc
Intel commit number: 7cf0c1cd0ce835d1833509b7b911e8a97380278b 
-------------------------------------------------------------------------
Note #1: Please reference "R12SPD OpenBMC Software Functional Specification_v07.pdf"
Note #2: obmc_smci_fda_r12spd_v2.9.1-10_20220524.mtd.tar is update file for WebUI and Redfish
Note #3: obmc_smci_fda_r12spd_v2.9.1-10_20220524.bin can update by uboot tftp and burn tool directly


1. Category: enhancement (bmc internal test, lab ignore)
   Description:
   [Enhancement] fix - auto set BMC's shared LAN MAC address by adding 1 to NCSI NIC's base MAC address
   Infected Motherboard: ALL
   Affected functions: share-nic
   Validation:
     1. Set eth0/eth1/eth2 MAC address by ipmitool
     2. AC power off. Plug in a AIOM card.
     3. AC power o
     4. Type ifconfig. Check if the eth0/eth2 MAC address is as settings, not adding 1 to NCSI NIC's base MAC address.
     5.Do network factory reset.
       5.1 busctl call xyz.openbmc_project.Network /xyz/openbmc_project/network xyz.openbmc_project.Common.FactoryReset Reset
       5.2 systemctl restart systemd-networkd
     6. check if the eth0/eth1/eth2 MAC address is kept.
    Note:
    eth1:  (bmc mac)
    ipmitool raw 0x0c 0x01 1 5 <MAC>
    eth0: (on board share mac)
    ipmitool raw 0x0c 0x01 2 5 <MAC>
    eth2: (aiom share mac)
    ipmitool raw 0x0c 0x01 3 5 <MAC>

2. Category: fix
   Description:
   [140751] fix - No CPU Thermal Trip event log
   Infected Motherboard: ALL
   Affected functions: thermal trip
   Validation:
     1. power on the system
     2. run "stress-ng --cpu 128" on ARM OS   #stress 128 cores
     3. wait for the cpu temperature up to 114 degree
     4. check event log on webui when power off

3. Category: fix
   Description:
   [141239] fix - PSU2 failed description typo under bmc event logs
   Infected Motherboard: ALL
   Affected functions: event log
   Validation:
     1. plugout power cable
     2. check message info of event log

4. Category: fix
   Description:
   [138660] fix - storage monitoring item not found on IPMI web
   [140737] fix - NVMe sensor reading and inventory info is incorrect
   Infected Motherboard: ALL
   Affected functions: NVMe
   Validation:
     1. insert NVMe from Intel, Samsung and Kioxia into BPN.
     2. AC power on.
     3. Check the hardware information in the WebUI and confirm the data

5. Category: fix
   Description:
   [140164] fix - There are no DIMM slot, Fans and Processors information in Inventory and LEDs page
   Infected Motherboard: ALL
   Affected functions: HW information
   Validation:
     1. AC power on
     2. Check the hardware information in the WebUI and confirm that the processor,
        memory and NVMe information are correct

6. Category: fix
   Description:
   [140330] fix - Not able to disable Network services 
   Infected Motherboard: ALL
   Affected functions: network services
   Validation:
     1. login WebUI
     2. Go to Security and access > Policies
     3. Turn off SSH button and refresh page
     4. Expected result: SSH button is disabled and IPMI button is enabled


=======================================================================================================
Firmware Version: 2.09.01-9
Firmware Name: obmc_smci_fda_r12spd_v2.9.1-9_20220518.bin
Build date: 05/18/2022
Supported Platform: R12SPD
Intel commit source: https://github.com/Intel-BMC/openbmc
Intel commit number: 7cf0c1cd0ce835d1833509b7b911e8a97380278b 
-------------------------------------------------------------------------
Note #1: Please reference "R12SPD OpenBMC Software Functional Specification_v07.pdf"
Note #2: obmc_smci_fda_r12spd_v2.9.1-9_20220518.mtd.tar is update file for WebUI and Redfish
Note #3: obmc_smci_fda_r12spd_v2.9.1-9_20220518.bin can update by uboot tftp and burn tool directly


1. Category: enhancement
   Description:
   [Enhancement] add read cpld version
   Infected Motherboard: ALL
   Affected functions: no
   Validation:
     1. ipmitool raw 0x30 0x68 0x29  #read CPLD version

2. Category: fix
   Description:
   [139855] fix - Power Failed LED is not working
   Infected Motherboard: ALL
   Affected functions: system led
   Validation:
     1. plugout fan
     2. look at the system led freq (1Hz)
     3. plugout power cable
     4. look at the fail led freq (0.25Hz)
     5. recover fan, the system led still keep power fail led freq.
     6. recover power cable
     7. the system led returns to normal state.

