==============================================================================================================================
Filename: BMC_X12AST2600-nonROT-F201MS_20210902_0.13.13_STDsp.bin version: 0.13.13 Date: 09-02-2021
U-Boot build time :
Java SOL Viewer version : v0.5.15
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_07302021

1.
        Category: Fix
        Description:
            [129885] There is a mis-leaded ghost “LAN” MAC address=00.00.00.00.00.00 from BMC Web GUI. (Remove MicroLP card)

        Impact motherboard:
            X12STE-F

        Affected functions:
        Validation:
            1. Remove MLP Card from MB.
            2. WebGUI > Check if system mac address field appeares or not.
2.
        Category: Fix
        Description:
            [130246] Dynamic DNS not works.

        Impact motherboard:
            X12STL-IF

        Affected functions:
        Validation:
            1. Go to network page, config dns server 10.135.15.195 on DNS Server2 IP
            2. Go to BMC Seetings page, cofig ntp server "tock.stdtime.gov.tw" and save
            3. Go to Dynamic DNS page, enable, and config DDNS server with 10.135.15.195
            4. config BMC Hostname with "x12.ddns.local", "ddns.lcoal" is requred
            5. Upload TSIG files and save
            6. Login web with https://x12.ddns.local
3.
        Category: Fix
        Description:
            [130158] [IPMI ECO 00.13.11] IPMI ECO automation test failed

        Impact motherboard:
               ALL MBs

        Affected functions:
        Validation :
            1. Check if IPMIECO TC102 PASS or not
==============================================================================================================================
Filename: BMC_X12AST2600-nonROT-F201MS_20210901_0.13.12_STDsp.bin version: 0.13.12 Date: 09-01-2021
U-Boot build time :
Java SOL Viewer version : v0.5.15
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_07302021

1.
        Category: Fix
        Description:
            [127558] STD-16914-- 01.00.07( 06/01/2021) – Reload IPMI Configuration will lose SMTP sender address

        Impact motherboard:
            X12/H12 Unit Test

        Affected functions:
        Validation:
            Following lab's standard validation
            1. Configure SMTP setting
            2. Factory Default Reset
            3. Reload COnfiguration.
2.
        Category: Fixed
        Description:
            Help - infomation doesn't sync with newest spec.

        Impact motherboard:
            X12STL-F-P

        Affected functions:
        Validation:
            Check in Help page
3.
        Category: Fix
        Description:
            [129965] There is no CPU Error log after trigger by DCI

        Impact motherboard:
            X12STH-F/LN4F/SYS

        Affected functions:
        Validation:
            Following lab's standard validation
4.
        Category: Fix
        Description:
            [129144] IPMI Web - Firmware Management - Inventory check fail

        Impact motherboard:
            X12STL-F

        Affected functions:
        Validation:
            1. Login in BMC Web Gui
            2. IPMI Web -> Maintenance -> Firmware Management -> Inventory
            3. BIOS ME and Power Supply are there
==============================================================================================================================
Filename: BMC_X12AST2600-nonROT-F201MS_20210816_0.13.11_STDsd&p.bin version: 0.13.11 Date: 08-16-2021
U-Boot build time :
Java SOL Viewer version : v0.5.15
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_07302021

1.
        Category: Fix
        Description:
           [129445] ECO --20122 -- 00.13.08--ikvm -- Can't play Recording media downloaded from ikvm(html5)
    
        Impact motherboard:
            X12STL-IF
    
        Affected functions:
        Validation:
            1.Open IKVM HTML5 window
            2.Click [Record] menu, starting record video then stop it.
            3.Open [recorder.web] by google chrome

2.
        Category: Fix
        Description:
            [127253][126778][126184] SATC Redfish automation test failed
    
        Impact motherboard:
               X12STL-IF,X12STE-F,X12STD-F
    
        Affected functions:
        Validation :
            1. Run Redfish Secure Boot automation with X12 Testing
            2. Automation test item with Secure Boot:
              2.1 GET SecureBoot URI
              2.2 Check Systems SecureBoot Required Keys
              2.3 PATCH SecureBootEnable
              2.4 POST SecureBoot ResetKeys


==============================================================================================================================
Filename: BMC_X12AST2600-nonROT-F201MS_20210812_0.13.10_STDsd&p.bin version: 0.13.10 Date: 08-12-2021
U-Boot build time :
Java SOL Viewer version : v0.5.15
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_07302021

1.
        Category: Enhancement
    
        Description:
            Implement internal version ID inside private API (/BmcInfo) to notify Redfish design changes to internal tools teams
    
        Impact motherboard:
            All Tatlow MBs
    
        Affected functions:
        Validation:
            1. GET internal fw version from /restapi/smci/BmcInfo/

2.
        Category: Fix
        Description:
            [129010] Alert-CPU overheat-CPU upper critical event info check fail
        Impact motherboard:
            X12STL-F
    
        Affected functions:
        Validation:
            1. Let CPU overheat
            2. CPU upper critical event info should have sensor name
3.
        Category: Fix
        Description:
            [129172] PVCC_CPU sensor will become to critical
        Impact motherboard:
            X12STH-F/LN4F/SYS
    
        Affected functions:
        Validation:
            Following lab's standard validation
            1. Open SensorReading Page of BMC Web.
            2. Check the PVCC_CPU is in normal statue.

4.
        Category: Fix
        Description:
            [129144] IPMI Web - Firmware Management - Inventory check fail.
    
        Impact motherboard:
            H12DGO-6
    
        Affected functions:
        Validation:
            1. Go to Maintenance - Firmware Management - Inventory page.
            2. Check PowerSupply in the list.

5.
    R: [128701] IPMI Web - Firmware Management - BIOS preserve configuration options check fail.
        Category: Fix
        Description:
            [128701] IPMI Web - Firmware Management - BIOS preserve configuration options check fail.
    
        Impact motherboard:
            X12STL-F
    
        Affected functions:
        Validation:
            1. Go to Maintenance - Firmware Management - Update page.
            2. Check Preserve BIOS Option match UI spec.
6.
        Category: Fix
        Description:
            [129440] ECO --20122 -- 00.13.08--SMCIPMItool -- Can't use command "NM " full function
    
        Impact motherboard:
               X12STL-IF
    
        Affected functions:
        Validation :
            1. not support nm
7.
       Category: Fix
        Description:
            [129477] Multi sensor reading function test fail with RSC-SR-68G4 Copy Project Issue Link
        Impact motherboard:
            X12STH-F/LN4F/SYS
    
        Affected functions:
        Validation:
            Following lab's standard validation
            1. Open SensorReading Page of BMC Web.
            2. Check the AOC_NIC and AOC_SAS temp value.

8.
        Category: Fix
        Description:
            [129606] [IPMI ECO v00.13.09] Automation tests Failure
    
        Impact motherboard:
               X12STL-IF
    
        Affected functions:
        Validation :
            1. power off system
            2. BIOS update
            3. can power on system

==============================================================================================================================
Filename: BMC_X12AST2600-nonROT-F201MS_20210804_0.13.09_STDsd&p.bin version: 0.13.09 Date: 08-04-2021
U-Boot build time :
Java SOL Viewer version : v0.5.15
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_07302021

1.
        Category: Enhancement
    
        Description:
            Implement internal version ID inside private API (/BmcInfo) to notify Redfish design changes to internal tools teams
    
        Impact motherboard:
            All Tatlow MBs
    
        Affected functions:
        Validation:
            1. GET internal fw version from /restapi/smci/BmcInfo/

2.
        Category: Fix
        Description:
            [129010] Alert-CPU overheat-CPU upper critical event info check fail
        Impact motherboard:
            X12STL-F
    
        Affected functions:
        Validation:
            1. Let CPU overheat
            2. CPU upper critical event info should have sensor name
3.
        Category: Fix
        Description:
            [129172] PVCC_CPU sensor will become to critical
        Impact motherboard:
            X12STH-F/LN4F/SYS
    
        Affected functions:
        Validation:
            Following lab's standard validation
            1. Open SensorReading Page of BMC Web.
            2. Check the PVCC_CPU is in normal statue.
4.
        Category: Fix
        Description:
            [129144] IPMI Web - Firmware Management - Inventory check fail.
    
        Impact motherboard:
            H12DGO-6
    
        Affected functions:
        Validation:
            1. Go to Maintenance - Firmware Management - Inventory page.


==============================================================================================================================
Filename: BMC_X12AST2600-nonROT-F201MS_20210723_0.13.08_STDsd&p.bin version: 0.13.08 Date: 07-23-2021
U-Boot build time :
Java SOL Viewer version : v0.5.15
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
    Category: Fix
    Description:
        [127886] Redfish SATC automation test has 8 item failed.
        1. Marvell firmware version.
        2. NIC URI 404 not found.

    Impact motherboard:
        H12DSU-INR

    Affected functions:
    Validation:
        1. Run Redfish automation.
2.
    Category: Fix
    Description:
        [128688] IPMI Web - BMC Settings - Reload IPMI Configuration will change ADMIN's password

    Impact motherboard:
        X12STL-F

    Affected functions:
    Validation :
        1. Go to IPMI Web -> change one alert settings
        2. Donwload ipmi configuration, save_config.bin
        3. Reload the ipmi configuration with save_config.bin
        4. User can login with original User name and password
3.
    Category: Enhancement
    Description:
        show the "IPv4StaticAddresses" and "IPv6StaticAddresses" porperties
        when there's no data content in /redfish/v1/Managers/1/EthernetInterfaces/1

    Impact motherboard:
        TSMC_H12SSW-AN6

    Affected functions:
    Validation:
        1. "IPv4StaticAddresses" of "IPv6StaticAddresses" will show in
        /redfish/v1/Managers/1/EthernetInterfaces/1 even ther's no data content.
4.
    Category: Fix
    Description:
        [128626] Beta -- 16914 --00.20.06 ｡V Failed to receive syslog/smtp after raw command triggered

    Impact motherboard:
        MBD-X12DPFR-AN6-P

    Affected functions:
    Validation:
        1. Setup syslog and smtp for notification.
        2. Generate a SEL and check both syslog server and email reviced.
5.
    Category: Fix
    Description:
        [121184] [DVT]No AOC GPU/Network info & GPU/Network Temp Sensor in IPMI Web GUI

    Impact motherboard:
        X12SPM-LN6TF-P

    Affected functions:
    Validation:
        Following lab's standard validation
6.
    Category: Fix
    Description:
        [128340] HWM DC Voltage reading issue

    Impact motherboard:
        X12STH-F/LN4F/SYS

    Affected functions:
    Validation:
        Following lab's standard validation
        1. Open SensorReading Page of BMC Web.
        2. Check the ADC value are less than 2% tolerance.
7.
    Category: Fix
    Description:
        [128415] IPMI Web - sensor check fail

    Impact motherboard:
           X12STL-F

    Affected functions:
    Validation :
        1. Go to IPMI Web sensor page
        2. Check sensor name rule "M2SSD1 Temp" and "CPU_VRMIN Temp"
        3. Check sensor status "PVNN PCH" and "3.3V BMC" are not x
8.
    Category: New
    Description:
        Implement OEM command Get/Set BMC_ME_MFR_MODE

    Impact motherboard:
        X12STL-F

    Affected functions:
    Validation:
        1. ipmitool -H <IP> -U <UID> -P <PWD> 0x30 0x70 0x6f
            Data 0: 0: Get BMC_ME_MFR_MODE GPIO status.
            Data 0: 1: Set BMC_ME_MFR_MODE GPIO status,
            Data 1: 1: Set BMC_ME_MFR_MODE GPIO to output high
            Data 1: 0: Set BMC_ME_MFR_MODE GPIO to output Low
==============================================================================================================================
Filename: BMC_X12AST2600-nonROT-F201MS_20210719_0.13.07_STDsp.bin version: 0.13.07 Date: 07-19-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
    Category: Fix
    Description:
        [122709] [SUM_2.5.2_20210112] The result of test case:255 display "stoi: no conversion"

    Impact motherboard:
        X12SPW-TF MB.
    Affected functions:
    Validation:
        1. Install Broadcom3108 and 6 HDD
        2. Check if SUMECO's "Test case 255 - OOB - SecureEraseRaidHdd" can pass
2.
    Category: Fix
    Description:
       [127253] SATC Redfish automation test failed

    Impact motherboard:
        X12STL-IF

    Affected functions:
    Validation:
        1.Using Rest API to test SMTP in Redfish
        2.You can patch any characters in [SmtpPassword] field
3.
    Category: Fix
    Description:
        [128415] IPMI Web - sensor check fail.

    Impact motherboard:
           X12STL-F

    Affected functions:
    Validation :
        1. Check Sensor has no fail items
4.
Category: New feature
Description:
    [New feature] Support NCSI OEM VLAN ID command
    1. Optimize ncsi task code flow
    2. Support INTEL X550 LAN chip, Broadcom 57508,57414, Mellanox CX4

Impact motherboard:

Affected functions:
Validation :
    1. Insert NICs with above LAN chip and SET/GET VLAN ID via redfish API
5.
    Category: Fix
    Description:
        [128124] No Storage Monitoring for AOC-SLG4-2E4T & 4E4T

    Impact motherboard:
        H12SSL-I MB.
    Affected functions:
    Validation:
        1. Install BPN-SAS3-LA26A-N12 on MB's JNVMe0
        2. Check if storage page can be displayed
6.
    Category: Fix
    Description:
        [128526] STD --18380 -- 01.00.35 (07/02/2021) -- Factory default options list will disappear during restore period.

    Impact motherboard:
        H12DGO-6

    Affected functions:
    Validation:
        1. Go to Maintenance - BMC Reset page.
        2. Perform factory default should keep the options list displayed.
7.
    Category: Fixed
    Description:
    Help Page is not matched with CarrierBoard IPMI Web

    Impact motherboard:
        X12DPG-U6-P, X12SAE-5-P, X12SCA-5F-P

    Affected functions:
    Validation:
       Check in Help page
8.
    Category: Fixed
    Description:
    Help Page is not matched with CarrierBoard IPMI Web

    Impact motherboard:
        X12DPG-U6-P, X12SAE-5-P, X12SCA-5F-P

    Affected functions:
    Validation:
       Check in Help page
9.
    Category: Fix
    Description:
       [128501] STD --18380 -- 01.00.35 (07/02/2021) -- Without GUP1~GPU8 details temperature when export to excel file.(Sensor)

    Impact motherboard:
        H12DGO-6

    Affected functions:
    Validation:
        1.Open [Sensor Reading] page
        2.Export excel and view detail (If there are details, they will be displayed in the table of [Information])
10.
Category: Fix
    Description:
        [127349][AST2600 A3] Redfish Automation ATT test failed with 8 failures

    Impact motherboard:
        X12DPU-6

    Affected functions:
    Validation:
        1. Re-run Redfish Automation ATT test
11.
    Category: Fix
    Description:
       [128627] Beta -- 16914 --00.20.06  Fail to block patch invalid user password from REDFISH

    Impact motherboard:
        X12DPFR-AN6

    Affected functions:
    Validation:
        1. Open the "Account Services" page.
        2. Add the username and password(use the special character ":").
12.
    Category: Fix
    Description:
        BMC will hang at the first startup (flash BMC FW by flash tool).

    Impact motherboard:
         X12STD-F X12STE-F

    Affected functions:
    Validation:
        1. Flash BMC FW by flash tool.
        2. AC on and check if BMC hang or not.
13.
    Category: Fix
    Description:
        [128611] BETA --20282 -- 09.00.10(06/26/2021)--Enhancement-- Sorting task list by time created is more user friendly

    Impact motherboard:
        X12DPU-6

    Affected functions:
    Validation:
        1. Go to Maintenance - Task List page.
        2. Change default tasks order.
14.
Category: Fix
Description:
    [122962] Beta -- 16914 -- 00.10.86 ? System entered Update Mode after web Port page stress test"
Impact motherboard:
    X12DDW-A6
Affected functions:
Validation:
    1. run port stress test.
15.
    Category: fix
    Description:
       [128491]Std – 16914 – 01.00.11 – [REDFISH] oem fwinventory update method with preserve option does not preserve config Copy Project Issue Link
    Impact motherboard:
       X12DPI-N6
    Affected functions:
    Validation:
       1. Modify some configuration (populate all users in user table)
       2. POST /redfish/v1/UpdateService/Oem/Supermicro/FirmwareInventory/BMC/Actions/SmcFirmwareInventory.EnterUpdateMode (no payload)
       3. POST /redfish/v1/UpdateService/Oem/Supermicro/FirmwareInventory/BMC/Actions/SmcFirmwareInventory.Upload
        Payload is type multipart/form-data, "bmc": <ipmi fw bin>
       4. POST /redfish/v1/UpdateService/Oem/Supermicro/FirmwareInventory/BMC/Actions/SmcFirmwareInventory.Update
          Payload is type application/json {"PreserveCfg": true, "PreserveSdr": true, "PreserveSsl": true}
       5. Check task to completion, wait until bmc back.
       6. Check configuration kept
16.
    Category: Fix
    Description:
        [128704] IPMI Web - Troubleshooting - shouldn't display "Console Capture" page.

    Impact motherboard:
           X12STL-F

    Affected functions:
    Validation :
        1. Go to IPMI Web - Maintenance - Troubleshooting
        2. "Troubleshooting" shouldn't display "Console Capture" page.
17.
    Category: New
    Description:
        Support AOM-BPN-MC12S4 (4 U.2 SSD).

    Impact motherboard:
         X12STE-F

    Affected functions:
    Validation:
        1. Use AOM-BPN-MC12S4 for back plane.
        2. Log in IPMI Web > Dashboard > Sensor Readings
        3. Check Sensor 'U2_SSD3' Temp and 'U2_SSD4 Temp' exist or not.
18.
    Category: Fix
    Description:
       [128597] IPMI Web - Network - Can't change RMCP port number.

    Impact motherboard:
        X12STL-F

    Affected functions:
    Validation:
        1.Go to [Network] page
        2.Config [RMCP Port] then save it
==============================================================================================================================
Filename: BMC_X12AST2600-nonROT-F201MS_20210709_0.13.06_STDsp.bin version: 0.13.06 Date: 07-09-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
    Category: Fix
    Description:
        [126251] "Digital Battery Reading Check Fail"

    Impact motherboard:
        X12STD-F

    Affected functions:
    Validation :
        1. Digital Battery Reading Check pass
2.
    Category: Fix
    Description:
       [127253] SATC Redfish automation test failed

    Impact motherboard:
        X12STL-IF

    Affected functions:
    Validation:
        1.Using Rest API to test SMTP in Redfish
        2.You can patch any characters in [SmtpPassword] field
3.
    Category: Fix
    Description:
        [128415] IPMI Web - sensor check fail.

    Impact motherboard:
           X12STL-F

    Affected functions:
    Validation :
        1. Check Sensor has no fail items
4.
    Category: Fix
    Description:
        [126705] No display CPLD version under BIOS.
        BIOS version on BMC web page is not the same with BIOS setup menu.

    Impact motherboard:
         X12STE-F

    Affected functions:
    Validation:
         1. Log in IPMI Web.
         2. Check the string of 'BIOS version' is the same with the one in BIOS steup menu.
5.
    Category: Fix
    Description:
        [127778] The system fan speed is not correct in IPMI

    Impact motherboard:
         X12STE-F

    Affected functions:
    Validation:
         1. Log in IPMI Web > Sensor Readings > FAN.
         2. Check FAN readings correct or not.
6.
    Category: Enhancement
    Description:
        Add 5 bios preserve options ipmi cmd and redfish arguments for new redfish hii TC220

    Impact motherboard:
        X12STD

    Affected functions:
        redfish/v1/UpdateService/upload

    Validation:
        1. FW update bios with PreserveBOOTCONF, PreserveOA, PreserveSECBOOTKEY, PreserveSETUPCONF and PreserveSETUPPWD options
        2. Get preserve flag from IPMI cmd 0x30 0xa0 0x15
==============================================================================================================================
Filename: BMC_X12AST2600-nonROT-F201MS_20210629_0.13.05_STDsp.bin version: 0.13.05 Date: 06-29-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
Category: Fix

Description:
    [128049] M.2 sensor does not report fan duty, cannot control fan speed.
    Rootcause is the M.2 in this system design is read from AOC Card, hence the
    M.2 sensor is naming with "AOCSSD" in sensor table lsit.

Impact motherboard:
    X12DPG_AR6

Affected functions:
    board_X12DPG_AR6.c -> DECLARE_PWM_TABLE(BOARD_NAME)

Validation:
    Using the SMCIPMITool.jar to check the PWM
2.
    Category: Fix

    Description:
        [128049] U.2 SSD does not report fan duty, cannot control fan speed
        Rootcause is the U.2 SSD  in this system design is naming with "U2_SSD"
        in sensor table lsit.

    Impact motherboard:
        X12DPG_AR6

    Affected functions:
        board_X12DPG_AR6.c -> DECLARE_PWM_TABLE(BOARD_NAME)

    Validation:
        Using the SMCIPMITool.jar to check the PWM
3.
Category: Fix

Description:
    R: [128098] [IPMI] WebGUI Network AOC Slot Location is N/A

Impact motherboard:
    X12DDW-A6

Affected functions:
    redfish/src/redfish/common/location/location.cpp

Validation:
    1. Install AOC-AG-I2M-P and AOC-AG-I4M-P into AIOM slot of X12DDW-A6
    2. Checnk the location field of Network AOC page
==============================================================================================================================
Filename: BMC_X12AST2600-nonROT-F201MS_20210623_0.13.04_STDsp.bin version: 0.13.04 Date: 06-23-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
    Category: Fix
    Description:
        [126603] IPMI WEB GUI Eject and Insert function can't work

    Impact motherboard:
        X12STD-F

    Affected functions:
    Validation:
        1. Install U.2 NVMe drive on BPN
        2. Check if Eject and Insert items disapeared in Physical View of Storage page
2.
    Category: Fix
    Description:
        [127266] There is no message to remind user to restart the SUT when updating BIOS finished through BMC WebGUI

    Impact motherboard:
        X12STL-IF / X12STE-F

    Affected functions:
    Validation:
        1. Go to Maintenance - Firmware Management - Update page.
        2. Update BIOS (nonROT platform).
        3. Display popup reset system message after finishing update.
3.
    Category: Fix
    Description:
        [126152] 	[EVT] Some IPMI sensor reading status failed.

    Impact motherboard:
           X12STL-IF

    Affected functions:
    Validation :
        1. change sensor name
4.
    Category: Fix
    Description:
        [127479] There is unnecessary item (CPLD) in Inventory page

    Impact motherboard:
        X12STH-LN4F

    Affected functions:
    Validation:
        1. Go to Maintenance - Firmware Management - Inventory page.
        2. Check Filter should not display CPLD when there is no CPLD info.
5.
    Category: Fix
    Description:
        [127518] HWM Digital Battery sensor reading Fail.

    Impact motherboard:
        X12STH-F/LN4F/SYS

    Affected functions:
    Validation:
        1. Open SensorReading Page of BMC Web.
        2. Set the VBAT input Voltage to 2.7V.
        3. Check the VBAT reading is 'Battery Presence Detected'.
6.
    Category: Fix
    Description:
        [126705] No display CPLD version under BIOS.
        CPLD version on BMC web page is not the same with BIOS setup menu.
        CPLD version should be uppercase letters.

    Impact motherboard:
         X12STE-F

    Affected functions:
    Validation:
         1. Log in IPMI Web.
         2. Check the string of 'CPLD Version' are uppercase leters or not.
7.
    Category: Fix
    Description:
        [127332] Digital Battery Reading Check Fail

    Impact motherboard:
         X12STE-F

    Affected functions:
    Validation:
        1. Take the battery that volatge is between than 2.55 ~ 2.4 and insert to X12STE-F MB.
        2. Log in IPMI Web > Sensor Readings.
        3. Check the reading of sensor 'VBAT' is 'Battery Low' or not.
8.
    Category: Fix
    Description:
        [127258][SuperDiag] Test fail with SuperDiag_1.5.0_20210507 via USB Key.

    Impact motherboard:
         X12STE-F

    Affected functions:
    Validation:
        1. Execute command: ipmitool -H $BMC_IP -U $BMC_UID -P $BMC_PWD raw 0x30 0x94
        2. The content of response should not be all 0xFF.
9.
    Category: Fix
    Description:
        [127655] The System Crash Dump/Console Capture Video/Crash Screen Capture functions should be unsupported.

    Impact motherboard:
        X12STH-F/LN4F/SYS

    Affected functions:
    Validation:
        1. Open SensorReading Page of BMC Web.
        2. Change web page to Maintainence -> Troubleshooting.
        3. Check the Console Capture is noe shown on Web.
10.
    Category: Fix
    Description:
        [127045] No Storage Page in the BMC Web GUI

    Impact motherboard:
           X12STL-IF

    Affected functions:
    Validation :
        1. Storage card works fine
11.
    Category: Fix
    Description:
       [126150] Node information display N/A under BMC Web Multi Node page

    Impact motherboard:
        X12STD-F

    Affected functions:
    Validation:
        1.Login in BMC Web Gui.
        2.Go to [Multi-Node] page
        3.If the machine is MicroCloud, this page should hide [BIOS ver],[CPLD ver],[BMC ver] and [POST Code]
12.
    Category: Fix
    Description:
        [127667] NO AOC M.2 sensor reading

    Impact motherboard:
           X12STL-IF

    Affected functions:
    Validation :
        1. has AOC M.2 sensor reading
13.
    Category: New feature
    Description:
        Support new special characters spec. (bmc_each_field_spec_v1.24)

    Impact motherboard:
        X12STD-F / X12STE-F / X12STH-F / X12STL-F / X12STL-IF

    Affected functions:
    Validation:
        1. Verify all the input fields should follow the spec.
14.
    Category: New feature
    Description:
        VROC support on BMC

    Impact motherboard:
        X12STD-F / X12STE-F / X12STH-F / X12STL-F / X12STL-IF

    Affected functions:
    Validation:
        1. Update enable ACL BIOS
        2. Intstall OOB to HOST
        3. Web can build raid on VROC way
15.
    Category: New feature
    Description:
        [Broadcom] Add FW update feature for Broadcom Gen4 storage card 38xx/39xx.

    Impact motherboard:
        X12STD-F / X12STE-F / X12STH-F / X12STL-F / X12STL-IF

    Affected functions:
    Validation:
        1. Install 38xx/39xx Broadcom Gen4 storage card.
        2. Login WebGUI.
        3. Go to Maintenance -> Fimrware Management.
        4. Update selected 38xx/39xx storage card.
16.
    Category: New Feature
    Description:
        Web UI - Update AOC NIC and PMem function

    Impact motherboard:
        X12STD-F / X12STE-F / X12STH-F / X12STL-F / X12STL-IF

    Affected functions:
    Validation:
        1. Go to Maintenance - Firmware Management.
        2. Update detected updatable AOC NIC and PMem.
17.
    Category: New Feature
    Description:
        AOC NIC PLDM firmware update flow and new Network AOC page

    Impact motherboard:
        X12STD-F / X12STE-F / X12STH-F / X12STL-F / X12STL-IF

    Affected functions:
    Validation:
        1. Insert AOC NIC with FW support PLDM protocol to X12MB.
        2. Go to Network AOC page, check NIC's firmware version.
        3. Go to Maintenance -> Firmware Management, select NIC you want to update.
        4. Execute NIC firmware update procedure, like update BMC and BIOS.
        5. when summit update requeset, go to Task List and check update progress.
        6. If update flow finished, run a power cycle or power reset.
        7. After system reboot done, go to Network AOC page, and check NIC's firmware version again.
           its version need be changed.
18.
    Category: New Feature
    Description:
        Follow change in Redfish Patch on array mechanism for below item, modify WebGUI related column
        - in AccountService
            - LDAP.ServiceAddresses
            - LDAP.RemoteRoleMapping
            - ActiveDirectory.RemoteRoleMapping
            - ActiveDirectory.ServiceAddresses

    Impact motherboard:
        X12STD-F / X12STE-F / X12STH-F / X12STL-F / X12STL-IF

    Affected functions:
    Validation:
        1. Login WebGUI
        2. Go to Configuration -> Account Services -> Directory Service
        3. Add / Modify / Delete Server Address, Rules and Search Base
19.
    Category: New Feature
    Description:
        Follow Redfish v1.8 spec, Add Redfish Patch on array mechanism
        - in Managers/1/EthernetInterfaces/1
            - IPv6StaticAddresses
        - in AccountService
            - LDAP.ServiceAddresses
            - LDAP.RemoteRoleMapping
            - ActiveDirectory.RemoteRoleMapping
            - ActiveDirectory.ServiceAddresses

    Impact motherboard:
        X12STD-F / X12STE-F / X12STH-F / X12STL-F / X12STL-IF

    Affected functions:
    Validation:
        1. PATCH Managers/1/EthernetInterfaces/1 property IPv6StaticAddresses with
            - {} to leave an element unchanged
            - null to remove an element
            - normal data to modify or add the element
        2. PATCH AccountService property LDAP.ServiceAddresses, LDAP.RemoteRoleMapping,
                                         ActiveDirectory.RemoteRoleMapping and ActiveDirectory.ServiceAddresses with
            - {} to leave an element unchanged
            - null to remove an element
            - normal data to modify or add the element
20.
    Category: New feature
    Description:
        IP Access Control support IPv6

    Impact motherboard:
        X12STD-F / X12STE-F / X12STH-F / X12STL-F / X12STL-IF

    Affected functions:
    Validation:
        1. Check IP Access Control for ipv4/ipv6 by webui, redfish, and ipmi command.
21.
    Category: New feature
    Description:
        Implement and modify SEL/MEL by following SPEC: SEL 1.32 and MEL 1.02.
        SEL: X12_IPMIManagement_Standarization_SPEC_SEL_ver. 1.32.xlsx
        MEL: X12_MEL_SPEC_ver. 1.02.xlsx

    Impact motherboard:
         X12STD-F / X12STE-F / X12STH-F / X12STL-F / X12STL-IF

    Affected functions:
    Validation:
         1. IPMI Web > System > Health Event Log.
            IPMI Web > Maintenance > Maintenance Event Log.
         2. Check serverity and descriptions of SEL and MEL correct or not.
22.
    Category: New features
    Description:
        Support new BIOS HII for Redfish

    Impact motherboard:
        X12STD-F / X12STE-F / X12STH-F / X12STL-F / X12STL-IF

    Affected functions:
    Validation:
        1. View and download full Bios attribute registry json file:
                URL: /redfish/v1/Registries/BiosAttributeRegistry.v1_0_0
                Method: GET
        2. Modify attributes:
                URL: /redfish/v1/Systems/1/Bios or /redfish/v1/Systems/1/Bios/SD
                Method: PATCH, PUT
                The user can GET current setting and PATCH/PUT desired settings.
                {"Attributes":{"COMMN030#0006": 1, "COMMN092#0133":"Apply to each LAN", "SMCBL0EA#010A":true, "SMCBL0E2#0102":"VT100+"}}
        3. View pending settings:
                URL: /redfish/v1/Systems/1/Bios/SD
                Method: GET
                The user can view any pending setting after PATCH/PUT.
                After PATCH/PUT, please reset system to set values to BIOS
        4. BIOS Reset:
                URL: /redfish/v1/Systems/1/Bios/Actions/Bios.ResetBios
                Method: POST
                POST a reset of the BIOS attributes to default values.
                After POST, please reset system to set values to BIOS.
                Bios reset will clear all user settings which patched before bios reset.
        5. Change BIOS booting Password:
                URL: /redfish/v1/Systems/1/Bios/Actions/Bios.ChangePassword
                Method: POST
                POST with "PasswordName", "OldPassword", "NewPassword" to change password.
                {"PasswordName":"COMMN032#0150", "OldPassword":"111111", "NewPassword":"aaaaaa"}
                {"PasswordName":"COMMN033#0151", "OldPassword":"222222", "NewPassword":"bbbbbb"}
                After POST, please reset system to set values to BIOS.
        6. View Bios BootOrder and BootNext settings:
                URL: /redfish/v1/Systems/1
                Method: GET
                The user can view any BootOrder and BootNext setting from current bios menu.
        7. Change BIOS BootOrder:
                URL: /redfish/v1/Systems/1
                Method: PATCH
                {"Boot": {"BootOrder":["Boot0003", "Boot0004", "Boot0005", "Boot0006", "Boot0001"]}}
                After PATCH, please reset system to set values to BIOS.
        8. Change BIOS BootNext:
                URL: /redfish/v1/Systems/1
                Method: PATCH
                {"Boot": {"BootNext":"Boot0001"}}
                After PATCH, please reset system to set values to BIOS.
23.
    Category: Enhancement
    Description:
        Add IPv6 default gateway field in web GUI. Fix some warnings by ipmitool.

    Impact motherboard:
        X12STD-F / X12STE-F / X12STH-F / X12STL-F / X12STL-IF

    Affected functions:
    Validation:
        1.Login BMC Web Gui and check the network page.
        2.There should be Gateway IP field in IPv6 settings.
        3.If there is a IPv6 gateway in the network, it should be displayed.
        4.issue the following command to query ipv6 settings, there should be no warnings.
          ipmitool -H $IP -U ADMIN -P ADMIN lan6 print
24.
    Category: Enhancement
    Description:
        Web UI - All the input fields are not allowed with any non-half-width characters
        [122583] BETA --18367 -- 09.12.01 BETA(01/12/2021) -- "BMC hostname" couldn't save changed even if the requested has successfully set at Dynamic DNS.
        [123140] STD --18380 -- 01.00.06(01/08/2021) -- Using full-width characters at "SMTP Server" , "Port Number" and "User name" has difference behavior (SMTP).
        [123132] STD --18380 -- 01.00.06(01/08/2021) -- Using full-width characters at "User name" , "Auth Key"," Private Key" will return "ERROR:A general ..." and wrong tips on SNMP page.
        [123136] STD --18380 -- 01.00.06(01/08/2021) -- Using space at "Systelog Server" will get difference behavior.
        [123129] STD --18380 -- 01.00.06(01/08/2021) -- Using full-width characters at "ROCommunity" and "RWCommunity" will return "ERROR:A general ..." on SNMP page.
        [123117] STD --18380 -- 01.00.06(01/08/2021) -- Using full-width characters at "Redfish" will return "Oops!" error and wrong tips.(Alerts)
        [123113] STD --18380 -- 01.00.06(01/08/2021) -- Using full-width characters at "SNTP" will return "Oops! something went wrong..." error.(Alerts)

    Impact motherboard:
        X12STD-F / X12STE-F / X12STH-F / X12STL-F / X12STL-IF

    Affected functions:
    Validation:
        1. Go to these pages
        2. Input any non-half-width characters, it will show [Please use Half-Width characters when entering data into textbox.]
25.
    Category: Enhancement
    Description:
        Web UI - Block UI style and behavior consistency

    Impact motherboard:
        X12STD-F / X12STE-F / X12STH-F / X12STL-F / X12STL-IF

    Affected functions:
    Validation:
        1. Change Block UI sytle
        2. Display to all pages
26.
    Category: Enhancement
    Description:
        Web UI - Storage Monitoring

    Impact motherboard:
        X12STD-F / X12STE-F / X12STH-F / X12STL-F / X12STL-IF

    Affected functions:
    Validation:
        1. Broadcom - drives slot number is wrong when in different enclosure
        2. Broadcom - add drive temperature
        3. Broadcom - create RAID check VD name length
        4. Broadcom - create RAID maximum of logical drives is 16
        5. Broadcom - display RAID10 number of drives
        6. NVMe - add Firmware Revision
27.
    Category: Enhancement
    Description:
        Web UI - License check display tips and message

    Impact motherboard:
        X12STD-F / X12STE-F / X12STH-F / X12STL-F / X12STL-IF

    Affected functions:
    Validation:
        1. Check actions or pages needed license in below pages
        2. Health Event Log page - SEL Acknowlegement actions
        3. Storage Monitoring - actions in Physical/Logical/Controller
        4. Directory Service page - LDAP input Bind Password
        5. Alerts page - Modify Alert with Redfish/SNMPv3
        6. Syslog page
        7. Virtual Media - Virtual CD-ROM with http or https
        8. System Lockdown page
        9. FW update page - update Broadcom, Marvell, PMem
        10.Console Capture page
28.
    Category: Enhancement
    Description:
        Web UI - Password field enhancement

    Impact motherboard:
        X12STD-F / X12STE-F / X12STH-F / X12STL-F / X12STL-IF

    Affected functions:
    Validation:
        1. Check password field in below pages
        2. Login page
        3. Users page - Add/Modify user
        4. Directory Service page - LDAP input Bind Password
        5. Directory Service page - RADIUS input Secret
        6. Alerts page - Modify Alert with SNMPv1/SNMPv3
        7. SNMP page - Modify SNMPv3
        8. SMTP page - Modify SMTP Password
        9. Virtual Media - Virtual CD-ROM input password
==============================================================================================================================
Filename: BMC_X12AST2600-nonROT-F201MS_20210528_0.13.03_STDsd.bin version: 0.13.03 Date: 05-28-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
    Category: Fix
    Description:
        [124783] [IPMICFG] Test fail via SMSTC with IPMICFG_1.32.0_build.200910.
    Impact motherboard:
        X12STD-F

    Affected functions:
    Validation:
        1. Test pass
2.
        Category: Fix
        Description:
            [126152] [EVT] Some IPMI sensor reading status failed.
    
        Impact motherboard:
               X12STL-IF
    
        Affected functions:
        Validation :
            1. sensor reading status pass
3.
        Category: Fix
        Description:
            [127047] No Power Consumption monitor in the BMC Web GUI
    
        Impact motherboard:
               X12STL-IF
    
        Affected functions:
        Validation :
            1. has power consumption
4.
        Category: Fix
        Description:
            [127054] BMC Web GUI should not have Multi Node page
    
        Impact motherboard:
               X12STL-IF
    
        Affected functions:
        Validation :
            1. no Multi Node page
5.
        Category: Fix
        Description:
            [126495] [AST2600_A1chip+BMC A3 patch]AOC M.2 devices Sensor name does Not Match Supermicro_X12 Temp Sensor Naming Guildline_1.0f
        Impact motherboard:
            X12SPM-LN4F/LN6TF/TF
    
        Affected functions:
        Validation:
             1. Open SensorReading Page of BMC Web.
             2. Check all of Sensor Reading is normal.
6.
        Category: Fix
        Description:
            [126711] "STD---BMC_20210510_01.00.06_STDsp-- Data cannot be remove when updateing BMC thru SUM wih option Non-preserve "
    
        Impact motherboard:
            X12SPL-F-P
    
        Affected functions:
        Validation:
            1.Modify something on WebGUI and then Save.
            2.Update BMC thru SUM with --overwrite_cfg option only.
            3.Check modified config setting has changed back to default value.

7.
        Category: Fix
        Description:
            [125640]No AOC-CTGS-i2T sensor reading
    
        Impact motherboard:
             X12STD-F
    
        Affected functions:
        Validation:
             1. Log in IPMI Web > Sensor Readings.
             2. Check if 'MLP_NIC' appear in the sensor list or not.

8.
        Category: Fix
        Description:
            [126710] "STD---BMC_20210510_01.00.06_STDsp-- Syslog page is modifiable in System lockdown mode "
    
        Impact motherboard:
            X12SPL-F-P
    
        Affected functions:
        Validation:
            1.Login in BMC Web Gui.
            2.Go to Syslog page and modify Syslog to On and save changes.
            3.Lockdown the system and go back to Sys
9.
        Category: Fix
        Description:
            [126712] "STD---BMC_20210510_01.00.06_STDsp-- Messy code when session timeout "
    
        Impact motherboard:
            X12SPL-F-P
    
        Affected functions:
        Validation:
            1.Login in BMC Web Gui.
            2.Change language to Chinese/Japanese
            3.When session timeout, check prompt message is correct.


==============================================================================================================================
Filename: BMC_X12AST2600-nonROT-F201MS_20210521_0.13.02_STDsd.bin version: 0.13.02 Date: 05-21-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
    Description:
        [126535] [EVT] CPU thermal trip test failed - no CPU thermal trip event in IPMI SEL
    Impact motherboard:
        X12STH-F/LN4F/SYS

    Affected functions:
    Validation:
        1. Test the CPU thermal trip function, the motherboard will shutdown when CPU thermal trip.
        2. Confirm the CPU Thermal Trip log in IPMI SEL.
2.
    Description:
        [126143] No CPU thermal trip event log on IPMI

    Impact motherboard:
           all Tatlow platform

    Affected functions:
    Validation :
        1. has CPU thermal trip event
3.
    Category: Fix
    Description:
        [126496] [AST2600_A1chip+BMC A3 patch]AOC M.2 devices Sensor is not availiable in BMC web interface sensor list
    Impact motherboard:
        X12SPM-LN4F/LN6TF/TF

    Affected functions:
    Validation:
        1. Open and Login to BMC Web.
        2. Confirm the  AOC_M2SSD6 Temperature was shown on the Sensor page.
==============================================================================================================================
Filename: BMC_X12AST2600-nonROT-F201MS_20210512_0.13.01_STDsd.bin version: 0.13.01 Date: 05-12-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
    C: Support new BIOS HII for Redfish
    Category: New features
    Description:
        Support new BIOS HII for Redfish
    Impact motherboard:
        All MBs
    Affected functions:
    Validation:
        1. Modify attributes:
            URL: /redfish/v1/Systems/1/Bios or /redfish/v1/Systems/1/Bios/SD
            Method: PATCH, PUT
        2. View pending settings:
            URL: /redfish/v1/Systems/1/Bios/SD
            Method: GET
        3. BIOS Reset:
            URL: /redfish/v1/Systems/1/Bios/Actions/Bios.ResetBios
            Method: POST
        4. Get full Bios attribute registry json file:
            URL: /redfish/v1/Registries/BiosAttributeRegistry.v1_0_0
            Method: GET
2.
R:[126329] Fan speed reading value in IPMI GUI is incorrect
    Category: Fix
    Description:
        [126329] Fan speed reading value in IPMI GUI is incorrect

    Impact motherboard:
           X12STD-F

    Affected functions:
    Validation :
        1. Fan speed reading is correct
3.
R: [126485] [EVT]JL1 can't work.
    Category: Fix
    Description:
        [126485] [EVT]JL1 can't work.
    Impact motherboard:
        X12STH-F/LN4F/SYS

    Affected functions:
    Validation:
        1. Open SensorReading Page of BMC Web.
        2. Open Case and Check Chassis Intrussion with Critial Status.
        3. After Pressing Intrusion Reset Button and Check Chassis Intrussion with Normal Status.
4.
R:[125096] BMC heart beat LED will not be solid on after BMC do factory reset
    Category: Fix
    Description:
        [125096] BMC heart beat LED will not be solid on after BMC do factory reset

    Impact motherboard:
           X12STD-F

    Affected functions:
    Validation :
5.
R: [125971] [BIOS ECO] BIOSECO Automation Test Failed.
    Category: Fix
    Description:
        [125971] BIOS ECO] BIOSECO Automation Test Failed.
    Impact motherboard:
        X12SPZ-LN4F/SPLN6F

    Affected functions:
    Validation:
         Run the BIOSECO test and check TC 105.
6.
R:[124983] [SMCIPMITool] Test fail via SMSTC with SMCIPMITool_2.25.0_build.210326
    Category: Fix
    Description:
        [124983] [SMCIPMITool] Test fail via SMSTC with SMCIPMITool_2.25.0_build.210326

    Impact motherboard:
           X12STD-F

    Affected functions:
    Validation :
        1. add work around for power cycle
7.
R:[125625] MicroLP card will display Unknown Slot3 in Network AOC page
    Category: Fix
    Description:
        [125625] MicroLP card will display Unknown Slot3 in Network AOC page

    Impact motherboard:
           X12STD-F

    Affected functions:
    Validation :
        1. correct location
==============================================================================================================================
Filename: SMT_X12AST2600_NONROT_RSA4K_001206d.bin version: 0.12.06 Date: 04-26-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
    R:[125845] Componet Info CPU page "Max Speed" should be the "CPU Speed"	
        Category: Fix
        Description:
            [125845]Componet Info CPU page "Max Speed" should be the "CPU Speed"	

        Impact motherboard:
               ALL

        Affected functions:
        Validation :
            1. Componet Info CPU page "Max Speed" should be the "CPU Speed"	
2.
    R:[125842] Componet info information "Product Name" sholud change to "Product Part Number" in Web GUI
        Category: Fix
        Description:
            [125842]Componet info information "Product Name" sholud change to "Product Part Number" in Web GUI

        Impact motherboard:
               ALL

        Affected functions:
        Validation :
            1. Componet info information "Product Name" sholud change to "Product Part Number" in Web GUI
3.
    R:[125838] No AOC-C25G-m1S sensor reading
        Category: Fix
        Description:
            [125838]No AOC-C25G-m1S sensor reading

        Impact motherboard:
               X12STD-F

        Affected functions:
        Validation :
            1. has AOC-C25G-m1S sensor reading
4.
    R:[125640] No AOC-CTGS-i2T sensor reading
        Category: Fix
        Description:
            [125640]No AOC-CTGS-i2T sensor reading

        Impact motherboard:
               X12STD-F

        Affected functions:
        Validation :
            1. has AOC-CTGS-i2T sensor reading
5.
    R:[125625] MicroLP card will display Unknown Slot3 in Network AOC page
        Category: Fix
        Description:
            [125625]MicroLP card will display Unknown Slot3 in Network AOC page

        Impact motherboard:
               X12STD-F

        Affected functions:
        Validation :
            1. MicroLP card will display correct location in Network AOC page
6.
    R:[125123] [SuperDiag] Test fail with SuperDiag_1.5.0_20210401 via USB Key.
        Category: Fix
        Description:
            [125123][SuperDiag] Test fail with SuperDiag_1.5.0_20210401 via USB Key.

        Impact motherboard:
               X12STD-F

        Affected functions:
        Validation :
7.
    R:[124359] IPMI sensor readings work abnormally
        Category: Fix
        Description:
            [124359]IPMI sensor readings work abnormally

        Impact motherboard:
               X12STD-F

        Affected functions:
        Validation :
            1. IPMI sensor readings work normally
8.
    R:[124011] [EVT]JPG1 can't work
        Category: Fix
        Description:
            [124011][EVT]JPG1 can't work

        Impact motherboard:
               X12STD-F

        Affected functions:
        Validation :

==============================================================================================================================
Filename: SMT_X12AST2600_NONROT_RSA4K_001205d.bin version: 0.12.05 Date: 04-14-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

R:[125192] No power consumption and power info in the IPMI Web GUI.
    Category: Fix
    Description:
        [125192] No power consumption and power info in the IPMI Web GUI.

    Impact motherboard:
           X12STD-F

    Affected functions:
    Validation :
        1. Have power consumtion
==============================================================================================================================
Filename: SMT_X12AST2600_NONROT_RSA4K_001204d.bin version: 0.12.03 Date: 04-13-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
Category: Fix
    Description:
        [124988] No Storage page on IPMI.

    Impact motherboard:
           X12STD-F

    Affected functions:
    Validation :
        1. have stroage page while insert a storage card
==============================================================================================================================
Filename: SMT_X12AST2600_NONROT_RSA4K_001203d.bin version: 0.12.03 Date: 04-09-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
Category: Enhancement
Description:
	fix X12STD-F can't get DIMM temp
Impact motherboard:
	*X12STD-F
Affected functions:
Validation :


==============================================================================================================================
Filename: SMT_X12AST2600_NONROT_RSA4K_001202d.bin version: 0.12.02 Date: 3-29-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
Category: Enhancement
Description:
	fix X12STD-F sensor abnoraml
Impact motherboard:
	*X12STD-F
Affected functions:
Validation :

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_001200.bin version: 0.12.00 Date: 12-10-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
Category: Fix
Description:
	[122808] No CPU thermal trip related event logs in IPMI SEL when CPU thermal trip occur
Impact motherboard:
	*X12SDV
Affected functions:
Validation :
	Check SEL

2.
Category: Fix
Description:
	[122459] [EVT]JD1 speaker can't work
Impact motherboard:
	*X12SDV
Affected functions:
Validation :
	Check Speaker


==============================================================================================================================
Filename: SMT_X12AST2500_ROT_001200.bin version: 0.12.00 Date: 12-10-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

Release NON-ROT IPMI FW