================================================
Standard BIOS in-band Update Procedure under UEFI Shell
================================================

1. Save the BIOS update package to your computer.

2. Extract the files from the UEFI folder of the BIOS package to a USB stick. 
   (Note: The USB stick doesn't have to be bootable, but has to be formatted
   with the FAT/FAT32 file system.)

3. Plug the USB stick into a USB port, boot to the Build-In UEFI Shell, and
   type FLASH.nsh BIOSname#.### to start the BIOS update:

     Shell> fs0:
     fs0:\> cd UEFI
     fs0:\UEFI> flash.nsh X11QPH.xxxx

4. The FLASH.NSH script will compare the Flash Descriptor Table (FDT) code in
   the new BIOS with the existing one in the motherboard:

   a. If a different FDT is found, a new file, STARTUP.NSH, will be created,
      and the system will go into reboot in 10 seconds if no key is pressed.
      Press "Y" to go into system reboot right away.  At the reboot, hit
      "F11" key to invoke the boot menu & boot into the build-in UEFI Shell
      again.  The BIOS update will resume, automatically. 

   b. If the FDT is the same, the BIOS update will be started right away.  No
      reboot will be needed.

5. Do not interrupt the process until the BIOS update is complete.

6. Perform an A/C power cycle after the message indicating the BIOS update
   has completed.

7. Go to the BIOS configuration, and restore the BIOS settings.



Notes:

* Supermicro no longer supports the BIOS update method in DOS.

* If the BIOS flash fails, you may contact our RMA Dept. to have the BIOS
  chip reprogrammed.  This will require shipping the board to our RMA Dept.
  for repair.  Please submit your RMA request at 
  http://www.supermicro.com/support/rma/.



