GIT SHA: 77344bf80614953db014f1930c6338874a12c151

Firmware Version: 01.01.07
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230710_01.01.07_STDsp.bin
Production signed Firmware CRC: 527EADFD
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230710_01.01.07_STDsp.bin
Production signed eMMC Firmware CRC: 96CD185E
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20230710_01.01.07_STDsp.bin
Production signed SPI NOR Firmware CRC: 417552B5
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230710_01.01.07_STDsd.bin
Debug signed Firmware CRC: 0B9D44A3
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230710_01.01.07_STDsd.bin
Debug signed eMMC Firmware CRC: BD3760E2
Build Date: 07/10/2023
Redfish API : Redfish_1_11_API_full_list_20230410
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH H13SSF
---------------------------------------------------------------------------------------------------------
***note 1: BMC version 01.01.00 start supporting Redfish Host interface driver ECM, and BIOS update required.


1. Category: Fix
   Description:
     [ENGINEERING] - SYS-221BT-HNR AOC Health Status Issue
   Infected Motherboard: X13DET-B AND ALL
   Affected Functions: AOC Network
   Validation:
     1) Installed one AOC-A25G-b2SM and two AOC-S25G-b2S.
     2) Check OC-A25G-b2SM's healthy status should be normal displayed on AOC NETWORK page.
     3) AOC-S25G-b2S's healthy stauts shoudl be N/A.
2. Category: Fix
   Description:
     [158958] - Hostname update/remove has duplicate record in MEL
   Infected Motherboard: X12DGQ AND ALL
   Affected Functions: Redfish
   Validation:
     1) Login to WebGUI and enter to Configuration > Network.
     2) Modify or remove the hostname and save.
     3) Check MEL and record should not duplicate.
3. Category: Fix
   Description:
     [ENGINEERING] - Add Security States Monitoring in Redfish
   Infected Motherboard: ALL
   Affected Functions: Redfish
   Validation:
     1) Get /restapi/smci/BmcInfo
4. Category: Fix
   Description:
     [133601] - Keep unique password when restore IPMI config
   Infected Motherboard: X13DEM AND ALL
   Affected Functions: 3rd AOC
   Validation:
     1) Install AOC-E810-XXVDA4 or AOC-E810-XXVDA4TGG1 to verify temperature reading
5. Category: Fix
   Description:
     [ENGINEERING] – Virtual media OEM command issue
   Infected Motherboard: ALL
   Affected Functions: :
     Validation :
     1) VM related IPMI command raw 0x30 0x68 0x0D
     2) It should respond correct data
6. Category: Fix
   Description:
     [15670] - Perform the "-lani 0" command on X13DET-B will show the error message "Failed to set the LAN interface. Completion Code=FFh"
   Infected Motherboard: ALL
   Affected Functions: Network
   Validation:
     1) Don’t insert any AIOM or AOC card on SUT.
     2) Login web, go to Configuration -> Network page, set Lan interface to Failover.
     3) Use IPMICFG tool "-lani 0" command, set Lan interface to Dedicated.
     4) Check IPMICFG tool response "done", check lan interface change to Dedicated, pass.
7. Category: Fix
   Description:
     [158741] - Redfish has 3 TC fails
   Infected Motherboard: X12DGQ AND ALL
   Affected Functions: Redfish
   Validation:
     1) Get /Systems/1 to check PowerOnDelaySeconds
8. Category: Fix
   Description:
     [157277] - User name string length only support to 16 not 31 for SNMPv3
   Infected Motherboard: ALL
   Affected Functions: Configuration
   Validation:
     1) Login web GUI -> Configuration -> Account Services -> Users
     2) Press down 'Add' button
9. Category: Fix
   Description:
     [157250] - "Edit" and "Connect" icon should be translated to Simplified Chinese and Japanese at Virtual Media page.
   Infected Motherboard: X13SEM-F-P
   Affected Functions: Configuration
   Validation:
     1) Login Web GUI and change page to Configuration -> Virtual Media
     2) Mount ISO file with Device 1 success
     3) Switching language: English/Simplified Chinese/Japanese
     4) Move muse on "Edit" and "Connect" icon, check tips
10. Category: Fix
    Description:
      [158136] - Some function of Account Services/Network/BMC Settings could be configurable by "User Privileges"
    Infected Motherboard: X13SEM-F-P AND ALL
    Affected Functions: Configuration
    Validation:
      1) Login BMC web GUI by "User Privileges" account
      2) Go Configuration -> Account Services -> check Advanced Settings
      3) Go Configuration -> Network -> check Advanced Settings
11. Category: Feature
    Description:
      [ENGINEERING] - Support fixed boot order
    Infected Motherboard: X13
    Affected Functions: Redfish
    Validation:
      1) Get /redfish/v1/Systems/1/Oem/Supermicro/FixedBootOrder
12. Category: Fix
    Description:
      [133601] - Keep unique password when restore IPMI config
    Infected Motherboard: ALL
    Affected Functions: Restore IPMI configuration, ADMIN password
    Validation:
      1) Scenario 1:
      2) BMC reset to factory default, which set ADMIN account to unique password
      3) Reload IPMI config which contain ADMIN password is not unique password
      4) Verify the ADMIN account must login by unique password
      5) Scenario 2:
      6) BMC reset to ADMIN/ADMIN, which set ADMIN account to ADMIN password
      7) Reload IPMI config which contain ADMIN password is any password
      8) Verify the ADMIN account must login by password of the restored IPMI config
13. Category: Fix
    Description:
      [156146] - Block reserved address when patching IPv6StaticAddresses property of EthernetInterfaces
    Infected Motherboard: X13SCW AND ALL
    Affected Functions: Redfish
    Validation:
      1) PATCH request on /redfish/v1/Managers/1/EthernetInterfaces/1 with payload {"IPv6StaticAddresses": [{"Address": "0::1","PrefixLength": 64}]}, should get 400 bad request
14. Category: Fix
    Description:
      [157041] - AOC-S25GC-i2S thermal sensor will lose when execute dc onoff test item
    Infected Motherboard: X13SEDW-F AND ALL
    Affected Functions: AOC-S25GC-i2S thermal sensor
    Validation:
      1) Install AOC-S25GC-i2S and check sensor reading
      2) Run cburn dc onoff testing
15. Category: Fix
    Description:
      [158488] - User only can enter 63 characters for SNMPv3 Authentication Key and Encryption Key.
    Infected Motherboard: ALL
    Affected Functions: Web
    Validation:
      1) Login web, go to Configuration -> Account Services page.
      2) Add a new user, check snmp Authentication Key and Encryption Key warning message, pass.
16. Category: Fix
    Description:
      [156927] - IPMI ECO Automation tests Failure
    Infected Motherboard: X12DPT-B6-P AND ALL
    Affected Functions: Configuration
    Validation:
      1) Try TC4007
17. Category: Fix
    Description:
      [158711] - User name string length only support to 16 not 31 for SNMPv3
    Infected Motherboard: X12DPG-OA6-GD2-P AND ALL
    Affected Functions: Configuration
    Validation:
      1) Login web GUI -> Configuration -> Account Services -> Users
      2) Press down 'Add' button
      3) Type in '1234567890123456' to 'User Name'
      4) Choice 'SNMP' at 'Account Type'
      5) Check 'User Name'
18. Category: Fix
    Description:
      [158568] - Sensors changed abnormally once sensor type category is selected
    Infected Motherboard: X12DPT-B6-P AND ALL
    Affected Functions: Configuration
    Validation:
      1) Login web GUI -> Sensors page
      2) Unselect any sensor type category
      3) Select the sensor type back
19. Category: Fix
    Description:
      [158073] - The order of LAN Interface on WebUI not follow SPEC
    Infected Motherboard: H13SSF-P AND ALL
    Affected Functions: Configuration
    Validation:
      1) Login web GUI -> Configuration -> Network
      2) Check order of LAN Interface
20. Category: Fix
    Description:
      [157627] – Hot plug issue in both Windows and Linux OS
    Infected Motherboard: H13SSH-P
    Affected Functions: :
      Validation :
      1) Login WebUI >> System >> Storage Monitoring >> Physical View
      2) Select all slots, press "Eject" or "Insert" button
      3) Each slot will take at least 20 seconds
      4) It should eject or insert successfully
21. Category: Fix
    Description:
      [158084] - System hang on POST code "A2" after executing AC on/off
    Infected Motherboard: H13SSF
    Affected Functions: BIOS hang A2
      Validation :
      1) AC OFF and AC ON , watch the BIOS status not hang on A2.


--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: cf997a79b452cdc4c102a56431f9d4697b4ef3c0

Firmware Version: 01.01.06
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230628_01.01.06_STDsp.bin
Production signed Firmware CRC: 211E3EA6
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230628_01.01.06_STDsp.bin
Production signed eMMC Firmware CRC: 680F6A50
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20230628_01.01.06_STDsp.bin
Production signed SPI NOR Firmware CRC: 417552B5
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230628_01.01.06_STDsd.bin
Debug signed Firmware CRC: B5F82FE4
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230628_01.01.06_STDsd.bin
Debug signed eMMC Firmware CRC: 8EF0EAF0
Build Date: 06/28/2023
Redfish API : Redfish_1_11_API_full_list_20230410
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH H13SSF
---------------------------------------------------------------------------------------------------------
***note 1: BMC version 01.01.00 start supporting Redfish Host interface driver ECM, and BIOS update required.


1. Category: fix
   Description:
     [157041] - AOC-S25GC-i2S thermal sensor will lose when execute dc onoff test item.
     [158504] - NVIDIA AOC Model and Serial # Missing From WebGUI Network AOC Page.
   Infected Motherboard: X13SEDW, X13DEM and ALL
   Affected functions: AOC, Senor
   Validation:
     1) Installed AOC-S25GC-i2S and run cburn DC ON/OFF.
2. Category: fix
   Description:
     [156927] - IPMI ECO Automation tests Failure
   Infected Motherboard: H13SSF-P and ALL
   Affected functions: Configuration
   Validation:
     1) Try TC4010

3. Category: fix
   Description:
     [158209] - X12DPD IPMI 1.03.03 cannot see the U250 sensor
   Infected Motherboard: X12DPD and ALL
   Affected functions: GPU
   Validation:
      1. check Sensor and GPU page

--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 50d7ea5f7c4c06e0cfbda83deed9c4b2c04d4a22

Firmware Version: 01.01.05
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230622_01.01.05_STDsp.bin
Production signed Firmware CRC: 458DAF12
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230622_01.01.05_STDsp.bin
Production signed eMMC Firmware CRC: 1B73D652
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20230622_01.01.05_STDsp.bin
Production signed SPI NOR Firmware CRC: 417552B5
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230622_01.01.05_STDsd.bin
Debug signed Firmware CRC: BBC88D33
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230622_01.01.05_STDsd.bin
Debug signed eMMC Firmware CRC: 972F6591
Build Date: 06/22/2023
Redfish API : Redfish_1_11_API_full_list_20230410
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH H13SSF
---------------------------------------------------------------------------------------------------------
***note 1: BMC version 01.01.00 start supporting Redfish Host interface driver ECM, and BIOS update required.


1. Category: Fix
   Description:
     [158148] - Login RADIUS account.
   Infected Motherboard: X13SEM AND ALL
   Affected Functions: Radius
   Validation:
     1) Navigate to ->  Configuration -> Account Services -> Directory Service
     2) Enable "RADIUS" and set secret/Server Address, then submit success.
     3) Logout and login RADIUS account in WebUI and check whether it could be successful or not.
2. Category: 
   Description:
     [ENGINEERING] - Add inlet temperature
   Infected Motherboard: H13SSF
   Affected Functions: Inlet temperature
     Validation :
     1) WebUI >> System >> Component Info >> Sensor
3. Category: Fix
   Description:
     [156405] - IPMIECO Automation test failed
     [156554] - IPMI ECO automation test failed.
   Infected Motherboard: X13SEM AND ALL
   Affected Functions: Network
   Validation:
     1) Login web, go to Configuration -> Network page, set DNS to Auto obtain and save.
     2) Memo DNS1 and DNS2 ip.
     3) Set lan interface to other and save.
     4) Compare DNS1 and DNS2 ip with step2 memo, still same, pass.
4. Category: Fix
   Description:
     [158195] - During System Lockdown SystemLockdown, Date and Time Auto Daylights Savings Time switch is not disabled when it should be
   Infected Motherboard: X13DET-B AND ALL
   Affected Functions: Configuration
   Validation:
     1) UI > BMC Settings > System Lockdown
     2) System Lockdown ON
     3) UI > BMC Settings > Date and Time
     4) Toggle Audto Daylight Savings Time
     5) Check the switch button
5. Category: Fix
   Description:
     [158151] - "background-color" of input field on both "Network" and "Port" tabs are as same as page background
   Infected Motherboard: X13DET-B AND ALL
   Affected Functions: Configuration
   Validation:
     1) Login Web GUI -> Configuration -> Network
     2) Check Network page
     3) Check Port page
6. Category: Fix
   Description:
     [156548] - Operator health event log advanced settings disabled; License activation Upload button enabled for admin even when no private key file is selected; and one more...
   Infected Motherboard: X12DPD-A6M25 AND ALL
   Affected Functions: Configuration
   Validation:
     1) Login Web GUI -> Maintenance -> License Activation
7. Category: Fix
   Description:
     [157983] - H13SSF MBD does not enable all FANs to FULL SPEED on AC Power UP causing thermal trip on 84 Core AMD CPU
   Infected Motherboard: H13SSF
   Affected Functions: FAN speed, SEL
   Validation:
     1) Power on system and didn't have thermal trip event
8. Category: Fix
   Description:
     [158070] The content loss and incorrect of Share LAN when set option to "Shared-AIOM2" , " Shared-AOC" , " Shared-AIOM1"
   Infected Motherboard: H13SSF AND ALL
   Affected Functions: Network
   Validation:
     1) Login web, power on and wait sensor ready.
     2) Web go to Configuration -> Network page, set lan mode to Shared mode.
     3) Check share lan info value format, pass.
9. Category: Fix
   Description:
     [158062] - "Enable TSIG Authentication" switcher doesn't disable when DDNS is off
   Infected Motherboard: X13SEDW AND ALL
   Affected Functions: Configuration
   Validation:
     1) Login web GUI -> Configuration -> BMC Settings -> Dynamic DNS
     2) Try to enable "Enable TSIG Authentication" switcher
     3) Enable DDNS and input Server address and BMC hostname
     4) Upload TSIG files and save it
     5) Enable TSIG Authentication" switcher should be disabled when DDNS is off
10. Category: Fix
    Description:
      [158007] - Failed Login Attempt Lockout Threshold radio buttons aren't all disabled for Operator and User privilege
    Infected Motherboard: X13SEDW AND ALL
    Affected Functions: Configuration
    Validation:
      1) Login Web GUI as Operator or User privilege
      2) Enter to Account Services page
      3) Unfold Advanced Setting and check all radio buttons
11. Category: Fix
    Description:
      [157245] - Date and Time can't sync NTP server at the first time saved.
    Infected Motherboard: H13SSF
    Affected Functions: Configuration
    Validation:
      1) Login web GUI -> Configuration -> BMC Settings
      2) Disable NTP Server
      3) Change time by ipmitool -I lanplus -H 172.31.3.43 -U ADMIN -P ADMIN sel time set "01/02/2020 01:02:03"
      4) Refresh Date and Time page until see the date time you set
      5) Enable NTP Server, Save
      6) After Web page release back to user, we expect to see correct date time that gets from NTP server
12. Category: Fix
    Description:
      [156715] - Power state ICON not refresh after power cycle complete
    Infected Motherboard: ALL
    Affected Functions: Configuration
    Validation:
      1) Check all PB issues and verify.
13. Category: Fix
    Description:
      [156505] - SNMPv2 Name Special Chars Checking Rule is not match with SPEC.
    Infected Motherboard: X12STW
    Affected Functions: Configuration
    Validation:
      1) Login web GUI -> Configuration -> Notifications -> SNMP
      2) Configuration -> Notifications -> SNMP -> Enable SNMP to "ON"
      3) SNMPv2 -> Press "Add" -> Name -> Input invalid string (e.g. !) -> Press "SAVE"
14. Category: Fix
    Description:
      [157244] Syslog packet not follow RFC3164
      [157353] Syslog packet not follow RFC3164
    Infected Motherboard: ALL
    Affected Functions: Syslog
    Validation:
      1) Web go to Configuration -> Notifications -> Syslog page.
      2) Enable Syslog and enter syslog server ip, press save.
      3) Do some action which will send MEL, e.g. login/logout web
      4) Check syslog server get message format.


--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: a0de5fde1ebb3349cb2e1cfcbbb12ed00c33e272

Firmware Version: 01.01.04
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230609_01.01.04_STDsp.bin
Production signed Firmware CRC: FCDCB3A5
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230609_01.01.04_STDsp.bin
Production signed eMMC Firmware CRC: C4A487B4
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20230609_01.01.04_STDsp.bin
Production signed SPI NOR Firmware CRC: 417552B5
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230609_01.01.04_STDsd.bin
Debug signed Firmware CRC: CA44BB28
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230609_01.01.04_STDsd.bin
Debug signed eMMC Firmware CRC: 80251EDB
Build Date: 06/09/2023
Redfish API : Redfish_1_11_API_full_list_20230410
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH H13SSF
---------------------------------------------------------------------------------------------------------
***note 1: BMC version 01.01.00 start supporting Redfish Host interface driver ECM, and BIOS update required.


1. Category: Fix
   Description:
     [ENGINEERING] - Support new Intel PVC GPU (DID: 0x0BDA)
   Infected Motherboard: ALL
   Affected Functions: GPU sensor and info
   Validation:
     1) Check Sensor Readings -> GPU Temp;
     2) Check System -> Component Info -> GPU;
     3) Check Maintenance -> Firmware Management -> Inventory for GPU info.
2. Category: Fix
   Description:
     [156963] - SUM test TC 002 fail due to the NTP information is not match after preserved update IPMI fw
     [156412] - BMC IP changed after executing SMCIPMITool ipmi raw 30 42
     [156313] - TC0005 call setLANModeCommand failed
     [156376] - It got Error message:145 != 0 "Can't connect to 10.184.14.229" on the X13DSF-A
     Infected Mother board: ALL
   Affected Functions: BMC network
   Validation:
     1) Run CombinedECO SUM test, test case have TC04 and TC05.
     2) SUM test PASS and check BMC ip still same.
3. Category: Feature
   Description:
     [ENGINEERING] - Upgrade the EnternetInterface version from v1.6.2 to v1.6.3 to align spec.
   Infected Motherboard: ALL
   Affected Functions: Redfish
   Validation:
     1) Check EthernetInterface version
4. Category: Fix
   Description:
     [157243] - Radius packet not follow RFC2865"
     [157351] - Radius packet not follow RFC2865"
   Infected Motherboard: H13SSF AND ALL
   Affected Functions: Radius
   Validation:
     1) Enabled Radius.
     2) Use tcpdump to filter packet 'tcpdump -c 25 -i bond0 port 1812 or port 1813 or port 3799'
     3) Check the payload as expected
5. Category: Fix
   Description:
     [157328] - Authentication Protocol and Encryption Protocol Range setting is not match Wiki SPEC(Each field 1.32) for SNMPv3
   Infected Motherboard: X12SPT-PT AND ALL
     Affected Function: WEB GUI
   Validation:
     1) Go to [Configuration] -> [Notifications] ->[SNMP] page
     2) Check SNMPv3 section
     3) The Authentication Protocol options are MD5/SHA1/Account
     4) The Encryption Protocol options are None/DES/AES/Account
6. Category: Fix
   Description:
     [157396] – The error message incorrect when launch more than 4 iKVM sessions
     [157246] – The error message incorrect when launch more than 4 iKVM sessions
   Infected Motherboard: H13SSF, X13SEDW AND ALL
   Affected Functions: HTML5
     Validation :
     1) WebUI >> Remote Control
     2) Open HTML5 iKVM to 5 sessions
     3) The fifth session should show "The maximum number of sessions has been reached!"
7. Category: Fix
   Description:
     [156906] – VM cannot save valid IPv6 address with port
   Infected Motherboard: X13DEM-P AND ALL
   Affected Functions: : Virtual Media
     Validation :
     1) WebUI >> Configuration >> Virtual Media
     2) Edit VM Connection
     Share Host: [2001:db8::a479:496a:961:5670]:1543
     Path to Image: /tmp.iso
     3) Click "Save" button
     4) It should save successfully
8. Category: Fix
   Description:
     [157096] – iKVM default setting is not HTML5 after factory default
   Infected Motherboard: X12SPT-PT AND ALL
   Affected Functions: :  iKVM
     Validation :
     1) Maintenance >> BMC Reset >> Factory Default
     2) WebUI >> Remote Control
     3) Interface should be "HTML 5" after factory default
     4) Check redfish command, it also should be "HTML 5"
9. Category: Fix
   Description:
     [157146] - "Number" should be translated to Simplified Chinese and Japanese at Virtual Media page.
   Infected Motherboard: X13DEM-P AND ALL
   Affected Functions: WEBUI
   Validation:
     1) Login web GUI -> Configuration -> Virtual Media
     2) Change language and check
10. Category: Fix
    Description:
      [157401] - "Export to Excel" button should be translated to Simplified Chinese and Japanese at Sensor page.
    Infected Motherboard: X13SEDW-F AND ALL
    Affected Functions: WEBUI
    Validation:
      1) Login web GUI -> System -> Component Info -> Sensor
      2) Righ Side bar -> Switching language: English/Japanese/Simplified Chinese
      3) Check "Export to Excel" button
11. Category: Fix
    Description:
      [157277] - User name string length only support to 16 not 31 for SNMPv3
    Infected Motherboard: H13SSF-P AND ALL
    Affected Functions: WEBUI
    Validation:
      1) Login web GUI -> Configuration -> Account Services -> Users
      2) Press down 'Add' button
      3) Type in '123456789012345678901234567890123' to 'User Name'
      4) Choice 'SNMP' at 'Account Type'
      5) Check 'User Name'
12. Category: Fix
    Description:
      [157090] - Auto Daylight Savings Time switcher doesn't disable for the Operator and User privilege
    Infected Motherboard: X13SEED AND ALL
    Affected Functions: Web
    Validation:
      1) Login web as Operator or User privilege -> go to BMC setting page
      2) Auto Daylight Savings Time button is grey out
13. Category: Fix
    Description:
      [157242] - Will display a prompt window similar to the one for switching on lockdown mode.
    Infected Motherboard: H13SSF-P AND ALL
    Affected Functions: Configuration
    Validation:
      1) Login web GUI -> Configuration -> BMC Setting -> System Lockdown
      2) Turn 'ON' -> Save
      3) Check the Lock icon at left page
      4) Switch off System Lockdown
      5) It sholud be swich off lockdown without prompt window
14. Category: Feature
    Description:
      [ENGINEERING] - Dark Theme update
    Infected Motherboard: X13/H13/B13/BM4
    Affected Functions: WEBUI
    Validation:
      1) BMC WEBUI new style
15. Category: Fix
    Description:
      [157118] - BIOS automation TC 5006 failed
    Infected Motherboard: X13SEM AND ALL
    Affected Functions: BIOS Update
    Validation:
      1) Update BIOS FW.
      2) Update BIOS golden image.
      3) Ensure System Host is powered up. BIOS active and golden version should
      4) Match in Web GUI FW inventory page.
16. Category: Fix
    Description:
      [154507] – WebUI share LAN interface naming is not matched
    Infected Motherboard: H13SSF-P
    Affected Functions: WEBUI
      Validation :
      1) Plug-in AIOM and AOC cards
      2) Login WebUI >> Configuration >> Network
      3) LAN interface should display correct select buttons
17. Category: Fix
    Description:
      [156701] - Unable to display information when the LAN interface is in shared mode.
      Infected Mothernoard: H13SSF and All
    Affected Functions: Web
    Validation:
      1) Login WebGUI
      2) Network -> Change lan interface to Share-XXX interface, need check all of them.
      3) Network -> share lan info show on page.


--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.01.03
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230526_01.01.03_STDsp.bin
Production signed Firmware CRC: F4E1D235
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230526_01.01.03_STDsp.bin
Production signed eMMC Firmware CRC: 8CEF8B46
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20230526_01.01.03_STDsp.bin
Production signed SPI NOR Firmware CRC: 417552B5
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230526_01.01.03_STDsd.bin
Debug signed Firmware CRC: 7AD64E02
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230526_01.01.03_STDsd.bin
Debug signed eMMC Firmware CRC: 70C18693
Build Date: 05/26/2023
GIT SHA: d43cc93c19ace247f58765f7f5daba4b890584e1
Redfish API : Redfish_1_11_API_full_list_20230410
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH H13SSF
---------------------------------------------------------------------------------------------------------
***note 1: BMC version 01.01.00 start supporting Redfish Host interface driver ECM, and BIOS update required.


1. Category: Fix
   Description:
     [154728] – System crash log content is empty when the AMD RAS tool triggers a CPU error
   Infected Motherboard: H13SSF-P
   Affected Functions: :
     Validation :
     1) Test IPMI raw command 0x30 0x80 0x00 0x01
     2) Login WebUI >> Maintenance >> Troubleshooting
     3) Download crash dump log
     4) The log should have correct content
2. Category: New
   Description:
     [ENGINEERING] - support BPN-NVME5-HS219N-S24 SATA mode on JRSI2C1
   Infected Motherboard: H13SSH
   Affected Functions: BPN-NVME5-HS219N-S24 SATA mode
   Validation:
     1) BPN-NVME5-HS219N-S24 support NVME or NVME+SAS on JNVI2C1
     2) BPN-NVME5-HS219N-S24 support SATA only on JRSI2C1
     3) Check storage page
3. Category: Fix
   Description:
     [157100] - Buttons and icons of Virtual Media page can operate while System Lockdown enable
   Infected Motherboard: ALL
   Affected Functions: Configuration
   Validation:
     1) Login web GUI -> Configuration -> BMC Setting -> System Lockdown
     2) Turn 'ON' -> Save
     3) Configuration -> Virtual Media
4. Category: Fix
   Description:
     [156892] - [IPMI ECO 01.01.01] Redfish automtion test fail
     [154769] - Redfish automation test failed
     [156925] - [IPMI ECO 01.01.02] Redfish automtion test fail.
     [156146] - SATC Redfish Automation Test Failed
     [156900] - Redfish automation test failed.
   Infected Motherboard: X13
   Affected Functions: Redfish
   Validation:
     1) Run SATC automation
     2) Test with DMTF Service validator, The NTPEnable case can pass.
5. Category: Enhancement
   Description:
     [ENGINEERING] - Retrieve BIOS version from 'OFID'
   Infected Motherboard: ALL
   Affected Functions: BIOS build date + revision get
   Validation:
     1) Prepare OEM BIOS FW.
     2) Update BIOS
     3) Check that BIOS ver in inventory and in OEM BIOS binary match.
6. Category: Fix
   Description:
     [155145] - With HBM CPU, only partial memory modules are listed in IPMI Web GUI memory info
   Infected Motherboard: ALL
   Affected Functions: Web Redfish
   Validation:
     1) Setup SUT with HBM CPU and DIMM
     2) Web Login -> System->Component Info-> Memory->should display HBM memory and regular DIMM
     3) Redfish GET /redfish/v1/Systems/1/Memory/%d -> show HBM memory or DIMM information
7. Category: Fix
   Description:
     [156778] - BMC GUI sensor arrangement order is not stable.
   Infected Motherboard: ALL
   Affected Functions: Configuration
   Validation:
     1) Login web GUI -> Sensor Readings
     2) Check sensor order


--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.01.02
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230516_01.01.02_STDsp.bin
Production signed Firmware CRC: 503AFD50
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230516_01.01.02_STDsp.bin
Production signed eMMC Firmware CRC: E9829583
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20230516_01.01.02_STDsp.bin
Production signed SPI NOR Firmware CRC: 417552B5
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230516_01.01.02_STDsd.bin
Debug signed Firmware CRC: 91AE6A5F
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230516_01.01.02_STDsd.bin
Debug signed eMMC Firmware CRC: 5A0F936E
Build Date: 05/16/2023
GIT SHA: 67717acc1db5b635d6dc464664f9479ad79d56da
Redfish API : Redfish_1_11_API_full_list_20230410
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH H13SSF
---------------------------------------------------------------------------------------------------------


1. Category: New
   Description:
     [ENGINEERING] - Auto Daylight Saving Time
   Infected Motherboard: ALL
   Affected Functions: IPMI OEMcmd Redfish Web
   Validation:
     1) Ex. (UTC-08:00) Pacific Time (US & Canada)
     2) Ipmitool sel time time '03/10/2024 01:59:50'
     3) Wait 10s
     4) Expected time get is 03/10/2024 03:00:00
     5) Ipmitool sel time time '11/03/2024 01:59:50'
     6) Wait 10s
     7) Expected time get is 11/03/2024 01:00:00
     8) OEMcmd GET 0x30 0x68 0x01 0x0 0x0
     9) SET 0x30 0x68 0x01 0x1 0x0 0x1 0x0a 0x01 -> last three bytes (0x01 ntp on, 0x0a timezone index, 0x01 autoDST enabled)
     10) Redfish GET or PATCH /redfish/v1/Managers/1/ get or patch datetime, timezone, autoDST
2. Category: Fix
   Description:
     [155964] - VM mount issue
   Infected Motherboard: H13SSH-P
   Affected Functions: Configuration
   Validation:
     1) IPMI Web -> Configuration -> Virtual Media
3. Category: Fix
   Description:
     [ENGINEERING] - Fix ipmi lan set ipsrc for dhcp to static ip missing.
   Infected Motherboard: ALL
   Affected Functions: Network
   Validation:
     1) In DHCP mode then ipmitool lan set 1 ipsrc static. check the ip can be set back.
4. Category: Fix
   Description:
     [156006] –Platform Resiliency Action event log will use 1970 timezone under MEL
   Infected Motherboard: H13SSF-P
   Validation:
     1) Update golden BMC then check MEL timestamp should not display 1970 unless user didn’t set time.


--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.01.01
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230429_01.01.01_STDsp.bin
Production signed Firmware CRC: 5C149F56
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230429_01.01.01_STDsp.bin
Production signed eMMC Firmware CRC: 7EC60E88
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20230429_01.01.01_STDsp.bin
Production signed SPI NOR Firmware CRC: 1CECBA97
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230429_01.01.01_STDsd.bin
Debug signed Firmware CRC: F5A6787D
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230429_01.01.01_STDsd.bin
Debug signed eMMC Firmware CRC: A56D7841
Build Date: 04/29/2023
Redfish API : Redfish_1_11_API_full_list_20230410
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH H13SSF
---------------------------------------------------------------------------------------------------------


1. Category: Fix
   Description:
     [156020] - Unable to close popup window under System lockdown mode
   Infected Motherboard: H13SSH and All
   Affected Function: Storage
   Validation:
     1) Login webgui
     2) Enable System lockdown mode
     3) Go to  Storage Monitoring page
     4) Visit Controller View page
     5) Click the lock sign which is on left button side.
     6) (a) Disable system lockdown mode and then click Close or Save button.
        (b) Or after step 5, directly go to Dynamic DNS age and then click OK button.

2. Category: fix
   Description:
     [152652] - [MEL-0028] AD related MEL should not shown when setup LDAP and Radius
   Infected Motherboard: X13DSF-A and All
   Affected functions: All
   Validation:
     1) Modify IPv4 addr(WebUi/Redfish) can get success response.
     2) Modify AD Setting check no MEL-0023.
     3) Patch
        {"StaticNameServers": ["10.135.0.250","10.135.0.251"]  } should success.
        {"StaticNameServers": ["10.135.0.250","10.135.0.250"]  } should fail.

3. Category: fix
   Description:
     [156022] User is able to click delete button on system lockdown mode
   Infected Motherboard: H13SSH and All
   Affected functions: Configuration
   Validation:
     1) Login web GUI -> Maintenance -> Firmware Management -> perform Upload BIOS
     2) BMC Setting -> System Lockdown
     3) Turn 'ON' -> Save
     4) Maintenance -> Task List
     5) Now 'del task' button should not be display during System Lockdown

4. Category: feature
   Description:
      [ENGINEERING] - Task Queue & Task List
   Infected Motherboard: All
   Affected functions: Configuration
   Validation:
     1) IPMI Web -> System -> Storage Monitoring -> Task Queue
     2) Maintenance -> Task List

5. Category: fix
   Description:
     [154722] - DMTF/Redfish standard API support test failed
   Infected Motherboard: H13SSF and All
   Affected functions: All
   Validation:
     1. Test with DMTF Service validator, no unexpected fail.

6. Category: fix
   Description:
     [155359] - Webgui crashed after uploading product key with invalid file
   Infected Motherboard: H13SSH and All
   Affected functions: Configuration
   Validation:
     1) IPMI Web -> Maintenance -> License Activation
     2) Select File -> Upload -> Save

5. Category: Fix
   Description:
     [155592] - Fail to use SecureErase with SAS 3816 IR card on X13SEM-F
   Infected Motherboard: X13SEM and All
   Affected functions: BRCM
   Validation:
     1) Install SAS 3816IR on X13SEM-F
     2) Login to WebGUI and enter to System > Storage Monitoring.
     3) Press Physical View tab.
     4) Select some HDD and do the Disk Erase.
     5) Check the progress whether 100% completed in Task List.

6. Category: fix
   Description:
     [156012] - IP changed after running raw command
   Infected Motherboard: H13SSH and All
   Affected functions: All
   Validation:
     1) no ip change occur after BMC update 
	 2) no ip change occur after raw command 0x30 0x42

7. Category: Fix
   Description:
    [ENGINEERING] - Network Setting Page Can Now Save With Only 1 Dedicated LAN Speed Capability
   Infected Motherboard: ALL
   Affected functions: Network
   Validation:
    1) Navigate to "Network" on the web GUI
    2) Query Redfish API "/redfish/v1/Managers/1/EthernetInterfaces/1"
    3) If there is only 1 value in "SpeedMbps@Redfish.AllowableValues", clicking "Save" on
       web page should be successful.

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.01.00
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230421_01.01.00_STDsp.bin
Production signed Firmware CRC: 9ABC44F2
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230421_01.01.00_STDsp.bin
Production signed eMMC Firmware CRC: 2A0DA764
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20230421_01.01.00_STDsp.bin
Production signed SPI NOR Firmware CRC: 1CECBA97
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230421_01.01.00_STDsd.bin
Debug signed Firmware CRC: 3A367144
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230421_01.01.00_STDsd.bin
Debug signed eMMC Firmware CRC: F89E0330
Build Date: 04/21/2023
Redfish API : Redfish 2020.3
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH H13SSF
---------------------------------------------------------------------------------------------------------


1. Category: feature
   Description:
     [ENGINEERING] - Redfish 2020.3 related feature
	 [ENGINEERING] - network enhancement feature
	 [ENGINEERING] - MEL 1.05 and SEL 1.36
	 [154769] - Redfish automation test failed
	 [150623] - The System Information test fail (Computer System:UUID is not AIOM LAN1 MAC,Processor:Current Clock Speed is abnormal)
	 [153747] - The System Information test fail lack the Processor:Current Clock Speed(MHz)
   Infected Motherboard: All
   Affected functions: All
   Validation:
     1) SW_LAB & Redfish SATC.

2.  Category: enhancement
    Description:
      [151306] - KVM launched and closed MEL should display user ID
    Infected Motherboard: X12STW-F and ALL
    Affected functions:
    Validation :
      1) WebUI >> Remote Control
      2) Launch HTML5 console
      3) Close HTML5 console
      4) KVM session ID of MEL should be user ID.

3. Category: fix
   Description:
     [155558] - SystemLockdown System Lockdown Storage Monitoring Physical View buttons are enabled while drive selection is disabled
   Infected Motherboard: X12DPD-A6M25-P and ALL
   Affected functions: Configuration
   Validation:
     1) Login web GUI -> Configuration -> BMC Setting -> System Lockdown
     2) Turn 'ON' -> Save
     3) System -> Storage Monitoring -> check Button state

4. Category: fix
   Description:
     [155719] - [Redfish] expect length of ServiceAddresses to be 1 but is actually 3	
   Infected Motherboard: H13SSH and ALL
   Affected functions: Configuration
   Validation:
     1) PATCH https://bmcip/redfish/v1/AccountService/ with body {"LDAP": {"ServiceAddresses": ["ldap://serverIP:389"]}}
     2) GET https://[IP)/redfish/v1/AccountService/
     3) The ServiceAddresses part should only showing one service address that we just patched.

5. Category: fix
   Description:
     [151836] - change BIOS password fail
   Infected Motherboard: X13DEM and ALL
   Affected functions: Configuration
   Validation:
     1) set BIOS AdministratorPassword through Redfish.
     2) set BIOS UserPassword through Redfish.

6. Category: fix
   Description:
     [155235] - MEL Log msg is incorrect when configure Syslog.
	 [155473] - Saving Syslog produces MEL even when there are no changes in the values.
   Infected Motherboard: X12DPT-PT6 and ALL
   Affected functions: Configuration
   Validation:
     1) Login WEB with ADMIN.
     2) Notifications ->Syslog→->Enable Syslog to "ON"
     3) Input value in Syslog Server ->Press "SAVE"
     4) Maintenance ->Maintenance Event Log

7. Category: fix
   Description:
     [155582] - Chassis intrusion Reset button not grey out when System Lockdown Mode is on
   Infected Motherboard: X13SCW-F-P and ALL
   Affected functions: Configuration
   Validation:
     1) Login web GUI -> Configuration -> BMC Setting -> System Lockdown
     2) Turn 'ON' -> Save
     3) Sensor Readings -> check Intrusion Reset button

8. Category: Fix
   Description:
     [ENGINEERING] - AOC-S25G-m2S sensor temp drop
   Infected Motherboard: ALL
   Affected functions: AOC sensor reading
   Validation:
     1) Install 2X AOC-S25G-m2S.
     2) Stress off/on testing. The AOC sensor reading should be there.

9.  Category:
    Description:
      [154384]Setting the default fan mode to Standard Speed fan mode.
    Infected Motherboard: H13SSF
    Affected functions: Fan mode
    Validation :
       1) WebUI >> System >> Component Info >> Fan
          Default is "Standard Speed fan mode".


--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.00.36
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230414_01.00.36_STDsp.bin
Production signed Firmware CRC: F99F23BE
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230414_01.00.36_STDsp.bin
Production signed eMMC Firmware CRC: E17D5DDB
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20230414_01.00.36_STDsp.bin
Production signed SPI NOR Firmware CRC: A8247CC4
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230414_01.00.36_STDsd.bin
Debug signed Firmware CRC: B5E0DE01
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230414_01.00.36_STDsd.bin
Debug signed eMMC Firmware CRC: DF1B3186
Build Date: 04/14/2023
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH H13SSF
---------------------------------------------------------------------------------------------------------


1. Category: fix
   Description:
     [155350] - H13 DCMI power no reading
   Infected Motherboard: H13SSH
   Affected functions: IPMI
   Validation:
     1) Use ipmitool to run dcmi power reading

2. Category: Fix
   Description:
    [155348] - 8th FAN unable to display in WebGUI
   Infected Motherboard: H13SSH
   Affected functions: FAN8
   Validation:
    1) Install FAN8 and check sensor reading

3.  Category:
    Description:
      [154384] - Remove PUE2 and Optimal mode, and add Standard Mode.
    Infected Motherboard: H13SSF
    Affected functions: Fan mode
    Validation :
       1) WebUI >> System >> Component Info >> Fan
          Fan mode will show "Standard Speed", "Full Speed", and "Heavy I/O Speed Mode"

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.00.35
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230407_01.00.35_STDsp.bin
Production signed Firmware CRC: 217CD42B
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230407_01.00.35_STDsp.bin
Production signed eMMC Firmware CRC: A5747B90
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20230407_01.00.35_STDsp.bin
Production signed SPI NOR Firmware CRC: A8247CC4
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230407_01.00.35_STDsd.bin
Debug signed Firmware CRC: 035D1D28
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230407_01.00.35_STDsd.bin
Debug signed eMMC Firmware CRC: F54C2371
Build Date: 04/07/2023
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH H13SSF
---------------------------------------------------------------------------------------------------------


1.  Category:
    Description:
      [153264] - IPMI sensor readings don't match Hardware_Monitor_Sensor spec
    Infected Motherboard: H13SSF
    Affected functions:
    Validation :
      1) WebUI >> System >> Component Info >> Sensor, the sensor namings are as sensor spec.

2. Category: fix
   Description:
     [154487] - Web session was not set to default value after "Remove current settings and restore to factory default
   Infected Motherboard: H13SSH
   Affected functions: All
   Validation:
     1) Check web session reset to default 30.
     2) Save Ipmi Configuration then reload IPMI Configuration, check the web session reload to current value.

3. Category: fix
   Description:
     [ENGINEERING] - Accept IP access control with prefix 0
   Infected Motherboard: ALL
   Affected functions: Web, Redfish
   Validation:
     1) Add an IP access control rule with prefix 0 on web page
     2) POST request on /redfish/v1/Managers/1/Oem/Supermicro/IPAccessControl/FilterRules with prefix 0

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.00.34
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230327_01.00.34_STDsp.bin
Production signed Firmware CRC: 5F83403A
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230327_01.00.34_STDsp.bin
Production signed eMMC Firmware CRC: 8B1780E3
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20230327_01.00.34_STDsp.bin
Production signed SPI NOR Firmware CRC: A8247CC4
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230327_01.00.34_STDsd.bin
Debug signed Firmware CRC: 4FA167F4
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230327_01.00.34_STDsd.bin
Debug signed eMMC Firmware CRC: E92C36CF
Build Date: 03/27/2023
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH H13SSF
---------------------------------------------------------------------------------------------------------


1.  Category:
    Description:
      [ENGINEERING] - Modify the data length check of OOB preserve command - 0x30 0xA0 0x15
    Infected Motherboard: X13 H13
    Affected functions: GetClearSMBIOSEraseFlag function
    Validation :
       1) run IPMI raw command raw 0x30 0xa0 0x15 0x0 should be successful.

2. Category: Fix
   Description:
     [ENGINEERING] - correct UUID format
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
      1) Get /redfish/v1/Systems/1, the UUID is the same as BIOS

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.00.33
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230317_01.00.33_STDsp.bin
Production signed Firmware CRC: 12538517
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230317_01.00.33_STDsp.bin
Production signed eMMC Firmware CRC: 17F59F20
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20230317_01.00.33_STDsp.bin
Production signed SPI NOR Firmware CRC: A8247CC4
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230317_01.00.33_STDsd.bin
Debug signed Firmware CRC: 4C6119B6
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230317_01.00.33_STDsd.bin
Debug signed eMMC Firmware CRC: 3BDE9263
Build Date: 03/17/2023
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH H13SSF
---------------------------------------------------------------------------------------------------------


1.  Category: fix
    Description:
      [153084] - Onboard have 8 Fan headers (FAN1~FAN8), but IPMI Fan list only shows FAN1~FAN7
      [153624] - M.2 has no sensor reading.
      [ENGINEERING] - Remove Inlet temp
    Infected Motherboard: H13SSF
    Affected functions: sensor
    Validation :
       1) WebUI >> System >> Component Info >> Fan
          Web can see FAN1~FAN8 as expected.
       2) WebUI >> System >> Component Info >> Sensors
          Web can see the M.2 SSD temperature.

2.  Category: fix
    Description:
      [ENGINEERING] - support NVME storage and BPN CPLD update
    Infected Motherboard: H13SSF
    Affected functions: BPN
    Validation :
       1) check NVME storage info and BPN CPLD update function.

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.00.32
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230309_01.00.32_STDsp.bin
Production signed Firmware CRC: 56F0A366
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230309_01.00.32_STDsp.bin
Production signed eMMC Firmware CRC: 96B8385C
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20230309_01.00.32_STDsp.bin
Production signed SPI NOR Firmware CRC: A8247CC4
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230309_01.00.32_STDsd.bin
Debug signed Firmware CRC: ED966B82
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230309_01.00.32_STDsd.bin
Debug signed eMMC Firmware CRC: 5FC7615A
Build Date: 03/09/2023
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH H13SSF
---------------------------------------------------------------------------------------------------------


1. Category: Fix
   Description:
     [ENGINEERING] - Support NVME BPN-NVME5-HS219N-S24
   Infected Motherboard: H13SSH
   Affected functions: storage
   Validation:
     1) check storage webpage

2. Category: Fix
   Description:
     [ENGINEERING] - remove FAN2 on 2U system
   Infected Motherboard: H13SSH
   Affected functions: FAN
   Validation:
    1) 1U has 8 FANs
    2) 2U has 4 FANs, 1,3,5,7

3. Category: Fix
   Description:
    [ENGINEERING] Fix - DIMM temp missing in IPMI for Micron MEM-DR564L-CL01-ER48 DIMMs with PN FGFF
   Infected MotherBoards: H13
   Affected Function: DIMM Temperature
   Validation:
    1) Check DIMM Temperature under "Component Info"->"Sensor"
    2) Check DIMM Temperature with IPMI Command (raw 0x30 0x94)

4. aplly the common fix reported in other platforms.
   [152600] - Redfish accountService commands error messages didn't match with expected
   [153024] - Deactivated and activated license MEL are inconsistent
   [153444] - Incorrect MEL "SMTP User Name was configured to successfully".
   [153347] - Patch DNS server thru redfish command, webgui doesn?t show outcome accordingly

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.00.31
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230217_01.00.31_STDsp.bin
Production signed Firmware CRC: CE2449B7
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230217_01.00.31_STDsp.bin
Production signed eMMC Firmware CRC: EF1F5BB7
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20230217_01.00.31_STDsp.bin
Production signed SPI NOR Firmware CRC: A8247CC4
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230217_01.00.31_STDsd.bin
Debug signed Firmware CRC: 99C03E35
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230217_01.00.31_STDsd.bin
Debug signed eMMC Firmware CRC: CAE2BDD7
Build Date: 02/17/2023
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH H13SSF
---------------------------------------------------------------------------------------------------------


1. Category: new feature
   Description:
    [ENGINEERING] - Support Motherboard CPLD Golden Image Version Display
   Infected Motherboard: MB with ROT 2.0
   Affected functions: Firmware Inventory
   Validation:
    1) Navigate to "Maintenance" -> "Firmware Management" -> "Inventory"
    2) "CPLD Motherboard Golden" should now be displayed along with its version.
    3) Redfish API to GET "/redfish/v1/UpdateService/FirmwareInventory/Golden_CPLD_Motherboard"
    4) IPMI OEMCMD to get "CPLD Motherboard Golden" Version: raw 0x30 0x68 0x28 0x06 0x02 0x02

2. Category: new feature
   Description:
    [ENGINEERING] - Support Motherboard CPLD Golden Image Update
   Infected Motherboard: MB with ROT 2.0
   Affected functions: Firmware Resiliency
   Validation:
    1) Navigate to "Maintenance" -> "Firmware Management" -> "Inventory"
    2) Click "Platform Resiliency Actions" button
    3) "CPLD Motherboard" and "CPLD Motherboard Golden" should now be listed
    4) Check the box next to "CPLD Motherboard Golden" allows "Update" to be performed. It will automatically trigger BMC reboot to perform.
    5) Redfish API to POST "/redfish/v1/UpdateService/Actions/Oem/SmcUpdateService.Install" with below parameters
        {
            "Targets":["/redfish/v1/UpdateService/FirmwareInventory/CPLD_Motherboard"],
            "InstallOptions":["UpdateGolden"]
        }
    6) IPMI OEMCMD to update CPLD Motherboard Golden image: raw 0x30 0x68 0x28 0x20 0x05 then raw 0x30 0x68 0x2b to reboot BMC

2. Category: Critical Issue
   Description:
    [152436] - DIMMs display yellow health status in WebGUI
   Infected MotherBoards: H13SSH
   Affected functions: Dimm Health Status
   Validation:
    1. Check Dimm Health Status in WebGUI


--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.00.29
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230201_01.00.29_STDsp.bin
Production signed Firmware CRC: 03249325
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230201_01.00.29_STDsp.bin
Production signed eMMC Firmware CRC: B35D1E4C
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20230201_01.00.29_STDsp.bin
Production signed SPI NOR Firmware CRC: A8247CC4
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230201_01.00.29_STDsd.bin
Debug signed Firmware CRC: 5D02F34A
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230201_01.00.29_STDsd.bin
Debug signed eMMC Firmware CRC: 9F62EFC1
Build Date: 02/01/2023
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH H13SSF
---------------------------------------------------------------------------------------------------------


1. Category: fix
   Description:
     [151770] - Port save without changes error message
   Infected Motherboard: All
   Affected functions: Configuration
   Validation:
     1) Log into IPMI Web -> Configuration -> Network -> Port
     2) Don't do any change and click on Save. The message will be "Nothing has been changed".

2. Category: fix
   Description:
     [151712] - Should not show Warning message after changing syslog Server with an illegal syslog server
   Infected Motherboard: All
   Affected functions: Configuration
   Validation:
     1) Log into IPMI Web -> Configuration -> Notifications -> Syslog
     2) Select Enable and Modify syslog sever with an illegal ip (ex: 1. 1. .1)
     3) Select Disable, the message "It is illegal IP format!" will be gone.

3. Category: fix
   Description:
     [151950] - CPU In Yellow Health Status After Flashing IPMI FW 1.00.28
     [151970] - "System" tab on IPMI web gui keep turning yellow during "On/Off" test, with only on IPMI version 01.00.28.
   Infected Motherboard: ALL
   Affected functions: health status
   Validation:
     1) Check "System" tab on IPMI web gui. it should be green if there is abnormal health.

4. Category: fix
   Description:
     [145276] - help page link naming confirm.
   Infected Motherboard: X13SEED and All
   Affected functions: Configuration
   Validation:
     1) IPMI Web -> Open Help page
     2) Check "BMC User Guide X13 H13.pdf" download link

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.00.28
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230130_01.00.28_STDsp.bin
Production signed Firmware CRC: 91A686C0
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230130_01.00.28_STDsp.bin
Production signed eMMC Firmware CRC: 02581658
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20230130_01.00.28_STDsp.bin
Production signed SPI NOR Firmware CRC: 3452F243
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230130_01.00.28_STDsd.bin
Debug signed Firmware CRC: B0F9ACEE
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230130_01.00.28_STDsd.bin
Debug signed eMMC Firmware CRC: 511EAD94
Build Date: 01/30/2023
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH H13SSF
---------------------------------------------------------------------------------------------------------


1. Category: fix
   Description:
     [151257] - FD Reset ADMIN/ADMIN Does Not Work After UID Button 12s Factory
     [151244] - FD Reset ADMIN/ADMIN Does Not Work After Factory Default Reset
   Infected Motherboard: X13DET-B, X12DPT-B6 and ALL
   Affected functions: Factory default function
   Validation:
     1) Press UID button over 12s to make BMC factory default
     2) Do factory default to ADMIN/ADMIN in web
     3) Login web with ADMIN/ADMIN

2. Category: fix
   Description:
     [150675] - AOC-653105A-HDAT and AOC-MCX515A-CCAT can't detected PN and SN under BMC Web.
   Infected Motherboard: X13DEM and ALL
   Affected functions: Network AOC
   Validation:
     1) Install card and check Network AOC page of BMC web.

3. Category: fix
   Description:
     [151085] - New added link IPV6 addresses are unavailable
   Infected Motherboard: X13OEI and ALL
   Affected functions: Configuration
   Validation:
     1) IPMI Web -> Configuration -> Network
     2) Check 'Address List' dropdown list on 'IPv6'

4. Category: fix
   Description:
     [151231] - Multi Node attribute 'POST CODE' is wrong when translated to Japanese and Simple Chinese
   Infected Motherboard: X12DPT-PT6 and ALL
   Affected functions: Configuration
   Validation:
     1) IPMI Web -> System -> Multi Node
     2) Check the 'POST CODE' translation

5. Category: fix
   Description:
     [150757] - The Introduction about Remote Control is incorrect at HELP page
   Infected Motherboard: X12DPT-PT6 and ALL
   Affected functions: Configuration
   Validation:
     1) IPMI Web -> Help -> Remote Control
     2) Check picture

6. Category: new
   Description:
     [ENGINEERING] - support RTX 3090 GPU card.
   Infected Motherboard: ALL
   Affected functions:  IPMI
   Validation:
     1) Check BMC web site, "Sensor Reading" -> "Sensors", the GPU temp sensor should be there.
     2) Check BMC web site, "Sensor Reading" -> "GPU", GPU card information should be listed.

7. Category: fix
   Description:
     [ENGINEERING] - BMC reset for new SSL certificate to take effect,
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) Upload the SSL certificate.
     2) Check there is a dialog to ask the user to confirm whether to reset the BMC.
     3) Click 'OK'.
     4) Check the BMC is reset and the new certificate has taken effect.

8. Category: fix
   Description:
     [149433] fix - H13SSH Redfish missing or incorrect power and thermal parameters
   Infected Motherboard: H13
   Affected functions: IPMI
   Validation:
     1) GET request on Chassis/1/Power, "PowerConsumedWatts" should between "MinConsumedWatts" and "MaxConsumedWatts"

9.  Category: new
    Description:
      [ENGINEERING] - support H13SSF
    Infected Motherboard: H13SSF
    Affected functions: ALL
    Validation : NA

10.  Category: fix
    Description:
      [150342] – SPM REST API test failed
    Infected Motherboard: H13SSH
    Affected functions:
    Validation :
      1) Test IPMI raw command 0x30 0x80 0x01 0x2
      2) BMC should respond correct data

11.  Category: fix
    Description:
      [147931] - on-board sensor not available
    Infected Motherboard: H13SSH
    Affected functions: Sensor
    Validation :
      1) Check with BIOS team to get new BIOS to support new location
      2) Check sensor reading and location

12.  Category: fix
    Description:
      [150295] - Superdiag report has memory detection issue.
    Infected Motherboard: H13SSH
    Affected functions: Superdiag
    Validation :
      1) Superdiag is using IPMI raw command 0x30 0x94
      2) Run IPMI command to read specific DIMM memory temperature
         raw 0x30 0x94 <cpu_no> <channel> <slot>
         read H13SSH - DIMMA2: ipmitool -H BMCIP -U ADMIN -P ADMIN raw 0x30 0x94 0 0 1
         read H13SSH - DIMMG2: ipmitool -H BMCIP -U ADMIN -P ADMIN raw 0x30 0x94 0 6 1
      3) Run IPMI command to read all DIMM memory temperatures
         if installed H13SSH - DIMMA2, DIMMG2, read all DIMMs in one command: 
         ipmitool -H BMCIP -U ADMIN -P ADMIN raw 0x30 0x94, the response data format:
         DIMMA1 DIMMA2 DIMMB1 DIMMB2 DIMMC1 DIMMC2 DIMMD1 DIMMD2 DIMME1 DIMME2 DIMMF1 DIMMF2 DIMMG1 DIMMG2 DIMMH1 DIMMH2
         DIMMI1 DIMMI2 DIMMJ1 DIMMJ2 DIMMK1 DIMMK2 DIMML1 DIMML2 .....

13. Category: fix
   Description:
     [151769]- IPMI config web session not saved
   Infected Motherboard: B12DPT-6 and All
   Affected functions: Web
   Validation:
     1) Login WebGUI -> Configuration -> BMC Settings -> Web Session -> save
     2) IPMI Configuration -> Download "save_config.bin"-> reload save_config.bin
     3) web session timeout value shold be restored

14. Category: fix
   Description:
     [151734]- Not clear MEL when saving hostname
   Infected Motherboard: B12SPE and All
   Affected functions: Web
   Validation:
     1) Login WebGUI -> Goto network page -> Save -> Check MEL

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.00.25
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230104_01.00.25_STDsp.bin
Production signed Firmware CRC: 0812E8AB
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230104_01.00.25_STDsp.bin
Production signed eMMC Firmware CRC: 87845D44
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20230104_01.00.25_STDsp.bin
Production signed SPI NOR Firmware CRC: 3452F243
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20230104_01.00.25_STDsd.bin
Debug signed Firmware CRC: 9F5C95F4
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20230104_01.00.25_STDsd.bin
Debug signed eMMC Firmware CRC: 62D3B1F9
Build Date: 01/04/2023
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH
---------------------------------------------------------------------------------------------------------


1. Category: enhancement
   Description:
     [ENGINEERING] Change fan policy to single fan zone
   Infected MotherBoards: H13SSH
   Affected functions: Fan Policy
   Validation:
     1) Verify BMC fan policy

2. Category: fix
   Description:
     [ENGINEERING] - Extend the size limitation of certificate and key files
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) POST /redfish/v1/UpdateService/Oem/Supermicro/SSLCert/Actions/SmcSSLCert.Upload
             with cert_file and key_file total size <= 30K bytes
     2) Check /nv/server.pem could be created and contains the cert_file and key_file

3. Category: Feature
   Description:
     [ENGINEERING] - Add HotSpare in Redfish API and WEBUI
   Infected Motherboard: ALL
   Affected functions: Redfish and WEBUI
   Validation:
     WEBUI:
     1) Install 3908 and HDDs;
     2) Create RAID; (1 or 5)
     3) Check Storage->Physical View;
     4) Test hot spare functions;
     Redfish:
     1) Check HotSpare payload by GET /redfish/v1/Chassis/HA-RAID.[idx].StorageEnclosure.[idx]/Drives/Disk.Bay.[idx]/Oem/Supermicro/AssignSpareActionInfo
     2) Assign HotSpare by POST /redfish/v1/Chassis/HA-RAID.[idx].StorageEnclosure.[idx]/Drives/Disk.Bay.[idx]/Actions/Oem/SmcDrive.AssignSpare
     3) Delete HotSpare by POST /redfish/v1/Chassis/HA-RAID.[idx].StorageEnclosure.[idx]/Drives/Disk.Bay.[idx]/Actions/Oem/SmcDrive.DeleteSpare

4. Category: Fix
   Description:
     [149334] -The health event log (SEL Version, Free Space, Recent Added /Erased time is empty
   Infected Motherboard: X13SEDW and ALL 
   Affected functions: EventLog
   Validation:
     1) run sel info and sel clear via SMCIPMITool

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 01.00.24
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20221222_01.00.24_STDsp.bin
Production signed Firmware CRC: EC36969A
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20221222_01.00.24_STDsp.bin
Production signed eMMC Firmware CRC: E5BFFF50
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20221222_01.00.24_STDsp.bin
Production signed SPI NOR Firmware CRC: 3452F243
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20221222_01.00.24_STDsd.bin
Debug signed Firmware CRC: 3DA994C5
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20221222_01.00.24_STDsd.bin
Debug signed eMMC Firmware CRC: 46396CED
Build Date: 12/22/2022
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH
---------------------------------------------------------------------------------------------------------


1. Category: fix
   Description:
     [ENGINEERING] - remove rollback ID configuration page, rollback ID always update when fw update.
   Infected Motherboard: ALL
   Affected functions: Web
   Validation:
     1) check Firmware Management page-> update
     2) no rollback ID configuration page.

2. Category: fix
   Description:
     [ENGINEERING] - Support Xilinx U250 GPU
   Infected Motherboard: ALL
   Affected functions: GPU
   Validation:
      1) check Sensor and GPU page

3. Category: fix
   Description:
     [150308] - Firmware inventory missing backup/golden images.
   Infected Motherboard: H13SSH and All
   Affected functions: Web
   Validation:
      1) check Firmware Management page

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 00.00.07
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20221214_00.00.07_STDsp.bin
Production signed Firmware CRC: F65F9CDD
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20221214_00.00.07_STDsp.bin
Production signed eMMC Firmware CRC: AA2301CE
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20221214_00.00.07_STDsp.bin
Production signed SPI NOR Firmware CRC: 3452F243
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20221214_00.00.07_STDsd.bin
Debug signed Firmware CRC: 5106F6A2
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20221214_00.00.07_STDsd.bin
Debug signed eMMC Firmware CRC: 7F63FA53
Build Date: 12/14/2022
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH
---------------------------------------------------------------------------------------------------------


1.Category: Fix
  Description:
    [149079] - BMC_not_displaying_capacity_for_Kioxia_CD6_drive_in_BMC_WebGUI
  Infected Motherboard: X13DEM and ALL
  Affected Function: storage
  Validation:
    1)Install KCD6XLUL3T84 on system
    2)Check NVMe information from Storage page

2. Category: fix
   Description:
     [149172] - Error HTTP message format at X13 and X12 redfish (/redfish/{string}.IKVM)
   Infected Motherboard: H12SSFF and ALL
   Affected functions: Redfish
   Validation:
     1) Use PATCH access /redfish/v1/Managers/1/Oem/Supermicro/IKVM with data
        {"Current interface":"HTML 5"}
     2) Use GET access /redfish/v1/Managers/1/Oem/Supermicro/IKVM to get ikvm url
     3) Wait for session timeout.
     4) Access url check content.

3. Category: Fix
   Description:
     [149246] - No MEL is generated when attempting to login with wrong password on Web
   Infected Motherboard: B13DET and ALL
   Affected functions: Redfish
   Validation:
      1) Login web GUI with invalid password password

4. Category: fix
   Description:
     [148842] - It should not pop up warning message when add difference "Policy" with same IP/Prefix Length.
   Infected Motherboard: X12STW and ALL
   Affected functions: Configuration
   Validation:
     1) IPMI Web -> Configuration -> Network -> IP Access Control
     2) Click 'Add'
     3) Input 'IP Address' & 'Prefix' which is duplicated exists data
     4) But 'Policy' is not exists
     5) Now will allow to Save without warning message

5. Category: fix
   Description:
     [148948] - Content-Length value is different from the Message Body length
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) Use the "Repeater" tab of Burp Suite software to send HTTP request
     2) GET /restapi and confirm that there isn't a \n at the end of message body
     3) GET /restapi/smci/OOB and confirm that there isn't a \n at the end of message body
     4) PATCH/POST with empty body to any Redfish interface and confirm that
        there isn't a \n at the end of message body

6. Category: fix
   Description:
     [148993] - The password for factory setting should be unique password.
   Infected Motherboard: X13DSF-A and ALL
   Affected functions: ADMIN Password
   Validation:
     1) Press UID button long time and make BMC to do factory default.
     2) ADMIN password should change to unique password

7. Category: Fix
   Description:
     [149125] - The frame of "SNMPv2" help window is not complete at right hand side (Japanese)
   Infected Motherboard: X12SPT-PT and ALL
   Affected functions: Web
   Validation:
     1) Login web GUI -> Go Configuration -> Notification -> SNMP
     2) Change language (English/ Simplified Chinese/Japanese)
     3) Turn On/Off SNMP
     4) Try to Turn ON SNMPv2
     5) Check help window

8. Category: fix
   Description:
     [148949] - Return two json data and cause error reply at H12 redfish (/redfish/v1/AccountService/Accounts/{num})
   Infected Motherboard: H12SSFF-AN6 and ALL
   Affected functions: Redfish
   Validation:
     1) Use PATCH method access /redfish/v1/AccountService/Accounts/{number} with following data:
        {
          "Locked": false
        }
        check the error message raw payload.

9. Category: fix
   Description:
     [ENGINEERING] - Fix the wrong BPN CPLD version on the firmware upgrade web page;
   Infected Motherboard: X13OEI and ALL
   Affected functions: Web
   Validation:
     1) Update the BPN CPLD firmware on the X13OEi board;
     2) Check the New Version on the web page;

10. Category: fix
   Description:
     [139668] – Fix Some Event log time zone is incorrect and not follow the latest MEL SPEC
   Infected Motherboard: X12SPT-PT and ALL
   Affected functions: MEL
   Validation:
     1) trigger MEL-278 to MEL-286 should match spec

11. Category: enhancement
   Description:
     [ENGINEERING] - when NTP disable, user cannot modify timezone from WEB.
   Infected Motherboard: ALL
   Affected functions: Web_Server
   Validation:
     1) In web page, Configuration -> BMC Settings -> Date and Time, check "Time Zone" is selectable

 12. Category: new
   Description:
     [ENGINEERING] - Add I3C Library and MemSensor to support DDR5 DIMM Temperature read
   Infected MotherBoards: H13SSH
   Affected Function: DDR5 DIMM Temperature Read
   Validation:
     1) Plug DDR5 DIMMs on slots
     2) Update BMC FW image with I3C library and memory sensor support
     3) Power on H13 system and boot to OS (POST)
     4) Login BMC Web Page System -> Component Info -> Sensor: Check Temperature Sensors - Name "DIMMA~F Temp", "DIMMG~L Temp"

13. Category: fix
   Description:
     [ENGINEERING] - Enable StatelessAddressAutoConfig in Redfish ethernetInterface
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) PATCH request on ethernetInterface/1 with payload StatelessAddressAutoConfig

14. Category: fix
    Description:
      [ENGINEERING] - Set HTML5 console as default selection
    Infected Motherboard: ALL
    Affected functions:
    Validation :
      1) Maintenance >> BMC Reset >> Factory Default
      2) WebUI >> Remote Control
      3) Current interface should be "HTML5"

15. Category: Fix
  Description:
    [ENGINEERING] - IPv6 auto-config option will be enabled after set others network parameters
  Infected Motherboard: ALL
  Affected Function: Network
  Validation:
    1) Disable IPv6 auto config option on network page
    2) Use Redfish API https://BMC IP/redfish/v1/Managers/1/EthernetInterfaces/1 to PATH following body
       {
          "HostName":"bmchost"
       }
    3) After PATCH, check IPv6 auto-config option on BMC WEB, it should be kept on disable.

16. Category: fix
   Description:
     [149119] - Fix Content-Length value is different from the Message Body length
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) PATCH to any Redfish interface with payload is an empty json object
        or partial fields of the json object contain empty value

17. Category: fix
   Description:
     [149260] fix - Response is incorrect when clear IPv6 null address via smcipmitool
   Infected Motherboard: X13SEED and ALL
   Affected functions: IPMI
   Validation:
     1) Login with SMCIPMITool shell
     2) Clear an empty IPv6 address with command ipmi lan ipv6 clear idx, should return 0xCC instead of 0x0

18. Category: fix
   Description:
     [ENGINEERING] - BMC can't get correct NIC healthy
   Infected Motherboard: ALL
   Affected functions: NIC healthy
   Validation:
     1) install AOC or AIOM and support PLDM
     2) check BMC web and show NIC healthy

19. Category: fix
   Description:
     [148850] - prompt message should be translate to Simplified Chinese and Japanese at IP Access Control.
     [149702] - "Duplicated Data" prompt message is not corresponding on selected "Policy"(ACCEPT/DROP).
   Infected Motherboard: X12STW-F and ALL
   Affected functions: Configuration
   Validation:
     1) IPMI Web -> Configuration -> Network -> IP Access Control
     2) Click 'Add'
     3) Input 'IP Address' & 'Prefix' & 'Policy' which is duplicated exists data
     4) Confirm the Duplicated rule warning message

20. Category: Fix
   Description:
     [149246] - No MEL is generated when attempting to login with wrong password on Web
   Infected Motherboard: B13DET and ALL
   Affected functions: MEL
   Validation:
      1) Post /redfish/v1/SessionService/Sessions with {"UserName": "ADMIN", "Password": "ADMIN1", "Interface": "web"}
      2) Post /redfish/v1/SessionService/Sessions with {"UserName": "ADMIN", "Password": "ADMIN1"}
      3) Login web with invalid password

21.  Category: fix
    Description:
      [146894] - SOL text is shown incorrectly on BH12SSi platform
    Infected Motherboard: BH12SSi and ALL
    Affected functions: SOL function
    Validation :
       1) Open SOL
       2) check the BIOS display and check the UEFI Shell , all should display normally.

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 00.00.06
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20221130_00.00.06_STDsp.bin
Production signed Firmware CRC: 00835C29
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20221130_00.00.06_STDsp.bin
Production signed eMMC Firmware CRC: AE1B1B50
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20221130_00.00.06_STDsp.bin
Production signed SPI NOR Firmware CRC: 3452F243
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20221130_00.00.06_STDsd.bin
Debug signed Firmware CRC: 74D2E42D
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20221130_00.00.06_STDsd.bin
Debug signed eMMC Firmware CRC: A85332B6
Build Date: 11/30/2022
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH
---------------------------------------------------------------------------------------------------------


1.Category: Fix
  Description:
    [149079] - BMC_not_displaying_capacity_for_Kioxia_CD6_drive_in_BMC_WebGUI
  Infected Motherboard: X13DEM and ALL
  Affected Function: storage
  Validation:
    1)Install KCD6XLUL3T84 on system
    2)Check NVMe information from Storage page

2. Category: fix
   Description:
     [149172] - Error HTTP message format at X13 and X12 redfish (/redfish/{string}.IKVM)
   Infected Motherboard: H12SSFF and ALL
   Affected functions: Redfish
   Validation:
     1) Use PATCH access /redfish/v1/Managers/1/Oem/Supermicro/IKVM with data
        {"Current interface":"HTML 5"}
     2) Use GET access /redfish/v1/Managers/1/Oem/Supermicro/IKVM to get ikvm url
     3) Wait for session timeout.
     4) Access url check content.

3. Category: Fix
   Description:
     [149246] - No MEL is generated when attempting to login with wrong password on Web
   Infected Motherboard: B13DET and ALL
   Affected functions: Redfish
   Validation:
      1) Login web GUI with invalid password password

4. Category: fix
   Description:
     [148842] - It should not pop up warning message when add difference "Policy" with same IP/Prefix Length.
   Infected Motherboard: X12STW and ALL
   Affected functions: Configuration
   Validation:
     1) IPMI Web -> Configuration -> Network -> IP Access Control
     2) Click 'Add'
     3) Input 'IP Address' & 'Prefix' which is duplicated exists data
     4) But 'Policy' is not exists
     5) Now will allow to Save without warning message

5. Category: fix
   Description:
     [148948] - Content-Length value is different from the Message Body length
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) Use the "Repeater" tab of Burp Suite software to send HTTP request
     2) GET /restapi and confirm that there isn't a \n at the end of message body
     3) GET /restapi/smci/OOB and confirm that there isn't a \n at the end of message body
     4) PATCH/POST with empty body to any Redfish interface and confirm that
        there isn't a \n at the end of message body

6. Category: fix
   Description:
     [148993] - The password for factory setting should be unique password.
   Infected Motherboard: X13DSF-A and ALL
   Affected functions: ADMIN Password
   Validation:
     1) Press UID button long time and make BMC to do factory default.
     2) ADMIN password should change to unique password

7. Category: Fix
   Description:
     [149125] - The frame of "SNMPv2" help window is not complete at right hand side (Japanese)
   Infected Motherboard: X12SPT-PT and ALL
   Affected functions: Web
   Validation:
     1) Login web GUI -> Go Configuration -> Notification -> SNMP
     2) Change language (English/ Simplified Chinese/Japanese)
     3) Turn On/Off SNMP
     4) Try to Turn ON SNMPv2
     5) Check help window

8. Category: fix
   Description:
     [148949] - Return two json data and cause error reply at H12 redfish (/redfish/v1/AccountService/Accounts/{num})
   Infected Motherboard: H12SSFF-AN6 and ALL
   Affected functions: Redfish
   Validation:
     1) Use PATCH method access /redfish/v1/AccountService/Accounts/{number} with following data:
        {
          "Locked": false
        }
        check the error message raw payload.

9. Category: fix
   Description:
     [ENGINEERING] - Fix the wrong BPN CPLD version on the firmware upgrade web page;
   Infected Motherboard: X13OEI and ALL
   Affected functions: Web
   Validation:
     1) Update the BPN CPLD firmware on the X13OEi board;
     2) Check the New Version on the web page;

10. Category: fix
   Description:
     [139668] – Fix Some Event log time zone is incorrect and not follow the latest MEL SPEC
   Infected Motherboard: X12SPT-PT and ALL
   Affected functions: MEL
   Validation:
     1) trigger MEL-278 to MEL-286 should match spec

11. Category: enhancement
   Description:
     [ENGINEERING] - when NTP disable, user cannot modify timezone from WEB.
   Infected Motherboard: ALL
   Affected functions: Web_Server
   Validation:
     1) In web page, Configuration -> BMC Settings -> Date and Time, check "Time Zone" is selectable

 12. Category: new
   Description:
     [ENGINEERING] - Add I3C Library and MemSensor to support DDR5 DIMM Temperature read
   Infected MotherBoards: H13SSH
   Affected Function: DDR5 DIMM Temperature Read
   Validation:
     1) Plug DDR5 DIMMs on slots
     2) Update BMC FW image with I3C library and memory sensor support
     3) Power on H13 system and boot to OS (POST)
     4) Login BMC Web Page System -> Component Info -> Sensor: Check Temperature Sensors - Name "DIMMA~F Temp", "DIMMG~L Temp"

13. Category: fix
   Description:
     [ENGINEERING] - Enable StatelessAddressAutoConfig in Redfish ethernetInterface
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) PATCH request on ethernetInterface/1 with payload StatelessAddressAutoConfig

14. Category: fix
    Description:
      [ENGINEERING] - Set HTML5 console as default selection
    Infected Motherboard: ALL
    Affected functions:
    Validation :
      1) Maintenance >> BMC Reset >> Factory Default
      2) WebUI >> Remote Control
      3) Current interface should be "HTML5"

15. Category: Fix
  Description:
    [ENGINEERING] - IPv6 auto-config option will be enabled after set others network parameters
  Infected Motherboard: ALL
  Affected Function: Network
  Validation:
    1) Disable IPv6 auto config option on network page
    2) Use Redfish API https://BMC IP/redfish/v1/Managers/1/EthernetInterfaces/1 to PATH following body
       {
          "HostName":"bmchost"
       }
    3) After PATCH, check IPv6 auto-config option on BMC WEB, it should be kept on disable.

--------------------------------------------------------------------------------------------------------------------------------------

Firmware Version: 00.00.05
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20221129_00.00.05_STDsp.bin
Production signed Firmware CRC: 21991A98
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20221129_00.00.05_STDsp.bin
Production signed eMMC Firmware CRC: 43A16DD3
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20221129_00.00.05_STDsp.bin
Production signed SPI NOR Firmware CRC: 3452F243
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20221129_00.00.05_STDsd.bin
Debug signed Firmware CRC: 51CC4E3E
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20221129_00.00.05_STDsd.bin
Debug signed eMMC Firmware CRC: 41EDA897
Build Date: 11/29/2022
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH
---------------------------------------------------------------------------------------------------------


1.Category: Fix
  Description:
    [149079] - BMC_not_displaying_capacity_for_Kioxia_CD6_drive_in_BMC_WebGUI
  Infected Motherboard: X13DEM and ALL
  Affected Function: storage
  Validation:
    1)Install KCD6XLUL3T84 on system
    2)Check NVMe information from Storage page

2. Category: fix
   Description:
     [149172] - Error HTTP message format at X13 and X12 redfish (/redfish/{string}.IKVM)
   Infected Motherboard: H12SSFF and ALL
   Affected functions: Redfish
   Validation:
     1) Use PATCH access /redfish/v1/Managers/1/Oem/Supermicro/IKVM with data
        {"Current interface":"HTML 5"}
     2) Use GET access /redfish/v1/Managers/1/Oem/Supermicro/IKVM to get ikvm url
     3) Wait for session timeout.
     4) Access url check content.

3. Category: Fix
   Description:
     [149246] - No MEL is generated when attempting to login with wrong password on Web
   Infected Motherboard: B13DET and ALL
   Affected functions: Redfish
   Validation:
      1) Login web GUI with invalid password password

4. Category: fix
   Description:
     [148842] - It should not pop up warning message when add difference "Policy" with same IP/Prefix Length.
   Infected Motherboard: X12STW and ALL
   Affected functions: Configuration
   Validation:
     1) IPMI Web -> Configuration -> Network -> IP Access Control
     2) Click 'Add'
     3) Input 'IP Address' & 'Prefix' which is duplicated exists data
     4) But 'Policy' is not exists
     5) Now will allow to Save without warning message

5. Category: fix
   Description:
     [148948] - Content-Length value is different from the Message Body length
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) Use the "Repeater" tab of Burp Suite software to send HTTP request
     2) GET /restapi and confirm that there isn't a \n at the end of message body
     3) GET /restapi/smci/OOB and confirm that there isn't a \n at the end of message body
     4) PATCH/POST with empty body to any Redfish interface and confirm that
        there isn't a \n at the end of message body

6. Category: fix
   Description:
     [148993] - The password for factory setting should be unique password.
   Infected Motherboard: X13DSF-A and ALL
   Affected functions: ADMIN Password
   Validation:
     1) Press UID button long time and make BMC to do factory default.
     2) ADMIN password should change to unique password

7. Category: Fix
   Description:
     [149125] - The frame of "SNMPv2" help window is not complete at right hand side (Japanese)
   Infected Motherboard: X12SPT-PT and ALL
   Affected functions: Web
   Validation:
     1) Login web GUI -> Go Configuration -> Notification -> SNMP
     2) Change language (English/ Simplified Chinese/Japanese)
     3) Turn On/Off SNMP
     4) Try to Turn ON SNMPv2
     5) Check help window

8. Category: fix
   Description:
     [148949] - Return two json data and cause error reply at H12 redfish (/redfish/v1/AccountService/Accounts/{num})
   Infected Motherboard: H12SSFF-AN6 and ALL
   Affected functions: Redfish
   Validation:
     1) Use PATCH method access /redfish/v1/AccountService/Accounts/{number} with following data:
        {
          "Locked": false
        }
        check the error message raw payload.

9. Category: fix
   Description:
     [ENGINEERING] - Fix the wrong BPN CPLD version on the firmware upgrade web page;
   Infected Motherboard: X13OEI and ALL
   Affected functions: Web
   Validation:
     1) Update the BPN CPLD firmware on the X13OEi board;
     2) Check the New Version on the web page;

10. Category: fix
   Description:
     [139668] – Fix Some Event log time zone is incorrect and not follow the latest MEL SPEC
   Infected Motherboard: X12SPT-PT and ALL
   Affected functions: MEL
   Validation:
     1) trigger MEL-278 to MEL-286 should match spec

11. Category: enhancement
   Description:
     [ENGINEERING] - when NTP disable, user cannot modify timezone from WEB.
   Infected Motherboard: ALL
   Affected functions: Web_Server
   Validation:
     1) In web page, Configuration -> BMC Settings -> Date and Time, check "Time Zone" is selectable

 12. Category: new
   Description:
     [ENGINEERING] - Add I3C Library and MemSensor to support DDR5 DIMM Temperature read
   Infected MotherBoards: H13SSH
   Affected Function: DDR5 DIMM Temperature Read
   Validation:
     1) Plug DDR5 DIMMs on slots
     2) Update BMC FW image with I3C library and memory sensor support
     3) Power on H13 system and boot to OS (POST)
     4) Login BMC Web Page System -> Component Info -> Sensor: Check Temperature Sensors - Name "DIMMA~F Temp", "DIMMG~L Temp"

13. Category: fix
   Description:
     [ENGINEERING] - Enable StatelessAddressAutoConfig in Redfish ethernetInterface
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) PATCH request on ethernetInterface/1 with payload StatelessAddressAutoConfig

14. Category: fix
    Description:
      [ENGINEERING] - Set HTML5 console as default selection
    Infected Motherboard: ALL
    Affected functions:
    Validation :
      1) Maintenance >> BMC Reset >> Factory Default
      2) WebUI >> Remote Control
      3) Current interface should be "HTML5"

15. Category: Fix
  Description:
    [ENGINEERING] - IPv6 auto-config option will be enabled after set others network parameters
  Infected Motherboard: ALL
  Affected Function: Network
  Validation:
    1) Disable IPv6 auto config option on network page
    2) Use Redfish API https://BMC IP/redfish/v1/Managers/1/EthernetInterfaces/1 to PATH following body
       {
          "HostName":"bmchost"
       }
    3) After PATCH, check IPv6 auto-config option on BMC WEB, it should be kept on disable.

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 00.00.05
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20221117_00.00.05_STDsp.bin
Production signed Firmware CRC: 49DE6AC5
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20221117_00.00.05_STDsp.bin
Production signed eMMC Firmware CRC: 002786B9
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20221117_00.00.05_STDsp.bin
Production signed SPI NOR Firmware CRC: 3452F243
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20221117_00.00.05_STDsd.bin
Debug signed Firmware CRC: E20E539A
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20221117_00.00.05_STDsd.bin
Debug signed eMMC Firmware CRC: D9EE2E04
Build Date: 11/17/2022
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH
---------------------------------------------------------------------------------------------------------


1. Category: fix
   Description:
     [ENGINEERING] - support Backplane NVME storage
   Infected Motherboard: H13SSH
   Affected functions: NVME
   Validation:
     1) Install Backplane and check NVME information.

2. Category: fix
   Description:
     [ENGINEERING] - Fix change BIOS password fail
   Infected Motherboard: X13
   Affected functions: Change BIOS password
   Validation:
     1) if current admin password is empty then set password 1111, POST with {"PasswordName":"AdministratorPassword#0156", "OldPassword":"", "NewPassword":"1111"} on https://$IP/redfish/v1/Systems/1/Bios/Actions/Bios.ChangePassword
     2) reboot host and into setup menu check then boot to OS
     3) if change admin password from 1111 to 1112, POST with {"PasswordName":"AdministratorPassword#0156", "OldPassword":"1111", "NewPassword":"1112"} on https://$IP/redfish/v1/Systems/1/Bios/Actions/Bios.ChangePassword
     4) reboot host and into setup menu check then boot to OS
     5) if current user password is empty then set password 1111, POST with {"PasswordName":"UserPassword#0157", "OldPassword":"", "NewPassword":"1111"} on https://$IP/redfish/v1/Systems/1/Bios/Actions/Bios.ChangePassword
     6) reboot host and into setup menu check then boot to OS
     7) if change user password from 1111 to 1112, POST with {"PasswordName":"UserPassword#0157", "OldPassword":"1111", "NewPassword":"1112"} on https://$IP/redfish/v1/Systems/1/Bios/Actions/Bios.ChangePassword
     8) reboot host and into setup menu check then boot to OS

3. Category: fix
   Description:
     [147795][147796] - Avoid path traversal payload download/delete files
   Infected Motherboard: X13
   Affected functions: Redfish
   Validation:
     1) POST request on /redfish/v1/Oem/Supermicro/DumpService/Dumps/AttestationDump/Actions/SmcAttestationDump.Generate to generate attestation file before testing
     2) POST request on /redfish/v1/Oem/Supermicro/DumpService/Dumps/AttestationDump/Actions/SmcAttestationDump.Delete with path traversal payload
     3) POST request on /redfish/v1/Oem/Supermicro/DumpService/Dumps/AttestationDump/Actions/SmcAttestationDump.Download with path traversal payload

4. Category: feature
   Description:
     [147363] - Add the network AOC inserted WebUI
   Infected Motherboard: X13DEM and ALL
   Affected functions: WebUI
   Validation:
     1) Insert an AOC NIC
     2) Check the WebUI's Dashboard page, the Network AOC field contain a link should be there

5. Category: feature
   Description:
     [ENGINEERING] - Redfish method to set BMC LAN interface
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
     1) GET request on /redfish/v1/Managers/1/EthernetInterfaces/1
     2) PATCH request on /redfish/v1/Managers/1/EthernetInterfaces/1 to change LANInterface setting

6. Category: fix
   Description:
     [148208] - It should be forbidden input decimal point value at "Host IP Address"
   Infected Motherboard: X13DSF-A and ALL
   Affected functions: Configuration
   Validation:
     1) IPMI Web -> Configuration -> BMC Setting -> Host Interface
     2) Enter point into "Host IP Address" will be clear field when leave focus
     3) Tooltip changed as given spec

7. Category: fix
   Description:
     [148000] - Username should not allow "!" which is not match with spec
   Infected Motherboard: X13DSF and ALL
   Affected functions: Configuration
   Validation:
     1) IPMI Web -> Configuration -> Notifications -> Alerts -> edit alert
     2) Change Protocol to 'SNMPv3'
     3) Type unavailable character to verify, now only allows [letters and numbers]

8. Category: fix
   Description:
     [148852] - "Duplicated rule" prompt message and behavior is not same as X12 UI SPEC define.
   Infected Motherboard: X12STW-F and ALL
   Affected functions: Configuration
   Validation:
     1) IPMI Web -> Configuration -> Network -> IP Access Control
     2) Click 'Add'
     3) Input 'IP Address' & 'Prefix' which is duplicated exists data
     4) Now un-focus input will show message, and cannot Save

9. Category: fix
   Description:
     [147952] - Prevent unspecified address and loopback address are added to static IPv6 addresses
   Infected Motherboard: X12DGQ and ALL
   Affected functions: IPMI
   Validation:
     1) Add unspecified address(::/128) through IPMI
     2) Add loopback address(::1/128) through IPMI
     3) Get IPv6 static address through IPMI, make sure unspecified address and loopback address doesn't exist

10. Category: fix
   Description:
     [148680] - SMCIPMITOOLIPMITOOL and WEB have different naming of power supply in inventory items
   Infected Motherboard: X12DPT-PT6 and ALL
   Affected functions: Redfish
   Validation:
     1) Get /redfish/v1/UpdateService/FirmwareInventory/PowerSupply1

11. Category: fix
   Description:
     [148821] - Doesn't show any popup message when press down reload button without BMC configuration file
   Infected Motherboard: X12DPT-PT6 and ALL
   Affected functions: Web
   Validation:
     1) goto IPMI Configuration page then enter Reload button should show "Required" message


--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 00.00.04
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20221031_00.00.04_STDsp.bin
Production signed Firmware CRC: 909FF5E4
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20221031_00.00.04_STDsp.bin
Production signed eMMC Firmware CRC: D47D4309
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20221031_00.00.04_STDsp.bin
Production signed SPI NOR Firmware CRC: 3452F243
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20221031_00.00.04_STDsd.bin
Debug signed Firmware CRC: 5F8B9A52
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20221031_00.00.04_STDsd.bin
Debug signed eMMC Firmware CRC: 6970BD5D
Build Date: 10/31/2022
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH
---------------------------------------------------------------------------------------------------------


apply common fix.

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 00.00.03
Production signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20221021_00.00.03_STDsp.bin
Production signed Firmware CRC: 09CF4406
Production signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20221021_00.00.03_STDsp.bin
Production signed eMMC Firmware CRC: A71929B0
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20221021_00.00.03_STDsp.bin
Production signed SPI NOR Firmware CRC: 3452F243
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20221021_00.00.03_STDsd.bin
Debug signed Firmware CRC: F709CBC0
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20221021_00.00.03_STDsd.bin
Debug signed eMMC Firmware CRC: 2BC63794
Build Date: 10/21/2022
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH
---------------------------------------------------------------------------------------------------------


1. Category: Fix
   Description:
     [ENGINEERING] - Change the response data of IPMI OEM command - Get OTP board serial number to align withe new IPMI command format
   Infected MotherBoards: ROT20
   Affected Function: RA Provision
   Validation:
     1) Use SUM tool to do RA Provision on the board
     2) Use IPMItool to send IPMI raw command (0x30 0x68 0x28 0x87)
     3) Check the response data of IPMI command, the first byte should be the length, the board serial number starts from the second byte

2. Category: Fix
   Description:
     [ENGINEERING] - Integrate new DDR4 driver to improves timing and signal quality in AST2600.
   Infected MotherBoards: ALL
   Affected Function: Reliability
   Validation:
     1) AC Cycle stress without any image recovery happen.

3. Category: fix
   Description:
     [ENGINEERING] - M.2 slot 2 temperature reading missing
   Infected Motherboard: H13SSH
   Affected functions: sensor
   Validation:
     1) M.2 slot 2(top one) temperature reading missing

4. Category: Fix
   Description:
    [ENGINEERING] - Update network hostname format
   Infected Motherboard: ALL
   Affected functions: Network Settings
   Validation:
    1) Navigate to "Configuration" -> "Network"
    2) Hostname should follow this format: <letter/digit>[*[<letter-or-digit-or-hyphen>]<letter-or-digit>]
    3) If the hostname is incorrect, the error message will show: “Up to 63 alphanumeric (a-z, A-Z, 0-9) and non-leading or non-ended hyphen (-) characters are allowed."

5. Category: fix
   Description:
     [ENGINEERING] - The readings style of "Power Consumption" graph should be use radio button.
   Infected Motherboard: X12STW-F-P
   Affected functions: Configuration
   Validation:
     1) Login BMC web GUI by ADMIN -> go Dashboard -> System -> Power page
     2) Check WebUI changed: radio button replaced drop down list component

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 00.00.02
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20221013_00.00.02_STDsp.bin
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20221013_00.00.02_STDsd.bin
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20221013_00.00.02_STDsd.bin
Build Date: 09/28/2022
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH
---------------------------------------------------------------------------------------------------------

1) use H13 BMC GUID E401MS
2) make more sensor available

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 00.00.01
Production signed SPI NOR Firmware Name: BMC_H13AST2600-ROT20-E401MS-NOR_20220928_00.00.01_STDsp.bin
Production signed SPI NOR Firmware CRC: A15EC7C0
Debug signed Firmware Name: BMC_H13AST2600-ROT20-E401MS_20220928_00.00.01_STDsd.bin
Debug signed Firmware CRC: E88B30BD
Debug signed eMMC Firmware Name: BMC_H13AST2600-ROT20-E401MS-eMMC_20220928_00.00.01_STDsd.bin
Debug signed eMMC Firmware CRC: 52A3F79E
Build Date: 09/28/2022
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
ROT AntiRollback ID: 0001h
Supported Platform: H13SSH
---------------------------------------------------------------------------------------------------------


Initial BMC FW 00.00.01

--------------------------------------------------------------------------------------------------------------------------------------

