BIOS Flash Procedure:
1.Decompress package onto a USB drive
2.Boot into UEFI shell and switch to USB directory (usually FS0:)
3.Switch to the directory containing the package
4.Type in the following command to start flashing BIOS (Do not interrupt this process as it might damage the BIOS)
	flash.nsh RomImgYY.MDD