Filename: BMC_X13AST2600-nonROT-0501MS_202309_01.01.17_STDsp.bin version: 01.01.17 Date: 05 Sep 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : Redfish_1_11_API_full_list_20230613
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH-F, X13SCL-F, X13SCD-F

1.
    Category: Fixed
    Description:
        C: [Catlow] Disable memory PFA MEL report function.
    Impact motherboard:
        Catlow
    Affected functions:
    Validation:
        Intel entry level server platform wonˇ¦t have AMT + hPPR so Catlow is not supported as well.

==============================================================================================================================
Filename: BMC_X13AST2600-nonROT-0501MS_20230828_01.01.16_STDsp.bin version: 01.01.16 Date: 28 Aug 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : Redfish_1_11_API_full_list_20230613
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH-F, X13SCL-F, X13SCD-F

1.
    Category: Fixed
    Description:
       R: [161456] [CombinedECO BIOS 1.0 & IPMI 01.01.15] P5V_AUX and P3V3_AUX voltage sensor is out of SMSTC specification.
    Impact motherboard:
        X13SCD-F
    Affected functions:
    Validation:
       Check sensor reading names.

2.
    Category: Fixed
    Description:
        R: [161193] Hardware Monitor Voltage test fail
    Impact motherboard:
        X13SCD-F
    Affected functions:
    Validation:
       Check sensor readings.

3.
    Category: Fixed
    Description:
        R: [161092] Redfish have health sensor failed.
    Impact motherboard:
        X13SCL-IF
    Affected functions:
    Validation:
       Testing HW component status check Warning CPU related events of SATC, Health Thermal Status goese OK as expected.

==============================================================================================================================
Filename: BMC_X13AST2600-nonROT-0501MS_20230821_01.01.15_STDsp version: 01.01.15 Date: 21 Aug 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : Redfish_1_11_API_full_list_20230613
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH-F, X13SCL-F, X13SCD-F

1.
    Category: Fixed
    Description:
        C: [X13SCD-F] Make CPU temperature read from ME.
    Impact motherboard:
        X13SCD-F
    Affected functions:
    Validation:
       ADC read - "CPU Temperature" shows pass.

==============================================================================================================================
Filename: BMC_X13AST2600-nonROT-0501MS_20230811_01.01.14_STDsp version: 01.01.14 Date: 11 Aug 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : Redfish_1_11_API_full_list_20230613
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH-F, X13SCL-F, X13SCD-F

1.
    Category: Fixed
    Description:
       C: [X13SCL-F] adjust "CPU Core" threshold -2
    Impact motherboard:
        X13SCL-F
    Affected functions:
    Validation:
       ADC read - "CPU Core" shows pass.

2.
    Category: Fixed
    Description:
        C: [X13SCD-F] Modify "CPU Core" threshold.
    Impact motherboard:
        X13SCD-F
    Affected functions:
    Validation:
       ADC read - "CPU Core" shows pass.

==============================================================================================================================
Filename: BMC_X13AST2600-nonROT-0501MS_20230807_01.01.13_STDsd version: 01.01.13 Date: 07 Aug 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : Redfish_1_11_API_full_list_20230613
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH-F, X13SCL-F, X13SCD-F

1.
    Category: Fixed
    Description:
       R: [158912] The CPLD update tool is not found in the CPLD package, please help to confirm.
    Impact motherboard:
        X13SCD-F
    Affected functions:
    Validation:
       Use the sum tool to update cpld.

==============================================================================================================================
Filename: BMC_X13AST2600-nonROT-0501MS_20230724_01.01.12_STDsd version: 01.01.12 Date: 24 Jul 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : Redfish_1_11_API_full_list_20230613
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH-F, X13SCL-F, X13SCD-F

1.
    Category: Fixed
    Description:
       R: [159375] WebUI sensor naming not matched with SPEC
    Impact motherboard:
        X13SCD-F
    Affected functions:
    Validation:
       Check Sensor Readings names.

==============================================================================================================================
Filename: BMC_X13AST2600-nonROT-0501MS_20230710_01.01.11_STDsd version: 01.01.11 Date: 10 Jul 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : Redfish_1_11_API_full_list_20230613
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH-F, X13SCL-F, X13SCD-F

1.
    Category: Fixed
    Description:
       R: [158546] After finishing a "Unit Reset" in bmc web when the host is in OS(windows), updating BIOS fw in bmc web will cause power on failure on the system.
    Impact motherboard:
        X13SCD-F
    Affected functions:
    Validation:
       1. Boot to OS.
       2. Pressing "Unit Reset" to reset BMC.
       3. Update BIOS via BMC WebUI.
       4. The BMC can control the power of the system.
2.
    Category: Fixed
    Description:
        R: [158528] IPMI sensor read - "CPU_PVC_CPU" shows lower than Low NR/Low CT when BOOT to OS.
    Impact motherboard:
        X13SCD-F
    Affected functions:
    Validation:
       Sensor read - "CPU_PVC_CPU" shows pass.

==============================================================================================================================
Filename: BMC_X13AST2600-nonROT-0501MS_20230704_01.01.10_STDsd version: 01.01.10 Date: 04 Jul 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : Redfish_1_11_API_full_list_20230613
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH-F, X13SCL-F, X13SCD-F

1.
    Category: Fixed
    Description:
       C: [158683] [IPMI 01.01.08] BMC WebUI will record "CPU Core" voltage going low events during DC onoff cycle
    Impact motherboard:
        X13SCL-IF
    Affected functions:
    Validation:
       1. Run DC onoff cycle.
       2. Check BMC events after DC onoff cycle.

2.
    Category: Fixed
    Description:
        C: [158811] An extra sensor, "Chassis Intru", is shown in SMCIPMITool and SDHM_tool. The sensor is not shown in bmc web.
    Impact motherboard:
        X13SCD-F
    Affected functions:
    Validation:
       1. X13SCD does not have this feature.
       2. Remove it.

==============================================================================================================================
Filename: BMC_X13AST2600-nonROT-0501MS_20230628_01.01.09_STDsd version: 01.01.09 Date: 28 Jun 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : Redfish_1_11_API_full_list_20230518
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH-F, X13SCL-F, X13SCD-F

1.
    Category: Fixed
    Description:
        C: [X13SCH-F] 1. To read memory temp via I2C bus9. 2. Support NVMe BPN. 3. Support RSC-S-6G5
    Impact motherboard:
        X13SCH-F
    Affected functions:
    Validation:
       1. Login web and change to Sensor page.
       2. Confirmation dimm temperature can be read.

2.
    Category: Fixed
    Description:
        C: [X13SCH-F] To meet Thermal design guide 4.7
    Impact motherboard:
        X13SCH-F
    Affected functions:
    Validation:
       1. Confirmation temperature sensors has followed Thermal design guide 4.7

==============================================================================================================================
Filename: BMC_X13AST2600-nonROT-0501MS_20230626_01.01.08_STDsd version: 01.01.08 Date: 26 Jun 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : Redfish_1_11_API_full_list_20230518
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH-F, X13SCL-F, X13SCD-F

1.
    Category: Fixed
    Description:
        C: [X13SCD-F] Modified CPU temperature readings to accommodate newer versions of hardware.
    Impact motherboard:
        X13SCD-F
    Affected functions:
    Validation:
       1. Login web and change to Sensor page.
       2. Confirmation CPU temperature can be read.

2.
    Category: Fixed
    Description:
        C: [X13SCL-IF] adjust CPU_Core low CT/NR for new MB(V1.01)
    Impact motherboard:
        X13SCL-IF
    Affected functions:
    Validation:
       1. run CBRUN for DC ON/OFF
       2. It would pass the validataion for 200 cycles.

==============================================================================================================================
Filename: BMC_X13AST2600-nonROT-0501MS_20230612_01.01.07_STDsd version: 01.01.07 Date: 12 Jun 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : Redfish_1_11_API_full_list_20230518
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH-F, X13SCL-F

1.
    Category: Fixed
    Description:
        [156958] When the system boot up, "[CPLD-0020] CATERR - Assertion" appears on the IPMI WEB GUI.
    Impact motherboard:
        X13SCL_IF
    Affected functions:
    Validation:
        1.Enable MCE AER http://10.135.200.1/enable_mce_aer/
        2.Remove AC power cable
        3.Plug in AC Power cable and powered on system
        4.[CPLD-0020] "CATERR - Assertion" doesnot appear on IPMI WEB GUI

==============================================================================================================================
Filename: BMC_X13AST2600-nonROT-0501MS_20230605_01.01.06_STDsd version: 01.01.06 Date: 05 Jun 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : Redfish_1_11_API_full_list_20230518
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH-F, X13SCL-F

1.
    Category: Fixed
    Description:
        [156957] "[IPMI-1009] CPU Temp ,Upper Critical-going high - Assertion" appears on IPMI WEB GUI after the system has been power cycled.
    Impact motherboard:
        X13SCL_IF
    Affected functions:
    Validation:
        1.Enable MCE AER http://10.135.200.1/enable_mce_aer/
        2.Remove AC power cable
        3.Plug PCI-E Card in PCI-E Slot7.(ex:AOC-S3108L-H8iR/ASC-29320LPE/Any LAN Card)
        4.Plug in AC Power cable and powered on system
        5." Power Cycle" via IPMI WebGUI.
        6.[IPMI-1009] CPU Temp ,Upper Critical-going high - Assertion" doesnot appear on IPMI WEB GUI

2.
    Category: Fixed
    Description:
        [156543] No release X13SCL-F Hardware_Monitoring_Sensor_Names_Other_Information spec. Copy Project Issue Link
    Impact motherboard:
        X13SCL-F
    Affected functions:
    Validation:
        1.sync up with Supermicro_BMC_Sensor_Naming_Guildeline_2.5_Draft_05222023
        2.CPU 1.1V_DDR --> CPU 1.1V_DDR
        3.CPU CORE --> CPU Core

==============================================================================================================================

Filename: BMC_X13AST2600-nonROT-0501MS_20230529_01.01.05_STDsd version: 01.01.05 Date: 29 MAY 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : Redfish_1_11_API_full_list_20230518
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH-F, X13SCL-F

1.
    Category: Fixed
    Description:
        [156370] SATC Redfish Automation Test Failed.
    Impact motherboard:
        Catlow
    Affected functions:
    Validation:
        1. /redfish/v1/Oem/Supermicro/DumpService/Actions/SmcDumpService.DeleteAll, permission test pass
        2. /redfish/v1/Oem/Supermicro/DumpService/Dumps/HostCrashDump/Actions/SmcDump.Download, permission test pass

==============================================================================================================================

Filename: BMC_X13AST2600-nonROT-0501MS_20230522_01.01.04_STDsd version: 01.01.04 Date: 22 MAY 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : Redfish_1_11_API_full_list_20230410
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH-F, X13SCL-F

1.
    Category: Fixed
    Description:
        [156676] Missing GPU sensor.
    Impact motherboard:
        X13SCL-F
    Affected functions:
    Validation:
        1. can detect GPU on PCIE slot6

2.
    Category: Fixed
    Description:
        [156543] No release X13SCL-F Hardware_Monitoring_Sensor_Names_Other_Information spec. Copy Project Issue Link
    Impact motherboard:
        X13SCL-F
    Affected functions:
    Validation:
        1. modify CPU 1.8VCC to CPU 1.8V

==============================================================================================================================

Filename: BMC_X13AST2600-nonROT-0501MS_20230516_01.01.03_STDsd version: 01.01.03 Date: 16 MAY 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : Redfish_1_11_API_full_list_20230410
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH-F, X13SCL-F

1.
    Category: Fixes
    Description:
        [154503] No release X13SCL-IF Hardware_Monitoring_Sensor_NamesOther_Information spec.
    Impact motherboard:
        X13SCL-IF
    Affected functions:
    Validation:
        1. Login web and change to Sensor page.
        2. Confirmation ADC sensor name has followed the latest SPEC.

==============================================================================================================================

Filename: BMC_X13AST2600-nonROT-0501MS_20230509_01.01.02_STDsd version: 01.01.02 Date: 09 MAY 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : Redfish_1_11_API_full_list_20230410
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH-F, X13SCL-F

1.
    Category: Fixes
    Description:
        [156040] Can not trigger CATERR/IERR by Intel DCI Cscript
    Impact motherboard:
        X13SCL-IF
    Affected functions:
    Validation:
        1. Using Intel DCI script to trigger CATERR/IERR event.
        2. Login web and change to Health Event Log page.
        3. Confirmation CATERR log that would be displayed.

==============================================================================================================================
Filename: BMC_X13AST2600-nonROT-0501MS_20230502_01.01.01_STDsd version: 01.01.01 Date: 02 MAY 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : X12_Redfish_1_90_API_full_list_11032021
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH-F, X13SCL-F

1.
    Category: Fixes
    Description:
        [155109] There is no show M2SSD1 temperatures sensor on WebGUI.
    Impact motherboard:
        X13SCL-IF
    Affected functions:
    Validation:
        1. Login web with ADMIN.
        2. Change to Sensor Page.
        3. Check the M2_SSD1 Temperature.

==============================================================================================================================
Filename: BMC_X13AST2600-nonROT-0501MS_20230424_01.01.00_STDsd version: 01.01.00 Date: 24 APR 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : X12_Redfish_1_90_API_full_list_11032021
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH-F, X13SCL-F

1.
    Category: Fixes
    Description:
        [155267] DMTF/Redfish Conformance test failed.	
    Impact motherboard:
        X13SCL-IF
    Affected functions: 
    Validation:
        Validation by SATC with X12_Redfish_1_90_API_full_list_11032021.

==============================================================================================================================
Filename: BMC_X13AST2600-nonROT-0501MS_20230417_00.00.05_STDsd version: 00.00.05 Date: 17 APR 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : X12_Redfish_1_90_API_full_list_11032021
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH_F, X13SCL-F

1.
    Category: Fixes
    Description:
        [155042] Hardware Monitor Voltage test fail.	
    Impact motherboard:
        X13SCL-IF
    Affected functions: 
    Validation:
        1. Login web with ADMIN.
        2. Change to Sensor Page.
        3. Validation with PVCC_CPU under +-2% tolerance.

2.  Category: Fixes
    Description:
        [155132] Host name can fill the 64 characters on BMC WebUI.
    Impact motherboard:
        X13SCL-IF
    Affected functions: 
    Validation:
        1. Login web with ADMIN
        2. Change to Network Page.
        3. Validation by typing hostname with 63 characters (maximum length).

3.  Category: Fixes
    Description:
        [155109] There is no show M2SSD1 temperatures sensor on WebGUI.
    Impact motherboard:
        X13SCL-IF
    Affected functions: 
    Validation:
        1. Login web with ADMIN.
        2. Change to Sensor Page.
        3. Check the M2_SSD1 Temperature.

4.  Category: Fixes
    Description:
        [155054] [BMC Sensor] The CPU Temp and Inlet Temp Sensor Reading are showing N/A under IPMI Web.
    Impact motherboard:
        X13SCL-F
    Affected functions: 
    Validation:
        1. can read inlet sensor

5.  Category: Fixes
    Description:
        [154905] [SMCIPMITool] Test fail via SMSTC with SMCIPMITool_2.27.2_build.230221.
    Impact motherboard:
        X13SCL-F
    Affected functions: 
    Validation:
        1. run SMCIPMITool ECO
        2. TC0202 & TC1709 will pass

==============================================================================================================================
Filename: BMC_X13AST2600-nonROT-0501MS_20230324_00.00.04_STDsd version: 00.00.04 Date: 10 Mar 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : X12_Redfish_1_90_API_full_list_08282020
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH_F, X13SCL-F

1.
    Category: Fixes
    Description:
        [154364] CPLD information is missing in BIOS/IPMI WebUI	
    Impact motherboard:
        X13SCL-IF
    Affected functions: 
    Validation:
        1. Login web with ADMIN.
        2. Change to Dashboard Page.
        3. Check the CPLD version.

2.  Category: Fixes
    Description:
        [153684] storage monitoring is not found on BMC web
    Impact motherboard:
        X13SCL-IF
    Affected functions: 
    Validation:
        1. Login web with ADMIN
        2. Change to Sensor Page.

3.  Category: Fixes
    Description:
        [154040][DVT] GPU card cannot detected sensor in BMC and SD5.
    Impact motherboard:
        X13SCL-IF
    Affected functions: 
    Validation:
        Validation with SD5 to confirm GPU thermal can be read.

==============================================================================================================================
Filename: BMC_X13AST2600-nonROT-0501MS_20230310_00.00.03_STDsd version: 00.00.03 Date: 10 Mar 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : X12_Redfish_1_90_API_full_list_08282020
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH_F, X13SCL-F

1.
    Category: Fixes
    Description:
        [153595][DVT] Cburn onoff test 48hr have sensor error		
    Impact motherboard:
        X13SCL-IF
    Affected functions: 
    Validation:
        1. Login web with ADMIN.
        2. Change to Sensor Page.

2.  Category: Fixes
    Description:
        [152219][EVT] JD1 SPEAKER has no sound output.
    Impact motherboard:
        X13SCL-IF
    Affected functions: 
    Validation:
        Following lab's standard validation

==============================================================================================================================
Filename: BMC_X13AST2600-ROT-C301MS_20211115_00.00.02_STDsp version: 00.00.02 Date: 06 Feb 2023
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : X12_Redfish_1_90_API_full_list_08282020
antiRBID: 0x0001
Supported MBs: X13SCL-IF, X13SCH_F

Category: Fixes
    Description:
        [152148][EVT] IPMI sensor read failed with many items showing N/A or Error.	
		[152130] BMC Sensor ppwer 12V/5//3.3V error when run pxe stress. 
    Impact motherboard:
        X13SCL-IF
    Affected functions:
    Validation:
        1. Login web with ADMIN.
        2. Change to Sensor Page.

==============================================================================================================================
Filename: BMC_X13AST2600-ROT-C301MS_20211115_00.00.01_STDsp version: 00.00.01 Date: 29 Dec 2022
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69.45
Redfish API : X12_Redfish_1_80_API_full_list_08282020
antiRBID: 0x0001
Supported MBs: X13SCL-IF

Initial board-bring-up bmc FW.
