Caution:
1. For factory use please untar "BIOS_xxxxx-xxxx_xxxxxxx_x.x_STD.TAR" to get "BIOS_xxxxx-xxxx_xxxxxxx_x.x_STD.BIN" file.
2. For factory use please untar "xxxxx_SCP_x.xx" to get "SCP altra_scp_signed_x.xx.xxxxx.slim" file.
3. Please use SCP altra_scp_signed_2.10.20230517.slim with this BIOS.

=========================================================================================================

[Update BIOS]
Update image steps via webui:

step1:
login obmc webui by https, please input default user name "root" and password "0penBmc".
mention: please follow the sticker on the motherboard for the factory default password.

step2:
switch page to Operations->Firmware and then upload BIOS image tar file.

step3:
press "Start update" button and wait bmcweb refresh message.


=========================================================================================================
[Update SCP]
Update image steps via webui:

step1:
login obmc webui by https, please input default user name "root" and password "0penBmc".
mention: please follow the sticker on the motherboard for the factory default password.

step2:
switch page to Operations->Firmware and then upload SCP image tar file.

step3:
press "Start update" button and wait bmcweb refresh message.


=========================================================================================================