GIT SHA: 83726718befba44ba8a0a70adf5e6f130b56dde1

Firmware Version: 01.02.15
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20240125_01.02.15_STDsp.bin
Production signed Firmware CRC: A0D027A1
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20240125_01.02.15_STDsp.bin
Production signed eMMC Firmware CRC: DD0C4FB8
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20240125_01.02.15_STDsp.bin
Production signed SPI NOR Firmware CRC: 2670E932
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20240125_01.02.15_STDsd.bin
Debug signed Firmware CRC: 02C321F2
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20240125_01.02.15_STDsd.bin
Debug signed eMMC Firmware CRC: 0D06D809
Build Date: 01/25/2024
Redfish API : Redfish_1_11_API_full_list_20231110
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: Minor
  Description:
    [169585] - IPv6 with SLAAC and DHCPv6 addr fails to properly route ipmitool commands through both addresses.
    [ENGINEERING] - Allow DHCPV6 and SLAAC to be able to access via IPMItool all the time
  Infected Motherboard: All
  Affected functions: Network, ipv6
  Validation:
    1) On BMC webpage, switch between stateful mode and stateless mode
       -> Stateful mode using ipmitool
          -> DHCPV6 address will response
          -> SLAAC address will response
       -> Stateless mode using ipmitool
          -> SLAAC address will response
2.  Category: Critical
    Description:
      [164992] – Power consumption graphs sometimes appear incorrect
    Infected Motherboard: G1SMH-G-P
    Affected functions:
    Validation:
      1) Reference PB issue 164992 to validate
3. Category: fix
   Description:
     [168610] - Redfish service validator fail
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: Redfish
   Validation:
     1) install TAS
     2) Get /redfish/v1/Systems/1/EthernetInterfaces/
     3) Get /redfish/v1/Systems/1/EthernetInterfaces/x



--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: cd576492d390fd6c483b1f1d7f8a06309a08a903

Firmware Version: 01.02.14
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20240123_01.02.14_STDsp.bin
Production signed Firmware CRC: F840429D
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20240123_01.02.14_STDsp.bin
Production signed eMMC Firmware CRC: 5195F60F
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20240123_01.02.14_STDsp.bin
Production signed SPI NOR Firmware CRC: 2670E932
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20240123_01.02.14_STDsd.bin
Debug signed Firmware CRC: 8936C72A
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20240123_01.02.14_STDsd.bin
Debug signed eMMC Firmware CRC: 52FAE25A
Build Date: 01/23/2024
Redfish API : Redfish_1_11_API_full_list_20231110
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: fix
   Description:
     [168605] - NVSSVT uris do not exist in resiliency IPMI redfish API BMCCore
   Infected Motherboard: G1SMH-G
   Affected functions: Redfish
   Validation:
     1) Send GET request to the API '/redfish/v1/UpdateService/SoftwareInventory'.
2. Category: Major
  Description:
    [ENGINEERING] - share LAN no IP at failover/failover-AOC mode
  Infected Motherboard: G1SMH-G-P, G1SMH, X13DEH
  Affected functions: Network
  Validation:
    1) At Failover/Failover-AOC mode，"Only connect shared lan，don't connect dedicated lan"，then physical AC cycle.
    2) Wait BMC boot up and shared lan get IP.
    3) insert dedicated lan and wait dedicated lan get IP，then plug out dedicated lan.
    4) bond0 will switch to shared lan and can get IP successful, can checked by login web.
3. Category: fix
   Description:
     [ENGINEERING] - more G2DMH-G sensors available
   Infected Motherboard: G2DMH-G
   Affected functions: sensor
   Validation:
     1) VBAT monitoring
     2) M2SSD Temp monitoring
     3) Liquid cool leakage detection event
     4) PCIE slot card monitoring
     5) CPU temp monitoring
     6) NVME BPN monitoring
     7) Power on/off control
4. Category: fix
   Description:
     [166380] - Arm sbmr acs test automation fail
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: Redfish
   Validation:
     1. Get /Systems/1, Check the Boot->AutomaticRetryConfig
5.  Category: Critical
    Description:
      [163413] – Remove PMEM sensor
    Infected Motherboard: X13DEH
    Affected functions:
    Validation:
      1) Upgrade BMC firmware
      2) WebUI >> Maintenance >> BMC Reset >> Factory Default
      3) WebUI >> Dashboard >> Sensor Readings
      4) PMEM sensors should disappear
6. Category: fix
   Description:
     [167615] - Redfish-Interop-Validator OCP Profile fail.
   Infected Motherboard: G1SMH
   Affected functions: Redfish
   Validation:
     1. Run the Redfish-Interop-Validator with OCP profile.
7. Category: fix
   Description:
     [ENGINEERING] - VirtualMedia SMB not support mount with port.
   Infected Motherboard: All
   Affected functions: USB-VD
   Validation:
     1. mount with cifs  ip:xxxx/shared/ should success.
8. Category: Fix
   Description:
     [167049] - The first attempting to turn on the system is always failed.
   Infected Motherboard:  G1SMH, G1SMH-G
   Affected functions: power control
   Validation:
     1) shutdown in OS
     2) ipmitool to power on
9. Category: Major
   Description:
     [169613] - No power supply health status after AC cycle in IPMI FW 1.02.12
   Infected Motherboard: G1SMH-G
   Affected functions: PSU
   Validation:
     1) Set Restore Power Policy to AlwaysOn.
     2) AC Cycle
     3) Check the PSU status shall be display correctly.
10. Category: fix
   Description:
     [169303] - NVSSVT OOB telemetry missing uri for CPU and GPU processors
   Infected Motherboard: Lego
   Affected functions: Redfish
   Validation:
     1) Send GET requeset to /redfish/v1/Systems/1/Processors/GPU_0
     2) Check the property {Oem:{ Nvidia:{ MIGModeEnabled}}}
11. Category: fix
   Description:
     [166301] - STD -- 23062 -- 01.02.12 -- NVSSVT OOB telemetry Sensors uri missing for ERoT_CPU, ERoT_GPU, and FPGA
     [169311] - STD -- 23062 -- 01.02.12 -- NVSSVT OOB telemetry missing uri for CPU and GPU processors
   Infected Motherboard: G1SMH
   Affected functions: Redfish
   Validation:
     1. Check the nvssvt result.
12. Category: Feature
  Description:
      [169230] - STD -- 23062 -- 01.02.12 -- NVSSVT system management OOB telemetry GPU missing properties
  Infected Motherboard: LEGO
  Affected functions: Redfish
  Validation:
      1. GET    /redfish/v1/Chassis/GPU_0 to verify content Pass.
      2. GET    /redfish/v1/Systems/1/Processors/GPU_0 to verify content Pass.
      3. Verity validator, Test Pass.
13. Category: Fix
   Description:
     [168328] - i2c_tegra driver spits out lots of transfer timeouts after idling for some time
   Infected Motherboard: LEGO
   Affected functions: SSIF, I2C.
   Validation:
     1) Run Cburn AC Cycle
     2) NO "I2C transfer timed out" error.
14. Category: Fix
   [164101] - System does not power-up automatically after golden nvbios update
   Infected Motherboards: C2/CG1
   Affected functions: NVBIOS golden update
   Validation
     1) Ensure that system host is powered off.
     2) Perform NVBIOS golden update.
     3) Verify that system host powers up after successful update.
15. Category: fix
   Description:
     [169169] - NVSSVT resiliency BMCCore missing values for ERoTGPU
   Infected Motherboard: G1SMH-G
   Affected functions: Redfish
   Validation:
     1) Get /redfish/v1/Chassis/FPGA_0
     2) Get /redfish/v1/Chassis/ERoT_CPU_0
     3) Get /redfish/v1/Chassis/ERoT_GPU_0
     4) Get /redfish/v1/UpdateService/FirmwareInventory/MGX_GPU_0
     5) Get /redfish/v1/Systems/1/Processors/GPU_0
16. Category: Major
   Description:
     [169103] [ECO] Sensor Tab is Green while Dashboard System tab and Chassis Intru sensor are Red
   Infected Motherboard: X13DEH-P
   Affected functions: Configuration
   Validation:
     1) IPMI Web -> check System status
     2) System -> Componenet Info -> check Sensor status



--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 89308698f0ef66f14d836212d7cbca6ec1529dfe

Firmware Version: 01.02.12
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20240106_01.02.12_STDsp.bin
Production signed Firmware CRC: 3C9FB1F8
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20240106_01.02.12_STDsp.bin
Production signed eMMC Firmware CRC: 3D2E46B3
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20240106_01.02.12_STDsp.bin
Production signed SPI NOR Firmware CRC: 2670E932
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20240106_01.02.12_STDsd.bin
Debug signed Firmware CRC: 41BE08CA
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20240106_01.02.12_STDsd.bin
Debug signed eMMC Firmware CRC: 32166E63
Build Date: 01/06/2024
Redfish API : Redfish_1_11_API_full_list_20231110
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: Major
   Description:
     [167057] - System is stuck on blank screen after trying to update an unsigned bios and reboot
   Infected MotherBoards: G1SMH-G, G1SMH
   Affected Function: FW Update
   Validation:
     1) Upload and update an unsigned BIOS FW image via BMC WebUI or Redfish API
     2) Once around 95% percentage of Task
        a. An warnning pop-up window with message "FW Update Failed, AC Cycle is required to recover. AC Cycle now?" will be shown and User can choose "Yes" or "No" to do the AC cycle or not.
        b. The BIOS Update Task will be exception state with corresponding Task Message "Error: FW Image Update Failed - AC Cycle Required to recover!"
     3) If "Yes", then an AC cycle will be triggered and the inactive BIOS flash will be recoverred during the AC cycle phase.
2. Category: new
   Description:
     [ENGINEERING] - update PSU firmware through BMC UI
   Infected Motherboard: G1SMH, G1SMH-G, X13DEH
   Affected functions: update PSU firmware
   Validation:
     1)Check PSU Model and upate PSU firmware
      "PWS-2K09A-1R"
      "PWS-2K09F-1R2"
      "PWS-2K71A-1R"
3.  Category: Major
    Description:
      [164992] – Power consumption graphs sometimes appear incorrect
    Infected Motherboard: G1SMH-G
    Affected functions:
    Validation:
      1) Reference PB issue 164992 to validate
4. Category: Minor
   Description:
    [166758] - MEL ID now shows after updating Nvidia-specific firmware components
   Infected Motherboard: ALL
   Affected functions: Firmware Update
   Validation:
    1) Update ERoT
    2) MEL should show with MEL ID 0353(success)/0354(fail)
5. Category: Minor
   Description:
    [167607] - MEL ID now shows after updating the AOM CPLD
   Infected Motherboard: ALL
   Affected functions: Firmware Update
   Validation:
    1) Update AOM CPLD
    2) MEL should show with MEL ID 0363(success)/0364(fail)
6. Category: Major
  Description:
    [168517] - AC cycling with 'Shared-AOC' LAN interface will set BMC IP to 0.0.0.0
  Infected Motherboard: G1SMH-G, G1SMH, X13DEH
  Affected functions: Network
  Validation:
    a) power restore policy to "always power on"
    1) Power on SUT, switch lan mode to "Shared-AOC".
    2) Go Configuration -> BMC Settings -> Power Restore Policy, set power restore policy to "always power on".
    3) Do physical AC cycle.
    4) Wait BIOS boot complete, BMC IP should be accessed succefully.
    b) power restore policy to "always power off"
    1) Power on SUT, switch lan mode to "Shared-AOC".
    2) Go Configuration -> BMC Settings -> Power Restore Policy, set power restore policy to "always power off".
    3) Do physical AC cycle.
    4) Wait BMC boot complete, and power on host by pressing physical power button
    5) BMC IP should be accessed succefully.
7. Category: Minor
   Description:
    [167606] - MEL ID now shows after updating the backplane CPLD
   Infected Motherboard: ALL
   Affected functions: Firmware Update
   Validation:
    1) Update Backplane CPLD
    2) MEL ID should show whether the update passed or failed
8. Category: Minor
   Description:
     [168714] - Change the wording in BMC GUI
   Infected Motherboard: ALL
   Affected functions: none
   Validation:
     1) the wording should be "Reset Intrusion"
9. Category: Major
   Description:
     [168596] - cburn fails due to configuration mismatch at cycle 70
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: AOC NIC
   Validation:
     1) Install AOC NIC and cburn stress. no AOC NIC SDR  missing
10. Category: fix
   Description:
     [168610] - Redfish service validator fail
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: Redfish
   Validation:
     1) install TAS
     2) Get /redfish/v1/Systems/1/EthernetInterfaces/
     3) Get /redfish/v1/Systems/1/EthernetInterfaces/x
11. Category: Major
  Description:
    [168072] - Dedicated LAN Interface is not selected by default on C2
  Infected Motherboard: G1SMH-P
  Affected functions: Network
  Validation:
    1) Use dedicated and share both support but no onboard lan platform
       a) plug out all NCSI deivce (AOC, AIOM).
       b) AC cycle, wait BMC web ready.
       c) Check web network page, have failover option, pass.
    2) Use shared only, have no dedicated platform (ex. X13SEED)
       a) login web and check network page.
       b) check don't have failover option, pass.
    3) Use dedicated only, have no shared but not blade platform (ex. X13SAW)
       a) login web and check network page.
       b) check don't have failover option, pass.
12. Category: Major
   Description:
     [167108] - Unable to update CX7 third party NIC AOC through IPMI WebGUI
   Infected Motherboard: G1SMH-G, G1SMH
   Affected functions:
   Validation:
      1) Verify NIC firmware update successfully. It will take 30 mins.


--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 9c3f130d32439b3b7c57b8b1d781f37b50cf89a5

Firmware Version: 01.02.10
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231229_01.02.10_STDsp.bin
Production signed Firmware CRC: C4CD8F69
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231229_01.02.10_STDsp.bin
Production signed eMMC Firmware CRC: D4A6C031
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20231229_01.02.10_STDsp.bin
Production signed SPI NOR Firmware CRC: 2670E932
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231229_01.02.10_STDsd.bin
Debug signed Firmware CRC: D7538765
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231229_01.02.10_STDsd.bin
Debug signed eMMC Firmware CRC: B52159DF
Build Date: 12/29/2023
Redfish API : Redfish_1_11_API_full_list_20231110
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: Major
   Description:
     [165670] - Unresponsive Power Button
   Infected Motherboards: G1SMH, G1SMH-G
   Affected Functions: power button
   Validation:
     1) AC cycle system, push button to power on when BMC is ready.
2. Category: Major
   Description:
     [163415] - X13DEH Redfish Automation Test Fails
   Infected Motherboard: X13DEH
   Affected functions: BIOS update on next-boot
   Validation:
     1) Perform BIOS update through the web page, selecting 'update on next-boot'.
     2) Verify that the update process works as expected."
3. Category: Minor
   Description:
     [160108] - IPv6 Address and Prefix Length data are not displayed when configuring to DHCPv6 Stateless
   Infected Motherboard: X13SEED and ALL
   Affected functions: Configuration
   Validation:
     1) Login web GUI -> Configuration -> Network
     2) Ensure IPv6 is On and DCHP state is "DHCPv6 Stateful"
     3) configuring to "DHCPv6 Stateless" -> Save
     4) Should show "Processing... please wait"
     5) After reach IPv6 address, will show "The requested configuration has been successfully ..."
     6) Auto-refresh page then shown given IPv6 Address
4. Category: fix
   Description:
     [167615] - Fix Redfish-Interop-Validator OCP Profile fail.
   Infected Motherboard: G1SMH
   Affected functions: Redfish
   Validation:
     1. Run the Redfish-Interop-Validator with OCP profile.


--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 5a5762a89f3afe3142727ced5b02c95571e15f79

Firmware Version: 01.02.09
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231221_01.02.09_STDsp.bin
Production signed Firmware CRC: 6CFB2EFE
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231221_01.02.09_STDsp.bin
Production signed eMMC Firmware CRC: 63F21BAD
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20231221_01.02.09_STDsp.bin
Production signed SPI NOR Firmware CRC: 2670E932
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231221_01.02.09_STDsd.bin
Debug signed Firmware CRC: 35256C7E
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231221_01.02.09_STDsd.bin
Debug signed eMMC Firmware CRC: 4835C8CF
Build Date: 12/21/2023
Redfish API : Redfish_1_11_API_full_list_20231110
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: Fix
   Description:
     [166322] - AC Cycle endpoint misspell
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: Redfish
   Validation:
     1) Get /redfish/v1/Systems/1 to verify
     2) Get /redfish/v1/Systems/1/Actions/Oem/OemSystemExtensions/ResetActionInfo to verify
2. Category: Minor
  Description:
    [167740] - Fail to enable and disable ipv6 autoconfig using SMCIPMITool.
  Infected Motherboard: G1SMH, G1SMH-G
  Affected functions: IPv6
  Validation:
    1) Use "SMCIPMITool ipmi lan ipv6 autoconfig" check status.
    2) Use "SMCIPMITool ipmi lan ipv6 autoconfig 1", enable autoconfig, should success.
    3) Use "SMCIPMITool ipmi lan ipv6 autoconfig 0", disable autoconfig, should success.
3. Category: Minor
   Description:
     [167629] - IPMI user account lock can't work. [P3]
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: IPMI
   Validation:
     1. Attempt to use the wrong password to log in bmc and let the user lock.
     2. During locked, The User with the correct password can not log in from Redfish/Web/IPMI.
        ipmitool -H ip -U user -P password raw 6 1 should fail.
     3. Run SATC AccountService test case all pass.
4. Category: Critical
  Description:
    [ENGINEERING] - the redfish HI failed between BMC and BIOS
  Infected Motherboard: G1SMH, G1SMH-G
  Affected functions: Redfish HI
  Validation:
    1) Change GPU or AOC to verify BMC has the correct GPU or AOC info reported by BIOS.
5. Category: Major
   Description:
     [ENGINEERING] - NCSI re-scan and switch to Failover in PWRON/PWROFF action.
   Infected Motherboard: G1SMH-G, G1SMH
   Affected functions: Configuration
   Validation:
     1) Login web GUI -> Configuration -> Network
     2) Shared / Shared-AOC should be enabled
     3) Power Off -> wait action complete
     4) Page auto refresh
     5) Shared / Shared-AOC should be disabled
6. Category: Major
  Description:
    [166377] - cburn LANPLUS interface not accessible after 'Shared AOC' was selected in WebGUI LAN interface.
    [163527] - LAN Interface should only have dedicated option.
  Infected Motherboard: G1SMH-G, G1SMH
  Affected functions: Network
  Validation:
    1) AC cycle with restore power policy always off.
    2) After BMC web can login, power on host.
    3) Check web Network page, should show lan mode Shared lan option.
    1) AC cycle with restore power policy always on.
    2) Wait until BMC web can login and host is power on.
    3) Check web Network page, should show lan mode Shared lan option.
    1) Power on host and set lan mode to Shared.
    2) After set Shared OK, then Power off.
    3) Lan mode should switch to Failover.


--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 6853925aace462cdc62da0bb2a07c8cc2f4599b5

Firmware Version: 01.02.08
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231218_01.02.08_STDsp.bin
Production signed Firmware CRC: A642187A
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231218_01.02.08_STDsp.bin
Production signed eMMC Firmware CRC: 1D0C8142
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20231218_01.02.08_STDsp.bin
Production signed SPI NOR Firmware CRC: 2670E932
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231218_01.02.08_STDsd.bin
Debug signed Firmware CRC: 5CC545C9
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231218_01.02.08_STDsd.bin
Debug signed eMMC Firmware CRC: 95924D13
Build Date: 12/18/2023
Redfish API : Redfish_1_11_API_full_list_20231110
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: Major
   Description:
     [167736] - PSU Status changes from Present to Not Present during AC ONOFF
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: PSU status in SMBIOS
   Validation:
     1) during AC ONOFF, check PSU status change in SMBIOS
2. Category: Minor
   Description:
     [ENGINEERING] - Motherboard CPLD update should be hidden in C2/CG1
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: firmware update
   Validation:
     1) (Motherboard) CPLD button should be not in firmware update page.
3. Category: Minor
   Description:
   [ENGINEERING] - incorrect FPGA FW version parsing and saving during FPGA FW update.
   Infected Motherboards: G1SMH, G1SMH-G
   Affected Functions: FPGA FW update + FW version in WebUI
   Validation:
     1) Perform FPGA MB FW update with FPGA_MBD-G1SMH-G-10XX1D31_20231205_F2.00.8C_STDsp.bin
     2) After update and AC cycle
     3) Perform FPGA Golden FW update
     4) Check FW versions of "FPGA motherboard" and "FPGA motherboard Golden"
4. Category: Fix
   Description:
    [ENGINEERING] Fix - Updating AOM now shows detailed location information in the MEL. Should follow firmware inventory naming.
   Infected Motherboard: ALL
   Affected functions: Firmware Update
   Validation:
    1) Update AOM
    2) After completion, MEL will display one of these variants:
       Updating AOM # CPLD firmware was successful
       Updating AOM <location> CPLD firmware was successful
       Updating AOM # <board> CPLD firmware was successful
       Updating AOM <location> <board> CPLD firmware was succesful.
       Example of 4) "Updating AOM rear IO board AOM-GP101-IPMI CPLD firmware was succesful."


--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 31f589af4f880fb3172f059e3d8dd39947905a35

Firmware Version: 01.02.07
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231215_01.02.07_STDsp.bin
Production signed Firmware CRC: C9DE0554
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231215_01.02.07_STDsp.bin
Production signed eMMC Firmware CRC: D2B93DA4
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20231215_01.02.07_STDsp.bin
Production signed SPI NOR Firmware CRC: 2670E932
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231215_01.02.07_STDsd.bin
Debug signed Firmware CRC: D6E86469
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231215_01.02.07_STDsd.bin
Debug signed eMMC Firmware CRC: BF96CD7B
Build Date: 12/15/2023
Redfish API : Redfish_1_11_API_full_list_20231110
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: Fix
   Description:
    [ENGINEERING] Fix - Functions that should not be running when firmware update is in progress should be behaving correctly now
   Infected Motherboard: ALL
   Affected functions: Firmware Update
   Validation:
    1) Upload firmware to BMC, but don't update yet.
    2) Try restoring to factory default via Web GUI. Restore button should be disabled.
    3) POST to /redfish/v1/Managers/1/Actions/Oem/SmcManagerConfig.Reset should return 503 status
    4) Raw commands:
       0x30 0x40
       0x30 0x41
       0x30 0x42
       Should return "Device firmeware in update mode"
2. Category: Fix
   Description:
     [167049] - The first attempting to turn on the system is always failed.
   Infected Motherboard:  G1SMH, G1SMH-G
   Affected functions: power control
   Validation:
     1) shutdown in OS
     2) ipmitool to power on

--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: df7866e5b777487913fadb137f7e3f7c85ce66a4

Firmware Version: 01.02.06
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231213_01.02.06_STDsp.bin
Production signed Firmware CRC: 0B710EE2
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231213_01.02.06_STDsp.bin
Production signed eMMC Firmware CRC: BD3F854F
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20231213_01.02.06_STDsp.bin
Production signed SPI NOR Firmware CRC: 2670E932
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231213_01.02.06_STDsd.bin
Debug signed Firmware CRC: 5E26BBA9
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231213_01.02.06_STDsd.bin
Debug signed eMMC Firmware CRC: 9A71A1E6
Build Date: 12/13/2023
Redfish API : Redfish_1_11_API_full_list_20231110
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: Minor
  Description:
    [167262] - Should not block setting ipv4 dns to 255.255.255.255.
  Infected Motherboard: G1SMH-P, G1SMH-G-P
  Affected functions: DNS
  Validation:
    1) Use command, ipmitool raw 30 68 0A 03 00 00 FF FF FF FF.
    2) Check web netwrok page manually DNS field, should set 255.255.255.255.
2. Category: Fix
   Description:
       [167282] - missing ProcessSummary "Model" value in /redfish/v1/Systems/1
   Infected Motherboard: ALL
   Affected functions: Redfish
   Validation:
       1) Get /redfish/v1/Systems/1 to verify
3. Category: fix
   Description:
     [166270] - [TAS on Arm] BMC error when command length is greater than 32 bytes
     [164159] - IPMICFG automation test failed.
     [ENGINEERING] - inband ipmitool does not work any more
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: inband ipmitool
   Validation:
     1) verify inband ipmitool operation
4. Category: fix
   Description:
     [166167] - CG1 is missing GPU after 'One Diag'
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: AC Cycle
   Validation:
     1) unplug PSU power cord do AC cycle once
     2) then use BMC do AC Cycle serveral time. each time should be good for CG1.
5. Category: Fix
   Description:
     [167274] - Fail to sync fru1 to fru
   Infected Motherboard: G1SMH, G1SMH-G, G2DMH-G
   Affected functions: FRU
   Validation:
     1) delete FRU0 BP, BM, BS
     2) Reset BMC
     3) expected see FRU0 being restored from FRU1
6. Category: Feature
  Description:
      [ENGINEERING] - Add clearlog action of postcodes
  Infected Motherboard: G1SMH, G1SMH-G
  Affected functions: Redfish
  Validation:
      1) GET    /redfish/v1/Systems/1/LogServices/PostCodes to verify content Pass.
      2) GET    /redfish/v1/Systems/1/LogServices/PostCodes/Entries to verify content Pass.
      3) POST   /redfish/v1/Systems/1/LogServices/PostCodes/Actions/LogService.ClearLog, Test pass
      4) Verity /redfish/v1/Systems/1/LogServices/PostCodes validator, Test Pass.
      5) GET    /redfish/v1/Oem/Supermicro/DumpService/Dumps/TroubleShooting  to verify content Pass.
      6) Maintenance Event Log, to verify content Pass.
      7) verity nvssvt tool for postcodes, Test Pass.


--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: ba7d2797378da19f19bf2a5b17d63d04e1ffc785

Firmware Version: 01.02.05
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231207_01.02.05_STDsp.bin
Production signed Firmware CRC: 6552D7DB
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231207_01.02.05_STDsp.bin
Production signed eMMC Firmware CRC: 9F08C526
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20231207_01.02.05_STDsp.bin
Production signed SPI NOR Firmware CRC: 70F1FF1F
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231207_01.02.05_STDsd.bin
Debug signed Firmware CRC: 9F767686
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231207_01.02.05_STDsd.bin
Debug signed eMMC Firmware CRC: 1735F599
Build Date: 12/07/2023
Redfish API : Redfish_1_11_API_full_list_20231110
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1.Category: Major
  Description:
    [166307] - Fail to set dedicated link and no MEL generated
  Infected Motherboard: G1SMH,G1SMH-G, X13DEH
  Affected Function: Network
  Validation:
    1) Go to Configuration -> Network
    2) Change LAN interface to "Dedicated"
    3) Its LAN capabilities support auto neg only
    4) Use raw command 30 70 63 02 to get Lan capabilities, BMC should return 0x01
2. Category: fix
   Description:
     [166162] - Severity in sensor excel table is incorrect for Chassis Intru
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: Configuration
   Validation:
     1) Please refere PB issue #166162
3. Category: fix
   Description:
     [ENGINEERING] - correct CPU fan curve
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: Fan control
   Validation:
     1) Thermal CPU fan curve
4. Category: Feature
  Description:
      [ENGINEERING] - Add postcodes for LogService and add registries of BIOS
  Infected Motherboard: LEGO_C2
  Affected functions: Redfish
  Validation:
      1. GET /redfish/v1/Systems/1/LogServices to verify content Pass.
      2. GET /redfish/v1/Systems/1/LogServices/PostCodes to verify content Pass.
      3. GET /redfish/v1/Systems/1/LogServices/PostCodes/Entries to verify content Pass.
      4. GET /redfish/v1/Systems/1/LogServices/PostCodes/Entries/1 to verify content Pass.
      5. GET /redfish/v1/Registries to verify content Pass.
      6. GET /redfish/v1/Registries/BIOS to verify content Pass.
      7. GET /registries/BIOS.1.0.0.json to verify content Pass.
      8. Verity (PostCodes related && registries related of BIOS) validator, Test Pass.
5. Category: Minor
   Description:
     [166039] - Fail to receive correct SNMPv3 alert
   Infected Motherboard: G1SMH
   Affected functions: Redfish
   Validation:
     1) Config workable event subscription and check can get the snmpv3trap form targe server.
      Patch /redfish/v1/EventService/Subscriptions/1 {"Oem":{"Supermicro":{"EnableSubscription":true,"UserName":"aflyfish","Severity":"Information"}},
      "Protocol":"SNMPv3","Destination":{IP},
      "SNMP":{"AuthenticationProtocol":"HMAC_MD5","EncryptionProtocol":"CBC_DES","AuthenticationKey":"AABBCC123c","EncryptionKey":"AABB1234c"},
      "EventTypes":["Alert"]}
     2) Patch with short length  {"SNMP": {"AuthenticationKey": "AABC123c", "EncryptionKey": "AAB1234c"}}
     3) issue raw 0x4 0x2 0x4 0x5 0xaa 0x8 0x0 0xff 0xff check can get the snmpv3trap form targe server.
6. Category: Minor
   Description:
     [166161] - AC Cycle option is not displayed when logging in to web for the first time
   Infected Motherboard: G1SMH-P, G1SMH-G-P
   Affected functions: WebUI
   Validation:
     1) clear browser cache/cookies->Login WebUI->Power Control->display AC Cycle option
7. Category: Fix
   Description:
    [165982] Fix - RoT State changed to disabled after factory reset
   Infected MotherBoards: ALL
   Affected Function: Security State
  Validation:
    For OTP provisioned system
    1) Login BMC webpage
    2) In "Dashboard" -> "Security" icon is Green
    3) In "System" -> "Security" -> "Rot State" is Green
    4) Issue IPMI cmd 0x30 0x41 and wait for BMC back to normal
    5) Login BMC webpage
    6) Check "Dashboard" -> "Security" icon is Green
    7) Check In "System" -> "Security" -> "Rot State" is Green
8. Category: Major
   Description:
     [166888] - GPU temp sensor assertion/deassertion events are recorded in IPMI SEL during on/off test
   Infected Motherboard: G1SMH and ALL
   Affected functions: SEL
   Validation:
     1) on/off stress testing.
9. Category: Major
   Description:
     [166380] - Arm sbmr acs test automation fail
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: IPMI
   Validation:
     1) Check SSIF capabilities by command 'Get System Interface Capabilities':
         ipmitool raw 0x06 0x57 0x0
10. Category: feature
   Description:
     [ENGINEERING] - Add Redfish APIs for NVSSVT test
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: Redfish
   Validation:
     1) Get following Redfish URL and check the result:
          /redfish/v1/Fabrics
          /redfish/v1/Fabrics/C2CLinkFabric_0
          /redfish/v1/Fabrics/GPU_NVLinkFabric_0
          /redfish/v1/Chassis/CPU_X  (X is the CPU index)
          /redfish/v1/Chassis/GPU_X  (X is the GPU index)
          /redfish/v1/Chassis/FPGA_0
          /redfish/v1/ComponentIntegrity/ERoT_CPU_X/SPDMGetSignedMeasurementsActionInfo  (X is the CPU index)
          /redfish/v1/ComponentIntegrity/ERoT_GPU_X/SPDMGetSignedMeasurementsActionInfo  (X is the GPU index)
11. Category: Minor
   Description:
     [166364] - The CPU sensor reading became "0" during DC onoff stress
     [164373] - While CPU temperature N/A, fan speed did not hold on Full speed 
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: CPU Temp
   Validation:
      1) CPU temperature become 0 or NA.
      2) Check if Fan is fullspeed.
      3) Check if "CPU x temperature access degraded or unavailable" will be generated.
12. Category: Minor
  Description:
    [165970] - Should not be able to set invalid ipv6 dns values using SMCIPMITool raw commands
  Infected Motherboard: G1SMH-G-P, G1SMH-P
  Affected functions: IPv6 DNS, IPv6 static IP
  Validation:
      Use below ipmi oem command test, all should block (return CC)
      1) Set IPv6 DNS 1:
         a) ipmitool raw 30 68 0A 01 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
         b) ipmitool raw 30 68 0A 01 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01
         c) ipmitool raw 30 68 0A 01 01 00 FF 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
         d) ipmitool raw 30 68 0A 01 01 00 FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF
         e) ipmitool raw 30 68 0A 01 01 00 Ff 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01
      2) Set IPv6 Dns 2:
         a) ipmitool raw 30 68 0A 03 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
         b) ipmitool raw 30 68 0A 03 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01
         c) ipmitool raw 30 68 0A 03 01 00 FF 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
         d) ipmitool raw 30 68 0A 03 01 00 FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF
         e) ipmitool raw 30 68 0A 03 01 00 Ff 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01
      3) Set IPv6 static address:
         a) ipmitool raw 30 68 09 01 02 00 00 FF 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 40
         b) ipmitool raw 30 68 09 01 02 00 00 Ff 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01 40
         c) ipmitool raw 30 68 09 01 02 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 40
         d) ipmitool raw 30 68 09 01 02 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01 40
         e) ipmitool raw 30 68 09 01 02 00 00 FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF 40
13. Category: Fix
   Description:
     [166770] - (NV) Bios evidence fails to generate after recovery
   Affected Motherboards: G1SMH-G, G1SMH
   Affected Functions: BIOS update/recovery
   Validation:
     1) Perform BIOS recovery.
     2) Generate BIOS evidence via Web GUI PFR action page
     3) Validate successful generation in Maintenance Event Log via Web GUI
     4) Verify additionally by Downloading BIOS evidence via PFR actions.
14. Category: Fix
   Description:
     [165904] - Incorrect cpld version and C2 cannot to get bios version from SMCIPMITool
   Affected Motherboards: G1SMH-G, G1SMH
   Affected Functions: FPGA
   Validation:
     1) verify FPGA version F2.00.8C
15. Category: Fix
   Description:
     [167049] - The first attempting to turn on the system is always failed.
     [165670] - Unresponsive Power Button
   Affected Motherboards: G1SMH-G, G1SMH
   Affected Functions: power on
   Validation:
     1) reboot BMC and power on
     2) AC cycle and power restore
15. Category: Fix
   Description:
     [167055] - GPU component page in BMC GUI hangs forever
   Affected Motherboards: ALL
   Affected Functions: GPU page
   Validation:
     1) Check GPU page available
16. Category: Minor
   Description:
     [167062] - CPU information is different between smbios type 4 and WebGUI
     [ENGINEERING] - Filter GPU information in CPU tab
   Infected Motherboard: G1SMH-G
   Affected functions: Configuration
   Validation:
     1) Login web GUI -> System -> CPU

--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 23c8b3d1538e69c436515b3dde5b612efa797239

Firmware Version: 01.02.03
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231118_01.02.03_STDsp.bin
Production signed Firmware CRC: 49B7AE32
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231118_01.02.03_STDsp.bin
Production signed eMMC Firmware CRC: D8E22A01
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20231118_01.02.03_STDsp.bin
Production signed SPI NOR Firmware CRC: 70F1FF1F
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231118_01.02.03_STDsd.bin
Debug signed Firmware CRC: C75ABC64
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231118_01.02.03_STDsd.bin
Debug signed eMMC Firmware CRC: 2416A9B5
Build Date: 11/18/2023
Redfish API : Redfish_1_11_API_full_list_20231110
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: Major
   Description:
     [ENGINEERING] - new threshold for CPU and GPU
   Infected Motherboard: G1SMH-P, G1SMH-G-P
   Affected functions: sensor
   Validation:
     1) C2/CG1 CPU threshold 85, 92, 94
     2) CG1 GPU threshold 80 90 92
2. Category: Major
   Description:
     [ENGINEERING] - FRU0 read and write failed
   Infected Motherboard: G1SMH-P, G1SMH-G-P
   Affected functions: FRU
   Validation:
     1) read and write FRU0 and FRU1
3. Category: Major
   Description:
     [ENGINEERING] - correct FPGA fan curve in all zones
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: fan curve
   Validation:
     1) FPGA fan curve follow spec
4. Category: Major
   Description:
     [164136] SuperDiag doesn't support X13DEH BMC FW
   Infected Motherboard: X13DEH
   Affected functions:
   Validation:
     1) Verify SuperDiag
5. Category: Major
   Description:
     [165798] - Power consumption graph issue
     [164992] - Power Consumption Graphs sometimes appear incorrect.
   Infected Motherboard: G1SMH,G1SMH-G, X13DEH
   Affected functions: Power consumption
   Validation:
     1) no 65K power consumption in Power consumption graph issue
6. Category: Major
   Description:
     [163527] - LAN Interface should only have dedicated option
   Infected Motherboard: G1SMH, G1SMH_G, X13DEH
   Affected functions: Share LAN
   Validation:
     1) Connect AOC NIC and connect JNCSI cable
     2) Web show Dedicated, Failover, Failover-AOC,Shared, and Shared-AOC
     3) Verify all LAN options
7. Category: Minor
   Description:
     [163546] - Different ui redirect behavior on different pages when there is no license
   Infected Motherboard: G1SMH, G1SMH-G, X13DEH
   Affected functions: Configuration
   Validation:
     1) Clear all License
     2) Login Web GUI -> Configuration -> Notifications -> Syslog
8. Category: Major
   Description:
     [164861] - Redfish service validator fail
   Infected Motherboard: G1SMH_G
   Affected functions: Redfish
   Validation:
     1) Get /redfish/v1/Systems/1/Processors/GPU_0
9.Category: Major
  Description:
    [166026] - BMC Host Interface becomes "Disabled"
  Infected Motherboard: All
  Affected Function: Host Interface
  Validation:
    1) Run on/off test to verify this issue.
10.Category: Major
  Description:
    [ENGINEERING] - Added MEL after changed Host Interface "RNDIS Connection" or "CDC-ECM Connection"
  Infected Motherboard: All
  Affected Function: Host Interface
  Validation:
    1) Check MEL after changed Host Interface "RNDIS Connection" or "CDC-ECM Connection"
11. Category: Feature
   Description:
       [ENGINEERING] - Add Property "Product" for /redfish/v1
   Infected Motherboard: all
   Affected functions: Redfish
   Validation:
       1) Redfish GET /redfish/v1 to verify Product
12. Category: Enhancement
   Description:
     [ENGINEERING] - Support BIOS update before post completion
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: BIOS update
   Validation:
     1) Power on + BIOS isn't done + BIOS update (immediate): should work.
     2) Power on + BIOS is done + BIOS update (immediate): should work.
     3) Power off + BIOS update (immediate): should work.
     4) BIOS update (next-boot) + power on: should work.
     5) BIOS update (next-boot) + power cycle: should work.
     6) BIOS update (next-boot) + power reset: should work.
     7) BIOS update (next-boot) + OS reset: should work.

--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: cc4fdfd3e79cd3429370139de69a160344c14934

Firmware Version: 01.02.02
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231110_01.02.02_STDsp.bin
Production signed Firmware CRC: F6272B32
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231110_01.02.02_STDsp.bin
Production signed eMMC Firmware CRC: E0CF8D4F
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20231110_01.02.02_STDsp.bin
Production signed SPI NOR Firmware CRC: 70F1FF1F
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231110_01.02.02_STDsd.bin
Debug signed Firmware CRC: 4FB96E61
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231110_01.02.02_STDsd.bin
Debug signed eMMC Firmware CRC: 2B4859FE
Build Date: 11/10/2023
Redfish API : Redfish_1_11_API_full_list_20230918
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: Major
   Description:
     [164439] - BIOS "Next-boot Update" behavior is different from our standard MB.
   Infected Motherboard: G1SMH-P, G1SMH-G-P
   Affected functions: BIOS update
   Validation:
     1) Power on: MCTP discovery after BIOS finishes.
     2) Power off: Immediate MCTP discovery.
     3) Power cycle: Two MCTP discoveries - immediate and after BIOS finishes.
     4) Power reset: MCTP discovery after BIOS finishes.
     5) Power on, BIOS update (immediate): Should work.
     6) Power off, BIOS update (immediate): Should work.
     7) Power on, BIOS update (next-update), power cycle: Should work.
     8) Power on, BIOS update (next-update), power reset: Should work.
     9) Power on, BIOS update (next-update), OS reset: Should work.
2. Category: Feature
   Description:
     [ENGINEERING] - support AC Cycle on WebUI HTML5 SNMP
   Infected Motherboards: G1SMH-P, G1SMH-G-P
   Affected Functions: WebUI iKVM SNMP
   Validation:
      1) Login Web -> Remote Control-> Launch Console -> AC Cycle -> should work
      2) SNMP: snmpset -v 2c -c public {BMC IP} .1.3.6.1.4.1.21317.1.4.0 i 3
      3) POST redfish/v1/Systems/1/Actions/Oem/ComputerSystem.AcCyle to do ac cycle
3.Category: Feature
   Description:
     [ENGINEERING] - Enable USB Lan 2 options feature (WEB)
   Infected Motherboard: ALL
   Affected Function: Host Interface
   Validation:
     1) Set Host Interface to RNDIS/CDC-ECM on WEB, then check result under OS
        1-1) Set USB Connection to RNDIS connection, and click Save, then check dmesg content under Linux OS,
             should see message similar with "usb0: register 'rndis_host' at usb-xxxx:xx:xx.xxx.x"
        1-2) Set USB Connection to CDC-ECM connection, and click Save, then check dmesg content under Linux OS,
             should see message similar with "usb0: register 'cdc_ether' at usb-xxxx:xx:xx.xxx.x"
     2) Run BMC load factory, check BMC default value, it should be RNDIS
4. Category: Major
   Description:
     [Enhancement] - OpenJDK support
   Infected Motherboard: All
   Affected functions: JavaAP, iKVM, SOL
   Validation:
     1) Login to WebGUI and enter to Remote Control and change Launch interface to JAVA plug-in.
     2) Press Launch Console.
     3) Use \\super-fs\SMCI-Apps-Repository\None-License-Required\Applications\RedHat OpenJDK and open with javaws.exe in java-1.8.0-openjdk\webstart to launch jnlp file.
     4) iKVM should be normal to launched.
5. Category: Major
   Description:
     [165656] - Unable to load SMTP page
   Infected Motherboard: G1SMH-P, G1SMH-G-P
   Affected functions: Configuration
   Validation:
     1) Login Web GUI -> Configuration -> Notifications -> SMTP
6. Category: Minor
   Description:
     [165796] - Typo in smc rakp modal when disable rakp
   Infected Motherboard: G1SMH and ALL
   Affected functions: WEBUI
   Validation:
     1) go to configuration -> BMC settings -> SMC RAKP page,  change the status from enable to disable, and check the modal content
7. Category: Minor
   Description:
     [165739] - 'Verify the certification of the server' checkbox is not checked by default when using https server on web Virtual media page
   Infected Motherboard: G1SMH-P, G1SMH-G-P and ALL
   Affected functions: Configuration
   Validation:
     1) Activate License as DCMS or OOB
     2) Login Web GUI -> Configuration -> Virtual Media
     3) Edit VM Connection of "Device 1"
     4) Input Share Host with IP "https://1.1.1.1"
8. Category: Minor
   Description:
     [163546] - Different ui redirect behavior on different pages when there is no license
   Infected Motherboard: G1SMH-P, G1SMH-G-P and ALL
   Affected functions: Configuration
   Validation:
     1) Clear all License
     2) Login Web GUI -> Configuration -> BMC Settings -> System Lockdown
9. Category: Minor
   Description:
     [165455] - [saa_1.0.0_alpha_G1SMH-G] Fail to get gpu info
   Infected Motherboard: G1SMH-G and ALL
   Affected functions: Redfish
   Validation:
     1) Get /redfish/v1/Systems/1/Processors/
10. Category: Minor
   Description:
     [164861] - Redfish service validator fail
   Infected Motherboard: G1SMH and ALL
   Affected functions: Redfish
   Validation:
     1. Run validator Pass.
11. Category: Minor
  Description:
    [164083] - SNMP traps from BMC resulting in malformed packets.
  Infected Motherboard: G1SMH-P and ALL
  Affected functions: Network SNMP
  Validation:
    1) Prepare another host and run WireShark 4.x.xx or snmptrapd for receiving snmp trap.
    2) Go web page, Configuration -> Notifications -> SNMP, enable SNMP(v1) on.
    3) Configuration -> Notifications -> Alert, set destination address as your snmp trap receive host ip.
    4) Use ipmitool raw 0x04 0x02 0x04 0x01 0x0B 0x0B 0x03 0xFF 0xFF, send an snmp trap message bigger than 127 bytes.
    5) Check your receiving host, should can revice a snmp trap and packet form is correct.

--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 5dfd8b9dbd47643eeb4e1d4b8b4ba6660a13d7c5

Firmware Version: 01.02.01
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231103_01.02.01_STDsp.bin
Production signed Firmware CRC: 65D845F8
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231103_01.02.01_STDsp.bin
Production signed eMMC Firmware CRC: E9BB22FC
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20231103_01.02.01_STDsp.bin
Production signed SPI NOR Firmware CRC: 70F1FF1F
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231103_01.02.01_STDsd.bin
Debug signed Firmware CRC: 9B2E2C5E
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231103_01.02.01_STDsd.bin
Debug signed eMMC Firmware CRC: 6554DAB8
Build Date: 11/03/2023
Redfish API : Redfish_1_11_API_full_list_20230918
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: Major
   Description:
     [ENGINEERING] - 01.02.00 I2C unstable
     [ENGINEERING] - rollback I2C enhancement in 01.02.00
   Infected Motherboard: All
   Affected functions: I2C
   Validation:
     1. Verify AOC Temp

--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 720e2b20cf6dd7b49ac5741573b49e414f0bcb3f

Firmware Version: 01.02.00
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231103_01.02.00_STDsp.bin
Production signed Firmware CRC: 5EA45581
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231103_01.02.00_STDsp.bin
Production signed eMMC Firmware CRC: D40D5FCA
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20231103_01.02.00_STDsp.bin
Production signed SPI NOR Firmware CRC: 70F1FF1F
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231103_01.02.00_STDsd.bin
Debug signed Firmware CRC: 0567FE9F
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231103_01.02.00_STDsd.bin
Debug signed eMMC Firmware CRC: FDD76536
Build Date: 11/03/2023
Redfish API : Redfish_1_11_API_full_list_20230918
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1.Category: Major
  Description:
    [ENGINEERING] - new thermal guide requirement
  Infected Motherboard: G1SMH, G1SMH-G
  Affected Function: NIC, FPGA thermal
  Validation:
    1) FPGA Temp’ to ref: SSTDG_v4.07, Sec 5.1.3
    2) AOC_NIC5, 6, 7 fan zone to connect with all PWM1, 2, 3
    3) "AOM IO Temp" ref: SSTDG_v4.07_5.1.3
2. Category: Enhancement
    Description:
      [ENGINEERING] - AC Cycle oem action for CG1
    Infected Motherboard: G1SMH, G1SMH-G
    Affected functions: Redfish
    Validation:
      1) POST redfish/v1/Systems/1/Actions/Oem/ComputerSystem.AcCyle to do ac cycle
      2) Get redfish/v1/Systems/1 for the ac cycle target.
3.Category: Major
  Description:
    [ENGINEERING] - power button cannot make force power off
  Infected Motherboard: G1SMH, G1SMH-G
  Affected Function: power button
  Validation:
    1) long press button then release to force power off and check MEL
4. Category: Major
   Description:
     [164369] - WebGUI storage monitoring unable to eject E1.S drives
   Infected MotherBoards: G1SMH, G1SMH-G
   Affected Function: E1.S eject
   Validation:
     1) Install Bridge board AOM-BB-GP102 and connect VPP to bridge board.
     2) E1.S eject should be there
     3) Remove Bridge board AOM-BB-GP102 and disconnect VPP
     4) E1.S eject should be hidden
5. Category: Major
   Description:
     [162615] - Watchdog is not working
     [164794] - cburn ONOFF BPC Hang on penguies/ watchdog issue
   Infected MotherBoards: G1SMH, G1SMH-G
   Affected Function: Watchdog
   Validation:
     1) verify the watchdog setting is under "BMC" tag in the BIOS.
     1) verify the watchdog setting is under "Advanced" tag in the BIOS.
6. Category: Minor
   Description:
     [164861] - Redfish service validator fail
   Infected Motherboard: G1SMH_G
   Affected functions: Redfish
   Validation:
     1) run Service Validator
7. Category: Minor
   Description:
     [164904] - Memory Serial Number and Part Number are not displayed correctly via web gui and SAA
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: Memory info
   Validation:
     1) GET https://BMCIP/redfish/v1/Systems/1/Memory/1
8. Category: Major
   Description:
     [162573] - CG1 CPU Temp somehow became "0"
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: CPU Temp
   Validation:
     1) check CPU Temp
9. Category: Minor
   Description:
     [163719] - Null user test failed, created null users are not displayed on users page
   Infected Motherboard: G1SMH and ALL
   Affected functions: Redfish, Web
   Validation:
     1) Use ipmitool to set user privilege, ipmitool user priv 3 0x4
     2) Make sure the anonymous user is showed on web
10. Category: Major
  Description:
    [#164760] SUM -- Failed to Set LAN AutoConfiguration DHCPv6Mode Configuration.
    [#164371] Fail to disable ipv6 autoconfig using SMCIPMITool.
    [#165279] SUM -- Failed to Set LAN AutoConfiguration DHCPv6Mode Configuration.
  Infected Motherboard: G1SMH-G, H12SSFF-AN6 and All
  Affected functions: IPv6
  Validation:
      1) Use "lan ipv6 mode 0", change ipv6 to stateless mode.
      2) Use "lan ipv6 autoconfig 1" command to enable autoconfig.
      3) Use "lan ipv6 autoconfig" command check current status.
      4) Use "lan ipv6 autoconfig 0" command.
      5) Use "lan ipv6 autoconfig" command check current status, should disable successfully.
11. Category: Major
   Description:
     [ENGINEERING] - Fix Redfish Inconsistency.
   Infected Motherboard: All
   Affected functions: Redfish
   Validation:
     1. Verify by TS & SW-Lab.

--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: af1597e234dc66139c5cb5cfa27e6bcfe1ac6704

Firmware Version: 01.00.12
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231021_01.00.12_STDsp.bin
Production signed Firmware CRC: D271BD59
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231021_01.00.12_STDsp.bin
Production signed eMMC Firmware CRC: 2905F1BB
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20231021_01.00.12_STDsp.bin
Production signed SPI NOR Firmware CRC: 70F1FF1F
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231021_01.00.12_STDsd.bin
Debug signed Firmware CRC: 859361EA
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231021_01.00.12_STDsd.bin
Debug signed eMMC Firmware CRC: 0CFEBCEA
Build Date: 10/21/2023
Redfish API : Redfish_1_11_API_full_list_20230918
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1.Category: Minor
  Description:
    [162966] - Set 0.0.0.0 to DNS Server IP would be replaced by valid DNS Server2 IP after setting saved.
    [163298] - Set 0.0.0.0 to DNS Server IP would be replaced by valid DNS Server2 IP after setting saved.
    [163549] - After saving network IPv4 DNS Server IP as 0.0.0.0, the field does not display 0.0.0.0, also no MEL.
  Infected Motherboard: ALL
  Affected functions: Network DNS
  Validation:
      1) Go web Configuration -> Network page
      2) Set IPv4 Manually obtain DNS server IP "0.0.0.0" and press save, should set success and show DNS 0.0.0.0.
      3) Set IPv6 Manually obtain DNS server IP "::", should show warning message and can't press save button.
2. Category: Minor
   Description:
     [162829] - Set correct format but invalid NTP Server IP, error message return 'Oops' instead of [MEL-0255]
   Infected Motherboard: H13SSF-P and ALL
   Affected functions: Configuration
   Validation:
     1) restore setting to factory default by smcipmitool: ipmi raw 30 41
     2) Login BMC WEB with ADMIN priviledge
     3) Set NTP: Configuration-> BMC Settings-> Date and Time
     4) NTP Enable: OFF to ON
     5) Primary NTP Server: localhost to wrong.google.com, then 'Save'
3. Category: Minor
   Description:
     [161789] - [GUI] Virtual Media/Network/User(SNMP) in Help page are inconsistent with Actual WEB page
   Infected Motherboard: H13SSF-P and ALL
   Affected functions: Configuration
   Validation:
     1) IPMI Web -> help page -> Configuration
     2) Find 'General' of Network' section
4. Category: Minor
   Description:
     [162794] - License require behavior/message not quite match with SW-PM definition
   Infected Motherboard: H13SSF-P and ALL
   Affected functions: Configuration
   Validation:
     1) License require behavior/message should match with SW-PM definition
5. Category: Minor
   Description:
     [164046] - Duplicate MEL when setup Dedicated Link Speed & 1G Full Duplex MEL not match with option name.
   Infected Motherboard: X12DPT-PT6 and ALL
   Affected functions: MEL
   Validation:
     1)  Log into Web GUI and change page to Configuration -> Network.
     2)  Set Dedicated Link from 'Auto Negotiation' to '1G Full Duplex'
     3)  Set Dedicated Link from '1G Full Duplex' to 'Auto Negotiation'
     4)  Check MEL
6. Category: Enhancement
   Description:
     [ENGINEERING] - display GPU on Web UI
   Infected Motherboard: G1SMG, G1SMH-G
   Affected functions: GPU
   Validation:
      check NV GPU on Web UI
7. Category: Major
    Description:
    [162991] - No MBFPGA ver in BIOS setup menu
    Infected Motherboards: G1SMH/G1SMH-G
    Affected Functions: 68subcmd - 0x30 0x68 0x29 + 0x30 0x68 0x28 0x03
    Validation:
      1) Check with BIOS team to get BIOS to support it.
      2) Use ipmitool raw command 0x30 0x68 0x29 to get MBFPGA version
      3) Verify MBFPGA version from command response output bytes and BIOS setup.
8. Category: Major
   Description:
     [164373] - While CPU temperature N/A, fan speed did not hold on Full speed
   Infected Motherboard: G1SMH, G1SMH-G, X13DEH
   Affected functions: Fan control
   Validation:
     1) CPU Temp duty cycle should be 100% if CPU Temp reading is 0
9. Category: Minor
   Description:
     [164311] - text "Next-boot Updat" is faulty.
   Infected Motherboard: X12DPG-QR-P and ALL
   Affected functions: Configuration
   Validation:
     1) UI > Maintenance > Firmware Management > Update > BIOS
     2) Notice the text under Choose Update Time
10. Category: Minor
    Description:
    PB Issue #164023 - No MEL for BIOS Golden Image update successful.
    Infected Motherbaord: C2/CG1
    Affected Functions: Golden image update + FW recovery.
    Validation:
      1) Update BIOS, EROT, MBFPGA golden images.
      2) Checked related Maintenance Event Logs on Web GUI for action
         initiation and completion status for each FW.
      3) Perform Recovery BIOS, EROT, MBFPGA.
      4) Check Maintenance Event Log page on Web GUI check MEL for completion
         status for each FW, respectively.
11. Category: Minor
   Description:
     [163206] - Authentication key and encryption key fields are not validated when adding SNMP account type in modify user form
   Infected Motherboard: G1SMH-P
   Affected functions: Configuration
   Validation:
     1) Please refere PB issue #163206
12. Category: Minor
   Description:
     [163546] - Different ui redirect behavior on different pages when there is no license
   Infected Motherboard: G1SMH-G-P, G1SMH-P
   Affected functions: Configuration
   Validation:
     1) Please refere PB issue #163546
13.Category: Major
  Description:
    [164381] - CPU temperature missing when do inband warm power reset
    [162573] - CG1 CPU Temp somehow became "0"
    [164566] - CPU temp going N/A during AC ONOFF
  Infected Motherboard: G1SMH, G1SMH-G
  Affected Function: CPU Temp sensor
  Validation:
    1) Run power reset, off/on, reboot in OS
    2) Check CPU Temp sensor reading
14.Category: Major
  Description:
    [ENGINEERING] - Motherboard FRU 0 broken when AC cycle
  Infected Motherboard: X13DEH
  Affected Function: FRU 0
  Validation:
    1) AC cycle and check Motherboard FRU 0
15. Category: Major
   Description:
     [164658] - Fan speed RPM reading is incorrect
   Infected Motherboard: G1SMH, G1SMH-G, X13DEH
   Affected functions: Fan reading
   Validation:
     1) check Fan reading reach to maxium 31000~32000RPM
16. Category: Major
   Description:
     [159198] - No Sensors/Information for GPU and BF3
     [164025] - X13DEH BMC 1.00.10 has multiple sensor errors
     [164435] - ARS-111GL-NHR' has issue which ensor 'AOC_NIC1 Temp', 'AOC_NIC2 Temp' and 'AOM IO Temp' are not available during burn-in
   Infected Motherboard: G1SMH, G1SMH-G, X13DEH
   Affected functions: AOC NIC Temp sensor
   Validation:
     1) check AOC_NICx Temp sensor reading
17.Category: Major
   Description:
     [162905] - Message "BMC Transfer Error is shown during POST
   Infected Motherboard: G1SMH, G1SMH-G
   Affected Function: AC Power on
   Validation:
     1) AC power on, power button will be blocked until BMC is ready.
     2) After Power on then check Post message.
17.Category: Major
   Description:
     [ENGINEERING] - no KVM video display after system power reset
   Infected Motherboard: G1SMH, G1SMH-G
   Affected Function: KVM video display
   Validation:
     1) Power on and check KVM video normal there.
     2) Reboot BMC
     3) Login BMC and check KVM video normal there still.
     4) Power reset through BMC, KVM video display should be still normal.
18. Category: Feature
   Description:
     [ENGINEERING] - Support MGX GPU VBIOS FW update on CG1.
   Infected Motherboard: G1SMH-G.
   Affected functions: VBIOS FW update.
   Validation:
      1) Update g530_0206_888__9600840002-prod.fwpkg on through WEBUI MGX GPU (VBIOS)
      2) System power reset
      3) Check Firmware Inventory MGX GPU 96.00.84.00.02


--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: d8b137c904373cfc769cfba5612fd8066b343302

Firmware Version: 01.00.11
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231012_01.00.11_STDsp.bin
Production signed Firmware CRC: BDFB516B
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231012_01.00.11_STDsp.bin
Production signed eMMC Firmware CRC: E591A679
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20231012_01.00.11_STDsp.bin
Production signed SPI NOR Firmware CRC: 70F1FF1F
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231012_01.00.11_STDsd.bin
Debug signed Firmware CRC: BC1A90B6
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231012_01.00.11_STDsd.bin
Debug signed eMMC Firmware CRC: 9669F646
Build Date: 10/12/2023
Redfish API : Redfish_1_11_API_full_list_20230918
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1.Category: Major
  Description:
    [164130] - bmc webGUI fail to update EROT CPU
  Infected Motherboard: C2/CG1
  Affected Function: update EROT
  Validation:
    1) Update EROT firmware
2. Category: Major
   Description:
     [164029] - X13DEH Redfish DMTF Service Validator Failed
   Infected Motherboard: X13DEH
   Affected functions: Redfish
   Validation:
     1. Run Redfish DMTF Service Validator
3. Category: Major
   Description:
     [ENGINEERING]- power brake happen in AOC slots
   Infected Motherboard: G1SMH, G1SMH-G
   Validation:
     1) check if power consumption is normal when stress components
4. Category: Major
   Description:
     [ENGINEERING] - CPU temperature missing when do inband warm power reset
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: CPU temperature
   Validation:
     1) reboot in OS
     2) check CPU temperature after post complete
5. Category: Major
   Description:
     [ENGINEERING] - Re-enable security state in WEBUI
   Infected Motherboard: G1SMH, G1SMH-G
   Affected functions: security state 
   Validation:
     1) security state dependes on production signed firmware and provisioin and measurement
6. Category: Major
   Description:
     [ENGINEERING] - failed to download IPMI configuration
   Infected Motherboard: G1SMH-G-P, G1SMH-P
   Affected functions: Configuration
   Validation:
     1) IPMI configuration will be downloaded successfully


--------------------------------------------------------------------------------------------------------------------------------------


GIT SHA: e68d22ca44fe66e16c09af0a346e2558248d873b

Firmware Version: 01.00.10
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231005_01.00.10_STDsp.bin
Production signed Firmware CRC: 47B96A9F
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231005_01.00.10_STDsp.bin
Production signed eMMC Firmware CRC: A5C82DC0
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20231005_01.00.10_STDsp.bin
Production signed SPI NOR Firmware CRC: 70F1FF1F
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231005_01.00.10_STDsd.bin
Debug signed Firmware CRC: FCD2CB29
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231005_01.00.10_STDsd.bin
Debug signed eMMC Firmware CRC: 6CBA1D94
Build Date: 10/05/2023
Redfish API : Redfish_1_11_API_full_list_20230918
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1.Category: Major
  Description:
    [ENGINEERING] - BIOS Update on Reset
  Infected Motherboard: C2/CG1
  Affected Function: BIOS update o reset
  Validation:
    1) Update BIOS firmware (update time = immediate update)
    2) Update BIOS firmware (update time = next-boot update)
    3) Apply steps 1 and 2 separately to C2/CG1.
2. Category: Major
   Description:
     [ENGINEERING] - Modify Redfish privilege and licensecheck for Redfish_1_11_API_full_list_20230918 update.
   Infected Motherboard: All
   Affected functions: Redfish
   Validation:
     1. Run SATC Redfish Permission test case should pass.
3. Category: Major
   Description:
     [162942] fix - X13DEH cannot recieve all the alert message through trap/email
   Infected Motherboard: X13DEH
   Validation:
     1) Setup SMTP and alert
     2) Trigger any SEL event twice to check if event sent.
4. Category: Minor
   Description:
     [163202] - Unable to modify user account type on web ui when it reaches maximum 16 users
   Infected Motherboard: G1SMH-P
   Affected functions: Configuration
   Validation:
     1) go to Configuration-> Account Services -> Users page, add users to maximum 16
     2) Modify any user, try to add SNMP account type
5. Category: fix
   Description:
     [163367] - When enable redfish protocol alerts, alert type events can still be received even if the alert type event is not selected
   Infected Motherboard: G1SMH
   Affected functions: Redfish
   Validation:
     1) Login/Logout BMC to check Redfish event
6. Category: fix
   Description:
     [163461] - sometimes KCS Control tab still exists on web gui
   Infected Motherboard: G1SMH-G-P, G1SMH-P
   Affected functions: Configuration
   Validation:
     1) Please refere PB issue #163461
7.  Category: fix
    Description:
      [163683] - Fail to get DCMI power reading using SMCIPMITool
    Infected Motherboard: G1SMH, G1SMH-G
    Affected functions: dcmi power reading
    Validation :
      1) ipmitool -U username -P pass -H BMCIP dcmi power reading
8. Category: fix
   Description:
     [163685/162861] - last power state function is not working
   Infected Motherboard: Lego CG1 / Lego C2
   Affected functions: last power state
   Validation:
     1). ipmitool chassis policy to set power restore policy  -> checked
     2). WebGui -> Configureation -> BMC setttings -> power restore policy Tab
     3). Configure settings to last state, wait Host system to be fully powered on / powered off
     4). Ac cycle the whole system, expected to see Host system perform powerOn/Off as laststate
9. Category: fix
   Description:
     [162188] - Inband ipmitool frequently fails
   Infected Motherboard: G1SMH-G, G1SMH
   Affected functions: I2C SSIF
   Validation :
     1) Power on system and wait boot complete.
     2) Check smbios.
     3) Check post snooping via WebUI.
        Maintenance > Trobuleshooting > POST Snooping
     4) Enter BIOS Setup menu and Check BMC Network IP.
     5) Enter BIOS Setup menu and set time. Then save and reset.
        Check RTC is modified.
     6) Do inband ipmi command loop test and check response is stable than
        before.


--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 87b1b58e05aeddac0f57b34abf245b8db24c114c

Firmware Version: 01.51.04
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231005_01.51.04_STDsp.bin
Production signed Firmware CRC: B1E2DF8A
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231005_01.51.04_STDsp.bin
Production signed eMMC Firmware CRC: 14B95C1B
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20231005_01.51.04_STDsp.bin
Production signed SPI NOR Firmware CRC: 70F1FF1F
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20231005_01.51.04_STDsd.bin
Debug signed Firmware CRC: 45C88658
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20231005_01.51.04_STDsd.bin
Debug signed eMMC Firmware CRC: 928A942B
Build Date: 10/05/2023
Redfish API : Redfish_1_11_API_full_list_20230918
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1.Category: Major
  Description:
    [ENGINEERING] - BIOS Update on Reset
  Infected Motherboard: C2/CG1
  Affected Function: BIOS update o reset
  Validation:
    1) Update BIOS firmware (update time = immediate update)
    2) Update BIOS firmware (update time = next-boot update)
    3) Apply steps 1 and 2 separately to C2/CG1.
2. Category: Major
   Description:
     [ENGINEERING] - Modify Redfish privilege and licensecheck for Redfish_1_11_API_full_list_20230918 update.
   Infected Motherboard: All
   Affected functions: Redfish
   Validation:
     1. Run SATC Redfish Permission test case should pass.
3. Category: Major
   Description:
     [162942] fix - X13DEH cannot recieve all the alert message through trap/email
   Infected Motherboard: X13DEH
   Validation:
     1) Setup SMTP and alert
     2) Trigger any SEL event twice to check if event sent.
4. Category: Minor
   Description:
     [163202] - Unable to modify user account type on web ui when it reaches maximum 16 users
   Infected Motherboard: G1SMH-P
   Affected functions: Configuration
   Validation:
     1) go to Configuration-> Account Services -> Users page, add users to maximum 16
     2) Modify any user, try to add SNMP account type
5. Category: fix
   Description:
     [163367] - When enable redfish protocol alerts, alert type events can still be received even if the alert type event is not selected
   Infected Motherboard: G1SMH
   Affected functions: Redfish
   Validation:
     1) Login/Logout BMC to check Redfish event
6. Category: fix
   Description:
     [163461] - sometimes KCS Control tab still exists on web gui
   Infected Motherboard: G1SMH-G-P, G1SMH-P
   Affected functions: Configuration
   Validation:
     1) Please refere PB issue #163461
7.  Category: fix
    Description:
      [163683] - Fail to get DCMI power reading using SMCIPMITool
    Infected Motherboard: G1SMH, G1SMH-G
    Affected functions: dcmi power reading
    Validation :
      1) ipmitool -U username -P pass -H BMCIP dcmi power reading
8. Category: fix
   Description:
     [163685/162861] - last power state function is not working
   Infected Motherboard: Lego CG1 / Lego C2
   Affected functions: last power state
   Validation:
     1). ipmitool chassis policy to set power restore policy  -> checked
     2). WebGui -> Configureation -> BMC setttings -> power restore policy Tab
     3). Configure settings to last state, wait Host system to be fully powered on / powered off
     4). Ac cycle the whole system, expected to see Host system perform powerOn/Off as laststate
9. Category: fix
   Description:
     [162188] - Inband ipmitool frequently fails
   Infected Motherboard: G1SMH-G, G1SMH
   Affected functions: I2C SSIF
   Validation :
     1) Power on system and wait boot complete.
     2) Check smbios.
     3) Check post snooping via WebUI.
        Maintenance > Trobuleshooting > POST Snooping
     4) Enter BIOS Setup menu and Check BMC Network IP.
     5) Enter BIOS Setup menu and set time. Then save and reset.
        Check RTC is modified.
     6) Do inband ipmi command loop test and check response is stable than
        before.


--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 0deeaf4ca5ccf9b9b04ee546901bfa2aef35714c

Firmware Version: 01.00.09
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230920_01.00.09_STDsp.bin
Production signed Firmware CRC: 44C56995
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230920_01.00.09_STDsp.bin
Production signed eMMC Firmware CRC: 69ED4EF9
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230920_01.00.09_STDsp.bin
Production signed SPI NOR Firmware CRC: 70F1FF1F
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230920_01.00.09_STDsd.bin
Debug signed Firmware CRC: 58CB7D5C
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230920_01.00.09_STDsd.bin
Debug signed eMMC Firmware CRC: 07FACBD2
Build Date: 09/20/2023
Redfish API : Redfish_1_11_API_full_list_20230918
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: Major
    Description:
        [ENGINEERING] - Fix Systems LogService entry empty data
    Infected Motherboard: ALL
    Affected functions: Redfish/Web
    Validation:
      1) WEBUI Maintenance->Maintenance Event Log
      2) WEBUI System->Health Event Log

--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 8c62c95c9ab8299e3980ffa14de554692eada8d2

Firmware Version: 01.00.08
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230918_01.00.08_STDsp.bin
Production signed Firmware CRC: 7E315C29
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230918_01.00.08_STDsp.bin
Production signed eMMC Firmware CRC: F947B0D5
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230918_01.00.08_STDsp.bin
Production signed SPI NOR Firmware CRC: 70F1FF1F
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230918_01.00.08_STDsd.bin
Debug signed Firmware CRC: B5AAEE08
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230918_01.00.08_STDsd.bin
Debug signed eMMC Firmware CRC: 40C59316
Build Date: 09/18/2023
Redfish API : Redfish_1_11_API_full_list_20230918
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: fix
   Description:
     [ENGINEERING] - BIOS got invalid RTC time
   Infected Motherboards: G1SMH, G1SMH-G
   Affected functions: Local Date and Time
   Validation:
     1) Enter BIOS setup menu
     2) Modify BIOS time, save and exit.
     3) Enter BIOS setup menu and check BIOS time
     4) Check BMC time with Redfish API
        /redfish/v1/Managers/1
     5) AC cycle
     6) Enter BIOS setup menu and check BIOS time
     7) Check BMC time with Redfish API
        /redfish/v1/Managers/1


--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 1ebd6ecc840509c5cddfac8f88270c84e0ad8330

Firmware Version: 01.00.07
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230916_01.00.07_STDsp.bin
Production signed Firmware CRC: 96C87C6D
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230916_01.00.07_STDsp.bin
Production signed eMMC Firmware CRC: E22E44E7
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230916_01.00.07_STDsp.bin
Production signed SPI NOR Firmware CRC: 70F1FF1F
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230916_01.00.07_STDsd.bin
Debug signed Firmware CRC: 53FBD191
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230916_01.00.07_STDsd.bin
Debug signed eMMC Firmware CRC: 550478F9
Build Date: 09/16/2023
Redfish API : Redfish_1_11_API_full_list_20230410
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: Major
   Description:
     [162566] - The fan speed is 25500rpm for all fans (Optimal mode)
   Infected Motherboard: G1SMH-G
   Affected functions: fan control
   Validation:
     1) check Fan PWM control
2. Category: Major
   Description:
     [ENGINEERING] - correct BIOS version
   Infected Motherboard: G1SMH, G1SMH-G
   Affected Functions: BIOS version
   Validation:
     1) check BIOS version match image file version


--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 85c165945f3cf73109a5d8bfc617fc3837267391

Firmware Version: 01.00.06
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230915_01.00.06_STDsp.bin
Production signed Firmware CRC: 124F61FF
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230915_01.00.06_STDsp.bin
Production signed eMMC Firmware CRC: 16007261
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230915_01.00.06_STDsp.bin
Production signed SPI NOR Firmware CRC: 70F1FF1F
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230915_01.00.06_STDsd.bin
Debug signed Firmware CRC: 7E8E132C
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230915_01.00.06_STDsd.bin
Debug signed eMMC Firmware CRC: 08D89150
Build Date: 09/15/2023
Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: Major
   Description:
     [ENGINEERING] - BMC Temp is missing
   Infected Function: X13DEH
   Affected Function: sensor
   Validation:
     1) check BMC Temp reading is there
2. Category: Major
   Description:
     [ENGINEERING] - VRM i2c protection
   Infected Motherboard: X13DEH
   Affected Functions: ROT
   Validation:
     1) mount JPFR2 to lower VRM protect.
3. Category: Major
   Description:
     [ENGINEERING] - NVME BPN is missing in UI.
   Infected Motherboard: X13DEH
   Affected functions: storage
   Validation:
     1. check NVME BPN there in UI

--------------------------------------------------------------------------------------------------------------------------------------


GIT SHA: 910a8a3539dff4557f2602f243efea175a2d406b

Firmware Version: 01.00.05
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230912_01.00.05_STDsp.bin
Production signed Firmware CRC: 4855DEC1
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230912_01.00.05_STDsp.bin
Production signed eMMC Firmware CRC: F36F4DAA
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230912_01.00.05_STDsp.bin
Production signed SPI NOR Firmware CRC: 70F1FF1F
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230912_01.00.05_STDsd.bin
Debug signed Firmware CRC: CAAA4631
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230912_01.00.05_STDsd.bin
Debug signed eMMC Firmware CRC: 038944B8
Build Date: 09/12/2023
Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: Major
   Description:
     [161986] - Fan duty show NA
   Infected Function: X13DEH, G1SMH, G1SMH-G
   Affected Function: Fan control
   Validation:
     1) Verify Fan Control
2. Category: Minor
   Description:
     [ENGINEERING] - remove VBAT monitoring
   Infected Motherboard: G1SMH, G1SMH-G
   Affected Functions: VBAT
   Validation:
     1) no VBAT sensor
3. Category: feature
   Description:
     [162462] - FRU information shows up in the command line, but not on the GUI
   Infected Motherboard: All
   Affected functions: FRU
   Validation:
     1. Check FRU in WEBUI

--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 2a7008bee82f82968dd1993a7d880b66d7df5733

Firmware Version: 01.00.04
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230908_01.00.04_STDsp.bin
Production signed Firmware CRC: 9AD9379E
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230908_01.00.04_STDsp.bin
Production signed eMMC Firmware CRC: F0DFDFA6
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230908_01.00.04_STDsp.bin
Production signed SPI NOR Firmware CRC: 70F1FF1F
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230908_01.00.04_STDsd.bin
Debug signed Firmware CRC: 6E4DE71F
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230908_01.00.04_STDsd.bin
Debug signed eMMC Firmware CRC: 76529EC5
Build Date: 09/08/2023
Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: Major
   Description:
     [161986] - Fan duty show NA
   Infected Function: X13DEH, G1SMH, G1SMH-G
   Affected Function: Fan control
   Validation:
     1) Verify Fan Control
2. Category: Major
   Description:
     [ENGINEERING] - support Multnode system
   Infected Motherboard: G1SMH, G1SMH-G
   Affected Functions: Multinode
   Validation:
     1) Install AOM-IO-GP102 and cable Multinode
     2) Check Multinode information
3. Category: feature
   Description:
     [ENGINEERING] - Feature support LDAP StartTLS
   Infected Motherboard: All
   Affected functions: Redfish/Web
   Validation:
     1. Login with LDAP account with StartTLS can login successfully

--------------------------------------------------------------------------------------------------------------------------------------


GIT SHA: cce89a2370cf4744513ef0d4fa9955e178bd7d7a

Firmware Version: 01.00.03
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230831_01.00.03_STDsp.bin
Production signed Firmware CRC: 35751E71
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230831_01.00.03_STDsp.bin
Production signed eMMC Firmware CRC: 3DE2FF89
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230831_01.00.03_STDsp.bin
Production signed SPI NOR Firmware CRC: 70F1FF1F
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230831_01.00.03_STDsd.bin
Debug signed Firmware CRC: 14222709
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230831_01.00.03_STDsd.bin
Debug signed eMMC Firmware CRC: 6EAC5713
Build Date: 08/31/2023
Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: Major
   Description:
     [159335] - took too long per cycle for AC test. almost 1 hour per cycle
     Infected Function: X13DEH, G1SMH, G1SMH-G
     Affected Function: SEL
   Validation:
     1) Run AC-ON/Off test to verify this issue.
2. Category: Major
   Description:
     [ENGINEERING] - Resolving VGA Loss Following BMC Reset
   Infected Motherboard: G1SMH, G1SMH-G
   Affected Functions: VGA
   Validation:
     1) Launch IKVM via web and SOL using ipmitool (e.g., ipmitool sol activate).
     2) Perform a power cycle in IKVM, anticipating UEFI shell visibility in both interfaces.
     3) Initiate a power reset in IKVM, looking for UEFI shell display in both interfaces.
3. Category: Major
   Description:
     [ENGINEERING] - BMC should block wrong FPGA firmware updating.
     Infected Motherboards: G1SMH, G1SMH-G
   Validation:
     1) Update FPGA on G1SMH or G1SMH-G via Web.
     2) Should accept only G1SMH or G1SMH-G related FPGA FW, respectively.
4. Category: Major
   Description:
     [ENGINEERING] - network drop issue during BMC cold reset test
   Infected Motherboard: G1SMH, G1SMH-G, X13DEH
   Affected Functions: BMC network
   Validation:
     1) Stress BMC cold reset test


--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: c4e9a8d3e2dcbe9cd4469be92cb5900226aea2fe

Firmware Version: 01.00.02
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230826_01.00.02_STDsp.bin
Production signed Firmware CRC: AB8CAEDF
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230826_01.00.02_STDsp.bin
Production signed eMMC Firmware CRC: 4B9FDCD9
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230826_01.00.02_STDsp.bin
Production signed SPI NOR Firmware CRC: 70F1FF1F
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230826_01.00.02_STDsd.bin
Debug signed Firmware CRC: 32D4F9AB
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230826_01.00.02_STDsd.bin
Debug signed eMMC Firmware CRC: A0DE1A4F
Build Date: 08/26/2023
Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: Critical issue
    Description:
      [ENGINEERING] - provision make BMC dead
    Infected Motherboard: G1SMH, G1SMH-G, X13DEH
    Affected Functions: provision
    Validation:
      1) BMC provision
2. Category: Fix
    Description:
    [158039] - BIOS RoT info missing in FW inventory page
    Add new Nvidia FW inventory for Lego C2 + Web PFR actions
   Infected Motherboards: G1SMH
   Validation:
     1) Check Web GUI FW management --> FW Inventory page for BIOS, CPU_EROT, and FPGA RoT FW inventory info.
     2) Perform PFR actions update BIOS, CPU_EROT, FPGA update golden.
     3) PFR action recovery for BIOS + CPU_EROT.
3. Category: major issue
    Description:
      [ENGINEERING] - read EROT version from image after EROT firmware upload
    Infected Motherboard: G1SMH, G1SMH-G
    Affected Functions: EROT firmware update
    Validation:
      1) EROT firmware update
4. Category: major issue
    Description:
      [ENGINEERING] - read FPGA version from image after FPGA firmware upload
    Infected Motherboard: G1SMH, G1SMH-G
    Affected Functions: FPGA firmware update
    Validation:
      1) FPGA firmware update

--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 9d65f6488aed300b36102a686584b646ea770473

Firmware Version: 01.00.01
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230822_01.00.01_STDsp.bin
Production signed Firmware CRC: 98396E3F
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230822_01.00.01_STDsp.bin
Production signed eMMC Firmware CRC: 98A81097
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230822_01.00.01_STDsp.bin
Production signed SPI NOR Firmware CRC: 6981C24C
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230822_01.00.01_STDsd.bin
Debug signed Firmware CRC: 8B96EA23
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230822_01.00.01_STDsd.bin
Debug signed eMMC Firmware CRC: F91E0569
Build Date: 08/22/2023
Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: fix
   Description:
     [161061] - The fan is running at full speed with all fan modes
   Infected Motherboard: G1SMH, G1SMH-G
   Affected Functions: Thermal
   Validation:
     1) Check fan speed become normal behavior.

--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 4055b3cf7ee5cdf4053d97e354b081f3fadee869

Firmware Version: 01.00.00
Production signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230818_01.00.00_STDsp.bin
Production signed Firmware CRC: 023FC4F8
Production signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230818_01.00.00_STDsp.bin
Production signed eMMC Firmware CRC: D0207633
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230818_01.00.00_STDsp.bin
Production signed SPI NOR Firmware CRC: 6981C24C
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230818_01.00.00_STDsd.bin
Debug signed Firmware CRC: 7685B297
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230818_01.00.00_STDsd.bin
Debug signed eMMC Firmware CRC: D68391BE
Build Date: 08/18/2023
Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: New
   Description:
     [Engineering] - add BF3 support
   Infected Motherboard: G1SMH, G1SMH-G, X13DEH
   Affected Functions: Thermal
   Validation:
     1) Check AOC_NICx temperature reading.
2. Category: Feature
   Description:
     [ENGINEERING] - Add Redfish APIs for Erot Certificate
   Infected Motherboard: G1SMH/G1SMH-G
   Affected Functions: Redfish
   Validation:
     1) Get following Redfish URL and check the Erot Certificate:
     2) Redfish/v1/Chassis/ERoT_CPU_X/Certificates
     3) Redfish/v1/Chassis/ERoT_CPU_X/Certificates/CertChain
     4) Redfish/v1/Chassis/ERoT_GPU_0/Certificates
     5) Redfish/v1/Chassis/ERoT_GPU_0/Certificates/CertChain
3. Category: Feature
   Description:
     [ENGINEERING] - Add Redish APIs of GPU in the processor module for CG1
   Infected Motherboard: G1SMH_G
   Affected Functions: Redfish
   Validation:
     1) Get following Redfish URL and check the result:
     2) Redfish/v1/Systems/1/Processors/GPU_0
4. Category: Fix
   Description:
     [ENGINEERING] - storage page missing if NVME BPN installed
   Infected Motherboard: G1SMH/G1SMH-G
   Affected Functions: BPN
   Validation:
     1) Storage WEB page is there if NVME BPN installed.
5. Category: Fix
   Description:
     [ENGINEERING] - BIOS update percentage more precise
   Infected Motherboard: G1SMH/G1SMH-G
   Affected Functions: BIOS update
   Validation:
     1) Update BIOS to see percentage.
6. Category: Fix
   Description:
     [X13DEH] - Update SDR for system temperature
   Infected Motherboard: X13DEH
   Affected Functions:: 
     Validation :
     1) Login WebUI >> Sensor Readings
     2) It should display "Inlet Temp, System Temp, Peripheral Temp, P1 Rear Temp, P2 Rear Temp"
7. Category: fix
   Description:
     [160542] - Console Capture Video Download button missing
   Infected Motherboard: X13DEH-P
   Affected functions: Configuration
   Validation:
     1) Log in GUI -> Maintenance -> Troubleshooting -> Console Capture
     2) Turn on Enable, then reset the SUT to let it record the video


--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 3eba1ad585da5470c7d0e0492cb32f47238c18c3

Firmware Version: 00.00.16
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230811_00.00.16_STDsp.bin
Production signed SPI NOR Firmware CRC: 6981C24C
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230811_00.00.16_STDsd.bin
Debug signed Firmware CRC: B7DEEF68
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230811_00.00.16_STDsd.bin
Debug signed eMMC Firmware CRC: 370FDAC7
Build Date: 08/11/2023
Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: AOM-SCM-NV, X13DEH, G1SMH, G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: Feature
   Description:
     [ENGINEERING] - Add APIs for Redfish to monitor processor sensors
   Infected Motherboard: G1SMH
   Affected Functions: Redfish
   Validation:
     1) Get following Redfish URLs and check the result:
     2) Redfish/v1/Chassis/ProcessorModule_0/Sensors/ProcessorModule_0_CPU_x_CoreUtil_xx
     3) Redfish/v1/Chassis/ProcessorModule_0/Sensors/ProcessorModule_0_CPU_x_Energy_0
     4) Redfish/v1/Chassis/ProcessorModule_0/Sensors/ProcessorModule_0_Energy_0
     5) Redfish/v1/Chassis/ProcessorModule_0/Sensors/ProcessorModule_0_CPU_x_CpuFreq_0
     6) Redfish/v1/Chassis/ProcessorModule_0/Sensors/ProcessorModule_0_MemCntl_x_Freq_0
     7) Redfish/v1/Chassis/ProcessorModule_0/Sensors/ProcessorModule_0_CPU_x_Power_0
     8) Redfish/v1/Chassis/ProcessorModule_0/Sensors/ProcessorModule_0_Power_0
     9) Redfish/v1/Chassis/ProcessorModule_0/Sensors/ProcessorModule_0_Vreg_x_CpuPower_0
     10) Redfish/v1/Chassis/ProcessorModule_0/Sensors/ProcessorModule_0_CPU_x_TempAvg_0
     11) Redfish/v1/Chassis/ProcessorModule_0/Sensors/ProcessorModule_0_CPU_x_TempLimit_0
     12) Redfish/v1/Chassis/ProcessorModule_0/Sensors/ProcessorModule_0_Vreg_x_CpuVoltage_0
     13) Redfish/v1/Chassis/ProcessorModule_0/Sensors/ProcessorModule_0_Vreg_x_SocVoltage_0
2. Category: Fix
   Description:
     [160191] - [DVT] GPU information missing on IPMI Web GUI
   Infected Motherboard: X13DEH
     Affected Function: GPU info
   Validation:
     1) Install one GPU to check GPU info page
3. Category: Feature
   Description:
     [ENGINEERING] - Add ERot_GPU version
   Infected Motherboard: G1SMH_G
   Affected Functions: Redfish
   Validation:
     1) Get /redfish/v1/UpdateService/FirmwareInventory/
     2) Get /redfish/v1/UpdateService/FirmwareInventory/ERoT_GPU_1
     3) Check web
4. Category: Feature
   Description:
     [ENGINEERING] - Add ERot_CPU update
   Infected Motherboard: G1SMH
   Affected Functions: ERoT_CPU update
   Validation:
     1) Web update ERoT_CPU FW
     2) Post /redfish/v1/UpdateService/upload
     3) UpdateParameters: {"Targets":["/redfish/v1/UpdateService/FirmwareInventory/ERoT_CPU_1"],"@Redfish.OperationApplyTime":"OnStartUpdateRequest"}
     4) Post /redfish/v1/UpdateService/Actions/UpdateService.StartUpdate
5. Category: Fix
   Description:
     [ENGINEERING] - Update SDR for system temperature
   Infected Motherboard: X13DEH
   Affected Functions:: 
     Validation :
     1) Login WebUI >> Sensor Readings
     2) It should display "Inlet Temp, System Temp, Peripheral Temp, P1 Rear Temp, P2 Rear Temp"
6. Category: Fix
   Description:
     [160202] - Storage Monitoring Tab Under System behavior is incorrect
   Infected Motherboard: X13DEH-P
   Affected Functions: Configuration
   Validation:
     1) Storage Monitoring Tab Under System behavior is there if storage controller detected.
7. Category: Fix
   Description:
     [ENGINEERING] - network drop issue during BMC cold reset test
   Infected Motherboard: G1SMH, G1SMH-G, X13DEH
   Affected Functions: BMC network
   Validation:
     1) stress BMC cold reset test
8. Category: Fix
   Description:
     [ENGINEERING] - BIOS updated but system cannot boot successfully
   Infected Motherboard: G1SMH, G1SMH-G
   Affected Functions: BIOS update
   Validation:
     1) verify BIOS update and power on wait for 4min at least.

--------------------------------------------------------------------------------------------------------------------------------------


GIT SHA: d00734f7993609722693d05c362ad22cf5eb875e

Firmware Version: 00.00.15
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230801_00.00.15_STDsp.bin
Production signed SPI NOR Firmware CRC: 6981C24C
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230801_00.00.15_STDsd.bin
Debug signed Firmware CRC: B57D3FE3
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230801_00.00.15_STDsd.bin
Debug signed eMMC Firmware CRC: 981752FA
Build Date: 08/01/2023
Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: AOM-SCM-NV, G1SMH, X13DEH G1SMH-G
---------------------------------------------------------------------------------------------------------


1. Category: Fix
    Description:
      [159346] - G1SMH didn't display bios info via WEB GUI. also the system couldn't boot up with 0.00.14 IPMI
      [157358] - BIOS and CPLD info is not available on WebGUI
    Infected Motherboard: G1SMH
    Affected Functions: BIOS version
    Validation:
      1) Check BIOS version and build date
2. Category: Fix
    Description:
      [157437] - IPMI power control_Graceful Shutdown is not working
    Infected Motherboard: G1SMH
    Affected Functions: power control
    Validation:
      1) Do gracefull shutdown
3. Category: Fix
    Description:
      [ENGINEERING] - support CG1 GPU tempeature reading
    Infected Motherboard: G1SMH-G
    Affected Functions: CG1 GPU
    Validation:
      1) Check CG1 GPU Temp
4. Category: Fix
    Description:
      [ENGINEERING] - VGA screen dead after reboot through server OS or UEFI shell
    Infected Motherboard: G1SMH
    Affected Functions: VGA
    Validation:
      1) VGA still alive after reboot through server OS or UEFI shell
5. Category: feature
   Description:
     [ENGINEERING] - Add ERoT URL to the Redfish
   Infected Motherboard: G1SMH
   Affected functions: Redfish, Web
   Validation:
     1) Check FirmwareInventory Collection for ERoT
      Get redfish/v1/UpdateService/FirmwareInventory
     2) Check ERoT URL
      Get redfish/v1/UpdateService/FirmwareInventory/ERoT_CPU_1
      Get redfish/v1/UpdateService/FirmwareInventory/ERoT_CPU_2


--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 31c963c57e69bf17096ee818a5aa1acbf75095ac

Firmware Version: 00.00.14
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230712_00.00.14_STDsp.bin
Production signed SPI NOR Firmware CRC: 6981C24C
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230712_00.00.14_STDsd.bin
Debug signed Firmware CRC: 495B9468
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230712_00.00.14_STDsd.bin
Debug signed eMMC Firmware CRC: A70CC2C3
Build Date: 07/12/2023
Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: AOM-SCM-NV, G1SMH, X13DEH 
---------------------------------------------------------------------------------------------------------


1. Category: Fix
    Description:
      [ENGINEERING] - Read/Write FRU0 data
    Infected Motherboard: G1SMH, G1SMH, X13DEH
    Affected Functions: FRU
    Validation:
      1) Write FRU data via OOB command.
      2) Read FRU data via OOB command.
      3) Check the FRU data is correct.
      4) Revmoe the FRU files, and then reboot BMC.
      5) Check the FRU data is correct.
2. Category: Enhancment
    Description:
      [ENGINEERING] - support G1SMH-G
    Infected Motherboard: G1SMH-G
    Affected Functions: BIOS FW update.
    Validation:
      1) Update CPLD to the version 07 and above
      2) Update EROT FW
      3) Check BMC related
3. Category: Fix
    Description:
      [ENGINEERING] - Support backplane CPLD update function
    Infected Motherboard: X13DEH
    Affected Functions: :
      Validation :
      1) Login WebUI >> Maintenance >> Firmware Management >> Update
      2) It should display backplane CPLD select item
      3) Update backplane CPLD image
      4) It should update successfully
4. Category: Fix
   Description:
     [ENGINEERING] - Fix IO board version not present
   Infected Motherboard: G1SMH, G1SMH_G, X13DEH
   Affected functions: Redfish
   Validation:
      1) Get /redfish/v1/UpdateService/FirmwareInventory/CPLD_IOboard1/UpdateService/FirmwareInventory/CPLD_IOboard


--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 722f5637541900e4d587d0d723608d85d7b0e020

Firmware Version: 00.00.13
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230624_00.00.13_STDsp.bin
Production signed SPI NOR Firmware CRC: 6981C24C
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230624_00.00.13_STDsd.bin
Debug signed Firmware CRC: 0481BF41
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230624_00.00.13_STDsd.bin
Debug signed eMMC Firmware CRC: 88682772
Build Date: 06/24/2023
Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: G1SMH, X13DEH 
---------------------------------------------------------------------------------------------------------


1. Category: Fix
   Description:
     [157741] - Sensor readings are all N/A after rebooting the system
   Infected Motherboard: G1SMH
   Affected Functions: sensor
   Validation:
     1) check sensor reading

2. Category: Fix
   Description:
     [157814] - Fan speed doesn't change when the fan failed.
     [ENGINEERING] - total 9 FAN instead of 12 FAN
   Infected Motherboard: G1SMH
   Affected Functions: fan
   Validation:
     1) check fan speed


--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 85fd78be47995b1ebe106d071abb98838c4b962d

Firmware Version: 00.00.12
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230622_00.00.12_STDsp.bin
Production signed SPI NOR Firmware CRC: 6981C24C
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230622_00.00.12_STDsd.bin
Debug signed Firmware CRC: 9AACFB1B
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230622_00.00.12_STDsd.bin
Debug signed eMMC Firmware CRC: F11BA009
Build Date: 06/22/2023
Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: G1SMH, X13DEH 
---------------------------------------------------------------------------------------------------------


1. Category: Fix
   Description:
     [ENGINEERING] - Support G1SMH-G
   Infected Motherboard: G1SMH-G
   Affected Functions: N/A
   Validation:
     1) N/A
2. Category: Fix
   Description:
     [ENGINEERING] - Support IOboard CPLD firmware inventory and firmware update
   Infected Motherboard: All
   Affected Functions: IO Board update
   Validation:
     1) verify IO Board update
3. Category: new
   Description:
     [ENGINEERING] - new dark theme WEBUI style
   Infected Motherboard: All
   Affected Functions: WEBUI
   Validation:
     1) check WEBUI style
4.  Category: fix
    Description:
      [ENGINEERING] Update fan zone info
    Infected Motherboard: X13DEH
    Affected functions:
    Validation :
      1) Stress CPU
      2) Fan control should run correctly
5.  Category: new
    Description:
      [ENGINEERING] C2 error event log
    Infected Motherboard: G1SMH
    Affected functions:
    Validation :
      1) N/A
6.  Category: enhancement
    Description:
      [ENGINEERING] - enhancement power on/off/reset and mctp discovery
    Infected Motherboard: G1SMH
    Affected functions:
    Validation :
      1) N/A

--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: 043efa4b014ec5c313f143432f6dfb7588fb1db4

Firmware Version: 00.00.11
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230620_00.00.11_STDsp.bin
Production signed SPI NOR Firmware CRC: 6981C24C
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230620_00.00.11_STDsd.bin
Debug signed Firmware CRC: 68AFC448
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230620_00.00.11_STDsd.bin
Debug signed eMMC Firmware CRC: D56DBDB7
Build Date: 06/20/2023
Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: G1SMH, X13DEH 
---------------------------------------------------------------------------------------------------------


1. Category: Fix
   Description:
     [ENGINEERING] - power on fail somehow because of protection feature enable
   Infected Motherboard: G1SMH
   Affected Functions: power on
   Validation:
     1) system power on
2. Category: Fix
   Description:
     [ENGINEERING] - enhance the BIOS update
   Infected Motherboard: G1SMH
   Affected Functions: BIOS update
   Validation:
     1) verify BIOS update
3. Category: Fix
   Description:
     [ENGINEERING] - sensor missing
   Infected Motherboard: G1SMH
   Affected Functions: Sensor
   Validation:
     1)  monitor sensors
4. Category: Fix
   Description:
     [ENGINEERING] - BMC network IP is gone somehow
   Infected Motherboard: G1SMH
   Affected Functions: BMC network IP
   Validation:
     1) stress BMC reboot or system power on/off
5. Category: Fix
   Description:
     [ENGINEERING] - CPLD update failure
   Infected Motherboard:X13DEH
   Affected Functions: CPLD update
   Validation:
     1) update CPLD and CPLD Misc

--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: fd60150e1daea24dcc08944c2177c0bcea4de79f

Firmware Version: 00.00.10
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230612_00.00.10_STDsp.bin
Production signed SPI NOR Firmware CRC: 6981C24C
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230612_00.00.10_STDsd.bin
Debug signed Firmware CRC: 98CE415A
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230612_00.00.10_STDsd.bin
Debug signed eMMC Firmware CRC: 93D6FA35
Build Date: 06/12/2023
Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: G1SMH, X13DEH 
---------------------------------------------------------------------------------------------------------


1. Category: Fix
   Description:
     [ENGINEERING] - power on fail somehow because of protection feature enable
   Infected Motherboard: G1SMH
   Affected Functions: power on
   Validation:
     1) system power on
2. Category: Fix
   Description:
     [ENGINEERING] - enhance the BIOS update
   Infected Motherboard: G1SMH
   Affected Functions: BIOS update
   Validation:
     1) verify BIOS update
3. Category: Fix
   Description:
     [ENGINEERING] - processor monitoring function in redfish
   Infected Motherboard: G1SMH
   Affected Functions: Sensor
   Validation:
     1)  monitor cpu rail power, cpu soc rail power, cpu grace power throuh redfish

--------------------------------------------------------------------------------------------------------------------------------------

GIT SHA: d7adde1478a889b9e8c1e50d8b1141e67fa60a88

Firmware Version: 00.00.09
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230602_00.00.09_STDsp.bin
Production signed SPI NOR Firmware CRC: 6981C24C
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230602_00.00.09_STDsd.bin
Debug signed Firmware CRC: DDF30CC1
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230602_00.00.09_STDsd.bin
Debug signed eMMC Firmware CRC: CF44E738
Build Date: 06/02/2023
Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: G1SMH, X13DEH 
---------------------------------------------------------------------------------------------------------


1. Category: Fix
   Description:
     [ENGINEERING] - system happen reboot when BMC reboot
   Infected Motherboard: G1SMH
   Affected Functions: BMC reboot
   Validation:
     1) System will not happen reboot when BMC reboot
2. Category: Fix
   Description:
     [ENGINEERING] - system cannot be detected correctyly and cannot power on when BMC Moodule switch between C2 and X86
   Infected Motherboard: G1SMH, H13DEH
   Affected Functions: System power on
   Validation:
     1) Check sensor list to confirm system can be detected correcty when BMC Moodule swap between C2 and X86
     2) Power on system when BMC Moodule swap between C2 and X86
3. Category: Fix
   Description:
     [ENGINEERING] - add FPGA and C2 module thermal sensor
   Infected Motherboard: G1SMH
   Affected Functions: Sensor
   Validation:
     1) Using BIOS_G1SMH-1D10_20230525_0.1_TES.bin
     2) Check sensor reading
4. Category: Fix
   Description:
     [ENGINEERING] - BIOS version and EROT version availabe in WEBUI and Redfish
   Infected Motherboard: G1SMH
   Affected Functions: Firmware inventory
   Validation:
     1) Using BIOS_G1SMH-1D10_20230525_0.1_TES.bin
     2) Check firmware inventory
5. Category: Fix
   Description:
     [ENGINEERING] - motherboard FRU available
   Infected Motherboard: G1SMH, H13DEH
   Affected Functions: FRU
   Validation:
     1) ipmicfg to read/write FRU

6. Category: Fix
   Description:
     [ENGINEERING] - C2 FRU available
   Infected Motherboard: G1SMH
   Affected Functions: FRU
   Validation:
     1) ipmitool fru print 2

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 00.00.08
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230518_00.00.08_STDsp.bin
Production signed SPI NOR Firmware CRC: 530B8EA4
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230518_00.00.08_STDsd.bin
Debug signed Firmware CRC: 7D8961EE
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230518_00.00.08_STDsd.bin
Debug signed eMMC Firmware CRC: 6BD5EDF3
Build Date: 05/18/2023
GIT SHA: dd7fbb268e8ba649b68021ff0674bf68adae2395
Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: G1SMH, X13DEH 
---------------------------------------------------------------------------------------------------------


1. Category: New
   Description:
     [ENGINEERING] - FPGA update availabe on Redfish/WEBUI
     [ENGINEERING] - FPGA firmware version in firmware inventory
   Infected Motherboard: G1SMH
   Affected Functions: FPGA update
   Validation:
     1) FPGA firmware update
     2) Check FPGA firmware inventory
2. Category: Fix
   Description:
     [ENGINEERING] - failed to update BIOS/EROT when system power on
     [ENGINEERING] - BIOS/EROT firmware version in firmware inventory
   Infected Motherboard: G1SMH
   Affected Functions: BIOS/EROT update
   Validation:
     1) BIOS/EROT firmware update
     2) Check BIOS/EROT firmware inventory
3. Category: Fix
   Description:
     [ENGINEERING] - add FPGA and C2 module thermal sensor
   Infected Motherboard: G1SMH
   Affected Functions: Thermal
   Validation:
     1) Need FPGA firmware 0.5A and BIOS support post complete then verify it.
4. Category: Fix
   Description:
     [ENGINEERING] - support both Fiber mode and SGMII mode.
   Infected Motherboard: G1SMH
   Affected Functions: BMC Dedicated LAN
   Validation:
     1) Only work with 1G network


--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 00.00.07
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230503_00.00.07_STDsp.bin
Production signed SPI NOR Firmware CRC: 2FA89191
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230503_00.00.07_STDsd.bin
Debug signed Firmware CRC: BBCD8B72
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230503_00.00.07_STDsd.bin
Debug signed eMMC Firmware CRC: A7FDAAD4
Build Date: 05/03/2023
Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: G1SMH, X13DEH 
---------------------------------------------------------------------------------------------------------


1.  Category: fix
    Description:
      [ENGINEERING] – BIOS update failed
    Infected Motherboard: G1SMH
    Affected functions:
    Validation :
      1) update BIOS through BMC WEBUI

2.  Category: fix
    Description:
      [ENGINEERING] - make physical power button works
    Infected Motherboard: G1SMH
    Affected functions: power control button
    Validation :
      1) used physical power button to power on/off/softshutdown and check MEL

3.  Category: fix
    Description:
      [ENGINEERING] - make physical UID button works
    Infected Motherboard: G1SMH
    Affected functions: UID control button
    Validation :
      1) used physical UID button to turn on/off UID and check MEL

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 00.00.06
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230421_00.00.06_STDsp.bin
Production signed SPI NOR Firmware CRC: 2FA89191
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230421_00.00.06_STDsd.bin
Debug signed Firmware CRC: 58811C9A
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230421_00.00.06_STDsd.bin
Debug signed eMMC Firmware CRC: 43B5C465
Build Date: 04/21/2023
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: G1SMH, X13DEH 
---------------------------------------------------------------------------------------------------------


1.  Category: fix
    Description:
      [ENGINEERING] – OEM set fan control command failed
    Infected Motherboard: X13DEH, G1SMH
    Affected functions:
    Validation :
      1) BMC set fan control bypass enable
         ipmitool raw 0x30 0x70 0x66 0x02 0x01
      2) BMC get thermal zone 0~2 fan duty
         ipmitool raw 0x30 0x70 0x66 0x00 <0x00~0x02>
      3) BMC set thermal zone 0~2 fan duty
         ipmitool raw 0x30 0x70 0x66 0x01 <0x00~0x02> <0-100>
      4) The fan speed should be correct after setting PWM command

2.  Category: fix
    Description:
      [ENGINEERING] - It failed to update BIOS before user did BMC reboot manually.
    Infected Motherboard: G1SMH
    Affected functions: BIOS update
    Validation :
      1) updating BIOS should be successful.

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 00.00.05
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230417_00.00.05_STDsp.bin
Production signed SPI NOR Firmware CRC: 2FA89191
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230417_00.00.05_STDsd.bin
Debug signed Firmware CRC: 384EC712
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230417_00.00.05_STDsd.bin
Debug signed eMMC Firmware CRC: 2CCEA20C
Build Date: 04/17/2023
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: G1SMH, X13DEH 
---------------------------------------------------------------------------------------------------------


1. local date and time configuation.
2. G1SMH BIOS Update.
3. X13DEH PSU info.
4. X13DEH BIOS update.
5. X13DEH CPLD update.

--------------------------------------------------------------------------------------------------------------------------------------

Firmware Version: 00.00.04
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230326_00.00.04_STDsp.bin
Production signed SPI NOR Firmware CRC: B174DACB
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230326_00.00.04_STDsd.bin
Debug signed Firmware CRC: 1E20223F
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230326_00.00.04_STDsd.bin
Debug signed eMMC Firmware CRC: 51C3383B
Build Date: 03/26/2023
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported Platform: G1SMH, X13DEH 
---------------------------------------------------------------------------------------------------------


1. Most sensors(Temperature, Voltage, Fan) are ready in G1SMH and X13DEH.
2. FAN control is there.
3. Remote control UID ON/OFF.
4. Push local UID to do BMC reset cold.
5. Push local UID to do BMC reset default.
6. Update Motherboard Miscellenous CPLD(CPLD2).
7. Display BIOS post progress code.
8. Use POST code for G1SMH post complete.
9. Remote USB mount, Keyboard and mouse need hardware rework.

--------------------------------------------------------------------------------------------------------------------------------------


Firmware Version: 00.00.03
Production signed SPI NOR Firmware Name: BMC_SCMAST2600-ROT20-2501MS-NOR_20230309_00.00.03_STDsp.bin
Production signed SPI NOR Firmware CRC: B174DACB
Debug signed Firmware Name: BMC_SCMAST2600-ROT20-2501MS_20230309_00.00.03_STDsd.bin
Debug signed Firmware CRC: 3270F116
Debug signed eMMC Firmware Name: BMC_SCMAST2600-ROT20-2501MS-eMMC_20230309_00.00.03_STDsd.bin
Debug signed eMMC Firmware CRC: 8AF1519D
Build Date: 03/09/2023
Redfish API : Redfish API : X12_Redfish_1_90_API_full_list_11032021
ROT AntiRollback ID: 0001h
Supported Platform: G1SMH, X13DEH
---------------------------------------------------------------------------------------------------------

1. BMC to power on and off C2
2. Enable Display Port (DP)
3. Support SOL
4. Support C2 FPGA MCTP over PCIE

--------------------------------------------------------------------------------------------------------------------------------------
