==============================================================================================================================
Filename: BMC_H13AST2600-ROT-1401MS_20240301_01.02.01_STDsp.bin version: 01.02.01 Date: 01 Mar 2024
U-Boot baseline : 2019.04
Java SOL Viewer version : v0.5.16
Java iKVM Viewer version : v1.69.54
Redfish API : Redfish_1_11_API_full_list_20231218
spl: 02.03.39
tee.bin: 0100.03.78
antiRBID: 0x0001
Supported MBs: H13SST-G, H13SST-GC, H13SSL-N, H13SSL-NT, H13DSG-O-CPU, H13SSW, H13DSH, H13SVW-N, H13SVW-NT
Signed key: new X13 ROT key

1.
    Category: Fix
    Description:
        BIOS stops at POST code A2 when using BMC 1.2.0
    Impact motherboard:
        H13SSL-N, H13SSL-NT, H13SSW, H13DSH, H13SVW-N, H13SVW-NT
    Affected functions:
    Validation:
        1. Run AC ON/OFF test
        2. Check whether the system starts normally

2.
    Category: Fix
    Description:
        [171605] ECO — 21603 — 01.02.00(2024/01/30) — [Function] — The AutoDST switch button should be disable when timezone is (UTC+02:00) Damascus
    Impact motherboard:
        H13DSG-O-CPU
    Affected functions:
    Validation:
        1. Go to Configuration - BMC Setting - Date and Time page
        2. Set Time Zone to (UTC+02:00) Damascus, and Save
        3. Check the 'Auto Daylight Savings Time' status

Protection maps:
    H13DSG_O    BitMap-20231113-170745.bin
    H13DSH      BitMap-20221128-184047-MPS.bin
    H13SSL_N    BitMap-20221128-184047-MPS.bin
    H13SST_G    BitMap-20221128-184047-MPS.bin
    H13SSW      BitMap-20221128-184047-MPS.bin
    H13SVW_N    BitMap-20221128-184047-MPS.bin

==============================================================================================================================
Filename: BMC_H13AST2600-ROT-1401MS_20240130_01.02.00_STDsp.bin version: 01.02.00 Date: 30 Jan 2024
U-Boot baseline : 2019.04
Java SOL Viewer version : v0.5.16
Java iKVM Viewer version : v1.69.53
Redfish API : Redfish_1_11_API_full_list_20231218
spl: 02.03.39
tee.bin: 0100.03.77
antiRBID: 0x0001
Supported MBs: H13SST-G, H13SST-GC, H13SSL-N, H13SSL-NT, H13DSG-O-CPU, H13SSW, H13DSH, H13SVW-N, H13SVW-NT
Signed key: new X13 ROT key

1.
    Category: Fix
    Description:
        Fix CVE-2023-4879 Terrapin Attack
    Impact motherboard:
        All X13/H13 ROT2-HW2 MBs
    Affected functions:
        ssh service
    Validation:
        1. Perform vulnerability scan using nmap for ssh2-enum-algos

2.
    Category: Fix
    Description:
        (CVE-2023-48795) SMC-2024010013 Terrapin Attack vulnerability
        SMC-2024010010 Command Injection attack
        SMC-2024010011 XSS attack
    Impact motherboard:
        All X13/H13 ROT2-HW2 MBs
    Affected functions:
    Validation:
        1. Please contact Glen's team to do the validation

3.
    Category: Fix
    Description:
        (CVE-2023-33413) SMC-2024010012 Command Injection attack
    Impact motherboard:
        All X13/H13 ROT2-HW2 MBs
    Affected functions:
    Validation:
        1. Please contact Glen's team to do the validation

4.
    Category: Fix
    Description:
        Fix(CPLD): Trapped in an endless loop of backup CPLD Golden
    Impact motherboard:
        All X13/H13 ROT2-HW2 MBs
    Affected functions:
    Validation:
        1. For Sean Fan LAB validation only
           Follow production line finding, stress test to prove the failure rate is much less than 2%.
           For more info, please contact Nash Liang or Hammer Chien

5.
    Category: Fix
    Description:
        [169590] Warning: NVMe_SSDA temperature 75 is higher than the threshold 70 C
    Impact motherboard:
        H13DSG-O-CPU
    Affected functions:
    Validation:
        1. Heat up the NVMe disk
        2. Check whether the fan speed in the corresponding cooling region of the NVMe disk increases

6.
    Category: Fix
    Description:
        [168645] [AS-1115SV-WTNRT][HDS-SUN-MZWLO1T9HCJA07] NVMe doesn't show Firmware Revision in Storage Monitoring Physical View
    Impact motherboard:
        H13SVW-N, H13SVW-NT
    Affected functions:
    Validation:
        1. Insert HDS-SUN-MZWLO1T9HCJA07
        2. Go to System - Storage Monitoring - Physical View page
        3. Check if NVMe firmware revision is correct

7.
    Category: Fix
    Description:
        [168628] [IPMI 01.01.13 ECO] There are no MEL when executing GMI error inject
        [151917] [AMD RAS][CH6] No show OS error log when execute "GMI3/xGMI3 Error Injection"
    Impact motherboard:
        H13SST-G, H13SST-GC, H13DSH
    Affected functions:
    Validation:
        1. Execute the GMI3/xGMI3 Error Injection
        2. Check SEL

8.
    Category: Fix
    Description:
        [165307] STD -- SW-- 01.01.09--No mel generated when changing Prefix length from 128 to 32
    Impact motherboard:
        H13DSH
    Affected functions:
    Validation:
        1. Go to Configuration - Network - IP Access Control page
        2. Enabled IP Address Control and add a rule
        3. Fill IP address, Set Prefix Length to 128, and Save
        4. Modify Prefix Length to 32, and Save
        5. Check MEL

Protection maps:
    H13DSG_O    BitMap-20231113-170745.bin
    H13DSH      BitMap-20221128-184047-MPS.bin
    H13SSL_N    BitMap-20221128-184047-MPS.bin
    H13SST_G    BitMap-20221128-184047-MPS.bin
    H13SSW      BitMap-20221128-184047-MPS.bin
    H13SVW_N    BitMap-20221128-184047-MPS.bin

==============================================================================================================================
Filename: BMC_H13AST2600-ROT-1401MS_20231226_01.01.13_STDsp.bin version: 01.01.13 Date: 26 Dec 2023
U-Boot baseline : 2019.04
Java SOL Viewer version : v0.5.16
Java iKVM Viewer version : v1.69.53
Redfish API : Redfish_1_11_API_full_list_20231218
spl: 02.03.38
tee.bin: 0100.03.76
antiRBID: 0x0001
Supported MBs: H13SST-G, H13SST-GC, H13SSL-N, H13SSL-NT, H13DSG-O-CPU, H13SSW, H13DSH, H13SVW-N, H13SVW-NT
Signed key: new X13 ROT key

1.
    Category: Fix
    Description:
        C: Fix the non-A node does not change the MB CPLD register When the smart power is turned off
    Impact motherboard:
        H13SST-G, H13SST-GC
    Affected functions:
    Validation:
        1. Turn the Smart power to ON in node A
        2. Check if node B/C/D MB CPLD GPIO bit 0 is 1
              ipmitool raw 0x30 0x68 0x28 0x09 0x00
        3. Turn the Smart power to OFF in node A
        2. Check if node B/C/D MB CPLD GPIO bit 0 is 0
              ipmitool raw 0x30 0x68 0x28 0x09 0x00

2.
    Category: Fix
    Description:
        [162259] ECO -- 21603 -- 01.01.03 -- MEL not match with SPEC with long input of remote User/remote group
    Impact motherboard:
        H13SSL-N, H13SSL-NT
    Affected functions:
    Validation:
        1. Verify according to issue 162259 content

Protection maps:
    H13DSG_O    BitMap-20231113-170745.bin
    H13DSH      BitMap-20221128-184047-MPS.bin
    H13SSL_N    BitMap-20221128-184047-MPS.bin
    H13SST_G    BitMap-20221128-184047-MPS.bin
    H13SSW      BitMap-20221128-184047-MPS.bin
    H13SVW_N    BitMap-20221128-184047-MPS.bin

==============================================================================================================================
Filename: BMC_H13AST2600-ROT-1401MS_20231218_01.01.12_STDsp.bin version: 01.01.12 Date: 18 Dec 2023
U-Boot baseline : 2019.04
Java SOL Viewer version : v0.5.16
Java iKVM Viewer version : v1.69.53
Redfish API : Redfish_1_11_API_full_list_20231110
spl: 02.03.38
tee.bin: 0100.03.76
antiRBID: 0x0001
Supported MBs: H13SST-G, H13SST-GC, H13SSL-N, H13SSL-NT, H13DSG-O-CPU, H13SSW, H13DSH, H13SVW-N, H13SVW-NT
Signed key: new X13 ROT key

1.
    Category: Fix
    Description:
        [167677] STD -- 21603 -- 01.01.11(2023/11/28) -- DNS Lookup toggle button isn't disabled when system lockdown mode is on
    Impact motherboard:
        H13SST-G, H13SST-GC
    Affected functions:
    Validation:
        1. Turn on system lockdown mode
        2. Enter to Directory Services pages and expand Active Directory area

2.
    Category: Fix
    Description:
        [167270] STD -- SW--01.01.10 -- Doesn't show IPv6 gateway IP after it was configured
    Impact motherboard:
        H13DSH
    Affected functions:
    Validation:
        1. Go to Configuration - Network page
        2. Set IPv6 to Static Configuration and iput Address, Prefix, Geteway 
        3. Refresh page, and then check Geteway

3.
    Category: Fix
    Description:
        [167196] [AS-2125HS-TNR_PVT_H1B2][AOC-S25GC-i4S] NC-SI function of AOC-S25GC-i4S cannot be workable
    Impact motherboard:
        H13DSH
    Affected functions:
    Validation:
        1. Insert the AOC-S25GC-i4S and connect the NCSI cable
        2. Go to Configuration - Network page
        2. Check if filed 'LAN Interface' has 'Shared' option

4.
    Category: Fix
    Description:
        [167011] [IPMI ECO 01.01.11] SATC Redfish Automation test failed
        [166944] ECO -- 21603 -- 01.01.11 (2023/11/28) -- Redfish -- Checking SmartPower URL return code error
    Impact motherboard:
        H13SVW-N, H13SVW-NT
    Affected functions:
    Validation:
        1. GET https://<bmc-ip>/redfish/v1/Managers/1/Oem/Supermicro/SmartPower
        2. Return code should be 404

5.
    Category: Fix
    Description:
        [166555] ECO -- 21603 -- 01.01.10(20231108) -- supposed to show ONLY the least required key of the limited function when no License is activated
    Impact motherboard:
        H13DSG-O-CPU
    Affected functions:
    Validation:
        1. Go to Configuration - Account Services - Directory Service page
        2. Go to Configuration - Notifications - Alerts page
        3. Check hint should only show minimum license requirement

6.
    Category: Fix
    Description:
        [166554] ECO -- 21603 -- 01.01.10(20231108) -- License require pop-up diagram not quite match with definition (string of the button)
    Impact motherboard:
        H13DSG-O-CPU
    Affected functions:
    Validation:
        1. Clear License Key
        2. Go to Configuration - Notifications - Syslog page
        3. Go to Configuration - BMC Settings - System Lockdown page
        4. Go to Maintenance - Troubleshooting - Console Capture page

7.
    Category: Fix
    Description:
        [166278] (BIOS_H13DSGO-1C7E_20231118_1.6a_STDsp.bin,SPPT) Get error event (Timestamp) in IPMI SEL when executed SPPT test
    Impact motherboard:
        H13DSG-O-CPU
    Affected functions:
    Validation:
        1. Make sure bmc use_ntp option is off
        2. Clear SEL
        3. BMC reset and wait BMC boot compeltely
        4. DC cycle and wait system boots to UEFI or OS
        5. Monitor SEL. There should be no timestamp sync SEL entry
        6. [optional] Follow the issueID to check with SPPT test

8.
    Category: Fix
    Description:
        [164843] ECO -- 21603 -- 01.01.08(2023/10/06) -- Part of alerts are missing after executing unit BMC reset
    Impact motherboard:
        H13SSL-N, H13SSL-NT
    Affected functions:
    Validation:
        1. Do BMC factory reset
        2. Go to Configuration - Notifications - Alerts page, Add 16 alerts
        3. BMC reset, wait for BMC to be ready
        4. Check if 16 alerts are correct

Protection maps:
    H13DSG_O    BitMap-20231113-170745.bin
    H13DSH      BitMap-20221128-184047-MPS.bin
    H13SSL_N    BitMap-20221128-184047-MPS.bin
    H13SST_G    BitMap-20221128-184047-MPS.bin
    H13SSW      BitMap-20221128-184047-MPS.bin
    H13SVW_N    BitMap-20221128-184047-MPS.bin

==============================================================================================================================
Filename: BMC_H13AST2600-ROT-1401MS_20231128_01.01.11_STDsp.bin version: 01.01.11 Date: 28 Nov 2023
U-Boot baseline : 2019.04
Java SOL Viewer version : v0.5.16
Java iKVM Viewer version : v1.69.53
Redfish API : Redfish_1_11_API_full_list_20231003
spl: 02.03.37
tee.bin: 0100.03.73
antiRBID: 0x0001
Supported MBs: H13SST-G, H13SST-GC, H13SSL-N, H13SSL-NT, H13DSG-O-CPU, H13SSW, H13DSH, H13SVW-N, H13SVW-NT
Signed key: new X13 ROT key

1.
    Category: New
    Description:
        Support AMD SB-RMI version 2.1
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Install AMD Turin CPU, MUST use a BIOS version that supports AMD Turin CPU
        2. CPU powers up, and wait for BMC sensor to be ready
        3. Go to System - Component Info - CPU page
        4. Check if the field "TDP Watts" is equal to the CPU TDP

2.
    Category: Enhancement
    Description:
        Support Smart_Power_Spec_v1.12
    Impact motherboard:
        H13SST-G, H13SST-GC
    Affected functions:
    Validation:
        1. MUST use CPLD F5.07.29
        2. Smart Power features should follow the spec

3.
    Category: Fix
    Description:
        [166052] ECO -- 21603 -- 01.01.10(2023/11/08) -- Web function -- Radio buttons of Host interface aren't disabled when system lockdown mode is on
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Go to Configuration - BMC Settings - System Lock down page
        2. Enable system lockdown mode
        3. Go to Configuration - BMC Settings - Host interface page
        4. Check "USB connection" radio buttons

4.
    Category: Fix
    Description:
        [165582] [Management Plug-in for Nagios Core V1.2.0_build_230911] Nagios doesn't have event in Supermicro Event Receiver after remove fan or power cord
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Go to Configuration - Notifications - Alerts page
        2. Set Alert
        3. Nagios should be alerted when FAN/power cord is removed

5.
    Category: Fix
    Description:
        [165307] STD -- SW-- 01.01.09--No mel generated when changing Prefix length from 128 to 32
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Go to Configuration - Network - IP Access Control page
        2. Enabled IP Address Control and add a rule
        3. Fill IP address, Set Prefix Length to 128, and Save
        4. Modify Prefix Length to 32, and Save
        5. Check MEL

6.
    Category: Fix
    Description:
        [165005] [AS-1115SV-WTNRT][HDS-TUN-KCMYXRUG1T92] Slot0 NVMe Link Speed will show N/A after AC power on system in Storage Monitoring Physical View
    Impact motherboard:
        H13SVW-N, H13SVW-NT
    Affected functions:
    Validation:
        1. Install Kioxia CM7 HDS-TUN-KCMYXRUG1T92 drive on BPN
        2. Check if the Link Speed info can be displayed in Storage page normally

7.
    Category: Fix
    Description:
        [164559] ECO -- 21603 -- 01.01.08(2023/10/06) -- IP access control permits identical duplicate rules
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Go to Configuration - Network - IP Access Control page
        2. Add ACCEPT 10.122.133.144/32, and Save
        3. Add another ACCEPT 10.122.133.144/32, and Save
        4. Add DROP 10.122.133.144/32, and Save
        5. Add another DROP 10.122.133.144/32, and Save

8.
    Category: Fix
    Description:
        [151917] [AMD RAS][CH6] No show OS error log when execute "GMI3/xGMI3 Error Injection"
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Execute the RAS error injection
        2. Check SEL

Protection maps:
    H13DSG_O    BitMap-20231113-170745.bin
    H13DSH      BitMap-20221128-184047-MPS.bin
    H13SSL_N    BitMap-20221128-184047-MPS.bin
    H13SST_G    BitMap-20221128-184047-MPS.bin
    H13SSW      BitMap-20221128-184047-MPS.bin
    H13SVW_N    BitMap-20221128-184047-MPS.bin

==============================================================================================================================
Filename: BMC_H13AST2600-ROT-1401MS_20231108_01.01.10_STDsp.bin version: 01.01.10 Date: 08 Nov 2023
U-Boot baseline : 2019.04
Java SOL Viewer version : v0.5.16
Java iKVM Viewer version : v1.69.53
Redfish API : Redfish_1_11_API_full_list_20231003
spl: 02.03.37
tee.bin: 0100.03.73
antiRBID: 0x0001
Supported MBs: H13SST-G, H13SST-GC, H13SSL-N, H13SSL-NT, H13DSG-O-CPU, H13SSW, H13DSH, H13SVW-N, H13SVW-NT
Signed key: new X13 ROT key

1.
    Category: New
    Description:
        Enable 16-bit POST code
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Login BMC WEB, Go to Maintenance - Troubleshooting - POST Snooping page
        2. POST Snooping should be shown hexadecimal digits

2.
    Category: Enhancement
    Description:
        Change RAS crash dump reset type to warm boot
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Install BIOS firmware that supports ADDC 1.8
        2. Unlock CPU, and inject error using AMD RAS tool
        3. Login BMC WEB, Go to Maintenance - Troubleshooting - System Crash Dump page, download file
        4. Check the file with AMD RAS crash dump Analyzer Tool

3.
    Category: Fix
    Description:
        Sensor list fails when temperature sensor is greater than or equal to 32
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Temperature sensor greater than 32
        2. Sensors should be normal on the Sensor page

4.
    Category: Fix
    Description:
        [161021] ECO -- 21603 -- 01.01.02(20230811) -- [GUI] Help page not list related info of SSDP & LLDP
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Check in Help page

5.
    Category: Fix
    Description:
        [163529] ECO — 21603 — 01.01.07(09/22/2023) — [MEL] — No related MEL when disable TSIG Authentication
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Change TSIG enabed/disabled
        2. Check MEL

6.
    Category: Fix
    Description:
        [164898] ECO -- 21603 -- 01.01.08(2023/10/06) -- Web Function -- "Verify SSL Certificate" and " Accept Self-signed Certificate" shouldn't be selected if setting File Server to "http://xxxxx"
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Login BMC WEB, Go to Configuration - Virtual Media page
        2. Edit VM Connection, Set File Server to "https://xxxxxx" and click Save button
        3. Edit the added VM Connection, Change File server from "https://xxxx" to "http://xxxxx" and click Save button
        4. Check the data of Verify SSL Certificate and Accept Self-signed Certificate

7.
    Category: Fix
    Description:
        [163233] Please check 'PLX Temp' IPMI sensor reading
        [164808] [AS-4125GS-TNRT1] Sensor page all sensor displayed gray out under BMC GUI
        [165045] [IPMI Sensor] No sensor reading after running GPU tests
    Impact motherboard:
        H13DSG-O-CPU
    Affected functions:
    Validation:
        1. Insert AOM-PCIE5-418P-1
        2. Reset the CPU more than 10 times
        3. Only one 'PLX Temp' on sensor page

8.
    Category: Fix
    Description:
        [165027] [ASG-2015S-E1CR24H][ECO_BIOS_BMC] BMC "Physicial View" function will abnormal after click "Make/Remove JBOD" function item
    Impact motherboard:
        H13SSW
    Affected functions:
    Validation:
        1. Login BMC WEB, Go to System - Storage Monitoring - Physical View page
        2. Select JBOD action and change to other actions, it should hide JBOD items

Protection maps:
    H13DSG_O    BitMap-20220623-160757-MPS.bin
    H13DSH      BitMap-20221128-184047-MPS.bin
    H13SSL_N    BitMap-20221128-184047-MPS.bin
    H13SST_G    BitMap-20221128-184047-MPS.bin
    H13SSW      BitMap-20221128-184047-MPS.bin
    H13SVW_N    BitMap-20221128-184047-MPS.bin

==============================================================================================================================
Filename: BMC_H13AST2600-ROT-1401MS_20231013_01.01.09_STDsp.bin version: 01.01.09 Date: 13 Oct 2023
U-Boot baseline : 2019.04
Java SOL Viewer version : v0.5.16
Java iKVM Viewer version : v1.69.53
Redfish API : Redfish_1_11_API_full_list_20231003
spl: 02.03.36
tee.bin: 0100.03.71
antiRBID: 0x0001
Supported MBs: H13SST-G, H13SST-GC, H13SSL-N, H13SSL-NT, H13DSG-O-CPU, H13SSW, H13DSH, H13SVW-N, H13SVW-NT
Signed key: new X13 ROT key

1.
    Category: Fix
    Description:
        [164264] [AS-1125HS-TNR][BPN] IPMI WebGUI Firmware Management only show one update option of Backplane CPLD due to system have two BPN
    Impact motherboard:
        H13DSH
    Affected functions:
    Validation:
        1. Insert BPN-NVME5-HS119N-S4R
        2. Update BPN-NVME5-HS119N-S4R CPLD firmware

2.
    Category: Fix
    Description:
        [163952] [AS-2015SV-WTNRT]When AOC-STG-b2T install on slot 5 ,"Health status" incorrect under BMC Web GUI
    Impact motherboard:
        H13SVW-N, H13SVW-NT
    Affected functions:
    Validation:
        1. Using a version later than BIOS 1.1 2023/09/27 and insert AOC-STG-b2T into slot-5
        2. Login BMC WEB, Go to Component Info - NetWork AOC page
        3. Check AOC-STG-b2T Health status

Protection maps:
    H13DSG_O    BitMap-20220623-160757-MPS.bin
    H13DSH      BitMap-20221128-184047-MPS.bin
    H13SSL_N    BitMap-20221128-184047-MPS.bin
    H13SST_G    BitMap-20221128-184047-MPS.bin
    H13SSW      BitMap-20221128-184047-MPS.bin
    H13SVW_N    BitMap-20221128-184047-MPS.bin

==============================================================================================================================
Filename: BMC_H13AST2600-ROT-1401MS_20231006_01.01.08_STDsp.bin version: 01.01.08 Date: 06 Oct 2023
U-Boot baseline : 2019.04
Java SOL Viewer version : v0.5.16
Java iKVM Viewer version : v1.69.53
Redfish API : Redfish_1_11_API_full_list_20231003
spl: 02.03.36
tee.bin: 0100.03.71
antiRBID: 0x0001
Supported MBs: H13SST-G, H13SST-GC, H13SSL-N, H13SSL-NT, H13DSG-O-CPU, H13SSW, H13DSH, H13SVW-N, H13SVW-NT
Signed key: new X13 ROT key

1.
    Category: Fix
    Description:
        Fix Current owner index is wrong after RA provision
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Do RA provision and get measurement
        2. The measurement should be verified pass by sum tool

2.
    Category: Fix
    Description:
        MEL-0135 displays more than 3 times
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. AC turns on, wait for BIOS POST to complete
        2. Check MEL

3.
    Category: Fix
    Description:
        BMC cannot obtain IP
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Only plug the ethernet cable into the system LAN 1
        2. BMC LAN Interface set to Failover mode
        3. BMC reset 50 times
        4. After each RESET, the BMC IP should be obtained

4.
    Category: Fix
    Description:
        [163528] ECO — 21603 — 01.01.07(09/22/2023) — [SUM] — IPv4 DNS setting comparison wasn't the same after executing "ChangeBmcCfg" command via SUM
        [163845] ECO — 21603 — 01.01.07(09/22/2023) — [SUM] — IPv4 DNS setting comparison wasn't the same after executing "ChangeBmcCfg" command via SUM
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Run SUM ECO Test Case 3073

5.
    Category: Fix
    Description:
        [163529] ECO — 21603 — 01.01.07(09/22/2023) — [MEL] — No related MEL when disable TSIG Authentication
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Login BMC WEB, Go to Configuration - BMC Settings - Date and Time page
        2. NTP Enable set to ON and Save
        2. Login BMC WEB, Go to Configuration - BMC Settings - Dynamic DNS page
        3. Dynamic Update Enable set to ON, Enable TSIG Authentication set to ON, Load TSIG key/private Files and Save
        4. Enable TSIG Authentication set to OFF and Save
        5. Check MEL

Protection maps:
    H13DSG_O    BitMap-20220623-160757-MPS.bin
    H13DSH      BitMap-20221128-184047-MPS.bin
    H13SSL_N    BitMap-20221128-184047-MPS.bin
    H13SST_G    BitMap-20221128-184047-MPS.bin
    H13SSW      BitMap-20221128-184047-MPS.bin
    H13SVW_N    BitMap-20221128-184047-MPS.bin

==============================================================================================================================
Filename: BMC_H13AST2600-ROT-1401MS_20230922_01.01.07_STDsp.bin version: 01.01.07 Date: 22 Sep 2023
U-Boot baseline : 2019.04
Java SOL Viewer version : v0.5.16
Java iKVM Viewer version : v1.69.53
Redfish API : Redfish_1_11_API_full_list_20230824
spl: 02.03.36
tee.bin: 0100.03.64
antiRBID: 0x0001
Supported MBs: H13SST-G, H13SST-GC, H13SSL-N, H13SSL-NT, H13DSG-O-CPU, H13SSW, H13DSH, H13SVW-N, H13SVW-NT
Signed key: new X13 ROT key

Rebuilt based on BMC FW 1.1.6

==============================================================================================================================
Filename: BMC_H13AST2600-ROT-1401MS_20230922_01.01.06_STDsp.bin version: 01.01.06 Date: 22 Sep 2023
U-Boot baseline : 2019.04
Java SOL Viewer version : v0.5.16
Java iKVM Viewer version : v1.69.53
Redfish API : Redfish_1_11_API_full_list_20230824
spl: 02.03.36
tee.bin: 0100.03.64
antiRBID: 0x0001
Supported MBs: H13SST-G, H13SST-GC, H13SSL-N, H13SSL-NT, H13DSG-O-CPU, H13SSW, H13DSH, H13SVW-N, H13SVW-NT
Signed key: new X13 ROT key

1.
    Category: New feature
    Description:
        Support IPv6 enhancement spec. (Proposal for BIOS-BMC IPv6 inconsistency_V11.pptx)
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. IPv6 features should follow the spec

2.
    Category: Enhancement
    Description:
        Update AMD RAS crash dump to ADDC 1.8
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Install BIOS firmware that supports ADDC 1.8
        2. Unlock CPU, and inject error using AMD RAS tool
        3. Login BMC WEB, Go to Maintenance - Troubleshooting - System Crash Dump page, download file
        4. Check the file with AMD RAS crash dump Analyzer Tool

3.
    Category: Enhancement
    Description:
        Support AS-1115S-FWTRT and AS-1115S-FDWTRT
    Impact motherboard:
        H13SVW-N, H13SVW-NT
    Affected functions:
    Validation:
        1. Test on AS-1115S-FWTRT/AS-1115S-FDWTRT

4.
    Category: Fix
    Description:
        [162844] STD -- 21603 -- 01.01.05 (2023/09/08) -- WEB -- MEL is incorrect after do ikvm reset
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Login BMC WEB, Go to Remote Control page
        2. Press the button "Launch Console"
        3. Press the button "Reset"
        4. Check MEL

5.
    Category: Fix
    Description:
        [162823] ECO -- 21603 -- 01.01.05 -- Remote Console Preview current interface button enabled
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Login BMC WEB, Go to Dashboard page
        2. Hover over the buttons HTML 5 and JAVA plug-in. Notice they are both clickable on hover

6.
    Category: Fix
    Description:
        [162697] ECO28568 / H13DSG-O-CPU R1.20 / Web slow issue (BMC)
    Impact motherboard:
        H13DSG-O-CPU
    Affected functions:
    Validation:
        1. Validated by CM

7.
    Category: Fix
    Description:
        [160509] ECO — 21603 — 01.01.01(07/21/2023) — [MEL] — should non-set IPv4 DNS Server IP related MEL be shown when setup Hostname or not
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Login BMC WEB, Go to Configuration - Network page
        2. Edit Hostname and Save, then check MEL
        2. Clear Hostname and Save, then check MEL

8.
    Category: Fix
    Description:
        [158525] [QCL- GPU-NVH100-80] There're GPU temp events when running GPU test(GBN / GME)
    Impact motherboard:
        H13DSH
    Affected functions:
    Validation:
        1. Insert the GPU-NVH100-80
        2. Check if GPS Temp sensor threshold is same as the "System Thermal Design Guide - GPU Temperature Threshold Rev 1.01 Aug 2023"

9.
    Category: Fix
    Description:
        [156498] ECO -- 21603 -- 01.00.18 -- [MEL] should non-set IPv4 DNS Server IP related MEL be shown when setup IPv6 DNS Server IP or not
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Login BMC WEB, Go to Configuration - Network page
        2. Setup IPv6 DNS Server IP to 2001:db8::fd and Save, then check MEL
        2. Clear IPv6 DNS Server IP and Save, then check MEL

10.
    Category: Fix
    Description:
        [162843] [IPMI 1.01.05 ECO ] IPMI display "PCIE PERR error" when inject memory UECC
        [162842] [IPMI 1.01.05 ECO ] IPMI display incorrect location when inject memory CECC
        [151917] [AMD RAS][CH6] No show OS error log when execute "GMI3/xGMI3 Error Injection"
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Execute the RAS error injection
        2. Check SEL

Protection maps:
    H13DSG_O    BitMap-20220623-160757-MPS.bin
    H13DSH      BitMap-20221128-184047-MPS.bin
    H13SSL_N    BitMap-20221128-184047-MPS.bin
    H13SST_G    BitMap-20221128-184047-MPS.bin
    H13SSW      BitMap-20221128-184047-MPS.bin
    H13SVW_N    BitMap-20221128-184047-MPS.bin

==============================================================================================================================
Filename: BMC_H13AST2600-ROT-1401MS_20230908_01.01.05_STDsp.bin version: 01.01.05 Date: 08 Sep 2023
U-Boot baseline : 2019.04
Java SOL Viewer version : v0.5.16
Java iKVM Viewer version : v1.69.53
Redfish API : Redfish_1_11_API_full_list_20230824
spl: 02.03.36
tee.bin: 0100.03.64
antiRBID: 0x0001
Supported MBs: H13SST-G, H13SST-GC, H13SSL-N, H13SSL-NT, H13DSG-O-CPU, H13SSW, H13DSH, H13SVW-N, H13SVW-NT
Signed key: new X13 ROT key

1.
    Category: Enhancement
    Description:
        Refactor detect PCIe board
    Impact motherboard:
        H13DSG-O-CPU
    Affected functions:
    Validation:
        1. When using a single motherboard, the speed of logging into the WEB should be normal
        2. Insert AOM-PCIE5-418N-1, PLX Temp should not be displayed
        3. Insert AOM-PCIE5-418N-1, PLX Temp should be displayed

2.
    Category: Enhancement
    Description:
        PSU FAN page synchronization with PSU page
    Impact motherboard:
        H13SST-G, H13SST-GC
    Affected functions:
    Validation:
        1. Check that the PSU FANA speed on the FAN page is close to the FAN1 speed of the 1st PSU on the PSU page
        2. Check that the PSU FANB speed on the FAN page is close to the FAN1 speed of the 2nd PSU on the PSU page

3.
    Category: Fix
    Description:
        [161179] [BIOS ECO 1.0] BIOS ECO Automation tests Failure
    Impact motherboard:
        H13SVW-N, H13SVW-NT
    Affected functions:
    Validation:
        1. Use H13SVW BIOS version 1.0 08/25/2023 or latest
        2. Verify with BIOS ECO

4.
    Category: Fix
    Description:
        [161767] Unable to set NTP using domain name via BMC WebUI
    Impact motherboard:
        H13SVW-N, H13SVW-NT
    Affected functions:
    Validation:
        1. Login BMC WEB, Go to Configuration - BMC Setting - Date and Time page
        2. Enable NTP and set primary NTP server

5.
    Category: Fix
    Description:
        [162260] ECO -- 21603 -- 01.01.03 -- SNMP(User) Auth/Private Key naming not match with MEL
    Impact motherboard:
        H13SSL-N, H13SSL-NT
    Affected functions:
    Validation:
        1. Login BMC WEB, Go to Configuration - Account Services - Users page
        2. Add a new user and configure it as in the screenshot of the issue
        3. Check MEL

6.
    Category: Fix
    Description:
        [162262] ECO -- 21603 -- 01.01.03 -- [GUI] Password can't be reverse of the User name, error return "Oops! Something went wrong." not quit match with the situation
    Impact motherboard:
        H13SSL-N, H13SSL-NT
    Affected functions:
    Validation:
        1. Login BMC WEB, Go to Configuration - Account Services - Users page
        2. Add a new user with the username and password set to 890DessertS, ans Save
        3. Error message should be correct

7.
    Category: Fix
    Description:
        [162263] ECO -- 21603 -- 01.01.03 -- SNMPv3(Alert) Authentication/Encryption Protocol naming not match with MEL
    Impact motherboard:
        H13SSL-N, H13SSL-NT
    Affected functions:
    Validation:
        1. Login BMC WEB, Go to Configuration - Notifications - SNMP page
        2. Enable NTP and SNMPv3
        3. Set Authentication/Encryption Protocolto HMAC_SHA96/CFB128_AES128 and Save
        4. Set Authentication/Encryption Protocolto HMAC_SHA96/CBC_DES and Save
        5. Check MEL

Protection maps:
    H13DSG_O    BitMap-20220623-160757-MPS.bin
    H13DSH      BitMap-20221128-184047-MPS.bin
    H13SSL_N    BitMap-20221128-184047-MPS.bin
    H13SST_G    BitMap-20221128-184047-MPS.bin
    H13SSW      BitMap-20221128-184047-MPS.bin
    H13SVW_N    BitMap-20221128-184047-MPS.bin

==============================================================================================================================
Filename: BMC_H13AST2600-ROT-1401MS_20230828_01.01.04_STDsp.bin version: 01.01.04 Date: 28 Aug 2023
U-Boot baseline : 2019.04
Java SOL Viewer version : v0.5.16
Java iKVM Viewer version : v1.69.53
Redfish API : Redfish_1_11_API_full_list_20230613
spl: 02.03.36
tee.bin: 0100.03.64
antiRBID: 0x0001
Supported MBs: H13SST-G, H13SST-GC, H13SSL-N, H13SSL-NT, H13DSG-O-CPU, H13SSW, H13DSH, H13SVW-N, H13SVW-NT
Signed key: new X13 ROT key

1.
    Category: Fix
    Description:
        Fix OTP flush error and should stop provision
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. ipmitool -H IP_ADDRESS -U USER_NAME -P PASSWORD raw 0x30 0x68 0x28 0x01

2.
    Category: Fix
    Description:
        [159725] [RoT] Update CPLD Golden image event log timestamp is incorrect
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Login BMC WEB, Go to Firmware Management - Inventory page
        2. Trigger CPLD golden update
        3. Check the date of related MEL

3.
    Category: Fix
    Description:
        [160511] ECO -- 21603 -- 01.01.01(07/21/2023) -- Could not mount ISO via SMCIPMITool when Virtual Media does not mount any ISO or floppy
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Open cmd and change path to SMCIPMITool tool
        2. Type command to mount ISO 'SMCIPMITool.exe <BMC_IP> ADMIN ADMIN wsiso mount <Server_IP> /Public/ISO/Redhat/RHEL9.1.iso admin <password>'
        3. Check return message

Protection maps:
    H13DSG_O    BitMap-20220623-160757-MPS.bin
    H13DSH      BitMap-20221128-184047-MPS.bin
    H13SSL_N    BitMap-20221128-184047-MPS.bin
    H13SST_G    BitMap-20221128-184047-MPS.bin
    H13SSW      BitMap-20221128-184047-MPS.bin
    H13SVW_N    BitMap-20221128-184047-MPS.bin

==============================================================================================================================
Filename: BMC_H13AST2600-ROT-1401MS_20230823_01.01.03_STDsp.bin version: 01.01.03 Date: 23 Aug 2023
U-Boot baseline : 2019.04
Java SOL Viewer version : v0.5.16
Java iKVM Viewer version : v1.69.53
Redfish API : Redfish_1_11_API_full_list_20230613
spl: 02.03.36
tee.bin: 0100.03.64
antiRBID: 0x0001
Supported MBs: H13SST-G, H13SST-GC, H13SSL-N, H13SSL-NT, H13DSG-O-CPU, H13SSW, H13DSH, H13SVW-N, H13SVW-NT
Signed key: new X13 ROT key

1.
    Category: Fix
    Description:
        Fix PCIe dump issue with AMD RAS crash dump
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Use a BIOS version that supports the AMD RAS crash dump feature (AGESA 1009)
        2. Unlock CPU, and inject error using AMD RAS tool
        3. Login BMC WEB, Go to Maintenance - Troubleshooting - System Crash Dump page, download file
        4. Check the file with AMD RAS crash dump Analyzer Tool

2.
    Category: Fix
    Description:
        [161009] Memory temp alerts showed at 60 degree
    Impact motherboard:
        H13DSG-O
    Affected functions:
    Validation:
        1. Cburn SAT test running
        2. Checking event logs

3.
    Category: Fix
    Description:
        [160532] STD -- HW-- 01.01.01-- Need to define MEL-ID for "LLDP was configured to enabled/disabled successfully
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Login BMC WEB, Go to Configuration - Network - LLDP page
        2. Enable LLDP and Save
        3. Disable LLDP and Save
        4. Check MEL

4.
    Category: Fix
    Description:
        [160511] ECO -- 21603 -- 01.01.01(07/21/2023) -- Could not mount ISO via SMCIPMITool when Virtual Media does not mount any ISO or floppy
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. SMCIPMITool.exe <BMC_IP> ADMIN ADMIN wsiso mount <Server_IP> /Public/ISO/Redhat/RHEL9.1.iso admin <password>
        2. Check return message

5.
    Category: Fix
    Description:
        [160497] ECO — 21603 — 01.01.01(07/21/2023) — [GUI] — Deditcated Link speed has 10M speed
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Login BMC WEB, Go to Configuration - Network page
        2. It's not support 10M link speed anymore

6.
    Category: Fix
    Description:
        [158603] IPMI web can't update BPN CPLD
    Impact motherboard:
        H13DSH
    Affected functions:
    Validation:
        1. Insert BPN-NVMe5-HS119N-S8L
        2. Update BPN firmware

Protection maps:
    H13DSG_O    BitMap-20220623-160757-MPS.bin
    H13DSH      BitMap-20221128-184047-MPS.bin
    H13SSL_N    BitMap-20221128-184047-MPS.bin
    H13SST_G    BitMap-20221128-184047-MPS.bin
    H13SSW      BitMap-20221128-184047-MPS.bin
    H13SVW_N    BitMap-20221128-184047-MPS.bin

==============================================================================================================================
Filename: BMC_H13AST2600-ROT-1401MS_20230811_01.01.02_STDsp.bin version: 01.01.02 Date: 11 Aug 2023
U-Boot baseline : 2019.04
Java SOL Viewer version : v0.5.16
Java iKVM Viewer version : v1.69.53
Redfish API : Redfish_1_11_API_full_list_20230613
spl: 02.03.35
tee.bin: 0100.03.63
antiRBID: 0x0001
Supported MBs: H13SST-G, H13SST-GC, H13SSL-N, H13SSL-NT, H13DSG-O-CPU, H13SSW, H13DSH, H13SVW-N, H13SVW-NT
Signed key: new X13 ROT key

1.
    Category: Enhancement
    Description:
        Support RSC-2-66G5+
    Impact motherboard:
        H13SVW-N, H13SVW-NT
    Affected functions:
    Validation:
        1. Insert RSC-2-66G5+ and AOC cards
        2. Check if sensor list is correct

2.
    Category: Enhancement
    Description:
        Modify fan speed control
    Impact motherboard:
        H13SVW-N, H13SVW-NT
    Affected functions:
    Validation:
        1. Verified by Thermal RD

3.
    Category: Fix
    Description:
        Provision failed
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Execute Provision

4.
    Category: Fix
    Description:
        [158637] [SSM_5.5.0_b1222] Diagnose System fail (Failed to restore the BIOS configurations) on the H13SVW-N
    Impact motherboard:
        H13SVW-N, H13SVW-NT
    Affected functions:
    Validation:
        1. Verify with SSM Diagnose System

5.
    Category: Fix
    Description:
        [160218] [AS-1115SV-WTNRT_EVT_H1] The NVMe info is incorrect
    Impact motherboard:
        H13SVW-N, H13SVW-NT
    Affected functions:
    Validation:
        1. Insert SAMSUNG MZQLB960HAJR-00007
        2. Check NVMe info

Protection maps:
    H13DSG_O    BitMap-20220623-160757-MPS.bin
    H13DSH      BitMap-20221128-184047-MPS.bin
    H13SSL_N    BitMap-20221128-184047-MPS.bin
    H13SST_G    BitMap-20221128-184047-MPS.bin
    H13SSW      BitMap-20221128-184047-MPS.bin
    H13SVW_N    BitMap-20221128-184047-MPS.bin

==============================================================================================================================
Filename: BMC_H13AST2600-ROT-1401MS_20230721_01.01.01_STDsp.bin version: 01.01.01 Date: 21 Jul 2023
U-Boot baseline : 2019.04
Java SOL Viewer version : v0.5.16
Java iKVM Viewer version : v1.69.52
Redfish API : Redfish_1_11_API_full_list_20230613
spl: 02.03.35
tee.bin: 0100.03.63
antiRBID: 0x0001
Supported MBs: H13SST-G, H13SST-GC, H13SSL-N, H13SSL-NT, H13DSG-O-CPU, H13SSW, H13DSH, H13SVW-N, H13SVW-NT
Signed key: new X13 ROT key

1.
    Category: Fix
    Description:
        [146984] [SD5_5.16.0_b1044] Redfish credential bootstrapping test fail flash BIOS need key-in user and password on the H13SSL-NT
        [147413] [SD5_5.16.0_b1044]Test Redfish credentials bootstrapping for flash BIOS on H13SSW need to login BMC account password
        [155635] [Bergamo][SD5_5.17.0_b1062] Redfish credential bootstrapping test fail flash BIOS need key-in user and password on H13SST
        [155638] [Bergamo][SD5_5.17.0_b1062] Redfish credential bootstrapping test fail flash BIOS need key-in user and password on H13SSW
        [158592] [SD5_5.17.0_build.1065] Redfish credential bootstrapping test fail flash BIOS need key-in user and password on the H13SVW-N
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Verify with SD5

2.
    Category: Fix
    Description:
        [150930] [SSM_5.4.0_b1211] The System Information test fail Processor:Current Clock Speed(MHz): 0 is abnormal on the H13SSL-NT 
        [155625] [Bergamo][SSM_5.4.0_build.1214]No CPU Speed in SSM System Information on H13SST
        [155626] [Bergamo][SSM_5.4.0_build.1214]No CPU Speed in SSM System Information on H13SSW
        [158599] [SSM_5.5.0_b1222] SSM System Information test fail on the H13SVW-N
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Verify with SSM

3.
    Category: Fix
    Description:
        [156576] ECO -- 21603 -- 01.00.18 -- [MEL] generated MEL not quite match when add SNMPv2 (based on MEL SPEC v1.03)
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Login BMC WEB, Go to Configuration - Notifications - SNMP page
        2. Input several communities
        3. Check MEL

4.
    Category: Fix
    Description:
        [157556] [IPMI ECO 01.00.19]Redfish automation failure
        [159180] [IPMI ECO 1.00.20]Redfish automation tool check is fail
        [159406] [BIOS 1.5][IPMI 01.00.20]Redfish automation Failed
        [159513] Redfish automation test failed
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Verify with Redfish automation tools

5.
    Category: Fix
    Description:
        [158323] [EVT] Fan sensor readings issue
    Impact motherboard:
        H13SVW-N, H13SVW-NT
    Affected functions:
    Validation:
        1. Login BMC WEB, Go to System - Component Info - Fan page
        2. Check sensor reading

6.
    Category: Fix
    Description:
        [158643] [EVT] Sensor naming doesn't match the SPEC
    Impact motherboard:
        H13SVW-N, H13SVW-NT
    Affected functions:
    Validation:
        1. Login BMC WEB, Go to System - Component Info - Sensor page
        2. Check sensor reading

7.
    Category: Fix
    Description:
        [158854] [SPM_1.12.0_build230109] SPM power cap function test fail on the H13SVW-N
    Impact motherboard:
        H13SVW-N, H13SVW-NT
    Affected functions:
    Validation:
        1. Verify with SPM

Protection maps:
    H13DSG-O-CPU    BitMap-20220623-160757-MPS.bin
    H13DSH          BitMap-20221128-184047-MPS.bin
    H13SSL-N        BitMap-20221128-184047-MPS.bin
    H13SST-G        BitMap-20221128-184047-MPS.bin
    H13SSW          BitMap-20221128-184047-MPS.bin
    H13SVW-N        BitMap-20221128-184047-MPS.bin

==============================================================================================================================
Filename: BMC_H13AST2600-ROT-1401MS_20230629_01.01.00_STDsp.bin version: 01.01.00 Date: 29 Jun 2023
U-Boot baseline : 2019.04
Java SOL Viewer version : v0.5.16
Java iKVM Viewer version : v1.69.52
Redfish API : Redfish_1_11_API_full_list_20230613
spl: 02.03.35
tee.bin: 0100.03.62
antiRBID: 0x0001
Supported MBs: H13SST-G, H13SST-GC, H13SSL-N, H13SSL-NT, H13DSG-O-CPU, H13SSW, H13DSH, H13SVW-N, H13SVW-NT
Signed key: new X13 ROT key

1.
    Category: New
    Description:
        Redfish support new OEM FixedBootOrder API to replace BootOrder for change bios boot option
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Get /redfish/v1/Systems/1/Oem/Supermicro/FixedBootOrder for current bios boot option
        2. PATCH /redfish/v1/Systems/1/Oem/Supermicro/FixedBootOrder and reboot system for change bios boot option
        3. Change "BootOrder" of /redfish/v1/Systems/1 to read-only
        4. Change /redfish/v1/Systems/1/BootOptions/Boot00{N} to read-only

2.
    Category: New
    Description:
        [299 Phase 1] Disable IPMI Lan Port Interface
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. User can decide whether to disable UDP 623 port and service
        2. SOL feature and other tools will be affected, when UDP 623 port is disable
        3. By default, UDP 623 port is enabled for IPMI LAN

3.
    Category: New
    Description:
        [299 Phase 1] HTML5 Console as default
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. HTML5 Console as default

4.
    Category: New
    Description:
        [299 Phase 1] Dual mode for network setting as default
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Dual mode for network setting as default

5.
    Category: New
    Description:
        [299][MultVM] Virtual media support 3 CD/FLOPPY image mounting
    Impact motherboard:
        All H13 MBs
    Affected functions:
    Validation:
        1. Support at most 3 CD/FLOPPY image mounting at the same time by Redfish and WebUI
           SPEC: https://wiki.supermicro.com/index.php/NS_SWPM:SW_PM/Functional_SPEC/Virtual_Media

6.
    Category: Enhancement
    Description:
        [Enhancement] Modify Dedicated Link options: Add 1G Full and remove 10M Half/Full
    Impact motherboard:
        All H13 MBs that support BMC dedicated LAN
    Affected functions:
    Validation:
        1. Login BMC WEB, Go to Configuration - Network page
        2. Check if Dedicated Link options are correct or not
        3. Change Lan Interface to Dedicated and change Dedicated Link option you want
        4. Click Save button.
        5. Check if Dedicated Status/Speed/Duplex are correct or not

Protection maps:
    H13DSG-O-CPU    BitMap-20220623-160757-MPS.bin
    H13DSH          BitMap-20221128-184047-MPS.bin
    H13SSL-N        BitMap-20221128-184047-MPS.bin
    H13SST-G        BitMap-20221128-184047-MPS.bin
    H13SSW          BitMap-20221128-184047-MPS.bin
    H13SVW-N        BitMap-20221128-184047-MPS.bin

==============================================================================================================================
Filename: BMC_H13AST2600-ROT-1401MS_20230526_01.00.19_STDsp.bin version: 01.00.19 Date: 26 May 2023
U-Boot baseline : 2019.04
Java SOL Viewer version : v0.5.16
Java iKVM Viewer version : v1.69.52
Redfish API : X12_Redfish_1_90_API_full_list_11032021
spl: 02.03.35
tee.bin: 0100.03.59
antiRBID: 0x0001
Supported MBs: H13SST-G, H13SST-GC, H13SSL-N, H13SSL-NT, H13DSG-O-CPU, H13SSW, H13DSH, H13SVW-N, H13SVW-NT
Signed key: new X13 ROT key

1.
    Category: Enhancement
    Description:
        Support H13SVW-N, H13SVW-NT
    Impact motherboard:
        H13SVW-N, H13SVW-NT
    Affected functions:
    Validation:

2.
    Category: Fix
    Description:
        [156144] [AS-4125GS-TNRT2_S2-C1 configuration] Can't correctly detected GPU sensor under BMC GUI
    Impact motherboard:
        H13DSG-O-CPU
    Affected functions:
    Validation:
        1. Inserts AOM-PCIE5-418P-1 and GPU card * 8
        2. On web, go to System > Component Info > Sensor
        3. GPU Information should be correct

3.
    Category: Fix
    Description:
        [156537] ECO -- 21603 -- 01.00.18 -- Fail to add valid Prefix length128 for IPv6 Static Route List
    Impact motherboard:
        H13SST-G, H13SST-GC, H13SSL-N, H13SSL-NT, H13DSG-O-CPU, H13SSW, H13DSH
    Affected functions:
    Validation:
        1. On web, go to Configuration > Nework > IPv6 > Advanced Setting > Enable Static Route, Turn ON
        2. Select ::/255 in IPv6 Static Route List
        3. Type ::/128 in Prefix to Route
        4. Type 2001:db8::fd in Route Address

4.
    Category: Fix
    Description:
        [155539] ECO—21603—01.00.17 (03/29/2023)—No generate MEL when setting Console Capture Video and Crash Screen Capture.
    Impact motherboard:
        H13SSL-N, H13SSL-NT
    Affected functions:
    Validation:
        1. On web, go to Maintenance > Troubleshooting > Console Capture Video
        2. Click enable on/off, setting mode or deleted video button about Console Capture Video
        3. Click button of Crash Screen Capture
        4. Check MEL

5.
    Category: Fix
    Description:
        [156426] CPU information show incorrect Threads in WebUI
    Impact motherboard:
        H13DSH
    Affected functions:
    Validation:
        1. Use a CPU with more than 255 threads
        2. webGUI -> CPU. Observe threads

6.
    Category: Enhancement
    Description:
        Suppoer 8 x GPU sensor
    Impact motherboard:
        H13DSH
    Affected functions:
    Validation:
        1. Insert 8 x GPU and check sensor reading

7.
    Category: Fix
    Description:
        When the AIOM shared LAN has no standby power, the Dedicated LAN will be re-initialized after the system power DC ON
    Impact motherboard:
        H13DSH, H13SSW
    Affected functions:
    Validation:
        1. Install a 10G AIOM card on the system as Shared LAN and make sure its JPAUX1 is set to Disable AUX Power in S5. (Refer to the AOC-ATGC-i2TM manual)
        2. Use Shared LAN mode in IPMI settings.
        3. Perform a shutdown under the OS.
        4. Remove the AC power cord after the OS shutdown is complete.
        5. Reconnect the AC power cord and wait a few minutes before turning on the system (DC ON).
        6. After leaving the BIOS stage, the BMC should be able to regain the network connection through the Shared LAN.

Protection maps:
    H13DSG_O    BitMap-20220623-160757-MPS.bin
    H13DSH      BitMap-20221128-184047-MPS.bin
    H13SSL_N    BitMap-20221128-184047-MPS.bin
    H13SST_G    BitMap-20221128-184047-MPS.bin
    H13SSW      BitMap-20221128-184047-MPS.bin
