IPMI Firmware Release Note
----------------------------
Filename:	SMT_257.bin	ver2.57 Date: 03-18-2013

1. [H8SME] Remove -12V, Fan2~Fan5 sensor reading (IssueID: 44388)

======================================================================================
Filename:	SMT_256.bin	ver2.56 Date: 02-11-2013

1. [H8SME] 
	a. Add a feature of HDD detection 
	b. Fix the issue that mouse mode cannot be restored from IPMI configuration.
	c. Remove chassis intrusion monitoring.

======================================================================================

Filename:	SMT_255.bin	ver2.55 Date: 01-17-2013

1. Prevent user key in invalid data in SMTP page.

Note: Please clear web cache.

======================================================================================

Filename:	SMT_254.bin	ver2.54 Date: 12-21-2012

1. [H8SME] Add sensor support.

======================================================================================

Filename:	SMT_253.bin	ver2.53 Date: 11-27-2012

1. [H8SML] Fix the issue of sensor monitoring.
2. Fix the issue of IP address rention while VLAN is being initialized.

======================================================================================

Filename:	SMT_252.bin	ver2.52 Date: 07-30-2012

1. Add feature of Preservation of LAN setting while Restore To Defualt is performed.

======================================================================================

Filename:	SMT_251.bin	ver2.51 Date: 07-16-2012

1.Add Swiss Keyboad of KVM.

2. Fix Case# SM1112223242:
Issue: It cannot be login using Active Directory if Domain Controller Server Address 1 off-line.

======================================================================================

Filename:	SMT_250.bin	ver2.50 Date: 04-19-2012

1.Fix security issue: IPMIv2.0 Cipher 0 Authentication(no password) is not allowed
Validation: User can't log in BMC from commands with parameters "-I lanplus -C 0" 
Example: ipmitool -I lanplus -C 0 -U ADMIN mc info

2.Update new Web SOL due to the fix of JDK security method. Web SOL version 0.5.6
Validation: IPMI Web-> Remote Control-> SOL

3.Prevent clock change during firmware cold reset
Validation: 1. AC on/off test, and 2. cold reset test

4.Renew SSL certificate, validated from 04/11/12 to 04/11/14
Validation: IPMI Web-> Configuration-> SSL Certification

5.Fix AD Server authentication fail.

======================================================================================

Filename:	SMT_249.bin	ver2.49 
*** Skip this version due to confusion of merge of SMT_265.bin ***

======================================================================================

Filename:	SMT_248.bin	ver2.48 Date: 03-21-2012

*** Note: Factory Default required ***

Improved on IPMI SEL circular buffer for Total Event and Maximum Record ID 
Validation:
1. If the total event is over 512, it will delete 1 event and add 1 event, so the total event is always 512
2. The SEL record ID will reach until 65535 then go back to 1 (ipmitool sel elist)
3. Verify the display of Event ID in the web represent correctly the SEL record ID.

======================================================================================
Filename:	SMT_247.bin	ver2.47 Date: 02-27-2012

Increase upper threshold limit of CPU VCORE

======================================================================================

Filename:	SMT_SX_243.bin	ver2.43 Date: 12-06-2011

1. Fix set user privilege command through KCS
   Validation: 
	1. Create a new user by the below command flow:
	ipmitool user set name [id] [name]
	ipmitool user set password [id] [password]
	ipmitool user enable [id]
	ipmitool user priv [id] [priv] 1
	ipmitool channel setaccess 1 [id] callin=on ipmi=on link=on privilege=[priv]

	2. Log into IPMI web and check if privilege complaint with features

======================================================================================
Filename:	SMT_SX_242.bin	ver2.42 Date: 11-22-2011

1. Fix iKVM alive after the web session close
Validation: iKVM console should be timed out as web session close

======================================================================================
Filename:	SMT_241.bin	ver2.41 Date: 11-18-2011

1. Bug Fix Operator priviledge can't launch KVM through IPMI GUI
2. [H8DGU-LN4] Bug fix CPU Temp reading (IssueID: 33060) 

======================================================================================
Filename:	SMT_240.bin	ver2.40 Date: 11-11-2011

1. [H8DGT, H8DGU] Adjust VTT lower threshold to be 0.608(LNC), 0.584(LC) and 0.56(LNR)
Note: Memory can be either 1.35V or 1.5V

2. Allow Operator access UID control

3. Bug fix security issue on IPMI Configuration & KVM prview snapshot
Validation:
	IPMI Configuration is downloadable by User privilege:
		1) save config as Administrator, and then log out
		2) login as User
		3) save config by the link
		http://IP-OF-IPMI/cgi/url_redirect.cgi?url_name=save_config.bin&url_type=file

	KVM preview snapshot can be accessed without authentication
		http://IP-OF-IPMI/images/Snapshot.bmp

======================================================================================
Filename:	SMT_239.bin	ver2.39 Date: 11-02-2011
1. Bug fix for "Chassis Intrusion Reset" button not showing up when there is event triggered.

======================================================================================
Filename:	SMT_238.bin	ver2.38 Date: 10-27-2011
1. Bug fix Administrator's username visible to Operator privilege at IPMI Web

======================================================================================
Filename:	SMT_237.bin	ver2.37 Date: 10-11-2011

1. Allowed Operator full access to KVM, Mouse Mode, and Virtual Media
Validation: Operator should be able to change mouse mode, virtual media setting, and access KVM as well

2. Bug fix undefined "SMTP SSL Auth" from Web

======================================================================================
Filename:	SMT_236.bin	ver2.36 Date: 08-25-2011

1. [H8DCT-HIBQF/H8DCT-HLN4F] Remove Chassis Intrusion from SDR

======================================================================================
Filename:	SMT_235.bin	ver2.35 Date: 08-24-2011

1. Bug fix: firmware revision

======================================================================================
Filename:	SMT_235.bin	ver2.35 Date: 08-23-2011

1. Bug fix for discrete sensors reporting to applications (IssueID: 31173)
   Validation: 1) turn the system off, 2) check if any false alarm of chassis intrusion or power fail

2. Bug fix for H8DCT-HLN4F sensors not able to read

======================================================================================
Filename:	SMT_234.bin	ver2.34 Date: 08-18-2011

1. CPU Temp reports 0xff during system off for application to know the status(IssueID: 30876)
   Validation: check if IPMIView reports N/A during shutdown

2. Add new board ID for H8DCT-HLN4F(IssusID: 31064)

======================================================================================
Filename:	SMT_233.bin	ver2.33 Date: 07-14-2011

1. Bug fix Event Log description undefined from web GUI(IssusID: 30352, 30327 and 30295)
   Validation: Server Health-> Event Log

2. Bug fix Gateway IP lost
   Validation: change network setting from static to dhcp by using ipmitool or IPMICFG

3. Add iKVM privilege verification
   Validation: virtual media can't be accessed by Operator account

4. [H8DGG] add GPU models, M2090 & M2075 support

======================================================================================
Filename:	SMT_232.bin	ver2.32 Date: 06-22-2011

1. Bug fix Event Log description undefined from web GUI
   Validation: Server Health-> Event Log

2. Bug fix sensor status icon missing at webpage header
   Validation: summarized sensor status icon located at up-right corner of webpage

3. Bug fix unable to delete newly added Users (IssueID=29907)
4. Bug fix Alert Email description of CPU Overheat event (IssueID=29583)
5. Bug fix SMASH login without password

======================================================================================
Filename:	SMT_231.bin	ver2.31 Date: 06-02-2011

1. [H8DCT] Added Chassis Intrusion status monitoring(IssueID=29556)
   Description: View chassis intrusion status at IPMI Web-> Server Health-> Sensor Reading

2. Support Circular Buffer evnet logs
   Description: Event logged as FIFO mechanism when number of logs exceeds the maximum fixed-size, 512

3. Support IP Control
   Validation: Verify IP Control feature at IPMI Web-> Configuration-> IP Control

======================================================================================
Filename:	SMT_230.bin	ver2.30 Date: 05-26-2011

1. Add "All Event" category as default selection at Event Log page

2. Renew SSL Certificate
Validation:	1) enter Web GUI->Configuration->SSL Certificate, and 2) verify the certificate's validity
*** Note:	Factory Default REQUIRED

3. [H8DGG] Display Chassis Intrusion at Sensor information page

======================================================================================
Filename: SMT_229.bin ver2.29 Date: 05-12-2011

1. New feature: launch SOL over SMASH
	Validation: 1) login IPMI SMASH through SSH, 2) follow the command flow: cd system1 -> cd sol1 -> start
	Note: only one SOL session can be launched at a time.

2. Improve security for IPMI Configuration backup
	Validation: Verify the following steps:
		1) open IPMI web 
		2) click on Maintenance -> IPMI Configuration 
		3) save IPMI configuration at local drive, and 
		4) check if the configuration can "NOT" be located at http://ipmi-ip-address/save_config.bin

======================================================================================
Filename: SMT_228.bin ver2.28 Date: 05-02-2011

1. [X8DTL, X8DTN+, X8DTU-6TF, X8DTU-LN4F]  Correct DIMM Temp threshold to 75, 80 and 85 degree C
2. [H8DGG] Fix GPU fan control issue (rev2.22 to rev2.27)

======================================================================================
Filename: SMT_227.bin ver2.27 Date: 03-29-2011

1. [X8SII/X8SIE/X8SI6/X8SIT/X7SPA/X7SPE] Remove Thermal Trip event log to prevent false alarm

2. Modify default FRU
Description:Board Manufacture modified as "Supermicro" and all other entries cleared
Note:		Required OEM command raw 0x30 0x41(wait for BMC reset) to replace with the new FRU content

======================================================================================
Filename: SMT_226.bin ver2.26 Date: 03-18-2011

1. Fix Alert table blank at the webpage when enter more than 29 characters (IssueID: 95761)
   Validation:	1. Connect to IPMI by web browser,
		2. Go to Configuration -> Alerts and select one entry for modify,
		3. In the Message space, enter 30 characters and then save it and then the alert table will be blank.

2. H8SCM: Support thermal trip event logs (IssueID=26744) 

3. H8SCM, H8DCT, H8DCL: Change CPU vcore threshold to 1.448 for CPU max vcore over 1.2V (IssueID=27374) 

======================================================================================
Filename: SMT_225.bin ver2.25 Date: 03-011-2011

1. X7SPA/X7SPE: Remove thermal trip events since gpio signal is unstable
2. Removed Air/VRD/NB Temp senors

======================================================================================
Filename: SMT_224.bin ver2.24 Date: 03-07-2011

1. H8DCL: Added Chassis Intrusion status monitoring(IssueID=27711)
   Description: View chassis intrusion status at IPMI Web-> Server Health-> Sensor Reading

2. H8DCT: Fixed CPU Temp reading shows wrong information (IssueID=27791)
   Validation: Check if the reading is changed accordingly to the real temperture   

======================================================================================
Filename: SMT_223.bin ver2.23 Date: 02-23-2011

1. H8DGU-LN4, H8DGT, H8DGU, X8DTU, X8SIU, X8DTN+, X8DTU-6TF, X8DTL-i/6F, X8DTT, H8DCT, H8DCL:
   Fix CPU Temp Overheat event log missing

2. New feature: Port Configuratioin at Web GUI in Configuration category
   Description: ports of web, web SSL, IKVM server, virtual media are modifiable through web GUI

3. Fix Gateway setting can't work through different subnets 

======================================================================================
Filename: SMT_222.bin ver2.22 Date: 02-09-2011

1. Correct ID for new motherboard support X8SIL-SIOM

2. Fix cpu temp "Overheat" logged when the reading reports "High"
   Description: CPU temp Overheat should be logged as the reading reaches "Overheat"

3. For security issue, set the privilege of user ID1(Anonymous) with no access and clear jnlp kvm cache
   Validation: 	1. open IPMI web, 2 click Configuration->Users, and 3 check the privilege of user shows Reserved;
		4. launch kvm console, and 5. check if kvm jnlp file is cached after exit

======================================================================================
Filename: SMT_221.bin ver2.21 Date: 02-01-2011

1. Add new motherboard support X8SIL-SIOM
2. Add new motherboard support H8DCL

======================================================================================
Filename: SMT_V220.bin ver2.20 Date: 01-11-2011

1. H8DGG: Add slot 4 M1060/M2050/M2070/M2070Q GPU support (fan speed control, shutdown and slowdown)
2. Fix KVM slight flashes of white space while screen resolustion is below 800*640

======================================================================================
Filename: SMT_V219.bin ver2.19 Date: 12-31-2010

1. H8DCT: remove VRD1 & VRD2 sensor items.
2. Fix uninstalled fans report lower threshold events while doing system reset
3. Fix lan1 lost connection issue while doing ipmi cold reset

======================================================================================
Filename: SMT_218.bin ver2.18 Date: 12-17-2010

1. X9SCL/X9SCM: modify Fan5 to FanA
2. X7SPT/X7SPA/X7SPE: fix wrong CPU Temp reading


======================================================================================

Filename: SMT_217.bin ver2.17 Date: 12-10-2010

1. H8SCM: Removed Fan6 sensor entry

======================================================================================

Filename: SMT_216.bin ver2.16 Date: 12-06-2010

1. Add new motherboard X7SPT support

======================================================================================
Filename: SMT_215.bin ver2.15 Date: 11-24-2010

1. Bug fix on Lan1 issue

======================================================================================
Filename: SMT_214.bin ver2.14 Date: 11-12-2010

1. Fix the screen splash or blank screen when doing the cold reset
Description: please do AC on/off after firmware update. 

======================================================================================
Filename: SMT_213.bin ver2.13 Date: 11-10-2010

1. Add new SSID for X9SCM
2. Fix incorrect sensor readings

======================================================================================
Filename: SMT_212.bin ver2.12 Date: 10-25-2010

1. Add new motherboard X9SCL/X9SCM support
2. H8DCT: Bug fix Fan3 speed is monitored  

======================================================================================

Filename: SMT_211.bin ver2.11 Date: 10-19-2010

1. Fixed Virtual Media can't mount hidden files

Description: VM should be able to mount hidden files with a dollar sign in the share like "\share$\dvdimage.iso"

======================================================================================


Filename: SMT_210.bin ver2.10 Date: 10-13-2010	***CPU clock fixed at 180MHz***

1. CPU clock fixed at 180MHz 
2. X8DGG: Added device ID for GPU models, M2070 & M2070Q
Description: GPU temperature are readable for new models. 


======================================================================================

Filename: SMT_208.bin ver2.08 Date: 09-29-2010

1. Update on ECC error event logs
2. Add support for the BIOS to set different ACPI state (S0: system on, S1: sleep, S3: hypernate and S5: system off)
3. H8DGU(Appro): change lower thresholds of CPU Vcore & CPU DIMM VTT to fix the problem when 1.35v 8GB memory installed.
	Note: CPU Vcore:  0.736(NR), 0.744(CT), 0.752(NC) and CPU DIMM VTT: 0.584(NR), 0.592(CT), 0.6(NC).
4. Correct entity IDs in SDR
5. H8DGT/H8SGL/H8SCM/H8DGU-LN4: modify upper thresholds of NB Temp to 90(NC), 100(CT) and 110(NR) degree c
6. H8DGG: Remove sensors of GPU3 & GPU4 temp
7. Add new motherboard H8DCT support

======================================================================================

Filename: SMT_207.bin ver2.07 Date: 09-15-2010

For X8SIL/X8SIE/X8SII/X8SIA/X8SIU:
1. Adjust lower thresholds of fan speed to 215, 400 and 585(rpm)
2. Adjust upper thretholds of -12v to -10.934, -10.74 and -10.546(volts) 

======================================================================================
Filename: SMT2_206.bin ver2.06 Date: 09-08-2010

Bug fixes:
1. CPU clock follows hardware strapping 
(to fix BMC crash by DDR using Winbond instead of Hynix chip) 

======================================================================================
Filename: SMT_206.bin ver2.06 Date: 09-03-2010

Bug fixes:
1. X8SIT: Fix event log cannot catch CPU thermal trip event log 
(issueID=24349) and modify sensor system temperature to read 
from RT1: Bank 2, Reg.50
2. H8DGU-LN4+: Fix sensor CPU temperature does not show medium/high 
(IssueID=24950)
3. H8DGT-HF: Modify bootloader to fix memory corrupted at production (Ferrari Project)


======================================================================================
Filename: SMT_205.bin ver2.05 Date: 08-27-2010

Bug fixes:
1. X7SPA: Modify sensor name "Vnbcore" to "Vichcore"
2. H8DG6-F: Fix CPU temperature reports 'Low' eventhough 
CPU is overheating (issueID=24719) 
3. Fix SSH login with user/password: ADMIN/C0rbisSMAdmin 


======================================================================================
Filename: SMT_204.bin ver2.04 Date: 08-13-2010

Bug fixes:
1. X8SIL/X8SIE/X8SIA/X8SIU: Modify system temperature to read 
from RT1: Bank 2, Reg.50 (issueID=24254) 
2. Add Daylight Saving Time in web gui: Configuration->Date & Time
3. H8DGG-QF: Support Fermi GPU M2050 which can slowdown and 
shutdown GPU when overheat 


======================================================================================
Filename: SMT_203_0805.bin  ver2.03  Date: 08-05-2010

Bug fixes:
1. X8DTU-6F+: Add 100ms delay for sensor polling to fix issue
wrong sensor readings on SD3 client after overnight stress test (issueID=23803)


======================================================================================
Filename: SMT_203_0803.bin  ver2.03  Date: 08-03-2010

Bug fixes:
1. H8DG6: Remove GPU from sensor readings (issueID=24521)
2. X7SPE-HF-D525: Modify +12V sensor calculation 


=====================================================================================
Filename: SMT_202_0727.bin  ver2.02  Date: 07-27-2010

Bug fixes:
1. H8DGU-LN4F: set GPIO34 to high to fix BIOS hangs with 
post code '3E' or 'E1' (IssueID=24461)
2. Add SMTP sender's email (Web gui: Configuration -> SMTP)


=====================================================================================
Filename: SMT_201_0721.bin  ver2.01  Date: 07-21-2010

Bug fixes:
1. Fix Lan1 issue for all motherboards with Hartwell (82574) LAN chip
Description: Cannot connect to BMC use onboard LAN1 after upgrade to new FW.
Validation: With default setting "failover" or default for non-dedicate LAN MB, 
BMC connect with LAN1, SUT in OS (WS2008R2, RH5.4, or RH5.5).  Please upgrade FW 
from previous release version to this new version using web GUI and check whether 
BMC can connect again after FW flashing.


=====================================================================================
Filename: SMT_200_0720.bin  ver2.00  Date: 07-20-2010

Bug fixes:
1. X8DTU-LN4F+: Add +1.1V sensor (issueID=24334)
2. X8DTU-F: Add sensor CPU1 DIMM and CPU2 DIMM (issueID=24269)
3. X7SPA/X7SPE: Rename sensor name "1.05V" to "Vnbcore" to sync with BIOS
(issueID=23092)

