X13SEW Release Note
==================================================================================================================================
 CPU Microcode                                           | Option ROM/uEFi driver                   | Intel RC/LT-SX/ME
----------------------------------------------------------------------------------------------------------------------------------
 CPUID Family                                            | Aspeed Graphic Legacy : 1.13.01          | RC Version : 1752.P05
 806F8 Intel(R) Processor SPR E-Stepping     : 2B000590  | Aspeed Graphic UEFI   : 1.13.01          | SPS        : 6.1.4.5
 806F8 Intel(R) Processor SPR HBM B-Stepping : 2C000360  | Intel VROC UEFI       : 8.5.0.1096       | BIOS ACM   : 20230913 (1.1.9)
 C06F2 Intel(R) Processor EMR A-Stepping     : 21000200  |                                          | SINIT ACM  : 20230913 (1.1.9)
==================================================================================================================================
 BIOS feature               | Support
----------------------------------------------------------------------------------------------------------------------------------
 OOB Flash BIOS             | Y
 OOB Update Setting         | Y
 OOB Change SMBIOS          | Y
 InBand Flash BIOS          | Y
 InBand Update Setting      | Y
 InBand Change SMBIOS       | Y
 InBand SMI E7h supported   | N
 InBand SMI D9h supported   | Y
 Firmware Authentication    | Y
----------------------------------------------------------------------------------------------------------------------------------
 SW ECO Caused By           | Status
----------------------------------------------------------------------------------------------------------------------------------
 BIOS/IPMI Customization    | N
 HW Vendor Updates          | Y
 BIOS/IPMI Workaround       | N
 BIOS/IPMI Vendor Updates   | Y
 BIOS/IPMI Enhancements     | Y
 BIOS/IPMI Bug fixes        | Y
==================================================================================================================================
 BIOS              : BIOS_X13SEW-1D3E_20240330_2.2_STDsp.bin  | Release Date        : 03/30/2024
 BIOS Revision     : 2.2                                      | BIOS Engineer       : Brown Wang
 IPMI Revision     : 51.2.6.1                                 | SVN Revision        : 3485
 FW Global Version : 0000h                                    | ROT AntiRollback ID : 1004h
 BIOS Checksum     : 463EDDB3h
 BIOS Change:

1. [Enhancements] Update kernel to AMI label 101 (Intel WW05 BKC - MR1).
    Description : Update kernel to AMI label 101 (Intel WW05 BKC - MR1).
                  RC 1752.P05
                             15014627868 : ReDisable KTI L0P status for EMR all Stepping
                             15014608608 : Revert "[EMR][SGX] - SIDE - Add recovery mechanism with Auto option"
                             15014599254 : EMR Seamless BIOS update failed, system will hang after reboot.
                  [High]     15014593399 : Revert previous pull request "Remove "PKGC SREF EN" setup knob".
                  [High]     15014543749 : Remove PKGC SREF EN setup knob for EMR and SPR.
                  [Low]      14020455393 : Update to version 3 of GPU log to the BIOS dumps for errors
    Validation  : System boots successfully.

2. [Enhancements] Correct BMC FW version display on BIOS setup.
    Description : OpneBMC FW version is 4 bytes. Update BMC FW version display porting to support OpneBMC FW.
    Validation  : BMC FW version displays correctly on BIOS setup.

3. [Enhancements] Expose "Directory Mode Enable" on BIOS setup for CXL type 3 device.
    Description : Expose "Directory Mode Enable" on BIOS setup for CXL type 3 device.
    Validation  : Observe "Directory Mode Enable" on BIOS setup.

4. [Enhancements] Update EDK2 NetworkPkg for AMI SA50218.
    Description : Address EDK2 NetworkPkg vulnerability (PixieFail VU#132380).
                  1. CEV-2023-45229/CWE-125 (6.5, Medium) Out-of-bounds read when processing IA_NA/IA_TA options
                  in a DHCPv6 Advertise message.

                  2. CEV-2023-45230/CWE-119 (8.3, High) Buffer overflow in the DHCPv6 client via a long Server ID option.

                  3. CEV-2023-45231/CWE-125 (6.5, Medium) Out-of-bounds read when handling a ND Redirect message
                  with truncated option.

                  4. CEV-2023-45232/CWE-835 (6.5, Medium) Infinite loop when parsing unknown options
                  in the Destination Options header.

                  5. CEV-2023-45233/CWE-835 (6.5, Medium) Infinite loop when parsing a PadN  options
                  in the Destination Options header.

                  6. CEV-2023-45234/CWE-119 (8.3, High) Buffer overflow when processing DNSServers option
                  in a DHCPv6 Advertise message.

                  7. CEV-2023-45235/CWE-119 (8.3, High) Buffer overflow when handling Server ID option
                  from a DHCPv6 proxy Advertis
    Validation  : System boots successfully.

5. [Enhancements] Update AMITSE module for AMI SA50230.
    Description : Address image parser corruption vulnerability (7.5, High).
    Validation  : System boots successfully.

6. [Enhancements] Update AMITSE module for AMI SA50216.
    Description : Address LogoFAIL vulnerability.
                  1. CVE-2023-39538 (7.5, High).
                  2. CVE-2023-39539 (7.5, High).
    Validation  : System boots successfully.

7. [Fixes] Disable NMI generation of GPIO E7 as default and enable it after EndOfDxe event is signaled.
    Description : Prevent NMI generation is triggered by BMC randomly during memory initialization.
    Validation  : 1. Use IPMI tool to trigger NMI generation during memory initialization. Exception dose not happen.
                  2. Use IPMI tool to trigger NMI generation on BIOS setup. Exception happens.
                  3. Exception dose not happen during CBurn 300 cycles.

8. [Enhancements] Disable USB connection status event.
    Description : USB connection status event sends SELs repeatedly during power cycle.
                  Disable it to prevent unnecssary concern.
    Validation  : 1. Shutdown system.
                  2. Clear SEL.
                  3. Power on system to BIOS setup.
                  4. Observe no SEL is similar with below.
                     | 12/13/23 | 14:03:00 TST | Slot / Connector #0x80 | Device Present | Asserted

9. [Enhancements] Disable inlet temperature reading.
    Description : Inlet temperature sensor is not supported. Disable it to prevent incorrect SEL.
    Validation  : 1. Use Intel FIT to open BIOS image.
                  2. Observe inlet temperature reading is disabled.

----------------------------------------------------------------------------------------------------------------------------------
 BIOS              : BIOS_X13SEW-1D3E_20240130_2.1_STDsp.bin  | Release Date        : 01/30/2024
 BIOS Revision     : 2.1                                      | BIOS Engineer       : Brown Wang
 IPMI Revision     : 51.2.6.1                                 | SVN Revision        : 3379
 FW Global Version : 0000h                                    | ROT AntiRollback ID : 1004h
 BIOS Checksum     : A520643Fh
 BIOS Change:

1. First Release.
