
**** PLDM Firmware Package Header BEGIN ****

**** Package Header information ****
Package Header Identifier           : f018878ccb7d49439800a02f059aca02
Package Header format version       : v1.0.1
Package Header Size                 : 441 bytes
Package Release date time           : 2024-08-13 04:05:37.000000 UTC +0 minutes (UTC resolution: UTCunspecified, Time resolution: microsecond)
Component Bitmap Bit Length         : 8
Package Version string type         : ASCII
Package Version String Length       : 11 bytes
Package Version String              : 01.24.12.08

**** Firmware Device Identification Area ****
Device ID Record Count              : 1

** Firmware Device ID Record 1 **
Record Length                       : 89
Descriptor Count                    : 6
Device Update OP Flags              : 0: Default
Component Image Set Version Str Type: ASCII
Component Image Set Version Str Len : 25 bytes
FW Device Package Data Length       : 0 bytes
Applicable Components               : 0xff
Component Image Set Version String  : AMD_MI300X_01.24.12.08.76

Initial Descriptor Type             : PCI Vendor ID
Initial Descriptor Length           : 2 bytes
Initial Descriptor Data             : 1002

Additional Descriptor Type          : IANA Enterprise ID
Additional Descriptor Length        : 4 bytes
Additional Descriptor Data          : 00000e78

Additional Descriptor Type          : UUID
Additional Descriptor Length        : 16 bytes
Additional Descriptor Data          : 4c6d071a420456beee111c45d6c3bc9d

Additional Descriptor Type          : PCI Device ID
Additional Descriptor Length        : 2 bytes
Additional Descriptor Data          : 74a1

Additional Descriptor Type          : PCI Subsystem Vendor ID
Additional Descriptor Length        : 2 bytes
Additional Descriptor Data          : 1002

Additional Descriptor Type          : PCI Subsystem ID
Additional Descriptor Length        : 2 bytes
Additional Descriptor Data          : 74a1


** Component Image Information Area **
Component Image Count               : 8

** Component 1 Image Information **
Component Classification            : Firmware
Component Identifier                : 0x104
Component Comparison Stamp          : 0xffffffff
Component Options                   : Default
Requested Component Act. Method     : System Reboot/ DC power cycle
Component Size                      : 1418 bytes
Component Version String Type       : ASCII
Component Version String Length     : 8 bytes
Component Version String            : APCFG_v1

** Component 2 Image Information **
Component Classification            : Firmware
Component Identifier                : 0x500
Component Comparison Stamp          : 0xffffffff
Component Options                   : Default
Requested Component Act. Method     : System Reboot/ DC power cycle
Component Size                      : 1634820 bytes
Component Version String Type       : ASCII
Component Version String Length     : 15 bytes
Component Version String            : IFWI_v272744088

** Component 3 Image Information **
Component Classification            : Firmware
Component Identifier                : 0x600
Component Comparison Stamp          : 0xffffffff
Component Options                   : Default
Requested Component Act. Method     : System Reboot/ DC power cycle
Component Size                      : 117614 bytes
Component Version String Type       : ASCII
Component Version String Length     : 17 bytes
Component Version String            : RETIMER_v33599564

** Component 4 Image Information **
Component Classification            : Firmware
Component Identifier                : 0x800
Component Comparison Stamp          : 0xffffffff
Component Options                   : Default
Requested Component Act. Method     : System Reboot/ DC power cycle
Component Size                      : 21384 bytes
Component Version String Type       : ASCII
Component Version String Length     : 12 bytes
Component Version String            : RM_v67108876

** Component 5 Image Information **
Component Classification            : Firmware
Component Identifier                : 0x1ff
Component Comparison Stamp          : 0xffffffff
Component Options                   : Default
Requested Component Act. Method     : System Reboot/ DC power cycle
Component Size                      : 114655 bytes
Component Version String Type       : ASCII
Component Version String Length     : 17 bytes
Component Version String            : ROT_PLDM_v7536640

** Component 6 Image Information **
Component Classification            : Firmware
Component Identifier                : 0x3ff
Component Comparison Stamp          : 0xffffffff
Component Options                   : Default
Requested Component Act. Method     : System Reboot/ DC power cycle
Component Size                      : 19706 bytes
Component Version String Type       : ASCII
Component Version String Length     : 21 bytes
Component Version String            : SMC_FPGA_PLDM_v155664

** Component 7 Image Information **
Component Classification            : Firmware
Component Identifier                : 0x200
Component Comparison Stamp          : 0xffffffff
Component Options                   : Default
Requested Component Act. Method     : System Reboot/ DC power cycle
Component Size                      : 37008389 bytes
Component Version String Type       : ASCII
Component Version String Length     : 16 bytes
Component Version String            : SMC_FW_v16793647

** Component 8 Image Information **
Component Classification            : Firmware
Component Identifier                : 0x400
Component Comparison Stamp          : 0xffffffff
Component Options                   : Default
Requested Component Act. Method     : System Reboot/ DC power cycle
Component Size                      : 338199 bytes
Component Version String Type       : ASCII
Component Version String Length     : 16 bytes
Component Version String            : UBB_FPGA_v155686

Package Header Checksum             : 0xc004e41c

**** PLDM Firmware Package Header END ****
