================================================================================
Supermicro System BIOS Update Package Operation Instructions
================================================================================

Please read this document in it before performing the system BIOS update.  
Please verify that your system meets the requirements.

********************************************************************************
This update package includes the following system software updates & utilities:

--- BIOS image ---

  BIOS          - BIOS_X13SCD-F-1D1B_20241018_2.0a_STDsp.bin             (REV 2.0a)

--- BIOS Update Tools ---

  afuefi.smc                (file for AFU)
  fdt.smc		       (Flash Descriptor Table for SMC jumper-free solution to adjust ME)
  Readme for AMI BIOS.txt   (AMI BIOS Readme file) 
  flash.nsh		    (Update Script)	
  X13SCD-F_BIOS_Package_Readme (This file)


--- Supported Products ---

  Supermicro Motherboards:
  X13SCD-F

  

*************************************************************************************
                                     Important notes
*************************************************************************************

1. The UEFI version of SUM tool will replace AMI AFU BIOS flash utility in X13 
motherboard BIOS.

2. Using AFU tool will end up with the BIOS corruption.  It should never be used!


*************************************************************************************
                       SYSTEM HARDWARE and FIRMWARE REQUIREMENTS
*************************************************************************************

<NONE>


*************************************************************************************
                                         Warning
*************************************************************************************

1. Do not interrupt, reboot or remove power from your system during the update.
   Doing so may cause the system failure.

2. If the software update fails, you may contact our RMA Department to have the BIOS/
   IPMI firmware chip reprogrammed.  This will require shipping the board to Supermicro
   for repair.  Please submit your RMA request at:
   http://www.supermicro.com/support/rma/.
