X12SPi-TF release note.
-------------------------------------------------------------------------------------------------------------------------------------------
 CPU Microcode                         | Option ROM/EFI driver                                       | Intel RC/TXT/ME
-------------------------------------------------------------------------------------------------------------------------------------------
 CPUID FAMILY                          | Aspeed VBIOS                : 1.11.03                       | RC Version : 30.P50
 606A4 IceLakeServer L0 : 0B000280     | Intel VROC Legacy           : 6.3.5.1003                    | SPS        : 4.4.4.702
 606A5 IceLakeServer C0 : 0C0002F0     | Intel VROC UEFI             : 8.6.0.1118                    | BIOS ACM   : 20240109 (1.3.7) 
 606A6 IceLakeServer D0 : 0D0003F5     | Intel PMEM UEFI             : 2.0.0.3887                    | SINIT ACM  : 20240109 (1.3.8)
------------------------------------------------------------------------------------------------------------------------------------------
 BIOS feature                          | Support
------------------------------------------------------------------------------------------------------------------------------------------
 OOB Flash BIOS                        | Y
 OOB Update Setting                    | Y
 OOB Change SMBIOS                     | Y
 InBand Flash BIOS                     | Y
 InBand Update Setting                 | Y
 InBand Change SMBIOS                  | Y
 InBand SMI E7h supported              | N
 InBand SMI D9h supported              | Y
 Hii to BMC supported                  | Y
 Firmware Authentication               | Y
------------------------------------------------------------------------------------------------------------------------------------------
 SW ECO Caused By                      | Status
------------------------------------------------------------------------------------------------------------------------------------------
 BIOS/IPMI Customization               | N
 HW Vendor Updates                     | Y
 BIOS/IPMI Workaround                  | N
 BIOS/IPMI Vendor Updates              | Y
 BIOS/IPMI Enhancements                | Y
 BIOS/IPMI Bug fixes                   | Y
------------------------------------------------------------------------------------------------------------------------------------------
BIOS              : BIOS_X12SPI-1B4A_20241125_2.2_STDsp.bin         Release Date            : 11/25/2024
BIOS Revision     : 2.2                                             BIOS Engineer           : TC Lin
IPMI Revision     : 1.1.46                                          SVN Revision            : 5851
FW Global Version : 00000h                                          ROT AntiRollback ID     : 01004h
BIOS Checksum     : DC916BFCh
BIOS Change:

1. [Enhancements] Update BIOS version to 2.2.
    Description : Update BIOS revision.
    Validation  : Check BIOS revision is corrected in BIOS setup.

2. [Enhancements] Update kernel to 5.22_WhitleyCrb_0ACMS_ICX_081 (2025.1 IPU PV).
    Description : For INTEL-SA-01039 Security Advisory to address CVE-2023-43758(8.2, High), CVE-2023-34440(7.5, High), CVE-2024-24582(7.5, High), 
                  CVE-2024-29214(7.5, High), CVE-2024-28127(7.5, High), CVE-2024-39279(6.5, Medium), CVE-2024-31157(5.3, Medium) and 
                  CVE-2024-28047(5.3, Medium) security issures.
                  For INTEL-SA-01213 Security Advisory to address CVE-2024-36293(6.5, Medium) security issure.
                  RC 30.P50
                  [N/A]      05b5498: Locked MMIO Access from VM Guest Causes Host Hang.
                  [N/A]      89dd875: Improper Input Validation may result in GenericTerm.
                  [N/A]      098e8be: Locked MMIO Access from VM Guest Causes Host Hang.
                  [N/A]      656e7c1: Improper Input Validation may result in GenericTerm.
                  [N/A]      e1c81d0: BIOS should remove invalid PPR entry even when coldfast boot is disabled.
                  [N/A]      8488eee: ServerSiliconPkg/Mem/Library/MemCpgcIpLib: GenericTerm failing DIMM
                             cannot be detected by type 16 and can be detected by AMT 13,14,15 of EWL type 4.
                  [Low]      eeca41b: Enhanced Advanced MemTest pattern for DDR4 (Type 17.
                  [N/A]      495260e: Update RP _DSM to return BDF number of device detect eDPC.
                  [Low]      744f5b8: IPU 2024.3 PV Whitley: Remove VMDDxeEfi.depex from IPClean CI build.
    Validation  : Use RU.efi to check Bus<0x7E>/<0xFE>/Device<0x00>/Function<0x02>/Reg<0x90> for RC version.

3. [Enhancements] Update Dx/Mx microcode M87606A6_0D0003F5 for IPU 2025.1.
    Description : Update Dx/Mx microcode M87606A6_0D0003F5 for IPU 2025.1.
                  For INTEL-SA-01039 Security Advisory to address CVE-2023-43758(8.2, High), CVE-2023-34440(7.5, High), CVE-2024-24582(7.5, High), 
                  CVE-2024-29214(7.5, High), CVE-2024-28127(7.5, High), CVE-2024-39279(6.5, Medium), CVE-2024-31157(5.3, Medium) and 
                  CVE-2024-28047(5.3, Medium) security issures.
                  For INTEL-SA-01153 Security Advisory to address CVE-2024-28956(5.6, Medium) security issue.
                  For INTEL-SA-01213 Security Advisory to address CVE-2024-36293(6.5, Medium) security issure.
    Validation  : Plugged Dx/Mx stepping CPU and enter setup to check microcode revision is M87606A6_0D0003F5.	

4. [Enhancements] Updated Intel Server Platform Services for Whitley Server Platforms IPU2023.3 4.4.4.702. 
    Description : For INTEL-SA-01039 Security Advisory to address CVE-2023-43758(8.2, High), CVE-2023-34440(7.5, High), CVE-2024-24582(7.5, High), 
                  CVE-2024-29214(7.5, High), CVE-2024-28127(7.5, High), CVE-2024-39279(6.5, Medium), CVE-2024-31157(5.3, Medium) and 
                  CVE-2024-28047(5.3, Medium) security issures.
                  For INTEL-SA-01209 Security Advisory to address CVE-2024-TBD(6.5, Medium)) security issue.
                  For INTEL-SA-01213 Security Advisory to address CVE-2024-36293(6.5, Medium) security issure.
    Validation  : Enter Setup menu to check the SPS revision is 4.4.4.702 and current state is operational.

------------------------------------------------------------------------------------------------------------------------------------------
BIOS              : BIOS_X12SPI-1B4A_20240722_2.1_STDsp.bin         Release Date            : 07/22/2024
BIOS Revision     : 2.1                                             BIOS Engineer           : TC Lin
IPMI Revision     : 1.1.46                                          SVN Revision            : 5707
FW Global Version : 00000h                                          ROT AntiRollback ID     : 01004h
BIOS Checksum     : 0E062E56h
BIOS Change:

1. [Enhancements] Update BIOS version to 2.1.
    Description : Update BIOS revision.
    Validation  : Check BIOS revision is corrected in BIOS setup.

2. [Enhancements] Update kernel to 5.22_WhitleyCrb_0ACMS_ICX_079 (2024.3 IPU).
    Description : Update kernel to 5.22_WhitleyCrb_0ACMS_ICX_079 (2024.3 IPU).
    Validation  : 1. System boots successfully.
                  2. Pass FW revision check.
                  RC 30.P47
                  [N/A]      14021394982: Ensure SWSMI gets reinstataed before exiting the function.
                  [Medium]   22019333705: [Customer_MiscVendor][PTK3339][Whitley][ICX] SGX Registration.
                  [Medium]   14021363729: Sgx Registration Protocol Shall introduce user.
                  [N/A]      14020949231: Save/Restore Software SMI during TXT.
                  [Medium]   22018932124: [ICX]Sgx Registration Protocol Shall introduce user controlled read-only mode.
                  [N/A]      14021389121: Revert "Fix support for SMM in IIO API library".
                  [N/A]      18034465998: Fix support for SMM in IIO API library.
                  [High]     14021239042: Update AMT with test type 21 support.
                  [N/A]      14021238862: Fix for Renesas SPD WA DIMM present.
                  [N/A]      14021065827: AMT memtest type 18 not able to detect bad row but can be detected by memtest type 13.
                  [Medium]   14021070870: Advanced MemTest Test Type 20 for DDR4.
                  [N/A]      14021020464: MRC still communicates with PMEM even if the PMEM is disabled during late config.
                  [N/A]      14020092349: [IPU24.1][ICX][CPX]'Smarttest key' string unable to found in boot log after AMT TestType 16 implemented.
                  [N/A]      22019088009: Support RP IFWI generation without FlashImageTool.
                  [N/A]      14021117320: Memory latency abnormal because BIOS doesn't report correct NUMA status.
                  [N/A]      22018900142: Implement the NVRAM Variable checking scripts.
                  [N/A]      16023026057: ICX fix Hackathon Issue in UpdateVlsVariable.
                  [N/A]      15014975601: ICX fix Hackathon Issue in UpdateMirrorFailoverVariable.
                  [Medium]   14021145725: Revert "ICX fix Hackathon Issue in UpdateMirrorFailoverVariable".
                  [N/A]      14021033629: ADDDC Uncorrectable Spare Error is logged incorrectly.
                  [N/A]      22018918375: Check whether OOB MSM DFX exists before initializing OOB MSM DFX BAR0, since OOB MSM DFX doesn't exist in production environment.

3. [Enhancements] Rollback secure boot MS2026 KEK and DB to fix SGX registration failure issue.
    Description : Fix SGX registration failure issue.
    Validation  : 1. Full DIMM population, enabled Memory Encryption (TME) and SW Guard Extensions (SGX).
	              2. Make sure SGX registration successful.

4. [Enhancements] Apply AMI SA50235 for extended parser corruption correction.
    Description : Apply SA50235 for extended parser corruption correction.
    Validation  : System boots successfully.

5. [Enhancements] Apply AMI SA50232 to address predictable TCP initial sequence numbers.
                  1. CVE-2023-45236 Use of a Weak PseudoRandom Number Generator (Risk Level : 5.8).
                  2. CVE-2023-45237 Predictable TCP initial sequence numbers (ISNs) generated by the TCP/IP stack (Risk Level : 5.3).
    Description : Apply AMI SA50232 to address predictable TCP initial sequence numbers.
    Validation  : IPV4 PXE boot succeeds.

6. [Enhancements] For SA50243 (CVSS3.1 (7.5, High)) fix that UsbRtSmm module has a TOCTOU vulnerability.
    Description : Avoid that attacker exploit a timing window which leading to arbitrary code execution at the SMM level.
    Validation: : USB device works during boot and under OS.

7. [Enhancements] Patch for Mellanox InfiniBand Controller MAC Address issue.
    Description : Get Mellanox InfiniBand Controller MAC Address from the original VPD field 'V3'.
    Validation  : Make sure the SMBIOS type 40 displays the correct MAC address in the VPD data when CX6/CX7 switches to IB mode.

8. [Enhancements] Update Dx/Mx microcode M87606A6_0D0003E7 for IPU2024.3 Security Advisory.
                  For INTEL-SA-01071 Security Advisory to address CVE-2023-43758(8.2, High), CVE-2023-42772(8.2, High), CVE-2024-23599(7.9, High),
                  CVE-2023-41833(7.5, High), CVE-2023-34440(7.5, High), CVE-2024-21829(7.5, High), CVE-2023-43626(7.5, High), CVE-2024-21871(7.5, High), CVE-2024-21781(7.2, High),
                  CVE-2023-23904(6.1, Medium), CVE-2023-22351(6.1, Medium), CVE-2023-43753(5.3, Medium) and CVE-2023-25546(2.5, Low) security issues.
                  For INTEL-SA-01079 Security Advisory to address CVE-2024-21820(7.2, High) and CVE-2024-23918(8.8, High) security issue. 
                  For INTEL-SA-01083 Security Advisory to address CVE-2024-24853(7.2, High) security issue. 
                  For INTEL-SA-01097 Security Advisory to address CVE-2024-24968(5.3, Medium) security issue. 
                  For INTEL-SA-01100 Security Advisory to address CVE-2024-25980(6.1, Medium) security issue. 
                  For INTEL-SA-01103 Security Advisory to address CVE-2024-23984(5.3, Medium) security issue. 
                  For INTEL-SA-01118 Security Advisory to address CVE-2024-25939(6.0, Medium) security issue. 
    Description : Update Dx/Mx microcode M87606A6_0D0003E7 for IPU2024.3 Security Advisory.
                  For INTEL-SA-01071 Security Advisory to address CVE-2023-43758(8.2, High), CVE-2023-42772(8.2, High), CVE-2024-23599(7.9, High),
                  CVE-2023-41833(7.5, High), CVE-2023-34440(7.5, High), CVE-2024-21829(7.5, High), CVE-2023-43626(7.5, High), CVE-2024-21871(7.5, High), CVE-2024-21781(7.2, High),
                  CVE-2023-23904(6.1, Medium), CVE-2023-22351(6.1, Medium), CVE-2023-43753(5.3, Medium) and CVE-2023-25546(2.5, Low) security issues.
                  For INTEL-SA-01079 Security Advisory to address CVE-2024-21820(7.2, High) and CVE-2024-23918(8.8, High) security issue. 
                  For INTEL-SA-01083 Security Advisory to address CVE-2024-24853(7.2, High) security issue. 
                  For INTEL-SA-01097 Security Advisory to address CVE-2024-24968(5.3, Medium) security issue. 
                  For INTEL-SA-01100 Security Advisory to address CVE-2024-25980(6.1, Medium) security issue. 
                  For INTEL-SA-01103 Security Advisory to address CVE-2024-23984(5.3, Medium) security issue. 
                  For INTEL-SA-01118 Security Advisory to address CVE-2024-25939(6.0, Medium) security issue. 
    Validation  : Plugged Dx/Mx stepping CPU and enter setup to check microcode revision is M87606A6_0D0003E7.

------------------------------------------------------------------------------------------------------------------------------------------
BIOS              : BIOS_X12SPI-1B4A_20240108_1.9_STDsp.bin         Release Date            : 01/08/2024
BIOS Revision     : 1.9                                             BIOS Engineer           : TC Lin
IPMI Revision     : 1.1.46                                          SVN Revision            : 5461
FW Global Version : 00000h                                          ROT AntiRollback ID     : 01004h
BIOS Checksum     : 14467AD5h
BIOS Change:

1. [Enhancements] Update BIOS version to 1.9.
    Description : Update BIOS revision.
    Validation  : Check BIOS revision is corrected in BIOS setup.
	
2. [Enhancements] Update AMITSE module for AMI SA50216 Security Advisory(LogoFAIL Vulnerability) to address CVE-2023-39538(7.5, High) and CVE-2023-39539(7.5, High) security issues.
    Description : An attacker can exploit this vulnerability by flashing firmware containing a maliciously-crafted logo image and booting this system with the altered image. 
                  On devices vulnerable to LogoFAIL, attackers can supply custom logos and thus exploit any vulnerabilities in the image parser. This weakness affects a variety of image formats including GIF, PNG, BMP and JPEG.
    Validation  : System boots successfully.
	
3. [Enhancements] Expose item Pre-boot DMA Protection.
    Description : Support to configure OS security features of secured-core for Azure Stack HCI system.
    Validation  : Make sure item Pre-boot DMA Protection is exposed in Advanced => Chipset Configuration => North Bridge => IIO Configuration => Intel VT for Directed I/O (VT-d)

------------------------------------------------------------------------------------------------------------------------------------------
BIOS              : BIOS_X12SPI-1B4A_20231129_1.8_STDsp.bin         Release Date            : 11/29/2023
BIOS Revision     : 1.8                                             BIOS Engineer           : TC Lin
IPMI Revision     : 1.1.46                                          SVN Revision            : 5408
FW Global Version : 00000h                                          ROT AntiRollback ID     : 01004h
BIOS Checksum     : 170b1264h
BIOS Change:

1. [Enhancements] Update BIOS version to 1.8.
    Description : Update BIOS revision.
    Validation  : Check BIOS revision is corrected in BIOS setup.
	
2. [Enhancements] Update M87606A6_0D0003D1 microcode for Dx/Mx stepping CPU.
                  For INTEL-SA-00950 Security Advisory to address CVE-2023-23583(8.8, High) security issue.
                  For INTEL-SA-00960 Security Advisory to address CVE-2022-41804(6.1, Medium)security issue.
    Description : Update M87606A6_0D0003D1 microcode for Dx/Mx stepping CPU.
                  For INTEL-SA-00950 Security Advisory to address CVE-2023-23583(8.8, High) security issue.
                  For INTEL-SA-00960 Security Advisory to address CVE-2022-41804(6.1, Medium)security issue.	
    Validation  : Plugged Dx/Mx stepping CPU and enter setup to check microcode revision is M87606A6_0D0003D1.
	
3. [Enhancements] Update base to 5.22_WhitleyCrb_0ACMS_ICX_077 (2024.1 IPU-PV) for INTEL-SA-00960 Security Advisory to address CVE-2022-41804(6.1, Medium)security issue.
    Description : Update base to 5.22_WhitleyCrb_0ACMS_ICX_077 (2024.1 IPU-PV) for INTEL-SA-00960 Security Advisory to address CVE-2022-41804(6.1, Medium)security issue.
                  RC 30.P41
                  [Medium]   18029238669: Revert ”[PSIRT_PTK3339][Whitley][ICX] SGX Registration Protocol shall introduce user controlled ’read-only’ mode”.
                  [Low]      14019386021: Requests new Advanced MemTest Test Type 20 for DDR4.                  
                  [High]     16020901470: BIOS SHALL update the DFX SAI_PG of the memory controllers to mitigate security exploits.
                  [High]     15013443915: BIOS SHALL update the DFX SAI_PG of the memory controllers to mitigate security exploits.
                  [N/A]      14019800028: [ICX] PCIe Reporting (PCIe Error SMM Handler) doesn’t function correctly.
                  [Low]      14019385344: Add new pattern for memtest type 16 to strengthen the AMT PPR.
                  [N/A]      14019230848: Invalid DIMM SPD CRC Causes Fatal Error ( or Boot Loop and Inoperable System ).
                  [N/A]      14019253026: AMT Memtest type 17 report false failure when 8Gb and 16Gb know bad DIMMs are present.
                  [High]     22018309082: Remove FDBin/CryptoComponents from Whitley MinPlatform builds.
                  [High]     18030509126: [PSIRT_PTK3339][Whitley][ICX] SGX Registration Protocol shall introduce user controlled ’read-only’ mode.
                  [High]     18029869387: [ICX] SGX Support - BIOS shall implement ICX CPU BWG 0.50 - 1.8.5.10 Configure PRMRRs - also supporting dynamic PCIe MMCFG base (1GB-3GB).
                  [Medium]   22018341284: Retire Descriptor Tool in Gen1 Programs.
                  [Medium]   14019403457: Adding Manufacturer ID Codes for MiscVendor.
                  [N/A]      16020026738: [Whitley][MinPlat]CpuMpPei MpInitLibInitialize() (inside InitializeCpuMpWorker( )) occasionally takes one minute to execute.
                  [N/A]      16019943714: PCH PCI-E RAS error reporting only occurs 1st time but fail then.	
    Validation  : Use RU.efi to check Bus<0x7E>/<0xFE>/Device<0x00>/Function<0x02>/Reg<0x90> for RC version.
	
4. [Enhancements] Updated Intel Server Platform Services for Whitley Server Platforms IPU2024.1 4.4.4.603 for INTEL-SA-00960 Security Advisory to address CVE-2022-41804(6.1, Medium)security issue.
    Description : Updated Intel Server Platform Services for Whitley Server Platforms IPU2024.1 4.4.4.603 for INTEL-SA-00960 Security Advisory to address CVE-2022-41804(6.1, Medium)security issue.
    Validation  : Enter Setup menu to check the SPS revision is 4.4.4.603 and current state is operational.

------------------------------------------------------------------------------------------------------------------------------------------
BIOS              : BIOS_X12SPI-1B4A_20231012_1.7_STDsp.bin         Release Date            : 10/12/2023
BIOS Revision     : 1.7                                             BIOS Engineer           : TC Lin
IPMI Revision     : 1.1.46                                          SVN Revision            : 5298
FW Global Version : 00000h                                          ROT AntiRollback ID     : 01004h
BIOS Checksum     : 5022f252h
BIOS Change:

1. [Enhancements] Update BIOS version to 1.7.
    Description : Update BIOS revision.
    Validation  : Check BIOS revision is corrected in BIOS setup.

2. [Enhancements] Update Dx/Mx BETA microcode for IPU2023.4 Out of band for Intel-SA-00950.
    Description : Update M87606A6_0D0003B9 microcode for Dx/Mx stepping CPU for INTEL-SA-00950 Security Advisory to address CVE-2023-23583(8.8, High) security issue.  
    Validation  : Plugged Dx/Mx stepping CPU and enter setup to check microcode revision is M87606A6_0D0003B9.

------------------------------------------------------------------------------------------------------------------------------------------
BIOS              : BIOS_X12SPI-1B4A_20230818_1.6_STDsp.bin         Release Date            : 08/18/2023
BIOS Revision     : 1.6                                             BIOS Engineer           : Brown Wang
IPMI Revision     : 1.1.46                                          SVN Revision            : 5219
FW Global Version : 00000h                                          ROT AntiRollback ID     : 01004h
BIOS Checksum     : 625033E0h
BIOS Change:

1. [Enhancements] Update 5.22_WhitleyCrb_0ACMS_ICX_076_BETA (IPU-PV 2023.3).
   Description : Update 5.22_WhitleyCrb_0ACMS_ICX_076_BETA (IPU-PV 2023.3).
   Validation  : Normal BIOS and debugging BIOS can boot successfully.

2. [Fixes] Remove duplicated "ENERGY_PERF_BIAS_CFG Mode" HII data.
    Description : Remove duplicated "ENERGY_PERF_BIAS_CFG Mode" HII data.
    Validation  : 1. Boot to BIOS setup.
                  2. configure "Power Performance Tuning" to "BIOS contyols EPB".
		          3. Configure "ENERGY_PERF_BIAS_CFG Mode" to "Maximum Performance".
		          4. Save and exit.
                  5. Boot to UEFI shell.
		          5. Can use SUM to update BIOS with preserving BIOS configuration.


3. [Fixes] Resolve configured SMBIOS can not be preserved after clear CMOS.
    Description : Resolve configured SMBIOS can not be preserved after clear CMOS.
    Validation  : 1. Boot to UEFI shell.
                  2. Use SUM to configure SMBIOS.
                  2. Reset system and configured SMBIOS is preserved.
                  3. Remove all power including coin battery to clear CMOS.
                  4. Power on system and configured SMBIOS is preserved.

4. [Enhancements] Support VPD of card MCX562A-ACAB.
   Description : Support VPD of card MCX562A-ACAB.
   Validation  : Serial number of card MCX562A-ACAB is displayed in BMC WebUI.

5. [Enhancements] Add SEL (Sensor Type : 0xC3, Data1 : 0x06, Data2 : CPU Index, Data3 : UPI Index) for UPI (topology change) link degraded.
   Description : Add SEL (Sensor Type : 0xC3, Data1 : 0x06, Data2 : CPU Index, Data3 : UPI Index) for UPI (topology change) link degraded.
   Validation  : N/A.

6. [Enhancements] Update secure boot DBX.
   Description : Update secure boot DBX.
   Validation  : N/A.

7. [Fixes] Fix incorrect total memory size on setup if install 6 memory.
   Description : Fix incorrect total memory size on setup if install 6 memory.
   Validation  : Total memory size is correct on setup if install 6 memory.

8. [Fixes] Fix memory still is mapped out because of UECC even after AC cycle.
   Description : Fix memory still is mapped out because of UECC even after AC cycle.
   Validation  : 1. Inject memory UECC.
                 2. Boot to setup and observe memory is mapped out on setup.
                 3. Do AC cycle.
                 4. Boot to setup and observe memory is not mapped out on setup.
------------------------------------------------------------------------------------------------------------------------------------------
BIOS              : BIOS_X12SPI-1B4A_20230424_1.5_STDsp.bin         Release Date            : 04/24/2023
BIOS Revision     : 1.5                                             BIOS Engineer           : Brown Wang
IPMI Revision     : 1.1.38                                          SVN Revision            : 5006
FW Global Version : 00000h                                          ROT AntiRollback ID     : 01004h
BIOS Checksum     : 50a827beh
BIOS Change:

1. [Enhancements] Update 5.22_WhitleyCrb_0ACMS_ICX_075 Intel 2023.2 IPU-PV.
   Description : Update 5.22_WhitleyCrb_0ACMS_ICX_075 Intel 2023.2 IPU-PV.
   Validation  : 1. Build succeeds.
                 2. System boots to UEFI shell successfully.

2. [Enhancements] Improve variable interface for buffer overflow case in security erase module.
   Description : Improve variable interface for buffer overflow case in security erase module.
   Validation  : N/A.

3. [Enhancements] Add PCIE leaky bucket degradation SEL (Sensor Type 0x13 Data1 0xAB).
   Description : Add PCIE leaky bucket degradation SEL (Sensor Type 0x13 Data1 0xAB).
   Validation  : N/A.

4. [Enhancements] Improve VROC key detection.
   Description : VMD is not enabled after install new VROC key (VROCPREMMOD).
   Validation  : Ensure VMD is enabled after install any one of all VROC key.

5. [Enhancements] Boot option is not created for single hard drive under RAID mode.
   Description : Boot option is not created for single hard drive under RAID mode.    
   Validation  : 1. Use single hard drive under RAID mode to install Windows.
                 2. Ensure boot option for the hard drive is displayed in boot order on BIOS setup.

6. [Fixes] Fix system halts after configure MMCFG Base to 1.5G and 1.75G.
   Description : Fix system halt after configure MMCFG Base to 1.5G and 1.75G.
   Validation  : System boots successfully after configure MMCFG Base to 1.75G.

7. [Fixes] Fix ECO test case 2020 fails.
   Description : Fix ECO test case 2020 fails.
   Validation  : ECO test case 2020 passes.
------------------------------------------------------------------------------------------------------------------------------------------
BIOS              : BIOS_X12SPI-1B4A_20230109_1.4b_STDsp.bin         Release Date            : 01/09/2023
BIOS Revision     : 1.4b                                             BIOS Engineer           : Brown Wang
IPMI Revision     : 1.00.17                                          SVN Revision            : 4772
FW Global Version : 00000h                                           ROT AntiRollback ID     : 01004h
BIOS Checksum     : 0be02dafh
BIOS Change:

1. [Enhancements] Update 5.22_WhitleyCrb_0ACMS_ICX_74 (Intel BKC WW46 IPU2023.1).
    Description : Update Intel BKC WW46 IPU2023.1 for below issues.
                  RC:
                    INTEL-SA-00717 CVE-2022-32231(7.5 High).
                    Intel-SA-00738:CVE-2022-33196(7.2 High).
                    [Medium] 22015774648 Change RemainingSize variable to INT to account for negative cases.
                    [Medium] 22015758320 Remove DFX variable from Security Policy struct to keep size of NVRAM struct.
                    [Low] 22015699667 Branch for PLR3 OOB.
                    [High] 22015542982 SGX MSR Inconsistency on across BSP.
                    [High] 15011562344 Need BIOS Devhide CHAs of disabled LLC on ICX-SP.
                    [High] 16016328984 Enable ESPI SMI Lock.
                    [High] 14017158030 BIOS needs to program 0x0 into temp_halfxref register field for MCHECK consistency for DDR4 channels.
                    [High] 22015539623 DfxLinkRetrainEn w/a not checking endpoint capabilities before executing.
                    [Medium] 22015469479 IsDcpmmPresentChannel should check per DIMM DcpmmPresent field instead of per channel ddrtEnabled.
                    [Medium] 22014638461 Revert Block Decoder will not get mapped if DDR is mapped up to MMIOH.
                    [High] 14015886212 Need to remove the WA to force closed page mode when ADDDC enabled.
                    [Meduim] 22014923207 1DPC configuration fails to flag transaction fatal EWL when there is WBD flush failure.
                    [High] 22015049995 Cannot find PostPackageRepair info in serial log when inject UCE.
                    [Medium] 16015903381 128GB LRDIMM IS UNABLE TO BOOT with 2400MT/s speed.
                    [High] 15010878057 Smbus recovery failed on socket0 and succeeded on socket1 when Smbus errors occurred on different sockets.
                    [Medium] 18021347488 Poison injected at last 512 bytes of SPA range is not getting cleared by ndctl.
                    [High] 14016209068 Inject UCE into failling DIMM, the PPR will show the wrong nibblemask and drammask bios.mrc_server.
                    [Medium] 14016334192 DDR4 Advanced Memtest Code update for SK MiscVendor to V2.8.7.
                    [High] 22014878309 The latest Whitley CLTT MRC whitepaper (doc# 612245) sets SPD Config register 1, bit 0 to 0 (comparator mode).
                    [Medium] 14014886735 Reboot hang at post code 05.
                  Microcode:
                    Intel-SA-00700:CVE-2022-21216(7.5 High) Insufficient granularity of access control in out-of-band management in some Intel(R) 
                                                            Atom(R) and Intel(R) Xeon(R) Scalable Processors may allow a privileged user to potentially 
                                                            enable escalation of privilege via adjacent network access.
                    Intel-SA-00738:CVE-2022-33196(7.2 High) Incorrect default permissions in some memory controller configurations for some Intel(R) 
                                                            Xeon(R) Processors when using Intel(R) Software Guard Extensions which may allow a privileged
                                                            user to potentially enable escalation of privilege via local access.
                    INTEL-SA-00767:CVE-2022-38090(6.0 Medium) Improper isolation of shared resources in some IntelR Processors may allow a privileged user 
                                                              to potentially enable information disclosure via local access.
                   Microcode Update Minimum Runtime Update Revision
                   PCIe Link Width May Degrade
                   Intel SGX TCB Recovery Boot flow sighting
                   ICX Warm Reset High Current
                   INTEL-SA-00767:CVE-2022-33972(6.1 Medium) Incorrect calculation in microcode keying mechanism for some 3rd Generation IntelR Xeon(R) 
                                                             Scalable Processors may allow a privileged user to potentially enable information disclosure
                                                             via local access.
    Validation  : 1. Use PCI.exe to check Bus (0x7E/0xFE)/Device 0/Function 2/Register 0x90 for RC version.
                  2. Verify processor, memory and PMem under both of MM mode and AD mode.
                  3. Use IceLake-SP Dx/Mx or later stepping processor to Verify PCIe function.
                  4. Install RDIMM and PMem then execute memory stress test and margin test.

2. [Fixes] Fixe memory error is not reported in SMBIOS event log.
    Description : N/A
    Validation  : 1. Inject memory CE/UCE error.
                  2. Ensure log for memory CE/UCE error is in BMC SEL and SMBIOS event log.

3. [Fixes] Enable all boot option first for test case 220, 271, 356 and 457.
   Description : Enable all boot option first for test case 220, 271, 356 and 457.
   Validation  : verify test case 220, 271, 356 and 457.

4. [Fixes] Resolve abnormal SOL resolution.
    Description : Resolve abnormal SOL resolution.
    Validation  : Verify SOL display.

5. [Enhancements] Update SEL for processor error.
    Description : Follow IPMI SEL specification 1.36 to modify sensor type from 0x07 to 0xD4.
    Validation  : N/A.
------------------------------------------------------------------------------------------------------------------------------------------
BIOS          : X12SPI0.A07_Signed     Release Date  : 10/07/2020
BIOS Revision : 1.00                   BIOS Engineer : Jimmy Chiu
IPMI Revision : 10.49                  SVN Revision  : 2099
BIOS Checksum : F911DF3Bh
BIOS Change:

1. First release.
