Before you start flashing the BIOS, please Follow following steps to proceed with flashing:


a. Turn off system and unplug the power connector.
b. Set "JPME2" to Manufacturing Mode (pin 2-3). (JPME2 is a jumper on the mother board, please refer to user's manual or Quick Reference guide for its detailed location.)
c. Connect the power back to the system, and power on the system and boot to the bootable USB/CD/DVD media that contains the BIOS flash package.
d. To start flashing BIOS, from this step, refer to "Readme for AMI BIOS.txt" Step1~Step 6.
e. After the update finished, Turn Off the system.
f. Set "JPME2" to Normal Mode (pin 1-2) 
