================================================================================
Supermicro System BIOS & IPMI Firmware Update Package Operation Instructions
================================================================================

Please read this document in it before performing the system BIOS or IPMI
firmware update.  Please verify that your system meets the requirments.


********************************************************************************
This update package includes the following system software updates & utilities:

--- BIOS/IPMI Firmware Update Package ---

  BIOS          - BIOS_H13DSG-OM-1D2A_20250117_3.3_STDsp.zip                  (REV 3.3)
  IPMI Firmware - BMC_H13AST2600-ROT20-8501MS_20241213_01.03.40_STDsp.zip     (REV 01.03.40)


--- BIOS/Firmware Update Tools ---

 Supermicro Update Manager Utility (SUM)  v2.14.0 :
  sum_2.14.0-p8_Win_x86_64_20240904.zip            (for Windows)
  sum_2.14.0-p8_Linux_x86_64_20240904.tar.gz       (for Linux)
  sum_2.14.0-p8_BSD_x86_64_20240904.tar.gz         (for FreeBSD) 


  Note: For BIOS update with SUM utility through Out-Of-Band (OOB) channel, the
        SFT-OOB-LIC or SFT-DCMS-Single is no longer required.

--- Supported Products ---

  Supermicro Motherboards:
  MBD-H13DSG-OM
  


*************************************************************************************
                                     Important notes
*************************************************************************************

1. To support AMD EPYC Bergamo, Genoa X processor, please update to BIOS v1.9 or higher version.
2. For AMD EPYC 9005 Series Processor support, please ensure your motherboard revision is R2.0 or higher. 
The BIOS and BMC package versions should be BIOS V3.0 or higher and BMC V01.03.35 or higher.
Please note that if you would like to roll back the BIOS from V3.x (AMD EPYC 9004/9005 Series Processor) 
dual BIOS to V1.x (AMD EPYC 9004 Series Processor) single BIOS, make sure to install AMD EPYC 9004 Series Processor before updating the BIOS.

*************************************************************************************
                       SYSTEM HARDWARE and FIRMWARE REQUIREMENTS
*************************************************************************************

<NONE>


*************************************************************************************
                                         Warning
*************************************************************************************

1. Do not interrupt, reboot or remove power from your system during the update.
   Doing so may cause the system failure.

2. If the software update fails, you may contact our RMA Department to have the BIOS/
   IPMI firmware chip reprogrammed.  This will require shipping the board to Supermicro
   for repair.  Please submit your RMA request at:
   http://www.supermicro.com/support/rma/.
