===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20250125_01.00.17.00_STDsp.bin version: 01.00.17.00 Date: 25 Jan 2025
Programmer Filename: BMC_X14AST2600-ROT-5601MS_20241112_09.00.08.00_STDsp_programmer.bin version: 09.00.08.00 Date: 12 Nov 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
      [192409] Modify IPMI OEM cmd compatible BIOS setup menu/SMCIPMITool Stateless/Stateful mode

    Impacted motherboard:
        ALL
    Affected functions:
        N/A
    Validation:
        1. Factory Default and Get data "Stateless(0), autonconfig ON(1) and SLAAC address"
                ipmi lan ipv6 mode
                ipmi lan ipv6 autoconfig
                ipmi lan ipv6 list

        2. Set IPv6 mode to "Stateful(1)", Get data "Stateful(1), autonconfig ON(1), DHCPv6 and SLAAC address"
                ipmi lan ipv6 mode 1
                ipmi lan ipv6 mode
                ipmi lan ipv6 autoconfig
                ipmi lan ipv6 list

        3. Set IPv6 mode to "Disabled(2)", Get data "Disabled(2), autonconfig OFF(0)"
                ipmi lan ipv6 mode 2
                ipmi lan ipv6 mode
                ipmi lan ipv6 autoconfig
                ipmi lan ipv6 list

        4. Set IPv6 mode to "Stateless(0)", Get data "Stateless(0), autonconfig ON(1) and SLAAC address"
                ipmi lan ipv6 mode 0
                ipmi lan ipv6 mode
                ipmi lan ipv6 autoconfig
                ipmi lan ipv6 list

2.
    Category: Fix
    Description:
      [191904][SYS-622B-TRT]BMC Web GUI will not display BPN CPLD FW update option.

    Impacted motherboard:
        ALL
    Affected functions:
        N/A
    Validation:
      1. Check Storage FW from Web (BPN-NVMe5-826N-B2B,  BPN-SAS4-825A-N4)

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20250120_01.00.16.00_STDsp.bin version: 01.00.16.00 Date: 20 Jan 2025
Programmer Filename: BMC_X14AST2600-ROT-5601MS_20241112_09.00.08.00_STDsp_programmer.bin version: 09.00.08.00 Date: 12 Nov 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
      [194020] [SYS-112B_522B-WR] "Intrusion Reset" buttom is missing under BMC webUI when triggering chassis intrusion sensor.
        
    Impacted motherboard:
        X14SBW-F
    Affected functions:
        N/A
    Validation:
        1. Check "Intrusion Reset" when chassis sensor is red

2.
    Category: Fix
    Description:
      [190832] [IPMI ECO 01.00.08.00] Redfish Automation Tool check fail.
       
    Impacted motherboard:
        X14SBW-F
    Affected functions:
        N/A
    Validation:
        1. Verify with Redfish SATC

3.
    Category: Fix
    Description:
      [193001] Cannot show the IP when use network AOC card change to shared lan/failover
       
    Impacted motherboard:
        X14SBW-F
    Affected functions:
        N/A
    Validation:
        1. Verify lan mode change

4.
    Category: Fix
    Description:
      [192723] 	[ECO BMC 01.00.03.01]Try to share lan function it needs power off the system then BMC IP can be recovered.
       
    Impacted motherboard:
        X14SBW-F
    Affected functions:
        N/A
    Validation:
        1. Verify Lan funciton


===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20250110_01.00.15.00_STDsp.bin version: 01.00.15.00 Date: 10 Jan 2025
Programmer Filename: BMC_X14AST2600-ROT-5601MS_20241112_09.00.08.00_STDsp_programmer.bin version: 09.00.08.00 Date: 12 Nov 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        [190832] [IPMI ECO 01.00.08.00] Redfish Automation Tool check fail.
    Impacted motherboard:
        X14SBW-F
    Affected functions:
        N/A
    Validation:
        1. Test Redfish Automation

2.
    Category: Fix
    Description:
        [191478] [IPMI ECO 01.00.10.00 | BIOS ECO 1.1a] Combined ECO automation fail.
    Impacted motherboard:
        X14SBW-F
    Affected functions:
        N/A
    Validation:
        1. Verify with Combined ECO automation

3.
    Category: Fix
    Description:
        [193102] [BIOS ECO] Some BIOS Automation Fails
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. Verify [BIOS ECO] Some BIOS Automation Fails
===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20250103_01.00.14.00_STDsp.bin version: 01.00.14.00 Date: 03 Jan 2025
Programmer Filename: BMC_X14AST2600-ROT-5601MS_20241112_09.00.08.00_STDsp_programmer.bin version: 09.00.08.00 Date: 12 Nov 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        [192890] BMCWebui LAN Interface failure
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. BMCWebUI TC4014

2.
    Category: Fix
    Description:
        [192121] please modify the standby fan duty to be 100% duty at S5
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. Monitor FANSTBY rpm reading in S5.

3.
    Category: Fix
    Description:
        [189728] [24988 -- ECO -- 01.00.06.01] SMTP Sender's Address entry in the MEL is improperly formatted
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. Monitor the format of MEL "SMTP Sender's Address entry"

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241219_01.00.13.00_STDsp.bin version: 01.00.13.00 Date: 19 Dec 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20241112_09.00.08.00_STDsp_programmer.bin version: 09.00.08.00 Date: 12 Nov 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        [191933] NVMes disappeared under Storage Monitoring -> Physical View after BMC Eject
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. [Optional] Precondition check if you know the RD command. Make sure the BPN cpld register bitmapPresent and bitmapSaveToRemove
           are with expected values.  If not, it could be BPN cpld fw problem.
        2. Make sure system boot to OS (e.g. cburn) and the OS is not from those drives to be ejected.
        3. webGUI -> STORAGE: eject, insert.

2.
    Category: Fix
    Description:
        [191013] [BMC] Web GUI does not detect when fans are ejected when removing FANS 1-10 
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. Boot system to cburn.
        2. Unplug fan modules and plug fan modules. Montior the webGUI Cooling fan rpm readings.

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241216_01.00.12.00_STDsp.bin version: 01.00.12.00 Date: 16 Dec 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20241112_09.00.08.00_STDsp_programmer.bin version: 09.00.08.00 Date: 12 Nov 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        [189728] [24988 -- ECO -- 01.00.06.01] SMTP Sender's Address entry in the MEL is improperly formatted
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. Plug AOC-NIC supporting PLDM to SUT
        2. Montior webGUI Network AOC page.  Observe Health Status icon.

2.
    Category: Fix
    Description:
        Modify power cycle behavior for on BIOS staged update
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        (For RD validation only)
        1. webGUI bios onNext fwUP.
        2. Montior power status and CPLD behaivor

3.
    Category: Fix
    Description:
        [191013] [BMC] Web GUI does not detect when fans are ejected when removing FANS 1-10
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. Unplug and plug fan modules in S0.
        2. Monitor fan rpm sensor reading and SEL.

4.
    Category: Fix
    Description:
        [191213] [ BMC ] Storage monitoring is unable to detect and display all the information for the installed u.2 nvmes
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. Navigate webGUI STORAGE tab.

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241204_01.00.11.00_STDsp.bin version: 01.00.11.00 Date: 04 Dec 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20241112_09.00.08.00_STDsp_programmer.bin version: 09.00.08.00 Date: 12 Nov 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        webGUI Network AOC page Health Status icon featuer broken, in 01.00.10.00
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. Plug AOC-NIC supporting PLDM to SUT
        2. Montior webGUI Network AOC page.  Observe Health Status icon.

2.
    Category: Fix
    Description:
        [190829] There isn't fan speed control function from AIOM_PORT sensor.
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        (Thermal team validation only)
        1. Validate FSC of AOC_PORT temperature sensor.

3.
    Category: Fix
    Description:
        [190200] STD -- 24502 -- 01.00.06.01(11/09/2024) -- BMC can not load WEB Network Page when no IPv4 addresses are present in the BMC
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        (IPv6 certification team validation only)
        1. Follow the description in the issueID

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241203_01.00.10.00_STDsp.bin version: 01.00.10.00 Date: 03 Dec 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20241112_09.00.08.00_STDsp_programmer.bin version: 09.00.08.00 Date: 12 Nov 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        [190829] There isn't fan speed control function from AIOM_PORT sensor. 
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        (Thermal team validation only)
        1. Monitor FSC with AOC_PORT temperature sensor

2.
    Category: Fix
    Description:
        [190721] transceiver temperature(AOC_PORT) is not available
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. Plug workable CX7 (or BF3) and transceiver to the SUT.
        2. webGUI -> Sensor Readings: Monitor the AOC_PORT temperature sensor readings.

3.
    Category: Fix
    Description:
        [190688] standby fan rpm shown 0 in WebGUI at S0
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. Monitor the FANSTBY sensor presentation in S0 and S5.
           Per thermal team expectation, if it is a dedicated standby fan (e.g. not shared with system fan),
           in S0, the rpm reading should be N/A (e.g. not 0).
           in S5, there should be rpm reading.

4.
    Category: Fix
    Description:
        [190480] CPLD Update Always Show 0%
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. webGUI MB_CPLD1 fwUP. Follow the UI flow.
        2. Monitor the UI progress anmiation should advance from 0% to 100%.

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241231_01.00.09.07_STDsp.bin version: 01.00.09.07 Date: 31 Dec 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20240727_09.00.08.00_STDsp_programmer.bin version: 09.00.08.00 Date: 12 Nov 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBI
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        [192675] ECO -- oBMC -- 24502 -- 01.00.09.04(2024/12/13) -- Web -- The descriptions of [MEL-0284] not match the spec 
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check MEL log

2.
    Category: Fix
    Description:
        [192674] ECO -- oBMC -- 24502 -- 01.00.09.04(2024/12/13) -- Web -- Unable to connect SSDP port after modifying the SSDP port number Copy Project Issue Link
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check SSDP port

3.
    Category: Fix
    Description:
        [190803] [SYS-622B-TRT]Detect BMC IP then remove BMC port and restart system,system still get BMC IP.
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check BMC IP from system

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241227_01.00.09.06_STDsp.bin version: 01.00.09.06 Date: 27 Dec 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20240727_09.00.08.00_STDsp_programmer.bin version: 09.00.08.00 Date: 12 Nov 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBI
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        [190842] [SYS-622B-TRT]Connect BMC port & Onboard LAN1 ,BMC IP will get Onboard LAN1 IP first.
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. AC on/off and check BMCIP

2.
    Category: Fix
    Description:
        [190803] [SYS-622B-TRT]Detect BMC IP then remove BMC port and restart system,system still get BMC IP.
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check BMC IP from system

3.
    Category: Fix
    Description:
        [190391] [SYS-622B-TRT]When set failover to shaer mode,press save BMC Web GUI will loading too long.
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Change network mode from Web

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241223_01.00.09.05_STDsp.bin version: 01.00.09.05 Date: 23 Dec 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20240727_09.00.08.00_STDsp_programmer.bin version: 09.00.08.00 Date: 12 Nov 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBI
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        [191904] [SYS-622B-TRT]BMC Web GUI will not display BPN CPLD FW update option. 
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check BPN CPLD FW from Web

2.
    Category: Fix
    Description:
        [190842] [SYS-622B-TRT]Connect BMC port & Onboard LAN1 ,BMC IP will get Onboard LAN1 IP first.
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. AC on/off and check BMCIP

3.
    Category: Fix
    Description:
        [190803] [SYS-622B-TRT]Detect BMC IP then remove BMC port and restart system,system still get BMC IP.
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check BMC IP from system

4.
    Category: Fix
    Description:
        [190391] [SYS-622B-TRT]When set failover to shaer mode,press save BMC Web GUI will loading too long.
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Change network mode from Web

5.
    Category: Fix
    Description:
        [199483] SYS-622B-TRT]NC-SI function failed with AOC-S25G-b2S. 
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check NCSI function

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241213_01.00.09.04_STDsp.bin version: 01.00.09.04 Date: 13 Dec 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20240727_09.00.08.00_STDsp_programmer.bin version: 09.00.08.00 Date: 12 Nov 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBI
BMC antiRBID: 0001


1.
    Category: Fix
    Description:
        [191152] [SCC_v3.7.0_b2411151445][SYS-622B-TRT] UID shows "off" under BMC web after turning on the UID via SCC.(Similar with issue#178938) Copy Project Issue Link
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check UID

2.
    Category: Fix
    Description:
        [184191] Redfish Automation Tool check fail.
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Run SATC

3.
    Category: Fix
    Description:
        [190480] CPLD Update Always Show 0% from Web 
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Update CPLD and check status

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241210_01.00.09.03_STDsp.bin version: 01.00.09.03 Date: 10 Dec 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20240727_09.00.08.00_STDsp_programmer.bin version: 09.00.08.00 Date: 12 Nov 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBI
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        [191140] [SCC_v3.7.0_b2411151445][SYS-622B-TRT] Chassis SN doesn't match in redfish and FRU. Copy Project Issue Link
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check FRU

2.
    Category: Fix
    Description:
        [190271] [BIOS ECO 1.0] IPMI get incorrect location SEL when using einj to inject UECC memory. Copy Project Issue Link
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check SEL log

3.
    Category: Fix
    Description:
        [189483] [SYS-622B-TRT]NC-SI function failed with AOC-S25G-b2S. 
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check NCSI function

4.
    Category: Fix
    Description:
        [189483] [SYS-622B-TRT]NC-SI function failed with AOC-S25G-b2S. 
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check NCSI function

5.
    Category: Fix
    Description:
        [182552] [SAA] SAA ECO SMSTC Test Failed on X14DBI-(T) Copy Project Issue Link
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Runn SMSTC

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241205_01.00.09.02_STDsp.bin version: 01.00.09.02 Date: 05 Dec 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20240727_09.00.08.00_STDsp_programmer.bin version: 09.00.08.00 Date: 12 Nov 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBI
BMC antiRBID: 0001


1.
    Category: Fix
    Description:
        [189483] Fix NC-SI function failed with AOC-S25G-b2S
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check share mode

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241204_01.00.09.01_STDsp.bin version: 01.00.09.01 Date: 04 Dec 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20240727_09.00.06.00_STDsp_programmer.bin version: 09.00.06.00 Date: 27 July 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBI
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        190842 Fixed [SYS-622B-TRT]Connect BMC port & Onboard LAN1 ,BMC IP will get Onboard LAN1 IP first.
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check onboard LAN1 IP

2.
    Category: Fix
    Description:
        190817 Fixed BMC not support the AOC NIC6 Fan Curve. Copy Project Issue Link
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check AOC NIC6 Fan

3.
    Category: Fix
    Description:
        190803 Fixed [SYS-622B-TRT]Detect BMC IP then remove BMC port and restart system,system still get BMC IP.
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check Network


4.
    Category: Fix
    Description:
        190619 Fixed [SYS-622B-TRT]Use BMC FW 1.0.8.0,BMC Web GUI cannot display AOC & onboard Lan info & temp. Copy Project Issue Link
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check Sensor list


5.
    Category: Fix
    Description:
        190532 Fixed [SYS-622B-TRT]Execute AC cycle,BMC Web GUI cannot display AOC-3916L-H16IR-32DD & HDD sensor. 
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check Sensor list

6.
    Category: Fix
    Description:
        190462 Fixed [SYS-622B-TRT]HGST HUS726T4TAL Manufacturer display worng info. Copy Project Issue Link
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check drive from Web

7.
    Category: Fix
    Description:
        190391 Fixed [SYS-622B-TRT]HGST HUS726T4TAL Manufacturer display worng info. Copy Project Issue Link
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check drive from Web

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241202_01.00.09.00_STDsp.bin version: 01.00.09.00 Date: 02 Dec 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20241112_09.00.08.00_STDsp_programmer.bin version: 09.00.08.00 Date: 12 Nov 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        190619 Fixed [X14DBI] Use BMC FW 1.0.8.0,BMC Web GUI cannot display AOC & onboard Lan info & temp.
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check onboard NIC on WEB

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241129_01.00.08.02_STDsp.bin version: 01.00.08.02 Date: 29 Nov 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20241112_09.00.08.00_STDsp_programmer.bin version: 09.00.08.00 Date: 12 Nov 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        [190200] STD -- 24502 -- 01.00.06.01(11/09/2024) -- BMC can not load WEB Network Page when no IPv4 addresses are present in the BMC
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. Trigger "no IPv4 address"
        2. Navigate webGUI Network page.

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241129_01.00.08.01_STDsp.bin version: 01.00.08.01 Date: 29 Nov 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20241112_09.00.08.00_STDsp_programmer.bin version: 09.00.08.00 Date: 12 Nov 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        [190514] Network AOC page has no AOC showing
    Impacted motherboard:
        All X14 ROT2HW2 5601MS MBs
    Affected functions:
        N/A
    Validation:
        1. Plug 2 (or more) AOC-NIC to the SUT. If the system has onboard slots, plug to onboard slots.
        2. webGUI -> Sensor Readings -> Network AOC: Observe the info in the page is not empty.

2.
    Category: Enhancement
    Description:
        BMC64MB 09.00.08.00 production image for CM.
    Impacted motherboard:
        All X14 ROT2HW2 5601MS MBs
    Affected functions:
        N/A
    Validation:
        (Validation by SWLab and RD)
        Precondition: Open-bench MB with bmc chip in socket.
        1. Use programmer to program the bmc chip externally. Install the bmc chip to the socket.
        2. AC on and wait system boot to UEFI or OS.
        3. IPMICFG -a, to assign bmc macAddr.
        4. webGUI login
        5. webGUI bmc fwUP to target bmc fw (e.g. 01.00.08.01)
        6. If UPW does not exists, IPMICFG to assign and lock UPW.
        7. IPMICFG -raw 30 41 to FD.
        8. Activate DCMS license by SMSTC.
        9. (You will need to contact RD for the detail of this step) Erase the provisioned status of your MB, and then execute MB provisioning.
        10. Use rot_checker.sh to examine the info.

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241127_01.00.08.00_STDsp.bin version: 01.00.08.00 Date: 27 Nov 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20240727_09.00.06.00_STDsp_programmer.bin version: 09.00.06.00 Date: 27 July 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        184929 Fixed [X14DBI] System cannot generate a crash dump log and IPMI no SEL after trigger "Three-Strike"
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check SEL log

2.
    Category: Fix
    Description:
        190128 Fixed [X14DBI] No fan cuuve of NVMe sensor
    Impacted motherboard:
        X14DBI
    Affected functions:
        N/A
    Validation:
        1. Check FAN duty

3.
    Category: Fix
    Description:
        189603 [ECO] WebUI timeout will showing another login window
    Impacted motherboard:
	All
    Affected functions:
        N/A
    Validation:
        1. Check WEBUI

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241121_01.00.07.00_STDsp.bin version: 01.00.07.00 Date: 21 Nov 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20240727_09.00.06.00_STDsp_programmer.bin version: 09.00.06.00 Date: 27 July 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        189682 Fixed [X14DBG-AP]Fan speed control set point isn't correct for GPU temp sensor
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. Check FAN speed control for GPU sensor

2.
    Category: Fix
    Description:
         187830 [SAA_1.1.0-p4_20241014] Test case 3173 - In-Band - Test "ClearCMOS" test failed on H14SHM
    Impacted motherboard:
        H14SHM
    Affected functions:
        N/A
    Validation:
        1. Check clearCMOS function

3.
    Category: Fix
    Description:
         [189724][189603] [ECO] WebUI timeout will showing another login window
    Impacted motherboard:
        ALL
    Affected functions:
        N/A
    Validation:
        1. Check WebUI

4.
    Category: Fix
    Description:
          [188273] ECO -- oBMC -- 24502 -- 01.00.03.01(20241023)-- WebUI -- Should remove "JAVA console option" in help page Dashboard part.
    Impacted motherboard:
        ALL
    Affected functions:
        N/A
    Validation:
        1. Check option on help page

5.
    Category: Fix
    Description:
          187348 Fixed [EVT][X14SAE-F]After trigger CPU thermal trip, every time start up SEL send [CPU-0001] Thermal Trip has occurred - Assertion
    Impacted motherboard:
        ALL
    Affected functions:
        N/A
    Validation:
        1. Check CPU thermal trip on SEL

		
 




===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241113_01.00.06.02_STDsp.bin version: 01.00.06.02 Date: 13 Nov 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20240727_09.00.06.00_STDsp_programmer.bin version: 09.00.06.00 Date: 27 July 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001

1.
Category: Fix
Description:
[189040] [IPMI ECO] Sensor reading fail when CPU overheat.
Fixed issue on bmc side.
Impacted motherboard:
X14SBI
Affected functions:
N/A
Validation:
    1. Heats the CPU to overheating, then cools it.
    2. check Sensor reading "CPU Temp".

2.
Category: Fix
Description:
[188598] [IPMI ECO] BMC Web UI Automation test fail.
Impacted motherboard:
X14SBI
Affected functions:
N/A
Validation:
    1. Pass test case 4018
===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241109_01.00.06.01_STDsp.bin  version: 01.00.06.01 Date: 09 Nov 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20240727_09.00.06.00_STDsp_programmer.bin version: 09.00.06.00 Date: 27 July 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        "PLX1 Temp" and "PLX2 Temp" temeprataure sensor feature broken in 01.00.06.00
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. webGUI -> Sensor Readings: Montior "PLX1 Temp" and "PLX2 Temp" readings

2.
    Category: Fix
    Description:
        [188344] CPU2-related sensors dropped during DC ONOFF on BMC FW 01.00.03.02
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. cburn ONOFF NASNSR. No CPU2 related sensors drop.
        Remarks: This is a bmc workaround. The ulimate fix should come from bios or MB_CPLD1 fw.

3.
    Category: Fix
    Description:
        [188805] PLX2 Temp sensor dropped during DC ONOFF with BMC FW 01.00.04.00
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. cburn ONOFF NASNSR. No PLX2 Temp sensor drop.

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241108_01.00.06.00_STDsp.bin  version: 01.00.06.00 Date: 08 Nov 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20240727_09.00.06.00_STDsp_programmer.bin version: 09.00.06.00 Date: 27 July 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        [188291] ECO -- oBMC -- 24502 -- 01.00.03.01(20241023)-- Web -- HEL advanced settings not restore to dafault value after doing ipmi raw 30 41
    Impacted motherboard:
        X14SBI-TF, X14SBW-TF
    Affected functions:
        N/A
    Validation:
        1. Login BMC web with ADMIN
        2. Go to System -> Health Event Log page
        3. Disable Enable FIFO Event Log
        4. ipmi raw 30 41
        5. Check HEL advanced settings

2.
    Category: Fix
    Description:
        [188045] ECO -- oBMC -- 24502 -- 01.00.02.00(20241018)-- Web -- SNMPv1 -- Failed to find correct trap in snmp log
    Impacted motherboard:
        X14SBI-TF, X14SBW-TF
    Affected functions:
        N/A
    Validation:
        1. ipmi raw 30 41
        2. Login BMC web with ADMIN
        3. Go to Notifications -> Alerts -> No.1 press edit button
        4. Enable switch button -> Protocol select SNMPv1 -> Severity select Warning -> Destination Address input 10.140.201.33 -> Trap Community input 1qaz2wsX
        5. Press Send Test Alert

3.
    Category: Fix
    Description:
        [187896] ECO -- oBMC -- 24502 -- 01.00.02.00(20241018)-- Web -- [MEL-0131] and [MEL-0132] need to display the iKVM session ID at the end
    Impacted motherboard:
        X14SBI-TF, X14SBW-TF
    Affected functions:
        N/A
    Validation:
        1. ipmi raw 30 41
        2. Login BMC web with ADMIN
        3. Go to Remote Control page
        4. Press Launch Console
        5. Close iKVM Session
        6. Check MEL

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241107_01.00.05.00_STDsp.bin version: 01.00.05.00 Date: 07 Nov 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20240727_09.00.06.00_STDsp_programmer.bin version: 09.00.06.00 Date: 27 July 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        [188598] [IPMI ECO] BMC Web UI Automation test fail.
        Fixed issue on bmc side.
    Impacted motherboard:
        X14SBI
    Affected functions:
        N/A
    Validation:
        1. BMC Web UI Automation test

2.
    Category: Fix
    Description:
        Fix Lan link LED state from blinking to solid on
    Impacted motherboard:
        X14SBI
    Affected functions:
        N/A
    Validation:
        1. Check Lan link LED state is solid on

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241101_01.00.04.00_STDsp.bin version: 01.00.04.00 Date: 01 Nov 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20240727_09.00.06.00_STDsp_programmer.bin version: 09.00.06.00 Date: 27 July 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        [185186] SuperDiag data collection cannot complete locally
        Fixed issue on bmc side.
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. Run SuperDiag UEFI and monitor if data collection stage can complete.

2.
    Category: Fix
    Description:
        [188344] CPU2-related sensors dropped during DC ONOFF on BMC FW 01.00.03.02
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. Run cburn ONOFF NASNSR stress test, and monitor if any drop from CPU2 related sensors

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241024_01.00.03.02_STDsp.bin version: 01.00.03.02 Date: 24 Oct 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20240727_09.00.06.00_STDsp_programmer.bin version: 09.00.06.00 Date: 27 July 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001

1.
    Category: Fix
    Description:
        [187999] BMC password resets to factory default after updating BMC to 01.00.03.01
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. fwup between 01.00.01.10 and 01.00.03.02
2.
    Category: Fix
    Description:
        [187944] There isn't fan speed control function from AOM_NIC13 sensor.
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. Check FSC on AOC_NIC13

3.
    Category: Fix
    Description:
        [187937] All NIC sensors lose temperature reading
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. Check NIC temperature semspr readings.

4.
    Category: Fix
    Description:
        [187583] BMC FW 01.00.01.10 showing sensor instability
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. Monitor sensor reading stability

5.
    Category: Fix
    Description:
        [187583] BMC FW 01.00.01.10 showing sensor instability
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. Monitor sensor reading stability

6.
    Category: Fix
    Description:
        [187083] ECO -- 01.00.01.08 -- func -- DCONOFF test failed due to unexpected sensors mismatch
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. cburn ONOFF NASNSR

7.
    Category: Fix
    Description:
        [186998] PLX1 Sensor Drop after downgrading Switchboard CPLD from A6 to A4
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. Monitor PLX1/PLX2 temperature sensor reading with SWBD cpld fw A7 (or newer).

8.
    Category: Fix
    Description:
        [186743] M.2 sensor dropped in Web GUI during DC ONOFF
    Impacted motherboard:
        X14DBG-AP
    Affected functions:
        N/A
    Validation:
        1. cburn ONOFF NASNSR

===============================================================================================================
Filename: BMC_X14AST2600-ROT-5601MS_20241018_01.00.02.00_STDsp.bin version: 01.00.02.00 Date: 18 Oct 2024
Programer Filename: BMC_X14AST2600-ROT-5601MS_20240727_09.00.06.00_STDsp_programmer.bin version: 09.00.06.00 Date: 27 July 2024
BMC type: Supermicro Openbmc
Redfish API : Redfish_1_11_API_full_list_20231218
Supported MB: X14DBG-AP, X14DBI, X14SBI, X14SBW
BMC antiRBID: 0001
1.
    Category: Fix
    Description:
        [187421] [IPMI ECO 01.00.01.09] Automation tests Failure
    Impacted motherboard:
        X14SBW-F
    Affected functions:
        N/A
    Validation:
        1. Verify combinedeco automation test
2.
    Category: Fix
    Description:
        [187408] ECO -- oBMC -- 24502 -- 01.00.01.09(20241014)-- Redfish -- Unable to modify AutoNeg via PATCH /redfish/v1/Managers/1/EthernetInterfaces/1/
    Impacted motherboard:
        X14SBW-F
    Affected functions:
        N/A
    Validation:
        1. Verify SATC Redfish automation