=========================================================================================
UEFI SAA Flash Script Package Modify Instructions
=========================================================================================
Please read this document in it before performing the system BIOS update.
Please verify that your system meets the requirments.

******************************************************************************************
Notes:
  1. This flash package is using UEFI SAA 1.2.0-p2 (2025/02/07),
     if you need to use SAA before 1.2.0 (20241227),
	 please use flash package: SAA_Firmware_Flash_Script_v1.1.0_20241121.
******************************************************************************************


1. Choose your package based on your project.
     Project which activate RHI by default.
     SAA_AOM_CPLD_FlashScript_vx.y.z
	 SAA_BIOS_FlashScript_vx.y.z
     SAA_BMC_FlashScript_vx.y.z 
	 SAA_CPLD_FlashScript_vx.y.z
	 SAA_FPGA_FlashScript_vx.y.z
  
  Example :
      AOM CPLD :	SAA_AOM_CPLD_FlashScript_v1.2.0.zip
      BIOS :		SAA_BIOS_FlashScript_v1.2.0.zip
	  BMC  :		SAA_BMC_FlashScript_v1.2.0.zip
	  CPLD :		SAA_CPLD_FlashScript_v1.2.0.zip
	  FPGA :		SAA_FPGA_FlashScript_v1.2.0.zip


2. Extract the package, and put the target image into the flash package.


3. The SAA used in this flash package is UEFI SAA 1.2.0-p2 (2025/02/07)
   You can change the UEFI SAA version if needed. (Note1)
   To change UEFI SAA version, please make sure the following file are also replaced from
   the same SAA package.

    - SAA.efi
    - UEFI_SAA_UserGuide.pdf
   
   If you need to user SAA version before 1.2.0 (20241227),
   Please use SAA_Firmware_Flash_Script_v1.1.0_20241121. (Note1)


4. Update ProjectName_FwType_Package_Readme.txt in the flash package.
   * FwType can be AOM CPLD/BIOS/BMC/CPLD/FPGA...

  a. Follow the 'Modify Instructions' and remove the section after updated.
  b. Update the image information according to your project.
     Search the whole file for the project/image name, make sure all the information is
     based on your project.
  c. Update the SAA version if you have change the bundled SAA package in Stpe.3
  d. Update the Supported Products based on your project.
  e. Update 'SYSTEM HARDWARE and FIRMWARE REQUIREMENTS' if needed.
  d. Update 'Steps to Update FwType through SAA Flash Script' based on your project.


5. Rename flash package and the ProjectName_FwType_Package_Readme.txt

  Example for X14SBW:
    a. SAA_BIOS_FlashScript_v1.2.0
    - package name : BIOS_X14SBW-1D49_20240920_1.1_STDsp
    - Readme       : X14SBW_BIOS_Package_Readme.txt
	
    b. SAA_BMC_FlashScript_v1.2.0
    - package name : BMC_X14AST2600-ROT-5601MS_20241109_01.00.06.01_STDsp
    - Readme       : X14SBW_BMC_Package_Readme.txt
	
    c. SAA_CPLD_FlashScript_v1.2.0
    - package name : CPLD_X14SBW-20000190_20241023_00.0A.XX_STDsp
    - Readme       : X14SBW_CPLD_Package_Readme.txt

  Example for X14SBHM:
    a. SAA_FPGA_FlashScript_v1.2.0
    - package name : FPGA_MBD-X14SBHM-40XXF374_20241108_37.XX.XX_STDsp
    - Readme       : X14SBHM_FPGA_Package_Readme.txt
	
  Example for AOM CPLD:
    a. SAA_AOM_CPLD_FlashScript_v1.2.0
    - package name : CPLD_AOM-DCPDB-MD101-4D00EE08_20250108_08.XX.XX_STDsp
    - Readme       : CPLD_AOM_Package_Readme.txt

