IPMI Firmware Release Note
----------------------------
Filename: SMT_X10_121.bin    version: 1.21    Date: 11-08-2013

U-Boot build time       : Nov 08 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

Feature:
Solve:

  ==>  Please remove current FruData by ipmicfg command (ipmicfg -raw 30 41 and then wait for bmc reboot)

  X10 Up boards, Dp boards
  
  Fru1 data cannot write
  [Validation steps] 
  1.Please remove current FruData by ipmicfg command (ipmicfg -raw 30 41 and then wait for bmc reboot)
  2.ipmicfg -fru1 list. Check if fru1 data exists
  3.jipmicfg -fru1 bp 1. Check if bp is equal to 1

  [48818] Uncorrect information in Power Source monitoring 
		[Validation steps] check dc12output voltage, ac input current, dc 12 output current (ps source webpage)

  X10SLX-F
  [48477] Fan PWM measurement fail 
		[Validation steps] measure descending fan curve

  [48763] CPU temperature only can up to 85 degree C with E3-1220L v3 CPU hence the fan speed can't run at full speed 
		[Validation steps] Select CPU which HighNR is under 90 degree and try to overheat it.

  X10QBI
  [46732] HWM test fail 
		[Validation steps] Check VBAT sensor voltage, should be close to 3.3v 

  A1SAM-F
  [46732] JL1 chassis intrusion jumper is not working.   
		[Validation steps] put JL1 jumper on, and then pull out. See if chassis intrusion still exists  

=====================================================================================
Filename: SMT_X10_120.bin    version: 1.20    Date: 11-01-2013

U-Boot build time       : Aug 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

Feature:
Solve:
	All X10 mother boards
  [48758] Unable to login to ADMIN account after changing passwords a few times 
		[Validation steps] 
			1. Login to IPMI Web GUI -> Configuration -> Users -> Modify ADMIN
			2. Change ADMIN password to ADMIN123
			3. Check ipmitool remotely with new password
			4. Change ADMIN password to ADMINADMIN
			5. Check ipmitool remotely with new password
			6. Change ADMIN password to ADMIN123
			7. Check ipmitool remotely with new password 
		[Root cause] there are garbage byte left at the end of the new password

  [48612] Power Fail Email Alert Does Not Have Event Description to Mention Power Fail Event
		[Validation steps] Install power supply and pull out the power cord
		[Root cause] Need to parse sel data to show power failure information before email alert is sent

  [48477] Fan PWM measurement fail 
		[Validation steps] measure the heavy io curve on cpu and dimm
		[Root cause] Should follow the spec of X10 SIM_TDG Draft 06282013.pdf to setup heavy io curve on cpu and dimm
		
  X10SLA-F 
  [48762] FAN sensor reading of 20,000 rpm FAN is not correct 
		[Validation steps] install the fan and set full speed mode. Check if rpm is over 20000
		[Root cause] Fan rpm calculation occurs overflow on high speed fan 
		 
	X10SLE-DF	
  [48606] iKVM Does Not Identify Node By Name 
		[Validation steps] Enter IPMI web page and see the host names on both node, "SLE_D_NODE_1" and "SLE_D_NODE_2"
		[Root cause] We setup the host name to judge which bmc is used and logged in now
	
=====================================================================================

Filename: SMT_X10_119.bin    version: 1.19    Date: 10-28-2013

U-Boot build time       : Aug 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

Feature:
Solve:
	All X10 mother boards

  [48659] Cannot read/write FRU by smcipmitool.exe
		[Validation steps] Read:  smcipmitool.exe <IP Address> ADMIN ADMIN ipmi fru
                       Write: smcipmitool.exe <IP Address> ADMIN ADMIN ipmi fruw <field> <value>
		[Root cause] the command responses the data from the wrong FRU block

  [48423] The memory ECC even log fail
		[Validation steps] Use ipmi command to test Dimm A1 has ecc errors
      ipmitool -I lanplus -H 10.133.176.182 -U ADMIN -P ADMIN raw 0x4 0x2 0x4 0x0c 0xff 0x6f 0x1 0x1A 0x80
		[Root cause] handle unused variable on event log web page 

  X10SLD-EF
  [48322] PUE, Standard, and Heavy IO Fan Modes have the same Fan Speed
		[Validation steps] Set each fan mode and observe the rpms
		[Root cause] Micro cloud series servers are special cases. Heavy I/O mode can be removed.
                 Fan speed table is changed

  [48609] Memory Sensor Does Not Match BIOS Setup Naming
		[Validation steps] Check IPMI sensor name and compare with the other on bios setup 
		[Root cause] Add the mechanism to judege BMC 1 and BMC2 by GPIOH2
 
  [48604] PCH Temperature Sensor Missing
		[Validation steps] Enter sensor page
		[Root cause] Need add PCH sensor for monitoring list 
 
  A1SAI-F, A1SAM-F
  [48322] Fan Mode Setting fail. 
		[Validation steps] Set heavy io mode and heat memory
		[Root cause] dimm sensor is not put in fan control list

  A1SAI-F, A1SAM-F
  [48322] Fan Mode Setting fail. 
		[Validation steps] Set heavy io mode and heat memory
		[Root cause] dimm sensor is not put in fan control list

  X10QBI
  [48300] Abnormal IPMI Fan fail event logs
		[Validation steps] Power on at initialization
		[Root cause] bank 0, reigster should be set 0xF4
                 Add protection to avoid ghost fans noise

  X10SEAA-LN4F,X10SL7-F, X10SLA-F
  [48279] FAN speed won't change when overheat memory with setting Fan to HeavyIO Speed
		[Validation steps] Set heavy io mode and heat memory
		[Root cause] The curve of heavyIO mode is not configured

=====================================================================================

Filename: SMT_X10_118.bin    version: 1.18    Date: 10-09-2013

U-Boot build time       : Aug 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Feature:
  @Support Fru inventory data 1 for PE & bios to write board information area

  @Support port change and enable/disable function on both port setting web page and oem commad
    -0x30	0x70	0x67	Get/Set ports & Services	
    Request
      Data 1: 0/1 [Get/Set]
      Data 2: Port service
        0: HTTP_PORT,1: HTTPS_PORT,2: IKVM_PORT,3:VM_PORT,4:SSH_PORT,5:WSMAN_PORT,6:HTTP_SERVICE,
        7:HTTPS_SERVICE,8:IKVM_SERVICE,9:VM_SERVICE,10:SSH_SERVICE,11:WSMAN_SERVICE,12:SSL_REDIRECT
      Data 3-4 :  [Set]
      Data 4: port number (LSB)
      Data 5: port number (MSB)"	"[Get]
    Response
      [Get]
        Data1: completion code
        Data2: port number (LSB)
        Data3: port number (MSB)
      [Set]
        Data1: completion code"

Solve:
  All X10 boards  

	[48321] YFan speed reading is incorrect with FAN-0141L4
		[Validation steps] install the fan and set full speed mode. Check if rpm is over 20000
		[Root cause] Fan rpm calculation occurs overflow on high speed fan 

	[48281] Your session has timed out. You will need to open a new session" error message popped when click "Post Snooping" in IPMIWeb GUI
		[Validation steps] Enter post snopping page	
		[Root cause] response the wrong data to browser and cause time-out

	[48279] FAN speed won't change when overheat memory with setting Fan to HeavyIO Speed
    [Validation steps] Switch to heavyIO mode and heat memory. Check if fan speed is up
		[Root cause]
      BMC don't include dimm sensor in fan control list

	[48206] SMTP server won't work if "Sender's Address" set @ " " (NULL)
    [Validation steps]
      1. Alert setting
      2. SMTP server setting (w/ sender's address) 
      3. Send Test Alert
      4. Checks email
		[Root cause]
      Some smtp server, it needs complete email name (BMCaabbccddeeff@X10SLM-F.com)

  X10SLX-F
	[48293] No CPU overheat alarm, jumper JOH1 no function
	[48236] CPU temperature reading shows "Not Present" in IPMI Web
	  [Validation steps] Heat CPU temperature or enter sensor page
    [Root cause]       BMC don't use peci to read cpu temperature
  
  X10SLH-F  
	[48236] Cannot reset to the factory default (clean LAN)
	  [Validation steps] ipmicfg -fde
    [Root cause]       BMC will clear fru inventory area on this oem command
    
  X10SLM-F  
	[48167] Ipmitool to check onboard LAN1 MAC address failed.
	  [Validation steps] 1. Use 0x30 0x21 command to get system mac address
	                     2. Compare this with another on the IPMI system information web page 
    [Root cause]       BMC don't completely to delete the data about system mac address
 
  X10SLL-F  
	[47470] The MAC address that use IPMITOOL to fetch is not match with MB
	  [Validation steps] 1. Use 0x30 0x21 command to get system mac address
	                     2. Compare this with another on the IPMI system information web page 
    [Root cause]       BMC don't completely to delete the data about system mac address 
    
  A1SAM-F  
	[48322] Fan Mode Setting fail
  [48239] IPMI sensor reading
	  [Validation steps] Enter sensor reading page
    [Root cause]       Previous BMC FW doesn't support this board yet.

=====================================================================================

Filename: SMT_X10_117.bin    version: 1.17    Date: 09-27-2013

U-Boot build time       : Aug 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:

  *All X10 Up boards
	[48112][48111] Error in launching iKVM console
	               Application Error: Unable to launch the appication error when launch Console Redirection Screen (KVM)

		[Validation steps]
		1. launch ikvm from the console redirection page.
		
		[root cause]
		the java viewer can't accept the empty hostname.
		[solution]
		pass the default the hostname to ikvm viewer if it is empty.

=====================================================================================

Filename: SMT_X10_116.bin    version: 1.16    Date: 09-26-2013

U-Boot build time       : Aug 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:

  *All X10 Up boards
	[48089][48088] Email Alert not working with IPMI FW v1.15
		[validation steps]
		1. configure SMTP server and the e-mail address on SMTP and alert pages.
  	2. trigger CPU or other sensors overheat.

	[48090] Factory default is not working
  	[validation steps]
		1. do factory-to-default on Factory default page.

  *MB -X10QBI-O-P
  [48006] System info LED is not on when fan failed or cpu overheat
  [47511] LED test for FAN Fail test Fail
 
  *MB -X10SLE-DF-O-P
	[47796] Cannot set up IPMI configuration on web 
		[validation steps]
		(1)go to the LDAP page
		(2)click Enable LDAP Authentication, it will pop up message from webpage and logout. 

  *MB -A1SAI-2750F-O-P   
	[47533] VCCP sensor error 
		[validation steps]
		(1)enter sensor reading page

	[47539] System unable to power back on neither by power button nor power control (IPMIWeb)
		[Validation steps]
		(1)make sure the lan cable be plugged to the share lan2.
		(2)do power on/off stress through ipmitool over the share lan 2. 
  
=====================================================================================

Filename: SMT_X10_115.bin    version: 1.15    Date: 08-30-2013

U-Boot build time       : Aug 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
  A1SAi-2750F/2550F
  
  Support 25MHz PWM frequency output
  
  [#47556] Failed to mount virtual drive via "Virtual Media --> CD-ROM Image" in IPMIWeb GUI
  Root cause: Need to add user/password account judgement
  Solution  : FW Update
  
  [#47535] Failed to update BIOS via IPMIWeb GUI 
  Root cause: This platform doesn't support ME.
  Solution  : Ignore ME region

  [#46347] Overheat LED at "JOH1" was lit and blinking if any of FAN-Failure asserted. 
  Root cause: GPOY3 OVERHEAT LED" and "GPOA3 PSU/FAN failure", they PWM together when FAN fails 
  Solution  : Setup GPIOY3 to lit JOH1 only

  X10SLE-DF
  [#47405] For cpu2 HWM measurement fail at Vbat
  Root cause: incorrect SDR
  [#47447] Please Remove Dedicated LAN Link Option
  Root cause: NIC speed is always 1G speed. Don't need to adjustify

  All X10 motherboards
  [#47470] The MAC address that use IPMITOOL to fetch is not match with MB. 
  Root cause: IPMI still record old share lan adderess after updating the nic eeprom
  Solution  : Synchronize the new share lan address
  Validation step:
              1. flsah eeprom with SLM13.zip
              2. use IPMITOOL and command 
                 IPMITOOL.exe -I lan -H 10.135.15.95 -U ADMIN -P ADMIN raw 0x30 0x21
              3. The result is not match with the MAC address of MB.    
=====================================================================================

Filename: SMT_X10_114.bin    version: 1.14    Date: 08-16-2013    SVN: 620

U-Boot build time       : Jun 14 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
  X10DRI-T
  [#47389] Missing FanA and FanB on the Sensor Reading Page
  Root cause: sensor number of FANA & FANB is not correct in FW
  Solution  : Modify them in FW
  Validation step: 
   See it in sensor reading page

  X10SLE-DF
  [#47397] Dedicated LAN Speed Always Shows 10M
  [#47196] Dedicated LAN Link Status Shows 10M
  Root cause: driver reading is not correct 
  Solution  : Modify in NIC driver
  Validation step: 
   See it in network page

  [#47334] HWM measurement fail at Vdimm
  Root cause: sensor reading is not accruate 
  Solution  : Adjust SDR value
  Validation step: 
    See in sensor page

 [#47193] After Update to IPMI FW 1.13, CPU Throttling to 800 MHz Observed
  Root cause: GPIOA4 pulls low 
  Solution  : Pull GPIOA4 high at BMC initialzation
  Validation step: 
    heat cpu over 80 degree by PwrThermalUtil tool 

  All X10 motherboards
  [#47198] Lan Interface Should be LAN Interface
  Root cause: Change "Lan"to all capital letters "LAN"
  Solution  : Correct wordings in FW
  Validation step:
    See "LAN interface" in network page

  X10SLL+-F
  [#47309] Email Alert for X10SLL+-F Shows X10SLA_F in Subject Header
  Root cause: Typo error
  Solution  : Correct wordings in FW
  Validation step:
    Setup email alert function
    
=====================================================================================
Filename: SMT_X10_113.bin    version: 1.13    Date: 07-29-2013    SVN: 553

U-Boot build time       : Jun 14 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r20

****** The user is not allowed to downgrade the fw from this release due to the security issue****** 

Improvement:
  1.Renew default SSL certificate from 7/17/2013 to 7/17/2014
  2.fix the security issue for the user password
    Encrypt the user password inside IPMI fw.
    Validation step:
	1. add/delete/modify the username/password through web or ipmitool.
	2. save/restore the ipmi configuration.

  [X10SLE-DF] 
    3.Add X10 SLE-DF sensor reading support
    4.Add RTL8363SB for dedicate lan 1G Support
    
    
    
Solve:
  X10SEAA-LN4F
  [#46904] FAN1 and FAN3 are not working properly. 
  Validation step:Try full speed
 
  All X10Up board
  [#46720,46709] Memory ECC Error Email Alert Shows Wrong DIMM Slot  
  Validation steps:
    1.Register the smtp setting
    2.Use ipmi command to test Dimm A1 has ecc errors
      ipmitool -I lanplus -H 10.133.176.182 -U ADMIN -P ADMIN raw 0x4 0x2 0x4 0x0c 0xff 0x6f 0x1 0x1A 0x80
    3.Receive the email and check if the dimm slot number is the same as the other in IPMI event log
 
  [#46595] In iKVM, IPMI firmware not supports others keyboard layout style except of "English" type  
  IKVM VERSION : 1.69.20
  Validation steps:
    1.Launched iKVM,go to input tab in preference tab.
    2.change the keyboard layout.
    3.none of keyboard layout are working expect for English one. 

  [#46592] Sender's address of SMTP setting not works properly.  
  Validation steps:
    1.Remote login into SUT IPMIWeb GUI via IPMI IP
    2.Setup an alert entry in "Alerts --> configuration" field
    3.Setup SMTP server with sender's address in "SMTP" --> configuration" field 
    4.Send a test alert and then check email     

  [#46409] Auto-resize windowsˇ¨ tab of iKVM is not working 
  Validation steps:
    1.Remote login-into SUT via IPMI LAN.      
    2.Launched iKVM, un-check the "auto-resize windows" tab under Option -> Preference -> Windows 
    3.Use mouse adjust iKVM windows size a failed, unable to adjust

  X10SLH-F,X10SLL+-F,X10SLM+-F,X10SLM+-LN4F
  [#46708] DIMM Temperature Sensor Naming Does Not Match Silkscreen 
  Validation steps:
    1.Burn the FW and don't preserve the configuration
    2.Enter IPMI sensor reading page

  X10SLM+-F,X10SLH-F
  [#46714] Email Alert Shows X10SLH_F  
  Validation steps:
    Register the smtp setting and send the email

=====================================================================================
Filename: SMT_X10_112.bin    version: 1.12    Date: 07-05-2013    SVN: 499

U-Boot build time       : Jun 14 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
  X10SLM-F, X10SLL-F
  [#46480] IPMI Logs Non-Critical Events.(CPU Temp)
  Validation step:
    heat the CPU temperature

  [#46141] Low Critical- Going Low during IPMI ON/OFF share LAN stress
  Validation step:
    System on-off test
    
  X10SEAA_LN4F 
  [#46374] No beep when no memory connect to the system.
  Validation step:
    don't plug in the memory and power on the machine

  [#46233] CPU Temp" and "Chassis Intrusion" shows "Not Present
  Validation step:
    Enter IPMI sensor page
=====================================================================================

Filename: SMT_X10_111.bin    version: 1.11    Date: 06-26-2013    SVN: 474

U-Boot build time       : Jun 14 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
 
  [#46381] Chassis Intrusion Not Logged in Event log,SNMP trap and E-mail alert 
  [#46373] Chassis Intrusion Not Logged in Even Log
  [#46349] While chassis intrusion asserted, no chassis intrusion event log was showed. No SNMP trap and Email alert as well

=====================================================================================

Filename: SMT_X10_110.bin    version: 1.10    Date: 06-21-2013    SVN: 462

U-Boot build time       : Jun 14 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:

X10SLM+_LN4F  
  2.[#46276] IPMI Web Orderly Shutdown Power Control Does Not Work

X10SEAA_LN4F
  3.[#46242] There is an extra "Optimal" Fan-mode was present in IMPIWeb GUI
  4.[#46237] Power supply information are not LINE-UP in IPMIWeb GUI
  5.[#46224] It will generate " Voltage VDIMM " after run E-burn SAT Test

=====================================================================================
     
Filename: SMT_X10_109.bin    version: 1.09    Date: 06-14-2013    SVN: 451

U-Boot build time       : Jun 14 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
  1.Add sensor support on X10SEAA_LN4F
  2.update sensor list according to IPMI_voltage_sensors_threhold_R01.xlsx
  2.#46139          LAN 1 disconnect after IPMI factory default setting
  2.#46132					-12V Events Lgged During IPMI KVM Stress
  3.#45908,#45905		IPMI Logs Non-Critical Events
  4.#45778					Remote Console Preview display is abnormal
  5.#46059					Random - Update BIOS setting via OOB with option "--reboot" fail.
  6.#46056					Random - The process is loop when update BIOS via OOB.  
     
=====================================================================================

Filename: SMT_X10_108.bin    version: 1.08    Date: 06-06-2013    SVN: 432

U-Boot build time       : May 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
  1.fine tune sensor values on X10DRI_T, X10QBI_F
  2.#46010											Please Change FAN1 Sensor to FAN
  3.#45939											Power Fail Logs About Every 5 Minutes
  4.#45938											HeavyIO FSC: FANA RPM Higher at 39C and lower at 42C 
  5.#45937											HeavyIO FSC Mode FanA Speed Higher Than Thermal Guideline Specification 
  6.#45928,#45926,#45908,#45905	IPMI Logs Non-Critical Events 
  7.#44075											dmesg has a "ipmi_si: Error clearing flags: cc" error message after running E-burn stress
        
=====================================================================================
Filename: SMT_X10_107.bin    version: 1.07    Date: 05-30-2013    SVN: 417

U-Boot build time       : May 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
	
	Fine tune VBAT, -12V sensor threshold on X10SLM-F, X10SLL-F and X10XLM+_LN4F
        
=====================================================================================

Filename: SMT_X10_106.bin    version: 1.06    Date: 05-27-2013    SVN: 410

U-Boot build time       : May 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
	
	Please clear Java cache (iKVM verion is updated)
  Please uncheck the preserved box in firmware upload page
  
  1.Add sensor on X10SLL+_F, X10QBI_T
  2.#45801,#45725,#45725,#45481		[OOB] System Will Shutdown After Flash BIOS Via OOB and Reset .
  3.#45712												There are many Vcore events in IPMI SEL when running eburn LIN test
  4.#45621,#45785									IPMI Virtual Keyboard didn't have Swiss language item
  5.#45682												FAN speed will up to 100% when IPMI initializing
        
=====================================================================================
Filename: SMT_X10_105.bin    version: 1.05    Date: 05-20-2013    SVN: 398

U-Boot build time       : May 20 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r18

Solve:
  
   1. [X10SLM-F/X10SLL-F] Output 50@ dutycycle when bmc reboots 
   2. [X10SLM-F/X10SLL-F] Change sensor name to "3.3V AUX"
   3. [X10SLL-SF]         BMC can't boot successfully
   4. #45619              It not work if run "ChnageBIOScfg" and "Loaddefault" of OOB functions
   5. [X10DRI_F]          Add sensor supports
   6. Preserve the whole 64k block where SMIBIOS data resides.
      [Validation Steps]
      a. Go to the bios update page 
      b. Update bios image only with preserving SMBIOS.
      
=====================================================================================

Filename: SMT_X10_104.bin    version: 1.04    Date: 05-10-2013    SVN: 388

U-Boot build time       : May 9 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r18

Solve:

  1. Output 100@ dutycycle for X10SLM-F/X10SLL-F. 
  2. Update the thermal curve for heavy IO fan mode.
  
  [45018] Sometimes Auto-Resize Window Does Not Work When Booting into OS 
  [45209] IPMI KVM window doesn't have Power Control option 
          Support high resolution up to 1920*1200.
  [45463,45401,45381,45347] BMC incorrect reponse detected during eburn test  
  
=====================================================================================
Filename: SMT_X10_103.bin    version: 1.03    Date: 05-03-2013    SVN: 376

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:

	Add OOB event log.
  	OOB file build date mis-match (Sensor type : 0xCA, Event Data 1)
	  OOB feature initial failure (Sensor type : 0xCA, Event Data 2)  
  
	[X10SL7-F]
  45347 BMC incorrect reponse detected during eburn test  
   
	[X10SLE-F/X10SLD-F]
  45381 BMC incorrect reponse detected during eburn test  
  
  
======================================================================================
Filename: SMT_X10_102.bin    version: 1.02    Date: 04-26-2013    SVN: 367

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:

  [X10SLM-F/X10SLL-F]
		45067 part of the Eburn stress test is fail (ipmi_si: Error clearing flags: cc) 
   
	[X10SLM+-LN4F/X10SLH-F/X10SL7-F/X10SLA-F]
		45231	Please Change Bios String in IPMI Web System Information Page to BIOS

	[X10SLE-F/X10SLD-F]
    45096 SSM Power Supply status is abnormal
  
======================================================================================
Filename: SMT_X10_101.bin    version: 1.01    Date: 04-19-2013    SVN: 352

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
  Support Heavy IO fan control mode
  Solve IPMI login web page is gone on ie8 & ie9

  [X10SLM-F/X10SLL-F]
		45044 IPMI SOL can't working.
    45040 X10SLM-F->please add heavy I/O mode at FAN speed control mode
    44962 IPMI Web GUI is gone with IE broswer
    Set smi pin as input low to aviod bios hang at 9A when system is powered on
   
	[X10SLM+-LN4F/X10SLH-F/X10SL7-F/X10SLA-F]
		45022	IPMI Web Not Working Correctly With Microsoft Internet Explorer
		44869	Email Alert Shows X10_XLH for X10SLH-F

	[X10SLE-F/X10SLD-F/X10SL7-F]
    Set up GPIOR3 for PHY Reset pin on rev 1.01	

	[X10SLE-F/X10SLE-F]
    Optimize the power consumption for these 2 motherboards
    When the system is off, lower the speed of dedicated LAN to 10M.
    When the system power up, the speed will come back to the original speed.

======================================================================================
Filename: SMT_X10_100.bin    version: 1.00    Date: 04-11-2013    SVN: 336

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

 For beta release
 
======================================================================================
Filename: SMT_X10_032.bin    version: 0.32    Date: 04-10-2013    SVN: 335

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
  Support power source page and power monitor page on IPMI web-gui
  Support set system mac address command (need bios support and clear browser cache after updating )

  [X10SLM-F]
    Use ME to read CPU temp instead of peci (Please re-work HW)

  [X10SLM-F/X10SLL-F]
		44361 Chassis intrusion doesn't work
 
	[X10SLM+-LN4F/X10SLH-F/X10SL7-F/X10SLA-F]
		44869	Email Alert Shows X10_XLH for X10SLH-F MB
		44854	All Fans Do Not Stay at Full Speed During Fan Failure
		44833	CPU Overheat Deassertion Thresholds Do Not Follow Thermal Guideline
 
======================================================================================
Filename: SMT_X10_031.bin    version: 0.31    Date: 04-03-2013    SVN: 329

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
  
  Please use factory reset after downloading new firmware

	[X10SLM-F]
		44312	IPMI IKVM Reset function is not working
		
	[X10SLM+-LN4F/X10SLH-F/X10SL7-F/X10SLA-F]
		Add VRM sensor
		44747	Shared LAN Not Working
		44426	[NM] Cannot Read Entire Platform Statistics
				 
======================================================================================
Filename: SMT_X10_030.bin    version: 0.30    Date: 03-29-2013    SVN: 320

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:

	[X10SLM-F/X10SLL-F]
		44672	BIOS IPMI Network Link Status is "No Connect" when IPMI connected
		44322	IP Access Control function is not working
		42897	IPMI Mouse default setting is incorrect

	[X10SL7-F]
		44145	Cannot get any ME information via SMCIPMITool
				
	[X10SLM-LN4F/X10SLH-F]
		44479	IPMI Network Link Status Shows "No Connect"
		44402	Cannot Flash BIOS via OOB

	[X10SLA-F]
		44369 CPU Temp. and Memory Temp. status is "N/A	 	 
		 
======================================================================================
Filename: SMT_X10_029.bin    version: 0.29    Date: 03-25-2013    SVN: 313

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13


Solve:
    Please use progrmmer to flash the firmware

	[X10SLM-F]
		Add board support
======================================================================================

Filename: SMT_X10_028.bin    version: 0.28    Date: 03-21-2013    SVN: 309

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13


Solve:
	1. Fix the issue smcipmitool can't upgrade the firmware.(smcipmitool verion MUST be 2.4.11 and later)
	Usage:
		smcipmitool  <BMC ip>  ADMIN ADMIN ipmi flasha <filename>
	2. Fix the issue SMCIBU will show  the error message "product key not active" when flash BIOS on X10SSL-F.
	
	[X10SLE-F] 
	[X10SLM-F]
		44312	 IPMI IKVM Reset function is not working
		41936  Fan Pulse-Width-Modulation Measurement fail

	[X10SLL-F]
		44382		How do I change the serial output from SOL to COM2 (header) 
		44136		No PCH temperature in IPMI sensor readings

======================================================================================

Filename: SMT_X10_027.bin    version: 0.27    Date: 03-15-2013    SVN: 298

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

**** After updating this firmware, please do factory reset in the maintainance page **** 

Solve:

  Fix the issue upgrading FW without preserving 

  [validation step]

  1.First burning the 00.27 firmware and then do factory reset in maintainance page
  2.Upload the 00.26 firmware and uncheck the preserved box in firmware upload page
  3.After burning process is finished, you can see the sensor positions are changed in sensor page 
    (In 0026, we swap the sensor orders )
  4.If you upgrade from 00.26 to 00.27 by above procedure. Then you will not see the sensors are swapped
  

	[X10SLE-F]
		44446	 "-12V" should be removed from IPMI sensor reading
		44384	 PCH Temperature Missing
		44383	 CPU Temperature Missing

	[X10SLM-LN4F/X10SLH-F]
		44421	 CPU and PCH Temperature Missing With IPMI FW v0.26
		44140	 CPU Overheat LED

	[X10SLM-F]
		44392	 Missing/bogus sensors from ipmitool
		44391	 Missing VCORE and VDIMM in IPMI sensor 
		44344	 IPMI Watchdog NMI function is not working
		44322	 IP Access Control function is not working
		44279	 IPMI sometimes will generate Chassis Intrusion and -12V event in Event log

	[X10SLL-F]
		44381	 Intrusion reset from IPMI will generate weird SEL
		44358	 IPMITOOL sdr command has some extra sensor readings compared to web-gui
		44325	 SEL has some voltage logs after running BMC reset test
		44136	 No PCH temperature in IPMI sensor readings

	[X10SLA-F]
		44369	  CPU Temp. and Memory Temp. status is "N/A" in IPMI Monitor sensor  
		44152	  The FAN pluse test fail 

	[X10SL7-F]
		44353	  [RE-OPEN] - Sensor readings incorrect after system wakes up from S3 

======================================================================================

Filename: SMT_X10_026.bin    version: 0.26    Date: 03-08-2013    SVN: 284

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:

   X10SLE-F
	[44098] Virtual Media: CD-ROM Image ISO Mount Shows Mounted as USB Floppy&Flash 
   
   X10SLL-F
    	[44210]  There won't be any sensor readings sometimes - via web or KCS interface
    	 

New feature:
   Flash dos tool (Must use this version and above.) 


======================================================================================

Filename: SMT_X10_025.bin    version: 0.25    Date: 03-04-2013    SVN: 274

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
  X10SLA-F
	[44152]		The FAN pluse test fail
	[44035]		Memory events log test fail

  X10SLH-F/ X10SLM-LN4F
    [44140]		CPU Overheat LED
    [42624]		DIMM Temperature Sensor Showing N/A 

  X10SLE-F
    [44097]		System Takes Long Time to Boot
    [44094]		No DIMM Temperature Seen on IPMI Web Sensor Readings
  
  X10SLD-F
    [44066]		no hardware monitor in ipmi

  X10SL7-F
    [44056]		IPMI initializes every time I reboot or turn on the system
======================================================================================
Filename: SMT_X10_024.bin    version: 0.24    Date: 02-23-2013    SVN: 252

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
  X10SLH-F/X10XLM-LN4F 
  [43961] Remote Console Preview Takes Longer to Refresh than Previous X9 Generation 

  X10SLL-F/X10XLM-F 
  [43893] Chassis Intrusion always is fail and didn't reset
  [43891] IPMI Event Log has some undefined message when system boot-up or OS reboot
  [43154] Watchdog function is not working 

  X10SL7-F
  [43878] After system wakes up from S3 and boots into OS there are not IPMI sensor readings
  [43329] IPMI LED is not blinking anymore after consective cold reset   

  X10SLE-F
  [43869] Unable to establish LAN session" after running IPMI Cold Reset for 2529 times through onboard LAN1 

  X10SLD-F 
    Add board support
======================================================================================
Filename: SMT_X10_023.bin    version: 0.23    Date: 02-01-2013    SVN: 234

U-Boot build time       : Jan 31 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

  Please clean web page before login the IPMI web page
Solve:
  [X10SLH-F/X10SLE-F] Failed to set static IPMI LAN IP address in BIOS 
  [X10SL7-F] Web-session times out after 15 mins
               Add the web session page and web session timeout value on web page (1-30 minutes)
             Sensor readings appear on IPMI web-gui before all the option ROM have been initialized

  Sometimes After Shutdown From OS and then Power On, Random Sensors Will Disappear

  IPMI restart occasionally after push reset button

  Add AC Power On Event Log on web page
		Ipmi command, 0x30 0x70 0x64
    	Data1  Get/Set ->[0/1] 
    	Data2  set ac power on event flag  -> [0/1] //disable / enable

======================================================================================
Filename: SMT_X10_022.bin    version: 0.22    Date: 02-01-2013    SVN: 218

U-Boot build time       : Jan 31 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
   [X10SL7-F/X10SLM-LN4F]IPMI KVM: No IKVM signal when resolution is set to 1024x768x8 mode
   [X10SL7-F] PCH temperature is shown as 4 degrees (Intel bug, work around solution)
   [X10SLL-F] Workaround solution to fix the power button can't work properly.
   [X10SLE-F] Support HDD sensor

    Solve the language hang problem in ikvm viewer
    Solve the SDR could not be updated [Denis]

======================================================================================
Filename: SMT_X10_021.bin    version: 0.21    Date: 01-30-2013

U-Boot build time       : 12-19 2012
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
[X10SLL-F/X10SLL-F] For CM release
                    set GPIOE5 as input pin after setting to output pin state to avoid power button fail solution

======================================================================================
Filename: SMT_X10_020.bin    version: 0.20    Date: 01-29-2013    SVN: 203

U-Boot build time       : 12-19 2012
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
[X10SLL-F/X10SLL-F] For CM release
                       set GPIOE5 output high at boot code stage to avoid i210 crash down
                       set GPIOC1 input, GPIOE2 output 
                       set GPIOE3 output
 
======================================================================================

Filename: SMT_X10_019.bin    version: 0.19    Date: 01-25-2013    SVN: 201

U-Boot build time       : 12-19 2012
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Please use programmer to burn this firmware
Please clear Java cache (SOL verion is updated)
Solve:
  [X10SLM-LN4F] Unreliable IPMI connection on shared LAN
  [X10SL7-F]    SOL Can Open Multiple Windows
  [X10SLE-F]    Add sensor list (HDD sensor is not ready)
 
======================================================================================
Filename: SMT_X10_018.bin    version: 0.18    Date: 01-18-2013    SVN: 187

U-Boot build time       : 12-19 2012
Java SOL Viewer version : v0.5.8
Java iKVM Viwer version : v1.69 r13

Please uncheck the Preserve Configuration box to restore the factory default setting of BMC
 
Solve:

   [X10XL7-F]    Fix vcore senor value is not right
                 Systerm Temperature (RT1) Event Cannot Be Logged
                 No IPMI Log for PCH Overheat  Hardware; IPMI

   [X10SLM-LN4F] KVM window closes itself

   [X10SLL-F]    The FAN speed control curves for CPU can't follow thermal design guide

   [X10SLE-F]    Add board support
 
======================================================================================

Filename: SMT_X10_017.bin    version: 0.17    Date: 01-11-2013    SVN: 175

Solve
	Preview function is working (  Remember it takes about 6 seconds to refresh the 
	                               screenshot in X10, and 1280 x 1024 resolution maximum )
  Device 3 function works at virtual storge
  Solve when switching to share LAN, can't get IP and network message is not correct on
    network page
  Solve peripheral Temperature overheat asserted event is not log in SEL.
  Solve BMC will has kernel panic after several times change on Lan Interface setting in Network configuration.

  [X10SLM_LN4F/X10SLH-F/X10SL7-F] Correct vcore voltage on web page 
                                  No overheat beep alarm (controlled by NCT6776)
                                  Correct system temp disappeared in sensor reading page
                                  Correct sensors will disappear in sensor reading page
                                  
  [X10SLL-F/X10SLM-F] 						Add watchdog function
  																Add Beep function (controlled by AST2400 PWM)
 
======================================================================================
Filename: SMT_X10_016.bin    version: 0.16    Date: 01-07-2013    SVN: 152

Solve
  [X10SL7-F/X10SLA-F] 						Add board support
  [X10SLM_LN4F/X10SLH-F/X10SL7-F] Correct vcore voltage on web page 
  [X10SLL-F/X10SLM-F] 						Correct -12v sensor voltage on web page
  																Add watchdog function
 
  Known issues
  1. Preview has some problems
======================================================================================

Filename: SMT_X10_015.bin    version: 0.15    Date: 12-28-2012    SVN: 134

Solve
  Fan control function is ok
  [X10SLH-F/SLM_LN4F] Chassis Intrusion Shows Wrong Time Stamp in Event Log
  [X10SLH-F/SLM_LN4F] Fine tune the parameters of superio NCT6776 based on sensor list
  [X10SLL-F/X10SLM-F] -12v sensor reading fails
 
Known issues
1. Preview has some problems

======================================================================================

Filename: SMT_X10_014.bin    version: 0.14    Date: 12-21-2012    SVN: 116

Solve
	Virtual media funciton is working
  Preview function is working
  It show wrong share/dedicate information on network config web page
  Add GUID for ATENX10 BMC is C 0 0 1 M S
  Set default Mac address of Bootloader is 00:00:00:00:00:00
  
	[X10SLL-F/X10SLM-F]			Voltage sensor has been fined tune
												  Power fail led and led works correctly
												  
	[X10SLH-F/X10SLM-LN4F]	Fan Fail Event Log for FAN1 and FAN2 Missing Lower Non-Critical Status
													Factory Default Will Cause BMC to Lose MAC Address 
	
	[X10SL7] 								support   

Known issues
1. Fan fail and pwm has some problems. 
2. [X10SLL-F/X10SLM-F] Front & Rear temperature sensors, smbus may be failed after long time testing

======================================================================================

Filename: SMT_X10_013.bin    version: 0.13    Date: 12-13-2012    SVN: 95

Solve
  Important !! <=Please use programmer to burn this firmware if previous firmware is older then fw.012 verion

1. Add board id BOARD_X10_SLM_LN4 0x806

2.[X10SLM-LN4] 1.Change Vcore threshold, M,B,K2,K1.
               2.Change ˇ§CPU VTTˇ¨ to ˇ§-12Vˇ¨ and Adjust this threshold, M, B, K2, K1
3. [X10SLM]    1.Add all sensors [except chassis intrusion]

Known issues
1. It can only mount virtual media at the 1st time, and umount/remount funciton failed
2. Preview is not working


======================================================================================

Filename: SMT_X10_012.bin    version: 0.12    Date: 12-07-2012    SVN: 73


Solve
1. Enable COM1 & COM2 at bootloader 
   Important !! <=Please use programmer to burn this firmware
2. Network function works
3. [X10SLL-F/X10SLM-F] sensors wroks (except CPU peci temp, overheat function)
4. UID funciton works
5. SOL function works
6  Post snoppy function works on IPMI web page
7. [X10SLH-F/X10SLM-LN4F] sensors wroks [except CPU peci temp, overheat function]

Known issues
1. Virtual media is not working
2. Remote control is not working
3. [X10SLL-F/X10SLM-F] fan speed is full speed now

======================================================================================

Filename: SMT_X10_011.bin    version: 0.11    Date: 11-30-2012    SVN: 49

This bin code is for all X10 boards.

Solve
1. Remote function ok
2. KCS works. bios please use KCS4 & KCS5; ipmicfg and other utilities will use KCS2 & KCS3
3. Add board id
 

Known issues
1.	Network driver has bugs. The failover mode fails, and dynamic plugging in/pulling out the network may fail. 
    After setting the bmc address, you may have to ac power off and power on again, and the network works.
2.	Sensors are working except memory temperature detection.
3.	SOL is not working
7.	Virtual media is not working
8.	Sensor without SIO (only completed 6776 SIO sensor)

======================================================================================

Filename: SMT_X10_010.bin    version: 0.10    Date: 11-26-2012    SVN: 33

This bin code is for all X10 boards.

Known issues
1.	Network driver has bugs. The failover mode fails, and dynamic plugging in/pulling out the network may fail. 
    After setting the bmc address, you may have to ac power off and power on again, and the network works.
2.	Sensors are working except memory temperature detection.
3.	In SOL, only one way is passed
4.	remote control is not working
5.	In KCS, only CA2 & CA3 works. Currently, bios & bmc cannot talk to each other.
6.	Ipmicfg works.
7.	Virtual media is not working
8.	Sensor without SIO (only completed 6776 SIO sensor)


======================================================================================