X10SLD Release note.
--------------------------------------------------------------------------------------------
-----------------------------------------------------------------------------------
 CPU Microcode          | Option ROM/EFI driver                 | Intel RC/TXT/ME
-----------------------------------------------------------------------------------
 CPUID FAMILY           | Aspeed VBIOS :  0.96.00               | RC Package :1.2.0
 306C1 Haswell A0  : 13 | Intel SATA RAID : 3.6.0.1023          |
 306C2 Haswell B0  : 06 | Intel RSTe SATA driver : 3.6.0.1023   |
 306C3 Haswell C0  : 09 |                                       | ME : 3.0.4.164
------------------------------------------------------------------------------------

-------------------------------------------------------------------------------
BIOS : X10SLD3.613			Release Date  : Jun-13-2013
BIOS revision: 1.0a         BIOS Engineer : Curtis Wen
BIOS Checksum: 0x4821BD82

1. AOC-CGP-I2 MAC address show in IPMI Web GUI
   Description: LAB report, can't see AOC-CGP-I2 MAC address in IPMI web GUI
   Validation:  Please check in IPMI web GUI

2. USB performance not stable issue
   Description: LAB report, USB write performance not stable
   Validation:  Please verify with this BIOS, and also check USB related function

3. OOB Support
   Description: Lab report, use OOB Load Factory Default w/ Reboot command have problem
   Validation:  Please verify with this BIOS

4. Correct setup item wording to meet silkscreen
   Description: Correct setup item wording to meet silkscreen
   Validation:  Please check with this BIOS

5. Default enable SOL console redirection
   Description: LAB report, after update BIOS, IPMI SOL will disconnect.
   Validation:  Please check with this BIOS

6. Update CPU microcode 
   Description: Update CPU micro code
   Validation:  Run mcu_sig.exe in DOS or CPU-z in Windows with the CPU installed.
                Haswell A0(CPUID 306C1), ver 13
                Haswell B0(CPUID 306C2), ver 06
                Haswell C0(CPUID 306C3), ver 09

6. Change BIOS revision to 1.0a
   Description: BIOS version control
   Validation:  Please check BIOS version in POST screen, setup menu and SMBIOS Type 0 Release version field

-------------------------------------------------------------------------------
BIOS : X10SLD3.522			Release Date  : May-22-2013
BIOS revision: 1.00         BIOS Engineer : Curtis Wen
BIOS Checksum: 0x1CD000E2

1. First release. 
