IPMI Firmware Release Note
----------------------------
Filename: SMT_X10_109.bin    version: 1.09    Date: 06-14-2013    SVN: 451

U-Boot build time       : Jun 14 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
  1.Add sensor support on X10SEAA_LN4F
  2.update sensor list according to IPMI_voltage_sensors_threhold_R01.xlsx
  2.#46139          LAN 1 disconnect after IPMI factory default setting
  2.#46132					-12V Events Lgged During IPMI KVM Stress
  3.#45908,#45905		IPMI Logs Non-Critical Events
  4.#45778					Remote Console Preview display is abnormal
  5.#46059					Random - Update BIOS setting via OOB with option "--reboot" fail.
  6.#46056					Random - The process is loop when update BIOS via OOB.  
     
=====================================================================================

Filename: SMT_X10_108.bin    version: 1.08    Date: 06-06-2013    SVN: 432

U-Boot build time       : May 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
  1.fine tune sensor values on X10DRI_T, X10QBI_F
  2.#46010											Please Change FAN1 Sensor to FAN
  3.#45939											Power Fail Logs About Every 5 Minutes
  4.#45938											HeavyIO FSC: FANA RPM Higher at 39C and lower at 42C 
  5.#45937											HeavyIO FSC Mode FanA Speed Higher Than Thermal Guideline Specification 
  6.#45928,#45926,#45908,#45905	IPMI Logs Non-Critical Events 
  7.#44075											dmesg has a "ipmi_si: Error clearing flags: cc" error message after running E-burn stress
        
=====================================================================================
Filename: SMT_X10_107.bin    version: 1.07    Date: 05-30-2013    SVN: 417

U-Boot build time       : May 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
	
	Fine tune VBAT, -12V sensor threshold on X10SLM-F, X10SLL-F and X10XLM+_LN4F
        
=====================================================================================

Filename: SMT_X10_106.bin    version: 1.06    Date: 05-27-2013    SVN: 410

U-Boot build time       : May 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
	
	Please clear Java cache (iKVM verion is updated)
  Please uncheck the preserved box in firmware upload page
  
  1.Add sensor on X10SLL+_F, X10QBI_T
  2.#45801,#45725,#45725,#45481		[OOB] System Will Shutdown After Flash BIOS Via OOB and Reset .
  3.#45712												There are many Vcore events in IPMI SEL when running eburn LIN test
  4.#45621,#45785									IPMI Virtual Keyboard didn't have Swiss language item
  5.#45682												FAN speed will up to 100% when IPMI initializing
        
=====================================================================================
Filename: SMT_X10_105.bin    version: 1.05    Date: 05-20-2013    SVN: 398

U-Boot build time       : May 20 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r18

Solve:
  
   1. [X10SLM-F/X10SLL-F] Output 50@ dutycycle when bmc reboots 
   2. [X10SLM-F/X10SLL-F] Change sensor name to "3.3V AUX"
   3. [X10SLL-SF]         BMC can't boot successfully
   4. #45619              It not work if run "ChnageBIOScfg" and "Loaddefault" of OOB functions
   5. [X10DRI_F]          Add sensor supports
   6. Preserve the whole 64k block where SMIBIOS data resides.
      [Validation Steps]
      a. Go to the bios update page 
      b. Update bios image only with preserving SMBIOS.
      
=====================================================================================

Filename: SMT_X10_104.bin    version: 1.04    Date: 05-10-2013    SVN: 388

U-Boot build time       : May 9 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r18

Solve:

  1. Output 100@ dutycycle for X10SLM-F/X10SLL-F. 
  2. Update the thermal curve for heavy IO fan mode.
  
  [45018] Sometimes Auto-Resize Window Does Not Work When Booting into OS 
  [45209] IPMI KVM window doesn't have Power Control option 
          Support high resolution up to 1920*1200.
  [45463,45401,45381,45347] BMC incorrect reponse detected during eburn test  
  
=====================================================================================
Filename: SMT_X10_103.bin    version: 1.03    Date: 05-03-2013    SVN: 376

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:

	Add OOB event log.
  	OOB file build date mis-match (Sensor type : 0xCA, Event Data 1)
	  OOB feature initial failure (Sensor type : 0xCA, Event Data 2)  
  
	[X10SL7-F]
  45347 BMC incorrect reponse detected during eburn test  
   
	[X10SLE-F/X10SLD-F]
  45381 BMC incorrect reponse detected during eburn test  
  
  
======================================================================================
Filename: SMT_X10_102.bin    version: 1.02    Date: 04-26-2013    SVN: 367

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:

  [X10SLM-F/X10SLL-F]
		45067 part of the Eburn stress test is fail (ipmi_si: Error clearing flags: cc) 
   
	[X10SLM+-LN4F/X10SLH-F/X10SL7-F/X10SLA-F]
		45231	Please Change Bios String in IPMI Web System Information Page to BIOS

	[X10SLE-F/X10SLD-F]
    45096 SSM Power Supply status is abnormal
  
======================================================================================
Filename: SMT_X10_101.bin    version: 1.01    Date: 04-19-2013    SVN: 352

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
  Support Heavy IO fan control mode
  Solve IPMI login web page is gone on ie8 & ie9

  [X10SLM-F/X10SLL-F]
		45044 IPMI SOL can't working.
    45040 X10SLM-F->please add heavy I/O mode at FAN speed control mode
    44962 IPMI Web GUI is gone with IE broswer
    Set smi pin as input low to aviod bios hang at 9A when system is powered on
   
	[X10SLM+-LN4F/X10SLH-F/X10SL7-F/X10SLA-F]
		45022	IPMI Web Not Working Correctly With Microsoft Internet Explorer
		44869	Email Alert Shows X10_XLH for X10SLH-F

	[X10SLE-F/X10SLD-F/X10SL7-F]
    Set up GPIOR3 for PHY Reset pin on rev 1.01	

	[X10SLE-F/X10SLE-F]
    Optimize the power consumption for these 2 motherboards
    When the system is off, lower the speed of dedicated LAN to 10M.
    When the system power up, the speed will come back to the original speed.

======================================================================================
Filename: SMT_X10_100.bin    version: 1.00    Date: 04-11-2013    SVN: 336

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

 For beta release
 
======================================================================================
Filename: SMT_X10_032.bin    version: 0.32    Date: 04-10-2013    SVN: 335

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
  Support power source page and power monitor page on IPMI web-gui
  Support set system mac address command (need bios support and clear browser cache after updating )

  [X10SLM-F]
    Use ME to read CPU temp instead of peci (Please re-work HW)

  [X10SLM-F/X10SLL-F]
		44361 Chassis intrusion doesn't work
 
	[X10SLM+-LN4F/X10SLH-F/X10SL7-F/X10SLA-F]
		44869	Email Alert Shows X10_XLH for X10SLH-F MB
		44854	All Fans Do Not Stay at Full Speed During Fan Failure
		44833	CPU Overheat Deassertion Thresholds Do Not Follow Thermal Guideline
 
======================================================================================
Filename: SMT_X10_031.bin    version: 0.31    Date: 04-03-2013    SVN: 329

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
  
  Please use factory reset after downloading new firmware

	[X10SLM-F]
		44312	IPMI IKVM Reset function is not working
		
	[X10SLM+-LN4F/X10SLH-F/X10SL7-F/X10SLA-F]
		Add VRM sensor
		44747	Shared LAN Not Working
		44426	[NM] Cannot Read Entire Platform Statistics
				 
======================================================================================
Filename: SMT_X10_030.bin    version: 0.30    Date: 03-29-2013    SVN: 320

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:

	[X10SLM-F/X10SLL-F]
		44672	BIOS IPMI Network Link Status is "No Connect" when IPMI connected
		44322	IP Access Control function is not working
		42897	IPMI Mouse default setting is incorrect

	[X10SL7-F]
		44145	Cannot get any ME information via SMCIPMITool
				
	[X10SLM-LN4F/X10SLH-F]
		44479	IPMI Network Link Status Shows "No Connect"
		44402	Cannot Flash BIOS via OOB

	[X10SLA-F]
		44369 CPU Temp. and Memory Temp. status is "N/A	 	 
		 
======================================================================================
Filename: SMT_X10_029.bin    version: 0.29    Date: 03-25-2013    SVN: 313

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13


Solve:
    Please use progrmmer to flash the firmware

	[X10SLM-F]
		Add board support
======================================================================================

Filename: SMT_X10_028.bin    version: 0.28    Date: 03-21-2013    SVN: 309

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13


Solve:
	1. Fix the issue smcipmitool can't upgrade the firmware.(smcipmitool verion MUST be 2.4.11 and later)
	Usage:
		smcipmitool  <BMC ip>  ADMIN ADMIN ipmi flasha <filename>
	2. Fix the issue SMCIBU will show  the error message "product key not active" when flash BIOS on X10SSL-F.
	
	[X10SLE-F] 
	[X10SLM-F]
		44312	 IPMI IKVM Reset function is not working
		41936  Fan Pulse-Width-Modulation Measurement fail

	[X10SLL-F]
		44382		How do I change the serial output from SOL to COM2 (header) 
		44136		No PCH temperature in IPMI sensor readings

======================================================================================

Filename: SMT_X10_027.bin    version: 0.27    Date: 03-15-2013    SVN: 298

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

**** After updating this firmware, please do factory reset in the maintainance page **** 

Solve:

  Fix the issue upgrading FW without preserving 

  [validation step]

  1.First burning the 00.27 firmware and then do factory reset in maintainance page
  2.Upload the 00.26 firmware and uncheck the preserved box in firmware upload page
  3.After burning process is finished, you can see the sensor positions are changed in sensor page 
    (In 0026, we swap the sensor orders )
  4.If you upgrade from 00.26 to 00.27 by above procedure. Then you will not see the sensors are swapped
  

	[X10SLE-F]
		44446	 "-12V" should be removed from IPMI sensor reading
		44384	 PCH Temperature Missing
		44383	 CPU Temperature Missing

	[X10SLM-LN4F/X10SLH-F]
		44421	 CPU and PCH Temperature Missing With IPMI FW v0.26
		44140	 CPU Overheat LED

	[X10SLM-F]
		44392	 Missing/bogus sensors from ipmitool
		44391	 Missing VCORE and VDIMM in IPMI sensor 
		44344	 IPMI Watchdog NMI function is not working
		44322	 IP Access Control function is not working
		44279	 IPMI sometimes will generate Chassis Intrusion and -12V event in Event log

	[X10SLL-F]
		44381	 Intrusion reset from IPMI will generate weird SEL
		44358	 IPMITOOL sdr command has some extra sensor readings compared to web-gui
		44325	 SEL has some voltage logs after running BMC reset test
		44136	 No PCH temperature in IPMI sensor readings

	[X10SLA-F]
		44369	  CPU Temp. and Memory Temp. status is "N/A" in IPMI Monitor sensor  
		44152	  The FAN pluse test fail 

	[X10SL7-F]
		44353	  [RE-OPEN] - Sensor readings incorrect after system wakes up from S3 

======================================================================================

Filename: SMT_X10_026.bin    version: 0.26    Date: 03-08-2013    SVN: 284

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:

   X10SLE-F
	[44098] Virtual Media: CD-ROM Image ISO Mount Shows Mounted as USB Floppy&Flash 
   
   X10SLL-F
    	[44210]  There won't be any sensor readings sometimes - via web or KCS interface
    	 

New feature:
   Flash dos tool (Must use this version and above.) 


======================================================================================

Filename: SMT_X10_025.bin    version: 0.25    Date: 03-04-2013    SVN: 274

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
  X10SLA-F
	[44152]		The FAN pluse test fail
	[44035]		Memory events log test fail

  X10SLH-F/ X10SLM-LN4F
    [44140]		CPU Overheat LED
    [42624]		DIMM Temperature Sensor Showing N/A 

  X10SLE-F
    [44097]		System Takes Long Time to Boot
    [44094]		No DIMM Temperature Seen on IPMI Web Sensor Readings
  
  X10SLD-F
    [44066]		no hardware monitor in ipmi

  X10SL7-F
    [44056]		IPMI initializes every time I reboot or turn on the system
======================================================================================
Filename: SMT_X10_024.bin    version: 0.24    Date: 02-23-2013    SVN: 252

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
  X10SLH-F/X10XLM-LN4F 
  [43961] Remote Console Preview Takes Longer to Refresh than Previous X9 Generation 

  X10SLL-F/X10XLM-F 
  [43893] Chassis Intrusion always is fail and didn't reset
  [43891] IPMI Event Log has some undefined message when system boot-up or OS reboot
  [43154] Watchdog function is not working 

  X10SL7-F
  [43878] After system wakes up from S3 and boots into OS there are not IPMI sensor readings
  [43329] IPMI LED is not blinking anymore after consective cold reset   

  X10SLE-F
  [43869] Unable to establish LAN session" after running IPMI Cold Reset for 2529 times through onboard LAN1 

  X10SLD-F 
    Add board support
======================================================================================
Filename: SMT_X10_023.bin    version: 0.23    Date: 02-01-2013    SVN: 234

U-Boot build time       : Jan 31 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

  Please clean web page before login the IPMI web page
Solve:
  [X10SLH-F/X10SLE-F] Failed to set static IPMI LAN IP address in BIOS 
  [X10SL7-F] Web-session times out after 15 mins
               Add the web session page and web session timeout value on web page (1-30 minutes)
             Sensor readings appear on IPMI web-gui before all the option ROM have been initialized

  Sometimes After Shutdown From OS and then Power On, Random Sensors Will Disappear

  IPMI restart occasionally after push reset button

  Add AC Power On Event Log on web page
		Ipmi command, 0x30 0x70 0x64
    	Data1  Get/Set ->[0/1] 
    	Data2  set ac power on event flag  -> [0/1] //disable / enable

======================================================================================
Filename: SMT_X10_022.bin    version: 0.22    Date: 02-01-2013    SVN: 218

U-Boot build time       : Jan 31 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
   [X10SL7-F/X10SLM-LN4F]IPMI KVM: No IKVM signal when resolution is set to 1024x768x8 mode
   [X10SL7-F] PCH temperature is shown as 4 degrees (Intel bug, work around solution)
   [X10SLL-F] Workaround solution to fix the power button can't work properly.
   [X10SLE-F] Support HDD sensor

    Solve the language hang problem in ikvm viewer
    Solve the SDR could not be updated [Denis]

======================================================================================
Filename: SMT_X10_021.bin    version: 0.21    Date: 01-30-2013

U-Boot build time       : 12-19 2012
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
[X10SLL-F/X10SLL-F] For CM release
                    set GPIOE5 as input pin after setting to output pin state to avoid power button fail solution

======================================================================================
Filename: SMT_X10_020.bin    version: 0.20    Date: 01-29-2013    SVN: 203

U-Boot build time       : 12-19 2012
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
[X10SLL-F/X10SLL-F] For CM release
                       set GPIOE5 output high at boot code stage to avoid i210 crash down
                       set GPIOC1 input, GPIOE2 output 
                       set GPIOE3 output
 
======================================================================================

Filename: SMT_X10_019.bin    version: 0.19    Date: 01-25-2013    SVN: 201

U-Boot build time       : 12-19 2012
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Please use programmer to burn this firmware
Please clear Java cache (SOL verion is updated)
Solve:
  [X10SLM-LN4F] Unreliable IPMI connection on shared LAN
  [X10SL7-F]    SOL Can Open Multiple Windows
  [X10SLE-F]    Add sensor list (HDD sensor is not ready)
 
======================================================================================
Filename: SMT_X10_018.bin    version: 0.18    Date: 01-18-2013    SVN: 187

U-Boot build time       : 12-19 2012
Java SOL Viewer version : v0.5.8
Java iKVM Viwer version : v1.69 r13

Please uncheck the Preserve Configuration box to restore the factory default setting of BMC
 
Solve:

   [X10XL7-F]    Fix vcore senor value is not right
                 Systerm Temperature (RT1) Event Cannot Be Logged
                 No IPMI Log for PCH Overheat  Hardware; IPMI

   [X10SLM-LN4F] KVM window closes itself

   [X10SLL-F]    The FAN speed control curves for CPU can't follow thermal design guide

   [X10SLE-F]    Add board support
 
======================================================================================

Filename: SMT_X10_017.bin    version: 0.17    Date: 01-11-2013    SVN: 175

Solve
	Preview function is working (  Remember it takes about 6 seconds to refresh the 
	                               screenshot in X10, and 1280 x 1024 resolution maximum )
  Device 3 function works at virtual storge
  Solve when switching to share LAN, can't get IP and network message is not correct on
    network page
  Solve peripheral Temperature overheat asserted event is not log in SEL.
  Solve BMC will has kernel panic after several times change on Lan Interface setting in Network configuration.

  [X10SLM_LN4F/X10SLH-F/X10SL7-F] Correct vcore voltage on web page 
                                  No overheat beep alarm (controlled by NCT6776)
                                  Correct system temp disappeared in sensor reading page
                                  Correct sensors will disappear in sensor reading page
                                  
  [X10SLL-F/X10SLM-F] 						Add watchdog function
  																Add Beep function (controlled by AST2400 PWM)
 
======================================================================================
Filename: SMT_X10_016.bin    version: 0.16    Date: 01-07-2013    SVN: 152

Solve
  [X10SL7-F/X10SLA-F] 						Add board support
  [X10SLM_LN4F/X10SLH-F/X10SL7-F] Correct vcore voltage on web page 
  [X10SLL-F/X10SLM-F] 						Correct -12v sensor voltage on web page
  																Add watchdog function
 
  Known issues
  1. Preview has some problems
======================================================================================

Filename: SMT_X10_015.bin    version: 0.15    Date: 12-28-2012    SVN: 134

Solve
  Fan control function is ok
  [X10SLH-F/SLM_LN4F] Chassis Intrusion Shows Wrong Time Stamp in Event Log
  [X10SLH-F/SLM_LN4F] Fine tune the parameters of superio NCT6776 based on sensor list
  [X10SLL-F/X10SLM-F] -12v sensor reading fails
 
Known issues
1. Preview has some problems

======================================================================================

Filename: SMT_X10_014.bin    version: 0.14    Date: 12-21-2012    SVN: 116

Solve
	Virtual media funciton is working
  Preview function is working
  It show wrong share/dedicate information on network config web page
  Add GUID for ATENX10 BMC is C 0 0 1 M S
  Set default Mac address of Bootloader is 00:00:00:00:00:00
  
	[X10SLL-F/X10SLM-F]			Voltage sensor has been fined tune
												  Power fail led and led works correctly
												  
	[X10SLH-F/X10SLM-LN4F]	Fan Fail Event Log for FAN1 and FAN2 Missing Lower Non-Critical Status
													Factory Default Will Cause BMC to Lose MAC Address 
	
	[X10SL7] 								support   

Known issues
1. Fan fail and pwm has some problems. 
2. [X10SLL-F/X10SLM-F] Front & Rear temperature sensors, smbus may be failed after long time testing

======================================================================================

Filename: SMT_X10_013.bin    version: 0.13    Date: 12-13-2012    SVN: 95

Solve
  Important !! <=Please use programmer to burn this firmware if previous firmware is older then fw.012 verion

1. Add board id BOARD_X10_SLM_LN4 0x806

2.[X10SLM-LN4] 1.Change Vcore threshold, M,B,K2,K1.
               2.Change ˇ§CPU VTTˇ¨ to ˇ§-12Vˇ¨ and Adjust this threshold, M, B, K2, K1
3. [X10SLM]    1.Add all sensors [except chassis intrusion]

Known issues
1. It can only mount virtual media at the 1st time, and umount/remount funciton failed
2. Preview is not working


======================================================================================

Filename: SMT_X10_012.bin    version: 0.12    Date: 12-07-2012    SVN: 73


Solve
1. Enable COM1 & COM2 at bootloader 
   Important !! <=Please use programmer to burn this firmware
2. Network function works
3. [X10SLL-F/X10SLM-F] sensors wroks (except CPU peci temp, overheat function)
4. UID funciton works
5. SOL function works
6  Post snoppy function works on IPMI web page
7. [X10SLH-F/X10SLM-LN4F] sensors wroks [except CPU peci temp, overheat function]

Known issues
1. Virtual media is not working
2. Remote control is not working
3. [X10SLL-F/X10SLM-F] fan speed is full speed now

======================================================================================

Filename: SMT_X10_011.bin    version: 0.11    Date: 11-30-2012    SVN: 49

This bin code is for all X10 boards.

Solve
1. Remote function ok
2. KCS works. bios please use KCS4 & KCS5; ipmicfg and other utilities will use KCS2 & KCS3
3. Add board id
 

Known issues
1.	Network driver has bugs. The failover mode fails, and dynamic plugging in/pulling out the network may fail. 
    After setting the bmc address, you may have to ac power off and power on again, and the network works.
2.	Sensors are working except memory temperature detection.
3.	SOL is not working
7.	Virtual media is not working
8.	Sensor without SIO (only completed 6776 SIO sensor)

======================================================================================

Filename: SMT_X10_010.bin    version: 0.10    Date: 11-26-2012    SVN: 33

This bin code is for all X10 boards.

Known issues
1.	Network driver has bugs. The failover mode fails, and dynamic plugging in/pulling out the network may fail. 
    After setting the bmc address, you may have to ac power off and power on again, and the network works.
2.	Sensors are working except memory temperature detection.
3.	In SOL, only one way is passed
4.	remote control is not working
5.	In KCS, only CA2 & CA3 works. Currently, bios & bmc cannot talk to each other.
6.	Ipmicfg works.
7.	Virtual media is not working
8.	Sensor without SIO (only completed 6776 SIO sensor)


======================================================================================