================================================
Notice:
================================================

For MB with IPMI Firmware 2.19 and above:

- Flash BIOS 3.0a first with package X9DRW3.808.zip, then

- Flash SMM_X9_2_35.ima from package SMM_X9_2_35.zip in Web or DOS mode.

For MB with IPMI firmware before 2.19:

- Use RKCS220.zip to update both BIOS & IPMI f/w in DOS mode. (Update process: BIOS a IPMI Recovery Image a IPMI firmware 2.20)

================================================
IPMI firmware update
================================================

1. Unzip SMM_X9_2_35.zip files to a bootable DOS USB Flash Disk or USB hard drive.

2. Plug USB Flash Disk or USB hard drive to MB USB port

3. Boot up system to DOS

4. Execute "rkcsflsh SMM_X9_2_35.ima" (without the quotes)

5. After update completes, reboot the system 	

================================================
IPMI update from firmware older than 2.19
================================================

1. Unzip RKCS220.zip to bootable DOS USB Flash Disk or USB hard drive.

2. Plug USB Flash Disk or USB hard drive to MB USB port

3. Set Boot disk to USB Hard Drive on BIOS set up 

4. boot up system to DOS

5. Execute RKCS220.BAT

6. Flashing X9DRW3.808 (BIOS 3.0a)

7. Flashing REC.ima

8. Flashing 220.ima

9. System will reboot after upgrade successful.

NOTE:  Please contact Tech Support to get BIOS 3.0a (X9DRW3.808) 