Filename: SMT_X10_188.bin version: 1.88 Date: 01-26-2015

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

1.
     Category: Fix
     Description:
      Enlarge VBAT voltage to avoid false event log

     Infected motherboard: A1SA2
     Affected functions:
     Validation :
         1. Do SAT or LAN test to check if false event log launch

2.
     Category: Fix
     Description:
      [59315] Time stamp on power consumption page not shown correctly

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Login the webgui and goto power consumption page.
         2. Check the time stamp.

3.
     Category: Fix
     Description:
      Node1 sensors are missing on IPMI web gui

     Infected motherboard: A1SA2 HW 1.01 version
     Affected functions:
     Validation :
         1. Check IPMI sensor reading web gui

4.
     Category: New Feature
     Description:
       Add Config_ID into the Multi-node function.

     Infected motherboard: Twin series 
     Affected functions: Multi-Node function.
     Validation :
         1. Login the Webgui.
         2. Check the Multinode page.

5.
     Category: Fix
     Description:
      [59401] Fans do not change speed at all.

     Infected motherboard: X10QBi
     Affected functions:
     Validation :
         1. Login the webgui and set the fan mode to full speed.
         2. Make one fan fail and check the fan speed of other fans.

6.
     Category: Fix
     Description:
      [59004] [DVT] Onboard buzzer keep beeping after CPU2 cooled down to normal temperature from overheat.

     Infected motherboard: X10QRH+
     Affected functions:
     Validation :
         1. Make the CPU overheat and hear beeping.
         2. Cool down the CPU, and check the beeping is stop.

7.
     Category: Fix
     Description:
      [58537] The Fan speed doesn't go down when the HDD temperature goes down.

     Infected motherboard: X10QBI
     Affected functions:
     Validation :
         1. Change the fan mode from Standard to Full. See the fans become full speed or not.
         2. Change the fan mode from Full to Heavy IO. See the fan behavior.
         3. Change the fan mode from Heavy IO back to Standard. See the fan behavior.

8.
     Category: Fix
     Description:
      [59386] Standard speed mode is missing from IPMI fan mode setting menu 

     Infected motherboard: X10DRD, X10DRD-L
     Affected functions:
     Validation :
         1. Check fan mode

9.
     Category: Fix
     Description:
      Support on-board mux function

     Infected motherboard: X10DRX
     Affected functions:
     Validation :
         1. Plug in LSI3108 card on Slot1-8.
         2. Power on and check if SAS sensor can be seen on IPMI sensor reading web page

10.
     Category: Enhancement
     Description:
      Support Expander On-die temperature and FSC

     Infected motherboard: X10DRT-P
     Affected functions:
     Validation :
         1. use BPN-ADP-E1C-L 
         2. Expander sensor will be shown on sensor reading web page
         3. The FSC is the same as 10G sensor. Please heat it and check FSC

11.
     Category: Work around
     Description:
      Support 1.01B X10SRL cpu & memory & 1.01B X10SRI cpu vrm sensor readings

     Infected motherboard: X10SRL & X10SRI
     Affected functions:
     Validation :
         1. Check the vrm sensor reading on X10SRL 1.01B & X10SRI 1.01B
         2. Also, please check the older motherboard version, X10SRL 1.01 & X10SRI 1.01

12.
     Category: Fix
     Description:
      [59507] X10DRT-L sensor reading has "IB temp" item show N/A 
     Infected motherboard: X10DRT-L
     Affected functions:
     Validation :
         1. update new bios which will tell bmc IB sensor is on the motherboard
         2. Check the sensor reading web gui

12.
     Category: Security Fix
     Description:
      ICMP timestamp issue
     Infected motherboard: All
     Affected functions:
     Validation :
		1. please use Retina network security scanner to scan IPMI fw.

--------------------------------------------------------------------------
Filename: SMT_X10_187.bin version: 1.87 Date: 01-14-2015

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

1.
     Category: Enhancement
     Description:
      Add Preserve SDR checkbox on  Firmware upload web page
     Infected motherboard: All
     Affected functions:
     Validation :
         1. Uncheck this option, the old SDR will be removed after new FW is updated
2.
     Category: Fix
     Description:
      [58968] IPMI Set "PW consumption" Sensor Reading Low Limit Value Too High (IPMI FW:1.85)

     Infected motherboard: X10DRT-P
     Affected functions:
     Validation :
         1. Observe "PW consumption" Sensor. High non-recoverable values should be higher than High crtital value

3.
     Category: Work around 
     Description:
      Let RT2 value is equal to (PCH - 4) value
     Infected motherboard: X10DRU-+
     Affected functions:
     Validation :
         1. After IPMI FW is updated, use this command to remove old SDR
            SMCIPMITool.exe 10.133.176.225 ADMIN ADMIN ipmi raw 30 44
         2. Check if RT2 value is equal to (PCH-4) value

4.
     Category: Fix
     Description:
      [59198] CPU FSC cannot meet thermal guide SIM_TDG REV. 4.04 (11192014)
     Infected motherboard: X10DRD-L
     Affected functions:
     Validation :
         1. Check CPU PUE3 FSC meets thermal guide 4.04 

--------------------------------------------------------------------------

Filename: SMT_X10_186.bin version: 1.86 Date: 01-xx-2015

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

1.
     Category: Fix
     Description:
      [58968] IPMI Set "PW consumption" Sensor Reading Low Limit Value Too High (IPMI FW:1.85)

     Infected motherboard: X10DRT-P
     Affected functions:
     Validation :
         1. Observe "PW consumption" Sensor reach low Limit values.

2.
     Category: Fix
     Description:
      [58971] IPMI monitor: RT1/RT2 Temperature Reading fail.

     Infected motherboard: X10DRD series
     Affected functions:
     Validation :
         1. Check the IPMI reading with the thermalmeter reading.

3.
     Category: Fix
     Description:
      [58977] No option of PUE3 mode.

     Infected motherboard: X10DRD series
     Affected functions:
     Validation :
         1. Check the Fan mode page of WebGUI.

4.
     Category: Fix
     Description:
      [59003] Optimal Fan Speed Mode not Working.

     Infected motherboard: X10DRH-IT
     Affected functions:
     Validation :
         1. Heat the 10G Temperature sensor.
         2. Observe the FAN speed. (Zone 1 should not change. Zone 2 should rise.)

5.
     Category: Fix
     Description:
      Enlarge 5VSTB and 3.3VSTB voltage to avoid false event log

     Infected motherboard: A1SA2
     Affected functions:
     Validation :
         1. Do SAT or LAN test to check if false event log launch

6.
     Category: Fix
     Description:
       Support GPU3 sensor on both Left & Right Cooling zone

     Infected motherboard: X10DRU-I+
     Affected functions:
     Validation :
         1. Heat GPU3 sensor and let it to dominate left zone and rigth zone
         2. check fan speed is going high on both left zone and right zone        
--------------------------------------------------------------------------

Filename: SMT_X10_185.bin version: 1.85 Date: 12-31-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

1.
     Category: Fix
     Description:
      [58687] [ECO] IPMI v1.82 Event Log Description Cannot Describe the Uncorrectable and Correctable Failure DIMM Info During POST.

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Generate DIMM SEL.
         2. Check the email and SNMP alert.

2.
     Category: Fix
     Description:
      [58766] X10DRC-LN4 IPMI ECO 1.80 Improvement Item #1 

     Infected motherboard: X10DRC
     Affected functions:
     Validation :
         1. Heat SAS and let it over 105 degree
         2. The sensor status over 105 degree should be "Upper Non-recoverable"

3.
     Category: Fix
     Description:
      [58807] [NM] Can't get entire platform CPU power statistics. 

     Infected motherboard: X10DRT-L
     Affected functions:
     Validation :
         1. try 0x30 0xe2 command. It should return non-zero value

4.
     Category: Fix
     Description:
      [58641] The IPMI Sensor readings test fail.

     Infected motherboard: X10SDV
     Affected functions:
     Validation :
         1. HW need to rework the DP, DN to 10G NIC.
         2. Check the 10G sensor reading

5.
     Category: Fix
     Description:
      [58708] [ECO] IPMI v1.82 Cannot Define the Correct Multi-Node Position.

     Infected motherboard: X10DRT-P
     Affected functions:
     Validation :
         1. Login the Webgui and go to Multi Node page.
         2. Check the node status.

6.
     Category: New Feature
     Description:
      InfiniBand Temperature Reading

     Infected motherboard: X10DRT-L
     Affected functions: InfiniBand Temperature Sensor
     Validation :
         1. Power up MB and check if IB Temp is available.

7.
     Category: Work around 
     Description:
      lower down the link speed to 100M for X10SLE / X10SLD

     Infected motherboard: X10SLE / X10SLD 
     Affected functions: S5 state
     Validation :
         1. Check if dedicate lan speed is 100Mbps at S5 state

--------------------------------------------------------------------------
Filename: SMT_X10_184.bin version: 1.84 Date: 12-24-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24


1.
     Category: Fix
     Description:
      [58537] The Fan speed doesn't go down when the HDD temperature goes down.

     Infected motherboard: X10QBI
     Affected functions:
     Validation :
         1. Change the fan mode from Standard to Full. See the fans become full speed or not.
         2. Change the fan mode from Full to Heavy IO. See the fan behavior.
         3. Change the fan mode from Heavy IO back to Standard. See the fan behavior.

2.
     Category: Fix
     Description:
      [58690] IPMI Hardware Monitor Check fail 

     Infected motherboard: X10DRT-L
     Affected functions:
     Validation :
         1. Check VBAT sensor on IPMI sensor reading web page

3.
     Category: Fix
     Description:
      [58687] [ECO] IPMI v1.82 Event Log Description Cannot Describe the Uncorrectable and Correctable Failure DIMM Info During POST.

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Generate DIMM SEL.
         2. Check the SEL in the WebGUI.
4.
     Category: Fix
     Description:
			  Decrease -5 degree on RT2 sensor 

     Infected motherboard: X10DRU-I+
     Affected functions:
     Validation :
         1. Check RT2

5.
     Category: Fix
     Description:
			  Insert 4 Xeon Phi GPUs and let it idle, sometimes GPU sensors are gone 

     Infected motherboard: X10DRG-Q. 
     Affected functions:
     Validation :
         1. Insert 4 Xeon Phi GPUs and put it idle
         2. Check if GPU sensors are still gone

--------------------------------------------------------------------------
Filename: SMT_X10_183.bin version: 1.83 Date: 12-18-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24


1.
     Category: Fix
     Description:
      [58621] VcpuVRM temperature shows "not-present" w/ rev 1.02 board.
      [58650] [VRM change to MPS] Missing IPMI VRM temp sensor reading of VcpuVRM temp and VmemVRM temp.

     Infected motherboard: X10DRU-i+, X10DRI-T
     Affected functions:
     Validation :
         1. Power on the system.
         2. Check the VcpuVRM sensor reading.

2.
     Category: Fix
     Description:
      [58637] IPMI FW not ready

     Infected motherboard: X10DRD-L
     Affected functions:
     Validation :
         1. Check IPMI sensor web gui
         
3.
     Category: Fix
     Description:
      [58630] AOC-2UR66-i4G does not show GPU temperature

     Infected motherboard: X10DRU-+
     Affected functions:
     Validation :
         1. Check IPMI sensor web gui

4.
     Category: Fix
     Description:
      [58341] The IPMI sensor readings test fail.

     Infected motherboard: X10SDV
     Affected functions:
     Validation :
         1. Check the VBAT sensor reading. It should be close to the DMM reading.

5.
     Category: Add new feature
     Description:
        Add Thermal trip

     Infected motherboard: X10DRU-+
     Affected functions:
     Validation :
         1. Remove fan and heat sink from CPU1 or CPU2.
		 2. Wait platform to shot down.
		 3. Check thermal trip event log.

6.
     Category: Support PUE2b Fan mode
     Description:
        Add Thermal trip

     Infected motherboard: X10DRU-+, X10DDW, X10DRFF
     Affected functions:
     Validation :
     1. Check PUE FSCs on CPU, DIMM, PCH, 10G, SAS

--------------------------------------------------------------------------
Filename: SMT_X10_182.bin version: 1.82 Date: 12-12-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24


1.
     Category: Fix
     Description:
      [58437] IPMI isn't offline when send warm reset command.

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Issue the command: ipmitool -H <IP> -U ADMIN -P ADMIN mc reset warm
         2. Wait about 10 seconds.
         3. Issue any IPMI commands should not be worked.
         4. Wait about 100 seconds.
         5. Issue IPMI commands should be fine.

2.
     Category: Fix
     Description:
      [58363] F-SKU reacts dual cooling zone behavior.
      [58376] F-SKU reacts dual cooling zone behavior.

     Infected motherboard: X10SRA, C7X99
     Affected functions:
     Validation :
         1. Change the fan mode to Heavy IO mode.
         2. Check the fan zone behavior.

3.
     Category: Fix
     Description:
      [56888] [Haswell] Vcpu1,2,3,4 reading status are shown as Upper Critical.

     Infected motherboard: X10QBI
     Affected functions:
     Validation :
         1. Please update BIOS to the X10QBi14.HSX.C10.
         2. Put the Haswell CPU onto the X10QBI.
         3. Check the Vcpu sensor readings.

4.
     Category: Fix
     Description:
      [58341] The IPMI sensor readings test fail.

     Infected motherboard: X10SDV
     Affected functions:
     Validation :
         1. Check the VBAT sensor reading. It should be close to the DMM reading.

5.
     Category: New Motherboard
     Description:
      Add new motherboard: X10QRH+.

     Infected motherboard: X10QRH
     Affected functions:
     Validation :
         1. IPMI bring up version.


--------------------------------------------------------------------------
Filename: SMT_X10_181.bin version: 1.81 Date: 12-xx-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24


1.
     Category: Fix
     Description:
      [58242] [JC2] Vcpu reading is incorrect in IPMI Sensor Reading page.

     Infected motherboard: X10QBL
     Affected functions:
     Validation :
         1. Please update BIOS to the latest version.
         2. Put the Haswell CPU onto the X10QBL.
         3. Check the Vcpu sensor readings.

2.
     Category: Fix
     Description:
      [57381] Existing BIOS shows "UNKNOWN" while updating BIOS via web-page.

     Infected motherboard: A1SRM-LN7F
     Affected functions:
     Validation :
         1. Update the BIOS from WebGUI.
         2. Check the current build date.

3.
     Category: Fix
     Description:
      [58345] Whran trying to re-insert NVME, slot number is missing.

     Infected motherboard: X10DRU-i+
     Affected functions:
     Validation :
         1. Eject the SSD.
         2. Insert the same one SSD.
         3. Check the page information.

4.
     Category: Fix
     Description:
      [58363] F-SKU reacts dual cooling zone behavior.
      [58376] F-SKU reacts dual cooling zone behavior.

     Infected motherboard: X10SRA, C7X99
     Affected functions:
     Validation :
         1. Change the fan mode to Heavy IO mode.
         2. Check the fan zone behavior.

--------------------------------------------------------------------------
Filename: SMT_X10_180.bin version: 1.80 Date: 12-02-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24


1.
     Category: Fix
     Description:
      [57441] AOC SAS Card overheat but no error sensor.

     Infected motherboard: All motherboard support AOC SAS Card
     Affected functions:
     Validation :
         1. Heat the AOC SAS card.
         2. Make the temperature over 95 degree C.
         3. Check the AOC_SAS_Temp sensor color is changed.
         4. Check the SEL.

2.
     Category: Fix
     Description:
      [57986] There are multiple devices under IPMI webgui PCIe SSD page.

     Infected motherboard: All motherboard support NVMe
     Affected functions:
     Validation :
         1. Keep only one NVMe device on board.
         2. Power on the system and check the NVMe SSD page.
         3. It should only have one Device:0.

3.
     Category: Fix
     Description:
      [56888] [Haswell] Vcpu1,2,3,4 reading status are shown as Upper Critical.

     Infected motherboard: X10QBI
     Affected functions:
     Validation :
         1. Please update BIOS to the latest version.
         2. Put the Haswell CPU onto the X10QBI.
         3. Check the Vcpu sensor readings.

4.
     Category: Fix
     Description:
      [58234] SYS-1028TR-TF system power red LED blinks fail 
      [58231] IPMI sensor readings power status fail
      [58206] IPMI Sensor readings fail


     Infected motherboard: X10DRT-L
     Affected functions:
     Validation :
         1. Check IPMI sensor web gui
         2. Check the fuction when power fail

5.
     Category: Fix
     Description:
      [58268] IPMI cannot provide K80 GPU Temp

     Infected motherboard: X10SRG
     Affected functions:
     Validation :
         1. Check IPMI sensor web gui
         2. Check if GPU sensors present

6.
     Category: Fix
     Description:
      [58180] No Dimm C2,D2 in sensor reading. 

     Infected motherboard: A1SA2
     Affected functions:
     Validation :
         1. Do factory default after new IPMI FW is downloaded
         2. Check if dimm sensors present
    
7.
     Category: Fix
     Description:
      [58286] AOC-S40G-i2Q isn't display on sensor reading
      [58275] o HDD in sensor reading

     Infected motherboard: A1SAM
     Affected functions:
     Validation :
         1. Use lastest BIOS which can send 0x3a and 0x5a commands
         2. Set JI2C1 JI2C2 jumpers to 1-2.
         3.Plug in 40G card and power on the system
         4.Check if 40G LAN card sensor appear
         5.Repeat step 3, Plug in LSI 3108 cards and power on the sytem
         6.Check if SAS sensors shows

8.
     Category: Fix
     Description:
      [58242] [JC2] Vcpu reading is incorrect in IPMI Sensor Reading page.

     Infected motherboard: X10QBL
     Affected functions:
     Validation :
         1. Please update BIOS to the latest version.
         2. Put the Haswell CPU onto the X10QBL.
         3. Check the Vcpu sensor readings.

         
------------------------------------------------------------------------------------------
Filename: SMT_X10_179.bin version: 1.79 Date: 11-21-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

1.
     Category: Fix
     Description:
		  [58041] Cancelling during ejection will appear to hang at "Cancelling" Screen
		  [58037] Cancelling Eject will show the same pop up window as Ejecting
		  [58035] The Help Page displays incorrectly for "NVMe SSD"
		  [58033] Wording was not changed from "Inject" to "Insert"
		  [58019] IPMI NVMe message still exist when a system shutdown state
		  [57953] IPMI NVMe SSD Page: Slot Pull-down Tab is Not Function
  
  
     Infected motherboard: All motherboards with NVMe devices installed
     Affected functions:
     Validation :
         1. Eject & Insert the NVMe device on NVMe web gui
         2. Verify the wording
         3. Check help page         
         4. When system is powered on. The NVMe web information will be hidden. Later user logins IPMI web, 
            no NVMe web page
         5. Try to pull down the Slot Pull-down Tab, the function should work as pulling down the Device Pull-down Tab

2.
     Category: Fix
     Description:
		  [57861] Deactivating Activate Smart Cooling shows false fan mode 
  
     Infected motherboard: X10DRU-I+
     Affected functions:
     Validation :
         1. Do factory default after FW is downloaded
         2. Check if the smart cooling mode is disable
         3. Select smart cooling mode and save
         4. Uncheck the smart cooling mode option
         5. Check if PUE2 mode is selected

3. 
     Category: Fix
     Description:
      [57980] The Fan speed doesn't change when I heat the HDD.

     Infected motherboard: X10QBI
     Affected functions:
     Validation :
         1. Heat the HDDs.
         2. Check the fan speed is rising or not.

4. 
     Category: Fix
     Description:
      [57799] IPMI on/off will lose IPMI sensor readings

     Infected motherboard: X10DRU-I+
     Affected functions:
     Validation :
         1. Do System On/Off test
         2. Check the sensors status show "No present" after system is powered on


5.
     Category: Fix
     Description:
                  [58105] There is no "Processor Automatically Throttled" event log.

     Infected motherboard: X10DBT-T
     Affected functions:
     Validation :
         1. Heat the CPU to processor hot.
         2. Check the "Processor Automatically Throttled" event log.

6. 
     Category: Fix
     Description:
      [58100] AOC-2UR68-i2XS does not provide GPU sensor readings

     Infected motherboard: X10DRU-I+
     Affected functions:
     Validation :
         1. Install GPUs and let system power on
         2. Check if GPU sensor displays on IPMI sensor web gui

7. 
     Category: Fix
     Description:
      [58065] Multinode page failed to show node B when viewed from Node A

     Infected motherboard: X10DRFR
     Affected functions:
     Validation :
         1. Login in node A
         2. Check the node B informaiton is not missing on multi-node web gui

8. 
     Category: Fix
     Description:
      [57373] IPMI sensor readings shows "2 X AOC_40G Temp" when "2 X AOC_10G " cards plugged in

     Infected motherboard: X10DDW
     Affected functions:
     Validation :
         1. Plugin 2 AOC_10G cards with new riser RSC_R2UW_2E8E16+
         2. Check the IPMI web gui, it should show "AOC_10G" sensor name

------------------------------------------------------------------------------------------

Filename: SMT_X10_178.bin version: 1.78 Date: 11-17-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

1.
     Category: Fix
     Description:
        Add a confirmation message after ¡§Eject¡¨ button is clicked
        Change the wording from ¡§Inject¡¨ to ¡§Insert¡¨

     Infected motherboard: All motherboards with NVMe devices installed
     Affected functions:
     Validation :
         1. Update the IPMI FW.
         2. Check NVMe web gui

2.
     Category: Enhancement
     Description:
        Default fan mode is PUE2 mode on X10DRU-+

     Infected motherboard: All motherboards with NVMe devices installed
     Affected functions:
     Validation :
         1. Update the IPMI FW.
         2. Do factory default

------------------------------------------------------------------------------------------

Filename: SMT_X10_177.bin version: 1.77 Date: 11-12-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24


1.
     Category: Fix
     Description:
        [57854] [IPMI V1.75 ECO] IPMI Share LAN Status show "Disabled" when IPMI link by onboard LAN1

     Infected motherboard: X10SRA, C7X99, C7Z97
     Affected functions:
     Validation :
         1. Update the IPMI FW.
         2. Restore to Factory Default by command: 0x30 0x41
         3. Power Cycle the SUT.
         4. Check the LAN Link status in IE Browser.

2.
     Category: Fix
     Description:
        [57866] IPMI Cannot Define Correct Current-Node Position Under Multi-Node Page

     Infected motherboard: X10DRT-P
     Affected functions:
     Validation :
         1. Setup two node and power up together
         2. Check multinode web page of node A
         3. Check if current node is node A, not node B

3.
     Category: Fix
     Description:
        [57847] [IPMI V1.75 ECO] Sometimes ACPI Status cannot sync up in "Power Control and Status" Page.

     Infected motherboard: X10SRA, C7X99, C7Z97
     Affected functions:
     Validation :
         1. Power on/off the SUT.
         2. Wait serveral seconds and check the power status in the same page.

4.
     Category: Fix
     Description:
        [57589] IPMI Web GUI still showing NVMe drive information and Eject option after successfully ejected NVMe SSD
        [57588] IPMI Web GUI still showing NVMe drive information and Eject option after successfully ejected NVMe SSD

     Infected motherboard: X10 Grantley motherboard  with NVMe device installed
     Affected functions:
     Validation :
         1.  If user clicked on the eject icon and did not unplug the NVMe drive, 
         2.  IPMI should not show NVMe drive information on IPMI web gui

5.
     Category: Fix
     Description:
        [56411] I loose all PCI_SSD tab info when I plug in "samsung NVMe SSD" in system

     Infected motherboard: X10 Grantley motherboard with Samsung NVMe device installed
     Affected functions:
     Validation :
         1.  Install Samsung NVMe drive 
         2.  Check if the information displays on the IPMI web gui

------------------------------------------------------------------------------------------
Filename: SMT_X10_176.bin version: 1.76 Date: 11-06-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

1.
     Category: Fix
     Description:
        [57789] After reload IPMI configuration, IPMI Configuration can be reloaded, but will generate unknown message in IPMI Configuration page 

     Infected motherboard: All
     Affected functions:
     Validation :
         1. After reload IPMI configuration
         2. No unkown message on IPMI Configuration page

2.
     Category: Fix
     Description:
        X10QBi BMC would be reboot issue.

     Infected motherboard: X10QBi
     Affected functions:
     Validation :
         1. Running cburn test, Blink the UID LED
         2. Check the UID LED keeps blinking continually in the test.

3.
     Category: Fix
     Description:
        [57691] [IPMI] When updating the FW in WEB GUI, the process stops at 93% instead of 100% 

     Infected motherboard: X10DDW
     Affected functions:
     Validation :
         1. Update the FW and check the update progress.
 
4.
     Category: Add new feature
     Description:
        Add Thermal trip

     Infected motherboard: X10DRH
     Affected functions:
     Validation :
         1. Remove fan and heat sink from CPU1 or CPU2.
		 2. Wait platform to shot down.
		 3. Check thermal trip event log.

5.	 
	 Category: Add new feature
     Description:
		1. Add two sensors, HDD status and HDD Temp. respectively for LSI controller.
		2. Fan control on HDD Temp. according to the thermal guide.

     Infected motherboard: 
     Affected functions:
     Validation :
         1. Check HDD Temp in sensor reading page
		 2. Heat up HDD temperature. 
		 3. Monitor the fan speed changing.	 

6.	 
	 Category: Fix
     Description:
		  [57841] CPU1 temp and CPU2 temp are still shown in multinode monitoring page when restarting system
		  [57826] IPMI Multinode Temperature reading shows CPU1 at 101 Degrees C when powering on the system 

     Infected motherboard: X10DRFR
     Affected functions:
     Validation :
         1. Enter multinode IPMI web gui
         2. Do power off & power on another mode
         3. Check if CPU1 Temp, CPU2 Temp information, it will show N/A during BIOS POST
 
------------------------------------------------------------------------------------------         
         
Filename: SMT_X10_175.bin version: 1.75 Date: 10-31-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

1.
     Category: Fix
     Description:
        [57369] FAN PWM measurement fail for Memory.

     Infected motherboard: X10QBL
     Affected functions:
     Validation :
         1. Heat the memory.
         2. Use the scope to see the duty cycle waveform.

2.
     Category: Fix
     Description:
        [56798] System will generate a lot of error event when run E-burn stress test.

     Infected motherboard: X10QBL
     Affected functions:
     Validation :
         1. Run the E-burn test
         2. Check the SEL, CPU Voltages and CPU Temperatures.

3.
     Category: Fix
     Description:
        [56082] IPMI sensor has no PCH Temp and VRM Temp is N/A.

     Infected motherboard: X10SRA
     Affected functions:
     Validation :
         1. Go to the Sensor list page of Webgui or issue the ipmitool sensor list command.
         2. Check the VcpuVRM Temp reading.

4. 
     Category: Fix
     Description:
        Memory reading issue on Intel C1 stepping CPU.

     Infected motherboard: X10SRI, X10DRI-T
     Affected functions:
     Validation :
         1. See the Sensor list page of Webgui or issue the ipmitool sensor list command.

5.
     Category: Fix
     Description:
        [57371] Unusual IPMI events logged.

     Infected motherboard: X10DRU-X
     Affected functions:
     Validation :
         1. Run the stress test under windows server 2K8 over night.
         2. Check the chassis_intru event is generated or not.

6.
     Category: Fix
     Description:
        [57703] FAN PWM measurement fail for Memory on PUE3 mode
        [57702] FAN PWM measurement fail for RT2 at PUE3 mode
        
     Infected motherboard: X10DRFF, X10DDW, X10DDW-IN, X10DRU-+
     Affected functions:
     Validation :
         1. Check PUE3 FSC is the same as PUE2 FSC

7.
     Category: Enhancement 
     Description:
        Change the default fan mode is Standard mode
        
     Infected motherboard: X10DRT-P, X10DRFF
     Affected functions:
     Validation :
         1. Do factory default action
         2. Check if the default fan speed is standard mode

8.
     Category: Fix 
     Description:
        The VBAT sensor will reproduce abnormal SEL
        
     Infected motherboard: A1SA2
     Affected functions:
     Validation :
         1. Do bmc coldreboot on node1
         2. Do bmc coldreboot on node2
         3. Checek the event log. It should not be reproduced

------------------------------------------------------------------------------------------
Filename: SMT_X10_174.bin version: 1.74 Date: 10-27-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

1.
     Category: Fix
     Description:
        [57225] NO AOC Temp reading when JPI2C is enabled
 
     Infected motherboard: A1SA7
     Affected functions:
     Validation :
         1. Check if AOC_40G Temp sensor will display on IPMI web gui

2.
     Category: Fix
     Description:
        [57601] System will record Vcpu Voltage incorrect event continually in IPMI Event Log.

     Infected motherboard: X10QBL
     Affected functions:
     Validation :
         1. Check the SEL log, after running linpack test.


------------------------------------------------------------------------------------------

Filename: SMT_X10_173.bin version: 1.73 Date: 10-24-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

1.
     Category: Fix
     Description:
        [57346] Fan mode does not change to optimal when GPUs are present 

     Infected motherboard: X10DRU-I+
     Affected functions:
     Validation :
         1. Power on the machine with GPUs installed
         2. Check if PUE3 mode is hidden on IPMI fan mode web gui
         3. Do fatctory default again and check step no.2

2.
     Description:
        R:[57529] VcpuVRM Temp reading is "N/A" in IPMI sensor reading page.

     Infected motherboard: X10SRA
     Affected functions:
     Validation :
         1. Go to the Sensor list page of Webgui or issue the ipmitool sensor list command.
         2. Check the VcpuVRM Temp reading.
3.
     Category: Enhancement
     Description:
        Support X10DDW-IN motherbaord
        
     Infected motherboard: X10DDW-IN
     Affected functions:
     Validation :
         1. Use 0x30 0x21 command to get if the board id is "0x086E"

------------------------------------------------------------------------------------------

Filename: SMT_X10_172.bin version: 1.72 Date: 10-21-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

1.
     Category: Enhancement
     Description:
        [57161] Force fan mode to full when resetting/updating IPMI with GPUs 

     Infected motherboard: X10DRG-H(T),X10DRG-Q,X10SRG-F,X10DRT-P(T)(IBF),X10DRU-i+ and X10DRU-X
     Affected functions:
     Validation :
         1. When the BMC is not able to get the sensor readings (ex. BMC reset) with
            supported GPU/Intel Xeon Phi installed on the motherboard, fan speed goes to 
            full speed (PWM = 100%) until BMC is able to get the sensor readings.
         2. Above motherboards with no supported GPU/Intel Xeon Phi installed and other
            GPU motherboards follow default fan speed PWM duty cycle (PWM - 50%) when
            BMC is not able to get the sensor readings.
         3. Setting fan PWM duty cycle to 50% after AC ON/OFF, i.e. AC power cord is 
            unplugged (no standby power) and re-plugged in again.

2.
     Category: Fix
     Description:
        [57364] FAN PWM measurement fail for PCH

     Infected motherboard: X10QBL
     Affected functions:
     Validation :
         1. Heat the PCH over 80 degree C. (Since CPU0 is nearby PCH, please take care not to heat CPU0 too much.)
         2. Monitor the fan speed changing.

3.
     Category: Fix
     Description:
        [57366] FAN PWM measurement fail for CPU

     Infected motherboard: X10QBL
     Affected functions:
     Validation :
         1. Heat the CPU over 70 degree C.
         2. Monitor the fan speed changing.

4.
     Category: Fix
     Description:
        [57369] FAN PWM measurement fail for Memory.

     Infected motherboard: X10QBL
     Affected functions:
     Validation :
         1. Heat one of the Memory to overheat.
         2. Monitor the fan speed changing.

5.
     Category: Fix
     Description:
        [57370] The temperature of memory isn't correct.

     Infected motherboard: X10QBL
     Affected functions:
     Validation :
         1. Heat one of the Memory to overheat.
         2. Check the SEL log.

6.
     Category: Fix
     Description:
        [57355] Error sensor reading on AOM-STG-i2T.

     Infected motherboard: X10DRFF
     Affected functions:
     Validation :
         1. Check sensor reading on AOM-STG-i2T.

7.
     Category: Fix
     Description:
        [57343] [Final Release] Multi-Node Power and Current Readings Are Wrong.

     Infected motherboard: X10DBT-T
     Affected functions:
     Validation :
         1. Move the Multi Node page.
         2. Check the Node Power and Current.

8.
     Category: Fix
     Description:
     	[57346] Fan mode does not change to optimal when GPUs are present 
     Infected motherboard: X10DRU-I+
     Affected functions:
     Validation :
		1. do reset-to-default and check the default fan mode on fan mode page.
9.

	 Category: Enhancement
     Description:
    	Per PM decision, changing NVMe sensors to "NVMe_SSD Temp." and renaming  the wording "PCIeSSD" to "NVMe" on NVMe page.
     Infected motherboard: All
     Affected functions:
     Validation :
    	check the sensor and NVMe pages.

10.
     Category: Fix
     Description:
        [57463] IPMI Memory sensor readings are incorrect.

     Infected motherboard: X10DRU-X(LL)
     Affected functions:
     Validation :
         1. Move the sensor page.
         2. Check the Memory sensor readings.

11.
     Category: Enhancement
     Description:
        Support Smart Cooling mode on fan mode page for specific CPUs.
        It will display when these CPUs are installed
        
        Supported CPU list : E5-2667 v3,E5-2643 v3,E5-2637 v3,E5-2623 v3
        
        Also, the CPU fan curve is changed. Please follow the latest Thermal guide (T.B.D)
        
        When GPU is installed on certain motherboard, PUE2 and PUE3 mode will be hidden.
        
     Infected motherboard: 
       Support Smart Cooling mode                          : X10DRU-I+, X10DDW-I, X10DRFF
       Support hidden PUE2 & PUE3 mode when installing GPUS: X10DRU-I+
     Affected functions: fan mode function and CPU fan curve 
     Validation :
         1. Validate CPU fan curve when specific CPUs are installed
         2. Make sure the smart cooling mode are default selected on the fan mode web gui
         3. If you install GPUs on X10DRU-I+, the PUE2 & PUE3 mode will be hidden on fan mode web gui


------------------------------------------------------------------------------------------
Filename: SMT_X10_171.bin version: 1.71 Date: 10-14-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24


1.
     Category: Fix
     Description:
        [57126] The setting mode of Fan isn't correct

     Infected motherboard: X10QBL
     Affected functions:
     Validation :
         1. Check the default Fan mode in the web page.

2.
     Category: Fix
     Description:
        [57125] IPMI Hardware Monitor Check fail
        [56764] IPMI Monitor sensor readings are incorrect.

     Infected motherboard: X10QBL
     Affected functions:
     Validation :
         1. Check the different value between reading value and measured value.

3.
     Category: Fix
     Description:
        [57127] Fan Pulse-Width-Modulation Measurement fail.
        [56985] CPU1~4 Temp/CPU4 VRM Temp will overheat and then system shutdown when system run full loading stress test.

     Infected motherboard: X10QBL
     Affected functions:
     Validation :
         1. Login the Webgui and move to Fan mode page.
         2. Change the fan mode.

4.
     Category: Fix
     Description:
        [57160] Fan mode not changed from PUE3 to Optimal when GPUs are present

     Infected motherboard: X10DRU-X, X10DRU-XLL
     Affected functions:
     Validation :
         1. Check the default Fan mode in the web page.

5.
     Category: Fix
     Description:
        [56814] IPMI sensor can't readings any VRM Temp

     Infected motherboard: X10DRW-E,X10DRW-N
     Affected functions:
     Validation :
         1. Check the memory VRM sensors on IPMI web gui

6.
     Category: Fix
     Description:
        [57177] It shows multiple "AOC_10G Temp" under IPMI webgui sensor reading page

     Infected motherboard: X10DDW
     Affected functions:
     Validation :
         1. Check AOC_10G Temp on IPMI web gui

7.
     Category: Enhancement
     Description:
        [57014] [IPMI]In full speed mode, fan speed will drop when reset the BMC  

     Infected motherboard: X10DRG-H(T)
     Affected functions:
     Validation :
         1. For motherboard X10DRG-H(T), fan speed goes to full speed (PWM = 100%) after 
            power on or BMC reset until BMC is able to get the sensor readings.  After that, 
            motherboard follows fan speed control curves when sensors start to poll

8.
     Category: Fix
     Description:
        [57289] No description about OS boot.

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Generate the SEL and Check the email.

9.
     Category: Fix
     Description:
        [57287] No deassertion - processor automatically throttled.

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Generate the Processor hot.
         2. Check the Assertion SEL.
         3. Cooling the Processor.
         4. Check the Deassertion SEL.

10.
     Category: Fix
     Description:
        [57063] LED frequency measurement fail.

     Infected motherboard: X10QBL
     Affected functions:
     Validation :
         1. Generate the power fail, fan fail and overheat events.
         2. Check the OHLED behavior.

11.
     Category: Fix
     Description:
        [57319] System Fans go to FULL SPEED during system BIOS POST

     Infected motherboard: X10DDW
     Affected functions:
     Validation :
         1. Do system power on, the fan duty cycle should be 50%, not 100%

12.
     Category: Fix
     Description:
        [57290] The hardware monitor test fail

     Infected motherboard: X10DRW-NT
     Affected functions:
     Validation :
         1. Check if on board 10G sensor on IPMI sensor gui

13.
     Category: Fix
     Description:
        [57323] After update IPMI V1.70 FW, IPMI Network status is incorrect in Network Settings page
        [57277] Can't access IPMI WEB GUI with shared LAN after set IP address to Static
        [57227] Share LAN - Static IP isn't work
        [57189] Share Lan status doesn't display
        [57164] Network interface alway shows "dedicate" LAN mode in IPMI Web GUI

      Infected motherboard: All
     Affected functions:
     Validation :
         1. Check if we can set status ip on IPMI network web gui
         2. Check the dedicate and share mode on IPMI network web gui work fine
                  
                  
14.
     Category: Fix
     Description:
        [57269] Fan speed control error

      Infected motherboard: X10DRU+
     Affected functions:
     Validation :
         1. Set full speed on IPMI fan mode web gui
         2. Check if the fan rpm  is reached to maximum

15.
     Category: Fix
     Description:
        Cipher suite 0 from ADMIN to Unused.

     Infected motherboard: All
     Affected functions:
     Validation :
         1. ipmitool -H <IP> -U ADMIN -P ADMIN lan print.
         2. aaaaXXaaaXXaaXX -> XaaaXXaaaXXaaXX

 
------------------------------------------------------------------------------------------
Filename: SMT_X10_170.bin version: 1.70 Date: 10-03-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

********** Please do factory default after this version is updated **********
1.
     Category: Fix
     Description:
        [56764] IPMI Monitor sensor readings are incorrect.
        [56964] The voltage items doesn't show on IPMI.
        [56798] System will generate a lot of error event when run E-burn stress test.

     Infected motherboard: X10QBL
     Affected functions:
     Validation :
         1. Login the WEBGUI
         2. Check the sensor reading page.

2.
     Category: Fix
     Description:
        [56751] [BIOS 1.0a ECO] IPMI SLOTs report function(3a/5a) - FAILED  

     Infected motherboard: X10QBI
     Affected functions:
     Validation :
         1. Support riser 0x3a or 0x5a commands

3.
     Category: Enhancement
     Description:
        Implement new thermal guide 4.02 version (09092014)
        Implement PUE3 mode
        [56998] Fan PWM fail 
     Infected motherboard: X10 motherboards
     Affected functions:
     Validation :
         1. Test fan control function

4.
     Category: Fix
     Description:
        [56981] Fan ramps up due to wrong temperature reading
     Infected motherboard: X10DRU+
     Affected functions:
     Validation :
         1. Enter IPMI web page and check the vaule of RT2 sensor. It should not show "-1" 
 
5.
     Category: Fix
     Description:
        [56921] IPMI hardware monitor fail
     Infected motherboard: X10DRD
     Affected functions:
     Validation :
         1. Check IPMI sensor gui 

6.
     Category: Fix
     Description:
        [57003] Function Fail, LAN temperature reading fail
        [56814] IPMI sensor can't readings any VRM Temp 
     Infected motherboard: X10DRW-E
     Affected functions:
     Validation :
         1. Check IPMI sensor gui

7.
     Category: New Feature
     Description:
        Enable FAN9 reading if users install a FAN device on RSC-W2-66
     Infected motherboard: X10DRU_I_PLUS
     Affected functions:
     Validation :

8.
     Category: Enhancement
     Description:
        Support AMD FirePro S10000 GPU
     Infected motherboard: X10DRG-H(T),X10DRU,X10QBi and X10DRT-P
     Affected functions:
     Validation :
         1. Install AMD FirePro S10000 GPU
         2. Check GPU Temp being present

9.
     Category: Fix
     Description:
        [57042] IPMI should not have Dedicate option in Network Configuration.

     Infected motherboard: A1SRM-LN7F, A1SRM-LN5F
     Affected functions:
     Validation :
         1. Check the Network Configuraion page

10. 
     Category: Fix
     Description:
		[57039][57034][56244] SUM- Test case211 (Changebmccfg and compare.) failed 

     Infected motherboard: C7Z97-MF X10DRU-X X10DRU-XLL
     Affected functions:
     Validation :
		1. run SUM Test case 211.

----------------------------------------------------------------------------------------------
Filename: SMT_X10_169.bin version: 1.69 Date: 09-23-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24


1.
     Category: Fix
     Description:
        [56428] Sometime when you are updating IPMI FW of both the nodes together the update progress will be stalled.

     Infected motherboard: X10DBT
     Affected functions:
     Validation :
         1. Perform the IPMI FW update by WebGUI
         2. Observe the update progress changing.

2.
     Category: Fix
     Description:
        [56400] Chassis Intrusion Events Logs During iKVM Stress

     Infected motherboard: X10DRC
     Affected functions:
     Validation :
         1. Do iKVM stress test
         2. Check the sel log about chassis intrusion. It should not happen again during the test

3.
     Category: Enhancement
     Description:
        Support second LSI infomation in web page

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Install 2 LSI cards in riser card(The maximum supported number of LSI device is 2)
         2. Check LSI information in Storage Monitoring category after system boot into OS

4.
     Category: New Feature
     Description:
        Enable SNMP configuration and port setting functions in WEB.

     Infected motherboard: All
     Affected functions:
     Validation :

5.
     Category: Fix
     Description:
        [56633] Memory sensor readings shows abnormally.

     Infected motherboard: C7X99
     Affected functions:
     Validation :
         1. C7X99 does not support RDIMM.
         2. Since UDIMM cannot support temperature reading, C7X99 would remove all memory temperature sensors.

6.
     Category: Fix
     Description:
        [56675] [Final Release]IPMI Email Alert Missing Event Description on Chassis Intrusion.

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Setup the setting of SMTP.
         2. Generate the Chassis Intrusion Event.
         3. Check the email.
        
7.
     Category: Fix
     Description:
        [56456] Logical Drive degraded event log in IPMI
        [55575] Got some false messages under SEL saying "Drive Fault @ slot2 /3

     Infected motherboard: X10 Grantley platforms
     Affected functions: 
                         Disable LSI event log temporarily
                         LSI event log functions
                         (Use 0x30 0x70 0xfb 0x1 to enable event log function)
     Validation :
         1. Do power on/off and check if any false alarm happen again.
8. 
	 Category: Fix
     Description:
        [55739]  iKVM- The auto stop recording function is not working
     Infected motherboard: X10DRU-XLL
     Affected functions:
     Validation :
       	1. go to option->preference->display and enable auto stop.
       	2. go to record->start
        3. when the timer expired,the ikvm will stop recording.
9. 
	 Category: Fix
	 Description:
    	[56674][Final_Release] IPMI Web Status Shown "Warning" While CPU Already OverHeat.
	 Infected motherboard:
	 Affected functions:
	 Validation :
    	1. overheat CPU and check if the system health icon changes to "Critical "

10. 
	 Category: New feature
	 Description:
		add PS consumption sensor 
	 Infected motherboard: X10DRT-P
	 Affected functions:
	 Validation :
		1. check if there is PS consumption sensor on IPMI web.(please do reset-to-default)

11.
         Category: Fix
         Description:
              [56656] Function test issue -> C7Z97-M/C7Z97-MF OHLED test fail
         Infected motherboard: C7Z97-MF
         Affected functions:
         Validation :
                1. Run SDHM
                2. Check the Red LED.

12.
     Category: Enhancement                                                                                                                                                    
     Description:
        Enhance ATEN-IPMI-MIB and ipmi agent so that users are able to know what sensor names are.

     Infected motherboard: All
     Affected functions:
     Validation :

12.
     Category: Fix                                                                                                                                                    
     Description:
        [56761] Fan Optimal mode shoud be removed because that this board support single cooling mode only
     Infected motherboard: X10DRD
     Affected functions:
     Validation :
        1.After updating the FW, please do factory default function
        2.Check IPMI fan mode web gui

13.
	 Category: Fix
     Description:
    	[56671]How to identify temp sensors for AOC-S40G-i2Q & AOC-STG-i2T under IPMI sensor reading page
     Infected motherboard: All
     Affected functions:
     Validation :
    	1. following the below name rule for LSI/NvME/10G/40 and please check IPMI sensor page.i
    	PS: please do reset-to-default.
    
    	MB/AOM_SAS Temp ==> onboard SAS
    	MB_NVMe Temp	==> onboard NvME
    	AOC_10G Temp	==> AOC 10G
    	AOC_40G Temp	==> AOC 40G
    	AOC_SAS Temp	==> AOC SAS
    	AOC_NvME Temp	==> AOC NvME

--------------------------------------------------------------------------------------------
Filename: SMT_X10_168.bin version: 1.68 Date: 09-15-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r23


1.
     Category: Fix
     Description:
        [56474] ACPI Status still show "Host is currently off" in IPMI Power Control and Status page after system power cycle.

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Login the webgui and switch to Power control page
         2. Select "Power Cycle" and press "Perform Action".

2.
     Category: Customer Requirement
     Description:
        0x30 0x70 0x72 command to set watch dog by seconds for A1SRM_LN7F

     Infected motherboard:  A1SRM_LN7F
     Affected functions:
     Validation :
         1. Set watchdog command to trigger after 300 seconds. ipmicfg -raw 30 70 72 1 1 2c 1
         2. Count 300 seconds and see if the system do reset

--------------------------------------------------------------------------------------------
Filename: SMT_X10_167.bin version: 1.67 Date: 09-12-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r23


1.
     Category: Fix
     Description:
        [56368] [IPMI 1.64 ECO] SMTP Setting error messages keeps popping up after entering incorrect values.

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Login the webgui and switch to SMTP page.
         2. Try the error case of SMTP setting.

2.
     Category: Enhancement
     Description:
        Show "Max Capable Speed" and "Operating Speed" in DIMM category (Hardware Information web page)
        [56260] [IPMI 1.63] IPMI hardware information memory speed does not meet the BIOS settings

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Max Capable Speed: SMBIOS Memory Device (Type 17) offset 15h
                               The maximum capablespeed of the device.
         2. Operating Speed: SMBIOS Memory Device (Type 17) offset 20h
                             The configured clock speed to the memory device

3.
     Category: Fix
     Description:
        [56393] Upload BIOS fail through IPMI

     Infected motherboard: A1SRM-LN7F family
     Affected functions:
     Validation :
         1. Login the webgui.
         2. Update the BIOS.

4.
     Category: Fix
     Description:
        [56393] Upload BIOS fail through IPMI

     Infected motherboard: A1SRM-LN7F family
     Affected functions:
     Validation :
         1. Login the webgui.
         2. Update the BIOS.

5.
     Category: Fix
     Description:
        [56456] Logical Drive degraded event log in IPMI
        [55575] Got some false messages under SEL saying "Drive Fault @ slot2 /3

     Infected motherboard: X10 Grantley platforms
     Affected functions: 
                         Disable LSI event log temporarily
                         LSI event log functions
                         (Use 0x30 0x70 0xfb 0x1 to enable event log function)
     Validation :
         1. Do power on/off and check if any false alarm happen again.

6.
     Category: Fix
     Description:
        [56377] Vendor ID under PCIe SSD monitoring tab is in wrong order

     Infected motherboard: X10 Grantley platforms with Intel NvMe devices
     Affected functions: 
     Validation :
         1. Enter NvMe web page
         2. Check the vendor id of Intel SSD is "80 86"

7.
     Category: Enhancement
     Description:
        Support AOC Temp for AOC-S40G-i2Q

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Install AOC-S40G-i2Q
         2. Check if AOC Temp is present in sensor list

8.
     Category: Fix
     Description:
        [56385] No 10G AOC temperature reading in IPMI

     Infected motherboard: X10DRG-H(T)
     Affected functions:
     Validation :
         1. Update X10DRG4.908 BIOS
         2. Check if AOC Temp is present in sensor list when AOC card is installed

9.
     Category: Add Motherboard
     Description:
        Add new motherboard configuration - X10DRW_E,X10DRD

     Infected motherboard:
     Affected functions:
     Validation :

10.
     Category: Workaround
     Description:
        Add ME Reset function if the ME is in abnormal state.

     Infected motherboard: X10QBi
     Affected functions:
     Validation :

11.
     Category: Fix
     Description:
        Fans are running at full speed even system is sitting idle at PXE screen

     Infected motherboard: X10DDW, X10DDW_I3
     Affected functions:
     Validation :
         1. Do S4 stress test
         2. When system is powered off, the fan speed is at full speed
         3. Select "Power On" function on IPMI web gui
         3. Check if the fan speed is back to normal

--------------------------------------------------------------------------------------------
Filename: SMT_X10_166.bin version: 1.66 Date: 09-09-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r23

1.
     Category: Fix
     Description:
        [56340] GPU Numbering in IPMI Does Not Follow GPU Thermal Guideline

     Infected motherboard: X10DRG-H(T)
     Affected functions:
     Validation :
         1. The GPU label will be GPU3/GPU4 in slot 4 for 2U 6 GPU
         2. The GPU label will be GPU5/GPU6 in slot 1 for 2U 6 GPU


2.
     Category: Enhancement
     Description:
        Support Nvidia M40 GPU
     Infected motherboard: X10DRG-H(T),X10DRU,X10QBi and X10DRT-P
     Affected functions:
     Validation :
         1. Install Nvidia M40 GPU
         2. Check GPU Temp being present

3.
     Category: Fix
     Description:
        [56401] Agent managed command-Reset chassis intrusion failed
     Infected motherboard: X10 motherboards with ast2400 internal superio
     Affected functions:
     Validation :
         1. Short JL1 pin to let chassis case open
         2. Enter dos mode and key-in "ipmicfg -raw 30 3"
         3. It should not have error message appear "IPMI command not completed normally, Completion Code=FFh"
 
--------------------------------------------------------------------------------------------
Filename: SMT_X10_165.bin version: 1.65 Date: 09-05-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r23

1.
     Category: Fix
     Description:
        [56320] OH LED comes up everytime for 20 seconds while doing windows S4 stress test
        [56294] Got lots of CPU1 & CPU2 "Processor Automatically Throttled" messages under IPMI SE

     Infected motherboard: X10 Grantley platforms
     Affected functions:
     Validation :
         1. Do the S4 stress test
         2. BMC should not have cpu prossor hot event log
         3. Buzzer should not beep
         4. Overheat Led should not be flashing

2.
     Category: Fix
     Description:
        [56339] CPU overheat audible and alert LED stays on even after CPUs are cooled down

     Infected motherboard: X10DRU
     Affected functions:
     Validation :
         1. Overheat CPU and let overheat LED turns on and the buzzer beeps.
         2. cooldown the CPU temperature
         3. Check if Overheat LED turns off and buzzer stop beeping 

3.
     Category: Fix
     Description:
        [56117] iKVM Reset function is fail 

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Do the iKVM reset function.
         2. Virtual media should not exist
         3. Check if Overheat LED turns off and buzzer stop beeping 

4.
     Category: Fix
     Description:
        [56157] [NVME injection btn] IPMI Web GUI information not updated during hot plug test. System need to reboot in order to bring up updated info  

     Infected motherboard: X10 Grantley motherboard with CPLD NvME backplane
     Affected functions:
     Validation :
         1. Do the eject button
         2. NVMe SSD information should not show after hot remove the drive 

5.
     Category: Fix
     Description:
        [56402] [Final Release Package] REOPEN ISSUES(PBID#56193, 56257, 56225, 56126) that happens on v1.65 again. 

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Generate the SEL.
         2. Check the mail and SEL.

--------------------------------------------------------------------------------------------
Filename: SMT_X10_164.bin version: 1.64 Date: 09-03-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r23

*****************Please do factory deafault after burning this FW****************

1.
     Category: Fix
     Description:
        [56257] 1.63]Email EVENT_DIRECTION show "De-assertio" when event deasserted
        [56252] Email EVENT DIRECTION show "De-assertion" when event deasserted.

     Infected motherboard: All
     Affected functions:
     Validation :
         1. De-assert the event.
         2. Check the Email.

2.
     Category: Fix
     Description:
        [56259] [ SUM 1.4.0 ] IPMI is not active but sum checkoobsupport isn't.

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Check the result of SUM checkoob support.

3.
     Category: Enhancement
     Description:
        [56091] [ SUM 1.4.0 ] Random - Soft shutdown is not work

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Please do software power shutdown fucntion on IPMI web gui to see if it works at Redhat system

4.
     Category: Fix
     Description:
        [56097] [2U-SYS] Xeon-Phi Lost After Running Cburn ONOFF 153 Cycles
     Infected motherboard: X10DRT-P
     Affected functions:
     Validation :
         1. Check if BMC finds GPU sensors

4.
     Category: Fix
     Description:
        [55667] Got some messages about AOM3108 controller under SEL
        [55604] "Drive Fault" during ONOFF test on X10DRC-LN4+
        [55575] Got some false messages under SEL saying "Drive Fault @
     Infected motherboard: X10 Grantley platforms
     Affected functions: 
                         Disable LSI event log temporarily
                         LSI event log functions
                         Use 0x30 0x70 0xfb 0x1 to enable event log function
     Validation :
         1. Do power on/off and check if any false alarm happen.

--------------------------------------------------------------------------------------------
Filename: SMT_X10_163.bin version: 1.63 Date: 08-29-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r23


1.
     Category: Fixed
     Description:
        [56206] BIOS can't update from IPMI WebGUI
        [56178] Can't update BIOS with IPMI Web GUI
        [56177] BIOS OOB update from IPMI webgui failed on IPMI FW 1-62 version
        [56163] [Final Release] IPMI v1.62 BIOS update Fail under Web GUI
        [56160] Cannot activate product key through SUM ./activate.sh
        [56112] Flash BIOS via IPMI web is fail

     Infected motherboard: All motherboards
     Affected functions:
     Validation :
         1. Login WebGui
         2. Update BIOS.

2.
     Category: Enhancement
     Description:
        Set/Get System Info Parameter command

     Infected motherboard: 
     Affected functions:
     Requirement :
         1. Please use TAS v1.0.1 and SUM v1.4.1 to work together.

3.
     Category: Fix
     Description:
       [56194] [Final Release] IPMI v1.61 - Email Alert Missing Event Description For "Processor Automatically Throttled"
       [56126] No description for the Processor Automatically Throttled email alert event.

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Setup the SMTP configuration.
         2. Trigger Processor Automatically Throttled event.
         3. Check the email.

4.
     Category: Fix
     Description:
       [55725] IPMI failed to detect more than 3 GPU temp 

     Infected motherboard: X10DRG-H(T)
     Affected functions:
     Validation :
         1. Install riser card RSC-G2FR-A66 in slot4
         2. Check GPU5/GPU6 is present correctly when GPU exists

5.
     Category: Fix
     Description:
       [56140] The email alert shows "OS Critical Stop" when the system is Graceful Shutdown.

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Setup the SMTP configuration.
         2. Graceful shutdown the system.
         3. Check the email.

6.
     Category: Fix
     Description:
       [56193] [Firmware v1.62 Final Release Package] Event Log description incorrect in IPMIWeb GUI.

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Setup the SMTP configuration
         2. Trigger the threshold event.
         3. Check the email.

7.
     Category: Fix
     Description:
       [56193] [Firmware v1.62 Final Release Package] Event Log description incorrect in IPMIWeb GUI.

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Setup the SMTP configuration
         2. Trigger the threshold event.
         3. Check the email.

8.
     Category: Fix
     Description:
       [56193]  Drive fault error while running HD stress test
       [55837]  LSI temperature will randomly disappear
       [55604]  "Drive Fault" during ONOFF test on X10DRC-LN4+
       [55575]  Got some false messages under SEL saying "Drive Fault @ slot2 /3"

     Infected motherboard: X10 Grantley platform
     Affected functions:
     Validation :
         1. Install the SAS HDD and create Raid. Clear all the event log message
         2. Do cburn on/off test
         3. Check if any false alarm happen

9.
     Category: Fix
     Description:
       [56162]  [IPMI] AOM Module got OH after IPMI reset

     Infected motherboard: X10DDW
     Affected functions:
     Validation :
         1. When bmc do coldrboot or sytem is powered on or reset
         2. Check the fan speed is near 100% duty cycle

10.
     Category: Fix
     Description:
       [56162] [SUM 1.4]Test case 235 "Clear event log" failed

     Infected motherboard: X10DRI-T
     Affected functions:
     Validation :
         1. First, update BMC firmware
         2. Update bios x10dri14.826
         3. Check [SUM 1.4]Test case 235

==================================================================================================
Filename: SMT_X10_162.bin version: 1.62 Date: 08-26-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r23

********************************* X10DRT-P Release Only**********************************

1.
     Category: Enhancement
     Description:
        [55962] CPU temp stays at 40C even when stressed at 4.6ghz
        [55899] CPU Overheat Buzzer Function does Not Work
 
     Infected motherboard: C7Z97_M, X10SRA
     Affected functions:
     Validation :
         1. Stress test and check the cpu temperature
         2. make CPU overheat and listen if the buzzer start working

2.
     Category: Fix
     Description:
        [56081] LSI 3108 temperature gone after doing IPMI factory default
 
     Infected motherboard: X10 Grantley platforms
     Affected functions:
     Validation :
         1. Wait and you can see LSI temperature appear on the IPMI sensor reading page
         2. Do factory default
         3. Enter the IPMI web gui again and refresh to see if LSI temperature value is gone

3.
     Category: Fix
     Description:
        [LSI] Disable LSI event log temporarily
     Infected motherboard: X10 Grantley platforms
     Affected functions: LSI event log functions
                         Use 0x30 0x70 0xfb 0x1 to enable event log function
     Validation :
         1. Do power on/off and check if any false alarm happen.

==================================================================================================

Filename: SMT_X10_161.bin version: 1.61 Date: 08-XX-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r23

1.
     Category: Enhancement
     Description:
        Support Nvidia M3-3020 GPU
     Infected motherboard: X10DRG-H(T),X10DRU,X10QBi
     Affected functions:
     Validation :
         1. Install Nvidia M3-3020 GPU
         2. Check GPU Temp being present

2.
     Category: Fix
     Description:
        [55856] IPMI only shows two GPU temperatures 
     Infected motherboard: X10DRU
     Affected functions:
     Validation :
         1. Check GPU2 Temp/GPU3 Temp being present if GPU exist

3.
     Category: Enhancement
     Description:
        Get NvME information from CPLD (No support old NvME protocol now)
     Infected motherboard: First support on X10DBT, X10DRU, X10DRT_P and X10DDW. Other X10 Grantley motherboards need to be regarbered.
                           Need new backplane support.  
     Affected functions:
     Validation :
         1. Check NvMe function

4.
     Category: Fix
     Description:
        [55894] Memory Temp readings are incorrect
     Infected motherboard: X10DRU
     Affected functions:
     Validation :
         1. Heat speicfic Memory.
         2. See the temperature value are rising or not.

5.
     Category: Fix
     Description:
        [55678] 'LAN Temp' is shown 'Upper Critical' after upgrading IPMI FW to v1.58
     Infected motherboard: X10DRH-I
     Affected functions:
     Validation :
         1. Make sure X10DRH-I has no any LAN Temp sensor.

6.
     Category: Fix
     Description:
        [55584] Sometimes some virtual keyboard color is black 
     Infected motherboard:
     Affected functions: Java viewer
     Validation :
         1. Check if some virtual keyboard color is black sometimes

7.
     Category: New platform
     Description:
        Support new motherboard: X10QBL
     Infected motherboard: X10QBL

8.
     Category: Fix
     Description:
        [ SUM 1.4.0 ] Change BMC configuration is fail.
     Infected motherboard: All
     Affected functions:
     Validation :
         1. run the test case 211

9.
     Category: Fix
     Description:
        [55886] 10G LAN Temperature and Fan Speed Unstable with System Idle 
     Infected motherboard: X10DRH-CT
     Affected functions:
     Validation :
         1. Make the system in idle.
         2. Observe the Zone2 fan speed(FanA, FanB) and Zone2 sensors(PCH, LAN, Peripheral, LSI).

==================================================================================================
Filename: SMT_X10_160.bin version: 1.60 Date: 08-19-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r22

1.
	 Category: Fix
     Description:
    	 [55739]  iKVM- The auto stop recording function is not working
     Infected motherboard: X10DRU-XLL
     Affected functions:
     Validation :
    	 1. go to option->preference->display and enable auto stop.
    	 2. go to record->start
    	 3. when the timer expired,the ikvm will stop recording.

2.
	 Category: Fix
     Description:
    	[ SUM 1.4.0 ] Change BMC configuration is fail.
     Infected motherboard: X10SRL-F
     Affected functions:
     Validation :
    	 1. run the test case 211

3.
     Category: Enhancement
     Description:
        Trigger CPU overheat by PROCHOT_N according to Thermal Guide Rev 4.02
     Infected motherboard: X10DP Motherboards
     Affected functions:
     Validation :
         1. Wait the PROCHOT_N has falling edge, the SEL would be generated.

==================================================================================================
Filename: SMT_X10_159.bin version: 1.59 Date: 08-14-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r22

1.
       Category: Fix
       Description:
         [55642] Wrong GPU temperature readings in SEL
         [55645] IPMI SEL gets Xeon Phi Temp going high when running onoff test
         [55684] [IPMI] Got GPU OH event when runing linpack on CPU but NO loading on GPUs
       Infected motherboard: X10DRG-H(T),X10DRU-i+,X10DRU-X,X10DRU-XLL
       Affected functions:
       Validation :
            1. Check no IPMI SEL of Xeon Phi Temp/GPU Temp going high when running onoff test

2.
       Category: Fix
       Description:
       		[55507] BMC reset fails, drops IPMI
       Infected motherboard: X10DRU
       Affected functions:
       Validation :
    		1. do BMC cold reset stress test

3.
       Category: Fix
       Description:
       		[55652] IPMI FW 1.58 does not even show "LSICtl1 Temp" under sensor reading page
       Infected motherboard: X10DRU
       Affected functions:
       Validation :
    		1.Need bios to send 0x3a and 0x5 commands
                2.Check if LSICtrl sensor value exists. If not, it means bios does not send them yet

4.
       Category: Fix
       Description:
       		[55589] UID need to support or not?
       Infected motherboard: C7Z97-M
       Affected functions:
       Validation :
    		1.Remove UID function
   
5.
	   Category: Fix
       Description:
    	    R: [55694]The privilege settings for User and Operator are incorrect.
       Infected motherboard: X10DRU
       Affected functions:
       Validation :
    	    1.login as the operateri or user privilege
    	    2.check if the user is able to  have full or view access on ipmi
    	    web pages, like ldap,ddns and so on.

6.
       Category: Fix
       Description:
            [55700] IPMI Summary page showed additional LAN device(LAN 7)
       Infected motherboard: All
       Affected functions:
       Validation :
                1. See the main page of WebGUI.

7.
       Category: Fix
       Description:
            [55661] [BETA RELEASE] CPU and MEM Temperature Sensor Lost with IPMI FW to 1.58
       Infected motherboard: X10DBT
       Affected functions:
       Validation :
                1. Run Cburn Test.
                2. Monitor the Sensor Reading page.

8.
       Category: Fix
       Description:
            [55533] Fan PWM of memory is fail
       Infected motherboard: A1SRM-LN7F
       Affected functions:
       Validation :
                1. Heat the Memory.
                2. Check the Fan Speed.

9.
       Category: Fix
       Description:
            [55712] R2 cpu stepping cause IPMI memory temperture sensor reading wrong detect
            [55689] IPMI sensor reading detect wrong memory slot temperture
       Infected motherboard: X10DRFR, X10DRFF
       Affected functions:
       Validation :
                1. plug P1-DIMMA1, P1-DIMME1. check if other dimm sensor has duplicate values

10.
       Category: Fix
       Description:
            [55667] Got some messages about AOM3108 controller under SEL
       Infected motherboard: X10DDW
       Affected functions:
       Validation :
                1. Check if LSI LNC, LC, LNR event log of LSI control sensor will be sent


-----------------------------------------------------------------------------------------------------------
Filename: SMT_X10_158.bin version: 1.58 Date: 08-11-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r22

1.
       Category: Fix
       Description:
         [55613] IPMI CPU sensor readings disappear when CPU overheats.
       Infected motherboard: X10DBT-P
       Affected functions:
       Validation :
            1. Heat the CPU to overheat.
            2. Monitor the sensor reading.

2.
       Category: Fix
       Description:
         [55577] System runs at 70% to 80% of fan speed with AOM-3108 temp reaches to 75C while sitting idle in room temperature
       Infected motherboard: X10DDW
       Affected functions:
       Validation :
            1. Heat the monitoered sensor to overheat
            2. Monitor the fan curve of PUE-optimal mode

3.
       Category: Fix
       Description:
         [55599] Fan sensor status indictor incorrect while FAN-Failure.
       Infected motherboard: All
       Affected functions:
       Validation :
            1. Remove a FAN.
            2. See the color of fan in the sensor reading page of WebGUI.

-----------------------------------------------------------------------------------------------------------
Filename: SMT_X10_157.bin version: 1.57 Date: 08-08-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r22
 
1.
       Category: Fix
       Description:
         [55560] [BIOS] Fail To Flash BIOS Under DOS
       Infected motherboard: X10DBT-P, X10QBI
       Affected functions:
       Validation :
            1. Please flash bios under the dos

2.
       Category: Fix
       Description:
         [55500] I lost PCie_SSD tab & also lost PCIeSSD temp from sensor reading whenever I try to remove HDD connected to AOC 3108
         [55466] PCIe SSD tab NVMe temp & sensor reading PCIe SSD temp do not match
         [54886] IPMI webgui does not show correct NVMe SSD temp under PCIe_SSD tab

       Infected motherboard: X10DDW
       Affected functions:
       Validation :
            1. Check NvMe sensor

3.
       Category: Fix
       Description:
         [55238] [SDIII] Some voltage values weren't in limit
         [55062] Some SDIII sensor reading is incorrect

       Infected motherboard: C7Z97_M, X10SRE-DS018
       Affected functions:
       Validation :
            1. Check NvMe sensor

4.
       Category: Fix
       Description:
         [55016] CPU fan speed control not correct under both PUE and Optimial Mode

       Infected motherboard: X10DRU-i+,X10DRU-X,X10DRU-XLL
       Affected functions:
       Validation :
            1. Heat CPU1 or CPU2
            2. Check fan control is working properly per region
 
-----------------------------------------------------------------------------------------------------------
Filename: SMT_X10_156.bin version: 1.56 Date: 08-06-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r22

1.
       Category: Fix
       Description:
         [55232] [EVT] "PCH Tempe" displays "Not Present" in IPMIWeb GUI with firmware v1.54
         [55229] [EVT] Sensors of Onboard "10G LAN Temperature" displays "Not Present" in IPMIWeb GUI with firmware v1.54 
       Infected motherboard: X10DRH
       Affected functions:
       Validation :
            1. Check the sensor reading of PCH and LAN Temp
2.
       Category: Fix
       Description:
         [55392] [EVT] There is no FAN PWM for AOM3108 controller
       Infected motherboard: X10DDW
       Affected functions:
       Validation :
            1. Heat LSI temperature sensor, and check if fan rpm is rising
3.
       Category: Fix
       Description:
         [55244] BIOS Resilience" is not working in firmware v1.54.
       Infected motherboard: X10DRG-Q
       Affected functions:
       Validation :
            1. Check the WebGUI.
4.
       Category: Fix
       Description:
         [55426] IPMI CPU status conflicting with threshold definition
       Infected motherboard: X10DRU-I+
       Affected functions:
       Validation :
            1.IPMI Follow the latest thermal guide SIM_TDG REV. 4.02 (07XX2014).pdf
            2.Non-recoverable and Critical thresholds show red color
            3.Only critical event log is required 

5.
       Category: Fix
       Description:
         [55272] PCI-e SSD tab is missing when you do factory default in IPMI
       Infected motherboard: X10DRU-I+
       Affected functions:
       Validation :
            1.Do factory default action
            2.Do not login in the IPMI web gui too quickly because BMC loads the riser configuration and then add dynamic sensors.
            3.Login in the web gui to check if PCIe SSD tab is not missing

6.
       Category: Fix
       Description:
         [55242] No GPU sensor reading in IPMI Webgui.
       Infected motherboard: X10DRG-Q
       Affected functions:
       Validation :
            1.Check IPMI sensor page.(need newer bios to set 0x3a/0x5a command)		

7.
       Category: Fix
       Description:
         [55397]  FAN 2, FAN 5 reading issue.
       Infected motherboard: X10DRG-Q
       Affected functions:
       Validation :
            1.Plug FAN5 and check IPMI sensor page to get FAN5's reading.
			2.Plug FAN2 and FAN5, then unplug FAN5. Check IPMI sensor page
			3.Plug FAN2 and FAN4, then unplug FAN2. Check IPMI sensor page

8.
       Category: Fix
       Description:
         [55368]  PUE fan mode should be removed and Optimal fan mode should be the default fan speed control
       Infected motherboard: X10DRU-I+
       Affected functions:
       Validation :
            1.Do factory default after update the latest IPMI FW
            2.Check the fan mode web page(default Optimal mode)
            3.PUE mode won't be removed
            4.Check PUE mode do fan control per region

9.
       Category: Fix
       Description:
         [54230] [ SUM 1.3.0 ] Change BMC configuration fail.
         [54229] [ SUM 1.3.0 ] Change BMC configuration fail.
       Infected motherboard: X10DRW-IT, X10SRL
       Affected functions:
       Validation :
            1. SUM test

10.
       Category: Fix
       Description:
         [54999] The temperature of memory is fail
       Infected motherboard: A1SRM-LN7F
       Affected functions:
       Validation :
            1. Check the sensor reading of Memory sensors.			

11.
       Category: Enhancement
       Description:
         Go full speed when boot or bmc reset
       Infected motherboard: X10DRG-H(T)
       Affected functions:
       Validation :
            1. FANs go full speed in 10 seconds after power on or BMC reset.
               FAN speed will get recovery when sensors start to poll.
12. 
	Category: Fix
	Description:
	  [55399][55398]IPMI_iLO test fail for VMware ESXi 5.5 Cert
        Infected motherboard: X10DRFF,X10DRW
        Affected functions:
        Validation :
    	    1. run Vsphere client to setting IPMI/iLO on vCenter5.5 and see if it is ok

13.
       Category: Fix
       Description:
          [55453] Unable to read GPU temperature on IPMI 1.54
       Infected motherboard: X10DRU-X(LL)
       Affected functions:
       Validation :
            1. Check the sensor reading of GPU.

-----------------------------------------------------------------------------------------------------------
Filename: SMT_X10_155.bin version: 1.55 Date: 07-30-2014         
                                                                 
U-Boot build time : 2009.01 (Nov 27 2013)                        
Java SOL Viewer version : v0.5.9                                 
Java iKVM Viwer version : v1.69 r22     

1.
       Category: Fix
       Description:
         [55272] PCI-e SSD tab is missing when you do factory default in IPMI
       Infected motherboard: X10DRU-+
       Affected functions:
       Validation :
            1. Do factory default action, then check if PCI-e SSD tab still exists
2.
       Category: Fix
       Description:
         [55266] Fan7 / Fan 8 are not working
       Infected motherboard: X10DRU-+
       Affected functions:
       Validation :
            1. Check IPMI sensor page
3.
       Category: Fix
       Description:
         [55236] PCIe_SSD tab is missing from IPMI webgui & PCIe_SSDsensor reading missing from sensor reading
         [54935] PCIeSSD temp sensor reading lost from sensor reading page
         [54886] IPMI webgui does not show correct NVMe SSD temp under PCIe_SSD tab
       Infected motherboard: X10DRU-+, X10DDW
       Affected functions:
       Validation :
            1. Check IPMI sensor page. (Need bios to pass command to tell IPMI the NvME card exist)
4.
       Category: Fix
       Description:
         [55227] IPMI FW 1.54 Shows Two Temperature Sensors for Onboard LSI Controller
       Infected motherboard: X10DRC
       Affected functions:
       Validation :
            1. Check IPMI web gui (need newer bios to set 0x3a/0x5a command to activate on board LSI) 
5.
       Category: Fix
       Description:
         [55140] Fan naming not matches with onboard Fan silkscreen [#54675 reopen]
       Infected motherboard: X10DRU-XLL
       Affected functions:
       Validation :
            1. Check the fan name and anothre on the silkscreen
6.
       Category: Fix
       Description:
         [54986] CPU Overeheat Events Do Not Log with PROCHOT Assertion
       Infected motherboard: X10DRI, X10DRC
       Affected functions:
       Validation :
            1. Check the thermal guide Rev. 4.02 
            2. COA is activated when PROCHOT_N signal is asserted
               System monitor sw is requirement to report and record CPU overheating events in event logs
            3. COA is de-activated when CPU is cooled down from PROCHOT_N and DTS reading is equal to or smaller
               than -2
7.
       Category: Fix
       Description:
         [54642] FAN C&D will not speed up when I set to "Full Speed" Fan mode
       Infected motherboard: X10SRG
       Affected functions:
       Validation :
            1. Check the IPMI web gui

--------------------------------------------------------------  

Filename: SMT_X10_154.bin version: 1.54 Date: 07-28-2014         
                                                                 
U-Boot build time : 2009.01 (Nov 27 2013)                        
Java SOL Viewer version : v0.5.9                                 
Java iKVM Viwer version : v1.69 r22                              

***** For product spec. supports smbus mux design/riser card/AOC sensor reading   *****
***** /GPU sensor reading on Grantley platform, IPMI needs newer bios to support *****
***** NetFn=0x30 Cmd=0x70 SubCmd=0x3a and 0x5a command                           *****

1.
       Category: New feature
       Description:
         Support 8 riser cards.
           AOC-UR-i2XT,AOC-UR-i4XT,AOC-2UR6-i4XT,AOC-UR-i4G,AOC-2UR68-i4G,AOC-UR-i4G
           RSC-R2UW-4E8, RSC-R1UW-2E16,RSC-R2UW-2E8E16,RSC-R1UW-E8R,
           AOC-2UR68-i2XT,RSC-R1UG-A2E16-X9,RSC-R1UG-E16-X9,
           RSC-R1UG-E16AR+II,RSC-R1UG-2E8AR+II,RSC-R1UG-E16R+II,
           RSC-G2F-A66,RSC-G2FR-A66,RSC-G2B-A66
         Need new bios to send 0x3a, 0x5a command to activate GPU, Arp 10G AOC,
           LSI AOC/AOM, and NvME. after IPMI 1.54, BMC will NO LONGER detect above devices
           by itself on X10 Grantley platform.
       Infected motherboard: X10 Grantely motherboards
       Affected functions: GPU cards, Arp 10G AOC, LSI AOC/AOM, NvME
       Validation :
            1. Check if BMC can show these sensors of GPU, Arp 10G AOC, LSI AOC/AOM, NvME

2.
       Category: Fix
       Description:
         [55159] System has lost all sensor readings from IPMI webgui
       Infected motherboard: X10DDW
       Affected functions:
       Validation :
            1. Do factory default

3.
       Category: Fix
       Description:
         [55158] [EVT] Fan mode not works at all
       Infected motherboard: X10DRH
       Affected functions:
       Validation :
            1. Check fan mode

4.
       Category: Fix
       Description:
         [55157] [EVT] Non Sensor was displayed in firmware v1.53
       Infected motherboard: X10DRH
       Affected functions:
       Validation :
            1. Check fan mode

5.
       Category: Fix
       Description:
         [55079] SD5 shows FAN1 in "red color" even though it is not connected
       Infected motherboard: X10DDW
       Affected functions:
       Validation :
            1. Check senors and SD5  

6.
       Category: Fix
       Description:
         [55050] Number of Fans in IPMI wengui sensor reading page do not match with physical fan headers on motherboard
       Infected motherboard: X10DDW
       Affected functions:
       Validation :
            1. Check all fans are working when fans are fully populated. 

7.
       Category: Fix
       Description:
         [55036] No RT1/system sensor reading on IPMIGUI
       Infected motherboard: X10DRU-i+, X10DRU-X, X10DRU-XLL
       Affected functions:
       Validation :
            1. Check IPMI web gui

8.
       Category: Fix
       Description:
         [54984] FW 1.53 Logs Upper Non-Recoverable Events
       Infected motherboard: X10 Grantley motherboards
       Affected functions:
       Validation :
            1. Heat the cpu to overheat state. Check no no-recoverable events occurs 

9.
       Category: Fix
       Description:
         [54935] PCIeSSD temp sensor reading lost from sensor reading page
       Infected X10DDW
       Affected functions:
       Validation :
            1. Check if NvME Temp sensor is sometimes gone when NvME device is detected
 

10.
       Category: Fix
       Description:
         [54935] PCIeSSD temp sensor reading lost from sensor reading page
         [54886] IPMI webgui does not show correct NVMe SSD temp under PCIe_SSD tab
       Infected X10DDW
       Affected functions:
       Validation :
            1. Check if NvME Temp sensor is sometimes gone when NvME device is detected 
            2. Check PCIe_SSD tab shows correct information

11.
       Category: Fix
       Description:
         [54764] No LAN temperature readings in IPMI web GUI
       Infected motherboard: X10DRU-i+
       Affected functions:
       Validation :
            1. Insert AOC-XX-card to check bmc can read X540 LAN sensor (need newer bios)

12.
       Category: Fix
       Description:
         [54388] No NVMe drive Location Menu in IPMI Web GUI
       Infected motherboard: X10DRU-I
       Affected functions:
       Validation :
             1. Insert AOC-XX-card to check bmc can read NvME device (need newer bios)

14.
       Category: Fix
       Description:
         [54069] [IPMI] IPMI web doesn't show correct GPU label
       Infected motherboard: X10DRG-H(T)
       Affected functions:
       Validation :
             1. Please refer GPU_info.xlsx to determine GPU label and supported GPU number

15.
       Category: Fix
       Description:
         [55232] PCH Tempe" displays "Not Present" in IPMIWeb GUI with firmware v1.54
         [55229] Sensors of Onboard "10G LAN Temperature" displays "Not Present" in IPMIWeb GUI with firmware v1.54
       Infected motherboard: X10DRH
       Affected functions:
       Validation :
             1. Check IPMI web page

--------------------------------------------------------------  
Filename: SMT_X10_153.bin version: 1.53 Date: 07-xx-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r22


1.
       Category: Fix
       Description:
         [54675][EVT] Fan naming not matches with onboard Fan silkscreen
       Infected motherboard: X10DRU-i+, X10DRU-X, X10DRU-XLL
       Affected functions:
       Validation :
            1. Check the fan5~8 sensor names.

2.
       Category: Fix
       Description:
         [54761]No standard mode function in IPMI 
       Infected motherboard: X10DRU-X, X10DRU-XLL
       Affected functions:
       Validation :
            1. Check the fan mode configuration page of WebGUI.

3.
       Category: Enhancement
       Description:
         Nvidia new GPU card(K80) support
       Infected motherboard: x10 all platform
       Affected functions:
       Validation :
            1. When K80 is installed, check GPU Temp on sensor page.

4.
       Category: Enhancement
       Description:
         [54840][EVT] LAN Temperature shows "not present"
       Infected motherboard: X10DRU-X, X10DRU-XLL, X10DRU-i+
       Affected functions:
       Validation :
            1. Check the LAN Temp sesnor on the sensor page.

5.
       Category: Enhancement
       Description:
         [54867][IPMI] IPMI drop XeonPhi #3 temperature reading and fan speed 
         is set to 1500 RPM during overnight cburn on/off test. 
       Infected motherboard: X10DRG-H(T)
       Affected functions:
       Validation :
            1. Check if XeonPhi #3 temperature reading is gone 
               during overnight cburn on/off test.
 
6.
       Category: Fix
       Description:
         [54817] CPU Overheat LED is not working when CPU overheat
       Infected motherboard: C7Z97-MF
       Affected functions:
       Validation :
            1. Overheat the cpu and observe if the led is solided on.
            
7.
       Category: Fix
       Description:
         [54812] FAN Failure LED is not working when FAN fail
       Infected motherboard: C7Z97-MF
       Affected functions:
       Validation :
            1. pull out the plugged fan and obseve if the led is flashing      

8.
       Category: Fix
       Description:
         [54812] Drive Not Present in IPMI SEL with AOM-3108
       Infected motherboard: X10DRW-I
       Affected functions:
       Validation :
            1. On/Off stress test on the motherboard with LSI HDDs installed
            2. Check the false alarm event happen.  

9.
       Category: New motherboards
       Description:
          C7X99_OCE, X10SRA-F
       Infected motherboard: C7X99_OCE, X10SRA-F
       Affected functions:
       Validation :
--------------------------------------------------------------
Filename: SMT_X10_152.bin version: 1.52 Date: 07-11-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r22

***X10DRT-P, X10DRC Production Release***

1. 
       Category: Fix
       Description:
         [54373] PCIe SSD sensor readings are wrong under IPMI webgui sensor page 
         [54372] IPMI sensor reading webpage only shows 3 PCIe SSD temp, it should be 4 as I have 4 ports on mb
       Infected motherboard: X10DDW
       Affected functions:
       Validation :
            1. Connect the PCIe NvME SSDs 
            2. Check if PCIeSSD web page appears and content are right
            3. Check if only one PCIeSSD temperature sensor on sensor reading pages
  
2.
       Category: Fix
       Description:
         [54264] 5VCC low on node2 when running cburn 
       Infected motherboard: A1SA2 1.02 motherboards
       Affected functions:
       Validation :
            1. Do cburn on/off on both node
            2. Check if 5VCC sensor sel log on node2 will appear.

3.
       Category: Fix
       Description:
         [54217] IPMI SEL (event log) got some unknown "Chassis Intrusion" messages
       Infected motherboard: X10DRi     
       Affected functions:
       Validation :
            1. Run system S4 stress test    
            2. Check SEL logs 

4.
       Category: Fix
       Description:
         [54561] RT2 Temperature in IPMI is Higher than Measured Thermocouple Value 
       Infected motherboard: X10DRC     
       Affected functions:
       Validation :
            1. Check the RT2 temperature of this version is lower 9 degree from ther preious IPMI version    

5.
       Category: Fix
       Description:
         [54556] LAN temperature in IPMI web shows as 9x degree C when system idle  
       Infected motherboard: X10DRG-Q   
       Affected functions:
       Validation :
            1. Check if no LAN sensor again on the IPMI sensor reading page
            2. If yes, do factory default  

6.
       Category: New Feature
       Description:
         The sensor reading of A1SRM_LN7F, X10DRU_X, C7Z97_M are supported 
       Infected motherboard:   A1SRM_LN7F, X10DRU_X, C7Z97_M
       Affected functions:
       Validation :
            1. Check on IPMI sensor reading page

7.
       Category: Fix
       Description:
         [54642] FAN C&D will not speed up when I set to "Full Speed" Fan mode.
       Infected motherboard:   X10SRG
       Affected functions:
       Validation :
            1. Check on fan mode if works

8.
       Category: Fix
       Description:
         [54606] Fan control function didn't work on Fan A, B, C and D 
       Infected motherboard:   X10SDRG-Q
       Affected functions:
       Validation :
            1. Check on fan mode if works

9.
       Category: Fix
       Description:
         [54552] [SYS-5038MA-H24TRF] No power supply column in sensor reading page. 
       Infected motherboard:   A1SA2, X10SLE-D,X10SLE,X10SLD
       Affected functions:     
       Validation :
            1. Check if power sensor exists on IPMI sensor reading page 

10.
       Category: Fix      
       Description:
         [54574] There is no chassis intrusion sensor reading on IPMI WebGUI
       Infected motherboard: X10DRU-X                        
       Affected functions:
       Validation :
            1. Check the Sensor list. 
            
11.
       Category: Fix      
       Description:
         [53518] [IPMIView] Trap Shows Incorrect Sensor Name for All DIMM Slots with Memory ECC Assertion
       Infected motherboard: X10DRC                      
       Affected functions:
       Validation :
            1. Setup the IPMI smtp setting
            2. Launch the Trap Receiver on IPMIView
            3. Trigger Memory ECC command to check. The sensor name should show "DIMMA1", not "DIMM1A".

12.
       Category: Fix      
       Description:
         [54532] Everytime I try to locate different NVMe SSDs (0,1,2,3) under PCIe SSD tab but it always locate slot 0
       Infected motherboard: X10DRC                      
       Affected functions:
       Validation :
            1. Enter PCIe web page
            2. Set locate function to other slot. Do not set to slot 0
            3. Check if the function works.

13.
       Category: Fix
       Description:
         [54326] System goes to full fan speed mode whenever I go to cburn.
       Infected motherboard: X10QBi
       Affected functions:
       Validation :
            1. Run the Cburn on/off test.
            2. Check the fan speed is normal or not.

14.
       Category: Enhancement
       Description:
         Remove duplicate systm info page.
       Infected motherboard: X10QBi
       Affected functions:
       Validation :
            1. Since System page and System info page show the same information. Just remove it

15.
       Category: Enhancement
       Description:
         Remove duplicate systm info page.
       Infected motherboard: X10 all platforms
       Affected functions:
       Validation :
            1. Since System page and System info page show the same information. Just remove it

16.
       Category: Enhancement
       Description:
         Add Hardware information page on System tab
       Infected motherboard: X10 all platforms
       Affected functions:
       Validation :
            1.Bios needs to send smbios information to bios
            2.Then IPMI web page will present this information

17.
       Category: Fix
       Description:
         [54607] Some fan speed sensor readings didn't match silkscreen 
       Infected motherboard: X10DRG-Q
       Affected functions:
       Validation :
            1.Check if fan number names are the same as another printed on the silkscreen

18.   
      Category: Fix
      Description:
        [51386] IPMI cannot handle network looping (ARP packet storm)
      Infected motherboard: X10DRT-P
      Affected functions:
      Validation :
    	1. do the loopback on the swicth and will cause the arp storm.
    	2. check if the heatbeat LED is blinking and IPMI FW is alive.

-----------------------------------------------------------------------------------------------

Filename: SMT_X10_151.bin version: 1.51 Date: 06-28-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r22

1. 
       Category: New Feature
       Description:
         [54095] [IPMI] No Email Alert Description for PCIE PERR and SERR 
       Infected motherboard: X10DRC-LN4, X10DRC-T4, X10DRI-T4
       Affected functions:
       Validation :
            1. Set the SMTP.
            2. Trigger the PCI PERR and SERR.
            3. Check the event log.
            4. Check the email.

2.
       Category: Fix
       Description:
         Add VmemVRM sensor
       Infected motherboard: X10DRG-H(T)
       Affected functions:
       Validation :
            1. Do reset factory default once
            2. Check VmemVRM sensors

3.
	   Category: Fix
       Description:
             [54224][ SUM 1.3.0 ] Reset IPMI will clear all bin files.
       Infected motherboard: X10SRL-F
       Affected functions:
       Validation :
            After reset IPMI , run some command will not success , such as "Clear Event Log".
            e.g.
             ./sum -i 10.135.171.134 -u ADMIN -p ADMIN -c  ClearEventLog
             
4. 
       Category: New Feature
       Description:
         Support sensor support X10DRT-H, X10DRG-Q  
       Infected motherboard: X10DRT-H, X10DRG-Q,  
       Affected functions:
       Validation :
            1. Check IPMI sensor reading page

5. 
       Category: Fix
       Description:
         [54178] SEL gets filled with Drive Fault logs  
       Infected motherboard: X10DRC, X10DRW
       Affected functions:
       Validation :
            1.Create 8 Raid 0 HDDs
            2.Do cuburn on/off
            3.Check if there is a false alarm about HDD event sel log
 
6.
       Category: Fix
       Description:
         [53739] Fan speed goes up and down during post in Standard Mode
       Infected motherboard: X10DBT
       Affected functions:
       Validation :
            1.Power on the SUT
            2.Change the fan mode to the standard mode
            3.Monitor Fans to see their fan speed.

7.
       Category: Fix
       Description:
         [54330] Xeon Phi fan function failed and all fans are at full speed 
       Infected motherboard: X10DRG-H(T)
       Affected functions:
       Validation :
            1.Check fan control function with Xeon Phi card

8.
       Category: Fix
       Description:
         [54372] IPMI sensor reading webpage only shows 3 PCIe SSD temp, it should be 4 as I have 4 ports on mb
       Infected motherboard: X10DDW
       Affected functions:
       Validation :
            1.Check if there are 4 SSDs appear on the NvME web page

9.
       Category: Fix
       Description:
         [54390] No NVMe drive location menu in IPMI Web GUI
       Infected motherboard: X10DBT
       Affected functions:
       Validation :
            1.Check if there are 4 SSDs appear on the NvME web page

10.
       Category: fix
       Description:
            [53921] Fan pulse width modulation test fail
       Infected motherboard: X10SLH-N6-ST031
       Affected functions:
       Validation :
            1. Heat the LAN chips and see if pwm cycle heated
            2. Power on the system, measure the pmw cycle is 50% in 40 seconds after system is powered on 
            3. Power off the system and power on, measure the pmw cycle is 50% in 40 seconds. 

-----------------------------------------------------------------------------------------------

Filename: SMT_X10_150.bin version: 1.50 Date: 06-13-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r22

1.
       Category: New Feature
       Description:
         Support NvME function
       Infected motherboard: X10 Grantley platform (Smbus no.7 for X10DDW, Smbus no.4 is for X10DBT. Other Smbus no.3). 
       Affected functions:
       Validation :
            1. Insert NvME Add on card on PCIe slot
            2. BMC will automatically detect and Add 2 NvME temperature sensors at least one PCIeSSD HDD is plugged in
            3. BMC will remove NvME sensors once No PCIeHDDs is populated.

2.
       Category: New Feature
       Description:
         [53550] VRM sensor reading are "Not Present!"
       Infected motherboard: X10DRFF, X10DRFR
       Affected functions:
       Validation :
            1. Power up the SUT.
            2. Login the WebGUI to see the sensor page.

3.
       Category: Fix
       Description:
         [54064] 10GLAN Temp sensor reading is incorrect
       Infected motherboard: X10DRG-H(T)
       Affected functions:
       Validation :
            1. Uncheck Preserve Configuration when upgrade IPMI.
            2. Reboot system.
            3. Verfiy X10DRG-HT has 10GLAN Temp.
               (X10DRG-H is 1G LAN model; X10DRG-HT is 10G LAN model)

4.
       Category: Fix
       Description:
         [54031] IPMI Configuration: Changes on Port settings can not be saved 
       Infected motherboard: X10 motherboards
       Affected functions:
       Validation :
            1. Change port setting in Configuration category.
            2. Check services are going to direct to new port

5. 		
	   Category: Fix
       Description:
        	[54092][ SUM 1.3.0 ] SMCIPMITool Raw command will cause DMI issue.  
       Infected motherboard: X10 motherboards
       Affected functions:
       Validation :
        Run the follow command to see if it is ok.
       ./sum -i 10.135.171.134 -u ADMIN -p ADMIN -c GetDMIInfo --file D_Cfg-X10SRL/dmi_first.txt --overwrite

6. 	   Category: Fix 
       Description:
          [54081]After update IPMI V1.49 FW, system will generate "Processor Thermal Trip - Asserted" message in Event Log   
          [54041]CPU thermal trip 1.49 IPMI
          [54093]IPMI logs "Processor Thermal Trip - Asserted" in event log every time the system is powering down 
          [54098]IPMI sel recorded "Thermal Trip" while system reboot or shutdown. 
       Infected motherboard: X10 motherboards
       Affected functions:
       Validation :
        1. do unit reset on web.
        2. check if there will not be the thermal trip event log.

7. 	   Category: Fix 
       Description:
          [54102] FAN6 fan fail action is incorrect.    
       Infected motherboard: X10SRW-F
       Affected functions:
       Validation :
        1. Insert fans on FAN6 and FAN7 connectors.Then enter IPMI sensor page
        2. pulled out FAN7 connector, check if BMC would show FAN6 and FAN7 fail.
8.
       Category: Fix
       Description:
         [54031] Fan speed goes up and down during post in Standard Mode
       Infected motherboard: X10DBT
       Affected functions:
       Validation :
            1. Update both of two X10DBT motheboards.
            2. Power on both of two X10DBT motherboards. And wait them to OS.
            3. Keep them idle.
            4. Observe the Fan behavior.

9.
       Category: Fix
       Description:
         [54102] FAN6 fan fail action is incorrect.
       Infected motherboard: X10DBT
       Affected functions:
       Validation :
            1. Pulled out FAN6 connector.
            2. Check the WebGUI.
            3. Pulled out FAN7 connector.
            4. Check the WebGUI. 
10.
       Category: Fix
       Description: High NR of CPU temp always show 'N/A', and sensor show green color if the value locates between UC to LC
       Infected motherboard: X10 series
       Affected functions:
       Validation :
			1. checking sensor readings web page that
			   1-1 if the threshold Hing NR of CPU Temp show 'N/A'
			   1-2 showing the sensor green while the reading value is between UC and LC
				   showing the sensor yellow while the reading value is between UC and UNR or between LC and LNR.
				   showing the sensor red while the reading value is upper then UNR or lower then LNR
-----------------------------------------------------------------------------------------------

Filename: SMT_X10_149.bin version: 1.49 Date: 06-06-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r22

1.
       Category: Fix
       Description:
         CPU# Not Match Between Email Alert Event Description and IPMI Event Log
       Infected motherboard: X10 motherboards
       Affected functions:
       Validation :
            1. Setup the smtp account and trigger the Memory ECC command
            2. Compare between the CPU number inside email and another one inside sel logs. It should be the same

2.
       Category: New feature
       Description:
		Add CPU thermal trip
       Infected motherboard: X10 motherboards
       Affected functions:
       Validation :
            1. heat CPU until the system shut down.
            2. we will have the event log of the thermal trip on IPMI web. 

3.
       Category: fix
       Description:
        [53558] [IPMI] FANs on right zone and left zone DO NOT run lowest speed when there is NO GPU detected
       Infected motherboard: X10DRG-H
       Affected functions:
       Validation :
            1. Check if the fan speed is following middle cooling zone
               when some other unsupported GPU or PCIe cards installed

4.
       Category: fix
       Description:
		[53433] SUM 1.3.0 - ChangeBMCcfg fail. 
	    [53746] [SUM 1.3.0 ] Invalid BMC configuration text file.
       Infected motherboard: A1SA2
       Affected functions:
       Validation :
		   1. issue the follow SUM commands.
			  a. sum -i IP -u ADMIN -p ADMIN -c getbmccfg --file bmc.cfg 
			  b. sum -i IP -u ADMIN -p ADMIN -c changebmccfg --file bmc.cfg

5.
       Category: fix
       Description:
            [53946] [IPMI ECO] CPU# Not Match Between Email Alert Event Description and IPMI Event Log 
            [53522] IPMI] Email Alert Event Description Not Shown For Memory ECC Error Assertion 
       Infected motherboard: All motherboard
       Affected functions:
       Validation :
            1. Set the SMTP.
            2. Generatre Ecc events.
            3. See the Email.

6.
       Category: fix
       Description:
            [53944] VmemVRM temperature missing 
       Infected motherboard: X10DRL-i
       Affected functions:
       Validation :
            1. Power up the SUT.
            2. Check the WebGui.
7.
       Category: fix
       Description:
            [53985] Upper Non-Critical Event logged in IPMI SEL
       Infected motherboard: X10DRC-T
       Affected functions:
       Validation :
            1. Heat the LAN chips and check if upper Non-Critical event is issued.

8.
       Category: fix
       Description:
            [53921] Fan pulse width modulation test fail
       Infected motherboard: X10SLH-N6-ST031
       Affected functions:
       Validation :
            1. Heat the LAN chips and see if pwm cycle heated
            2. Power on the system, measure the pmw cycle is 50% in 40 seconds after system is powered on 
            3. Power off the system and power on, measure the pmw cycle is 50% in 40 seconds. 

-----------------------------------------------------------------------------------------------

Filename: SMT_X10_148.bin version: 1.48 Date: 05-23-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r22

1.
       Category: Enhancement
       Description:
         The overheat criteria is changed to DTS - 0 when cpu is overheated.
         Follow the latest Thermal Guide SIM_TDG REV. 4.01 (05292014).pd)
       Infected motherboard: X10 motherboards
       Affected functions:
       Validation :
            1. Change the overheat condition occurs

2.
       Category: fix
       Description:
        [53739] Fan speed goes up and down during post in Standard Mode
       Infected motherboard: X10DBT
       Affected functions:
       Validation :
            1. Set the fan mode to Standard Mode.
            2. Power up the SUT.
            3. Wait about 90 seconds. (Temperature sources will have keen competition during this time.)
            4. Make sure no scripts are running.
            5. Observing the fan speed.

3.
       Category: fix
       Description:
        [53871] There is no Power supply info present under IPMI webgui sensor reading page.
       Infected motherboard: X10QBi
       Affected functions:
       Validation :
            1. Login the WebGui and switch to the Sensor Readings page.

4.
       Category: fix
       Description:
        [53522] [IPMI] Email Alert Event Description Not Shown For Memory ECC Error Assertion.
       Infected motherboard: All motherboards
       Affected functions:
       Validation :
            1. Set the SMTP.
            2. Generatre Ecc events.
            3. See the Email.

5.
       Category: fix
       Description:
        [53809] Power supply sensor missing with IPMI 1.47
       Infected motherboard: X10DRG
       Affected functions:
       Validation :
            1. Login to the sensor reading page of WebGUI

6.
       Category: fix
       Description:
        [53728] IPMI user privilege settings are incorrect
       Infected motherboard: X10DRU-I
       Affected functions:
       Validation :
            1. Using user account that privilege is USER/OPERATOR to login web page.
            2. Check mouse mode and sel page.

-----------------------------------------------------------------------------------------------

Filename: SMT_X10_147.bin version: 1.47 Date: 05-23-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r22

1.
       Category: fix
       Description:
        [53522] [IPMI] Email Alert Event Description Not Shown For Memory ECC Error Assertion.
       Infected motherboard: X10DRC and X10DBT
       Affected functions:
       Validation :
            1. Set the SMTP.
            2. Generatre Ecc event.
            3. See the Email.

2.
       Category: fix
       Description:
        [53512] Zone two(Fan A,B,C,D) always keep in 46.3% at HeavyIO mode 
        [53552] [IPMI] FSC doesn't follow thermal guideline when only one GPU is heating up
       Infected motherboard: X10DRG-H
       Affected functions:
       Validation :
            1. Need to reset factory default once for X10DRG-H.
            2. Use PCH FSC profile for GPU sensors at HeavyIO mode.
            3. Only optimal, heavy I/O, and full speed fan modes are options (optimal mode
               is the default setting).
            4. Check fan speed control for all GPU slots in different fan mode.

3.
       Category: fix
       Description:
        [53558] [IPMI] FANs on right zone and left zone DO NOT run lowest speed when there is NO GPU detected
       Infected motherboard: X10DRG-H
       Affected functions:
       Validation :
            1. When Full Speed Mode is chosen, all fans run at full speed
            2. When there is no card detected on PCI-E slot 1, 2, 3, 4, 5, or 6, Fans A-H
               remain on the lowest fan speed

4. 
		Category: fix
        Description:
         [53586] Four fan sensors are missing
        Infected motherboard: X10DRU-I+
        Affected functions:
        Validation :
             Login web GUI and check sensor reading.

5.
		Category: fix
        Description:
         [53588] The power supply sensor reading is incorrect
         [53624] The multi node monitoring function should not show on IPMI WebGUI
		 [53581] No power fail led 
		 [53585] No Overheat LED When CPU overheat
        Infected motherboard: X10DRU-I
        Affected functions:
        Validation :
             1. Login to the sensor reading page of WebGUI
             
6.
		Category: fix
        Description:
         [52449] Voltage sensors reading are gone after BMC reset on X10SLM-F
        Infected motherboard: X10SLM-F
        Affected functions:
        Validation :
             1. Check the IPMI web gui to see if all adc sensors are gone when sensors are starting polling             

7. 
     	Category: fix
        Description:
    	 [53621] The VmemVRM Temp sensor readings are showing N/A
        Infected motherboard: X10DRU-I
        Affected functions:
        Validation :
           1. Login to the sensor reading page of WebGUI

8. 
		Category: fix
        Description:
         [53623] The description for BIOS Resileence is incorrect and the help description is missing
        Infected motherboard: X10DRU-I
        Affected functions:
        Validation :
               1. Login to the BIOS Resilience page of WebGUI

9.
    Category: fix
    Description:
     [53463] Event log gets filled with SEL that is not related
    Infected motherboard: X10DBT
    Affected functions:
    Validation :
         1. Clear the SEL first.
         2. Power cycle the SUT.
         3. Check the SEL.

10. 
		Category: fix
    Description:
			[53728] IPMI user privilege settings are incorrect 
    Infected motherboard: X10DRU-I
    Affected functions:
    Validation :
           1. Using user account that privilege is USER/OPERATOR to login web page.
					 2. Check mouse mode and sel page.

-----------------------------------------------------------------------------------------------
Filename: SMT_X10_146.bin version: 1.46 Date: 05-xx-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r22

1.
       Category: fix
       Description:
		[53388] IPMI web-gui detects wrong speed for shared LAN 
		[53465] Network speed in IPMI web-gui shows 100M when connected to shared network  
       Infected motherboard: X10DRC and X10DBT
       Affected functions:
       Validation :
		    1. go to the network page and check if the link status of the share
               lan.


2.
       Category: fix
       Description:
		[47450] [EVT] JI2C1 / JI2C2 header not Functioning  
		[52571] Storage Monitoring needs to be enabled in IPMI for onboard 3108 
		[52410] IPMI sensor readings can't detection HDD status on AOM-S3108-H8 
		[52751] Storage Monitoring needs to be enabled in IPMI for onboard 3108  
		[52337] We can not see Storage monitoring page when installing LSI2208 storage card to the board 
       Infected motherboard: X10DRC ,X10DRI,X10DRW,X10DRFF
       Affected functions:
       Validation :
			1. check the phsical/Logic HDD status on Storage Monitoring page

3.
       Category: fix
       Description:
		[53381] Where does IPMI read the LSI ctrl temperature from?  
       Infected motherboard: X10DRC 
       Affected functions:
       Validation :
			1. heat LSI chip and check if LSI Ctrl temperature sensor goes higher.

4.
       Category: fix
       Description:
        [52888] Power supply sensor missing
       Infected motherboard: X10DRG-H
       Affected functions:
       Validation :
            1. check if power supply sensor presents

5.
       Category: fix
       Description:
        [53392] IPMI sensor issue: DIMMA2 is not working correctly
       Infected motherboard: X10DRG-H
       Affected functions:
       Validation :
            1. install DIMMA2 and DIMMB1 separately
            2. check if DIMMA2 and DIMMB1 present correctly

6.
       Category: fix
       Description:
        [53464] Some of the sensor readings show N/A
       Infected motherboard: X10DBT
       Affected functions:
       Validation :
            1. check the sensor list in WebGUI or ipmitool

7.
       Category: fix
       Description:
        [52802] 5 LED Front Panel's OH doens't blink when there is power failure
       Infected motherboard: X10DRG-H
       Affected functions:
       Validation :
            1. check if event is logged when there is power failure
            2. check if 5 LED Front Panel's OH blinks 

8.
       Category: fix
       Description:
        [53509] Peripheral temperature RT2 swapped with systemtemperature RT1
       Infected motherboard: X10DRG-H
       Affected functions:
       Validation :
            1. heat RT1/RT2
            2. check if temperature goes up correctly

9.
       Category: fix
       Description:
        [53462] IPMI 1.45 fw has problems changing different fan speed mode
        [53527] HeavyIO FPWM failed
       Infected motherboard: X10DBT
       Affected functions:
       Validation :
            1. Login to the fan mode page of WebGUI
            2. Change the fan mode and see the fan speed.

10.
       Category: fix
       Description:
        [53125] Some SDIII readings are incorrect
       Infected motherboard: X10SRI
       Affected functions:
       Validation :
            1. Run the SD3 and see the result.


12.
       Category: fix
       Description:
				[53536]CPU overheat cause OS reboot and alarm & LED won't turn off after reboot on X10DRC-T4+ 
       Infected motherboard: X10DRC
       Affected functions:
       Validation :
		  1. do CPU overheat test and LED will be on. 
		  2. reboot system and check if LED will be off when cpu is not in
			overheat state

13.
			Category: fix
      Description:
        [53588] The power supply sensor reading is incorrect
				[53586] Four fan sensors are missing
       Infected motherboard: X10DRU-I
       Affected functions:
       Validation :
 					1. Login to the sensor reading page of WebGUI

14.
 			Category: fix
       Description:
				[53581] No power fail led
       Infected motherboard: X10DRU-I
       Affected functions:
       Validation :
 					1. Create a power fault, ex: AC loss, and check power led 
  
 
=============================================================
Filename: SMT_X10_145.bin version: 1.45 Date: 05-08-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r22

***A1SA2 Production Release***
Notice:Please read the item 1 description when you update node2 FW.

1.
       Category: Enhanecement
       Description:
               The BMC slave address is changed to 0x20 
       Infected motherboard: The node 2 of A1SA2
       Affected functions:
       Validation :
               FW update though web
               1. Update this FW but keep the check on the preseve box on the FW update web page
               2. Wait for updating and bmc will reboot
               3. Then execute "Factory default" on IPMI web page
               4. Use ipmitool command, "ipmitool sdr" to see if sensor information is displayed correctly
               
               FW update though dos
               1. execute "ADupdate -f SMT_X10_145.bin -r y" (Preseve the original setting)
               2. Wait for updating and bmc will reboot
               3. Then execute "ipmicfg -fd" to do factory default
               4. Use ipmitool command, "ipmitool sdr" to see if sensor information is displayed correctly

2.
       Category: Fix
       Description:
               [53313] No Alert LED or IPMI event log when CPU overheat 
       Infected motherboard: X10DRG-H
       Affected functions:
       Validation :
               1. Need to reset factory default once for X10DRG-H.
               2. Check if IPMI event is logged when CPU overheat
3.
       Category: Fix
       Description:
               [53024] Jordan Creek Memory Buffer Temperature not available in IPMI
       Infected motherboard: X10DBT
       Affected functions:
       Validation :
               Note: Please make sure the A1 should be the first DIMM slot. If A1 does not have DIMM, the JC sensor would not be shown.

               1. Check the sensor list page or sensor list command.
4.
       Category: Fix
       Description:
               [53347] Always full fan with IPMI 1.44
       Infected motherboard: X10DRW-I
       Affected functions:
       Validation :
               1. Check the fan sensor in the WebGUI or sensor list command.
5.
       Category: Fix
       Description:
               [53377] CPU temperature status readings are still showing values in IPMI Multinode monitoring status page when the node is off
       Infected motherboard: X10DRFR
       Affected functions:
       Validation :
               1. Check IPMI multinode web page
6.
       Category: Fix
       Description:
               [53356] CPU temperatures are not shown correctly under IPMI Web GUI multinode page
       Infected motherboard: X10DRFR
       Affected functions:
       Validation :
               1. Check IPMI multinode web page

=============================================================
Filename: SMT_X10_144.bin version: 1.44 Date: 05-06-2014
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r22

***X10DRI Beta Release***

1.
        Category: Fix
        Description:
                [52867] FAN sensors in IPMI are incorrect 
        Infected motherboard: X10DRG-H
        Affected functions:
        Validation :
                1. Disconnect FAN A, B, C and D(according to MB silkscreen).
                2. Check if IPMI logs correct event log.

2.
        Category: Fix
        Description:
                [53112] Battery voltage reading fail
        Infected motherboard: X10DRG-H
        Affected functions:
        Validation :
                1. Need to reset factory default once for X10DRG-H.
                2. Verify the reading of VBAT.

3.
        Category: Fix
        Description:
                [53072] CPU2 VRM Temperature not available in IPMI
        Infected motherboard: X10DBT
        Affected functions:
        Validation :
                1. Verify the reading of CPU2 VRM.

4.
        Category: Fix
        Description:
                [53100] IPMI firmware 1.41 (1.43 cannot see CPU3 Temp & CPU4 Temp)
        Infected motherboard: X10QBi
        Affected functions:
        Validation :
                1. Check the CPU3 Temp and CPU4 Temp value.
5.	
        Category: Fix
        Description:
                [52396]  FAN always run full speed 
        Infected motherboard: X10SLM+-LN4F
        Affected functions:
        Validation :
                1. Please left system idle overnight and see if FANs speed is
				at the full speed.

6. 
        Category: Fix
        Description:
                [53164]  No LSI Ctrl Temp in IPMI Web GUI  
        Infected motherboard: X10DRW-I
        Affected functions:
        Validation :
				1. please check if LSI sensor has reading.
				(be noted the motherboard must be reworked)
7. 		

        Category: Fix
        Description:
                [47450]  I2C1 / JI2C2 header not Functioning  
		Infected motherboard: X10DRI-T
		Affected functions:
        Validation :
				1.please check if there is the storage monitoring on ipmi web.

8. 		
        Category: Enhancement
        Description:
                New backplane is supported on X10DRFR  
		Infected motherboard: X10DRFR
		Affected functions:
        Validation :
				1.Please use new backplane and use IPMI 1.44 after.
				
9. 		
        Category: Enhancement
        Description:
                Support A1SA2 HW reversion 1.02
		Infected motherboard: A1SA2
		Affected functions:
        Validation :
 
=============================================================
Filename: SMT_X10_143.bin version: 1.43 Date: 04-xx-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r22

1.
       Category: Fix
       Description:
               [52591] Processor error message during SAT test on X10SLM-F
       Infected motherboard: All motherboard with ME
       Affected functions:
       Validation :
               1. Run SAT 24 hour test.
               2. Check the SEL and Error messages.

2.
       Category: Fix
       Description:
               [52118] Node 2 CPU overheat will not trigger Alert LED to turn solid on
       Infected motherboard: X10SLE-DF
       Affected functions:
       Validation :
               1. Let CPU overheat on node 2
               2. Check if the Alert LED turns solid on

3
       Category: Fix
       Description:
               [52495] No DIMM 2 to be detected on ipmi web
               [52716] No PCH Temp & memory dim temp reading in the IPMI Web GUI
       Infected motherboard: X10DRW
       Affected functions:
       Validation :
               1. Check the sensor reading page of Web GUI

4.
       Category: Fix
       Description:
               [52967] Memory temperature doesn't show in IPMI
       Infected motherboard: X10SRH
       Affected functions:
       Validation :
               1. Check the sensor reading page of Web GUI

5.
       Category: Fix
       Description:
               [52887] FAN always is full speed.
               [52886] Power status always is "Not Present" in IPMI Power Source page
               [52886] No any sensor reading in IPMI
       Infected motherboard: X10SLH-N6
       Affected functions:
       Validation :
               1. Check the sensor reading page of Web GUI.

6.
       Category: Fix
       Description:
               [52434] VDIMM sensor readings are correct but show "Upper Non-recoverable" error message
       Infected motherboard: X10DDW
       Affected functions:
       Validation :
               1. Check VDIMM sensor value is normal

7.
       Category: Fix
       Description:
               [52093] IPMI "DIMM Temp" sensor reading show "Not Present"
       Infected motherboard: X10SRI
       Affected functions:
       Validation :
               1. Check the sensor reading page of Web GUI

8.
       Category: Enhancement 
       Description:
	   	add LSI Ctrl temp. sensor and do the fan control according
	   	to its temperature.
       Infected motherboard: X10DRW X10DRC
       Affected functions:
       Validation :
               1. Please do the reset-to-default 
			   2. Check if LSI Ctrl sensor on IPMI web.

9. 		
       Category: Fix
       Description:
               [52859] vmem VRM readings missing
       Infected motherboard: X10DRL-I
       Affected functions:
       Validation :
               1. Check the sensor reading page of Web GUI

=============================================================
Filename: SMT_X10_142.bin version: 1.42 Date: 04-xx-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r22
1.
		Category: Fix 
		Description:
			[52620] [BIOS] CTLM Memory Throttling Not Working 
			[52730]CLTM Memory Throttling Not Working. 
		Infected motherboard: X10SLH and X10SLM
		Affected functions:
		Validation :
			1. heat on the memory and see if the memory throttling works.

2.
		Category: Fix 
		Description:
			[52682] Event logs get filled with Vmem temperature logs 
			[52675] IPMI sensor reading abnormal
			[52671] VmemVRM Temp senosr reading abnormal
			[52661] X10SRI-F system got "Lower Non-recoverable" error drung the CPU linpack testing
			
		Infected motherboard: X10 motherboard with Grantley CPUs
		Affected functions:
		Validation :
		  1. Check the memory VRM values are normal on IPMI web gui
		  2. Do linpack testing to see if event log is issued

3.
    Category: Fix
    Description:
      [52671] VmemVRM Temp senosr reading abnormal
    Infected motherboard: X10 motherboard with Grantley CPUs
    Affected functions:
    Validation :
      1. Check the memory VRM values are normal on IPMI web gui
      2. Do linpack testing to see if event log is issued

4.
    Category: Fix
    Description:
		  [52464]Inconsistent behavior under IE9/Chrome/Firefox/Safari after prompt for
		updating Java in IPMI webpage 
    Infected motherboard:A1SA7
    Affected functions:
    Validation :
		  1.  in IPMI webpage, if one clicks 'system information' menuitem, a
			    dialog box will prompt if necessary to update java 
		  2.  click "yes" and check if you can get the same behavior using the
			    different browsers. 

4.
    Category: Fix
    Description:
		[52191]IPMI Web Report Wrong Node Position
    Infected motherboard:X10DRT-P
    Affected functions:
    Validation :
		1.login in other nodes except node A.
		2.Enter multinode page and check currnet node

=============================================================
Filename: SMT_X10_141.bin version: 1.41 Date: 04-16-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r22
1.
        Category: Fix
        Description:
        [49610] There should not be more than one IPMI console redirection allowed from IPMI webgui.  
        Infected motherboard: All
        Affected functions:
        Validation :
                 the goal for this enhancement is to avoid the users do the harmful thing to the system when the bios 
                 is updating though OOB.
                 1. while bios is updating though web/SUM,iKVM viewer will got the notification and
                   close itself. 
                 2. while the bios is updating through web/SUM, the user can't launch iKVM viewer. 

2.
        Category: Fix
        Description:
        [52663] [IPMI Firmware v1.40 ECO]No SNMP Trap, Email Alert and Event Log when CPU Overheat
        Infected motherboard: X10QBi X10DRi-T X10DRi-T_10G
        Affected functions:
        Validation :
                 1. Make CPU overheat, and then check the SEL, SNMP Trap, Email

3.
		Category: Fix
        Description:
        [52301] Failed to boot from CDROM & Floppy by ipmitool.                                                                    
        Infected motherboard: X10DRL
        Affected functions:
        Validation :
                 1. ipmitool chassis bootparam get <option number>
                 2. reboot the system.

4.
        Category: Enhancement
        Description:
        Brickland memory ECC & non-ECC erros definition
        Infected motherboard: X10QBi
        Affected functions:
        Validation :
                 1. Correctable Memory ECC @ [DIMM silkscreen on Memory Riser]([SMI slot silkscreen on MB]
                    example : Correctable Memory ECC @DIMMC2[P3M1]
                    ipmitool -I lanplus -H 172.31.40.89 -U ADMIN -P ADMIN raw 0x4 0x2 0x4 0x0c 0xff 0x6f 0x0 0x2C 0x82

5.
        Category: Fix
        Description:
        [52503] IPMI NO SENSOR READINGS AND NO FAN CONTROL
        Infected motherboard: X10DRG-H
        Affected functions:
        Validation :
                 Add X10DRG-H board support

============================================================================================
Filename: SMT_X10_140.bin version: 1.40 Date: 04-12-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r22

***X10QBI Product Release***

1.
        Category: Fix
        Description:
        [52443][IPMI]Power Fail Email Alert Does Not Have Event Description to Mention Power Fail Event
        Infected motherboard: All
        Affected functions:
        Validation :
                 1. Set SMTP in web Gui.
                 2. Generate a power fail event.
                 3. Check the E-mail.
2.
        Category: Fix
        Description:
        [52552]ipmi FW1.39 shows abnormal reading from sensor readings
        Infected motherboard: All DP motherboards
        Affected functions:
        Validation :
                 1. Login Web Gui, and check sensor reading page.
3.
        Category: Fix
        Description:
        [51948]Half of the DIMM temp don't show up
        Infected motherboard: X10DRi-T
        Affected functions:
        Validation :
                 1. Login Web Gui, and check sensor reading page.

4.
        Category: Fix
        Description:
        [50628] When updating BIOS through IPMI WEB GUI, user is still able to browse through other IPMI tabs. 
                BIOS Update status is lost afterwards
        Infected motherboard: All
        Affected functions:
        Validation :
                 1. Browse through other IPMI Tabs while updating BIOS through IPMI Web GUI.
                 2. Go back to BIOS Update Page.

5.      
        Category: Fix
        Description:
        [52464] Some characters missing in the help description in IPMI
                webpage under IE9
        Infected motherboard: A1SA7
        Affected functions:
        Validation :
                 1. launch IE9 and login in IPMI web.
                 2. click the help tab and check if the help wordings miss.

6.
        
        Category: Fix
        Description:
        [52383]  Power monitoring incorrect units
        Infected motherboard: X10DRL
        Affected functions:
        Validation :
                 this page is not used any longer and it is replaced with Power
                 consumption page.
7.
         Category: Fix
         Description:
         the password of AD user can't be more than 19 characters.
         Infected motherboard: All
         Affected functions:
         Validation :
                  1. add the AD user with the passowrd which length is exceeding
                      30 characters.
                  2. set up the AD setting on AD webpage.
                  3. enter AD username and password on the login page and see if
                      the login is ok.
8.
         Category: Fix
         Description:
         Only detect 3 GPU sensors when all 4 GPU sensors are installed
         Infected motherboard: X10QBI
         Affected functions:
         Validation :
                  1. Check IPMI web gui to check GPU sensor status

9.
         Category: Fix
         Description:
         [52191] IPMI Web Report Wrong Node Position
         Infected motherboard: X10DRT-P
         Affected functions:
         Validation :
                  1. Check the multinode web page
            
============================================================================================
Filename: SMT_X10_139.bin version: 1.39 Date: 04-09-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

*** ME smbus 400KHz support on X10 Grantley platform ***

1.
        Category: Fix
        Description:
        [52450] X10DDW-i3 MCE and Voltage error during cburn test
        [52434] VDIMM sensor readings are correct but show "Upper Non-recoverable" error message. 
        Infected motherboard: X10DDW
        Affected functions:
        Validation :
                 1. Check the status of the VDIMMxx sensors are normal. No touch LC, HC
2.
        Category: Fix
        Description:
        [52355] Inconsistent readings for invalid sensor data in Web/SD5/IPMIView
        Infected motherboard: A1SA7
        Affected functions:
        Validation :
                 1. Check the TR1,TR2 sensor status shold be N/A when sensors are not installed
3.
        Category: Fix
        Description:
        [52459] Help description is missing for "HDD control" menu in IPMI web page
        Infected motherboard: A1SA7
        Affected functions:
        Validation :
                 1. Check Help page of HDD control
4.
        Category: Fix
        Description:
        [52497] [ IPMIView for Android 0.0.18 ] Sensor readings are different
        Infected motherboard: X10DRW
        Affected functions:
        Validation :
                 1. Use ipmitool command to check if fan5 and fan6 sensors still exist on SDR 
                                               
============================================================================================

Filename: SMT_X10_138.bin version: 1.38 Date: XX-XX-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

*** ME smbus 400KHz support on X10 Grantley platform ***

1.
        Category: Fix
        Description:
        [52088] GPU temperatures will sometimes show N/A in IPMI after A/C cycle
        Infected motherboard: All grantley motherboards & X10QBI
        Affected functions:
        Validation :
                 1. Run A/C cycle test
                 2. Check the GPU temperature sensor values

2.
        Category: Fix
        Description:
        [50381] NM Policy alert function is not working
        Infected motherboard: All motherboards with ME
        Affected functions:
        Validation :
                 1. Set SNMP by SMCipmitool
                 2. Set Alert by SMCipmitool
                 3. Set Power Policy by SMCipmitool
                 4. Disable NM Policy
                 5. Enable NM Policy

3.      
        Category: Fix
        Description:
        [52396] FAN always run full speed 
        [52385] Fan always runing full speed on x10slm-f with IPMI 1.37  
        Infected motherboard: X10SLM+-LN4F X10SLM-F
        Affected functions:
        Validation :
                1. check if the fan speed is full.
4.
        Category: Fix
        Description:
        [52355][52330] [NM] Some SMCIPMITool Commands Not Working  
        Infected motherboard: All
        Affected functions:
        Validation :
            run the following command.
            java -jar SMCIPMITool ip ADMIN  ADMIN nm20 ver
5.       
        Category: Fix
        Description:
        [customer issue]Active directory authentication does not work with User Domain Name
        Infected motherboard:
        Affected functions:
        Validation :
            1. go to AD setting web and input more than 16 characters in
            the user domain name
            2. save it and see if the user domain is saved successfully.
6.
    
        Category: Fix
        Description:
        [customer issue]firefox showed  Cert error "sec_error_reused_issuer_and_serial" when using https.
        Infected motherboard:
        Affected functions:
        Validation :
            1. run firefox to surf IPMI web though https and the ssl certificate will be saved
            2. run the following command to clear SSL certiifcate and
            ipmitool -I lanplus -H 10.133.176.44 -U ADMIN -P ADMIN raw 0x30 0x68 0
            2. surf IPMI web using firefox through https
 
7.
            
        Category: Fix
        Description: 
        [52411] the bridge command through RMCP 1.5 can't work.
        [52353] Some SMCIPMITool Commands Not Working
        [52330] Some SMCIPMITool Commands Not Working

        Infected motherboard: ALL
        Affected functions:
        Validation :
        please issue the below command
        ipmitool -H 10.133.176.175 -U ADMIN -P ADMIN -t 0x2c -b 0 raw 6 1

8.
            
        Category: Fix
        Description: 
        [52410] IPMI sensor readings can't detection HDD status on AOM-S3108-H8 

        Infected motherboard: X10 DP motherboards
        Affected functions:
        Validation :
      1.Check if storage web menu occured on the IPMI web gui   (bios need to set bit 6 of 1st byte on 0x30 0x99 command)

9.
            
        Category: Enhancement
        Description: 
        [52410] Add memory VRM sensors
        Infected motherboard: X10DRC, X10SRH,X10SRL,X10SRI,X10SRW
        Affected functions:
        Validation :
      1.Check these on IPMI web page
 
============================================================================================
Filename: SMT_X10_137.bin version: 1.37 Date: 03-28-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

*** ME smbus 400KHz support on X10 Grantley platform ***

1.    
    Category: Fix
    Description:
    [52054] Whange ME SMbus clock to 400KHZ  for all DP motherboards. 
    Infected motherboard: All grantley motherboards & X10QBI
    Affected functions:
    Validation :
         Please make sure if PCH clock is 400KHZ.
2.    
    Category: Fix
    Description:
    [52182] System fans randomly fluctuates between full speed and regular speed under PUE mode
    [52179] Heavy I/O FSC mode missing in IPMI web GUI

    Infected motherboard: X10SLE-D
    Affected functions:
    Validation :
        Check fan mode function

3.    
    Category: Fix
    Description:
    [52127] Some fail event in mail isn't complete. 
    Infected motherboard: A1SA2
    Affected functions:
    Validation :
        1.Setup smtp server and personal email
        2.Heat the CPU temperature and let it hit non-recoverable threshold
        3.Chek the email to see "UNR_going high" string completely 

4.    
    Category: Fix
    Description:
    [52054] Web GUI Console Redirection Crashed for Mac OS with Firefox and Safari Web Browser 
    Infected motherboard: X10 motherboards
    Affected functions:
    Validation :
        1.Use Mac book and launch console redirection

5.    
    Category: New feature
    Description: [52126]Support Dual BIOS boot block.
    Infected motherboard: All grantley motherboards
    Affected functions:
    Validation :
        Please take a look at the BIOS Resilience page on the Miscellaneous
        tab.

6.    
  Category: New feature
  Description: Support the Brickland platform ME function
               Read CPU and Memory temps from ME
               Fill the temps into sensor reading value
               Add Memory temp into Fan control algorithm
  Infected motherboard: X10QBI
  Affected functions:
  Validation :
    
7.
  Category: new feature
  Description: Add AOC sensors
  Infected motherboard: X10SRL
  Affected functions:
  Validation :
    1. check the sensor list on ipmi web.

=====================================================================================

Filename: SMT_X10_136.bin version: 1.36 Date: 03-XX-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

1.
    Category: new feature
    Description: add VM ISO/IMA oem commands
    Infected motherboard:
    Affected functions:
    Validation :
      please check the function of cdrom and floppy image on ipmi web.
2.    
    Category: Fix
    Description:
    [51802] System lost IPMI MAC address & IPMI address while running system on-off test & also lost KCS interface
    [51916] "BMC's KCS interface not working after 592 cycles of on/off test"
    [51498] KCS Interface Doesn't Work After Running 200 Times ONOFF Test  
    [51463] IPMI got rebooted automatically & then lost its MAC address while doing system on-off test 

    Infected motherboard: X10DRL X10QBI X10DRI
    Affected functions:
    Validation :
        run c-burn test
3.
    Category: Fix
    Description: [51695] [ SUM 1.3.0 ] ChangeBMCcfg fail.
    Infected motherboard: All
    Affected functions:
    Validation :
    Run the following commands.
        1 sum -i 10.135.169.12 -u ADMIN -p ADMIN -c getbmccfg --file bmc.cfg
        2 sum -i 10.135.169.12 -u ADMIN -p ADMIN -c changebmccfg --file bmc.cfg
4.
    Category: Fix
    Description: [51460] VBAT Reading is wrong 
    Infected motherboard: X10DDW
    Affected functions:
    Validation :
      1.Check IPMI sensor reading web page
5.
    Category: Fix
    Description: [51851] VBAT Voltage is high while doing Cburn 
    Infected motherboard: X10DRi X10DRi-T
    Affected functions:
    Validation :
      1.Check IPMI sensor reading web page
6.
    Category: Fix
    Description: [51868] IPMI web GUI sensor readings does not change to upper non-recoverable
    Infected motherboard: All
    Affected functions:
    Validation :
      1.Check IPMI sensor reading web page

7.
    Category: Fix
    Description: [51697] OEM SEL record while running IPMI on/off
    Infected motherboard: All
    Affected functions:
    Validation :
      1.Running IPMI on/off test
      2.Check SEL from the web GUI or ipmitool
8.
    Category: Fix
    Description: [51930] IPMI Firmware v1.35 has major issues
    Infected motherboard: All
    Affected functions:
    Validation :
      1.Setting smtp from web GUI
      2.Setting alert from web GUI
      3.Send alert and check the mailbox
9.
    Category: Fix
    Description: [51653] No Dual boot block UI 
    Infected motherboard: X10SRL
    Affected functions:
    Validation :
      1.Check web page Miscellaneous -> BIOS Resillience
      2.Insert usb key with BIOS recovery utility and afudos.
      3.Power on the system and update BIOS by afudos.
      4.Cut the AC Power during erasing stage.
      5.Recover the AC Power, make sure the BIOS is broken.
      6.Miscellaneous -> BIOS Resillience -> Click "Resile"
        (This action would power off the system.)
      7.Power on the system, it will entry into the BIOS Setup Menu, Recovery page.
      8.Power cycle the system.

10.
  Category: Fix
  Description: [52041] Some IPMI readings are missing after restarting
  Infected motherboard: A1SA7
  Affected functions:
  Validation :
    1.Ac off & on, check RT1, TR1 and TR2 sensors if gone

=====================================================================================

Filename: SMT_X10_135.bin version: 1.35 Date: 03-14-2014

U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

*** Only solve on A1SA2, A1SA7 and X10QBI ***
*** After finishing the update, please restore factory default. ***

    Category: Enhancement
    Description: Support A1SA7, X10SRH sensor readings
    Infected motherboard: 1SA7, X10SRH
    Affected functions:
    Validation :
      1.Check sensor readings page on IPMI web gui


    Category: Fix
    Description: [51774] No IPMI sensor reading
    Infected motherboard: A1SA7
    Affected functions:
    Validation :
      1.Check sensor readings page on IPMI web gui

    Category: Fix
    Description: [50646] Dual boot block function is failed.
                [50647] Dual Boot Block check fail.
                [51653] No Dual boot block UI.
    Infected motherboard: X10DRFF X10DRW X10SRL
    Affected functions:
    Validation:
     1. Insert usb key with BIOS recovery utility and afudos.
     2. Power on the system and update BIOS by afudos.
     3. Cut the AC Power during erasing stage.
     4. Recover the AC Power, make sure the BIOS is broken.
     5. ipmitool -I lan -H <IP> -U ADMIN -P ADMIN raw 0x30 0x70 0x68 0x1 0x2
        (Change to boot block 2, and power off the system.)
     6. Power on the system, it will entry into the BIOS Setup Menu, Recovery page.
     7. After finishing the recovery, change back to boot block 1 by command.
        (ipmitool -I lan -H <IP> -U ADMIN -P ADMIN raw 0x30 0x70 0x68 0x1 0x1)
     8. Power cycle the system.

  Category: Fix
  Description: [51380]IPMI 1.33 FW falsely detects PSU failure
  Infected motherboard: X10DRT-P
  Affected functions:
  Validation :
    check if the sensor page can show 2 PSU status.

  Category: Fix
    Description: [51788] No information in event log of IPMI on CPU1's memory slot. (Memory ECC test)
                 [51787] Wrong memory slot loacation in event log of BIOS and IPMI on CPU2's memory slot. (Memory ECC test)
    Infected motherboard: A1SA2
    Affected functions:
    Validation :
      1.Do Memory ECC/ non ECC test to check if the dimm location is the correct

    Category: Fix
    Description: [49516] IPMIView "System AC Power State" always is
                "S5/G2" state after press "Power Cycle" button
    Infected motherboard
    Affected functions:  X10SRE-DS018
    Validation :
    press power cycle button and check ACPI power status in IPMIview.

  Category: Fix
  Description: [51489] Function fail : A1SA2-2750F easy can't detect hardware monitor value
  Infected motherboard: A1SA2
  Affected functions:
  Validation :
  1. run ipmifcg -sdr and check if the sensor reading is ok

  Category: Fix
  Description: [51384] 1.33 IPMI in Internet Explorer 8 has error
  Infected motherboard: All
  Affected functions:
  Validation :
  Use IE8 to do login IPMI web and check if the login page is ok.

  Category: Fix
  Description: [51547] IPMI Web GUI-Some Tags don't have Japanese traniation.
  Infected motherboard: All
  Affected functions:
  Validation:
    1. Login WebGui and select Japanese.

  Category: Fix
  Description: [51524]IPMI Login page has some issues when using IE
  Infected motherboard: All
  Affected functions:
  Validation :
    1. use IE10 (without compatibility mode) to do login in IPMI web.

  Category: Fix
  Description: fix the issue KNC GPU can't run at the full speed.
  Infected motherboard: X10QBI
  Affected functions:
  Validation :
    1. check if KNC GPU can run at the high performance.

  Category: Fix
  Description: [51460] VBAT Reading is wrong
  Infected motherboard: X10DDR
  Affected functions:
  Validation :
    1.Enter IPMI sensor reading web page

=====================================================================================
Filename: SMT_X10_134.bin version: 1.34 Date: 02-27-2014
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21


*** After finishing the update, please restore factory default. ***

 Category: Fix
 Description: [51441] The DIMM temp and VDIMM of IPMI sensor web reading is incorrect 
              [51415] Some IPMI Monitor sensor reading is incorrect
              [51077] IPMI/BIOS Hardware Monitor Check Error
 Infected motherboard: X10SRL, X10SRI
 Affected functions: 
 Validation : 
   1.Enter IPMI sensor page

 Category: Fix
 Description: [51425] No sensors present complains IPMI webgui - 1.33 IPMI and 2/20 BIOS
              [51424] No Sensors Persent In The System
              [51032] 3rd DIMM Slot from Each Channel Missing Temperature Sensor
 Infected motherboard: X10DRC
 Affected functions: 
 Validation : 
   1.Enter IPMI web page

 Category: Fix
 Description: [51427] System failed to power on after running Dedicated LAN on/off for 119 cycles
              [51198] System on/off via IPIM stress failed
              [51178] System failed to power on when running share LAN IPMI on/off at the first cycle             
 Infected motherboard: X10DP motherboards
 Affected functions: 
 Validation : 
   1.Execute IPMI on&off script to power on & off the system repeatedly
  
 Category: Fix
 Description: [51537] IPMI sensor readings are incorrect
              [51460] VBAT Reading is wrong       
 Infected motherboard: X10SRW,X10DDW
 Affected functions: 
 Validation : 
   1.Don't Preserve Configuration before download
   2.Check IPMI sensor page

 Category: Fix
 Description: [51498]KCS Interface Doesn't Work After Running 200 Times ONOFF Test    
 Infected motherboard: X10DRI-T
 Affected functions: change mouse mode.
 Validation : 
   1.run Cburn
  
 Category: Fix
 Description: BMC kernel panic
 Infected motherboard: X10QBI
 Affected functions:
 Validation :
   1.It randomly happened.
   2.run Cburn or stay in red hat OS.
    
 Category: Fix
 Description: intermittent??problem of USB connect/disconnect issue
 Infected motherboard: X10QBI
 Affected functions:
 Validation :
   1.run Cburn
=====================================================================================
   
IPMI Firmware Release Note
----------------------------
Filename: SMT_X10_133.bin    version: 1.33    Date: 02-21-2014
U-Boot build time       : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

 Category: Fix
  Description: Read Tjmax value from ME to adjust the CPU tempeature throttling level    
  Infected motherboard: X10SLM-F
  Affected functions:  
  Validation : 
    1.Select one CPU which Tjmax is not 100
    2.Use "cpuMemTemp" command on smcipmitool to get Tjmax value
    3.Compare High NR value of CPU sensor on IPMI sensor readings page. Check if they are the same

  Category: Fix
  Description: [51240] Sometimes IPMI cannot work     
  Infected motherboard: X10SRI
  Affected functions:  
  Validation : 
    1. Check if bmc heart led is flashing at 1st system power-on

  Category: Fix
  Description: [50495] Fan speed goes up and down randomly when system is idle      
  Description: [50391] Fan speed unstable      
  Infected motherboard: X10DP motherboards
  Affected functions:  
  Validation : 
    1. Let system is idle and check if fan speed go up and down

  Category: Fix
  Description: [51240] Sometimes IPMI cannot work     
  Infected motherboard: X10SRI
  Affected functions:  
  Validation : 
    1. Check if bmc heart led is flashing at 1st system power-on

  Category: Fix
  Description: [51199] firmware v1.31 not supports "Help" Screen under BIOS Update fileld.     
  Infected motherboard: All
  Affected functions:  
  Validation : 
    1. Launch Help page on bios upload page

  Category: Fix
  Description: [50406] Cannot communicate with ME locally via KCS       
  Infected motherboard: X10DRT-P
  Affected functions:  
  Validation : 
    1. At linux environment, set "ipmitool -t 0x2c mc info
 
----------------------------
Filename: SMT_X10_132.bin    version: 1.32    Date: 02-13-2014
U-Boot build time       : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

  **** X10QBI Product Release Candidate ****
  ****Uncheck the preserved box while updating FW or do factory default after FW is updated ****

  Category: Fix
  Description: [51001] AER Uncorrected Fatal Error was logged in MCELOG when heating up GPU to High CT / High Non-Recoverable    
  Infected motherboard: X10QBI
  Affected functions:  
  Validation : 
    1. Check if fan speed is full speed when you heat GPU temperature over 75 degree

  Category: Fix
  Description: [51077] IPMI/BIOS Hardware Monitor Check Error     
  Infected motherboard: X10SRL-F
  Affected functions:  
  Validation : 
    1. Check VDIMM temperature is 1.2v

  Category: Fix
  Description: [51032] 3rd DIMM Slot from Each Channel Missing Temperature Sensor     
  Infected motherboard: X10DRC-F
  Affected functions:  
  Validation : 
    1. Use C0 CPU
    2. Check if 3rd dimms shows on the IPMI sensor page
    
  Category: Fix
  Description: [51000] No events were logged in IPMI event log when Xeon Phi was overheating (High Non Recoverable >104 degrees C)
  Infected motherboard: X10QBI
  Affected functions:  
  Validation : 
    1. Heat Xeon Phi GPU over 105 degree
    2. Check if event logs show correctly
    
  Category: Fix
  Description: [50673] Sometimes sensor reading appears (only few) before BIOS hand-off
  Infected motherboard: X10DP motherbaords
  Affected functions:  
  Validation : 
    1. Power on the system
    2. Check if sensors appeared early on IPMI sensor readings page

  Category: Fix
  Description: [49428] BIOS/IPMI cannot record the correctable or uncorrectable error for QPI/PCIE/Memory errors
  Infected motherboard: X10DRI
  Affected functions:  
  Validation : 
    1. Using Cscripts to inject QPI/PCIE/Memory correctable error
    2. Check if QPI error event log show on IPMI event log page

----------------------------
Filename: SMT_X10_131.bin    version: 1.31    Date: 02-07-2014
U-Boot build time       : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

  ****Uncheck the preserved box while updating FW or do factory default after FW is updated ****

  Category: Fix
  Description: [50871] IPMI Sensor Name Has Some Typo Error     
  Infected motherboard: X10DP motherboards
  Affected functions:  
  Validation : 
    1. ipmitool -H 10.133.176.74 -U ADMIN -P ADMIN sdr
    2. Check if the string of SDR name is not the same as another on IPMI web gui

  Category: Fix
  Description: [50847] PUE Fan mode missing in IPMI Fan Mode Setting     
  Description: [50473] FAN PWM measurement fail
  Infected motherboard: X10 Fat twin motherboards
  Affected functions:  
  Validation : 
    1. ipmitool -H 10.133.176.74 -U ADMIN -P ADMIN sdr
    2. Check if the string of SDR name is not the same as another on IPMI web gui

  Category: Fix
  Description: [49476] No GPU temperature reading shown in IPMI Web GUI   
  Infected motherboard: X10QBI
  Affected functions:  
  Validation : 
    1. Check GPU sensor exists at slot 11

  Category: Fix
  Description: the production issue-the mac address may be lost
  Infected motherboard: All
  Affected functions:
  Validation :
    1. upgrade the firmware using programmer and then set mac address
    2. Do AC-Off and AC-on and then check if the mac adress is ok.
    Or
    1. do factory-to-default on web and see if the mac address is ok.
----------------------------
Filename: SMT_X10_130.bin    version: 1.30    Date: 01-29-2014
U-Boot build time       : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

  Category: Fix
  Description: [50673] Sometimes sensor reading appears (only few) before BIOS hand-off     
  Infected motherboard: X10DP motherboards
  Affected functions:  
  Validation : 
    1. Check if bios is posting, IPMI sensor will appear

  Category: Fix
  Description: [50608] FAN speed control is not working and always is Full speed
               [50452] FANA and FANB are full speed in Heavy I/O mode 
               [50361] IPMI fan mode does't response 
               [50300] Fan PWM measurement fail  
               [49227] Fan PWM Test Fail                     
  Infected motherboard: All
  Affected functions:  
  Validation : 
    1. Check all fan mode works properly and fan curve is right

  Category: Fix
  Description: [50595] LAN reading is abnormal
  Description: [50336] LAN Temperature status is in Upper Non-Recoverable 127 degrees C
  Infected motherboard: X10 motherboards with 10G LAN models
  Affected functions:  
  Validation : 
    1. Check IPMI sensor readings page

  Category: Fix
  Description: [50525] CPU overheats and shuts down the system when system is in BIOS setup
  Infected motherboard: All
  Affected functions:  
  Validation : 
    1. Stay at bios menu
    2. Check if pwm duty cycle keeps 50%

  Category: Fix
  Description: [50519] "IP Access Control" cannot back to default setting after BMC load factory default
               [50397] "IP Access Control" cannot back to default setting after BMC load factory default
  Infected motherboard: All
  Affected functions:  
  Validation : 
    1. Add something on IPMI Access Control page
    2. Do factory reset on IPMI web gui
    3. Check if empty conten on IPMI Access Control page

  Category: Fix
  Description: [50451] Cannot reload "Web Session", "FAN Mode" and "IP Access Control" item after reload IPMI Configuration
               [50518] Cannot reload "Web Session", "FAN Mode" and "IP Access Control" item after reload IPMI Configuration 
  Infected motherboard: All
  Affected functions:  
  Validation : 
    1. Load IPMI configuration
    2. reload the IPMI configuation and check the values of if web session, fan mode and IP access control resume
 
  Category: Fix
  Description: [50511] FAN mode no "Optimal", "PUE" item 
               [50473] FAN PWM measurement fail
  Infected motherboard: Fan twin motherboards
  Affected functions:  
  Validation : 
    1. Support PUE mode
 
  Category: Fix
  Description: [50495] Fan speed goes up and down randomly when system is idle
               [50391] Fan speed unstable
  Infected motherboard: Fan twin motherboards
  Affected functions:  
  Validation : 
    1. Let system enter idle mode, and monitor fan speed will suddenly up & down
            
  Category: Fix
  Description: [50423] After updating IPMI FW v1.29, IPMI function is not working any more  
  Infected motherboard: Twin pro motherboards
  Affected functions:  
  Validation : 
    1. Enter bios menu after updating IPMI FW
    2. Check if IPMI status in BIOS still shows "Not Working". 
    3. BMC Firmware Revision in BIOS still shows "79.7b"
 
  Category: Fix
  Description: [50406] Cannot communicate with ME locally via KCS 
  Infected motherboard: Twin pro motherboards
  Affected functions:  
  Validation : 
    1. At Remote site : ipmitool -H <BMC_IP> -U user -P password -t 0x2c mc info
    2. At localt site : ipmitool -t 0x2c mc info 
    3. Check if two functions work.
 
  Category: Fix
  Description: [50395] Hardware monitor fail
               [50392] RT1/RT2 reading abnormal   
  Infected motherboard: X10DRFF
  Affected functions:  
  Validation : 
    1. Check if the Thermometer reading is close to another one on IPMI web gui (RT1 & RT2)

  Category: Fix
  Description: [50339] No power supply sensor reading in IPMI 
  Infected motherboard: Fan twin motherboards
  Affected functions:  
  Validation : 
    1. Check if power supply sensor exists on IPMI sensor readings page

  Category: Fix
  Description: [50266] Power Fail LED Frequency Fail 
  Infected motherboard: Fan twin motherboards
  Affected functions:  
  Validation : 
    1. Insert two power supplies and plug out one
    2. Check if power fail led is flashing
  
  Category: Fix
  Description: [49697] 10G LAN temperature" sensor is not working properly  
  Description: [49476] No GPU temperature reading shown in IPMI Web GUI   
  Infected motherboard: X10QBI
  Affected functions:  
  Validation : 
    1. Check IPMI sensor readings page
    2. heat LAN sensor to check if value goes high

----------------------------
Filename: SMT_X10_129.bin    version: 1.29    Date: 01-17-2014
U-Boot build time       : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

**** X10SRE-DS018 Product Release Candidate ****

  Category: Fix
  Description: [50392] RT1/RT2 reading abnormal   
               [50391] Fan speed unstable    

  Infected motherboard: X10DRFF
  Affected functions:  
  Validation : 
    1. Check RT1 temperature is lower then RT2
    2. Check Fan speed is table at OS idle
    
  Category: Fix
  Description: [50361] IPMI fan mode does't response 
               [50360] Lan temperature
               [50354] Optimal speed should not show on the IPMI Fan mode meau
               [50336] LAN Temperature status is in Upper Non-Recoverable 127 degrees C                    
               [50266] Power Fail LED Frequency Fail      
  Infected motherboard: X10DRFR
  Affected functions:  
  Validation : 
    1.After download new IPMI FW, do factory reset again to clear older SDR
    2. Check sensor readings page    
    3. Check fan mode
    4. Check fan fail led if works
    
  Category: Fix
  Description: [50300] Fan PWM measurement fail                 
  Infected motherboard: A1SA2
  Affected functions:  
  Validation : 
    1.Check fan curve

  Category: Fix
  Description: [50150] FPWM Heavy IO temperature always keep in 44.36%  
               [50148] Stand FPWM low temp PWM
  Infected motherboard: X10DRT-PT-
  Affected functions:  
  Validation : 
    1. Check fan curve

  Category: Fix
  Description: [50139] The "Vcpux" sensor naming should be "VCpu1" & "Vcpu2"  
  Infected motherboard: All X10DP motherboards
  Affected functions:  
  Validation : 
    1. Check cpu sensor name

  Category: Fix
  Description: [50017] Fan PWM Test Failed    
  Infected motherboard: X10DRL-I
  Affected functions:  
  Validation : 
    1. Check fan curve

  Category: Fix
  Description: [49476] No GPU temperature reading shown in IPMI Web GUI   
  Infected motherboard: X10QBI
  Affected functions:  
  Validation : 
    1. Check GPU sensor appeared at slot 9 and slot 11

  Category: Enhancement
  Description: [49476] Fan Pulse-Width-Modulation Measurement fail    
  Infected motherboard: X10SRE-DS018
  Affected functions:  
  Validation : 
    1. Check the fun duty cycle is 100% all the times


  Category: Fix
  Description: [49227] Fan PWM Test Fail    
  Infected motherboard: X10DRL-I
  Affected functions:  
  Validation : 
    1. Check fan curve
----------------------------
Filename: SMT_X10_129.bin    version: 1.29    Date: 01-17-2014
U-Boot build time       : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

**** X10SRE-DS018 Product Release Candidate ****

  Category: Fix
  Description: [50392] RT1/RT2 reading abnormal   
               [50391] Fan speed unstable    

  Infected motherboard: X10DRFF
  Affected functions:  
  Validation : 
    1. Check RT1 temperature is lower then RT2
    2. Check Fan speed is table at OS idle
    
  Category: Fix
  Description: [50361] IPMI fan mode does't response 
               [50360] Lan temperature
               [50354] Optimal speed should not show on the IPMI Fan mode meau
               [50336] LAN Temperature status is in Upper Non-Recoverable 127 degrees C                    
               [50266] Power Fail LED Frequency Fail      
  Infected motherboard: X10DRFR
  Affected functions:  
  Validation : 
    1.After download new IPMI FW, do factory reset again to clear older SDR
    2. Check sensor readings page    
    3. Check fan mode
    4. Check fan fail led if works
    
  Category: Fix
  Description: [50300] Fan PWM measurement fail                 
  Infected motherboard: A1SA2
  Affected functions:  
  Validation : 
    1.Check fan curve

  Category: Fix
  Description: [50150] FPWM Heavy IO temperature always keep in 44.36%  
               [50148] Stand FPWM low temp PWM
  Infected motherboard: X10DRT-PT-
  Affected functions:  
  Validation : 
    1. Check fan curve

  Category: Fix
  Description: [50139] The "Vcpux" sensor naming should be "VCpu1" & "Vcpu2"  
  Infected motherboard: All X10DP motherboards
  Affected functions:  
  Validation : 
    1. Check cpu sensor name

  Category: Fix
  Description: [50017] Fan PWM Test Failed    
  Infected motherboard: X10DRL-I
  Affected functions:  
  Validation : 
    1. Check fan curve

  Category: Fix
  Description: [49476] No GPU temperature reading shown in IPMI Web GUI   
  Infected motherboard: X10QBI
  Affected functions:  
  Validation : 
    1. Check GPU sensor appeared at slot 9 and slot 11

  Category: Enhancement
  Description: [49476] Fan Pulse-Width-Modulation Measurement fail    
  Infected motherboard: X10SRE-DS018
  Affected functions:  
  Validation : 
    1. Check the fun duty cycle is 100% all the times


  Category: Fix
  Description: [49227] Fan PWM Test Fail    
  Infected motherboard: X10DRL-I
  Affected functions:  
  Validation : 
    1. Check fan curve
 
----------------------------
Filename: SMT_X10_128.bin    version: 1.28    Date: 01-10-2014
U-Boot build time       : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21


  Category: Fix
  Description: [50125] GPU temperature is shown in-between PS1 and PS2, please see attached picture  
  Infected motherboard: X10QBI
  Affected functions:  
  Validation : 
    1. Check IPMI sensor readings page

  Category: Fix
  Description: [50101] The hardware monitor test fail  
  Infected motherboard: 10X10DRW-IT
  Affected functions:  
  Validation : 
    1. Check IPMI sensor readings page

  Category: Fix
  Description: [50059] CTLM Memory Throttling Not Working  
  Infected motherboard: All
  Affected functions:  
  Validation : 
    1. Enter CLTM memory Throttling test

  Category: Fix
  Description: [50028] Power LED and Overheat LED no signal 
               [50024] IPMI/BIOS Hardware Monitor Check (VDIMM Voltage)
               [50023] Standard Speed OF FAN (PWM duty cycle) always keep around 50%.
               [49988] IPMI Sensor Readings shows VBAT voltage as 13.545 volts
               [49987] IPMI event log shows LAN TEMP as 127 degrees C

  Infected motherboard: X10DRT-PT,X10DRT-PIBQ
  Affected functions:  
  Validation : 
    1. Check the sensor status in IPMI web gui

  Category: Fix
  Description: [50022] Hardware Monitor Check Failed 
               [50017] Fan PWM Test Failed
               [49994] Teperature sensor are showing incorrect in IPMIWeb GUI
               [49992] [EVT] Voltage sensor "VBAT" shows "Upper Non-Recoverable" error in IPMIWeb GUI
                       
  Infected motherboard: X10DRL_I
  Affected functions:  
  Validation : 
    1. Check all sensor status are ok on IPMI web gui
    2. Check vdimm (1.2v) and vbat (3.21v) on IPMI web gui
    3. Check dimm sensor(1.2v) and vbat (3.21v) on IPMI web gui


  Category: Fix
  Description: [49982] Fail to install win2008 from remote iso file 
               [49962] iKVM stress failed
                       
  Infected motherboard: A1SAM
  Affected functions:  
  Validation : 
    1. Install win2008 from remote iso file
    2. iKVM stress (video playback in the background and use wintrax to copy iso file from VM 
    
  Category: Fix
  Description: [49927] IPMI power control "reset" function is not working  
  Infected motherboard: X10DRFF
  Affected functions:  
  Validation : 
    1. Try to reset function on IPMI web gui

  Category: Fix
  Description: [49925] IPMI Event Log Time stamp always is 1970/01/01  
  Infected motherboard: X10Dp boards
  Affected functions:  
  Validation : 
    1. Set date & time on bmc web gui randomly when syste is powered on
    2. BMC Unit reset
    3. Check if date & time synchronized from ME 

  Category: Fix
  Description: [49428] BIOS/IPMI cannot record the correctable or uncorrectable error for QPI/PCIE/Memory errors  
  Infected motherboard: X10Dp boards
  Affected functions:  
  Validation : 
    1. Set date & time on bmc web gui randomly when syste is powered on
    2. BMC Unit reset
    3. Check if date & time synchronized from ME 

  Category: Fix
  Description: [49227] Fan PWM Test Fail  
  Infected motherboard: X10Dp boards
  Affected functions:  
  Validation : 
    1. Set date & time on bmc web gui randomly when syste is powered on
    2. BMC Unit reset
    3. Check if date & time synchronized from ME 

----------------------------
Filename: SMT_X10_127.bin    version: 1.27    Date: 01-06-2014
U-Boot build time       : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

  Category: New feature
  Description: OOB server Asset management -DDNS 
             
  Infected motherboard: All
  Affected functions: ddns function on ipmi web
  Validation : 
    1. go to DDNS page and verify if it works.

  Category: New feature
  Description: Add X10DRFR sensor suppport 
  Infected motherboard: X10DRFR
  Affected functions:
  Validation : 
    1. 

  Category: Fix
  Description: [49994] [EVT] Teperature sensor are showing incorrect in IPMIWeb GUI
               [49992] [EVT] Voltage sensor "VBAT" shows "Upper Non-Recoverable" error in IPMIWeb GUI
   
  Infected motherboard: X10DRL-I
  Affected functions:  
  Validation : 
    1. Check IPMI sensor status on web page 

  Category: Fix
  Description: [49988] [EVT] IPMI Sensor Readings shows VBAT voltage as 13.545 volts
               [49992] [EVT] IPMI event log shows LAN TEMP as 127 degrees C
   
  Infected motherboard: X10DRL-I
  Affected functions:  
  Validation : 
    1. Check IPMI sensor status on web page 

  Category: Fix
  Description: [49958] SMCIPMITool NM command is not work 
  Infected motherboard: A1SA2
  Affected functions:  
  Validation : 
    1. Use nm20 command by smcipmitool 

  Category: Fix
  Description: [49860] Fan PWM measurement fail 
               [49802] Hardware monitor fail  
               [49799] Sensor readings are fail 
  Infected motherboard: A1SA2
  Affected functions:  
  Validation : 
    1. Check if fan sensor exists on IPMI web page 
    2. Check if we can see all sensors on BMC2 IPMI web page

  Category: Fix
  Description: [49788] The date format are different. 
  Infected motherboard: All
  Affected functions:  
  Validation : 
    1. Check if BMC build date format is the same as Bios 

  Category: Fix
  Description: [49476] No GPU temperature reading shown in IPMI Web GUI
  Infected motherboard: X10QBI
  Affected functions:  
  Validation : 
    Support KNC and Kelper. 

  Category: Fix
  Description: [49227] Fan PWM Test Fail 
  Infected motherboard: DRI_T, DRI
  Affected functions:  
  Validation : 
    1. Check IPMI web page if sensors are good 

  Category: Fix
  Description: [49318] FPWM Heavy IO mode does not start from 50% duty cycle 
  Infected motherboard: QBI
  Affected functions:  
  Validation : 
    1. Set the HeavyIO mode on QBI and power on. Measure the pwm cycle.

  Category: Fix
  Description: [48951] FPWM Heavy IO mode does not start from 50% duty cycle 
  Infected motherboard: QBI
  Affected functions:  
  Validation : 
    1. Set the HeavyIO mode on QBI and power on. Measure the pwm cycle.
 


  Category: Fix
  Description: [48951] Fan PWM Test Fail 
               [49992]
  Infected motherboard: X10SRE-DS018
  Affected functions:  
  Validation : 
    1. Check IPMI sensor status on web page   
  
----------------------------
Filename: SMT_X10_126.bin    version: 1.26    Date: 12-25-2013
U-Boot build time       : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

  **For X10DRI_T, X10DRI beta release only

  Category: Fix
  Description: [49762] Can't login to SUT IPMI IP by ipmi command during SUM test, but can login by web browser 
  Infected motherboard: X10SLL
  Affected functions:  
  Validation : 
    1. doing SUM stress test and see if SUM failed to login to IPMI firmware.

  Category: Fix
  Description: [49762] Can't login to SUT IPMI IP by ipmi command during SUM test, but can login by web browser 
  Infected motherboard: X10SLL
  Affected functions:  
  Validation : 
    1. doing SUM stress test and see if SUM failed to login to IPMI firmware.

  Category: Fix
  Description: [49656] VRM temperatures don't present and Naming doesn't follow thermal guildeline 
  Infected motherboard: X10DRI, X10DRI_T
  Affected functions:  
  Validation : 
    1. Enter IPMI sensor page to see if only one VRM sensor exists
    
  Category: Fix
  Description: [49641] CPUs reading got disappeared after a while with 12-10-2013 bios & IPMI FW 1.24 
  Infected motherboard: X10DRI, X10DRI_T
  Affected functions:  
  Validation : 
    1. Power On & Off the system to see if cpu sensor is missing

  Category: Fix
  Description: [49640] IPMI system power consumption monitoring is misbehaving 
  Infected motherboard: X10SLE-DF
  Affected functions:  
  Validation : 
    1. AC unplugged & plugged the system, and check the values of power consumption are correct
       (power consumption web page)

  Category: Fix
  Description: [49609] IPMI Web GUI shows incorrect IPMI Share LAN link status when the cable is unplugged. 
  Infected motherboard: All
  Affected functions:  
             (1)the network connectivity under all lan modes.
             (2)switch lan mode,e.g. switch the failover mode to share or dedicated mode.
  Validation : 
  (1) Connect cables to both IPMI Share and delicated LAN
  (2) Check IPMI Web GUI -> Configuration -> Network -> Network Link Status. It shows both are connected
  (3) Then remove cable from Share LAN and check the network link status again.


  Category: Fix
  Description: [49605] there are no DIMMs temperature readings under IPMI webgui sensor reading page
  Infected motherboard: X10DRI, X10DRI_T
  Affected functions:  
  Validation : 
    1.Enable the CLTT mode
    2.there are no DIMMs temperature readings under IPMI webgui sensor reading page

   Category: Fix
  Description: [49415] Fan Pulse-Width-Modulation Measurement fail 
  Infected motherboard: X10SRE_DS018
  Affected functions:  
  Validation : 
    1.Enable the CLTT mode
    2.there are no DIMMs temperature readings under IPMI webgui sensor reading page
----------------------------
Filename: SMT_X10_125.bin    version: 1.25    Date: 12-13-2013
U-Boot build time       : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

[New feature]
  Description: SMC RAKP 
  Infected motherboard: ALL
  Affected functions: IPMI Lan connection
  Validation :
    1.Please use SMCIPMITool 2.6.4 in project board id = 1360. 
    2.To enable SMC RAKP in misc SMC RAKP page. 
    3.Modify SMCIPMITool.properties(oem_rakp=on/off).
    4.use SMCIPMITool to connect BMC via Lan 
      Usage:
    smcipmitool  <BMC ip>  ADMIN ADMIN ipmi sr
    5.when oem_rakp=on, SMCIPMITool can connect to BMC.
      when oem_rakp=off,SMCIPMITool cannot connect to BMC.
   
    6.To disable SMC RAKP in misc SMC RAKP page.    
      use SMCIPMITool to connect BMC via Lan
    7.when oem_rakp=on, SMCIPMITool cannot connect to BMC.
      when oem_rakp=off,SMCIPMITool can connect to BMC.
  
[Enhancement]

  Category: Enhancement
  Description: A1SA2, X10DRFF and X10DRW_I board support
  Infected motherboard: A1SA2, X10DRFF and X10DRW_I
  Affected functions:  BMC2 is not supported yet (A1SA2)
  Validation : 

  Category: Enhancement
  Description: [Production request]add bios revision when doing bios update through web and SMCIPMItool
  Infected motherboard: All
  Affected functions:  
    (1) BIOS update on web.
    (2) OOB BIOS update 
  Validation : 
    (1) make sure the bios image can support bios revision. otherwise,it is not shown.
    (2) do bios update through web and SMCIpmitool.

  Category: Enhancement
  Description: Enhance the polling time for VBAT sensor to make it more durable
  Infected motherboard: All
  Affected functions:  All
  Validation : make sure if any VBAT event logs appears when doing the on-off stress test or c-burn test.

[Fix]

  Category: Fix
  Description: [49373] IPMI WebGUI not working properly after updating to version 1.24 
  Infected motherboard: X10QBI
  Affected functions: NONE
  Validation : login in IPMI web by using Firefox/IE/chrome and check if it works.

  Category: Fix
  Description: [49373] Fan PWM measurement fail 
  Infected motherboard: X10SLX-F
  Affected functions: NONE
  Validation : measure descending fan curve
  
  Category: Fix
  Description: BMC's NM Discovery SDR is incorrect.Please take a look at attached and see the last 4 bytes.
  Infected motherboard: The motherboard with ME function 
  Affected functions: It just not fit the standard
  Validation:
   Use smcipmitool to key in "nm20 nmSDR". It should like the following values
   Health Event Sensor Number             = 25h
   Exception Event Sensor Number          = 24h
   Operational Capailities Sensor Number  = 26h
   Alert Threshold Exceeded Sensor Number = 27h



----------------------------
Filename: SMT_X10_124.bin    version: 1.24    Date: 11-29-2013

U-Boot build time       : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

[Enhancement]
  Description: Add firmware recovery 
  Infected motherboard: ALL
  Affected functions:   
    1. firmware upgrade through http and https
    2. firmware upgrade though dos/windows/linux utilities.
  Validation :
    1. make sure the firmware 1.24 or later resides in the flash
    2. upgrade the firmware and plug off the power cable during fw upgrade.
    3. plug in the power cable and then recover the firmware using the dos adupate under dos.

  Description: Support SUM to upgrade firmware.
  Infected motherboard: ALL
  Validation :
    1. make sure the SUM version and MUST use the version after "1.2.0 2013/11/14".(this version is not included).
    2. make sure the IPMI firmware version and MUST use 1.24 or later.(include 1.24)
    3. upgrade the firmware using SUM tools via https and http. Please refer to the SUM document to learn the usage.


[Bug fix]
  Description: The security holes about implementing the numerous unsafe string function through web interface
        Please refer to the followinginfromation on CVE web site
    CVE-2013-3623,CVE-2013-3622,CVE-2013-3621,CVE-2013-3623
  Infected motherboard: ALL. 
  Affected functions:
     all web functions. 
  Validation:
     Check if all functinons on web works .

  Description: The fan fail pin will be set output high at BMC Initialization (X10SRE-DS018 HW requirement)
  Infected motherboard: ALL.
  Validation:
     Please test fan failed funciton to see if this function works.
 
  [49236]  System cannot be booted up with IPMI 1.23
  Infected motherboard: X10DRI, X10SRE-DS018
  Validation:
      Power off the motherboard and power on again.

  [49292]  Email alert motherboard name is wrong
  Infected motherboard: X10DRI
  Validation:
      Setup email alert and check the tile

  [49140]  Watchdog Timer test failed
  Infected motherboard: X10QBI
  Validation:
      Boot system to bios setup menu--> Boot Feature--> "Enabled" Watch Dog Function--> 
      Save Changes & boot to OS--> Leaving system IDLE--> Result: Watchdog Timer test failed
 
  [48963]  Lower Critical - Going Low - Asserted during system on/off test on X10SLL-F
  Infected motherboard: X10SLL-F
  Validation:
      System on/off test, 5VCC event log occurs 

  [48477]  Fan PWM measurement fail
  Infected motherboard: X10SLX-F
  Validation:
      measure descending fan curve of CPU, PCH. measure the all curves of RT2 

=====================================================================================

Filename: SMT_X10_123.bin    version: 1.23    Date: 11-15-2013    SVN: 906

U-Boot build time       : Aug 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

Feature:
Solve:

  Heart beat & UID LED funcitons work not properly
  [validation steps] Power on the machine and setup the UI light
  [Root cause] Multifunction does not setup 

=====================================================================================
Filename: SMT_X10_122.bin    version: 1.22    Date: 11-15-2013    SVN: 882

U-Boot build time       : Aug 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

Feature:
Solve:

  ==>  Please clear broswer cache to veriy LDAP problem

  [49070,49068] IPMI-LDAP setting problem  
        [Validation steps] enter  ',', ';' character in in the text filed of Bind DN and Searchbase in LDAP page
        [Root cause] The user cannot input ',', ';' in the text filed of Bind DN and Searchbase due to security issue, 

  there is  flicker screen in the ikvm viewer.
  [validation steps]
    1.  Launch IKVM viewer
    2.  switch to the high resolution under OpenSUSE 12.03 and Ubuntu 13.04
  [Solution]
    Provide the solution to fix VGA BIOS and VGA driver version mismatch.

=====================================================================================
Filename: SMT_X10_121.bin    version: 1.21    Date: 11-08-2013    SVN: 882

U-Boot build time       : Nov 08 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

Feature:
Solve:

  ==>  Please remove current FruData by ipmicfg command (ipmicfg -raw 30 41 and then wait for bmc reboot)

  X10 Up boards, Dp boards
  
  Fru1 data cannot write
  [Validation steps] 
  1.Please remove current FruData by ipmicfg command (ipmicfg -raw 30 41 and then wait for bmc reboot)
  2.ipmicfg -fru1 list. Check if fru1 data exists
  3.jipmicfg -fru1 bp 1. Check if bp is equal to 1

  [48818] Uncorrect information in Power Source monitoring 
        [Validation steps] check dc12output voltage, ac input current, dc 12 output current (ps source webpage)
        [Root cause] Correct the formula toward these values

  X10SLX-F
  [48477] Fan PWM measurement fail 
        [Validation steps] measure descending fan curve
        [Root cause] It doesn't change the fan curve when descending

  [48763] CPU temperature only can up to 85 degree C with E3-1220L v3 CPU hence the fan speed can't run at full speed 
        [Validation steps] Select CPU which HighNR is under 90 degree and try to overheat it.
        [Root cause] Old FW doesn't consider the case when Tjmax is lower then 90 degree

  X10QBI
  [46732] HWM test fail 
        [Validation steps] Check VBAT sensor voltage, should be close to 3.3v 
        [Root cause] The typical voltage of battery component is 3.3v
        [Solution] Modify SDR

  A1SAM-F
  [46732] JL1 chassis intrusion jumper is not working.   
        [Validation steps] put JL1 jumper on, and then pull out. See if chassis intrusion still exists  
        [Root cause] BMC should keep chassis intrusion state until this state resets

=====================================================================================
Filename: SMT_X10_120.bin    version: 1.20    Date: 11-01-2013

U-Boot build time       : Aug 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

Feature:
Solve:
    All X10 mother boards
  [48758] Unable to login to ADMIN account after changing passwords a few times 
        [Validation steps] 
            1. Login to IPMI Web GUI -> Configuration -> Users -> Modify ADMIN
            2. Change ADMIN password to ADMIN123
            3. Check ipmitool remotely with new password
            4. Change ADMIN password to ADMINADMIN
            5. Check ipmitool remotely with new password
            6. Change ADMIN password to ADMIN123
            7. Check ipmitool remotely with new password 
        [Root cause] there are garbage byte left at the end of the new password

  [48612] Power Fail Email Alert Does Not Have Event Description to Mention Power Fail Event
        [Validation steps] Install power supply and pull out the power cord
        [Root cause] Need to parse sel data to show power failure information before email alert is sent

  [48477] Fan PWM measurement fail 
        [Validation steps] measure the heavy io curve on cpu and dimm
        [Root cause] Should follow the spec of X10 SIM_TDG Draft 06282013.pdf to setup heavy io curve on cpu and dimm
        
  X10SLA-F 
  [48762] FAN sensor reading of 20,000 rpm FAN is not correct 
        [Validation steps] install the fan and set full speed mode. Check if rpm is over 20000
        [Root cause] Fan rpm calculation occurs overflow on high speed fan 
         
    X10SLE-DF   
  [48606] iKVM Does Not Identify Node By Name 
        [Validation steps] Enter IPMI web page and see the host names on both node, "SLE_D_NODE_1" and "SLE_D_NODE_2"
        [Root cause] We setup the host name to judge which bmc is used and logged in now
    
=====================================================================================

Filename: SMT_X10_119.bin    version: 1.19    Date: 10-28-2013

U-Boot build time       : Aug 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r21

Feature:
Solve:
    All X10 mother boards

  [48659] Cannot read/write FRU by smcipmitool.exe
        [Validation steps] Read:  smcipmitool.exe <IP Address> ADMIN ADMIN ipmi fru
                       Write: smcipmitool.exe <IP Address> ADMIN ADMIN ipmi fruw <field> <value>
        [Root cause] the command responses the data from the wrong FRU block

  [48423] The memory ECC even log fail
        [Validation steps] Use ipmi command to test Dimm A1 has ecc errors
      ipmitool -I lanplus -H 10.133.176.182 -U ADMIN -P ADMIN raw 0x4 0x2 0x4 0x0c 0xff 0x6f 0x1 0x1A 0x80
        [Root cause] handle unused variable on event log web page 

  X10SLD-EF
  [48322] PUE, Standard, and Heavy IO Fan Modes have the same Fan Speed
        [Validation steps] Set each fan mode and observe the rpms
        [Root cause] Micro cloud series servers are special cases. Heavy I/O mode can be removed.
                 Fan speed table is changed

  [48609] Memory Sensor Does Not Match BIOS Setup Naming
        [Validation steps] Check IPMI sensor name and compare with the other on bios setup 
        [Root cause] Add the mechanism to judege BMC 1 and BMC2 by GPIOH2
 
  [48604] PCH Temperature Sensor Missing
        [Validation steps] Enter sensor page
        [Root cause] Need add PCH sensor for monitoring list 
 
  A1SAI-F, A1SAM-F
  [48322] Fan Mode Setting fail. 
        [Validation steps] Set heavy io mode and heat memory
        [Root cause] dimm sensor is not put in fan control list

  A1SAI-F, A1SAM-F
  [48322] Fan Mode Setting fail. 
        [Validation steps] Set heavy io mode and heat memory
        [Root cause] dimm sensor is not put in fan control list

  X10QBI
  [48300] Abnormal IPMI Fan fail event logs
        [Validation steps] Power on at initialization
        [Root cause] bank 0, reigster should be set 0xF4
                 Add protection to avoid ghost fans noise

  X10SEAA-LN4F,X10SL7-F, X10SLA-F
  [48279] FAN speed won't change when overheat memory with setting Fan to HeavyIO Speed
        [Validation steps] Set heavy io mode and heat memory
        [Root cause] The curve of heavyIO mode is not configured

=====================================================================================

Filename: SMT_X10_118.bin    version: 1.18    Date: 10-09-2013

U-Boot build time       : Aug 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Feature:
  @Support Fru inventory data 1 for PE & bios to write board information area

  @Support port change and enable/disable function on both port setting web page and oem commad
    -0x30   0x70    0x67    Get/Set ports & Services    
    Request
      Data 1: 0/1 [Get/Set]
      Data 2: Port service
        0: HTTP_PORT,1: HTTPS_PORT,2: IKVM_PORT,3:VM_PORT,4:SSH_PORT,5:WSMAN_PORT,6:HTTP_SERVICE,
        7:HTTPS_SERVICE,8:IKVM_SERVICE,9:VM_SERVICE,10:SSH_SERVICE,11:WSMAN_SERVICE,12:SSL_REDIRECT
      Data 3-4 :  [Set]
      Data 4: port number (LSB)
      Data 5: port number (MSB)"    "[Get]
    Response
      [Get]
        Data1: completion code
        Data2: port number (LSB)
        Data3: port number (MSB)
      [Set]
        Data1: completion code"

Solve:
  All X10 boards  

    [48321] YFan speed reading is incorrect with FAN-0141L4
        [Validation steps] install the fan and set full speed mode. Check if rpm is over 20000
        [Root cause] Fan rpm calculation occurs overflow on high speed fan 

    [48281] Your session has timed out. You will need to open a new session" error message popped when click "Post Snooping" in IPMIWeb GUI
        [Validation steps] Enter post snopping page 
        [Root cause] response the wrong data to browser and cause time-out

    [48279] FAN speed won't change when overheat memory with setting Fan to HeavyIO Speed
    [Validation steps] Switch to heavyIO mode and heat memory. Check if fan speed is up
        [Root cause]
      BMC don't include dimm sensor in fan control list

    [48206] SMTP server won't work if "Sender's Address" set @ " " (NULL)
    [Validation steps]
      1. Alert setting
      2. SMTP server setting (w/ sender's address) 
      3. Send Test Alert
      4. Checks email
        [Root cause]
      Some smtp server, it needs complete email name (BMCaabbccddeeff@X10SLM-F.com)

  X10SLX-F
    [48293] No CPU overheat alarm, jumper JOH1 no function
    [48236] CPU temperature reading shows "Not Present" in IPMI Web
      [Validation steps] Heat CPU temperature or enter sensor page
    [Root cause]       BMC don't use peci to read cpu temperature
  
  X10SLH-F  
    [48236] Cannot reset to the factory default (clean LAN)
      [Validation steps] ipmicfg -fde
    [Root cause]       BMC will clear fru inventory area on this oem command
    
  X10SLM-F  
    [48167] Ipmitool to check onboard LAN1 MAC address failed.
      [Validation steps] 1. Use 0x30 0x21 command to get system mac address
                         2. Compare this with another on the IPMI system information web page 
    [Root cause]       BMC don't completely to delete the data about system mac address
 
  X10SLL-F  
    [47470] The MAC address that use IPMITOOL to fetch is not match with MB
      [Validation steps] 1. Use 0x30 0x21 command to get system mac address
                         2. Compare this with another on the IPMI system information web page 
    [Root cause]       BMC don't completely to delete the data about system mac address 
    
  A1SAM-F  
    [48322] Fan Mode Setting fail
  [48239] IPMI sensor reading
      [Validation steps] Enter sensor reading page
    [Root cause]       Previous BMC FW doesn't support this board yet.

=====================================================================================

Filename: SMT_X10_117.bin    version: 1.17    Date: 09-27-2013

U-Boot build time       : Aug 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:

  *All X10 Up boards
    [48112][48111] Error in launching iKVM console
                   Application Error: Unable to launch the appication error when launch Console Redirection Screen (KVM)

        [Validation steps]
        1. launch ikvm from the console redirection page.
        
        [root cause]
        the java viewer can't accept the empty hostname.
        [solution]
        pass the default the hostname to ikvm viewer if it is empty.

=====================================================================================

Filename: SMT_X10_116.bin    version: 1.16    Date: 09-26-2013

U-Boot build time       : Aug 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:

  *All X10 Up boards
    [48089][48088] Email Alert not working with IPMI FW v1.15
        [validation steps]
        1. configure SMTP server and the e-mail address on SMTP and alert pages.
    2. trigger CPU or other sensors overheat.

    [48090] Factory default is not working
    [validation steps]
        1. do factory-to-default on Factory default page.

  *MB -X10QBI-O-P
  [48006] System info LED is not on when fan failed or cpu overheat
  [47511] LED test for FAN Fail test Fail
 
  *MB -X10SLE-DF-O-P
    [47796] Cannot set up IPMI configuration on web 
        [validation steps]
        (1)go to the LDAP page
        (2)click Enable LDAP Authentication, it will pop up message from webpage and logout. 

  *MB -A1SAI-2750F-O-P   
    [47533] VCCP sensor error 
        [validation steps]
        (1)enter sensor reading page

    [47539] System unable to power back on neither by power button nor power control (IPMIWeb)
        [Validation steps]
        (1)make sure the lan cable be plugged to the share lan2.
        (2)do power on/off stress through ipmitool over the share lan 2. 
  
=====================================================================================

Filename: SMT_X10_115.bin    version: 1.15    Date: 08-30-2013

U-Boot build time       : Aug 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
  A1SAi-2750F/2550F
  
  Support 25MHz PWM frequency output
  
  [#47556] Failed to mount virtual drive via "Virtual Media --> CD-ROM Image" in IPMIWeb GUI
  Root cause: Need to add user/password account judgement
  Solution  : FW Update
  
  [#47535] Failed to update BIOS via IPMIWeb GUI 
  Root cause: This platform doesn't support ME.
  Solution  : Ignore ME region

  [#46347] Overheat LED at "JOH1" was lit and blinking if any of FAN-Failure asserted. 
  Root cause: GPOY3 OVERHEAT LED" and "GPOA3 PSU/FAN failure", they PWM together when FAN fails 
  Solution  : Setup GPIOY3 to lit JOH1 only

  X10SLE-DF
  [#47405] For cpu2 HWM measurement fail at Vbat
  Root cause: incorrect SDR
  [#47447] Please Remove Dedicated LAN Link Option
  Root cause: NIC speed is always 1G speed. Don't need to adjustify

  All X10 motherboards
  [#47470] The MAC address that use IPMITOOL to fetch is not match with MB. 
  Root cause: IPMI still record old share lan adderess after updating the nic eeprom
  Solution  : Synchronize the new share lan address
  Validation step:
              1. flsah eeprom with SLM13.zip
              2. use IPMITOOL and command 
                 IPMITOOL.exe -I lan -H 10.135.15.95 -U ADMIN -P ADMIN raw 0x30 0x21
              3. The result is not match with the MAC address of MB.    
=====================================================================================

Filename: SMT_X10_114.bin    version: 1.14    Date: 08-16-2013    SVN: 620

U-Boot build time       : Jun 14 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
  X10DRI-T
  [#47389] Missing FanA and FanB on the Sensor Reading Page
  Root cause: sensor number of FANA & FANB is not correct in FW
  Solution  : Modify them in FW
  Validation step: 
   See it in sensor reading page

  X10SLE-DF
  [#47397] Dedicated LAN Speed Always Shows 10M
  [#47196] Dedicated LAN Link Status Shows 10M
  Root cause: driver reading is not correct 
  Solution  : Modify in NIC driver
  Validation step: 
   See it in network page

  [#47334] HWM measurement fail at Vdimm
  Root cause: sensor reading is not accruate 
  Solution  : Adjust SDR value
  Validation step: 
    See in sensor page

 [#47193] After Update to IPMI FW 1.13, CPU Throttling to 800 MHz Observed
  Root cause: GPIOA4 pulls low 
  Solution  : Pull GPIOA4 high at BMC initialzation
  Validation step: 
    heat cpu over 80 degree by PwrThermalUtil tool 

  All X10 motherboards
  [#47198] Lan Interface Should be LAN Interface
  Root cause: Change "Lan"to all capital letters "LAN"
  Solution  : Correct wordings in FW
  Validation step:
    See "LAN interface" in network page

  X10SLL+-F
  [#47309] Email Alert for X10SLL+-F Shows X10SLA_F in Subject Header
  Root cause: Typo error
  Solution  : Correct wordings in FW
  Validation step:
    Setup email alert function
    
=====================================================================================
Filename: SMT_X10_113.bin    version: 1.13    Date: 07-29-2013    SVN: 553

U-Boot build time       : Jun 14 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r20

****** The user is not allowed to downgrade the fw from this release due to the security issue****** 

Improvement:
  1.Renew default SSL certificate from 7/17/2013 to 7/17/2014
  2.fix the security issue for the user password
    Encrypt the user password inside IPMI fw.
    Validation step:
    1. add/delete/modify the username/password through web or ipmitool.
    2. save/restore the ipmi configuration.

  [X10SLE-DF] 
    3.Add X10 SLE-DF sensor reading support
    4.Add RTL8363SB for dedicate lan 1G Support
    
    
    
Solve:
  X10SEAA-LN4F
  [#46904] FAN1 and FAN3 are not working properly. 
  Validation step:Try full speed
 
  All X10Up board
  [#46720,46709] Memory ECC Error Email Alert Shows Wrong DIMM Slot  
  Validation steps:
    1.Register the smtp setting
    2.Use ipmi command to test Dimm A1 has ecc errors
      ipmitool -I lanplus -H 10.133.176.182 -U ADMIN -P ADMIN raw 0x4 0x2 0x4 0x0c 0xff 0x6f 0x1 0x1A 0x80
    3.Receive the email and check if the dimm slot number is the same as the other in IPMI event log
 
  [#46595] In iKVM, IPMI firmware not supports others keyboard layout style except of "English" type  
  IKVM VERSION : 1.69.20
  Validation steps:
    1.Launched iKVM,go to input tab in preference tab.
    2.change the keyboard layout.
    3.none of keyboard layout are working expect for English one. 

  [#46592] Sender's address of SMTP setting not works properly.  
  Validation steps:
    1.Remote login into SUT IPMIWeb GUI via IPMI IP
    2.Setup an alert entry in "Alerts --> configuration" field
    3.Setup SMTP server with sender's address in "SMTP" --> configuration" field 
    4.Send a test alert and then check email     

  [#46409] Auto-resize windows??tab of iKVM is not working 
  Validation steps:
    1.Remote login-into SUT via IPMI LAN.      
    2.Launched iKVM, un-check the "auto-resize windows" tab under Option -> Preference -> Windows 
    3.Use mouse adjust iKVM windows size a failed, unable to adjust

  X10SLH-F,X10SLL+-F,X10SLM+-F,X10SLM+-LN4F
  [#46708] DIMM Temperature Sensor Naming Does Not Match Silkscreen 
  Validation steps:
    1.Burn the FW and don't preserve the configuration
    2.Enter IPMI sensor reading page

  X10SLM+-F,X10SLH-F
  [#46714] Email Alert Shows X10SLH_F  
  Validation steps:
    Register the smtp setting and send the email

=====================================================================================
Filename: SMT_X10_112.bin    version: 1.12    Date: 07-05-2013    SVN: 499

U-Boot build time       : Jun 14 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
  X10SLM-F, X10SLL-F
  [#46480] IPMI Logs Non-Critical Events.(CPU Temp)
  Validation step:
    heat the CPU temperature

  [#46141] Low Critical- Going Low during IPMI ON/OFF share LAN stress
  Validation step:
    System on-off test
    
  X10SEAA_LN4F 
  [#46374] No beep when no memory connect to the system.
  Validation step:
    don't plug in the memory and power on the machine

  [#46233] CPU Temp" and "Chassis Intrusion" shows "Not Present
  Validation step:
    Enter IPMI sensor page
=====================================================================================

Filename: SMT_X10_111.bin    version: 1.11    Date: 06-26-2013    SVN: 474

U-Boot build time       : Jun 14 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
 
  [#46381] Chassis Intrusion Not Logged in Event log,SNMP trap and E-mail alert 
  [#46373] Chassis Intrusion Not Logged in Even Log
  [#46349] While chassis intrusion asserted, no chassis intrusion event log was showed. No SNMP trap and Email alert as well

=====================================================================================

Filename: SMT_X10_110.bin    version: 1.10    Date: 06-21-2013    SVN: 462

U-Boot build time       : Jun 14 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:

X10SLM+_LN4F  
  2.[#46276] IPMI Web Orderly Shutdown Power Control Does Not Work

X10SEAA_LN4F
  3.[#46242] There is an extra "Optimal" Fan-mode was present in IMPIWeb GUI
  4.[#46237] Power supply information are not LINE-UP in IPMIWeb GUI
  5.[#46224] It will generate " Voltage VDIMM " after run E-burn SAT Test

=====================================================================================
     
Filename: SMT_X10_109.bin    version: 1.09    Date: 06-14-2013    SVN: 451

U-Boot build time       : Jun 14 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
  1.Add sensor support on X10SEAA_LN4F
  2.update sensor list according to IPMI_voltage_sensors_threhold_R01.xlsx
  2.#46139          LAN 1 disconnect after IPMI factory default setting
  2.#46132                  -12V Events Lgged During IPMI KVM Stress
  3.#45908,#45905       IPMI Logs Non-Critical Events
  4.#45778                  Remote Console Preview display is abnormal
  5.#46059                  Random - Update BIOS setting via OOB with option "--reboot" fail.
  6.#46056                  Random - The process is loop when update BIOS via OOB.  
     
=====================================================================================

Filename: SMT_X10_108.bin    version: 1.08    Date: 06-06-2013    SVN: 432

U-Boot build time       : May 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
  1.fine tune sensor values on X10DRI_T, X10QBI_F
  2.#46010                                          Please Change FAN1 Sensor to FAN
  3.#45939                                          Power Fail Logs About Every 5 Minutes
  4.#45938                                          HeavyIO FSC: FANA RPM Higher at 39C and lower at 42C 
  5.#45937                                          HeavyIO FSC Mode FanA Speed Higher Than Thermal Guideline Specification 
  6.#45928,#45926,#45908,#45905 IPMI Logs Non-Critical Events 
  7.#44075                                          dmesg has a "ipmi_si: Error clearing flags: cc" error message after running E-burn stress
        
=====================================================================================
Filename: SMT_X10_107.bin    version: 1.07    Date: 05-30-2013    SVN: 417

U-Boot build time       : May 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
    
    Fine tune VBAT, -12V sensor threshold on X10SLM-F, X10SLL-F and X10XLM+_LN4F
        
=====================================================================================

Filename: SMT_X10_106.bin    version: 1.06    Date: 05-27-2013    SVN: 410

U-Boot build time       : May 27 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r19

Solve:
    
    Please clear Java cache (iKVM verion is updated)
  Please uncheck the preserved box in firmware upload page
  
  1.Add sensor on X10SLL+_F, X10QBI_T
  2.#45801,#45725,#45725,#45481     [OOB] System Will Shutdown After Flash BIOS Via OOB and Reset .
  3.#45712                                              There are many Vcore events in IPMI SEL when running eburn LIN test
  4.#45621,#45785                                   IPMI Virtual Keyboard didn't have Swiss language item
  5.#45682                                              FAN speed will up to 100% when IPMI initializing
        
=====================================================================================
Filename: SMT_X10_105.bin    version: 1.05    Date: 05-20-2013    SVN: 398

U-Boot build time       : May 20 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r18

Solve:
  
   1. [X10SLM-F/X10SLL-F] Output 50@ dutycycle when bmc reboots 
   2. [X10SLM-F/X10SLL-F] Change sensor name to "3.3V AUX"
   3. [X10SLL-SF]         BMC can't boot successfully
   4. #45619              It not work if run "ChnageBIOScfg" and "Loaddefault" of OOB functions
   5. [X10DRI_F]          Add sensor supports
   6. Preserve the whole 64k block where SMIBIOS data resides.
      [Validation Steps]
      a. Go to the bios update page 
      b. Update bios image only with preserving SMBIOS.
      
=====================================================================================

Filename: SMT_X10_104.bin    version: 1.04    Date: 05-10-2013    SVN: 388

U-Boot build time       : May 9 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r18

Solve:

  1. Output 100@ dutycycle for X10SLM-F/X10SLL-F. 
  2. Update the thermal curve for heavy IO fan mode.
  
  [45018] Sometimes Auto-Resize Window Does Not Work When Booting into OS 
  [45209] IPMI KVM window doesn't have Power Control option 
          Support high resolution up to 1920*1200.
  [45463,45401,45381,45347] BMC incorrect reponse detected during eburn test  
  
=====================================================================================
Filename: SMT_X10_103.bin    version: 1.03    Date: 05-03-2013    SVN: 376

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:

    Add OOB event log.
    OOB file build date mis-match (Sensor type : 0xCA, Event Data 1)
      OOB feature initial failure (Sensor type : 0xCA, Event Data 2)  
  
    [X10SL7-F]
  45347 BMC incorrect reponse detected during eburn test  
   
    [X10SLE-F/X10SLD-F]
  45381 BMC incorrect reponse detected during eburn test  
  
  
======================================================================================
Filename: SMT_X10_102.bin    version: 1.02    Date: 04-26-2013    SVN: 367

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:

  [X10SLM-F/X10SLL-F]
        45067 part of the Eburn stress test is fail (ipmi_si: Error clearing flags: cc) 
   
    [X10SLM+-LN4F/X10SLH-F/X10SL7-F/X10SLA-F]
        45231   Please Change Bios String in IPMI Web System Information Page to BIOS

    [X10SLE-F/X10SLD-F]
    45096 SSM Power Supply status is abnormal
  
======================================================================================
Filename: SMT_X10_101.bin    version: 1.01    Date: 04-19-2013    SVN: 352

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
  Support Heavy IO fan control mode
  Solve IPMI login web page is gone on ie8 & ie9

  [X10SLM-F/X10SLL-F]
        45044 IPMI SOL can't working.
    45040 X10SLM-F->please add heavy I/O mode at FAN speed control mode
    44962 IPMI Web GUI is gone with IE broswer
    Set smi pin as input low to aviod bios hang at 9A when system is powered on
   
    [X10SLM+-LN4F/X10SLH-F/X10SL7-F/X10SLA-F]
        45022   IPMI Web Not Working Correctly With Microsoft Internet Explorer
        44869   Email Alert Shows X10_XLH for X10SLH-F

    [X10SLE-F/X10SLD-F/X10SL7-F]
    Set up GPIOR3 for PHY Reset pin on rev 1.01 

    [X10SLE-F/X10SLE-F]
    Optimize the power consumption for these 2 motherboards
    When the system is off, lower the speed of dedicated LAN to 10M.
    When the system power up, the speed will come back to the original speed.

======================================================================================
Filename: SMT_X10_100.bin    version: 1.00    Date: 04-11-2013    SVN: 336

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

 For beta release
 
======================================================================================
Filename: SMT_X10_032.bin    version: 0.32    Date: 04-10-2013    SVN: 335

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
  Support power source page and power monitor page on IPMI web-gui
  Support set system mac address command (need bios support and clear browser cache after updating )

  [X10SLM-F]
    Use ME to read CPU temp instead of peci (Please re-work HW)

  [X10SLM-F/X10SLL-F]
        44361 Chassis intrusion doesn't work
 
    [X10SLM+-LN4F/X10SLH-F/X10SL7-F/X10SLA-F]
        44869   Email Alert Shows X10_XLH for X10SLH-F MB
        44854   All Fans Do Not Stay at Full Speed During Fan Failure
        44833   CPU Overheat Deassertion Thresholds Do Not Follow Thermal Guideline
 
======================================================================================
Filename: SMT_X10_031.bin    version: 0.31    Date: 04-03-2013    SVN: 329

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
  
  Please use factory reset after downloading new firmware

    [X10SLM-F]
        44312   IPMI IKVM Reset function is not working
        
    [X10SLM+-LN4F/X10SLH-F/X10SL7-F/X10SLA-F]
        Add VRM sensor
        44747   Shared LAN Not Working
        44426   [NM] Cannot Read Entire Platform Statistics
                 
======================================================================================
Filename: SMT_X10_030.bin    version: 0.30    Date: 03-29-2013    SVN: 320

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:

    [X10SLM-F/X10SLL-F]
        44672   BIOS IPMI Network Link Status is "No Connect" when IPMI connected
        44322   IP Access Control function is not working
        42897   IPMI Mouse default setting is incorrect

    [X10SL7-F]
        44145   Cannot get any ME information via SMCIPMITool
                
    [X10SLM-LN4F/X10SLH-F]
        44479   IPMI Network Link Status Shows "No Connect"
        44402   Cannot Flash BIOS via OOB

    [X10SLA-F]
        44369 CPU Temp. and Memory Temp. status is "N/A      
         
======================================================================================
Filename: SMT_X10_029.bin    version: 0.29    Date: 03-25-2013    SVN: 313

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13


Solve:
    Please use progrmmer to flash the firmware

    [X10SLM-F]
        Add board support
======================================================================================

Filename: SMT_X10_028.bin    version: 0.28    Date: 03-21-2013    SVN: 309

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13


Solve:
    1. Fix the issue smcipmitool can't upgrade the firmware.(smcipmitool verion MUST be 2.4.11 and later)
    Usage:
        smcipmitool  <BMC ip>  ADMIN ADMIN ipmi flasha <filename>
    2. Fix the issue SMCIBU will show  the error message "product key not active" when flash BIOS on X10SSL-F.
    
    [X10SLE-F] 
    [X10SLM-F]
        44312    IPMI IKVM Reset function is not working
        41936  Fan Pulse-Width-Modulation Measurement fail

    [X10SLL-F]
        44382       How do I change the serial output from SOL to COM2 (header) 
        44136       No PCH temperature in IPMI sensor readings

======================================================================================

Filename: SMT_X10_027.bin    version: 0.27    Date: 03-15-2013    SVN: 298

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

**** After updating this firmware, please do factory reset in the maintainance page **** 

Solve:

  Fix the issue upgrading FW without preserving 

  [validation step]

  1.First burning the 00.27 firmware and then do factory reset in maintainance page
  2.Upload the 00.26 firmware and uncheck the preserved box in firmware upload page
  3.After burning process is finished, you can see the sensor positions are changed in sensor page 
    (In 0026, we swap the sensor orders )
  4.If you upgrade from 00.26 to 00.27 by above procedure. Then you will not see the sensors are swapped
  

    [X10SLE-F]
        44446    "-12V" should be removed from IPMI sensor reading
        44384    PCH Temperature Missing
        44383    CPU Temperature Missing

    [X10SLM-LN4F/X10SLH-F]
        44421    CPU and PCH Temperature Missing With IPMI FW v0.26
        44140    CPU Overheat LED

    [X10SLM-F]
        44392    Missing/bogus sensors from ipmitool
        44391    Missing VCORE and VDIMM in IPMI sensor 
        44344    IPMI Watchdog NMI function is not working
        44322    IP Access Control function is not working
        44279    IPMI sometimes will generate Chassis Intrusion and -12V event in Event log

    [X10SLL-F]
        44381    Intrusion reset from IPMI will generate weird SEL
        44358    IPMITOOL sdr command has some extra sensor readings compared to web-gui
        44325    SEL has some voltage logs after running BMC reset test
        44136    No PCH temperature in IPMI sensor readings

    [X10SLA-F]
        44369     CPU Temp. and Memory Temp. status is "N/A" in IPMI Monitor sensor  
        44152     The FAN pluse test fail 

    [X10SL7-F]
        44353     [RE-OPEN] - Sensor readings incorrect after system wakes up from S3 

======================================================================================

Filename: SMT_X10_026.bin    version: 0.26    Date: 03-08-2013    SVN: 284

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:

   X10SLE-F
    [44098] Virtual Media: CD-ROM Image ISO Mount Shows Mounted as USB Floppy&Flash 
   
   X10SLL-F
        [44210]  There won't be any sensor readings sometimes - via web or KCS interface
         

New feature:
   Flash dos tool (Must use this version and above.) 


======================================================================================

Filename: SMT_X10_025.bin    version: 0.25    Date: 03-04-2013    SVN: 274

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
  X10SLA-F
    [44152]     The FAN pluse test fail
    [44035]     Memory events log test fail

  X10SLH-F/ X10SLM-LN4F
    [44140]     CPU Overheat LED
    [42624]     DIMM Temperature Sensor Showing N/A 

  X10SLE-F
    [44097]     System Takes Long Time to Boot
    [44094]     No DIMM Temperature Seen on IPMI Web Sensor Readings
  
  X10SLD-F
    [44066]     no hardware monitor in ipmi

  X10SL7-F
    [44056]     IPMI initializes every time I reboot or turn on the system
======================================================================================
Filename: SMT_X10_024.bin    version: 0.24    Date: 02-23-2013    SVN: 252

U-Boot build time       : Feb 22 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
  X10SLH-F/X10XLM-LN4F 
  [43961] Remote Console Preview Takes Longer to Refresh than Previous X9 Generation 

  X10SLL-F/X10XLM-F 
  [43893] Chassis Intrusion always is fail and didn't reset
  [43891] IPMI Event Log has some undefined message when system boot-up or OS reboot
  [43154] Watchdog function is not working 

  X10SL7-F
  [43878] After system wakes up from S3 and boots into OS there are not IPMI sensor readings
  [43329] IPMI LED is not blinking anymore after consective cold reset   

  X10SLE-F
  [43869] Unable to establish LAN session" after running IPMI Cold Reset for 2529 times through onboard LAN1 

  X10SLD-F 
    Add board support
======================================================================================
Filename: SMT_X10_023.bin    version: 0.23    Date: 02-01-2013    SVN: 234

U-Boot build time       : Jan 31 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

  Please clean web page before login the IPMI web page
Solve:
  [X10SLH-F/X10SLE-F] Failed to set static IPMI LAN IP address in BIOS 
  [X10SL7-F] Web-session times out after 15 mins
               Add the web session page and web session timeout value on web page (1-30 minutes)
             Sensor readings appear on IPMI web-gui before all the option ROM have been initialized

  Sometimes After Shutdown From OS and then Power On, Random Sensors Will Disappear

  IPMI restart occasionally after push reset button

  Add AC Power On Event Log on web page
        Ipmi command, 0x30 0x70 0x64
        Data1  Get/Set ->[0/1] 
        Data2  set ac power on event flag  -> [0/1] //disable / enable

======================================================================================
Filename: SMT_X10_022.bin    version: 0.22    Date: 02-01-2013    SVN: 218

U-Boot build time       : Jan 31 2013
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
   [X10SL7-F/X10SLM-LN4F]IPMI KVM: No IKVM signal when resolution is set to 1024x768x8 mode
   [X10SL7-F] PCH temperature is shown as 4 degrees (Intel bug, work around solution)
   [X10SLL-F] Workaround solution to fix the power button can't work properly.
   [X10SLE-F] Support HDD sensor

    Solve the language hang problem in ikvm viewer
    Solve the SDR could not be updated [Denis]

======================================================================================
Filename: SMT_X10_021.bin    version: 0.21    Date: 01-30-2013

U-Boot build time       : 12-19 2012
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
[X10SLL-F/X10SLL-F] For CM release
                    set GPIOE5 as input pin after setting to output pin state to avoid power button fail solution

======================================================================================
Filename: SMT_X10_020.bin    version: 0.20    Date: 01-29-2013    SVN: 203

U-Boot build time       : 12-19 2012
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Solve:
[X10SLL-F/X10SLL-F] For CM release
                       set GPIOE5 output high at boot code stage to avoid i210 crash down
                       set GPIOC1 input, GPIOE2 output 
                       set GPIOE3 output
 
======================================================================================

Filename: SMT_X10_019.bin    version: 0.19    Date: 01-25-2013    SVN: 201

U-Boot build time       : 12-19 2012
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r13

Please use programmer to burn this firmware
Please clear Java cache (SOL verion is updated)
Solve:
  [X10SLM-LN4F] Unreliable IPMI connection on shared LAN
  [X10SL7-F]    SOL Can Open Multiple Windows
  [X10SLE-F]    Add sensor list (HDD sensor is not ready)
 
======================================================================================
Filename: SMT_X10_018.bin    version: 0.18    Date: 01-18-2013    SVN: 187

U-Boot build time       : 12-19 2012
Java SOL Viewer version : v0.5.8
Java iKVM Viwer version : v1.69 r13

Please uncheck the Preserve Configuration box to restore the factory default setting of BMC
 
Solve:

   [X10XL7-F]    Fix vcore senor value is not right
                 Systerm Temperature (RT1) Event Cannot Be Logged
                 No IPMI Log for PCH Overheat  Hardware; IPMI

   [X10SLM-LN4F] KVM window closes itself

   [X10SLL-F]    The FAN speed control curves for CPU can't follow thermal design guide

   [X10SLE-F]    Add board support
 
======================================================================================

Filename: SMT_X10_017.bin    version: 0.17    Date: 01-11-2013    SVN: 175

Solve
    Preview function is working (  Remember it takes about 6 seconds to refresh the 
                                   screenshot in X10, and 1280 x 1024 resolution maximum )
  Device 3 function works at virtual storge
  Solve when switching to share LAN, can't get IP and network message is not correct on
    network page
  Solve peripheral Temperature overheat asserted event is not log in SEL.
  Solve BMC will has kernel panic after several times change on Lan Interface setting in Network configuration.

  [X10SLM_LN4F/X10SLH-F/X10SL7-F] Correct vcore voltage on web page 
                                  No overheat beep alarm (controlled by NCT6776)
                                  Correct system temp disappeared in sensor reading page
                                  Correct sensors will disappear in sensor reading page
                                  
  [X10SLL-F/X10SLM-F]                       Add watchdog function
                                                                Add Beep function (controlled by AST2400 PWM)
 
======================================================================================
Filename: SMT_X10_016.bin    version: 0.16    Date: 01-07-2013    SVN: 152

Solve
  [X10SL7-F/X10SLA-F]                       Add board support
  [X10SLM_LN4F/X10SLH-F/X10SL7-F] Correct vcore voltage on web page 
  [X10SLL-F/X10SLM-F]                       Correct -12v sensor voltage on web page
                                                                Add watchdog function
 
  Known issues
  1. Preview has some problems
======================================================================================

Filename: SMT_X10_015.bin    version: 0.15    Date: 12-28-2012    SVN: 134

Solve
  Fan control function is ok
  [X10SLH-F/SLM_LN4F] Chassis Intrusion Shows Wrong Time Stamp in Event Log
  [X10SLH-F/SLM_LN4F] Fine tune the parameters of superio NCT6776 based on sensor list
  [X10SLL-F/X10SLM-F] -12v sensor reading fails
 
Known issues
1. Preview has some problems

======================================================================================

Filename: SMT_X10_014.bin    version: 0.14    Date: 12-21-2012    SVN: 116

Solve
    Virtual media funciton is working
  Preview function is working
  It show wrong share/dedicate information on network config web page
  Add GUID for ATENX10 BMC is C 0 0 1 M S
  Set default Mac address of Bootloader is 00:00:00:00:00:00
  
    [X10SLL-F/X10SLM-F]         Voltage sensor has been fined tune
                                                  Power fail led and led works correctly
                                                  
    [X10SLH-F/X10SLM-LN4F]  Fan Fail Event Log for FAN1 and FAN2 Missing Lower Non-Critical Status
                                                    Factory Default Will Cause BMC to Lose MAC Address 
    
    [X10SL7]                                support   

Known issues
1. Fan fail and pwm has some problems. 
2. [X10SLL-F/X10SLM-F] Front & Rear temperature sensors, smbus may be failed after long time testing

======================================================================================

Filename: SMT_X10_013.bin    version: 0.13    Date: 12-13-2012    SVN: 95

Solve
  Important !! <=Please use programmer to burn this firmware if previous firmware is older then fw.012 verion

1. Add board id BOARD_X10_SLM_LN4 0x806

2.[X10SLM-LN4] 1.Change Vcore threshold, M,B,K2,K1.
               2.Change ?œCPU VTT??to ??12V??and Adjust this threshold, M, B, K2, K1
3. [X10SLM]    1.Add all sensors [except chassis intrusion]

Known issues
1. It can only mount virtual media at the 1st time, and umount/remount funciton failed
2. Preview is not working


======================================================================================

Filename: SMT_X10_012.bin    version: 0.12    Date: 12-07-2012    SVN: 73


Solve
1. Enable COM1 & COM2 at bootloader 
   Important !! <=Please use programmer to burn this firmware
2. Network function works
3. [X10SLL-F/X10SLM-F] sensors wroks (except CPU peci temp, overheat function)
4. UID funciton works
5. SOL function works
6  Post snoppy function works on IPMI web page
7. [X10SLH-F/X10SLM-LN4F] sensors wroks [except CPU peci temp, overheat function]

Known issues
1. Virtual media is not working
2. Remote control is not working
3. [X10SLL-F/X10SLM-F] fan speed is full speed now

======================================================================================

Filename: SMT_X10_011.bin    version: 0.11    Date: 11-30-2012    SVN: 49

This bin code is for all X10 boards.

Solve
1. Remote function ok
2. KCS works. bios please use KCS4 & KCS5; ipmicfg and other utilities will use KCS2 & KCS3
3. Add board id
 

Known issues
1.  Network driver has bugs. The failover mode fails, and dynamic plugging in/pulling out the network may fail. 
    After setting the bmc address, you may have to ac power off and power on again, and the network works.
2.  Sensors are working except memory temperature detection.
3.  SOL is not working
7.  Virtual media is not working
8.  Sensor without SIO (only completed 6776 SIO sensor)

======================================================================================

Filename: SMT_X10_010.bin    version: 0.10    Date: 11-26-2012    SVN: 33

This bin code is for all X10 boards.

Known issues
1.  Network driver has bugs. The failover mode fails, and dynamic plugging in/pulling out the network may fail. 
    After setting the bmc address, you may have to ac power off and power on again, and the network works.
2.  Sensors are working except memory temperature detection.
3.  In SOL, only one way is passed
4.  remote control is not working
5.  In KCS, only CA2 & CA3 works. Currently, bios & bmc cannot talk to each other.
6.  Ipmicfg works.
7.  Virtual media is not working
8.  Sensor without SIO (only completed 6776 SIO sensor)


======================================================================================
