B10DRi/C-N release note.
=============================================================================================================
CPU Microcode                             | Option ROM/EFI driver               | Intel RC/TXT/ME
-------------------------------------------------------------------------------------------------------------
CPUID FAMILY                              | Aspeed VBIOS           : 0.98.03    | RC Package : 3.0.0
306F2 Haswell-EP C-0, C-1, M-1       :036 | Intel SATA RAID Legacy : 4.3.0.1018 | SPS : 3.1.3.21
306F1 Haswell-EP B-0                 :014 | Intel sSATA RAID Legacy: 4.3.0.1018 | BIOS ACM   : 20151110(3.0.2)
406F0 Broadwell-EP L0,A0,A1          :014 | Intel Giga PXE         : 1.3.95     | SINIT ACM  : 20150805(3.0.1)
406F1 Broadwell-EP B0,M0,R0     :0B000010 | Intel 10G PXE          : 2.3.04     |
                                          | Intel iSCSI            : 2.8.16     |
                                          | Intel Giga UEFI driver : 6.9.07     |
                                          | Intel 10G UEFI driver  : 5.1.11     |
                                          | Intel SATA RAID UEFI   : 4.3.0.1018 |
                                          | Intel sSATA RAID UEFI  : 4.3.0.1018 |
=============================================================================================================
BIOS feature             |  Support
--------------------------------------------------------------------------------
OOB Flash BIOS           |     Y
OOB Update Setting       |     Y
OOB Change SMBIOS        |     Y
InBand Flash BIOS        |     Y
InBand Update Setting    |     Y
InBand Change SMBIOS     |     Y
InBand SMI E7h supported |     Y
=============================================================================================================

BIOS Changes:

b10dri6.120: 
1.Category: Fix
Description:
Change LANCOUNT from 2 to 1 in CMM EEPROM. 
Infected Motherboard: ALL
Affected functions: MAC display in CMM
Validation : Check NIC MAC address in CMM

2. Category: Fix
Description: Keep booting when there is memory error in MRC.
Infected Motherboard: ALL
Affected functions: 
Validation :


B10DRI5.c22:
1.Category: Implement
Description:
Update Intel RC code to 3.0
Infected Motherboard: ALL
Affected functions: Memory and PCIE
Validation: Memory and PCIE reliability

2.Category: Implement
Description:
Add setup options to support IPMI VLAN settings.
Infected Motherboard: ALL
Affected functions: BMC VLAN settings
Validation : Change BMC VLAN settting in BIOs setup.

3.Category: Implement
Description:
Change revision to 2.0.
Infected Motherboard: ALL
Affected functions: None
Validation : Check BIOS version in BIOS setup.

4.Category: Implement
Description:
Disble DDR Phase Shedding by default.
Infected Motherboard: ALL
Affected functions: Memory
Validation : No need to test

5.Category: Implement
Description:
Remove CpuMpPei function.
Infected Motherboard: ALL
Affected functions: None
Validation : Fix Cburn on/off testing hang at POST code 33

6.Category: Implement
Description:
Change QPI CTLE setting to original values
Infected Motherboard: ALL
Affected functions: QPI
Validation : No need to test

7.Category: Implement
Description:
Program CMM EEPROM max power dynamically.
Infected Motherboard: ALL
Affected functions: CMM power control
Validation : check CMM system power consumption with different SKU of processors 

8.Category: Implement
Description:
Remove duplicated LAN1 OPROM setup option.
Infected Motherboard: ALL
Affected functions: Setup looking feel
Validation : There should be one LAN 1 OPROM option in Advance->PCIe/PCI/PnP Configruation

9.Category: Implement
Description:
Remove ME predictive power cap feature
Infected Motherboard: ALL
Affected functions: NM power capping
Validation : No need to test

10.Category: Implement
Description:
Update BDX CPU Microcode to 10/11
Infected Motherboard: ALL
Affected functions: CPU Microcode
Validation : Check BDX CPU Microcode in BIOS setup CPU configuration 

11.Category: Implement
Description:
Program CPUID bit 4-19 to CMM EEPROM.
Infected Motherboard: All
Affected functions: CMM CPU display
Validation : Check CPU name in CMM

12.Category: Fix
Description:
Correct memory info in SMBIOS Type 17.
Infected Motherboard: ALL
Affected functions: DMI 
Validation : No need to test


13.Category: Fix
Description:
Fix system hang AF after running SUM LoadDefaultBiosCfg command
Infected Motherboard: ALL
Affected functions: BIOS booting
Validation : Run SUM LoadDefaultBiosCfg command and reboot system
