Firmware Version: 2.48
Firmware Name: SMT_X10IPMI_248.bin
Firmware CRC: 99c6020f
Release date: 06/04/2016
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X10DSC+, X10DRL_LN4

1.
    Category: Fix
    Description:
		PB #70923, no CPU thermal trip message 

    Infected Motherboard:  X10DRL_LN4
    Affected functions:
    Validation :
	 1). Remove heat sink, make CPU hot crash trigger event log

2.
    Category: Fix
    Description:
		PB #70927, PCIE SERR/PERR Alert mail "Sensor ID" is empty

    Infected Motherboard: ALL
    Affected functions:
    Validation :
	 1). Set SMTP server config
	 2). Set alert evert config
         3). Trigger PCIE SERR/PERR event alert and check mail content

3.
    Category: Fix
    Description:
		PB #71428, "No AOC card sensor reading in IPMI Web"

    Infected Motherboard: ALL
    Affected functions:
    Validation :
	 1). Install AOC card
	 2). Check AOC sensor reading

4.
    Category: Enhancement
    Description:
		New solution to detect VBAT value. Extend battery life cycle.

    Infected Motherboard: ALL
    Affected functions:
    Validation :
	 1). Check VBAT sensor value

5.
    Category: Fix
    Description:
		Session timeout webpage logged out by enter key

    Infected Motherboard: ALL
    Affected functions:
    Validation :
	 1). Access Web Session webpage
         2). Foucus on session timeout value and key in "ENTER"
         3). BMC can't be logged out

6.
    Category: Enhancement
    Description:
		Change Copyright from 2014 to 2016

    Infected Motherboard: ALL
    Affected functions:
    Validation :
	 1). Check main page website

--------------------------------------------------------------------------------------

Firmware Version: 2.45
Firmware Name: SMT_X10IPMI_245.bin
Firmware CRC: 5FE4682D
Release date: 04/29/2016
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X10DSC+, X10DRL_LN4

1.
    Category: Fix
    Description:
		PB #70537, CPU temperature reading is incorrect"
		PB #70538, FANs do not spin at full speed

    Infected Motherboard:  ALL
    Affected functions:
    Validation :
	 1). Run BIOS update from BMC web
	 2). After updated BIOS then resetting host
	 3). Check all sensor temperature values
	 4). Change FAN mode to full speed then checking FAN RPM

2.
    Category: Fix
    Description:
		PB #70213, "No IB temperature reading for AOC-MHIBF-1QG/2QG in X10DSC+ IPMI web GUI"

    Infected Motherboard: X10DSC+
    Affected functions:
    Validation :
	 1). Install AOC-MHIBF-1QG/2QG
	 2). Reset host
	 3). Check BMC sensor reading and it need to show IB temp.
	 
3.
    Category: Enhancement
    Description:
		Support SDR preserve setting during BMC WEB FW updated

    Infected Motherboard: ALL
    Affected functions:
    Validation :
	 1). Change SDR preserve setting
	 2). Do BMC WEB FW update then checked SDR

--------------------------------------------------------------------------------------

Firmware Version: 2.43
Firmware Name: SMT_X10IPMI_243.bin
Firmware CRC: 21C395B2
Release date: 04/08/2016
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X10DSC+, X10DRL_LN4

***************  Need Factory default after updated this FW ******************

1.
    Category: New
    Description:
		Support X10DRL_LN4

    Infected Motherboard: X10DRL_LN4
    Affected functions:
    Validation :
     1). Check BMC functions

2.
    Category: New
    Description:
		BPN temperature sensor for backplane BPN-SAS3-826SEL1-N4 and BPN-SAS3-226SEL1-N4
		BPN temperature sensor and expander temperature sensor for backplane BPN-SAS3-946SEL2
		
    Infected Motherboard: X10DSC+
    Affected functions:
    Validation :
     1). Check BPN temperature sensor and expander temperature on different backplane boards.
	 
3.
    Category: Fix
    Description:
		Fix PB #69907, PCH temp goes below threshold 

    Infected Motherboard: X10DSC+
    Affected functions:
    Validation :
     1). Run DC on/off testing
	 2). Check PCH event log

4.
    Category: Fix
    Description:
		Fix PB #69305, Storage monitoring tab shows inccorect logical drive data 

    Infected Motherboard: X10DSC+
    Affected functions:
    Validation :
	 1). Check storage monitoring information in Storage monitoring tab
     2). Check logical drive data

--------------------------------------------------------------------------------------
	 	 
Firmware Version: 2.41
Firmware Name: SMT_X10IPMI_241.bin
Firmware CRC: CEBA5D0B
Release date: 03/25/2016
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X10DSC+

***************  Need Factory default after updated this FW ******************

1.
    Category: Fix
    Description:
		Fix PB #69906, SUM test is fail. 
		Fix virtual media(storage) of KVM can't real mount

    Infected Motherboard: All
    Affected functions:
    Validation :
     1). Run BMC mount ISO
	 2). Check BIOS can detect new device from BMC

2.
    Category: Fix
    Description:
		Fix incorrect threshold values of CPU temperature sensor

    Infected Motherboard: All
    Affected functions:
    Validation :
     1). Check threshold values of CPU temperature sensor 
	 
3.
    Category: Fix
    Description:
		Fix PB #69907, PCH temp goes below threshold 

    Infected Motherboard: X10DSC+
    Affected functions:
    Validation :
     1). Run DC on/off testing
	 2). Check PCH event log

4.
    Category: Fix
    Description:
		Fix no storage monitoring information on the system
		Fix PB #69305, Storage monitoring tab shows inccorect logical drive data 

    Infected Motherboard: X10DSC+
    Affected functions:
    Validation :
	 1). Check storage monitoring information in Storage monitoring tab
     2). Check logical drive data
	 	 
--------------------------------------------------------------------------------------

Firmware Version: 2.39
Firmware Name: SMT_X10IPMI_239.bin
Firmware CRC: A5B85967
Release date: 03/14/2016
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X10DSC+

***************  Need Factory default after updated this FW ******************

1.
    Category: Fix
    Description:
		PB #69318, Null Value Found for Max Capable Speed (Hardware Information)

    Infected Motherboard: All
    Affected functions:
    Validation :
     1). Check Max Capable Speed in Hardware Information page

2.
    Category: Enhanecement
    Description:
		Support Thermal Guide v4.05 threshold values

    Infected Motherboard: All
    Affected functions:
    Validation :
     1). Check sensor threshold values

3.
    Category: Fix
    Description:
		PB #69305, Storage monitoring tab shows inccorect logical drive data 

    Infected Motherboard: X10DSC+
    Affected functions:
    Validation :
     1). Check logical drive data in Storage monitoring tab

4.
    Category: Enhancement
    Description:
		Support SMCI IPMI Help Message Guide v1.1

    Infected Motherboard: All
    Affected functions:
    Validation :
     1). Check IPMI help messages and web content

--------------------------------------------------------------------------------------

Firmware Version: 2.36
Firmware Name: SMT_X10IPMI_236.bin
Firmware CRC: FB5286E5
Release date: 02/02/2016
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X10DSC+

1.
    Category: Enhance
    Description:
		Enhance dynamic sensor adjustment to avoid BMC kernel panic

    Infected Motherboard: All
    Affected functions:
    Validation :
     1). Installed LSI card, 10G card, and power supply
	 2). Check BMC sensor reading and BMC status

---------------------------------------------------------------------------------------

Firmware Version: 2.35
Firmware Name: SMT_X10IPMI_235.bin
Firmware CRC: 66F3C0EE
Release date: 01/30/2016
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X10DSC+

1.
    Category: Fix
    Description:
	PB #68578, IPMI FailOver function is fail  	   	

    Infected Motherboard: X10DRL_CT
    Affected functions:
    Validation :
     1). plug in/out either one LAN cables and check IPMI Lan fail over function

2.
    Category: Fix
    Description:
	PB #68649, SMSTC test fail

    Infected Motherboard: X10DRL_CT
    Affected functions:
    Validation :
     1). Run SMSTC ECO mode

3.
    Category: Fix
    Description:
    	PB #67994, Help Message Content Misalignment
	PB #67951, Compatibility Issue with IE11

    Infected Motherboard: All
    Affected functions:
    Validation :
     1). Check all BMC web help messages and web pages 

4.
    Category: Fix
    Description:
    	Expander temperature sensor show 1 degree after AC cycle or IPMI FW reset.

    Infected Motherboard: X10DSC+
    Affected functions:
    Validation :
     1). Check expander temperature sensor reading after AC cycle or IPMI FW reset.

---------------------------------------------------------------------------------------

Firmware Version: 2.33
Firmware Name: SMT_X10IPMI_233.bin
Firmware CRC: B8B820DA 
Release date: 01/21/2016
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X10DSC-T+

1.
    Category: Fix
    Description:
    	PB #68647, [ECO] BMC don't detect "Processor Automatically Throttled De-assertion" log when CPU temp restored.

    Infected Motherboard: X10DRL_CT
    Affected functions:
    Validation :
     1). Heat up CPU temp and check "Processor Automatically Throttled assertion" log
     2). Check "Processor Automatically Throttled De-assertion" log when CPU temp restored.

---------------------------------------------------------------------------------------

Firmware Version: 2.32
Firmware Name: SMT_X10IPMI_232.bin
Firmware CRC:  BB5C8D28
Release date: 01/08/2016
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X10DSC-T+

1.
    Category: Modify
    Description:
    	Adjust RGMII1 driving strength to high driving when used X10DRL-IT v1.10 or X10DRL-CT v1.10.

    Infected Motherboard: X10DRL_CT
    Affected functions:
    Validation :
     1). Programing FRU1 as production
     2). Testing NCSI funtion and check RGMII1 signal

---------------------------------------------------------------------------------------

Firmware Version: 2.31
Firmware Name: SMT_X10IPMI_231.bin
Firmware CRC:  E9E8C7C7
Release date: 12/31/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X10DSC-T+

1.
    Category: New
    Description:
    	Support X540 NCSI port

    Infected Motherboard: X10DRL_CT
    Affected functions:
    Validation :
     1). Test X540 LAN port and the port is LAN3 on motherboard

2.
    Category: New
    Description:
    	Show expander EC revision on EC udpated page

    Infected Motherboard: X10DSC-T+
    Affected functions:
    Validation :
     1). Check expander EC revision on EC udpated page

---------------------------------------------------------------------------------------

Firmware Version: 2.30
Firmware Name: SMT_X10IPMI_230.bin
Firmware CRC:  1B13F69F
Release date: 12/17/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X10DSC-T+

1.
    Category: Enhancement
    Description:
    	Support 48 bay NVME

    Infected Motherboard: all
    Affected functions:
    Validation :
     1). Installed correct expander board and 48 NVME
     2). Check NVME status in IPMI GUI

2.
    Category: Fix
    Description:
    	PB #66844, Issues on storage monitoring tab in IPMI GUI 

    Infected Motherboard: X10DSC-T+
    Affected functions:
    Validation :
     1). Check storage monitoring tab in IPMI GUI

3.
    Category: Fix
    Description:
    	PB #66635, No "Processor Automatically Throttled" event on the CPU2 when the CPU2 is overheated 

    Infected Motherboard: X10DSC-T+
    Affected functions:
    Validation :
     1). Heat up CPU2 and waitting system shutdown
     2). Check "Processor Automatically Throttled" event in IPMI GUI or IPMI utility

4.
    Category: Fix
    Description:
    	PB #66640, Some tags and Help information are showing "undefined"  

    Infected Motherboard: X10DSC-T+
    Affected functions:
    Validation :
     1). Check all IPMI GUI pages and help information

5.
    Category: Fix
    Description:
    	PB #66656, The SNMP is not working
	PB #67552, (SMT_X10IPMI_229 ,IPMIWebTest) SNMP Issue --When enabled SNMP v2/v3, we can¡¦t get SNMP status 

    Infected Motherboard: X10DSC-T+, X10DRL_CT
    Affected functions:
    Validation :
     1). Use 'MIB browser' or 'SnmpWalk' to check BMC SNMP response

6.
    Category: Fix
    Description:
    	PB #67914, Storage monitoring shows incorrect hard drive size 

    Infected Motherboard: X10DSC-T+
    Affected functions:
    Validation :
     1). Installed 6TB or 5TB to check hard drive size in IPMI GUI

7.
    Category: Fix
    Description:
    	PB #67915, Creating incorrect storage configuration forces IPMI log out when using storage monitoring tab 

    Infected Motherboard: X10DSC-T+
    Affected functions:
    Validation :
     1). Creating incorrect storage configuration like selecting over 32 HDD for raid configuration
     2). BMC can't happen 'log out'

8.
    Category: Fix
    Description:
    	PB #67918, Storage monitoring shows an additional read policy option

    Infected Motherboard: X10DSC-T+
    Affected functions:
    Validation :
     1). Check read policy option and it can't have adaptive read policy option

9.
    Category: Fix
    Description:
    	PB #67556, (SMT_X10IPMI_229, IPMIWebTest) Daylight Saving Time Checkbox of Date Time are different between SMT_X10_223 and SMT_X10IPMI_229 

    Infected Motherboard: X10DRL-CT
    Affected functions:
    Validation :
     1). Check Daylight Saving Time Checkbox

10.
    Category: Fix
    Description:
    	PB #67838, Memory Temp. reading will fail when system in chamber under 0 degree  

    Infected Motherboard: X10DRL-CT
    Affected functions:
    Validation :
     1). Memory Temp. reading will not be fail when system in chamber under 0 degree.

11.
    Category: Fix
    Description:
    	PB #67804, Factory Default message is reverse

    Infected Motherboard: X10DRL-CT
    Affected functions:
    Validation :
     1). Run factory default in IPMI GUI, it should show Warning message first and then show Waiting message.

12.
    Category: Fix
    Description:
    	PB #67803, Always show "Java Update" message in IPMI Console Redirection page 

    Infected Motherboard: X10DRL-CT
    Affected functions:
    Validation :
     1). Check "Java Update" message in IPMI Console Redirection page.


---------------------------------------------------------------------------------------

Firmware Version: 2.29
Firmware Name: SMT_X10IPMI_229.bin
Firmware CRC:  1D73DD2D
Release date: 11/13/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X10DSC-T+

1.
    Category: Fix
    Description:
    	SUM v1.4.2 and v1.6.0 testing error

    Infected Motherboard: X10DRFF-IG, X10DRL_CT
    Affected functions:
    Validation :
     1). Run SMSTC testing

---------------------------------------------------------------------------------------

Firmware Version: 2.25
Firmware Name: SMT_X10IPMI_225.bin
Firmware CRC:  D142C800
Release date: 10/27/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X10DSC-T+

1.
    Category: Fix
    Description:
    	Happen 'Voltage Protection (Force Shutdown)' event during CPU stress testing

    Infected Motherboard: X10DRFF-IG
    Affected functions:
    Validation :
     1). Run CPU stress testing
     2). Check SEL

---------------------------------------------------------------------------------------

Firmware Version: 2.24
Firmware Name: SMT_X10IPMI_224.bin
Firmware CRC:  CD19213F
Release date: 10/27/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X10DSC-T+

1.
    Category: Fix
    Description:
    	"The fan speed is up and down when the Memory is overheated." (IssueID=66183) 

    Infected Motherboard: X10DSC-T+
    Affected functions:
    Validation :
     1). Check fan speed when the Memory is overheated

2. 
    Category: Fix
    Description:
	BMC show unexpected 'Voltage Protection (Force Shutdown)' SEL	

    Infected Motherboard: X10DRFF-IG
    Affected functions:
    Validation :
     1). Rework one board to make lower 12V voltage for BMC monitoring
     2). Power on the board and it will be power off after a few seconds  
     3). Check 'Voltage Protection (Force Shutdown)' SEL in event log page

3.
    Category: Enhancement
    Description:
    	New 0xAE OEM command for auto recovery Bios

    Infected Motherboard: X10DRL_CT
    Affected functions:
    Validation :
     1). Please use BIOS that build date after 10/27/2015.
     2). Used utility to update bad BIOS image then rebooting system. 

---------------------------------------------------------------------------------------

Firmware Version: 2.23
Firmware Name: SMT_X10IPMI_223.bin
Firmware CRC: 9FBE4DC0
Release date: 10/16/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X10DSC-T+

1.
    Category: Fix
    Description:
    	"The fan speed doen't increase when the RT2 temp. is high." (IssueID=66180) 

    Infected Motherboard: X10DSC-T+
    Affected functions:
    Validation :
     1). Heating RT2 temperature and check fan speed

2. 
    Category: Fix
    Description:
    	"X10DRC+ Rev1.00: Fan PWM Fail" (IssueID=66286) 

    Infected Motherboard: X10DSC-T+
    Affected functions:
    Validation :
     1). Heating RT2/PCH temperature and check fan speed

3.
    Category: Fix
    Description:
    	No "Thermal trip-Assertion" ipmi event when the thermal trip is triggered. (IssueID=66123) 

    Infected Motherboard: X10DSC-T+
    Affected functions:
    Validation :
     1). Heating CPU chip and make thermal trip is triggered
     2). Check ipmi event

4. 
    Category: Fix
    Description:
    	VCPU_VRM Temp status is shown as N/A in IPMI Sensor Reading page. (IssueID=66114) 
 
    Infected Motherboard: X10DSC-T+
    Affected functions:
    Validation :
     1). Check sensor reading page

5. 
    Category: New
    Description:
    	Update EC FW for BPN-SAS3-946SEL1/2

    Infected Motherboard: X10DSC-T+
    Affected functions:
    Validation :
     1). Press 'EC Update' in 'Maintenance' page of web
     2). Select expander board and file then pressing 'Update'

6. 
    Category: New
    Description:
    	Expander temperature for BPN-SAS3-946SEL1/2 board

    Infected Motherboard: X10DSC-T+
    Affected functions:
    Validation :
     1). Install BPN-SAS3-946SEL1/2 board
     2). Check 'Expander Temp' sensor 

7. 
    Category: Fix
    Description:
    	Fix: false 12V protection alert when stress testing for power on or power off

    Infected Motherboard: X10DRFF-IG
    Affected functions:
    Validation :
     1). stress testing for power on/off

---------------------------------------------------------------------------------------

Firmware Version: 2.22
Firmware Name: SMT_X10IPMI_222.bin
Firmware CRC: 689BFC76
Release date: 09/25/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X10DSC-T+

1.
    Category: Fix
    Description:
    	No multi-node information in BMC web

    Infected Motherboard: X10DRFF-IG
    Affected functions:
    Validation :
     1). Check node information on Multi Node Monitoring page

2. 
    Category: New
    Description:
    	LSI HDD status sensor

    Infected Motherboard: ALL
    Affected functions:
    Validation :
     1). Check HDD status sensor on sensor readings page

3. 
    Category: Enhance
    Description:
    	Enhance LSI storage monitoring page. Support to create/add/delete virtual drive

    Infected Motherboard: ALL
    Affected functions:
    Validation :
     1). Activate OOB key
     2). Create/add/delete virtual drive on storage monitoring page

4. 
    Category: New
    Description:
    	12V protection

    Infected Motherboard: X10DRFF-IG
    Affected functions:
    Validation :
     1). Rework one board to make lower 12V voltage for BMC monitoring
     2). Power on the board and it will be power off after a few seconds  
     3). Check 'Voltage Protection (Force Shutdown)' SEL in event log page

5. 
    Category: Fix
    Description:
    	Case 223 in issue "[SUMv1.4.2] SUM test fail." (IssueID=64450)

    Infected Motherboard: X10DRFF-IG
    Affected functions:
    Validation :
     1). Run Full mode testing in SMSTC web page

6. 
    Category: New
    Description:
    	Show GPU temperature sensor for M60 GPU card

    Infected Motherboard: ALL
    Affected functions:
    Validation :
     1). Check GPU sensor reading

---------------------------------------------------------------------------------------

Firmware Version: 2.21
Firmware Name: SMT_X10IPMI_221.bin
Firmware CRC: 35142B03
Release date: 08/26/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X11SSW_F, X10DSC-T+

1.
    Category: Fix
    Description:
    	SUM test cases

    Infected Motherboard: ALL
    Affected functions:
    Validation :
     1). Run full mode test in new SMSTC

---------------------------------------------------------------------------------------

Firmware Version: 2.20
Firmware Name: SMT_X10IPMI_220.bin
Firmware CRC: 5BFA3B3B
Release date: 08/19/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X11SSW_F, X10DSC-T+

1.
    Category: Fix
    Description:
    	64575, Several minor errors found in web gui 

    Infected Motherboard: ALL
    Affected functions:
    Validation :
     1). Check 'Server Health' page
     2). Check 'Configuration' page
     3). Check 'Maintenance' page

2.
    Category: Enhancement
    Description:
    	Add more Web event log descriptions of memory errors 

    Infected Motherboard: All
    Affected functions:
    Validation :
     1). Produce memory error event log by instlled bad dimm or other way
     2). Check 'Event Log' page

---------------------------------------------------------------------------------------

Firmware Version: 2.19
Firmware Name: SMT_X10IPMI_219.bin
Firmware CRC:  11343E90
Release date: 08/12/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X11SSW_F, X10DSC-T+

1.
    Category: Fix
    Description:
    	64331, No AOC card temperature reading on IPMI Web    

    Infected Motherboard: X11SSW_F
    Affected functions:
    Validation :
     1). Install AOC card and reboot SUT
     2). check sensor reading

2.
    Category: Enhancement
    Description:
    	Fix Missing/inaccurate power consumption data and Time showing in Power/Temperature Record

    Infected Motherboard: All
    Affected functions:
    Validation :
     1). Power on SUT and wait over one week
     2). Check all power item in Power/Temperature web page

3.
    Category: New
    Description:
    	Update EC firmware on BMC web

    Infected Motherboard: X11SSW_F
    Affected functions:
    Validation :
     1). Login BMC Web
     2). Click Maintenance->EC Update page
     3). Select file to upload and click update button
     4). Check new EC revision in BMC Summary page

4. 
    Category: Fix
    Description:
    	64423, Vcpu sensor show Lower Non-recoverable    

    Infected Motherboard: X11SSW_F
    Affected functions:
    Validation :
     1). check sensor reading and event log

---------------------------------------------------------------------------------------

Firmware Version: 2.18
Firmware Name: SMT_X10IPMI_218.bin
Firmware CRC:  E0C3AF2E
Release date: 08/05/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X11SSW_F, X10DSC-T+

1.
    Category: Fix
    Description:
    	63926 - IPMI monitor Vcpu reading fail.    

    Infected Motherboard: X11SSW_F
    Affected functions:
    Validation :
     1). check sensor reading

2.
    Category: Fix
    Description:
    	63851 - Fan control cannot meet spec curve.

    Infected Motherboard: X11SSW_F
    Affected functions:
    Validation :
     1). testing fan control

---------------------------------------------------------------------------------------

Firmware Version: 2.17
Firmware Name: SMT_X10IPMI_217.bin
Firmware CRC:  400F9296
Release date: 07/31/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X11SSW_F, X10DSC-T+

1.
    Category: Fix
    Description:
    	64123 - Standard FAN mode FAN speed doesn't go up when CPUs temp goes high     

    Infected Motherboard: ALL
    Affected functions:
    Validation :
     1). test fan control.
---------------------------------------------------------------------------------------

Firmware Version: 2.16
Firmware Name: SMT_X10IPMI_216.bin
Firmware CRC:  86EC412B
Release date: 07/28/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X11SSW_F, X10DSC-T+

1.
    Category: Fix
    Description:
    	64041 - BIOS Resilience shown in Miscellaneous description   

    Infected Motherboard: X10DRFF-IG
    Affected functions:
    Validation :
     1). Miscellaneous page 

2.
    Category: fix
    Description:
    	63666 - [IPMI] Power/Temperature record page doesn't record the correct CPU temperature. 

    Infected Motherboard: X10DGQ
    Affected functions:
    Validation :
     1). check Power/Temperature record page
3.
    Category: fix
    Description:
    	"IPMI Power/Temperature Record page is not showing CPU temperature correctly" (IssueID=63715)  

    Infected Motherboard: X10DRFF-IG
    Affected functions:
    Validation :
     1). check Power/Temperature record page
4.
    Category: fix
    Description:
    	"card temperature shows 0 in Power/Temperature Record page" (IssueID=63719)  

    Infected Motherboard: X10DRFF-IG
    Affected functions:
    Validation :
     1). check Power/Temperature record page

5.
    Category: fix
    Description:
    	63992 - PUE2 should NOT be the default fan mode in IPMI 2.15 for X10DRFF-IG . 

    Infected Motherboard: X10DRFF-IG
    Affected functions:
    Validation :
     1). reset to default
     2). the default fan mode should be standard
6.
    Category: fix
    Description:
    	fix - correct multi node DC current and DC power when configuration ID is 1 

    Infected Motherboard: X10DRFF-IG
    Affected functions:
    Validation :
     1). check multi node page

7.
    Category: fix
    Description:
    	fix - SUM faild to update BMC

    Infected Motherboard: X10DRFF-IG
    Affected functions:
    Validation :
     1). update BMC firmware via SUM
--------------------------------------------------------------------------------

Firmware Version: 2.15
Firmware Name: SMT_X10IPMI_215.bin
Firmware CRC:  6A5A682B
Release date: 07/13/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X11SSW_F, X10DSC-T+

1.
    Category: Fix
    Description:
    	63291 - [IPMI]MIssing CPU VRM Temperature and Card Tempreture on Power/Temperature record page.  

    Infected Motherboard: X10DGQ
    Affected functions:
    Validation :
     1). check Power/Temperature record page

2.
    Category: New
    Description:
    	Support X10DSC_T+

    Infected Motherboard: X10DSC-T+
    Affected functions:
    Validation :
     1). Support X10DSC_T+
--------------------------------------------------------------------------------

Firmware Version: 2.14
Firmware Name: SMT_X10IPMI_214.bin
Firmware CRC:  CB6B42C9
Release date: 07/08/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X11SSW_F

1.
    Category: Fix
    Description:
    	[SUM] test cases failed" (IssueID=63154) 

    Infected Motherboard: X10DRFF-IG
    Affected functions:
    Validation :
     1). check SUM test cases result

2.
    Category: Fix
    Description:
    	[SUM] Test cases failed" (IssueID=62542) 

    Infected Motherboard: X10DGQ
    Affected functions:
    Validation :
     1). check SUM test cases result


--------------------------------------------------------------------------------

Firmware Version: 2.13
Firmware Name: SMT_X10IPMI_213.bin
Firmware CRC:  A2F980F3
Release date: 07/03/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X11SSW_F

1.
    Category: Fix
    Description:
    fix - DIMM temperature sensor reading

    Infected Motherboard: X11SSW_F
    Affected functions:
    Validation :
     1). check DIMM temperature sensor

--------------------------------------------------------------------------------

Firmware Version: 2.12
Firmware Name: SMT_X10IPMI_212.bin
Firmware CRC:  2F8EB876
Release date: 06/30/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X11SSW_F

1.
    Category: Fix
    Description:
    fix - power consumption page 

    Infected Motherboard: ALL
    Affected functions:
    Validation :
     1). check power consumption page

2.
    Category: Fix
    Description:
    fix - SUM test fail 

    Infected Motherboard:  ALL
    Affected functions:
    Validation :
     1). check SUM
--------------------------------------------------------------------------------

Firmware Version: 1.91
Firmware Name: SMT_X10IPMI_191.bin
Firmware CRC:   C99AA2C6
Release date: 06/23/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X11SSW_F

1.
    Category: Fix
    Description:
     When node plug in but  turn off, power status display should show Off, but current display shown On

    Infected Motherboard:  X10DRFF-IG
    Affected functions:
    Validation :
     1). check multi node webpage
2.
    Category: Fix
    Description:
     When Backplane BPlocation not = 01 (left) or 10 (right) , the BMC should display node as A,B,C,D,E,F,G,H
  Instead of 1,2,3,4,5,6,7,8

    Infected Motherboard:  X10DRFF-IG
    Affected functions:
    Validation :
     1). check multi node webpage
--------------------------------------------------------------------------------

Firmware Version: 1.90
Firmware Name: SMT_X10IPMI_190.bin
Firmware CRC:   4A8923C0
Release date: 06/19/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X11SSW_F

1.
    Category: Fix
    Description:
     fix - follow spec to change multi page for Fat Twin

    Infected Motherboard:  X10DRFF-IG
    Affected functions:
    Validation :
     1). check multi node webpage
--------------------------------------------------------------------------------

Firmware Version: 1.89
Firmware Name: SMT_X10IPMI_189.bin
Firmware CRC:  EA1B5DC4
Release date: 06/17/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X11SSW_F

1.
    Category: Fix
    Description:
     fix - X10DRFF-IG power consumption wrong

    Infected Motherboard:  X10DRFF-IG
    Affected functions:
    Validation :
     1). check power consumption

2.  Category: fix
    Description:
     fix - UM caase #217 and #211

    Infected Motherboard: ALL
    Affected functions:
    Validation :
     1). sum test

3.  Category: fix
    Description:
     fix - power control buttons do not work in sys_info.www page when use Chrome browser.

    Infected Motherboard: ALL
    Affected functions:
    Validation :
     1). check power button in system information
---------------------------------------------------------------------------------

Firmware Version: 1.88
Firmware Name: SMT_X10IPMI_188.bin
Firmware CRC: 127327FA
Release date: 06/5/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X11SSW_F

1.
    Category: Fix
    Description:
     fix again- 61207 System failed to power on after running AC on/off for 476 cycles 

    Infected Motherboard: X10DGQ
    Affected functions:
    Validation :
     1). running AC on/off

2.  Category: fix
    Description:
     fix - change back to just support failover on Dedicated LAN, LAN1 but no LAN2 because of side effect.

    Infected Motherboard: ALL
    Affected functions:
    Validation :
     1). failover on Dedicated LAN, LAN1

---------------------------------------------------------------------------------
Firmware Version: 1.47
Firmware Name: SMT_X10IPMI_147.bin
Firmware CRC: 136FD2EE
Release date: 05/29/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X11SSW_F

1.
    Category: fix
    Description:
     fix - 62026 [IPMI] Fans don't go full speed after IPMI cold reset when GPUs present.  

    Infected Motherboard: X10DGQ
    Affected functions:
    Validation :
     1). Fans will go full speed after IPMI cold reset when GPUs present.

2.
    Category: Fix
    Description:
     fix - 61207 System failed to power on after running AC on/off for 476 cycles 

    Infected Motherboard: X10DGQ
    Affected functions:
    Validation :
     1). running AC on/off

3.
    Category: Fix
    Description:
     fix - 61894 [IPMI] IPMI 24hr cold reset stress is failed. IPMI FW is crashed in 6hr  

    Infected Motherboard: X10DGQ
    Affected functions:
    Validation :
     1). running IPMI cold reset

4.  Category: Feature
    Description:
     feature - support failover on Dedicated LAN, LAN1 and LAN2 

    Infected Motherboard: ALL
    Affected functions:
    Validation :
     1). failover on Dedicated LAN, LAN1 and LAN2 

---------------------------------------------------------------------------------

Firmware Version: 1.46
Firmware Name: SMT_X10IPMI_146.bin
Firmware CRC: A41F316A
Release date: 05/26/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT, X11SSW_F

1.
    Category: Add
    Description:
     Support new platform X11SSW_F with Board ID 0x89B.

    Infected Motherboard: X11SSW_F
    Affected functions:
    Validation :
     1). Check all IPMI functions and IPMI version.

2.
    Category: Fix
    Description:
     No email alert when SMTP setting too long.

    Infected Motherboard: X10DGQ, X10DRFF-IG, X10DRL_CT
    Affected functions:
    Validation :
     1). Set long SMTP setting and Alert setting in BMC web
     2). Used 'Add SEL' ipmi command to produce SEL
	 3). Check email in email address of Alert setting

---------------------------------------------------------------------------------

Firmware Version: 1.45
Firmware Name: SMT_X10IPMI_145.bin
Firmware CRC: FB7FB5C0
Release date: 05/20/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT

1.
    Category: Fix
    Description:
     Resize OEMPS from 0x400 to 0x1200 to fix OEMPS data can't be stored issue

    Infected Motherboard: X10DGQ
    Affected functions:
    Validation :
     1). check all the configurations that should be able to be stored even AC lost or FW reboot

2.
    Category: Modify
    Description:
     Set default value to Enable for "System Event Log" and "AC Power On Event Log" to log detailed event log

    Infected Motherboard: X10DGQ, X10DRFF-IG, X10DRL_CT
    Affected functions:
    Validation :
     1). Do "Restore Factory Default" once to update the new default settings
     2). Check the settings are Enable from web pages "Event Log - Advanced Settings" and "List of System Event Log"

---------------------------------------------------------------------------------

Firmware Version: 1.44
Firmware Name: SMT_X10IPMI_144.bin
Firmware CRC: 0E50A957
Release date: 05/15/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT

1.
    Category: Fix
    Description:
     #61597 IPMI sensor reading for DIMM temp is incorrect

    Infected Motherboard: X10DGQ
    Affected functions:
    Validation :
     1). check sensor reading

2.
    Category: Fix
    Description:
     #61207 System failed to power on after running AC on/off for 476 cycles

    Infected Motherboard: X10DGQ, X10DRFF-IG, X10DRL_CT
    Affected functions:
    Validation :
     1). Run our testing script file to verify that.

3.
    Category: Add
    Description:
     Implement 12V protection function

    Infected Motherboard: X10DGQ, X10DRFF-IG, X10DRL_CT
    Affected functions:
    Validation :
     1). Make 12V sensor trigger LNR event
     2). System shutdown by BMC

4.
    Category: Add
    Description:
     Support sensors temperature history record

    Infected Motherboard: X10DGQ, X10DRFF-IG, X10DRL_CT
    Affected functions:
    Validation :
     1). Clear browser's and Java's catch in client computer side
     2). Log in IPMI Web page "Power/Temperature Record"

---------------------------------------------------------------------------------

Firmware Version: 1.42
Firmware Name: SMT_X10IPMI_142.bin
Firmware CRC: 6DE8FBE7
Release date: 05/04/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT

1.
    Category: Fix
    Description:
     61513 Cannot show AOC 40G temperature reading in IPMI while the AOC card is inserted on the RSC-F-88-F1 

    Infected Motherboard: X10DRFF-IG
    Affected functions:
    Validation :
     1). check sensor reading

2.
    Category: Fix
    Description:
     61412 RSC-F-88-F1 cannot show AOC temperature reading in IPMI.  

    Infected Motherboard: X10DRFF-IG
    Affected functions:
    Validation :
     1). check sensor reading

3.
    Category: Fix
    Description:
     61443 System fans go full speed when IPMI got any temperature reading is under 0C 

    Infected Motherboard: X10DGQ, X10DRFF-IG, X10DRL_CT
    Affected functions:
    Validation :
     1). check sensor reading

---------------------------------------------------------------------------------

Firmware Version: 1.41
Firmware Name: SMT_X10IPMI_141.bin
Firmware CRC: 18208278
Release date: 4/29/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT

1.
    Category: Fix
    Description:
     61413 IPMI Sensor wrong DIMM Temp.

    Infected Motherboard: X10DRFF-IG
    Affected functions:
    Validation :
     1). check sensor reading

2.
    Category: Fix
    Description:
     61412 RSC-F-88-F1 cannot show AOC temperature reading in IPMI.  

    Infected Motherboard: X10DRFF-IG
    Affected functions:
    Validation :
     1). Update latest BIOS X10DRFG5.428 or latest
     2). check sensor reading

3.
    Category: Fix
    Description:
     61282 [IPMI] AOC 40G temp shows -1C for new installed AOC 40Gb card 

    Infected Motherboard: X10DRFF-IG, X10DGQ
    Affected functions:
    Validation :
     1). check sensor reading

4.
    Category: Fix
    Description:
     61408 [ipmi] Missing XeonPhi Sensor Reading 

    Infected Motherboard: X10DGQ
    Affected functions:
    Validation :
     1). check sensor reading

---------------------------------------------------------------------------------

Firmware Version: 1.39
Firmware Name: SMT_X10IPMI_139.bin
Firmware CRC: C37B37C3
Release date: 4/20/2015
Supported Platform: X10DGQ, X10DRFF-IG, X10DRL_CT

1.
    Category: Add
    Description:
     Support new platform X10DGQ with Board ID 0x893.
     (Note that: Current BIOS FW x10dgq5.415 doesn't send correct platform ID (0x893) to BMC, so all IPMI functions and Sensors may not work normally)

    Infected Motherboard: X10DGQ
    Affected functions:
    Validation :
     1). After BIOS post complete, issue IPMI raw Cmd "0x30 0x20 0x93 0x8 0 0x40 0 0 0 0 0 0" to manually set correct platform ID to BMC.
     2). Check all IPMI functions and IPMI version.

---------------------------------------------------------------------------------

Firmware Version: 1.38
Firmware Name: SMT_X10DRTH_138.bin
Firmware CRC: 01AEDE6D
Release date: 4/14/2015
Supported Platform: X10DRT-H, X10DRT-HIBF

1.
    Category: fix
    Description:
     61103 - IPMI Power Control Not Working   

    Infected Mothboard: X10DRT-H, X10DRT-HIBF
    Affected functions:
    Validation :
     1). IPMI power control
2. 
    Category: fix    
    Description:
     60943 - IPMI loses sensor readings after system reboot 
     Validation :
	1). check sensor reading
---------------------------------------------------------------------------------