Filename: REDFISH_X10_372.bin  version: 3.72  Date: 05-15-2018
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r37
Redfish/iKVM version       : 1.0.1
Redfish API : Redfish_API_full_list_2018_03_16.xlsx

1.
    Description: Fix
        [90447] [ECO IPMI3.71] Total average power of the system would shake up and down under system stress.
        [90404] ECO] Total average power of the system would shake up and down under system stress.
        [90403] ECO] [ECO REDFISH3.71] System power consumption is unstable under the given power policy limits.
        [90342] ECO] [ECO] Total average power of the system would shake up and down under system stress.

        Impact motherboard:
            X10DRG-Q, X10DRX, X10DRW-IT, X10DRW-E

    Validation :
        1. Run the PTU test.
        2. Lanuch SPM software to monitor power consumption.
        3. Verify if the statistics is normal.

2.
    Description: Fix
        [90265] Update 3108's FW over BMC's WEB page
        [89936]
        [90153]

    Impact motherboard:
        All MBs that are suitable and installed with 3108

    Affected functions:
    Validation :
        1. First of all, you must make sure firmware version of target 3108 is
           already flashed 4.680.00-8290 that support OOB-I2C-way only.
        2. Prepare two more 3108 FW files that are versioned as 4.650.00-6223 and
           4.680.00-8290 respectively (You can download from project board,
           ProjectID: 8259, zipped file name: AVG3108M6B3H101.rar and
           AVG3108M6E3H103.rar).
        3. Login BMC WEB and go to "Stoage monitoring" submenu, then go
           controller information's subpage and there shall be a button - "ROM
           Update" for this feature.
        4. Please notice one thing - because OOB-I2C-way is a slow way to flash
           3108, so it will take almost 30 minutes to complete whole flashing
        5. Cross flashing and validation on the flashed version to see if it
           is changed or not.

        <Notice> If you set current 3108 FW to be "JBOD personality".
                 Then there won't be the "ROM Update" button shown.

3. Features
    Description: Features
        Add PUE2 mode for A2SDV-LN8F/LN10PF

    Impact motherboard:
        A2SDV-LN8F/LN10PF

    Affected functions:
    Validation :
        1. Check the Fan mode setting.

-------------------------------------------------------------------------------------
Filename: REDFISH_X10_371.bin  version: 3.71  Date: 04-23-2018
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r37
Redfish/iKVM version       : 1.0.1
Redfish API : Redfish_API_full_list_2018_03_16.xlsx

1.
    Description: Fix
        [90228] [IPMI ECO] Redfish Automation test got 9 fails.
        [90227] Redfish 500 returned when PATCH NetworkProtocol after factory default.

        Impact motherboard:
            All motherboards.

    Validation :
        1. Run the redfish test.
-------------------------------------------------------------------------------------
Filename: REDFISH_X10_370.bin  version: 3.70  Date: 04-20-2018
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r37
Redfish/iKVM version       : 1.0.1
Redfish API : Redfish_API_full_list_2018_03_16.xlsx

1.
    Description: Fix
        Remove 10G sensor on sensor reading web gui.

    Impact motherboard:
         X10SDV-xC?�LN2F

    Affected functions:
    Validation :
        1. Update FW and remove current SDRs.
        2. Check the sensor reading web gui.

2.
    Description: Fix
        [89574] IPMI no Memory Temp and M.2 Temp sensor item.

    Impact motherboard:
        A2SDV-8C-LN8F

    Affected functions:
    Validation :
        1. Check the Memory Temp sensors.
        2. M.2 Temp sensor is not supported in X10 projects.

3.
    Description: Fix
        [89982] The sensor reading of AOC-STG-i4S card work abnormally.
        [89984] The sensor reading of AOC-STG-i4S card work abnormally.
        [89985] [IPMI ECO 3.69] AOC-STG-i4S sensor shows N/A.

    Impact motherboard:
        Motherboards with AOC-STG-i4S

    Affected functions:
    Validation :
        1. Insert the AOC-STG-i4S card.
        2. Check the AOC_NIC Temp reading.

4.
    Description: Fix
        [89885] SUM:Fail test case#215 Outband - ChangeBmcCfg and compare.

    Impact motherboard:
        X10OBi

    Affected functions:
    Validation :
        1. Use the sum to issue "-c GetNvmeInfo".
        2. The result should be "No NVMe controller is detected on the mother
           board.", if no NVMe devices are on the system.

5.
    Description: Fix
        [90161] IPMI 3.69 - Redfish AT has 9 fails.
        [90132] [IPMI V3.69 FW ECO] SATC test is fail.
        [90086] RedFish automation test fail.
        [90076] [IPMI ECO 3.69]Redfish Automation Tool check fail.
        [90045] [IPMI ECO] Redfish Automation test failed.
        [89983] Redfish API test fail.
        [89981] Redfish API test fail.
        [89924] [IPMI ECO 3.68] Redfish automation test fail.
        [89849] Redfish automation: 9 critical tests failed.
        [89729] [IPMI ECO] Redfish Automation test got 8 fails.
        [89316] [IPMI ECO] Redfish Automation test failed in get LDAP URI.

    Impact motherboard:
        All motherboards.

    Validation :
        1. Run the redfish test.

6.
    Description: Fix
        [90146] Power supply#5 sensor reading is N/A.

    Impact motherboard:
        X10OBi

    Affected functions:
    Validation :
        1. Check the PSU5 reading.

-------------------------------------------------------------------------------------
Filename: REDFISH_X10_369.bin  version: 3.69  Date: 04-09-2018
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r37
Redfish/iKVM version       : 1.0.1
Redfish API : Redfish_API_full_list_2018_03_16.xlsx

1.
    Description: Fix
        [88929] IPMI -- Grammar error in Event Log page.

    Impact motherboard:
        All MBs

    Affected functions:
    Validation :
        1. Check the string "Event Log:Max= 512,Used= 1" should be "Event Log:Max=512, Used= 1".

2.
    Description: Fix
        Duplicate AOC NIC sensor show on sensor reading web gui.

    Impact motherboard:
        AOC-STG-I4S

    Affected functions:
    Validation :
        1. Check the sensor reading. It should appear one AOC NIC sensor on web gui.

3.
    Description: Fix
        [88364] Walmart system SEL did not show bad disks at very beginning.

    Impact motherboard:
        Walmart system with AOC-3108 (MB: X10DRU-i+)

    Affected functions:
        Event logs for 3108 HDD removing

    Validation :
        1. Firstly, Install bad drives and make sure they can be shown on "Storage Monitoring" submenu.
        2. AC off system, after AC on at every beginning, Check if there will be respective bad drive event assertion each AC cycle.

4.
    Description: Fix
        [88370] Walmart system IPMI could not be able to detect remove or insert HDD activity intermittently.

    Impact motherboard:
        Walmart system with AOC-3108 (MB: X10DRU-i+)

    Affected functions:
        Event logs for 3108 HDD removing

    Validation :
        1. Make sure you have seen all connected drives shown on "Storage Monitoring" submenu.
        2. Prepare a command window to keep ping BMC. And then reboot/reset BMC
        3. Once the ping window is showing BMC is active.
           Login BMC WEB to check if there is any connected drives are shown in "Storage Monitoring" submenu.
        4. Make sure at this time, there is no any dirve showing on that menu.
           Remove some drives from backplane.
        5. Then wait a few minutes to see if there is any log about drive removing assertion showing in "Event Log" submenu.
        6. Once log is showing. Put it back and check if any de-assertion is logged.

5.
    Description: Fix
        [88371] Walmart systems could not see de-assertion messages after put back removed disks.

    Impact motherboard:
        Walmart system with AOC-3108 (MB: X10DRU-i+)

    Affected functions:
        Event logs for 3108 HDD removing

    Validation :
        1. Pull 10 HDD at same time, SEL show assertion message for each slot.
        2. Reset system
        3. After reset is done. Push back all 10HDD to see if any de-assertion messages

6.
    Category: Features
    Description:
        New Redfish features for download/upload ipmi confiuration.
        This function is equivalent to WEB UI like below
            "Maintenance"
                |
                |___"IPMI configuration"
                        |
                        |_ "Save IPMI Configuration"
                        |_ "Reload IPMI Configuration"

        Please also refer "Redfish_API_full_list_2018_03_16.xlsx ".

    Impact motherboard:
        All MBs

    Affected functions:
        IPMI configuration

    Validation:
        Before test firmware update, you need to install the DHC (By Restlet) Chrome extension:

            https://chrome.google.com/webstore/detail/restlet-client-dhc/

        [Download("Save" in WEB)]
        1. Issue a POST on the following URL. After BMC replied done, find a
           "Download" icon at the right-lower corner of DHC to press

           URL:
               https://{BMC_IP}/redfish/v1/UpdateService/IPMIConfig/Actions/IPMIConfig.Download
           Request body:
               N/A

        2. Then you can go to WEB UI to perform equivalent operation to check both
           downloaded files size and content.

        [Upload("Reload" in WEB)]
        1. Upload configuration file by issuing the following request with POST method and
           expect to receive a response with "Successfully Completed Request".
           The content type must be "multipart/form-data"

           URL:
               https://{BMC_IP}/redfish/v1/UpdateService/IPMIConfig/Actions/IPMIConfig.Upload
           Request header:
               Content-Type = multipart/form-data
           Request body:
               Since header indicate "form-data", please add a form parameter as "File"
               Parameter name: ipmi_config_file
               Paremeter file: browse a configuration file to attach

7.
    Category: Features
    Description:
        Revised Redfish "Actions" for clear event log.
        Please also refer "Redfish_API_full_list_2018_03_16.xlsx ".

    Impact motherboard:
        All MBs

    Affected functions:
        Clear event logs

    Validation:
        Use POSTMan or DHC to issue a POST on the following new URL
        [Old]
            https://{BMC_IP}/redfish/v1/Managers/1/LogServices/Log1/Actions/LogService.Reset
        [New]
            https://{BMC_IP}/redfish/v1/Managers/1/LogServices/Log1/Actions/LogService.ClearLog

8.
    Description: Fix
        [89611] IPMI Troubleshooting function is wrong.

    Impact motherboard:
        A2SDV-LN8F/LN10PF

    Validation :
        1. Go to Troubleshooting page.
        2. Press Dump button.
        3. Press the Download button.

9.
    Description: Fix
        [89172] no sensor reading for AOC-MHFI-i1C.

    Impact motherboard:
        X10DSC-TP4S

    Validation :
        1. Insert the AOC=MHFI-i1C.
        2. Power on the system and wait it to the OS.
        3. Check the AOC_NIC_Temp sensor.

10.
    Description: Fix
        [89764] [IPMI ECO 3.68] Redfish Automation Tool test fail.
        [89729] [IPMI ECO] Redfish Automation test got 8 fails.

    Impact motherboard:
        All motherboards.

    Validation :
        1. Run the redfish test.

11.
    Description: Fix
        [89807] [ECO IPMI3.68]Run smcipmitool pminfo command failed.

    Impact motherboard:
        X10SRG-F

    Validation :
        1. Use the SMCIPMITool pminfo command.
        2. Check the result.

-------------------------------------------------------------------------------------
Filename: REDFISH_X10_368.bin  version: 3.68  Date: 03-20-2018
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r37
Redfish/iKVM version       : 1.0.1
Redfish API : Redfish_API_full_list_2018_02_22.xlsx

1.
    Category: New feature
    Description:
        Adaptive temperature threshold in SDR for drives connected to 3108

    Impact motherboard:
        All MBs installed with 3108

    Affected functions:
    Validation :
        Threshold values in SDR for drives temperature is adaptive by their types
        1. If all HDD(rotational hard drive), then threshold is (UC:55, UNR:60)
        2. If all SSD, then threshold is (UC:70, UNR:75)
        3. If mix, then threshold is the same as HDD(rotational hard drive)

2.
    Category: New feature
    Description:
        Enable AC Power On Event log

    Impact motherboard:
        All MBs

    Affected functions:
    Validation :
        1. AC power off the system after new BMC FW is updated.
        2. AC power on.
        3. Check that AC Power On event log should exist.

3.
    Description: Fix
        AC Power On Event log reported when BMC do coldreboot.

    Impact motherboard:
        All MBs

    Affected functions:
    Validation :
        1. Disable AC Power On Event Log function (IPMI Web).
        2. Turn off AC powers.
        3. Turn on AC powers.
        4. Enable AC Power On Event Log function (IPMI Web).
        5. Unit Reset (IPMI Web).
        6. Check that AC Power On event log should not exist.

4.
    Category: New feature
    Description:
        Update 3108's FW over BMC's WEB page

    Impact motherboard:
        All MBs suitable for 3108 and also install with 3108

    Affected functions:
    Validation :
        1. First of all, you must make sure firmware version of target 3108 is
           already flashed 4.680.00-8290 that support I2C-way only.
        2. Prepare two more 3108 FW files that are versioned as 4.650.00-6223 and
           4.680.00-8290 respectively (You can download from project board,
           ProjectID: 8259, zipped file name: AVG3108M6B3H101.rar and
           AVG3108M6E3H103.rar).
        3. Login BMC WEB and go to "Stoage monitoring" submenu, then go
           controller information's subpage and there shall be a button - "ROM
           Update" for this feature.
        4. Please notice one thing - because I2C-way is a slow way to flash
           3108, so it will take almost 30 minutes to complete whole flashing
        5. Cross flashing and validation on the flashed version to see if it
           is changed or not.

5.
    Category: New feature
    Description:
        Enable/disable 3108's JBOD mode over -
        1. BMC's WEB page
        2. Redfish API: "/redfish/v1/Systems/1/Storage/HA-RAID"

    Impact motherboard:
        All MBs suitable for 3108 and also install with 3108

    Affected functions:
    Validation :
        1. [WEB]
           Login BMC WEB and go to "Stoage monitoring" submenu, then go
           controller information's subpage and there shall be a information
           about "JBOD Mode" with a drop-down menu for Enable/Disable.
        2. [BIOS]
           Current value of that drop-down menu means current setting of JBOD
           mode. So pick up different value to "Save" and reset system to go
           to 3108's BIOS configuration menu(during BIOS POST stage and after
           3108 being 100% initialized, press "Ctrl + R" to enter 3108's BIOS)
           to check if value is changed or not. After checking, please let go
           this BIOS menu to unlock 3108 so as to let it free run again.
        3. [Redfish]
           Go to browse Redfish API - "/redfish/v1/Systems/1/Storage/HA-RAID"
           and check the property, "JBODMode", whithin "StorageControllers".
           Check if this value matches what you see in step 2.
        4. [Redfish]
           Finally to perform the "Actions" - "HARAIDControllers.Save" to change
           jbod mode again.
           Operation details as below:
              URL:
                 https://${BMC_IP}/redfish/v1/Systems/1/Storage/HA-RAID/Actions/Oem/HARAIDController.Save
              HTTP method:
                 PATCH
              Example Body:
                 {
                    "ControllerId": 0,
                    "BIOSBootMode": "PauseOnError",
                    "JBODMode": "Enable"
                 }

           After successful execution of this PATCH, go to step 2[BIOS] to
           check again and of course you shall check again value in BMC WEB,
           too.

4.
    Description: New feature
        CPU VRM sensors are missing.

    Impact motherboard:
        X10DRH-I, X10DRH-C

    Affected functions:
    Validation :
        1. Check the sensor reading.
---------------------------------------------------------------------------------------------
Filename: REDFISH_X10_367.bin  version: 3.67  Date: 02-24-2018
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r37
Redfish/iKVM version       : 1.0.1
Redfish API : Redfish_API_full_list_2018_02_22.xlsx

1.
    Category: Fix
    Description:
        During system is booting and after Broadcom 3108 storage controller is
        initialized, when user removes those pre-installed HDDs(connect to
        storage backplane to 3108), BMC won't log events

    Impact motherboard:
        All MBs with Broadcom 3108 storage controller being installed

    Affected functions:
        Log HDD absent events

    Validation :
        1. Prepare a MB and install an AOC-H3108L-H8iR then and storage
           backplane, then connect some HDDs onto.
        2. Power on system, and after 3108's option ROM is loaded at BIOS
           stage, then check BMC can show "Storage monitoring" submenu.
        3. Once its attached HDDs also shown on that submenu, got to remove
           some HDDs and wait a moment(maybe 15 seconds) to check if BMC log
           these event or not.

2.
    Category: New feature
    Description: Add redfish memory information feature.
    Infected motherboard:
        All MBs
    Affected functions:
    Validation :
        1. check mothboard memory information from redfish(postman).

-------------------------------------------------------------------------------------------
Filename: REDFISH_X10_366.bin  version: 3.66  Date: 01-30-2018
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r37
Redfish/iKVM version       : 1.0.1
Redfish API : Redfish_API_full_list_2017_11_13.xlsx

1.
    Category: Features
    Description:
        Suppor redfish firmware inventory (bios/bmc update).

    Impact motherboard:
        All MBs
    Affected functions:
    Validation :
        Before testing the IPMI configuration download operation, you need
        to install the DHC (By Restlet) Chrome extension:
        https://chrome.google.com/webstore/detail/restlet-client-dhc/

        BIOS update
        1. Enter BIOS update mode by issuing the following request with
        POST method and expect to receive a response with ??Successfully
        Completed Request??
        https://<IP>/redfish/v1/UpdateService/FirmwareInventory/BMC/Actions/Oem/FirmwareInventory.UploadBMC
        2. Upload BIOS image by issuing the following request with POST
        method and expect to receive a response with ??Successfully Completed
        Request?? The content type must be ??multipart/form-data??
        https://<IP>/redfish/v1/UpdateService/FirmwareInventory/BIOS/Actions/Oem/FirmwareInventory.UploadBIOS
        3. Start to update BIOS by issung the following request with POST
        method and expect to receive a response with ??Successfully Completed
        Request?? 3 parameters, PreserveME, PreserveNVRAM and PreserveSMBIOS
        are required in the request body.
        https://<IP>/redfish/v1/UpdateService/FirmwareInventory/BIOS/Actions/Oem/FirmwareInventory.UpdateBIOS
        4. Check the BIOS update status by issuing the following request
        with GET method and expect to receive a response with BIOS
        information.
        https://<IP>/redfish/v1/UpdateService/FirmwareInventory/BIOS/

        BMC update
        1. Enter BMC firmware update mode by issuing the following
        request with POST method and expect to receive a response with
        ??Successfully Completed Request??
        https://<IP>/redfish/v1/UpdateService/FirmwareInventory/BMC/Actions/Oem/FirmwareInventory.EnterBMCUpdateMode
        2. Upload BMC image by issuing the following request with POST method
        and expect to receive a response with ??Successfully Completed
        Request?? The content type must be ??multipart/form-data??
        https://<IP>/redfish/v1/UpdateService/FirmwareInventory/BMC/Actions/Oem/FirmwareInventory.UploadBMC
        3. Start to update BMC by issung the following request with POST
        method and expect to receive a response with ??Successfully Completed
        Request?? 3 parameters, PreserveCfg, PreserveSdr and PreserveSsl are required in the request body.
        https://<IP>/redfish/v1/UpdateService/FirmwareInventory/BMC/Actions/Oem/FirmwareInventory.UpdateBMC
        4. Check the BMC firmware information by issuing the following
        request with GET method and expect to receive a response with BMC
        information.
        https://<IP>/redfish/v1/UpdateService/FirmwareInventory/BMC/

2.
    Category: Features
    Description:
        Support new SIOM AOC-MH25G-b2s2G.

    Impact motherboard:
        All MBs with SIOM.

    Affected functions:

    Validation :
        1. Insert the AOC-MH25G-b2s2G.
        2. Power cycle the system.
        3. Check the AOC NIC Temp reading.

3.
    Category: Features
    Description:
        Support A2SDV-LN10PF/LN8F

    Impact motherboard:
        A2SDV-LN10PF/LN8F

    Affected functions:

    Validation :
        1. For bring up.

4.
    Category: Fix
    Description:
        [87913] System Temp shows incorrect temperature when doing Redfish manual

    Impact motherboard:
        X10QRH+-P

    Affected functions:

    Validation :
        1. check System Temp in https://$IP/redfish/v1/Chassis/1/Thermal

5.
    Category: Fix
    Description:
        [87910] Redfish Automation failed
        [87581] Redfish Automation Test Fail 8 items
        [87576] Redfish Automation failed 3 items
        [87472] Redfish 4 test items failed

    Impact motherboard:
        X10QRH+-P, X10DRT, X10DRT-PS, X10DRi

    Affected functions:

    Validation :
        1.Please run Redfish Automation Tool again.

6.
    Category: Fix
    Description:
        [87663] IPMI --- in Trouble Shooting page, the title should be
        Troubleshooting.

    Impact motherboard:
        X10DRU-i

    Affected functions:

    Validation :
        1.Check Web page of Troubleshooting.

7.
    Category: Fix
    Description:
        [87662] IPMI --- IPMI updated message need to fix.

    Impact motherboard:
        X10DRU-i

    Affected functions:

    Validation :
        1.Update BMC fw and check message.

8.
    Category: Fix
    Description:
        [87657] IPMI --- CD-ROM image page's pop-up window has syntax problem.

    Impact motherboard:
        X10DRU-i

    Affected functions:

    Validation :
        1. Set all setting in CD-ROM correctly.
        2. Press "Save" button.
        3. It should not pop out windows.

9.
    Category: Workaround
    Description:
        [87706] IPMI Web GUI shows an extra line for MAC address

    Impact motherboard:
        X10DRR-PS with AOC-MH25G-B2S2G

    Affected functions:

    Validation :
        1. Check the system information page.
        2. There is no "00:00:00:00:00:00" address.

10.
    Category: Fix
    Description:
       [87714] [IPMI ECO] The help page of iKVM/HTML5 console didn't support multi-language.

    Impact motherboard:
        X10DRW-N

    Affected functions:

    Validation :
        1. Open iKVM/HTML5.
        2. Change the language.
        3. Check the "Help" word is changed or not.
        4. The help page content will keep English until received PM's 299 form.

-------------------------------------------------------------------------------------------
Filename: REDFISH_X10_365.bin  version: 3.65  Date: 12-15-2017
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r33
Redfish/iKVM version       : 1.0.1
Redfish API : Redfish_API_full_list_2017_07_11.xlsx

1.
    Category: Fix
    Description:
        [86447] A2SD1 IPMI sensor reading for PVCC_REF is incorrect.

    Impact motherboard: A2SD1

    Affected functions:

    Validation :
        1. Check the sensors.

-------------------------------------------------------------------------------------------
Filename: REDFISH_X10_364.bin  version: 3.64  Date: 12-14-2017
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r33
Redfish/iKVM version       : 1.0.1
Redfish API : Redfish_API_full_list_2017_07_11.xlsx

1.
    Category: Fix
    Description:
        [86755] [IPMI ECO 3.63] SUM 2.0.1 test fail.
        [86722] [IPMI ECO 3.63] SUM 2.0.1 Test fail.
        [86706] [IPMI ECO] sum test fail.
        [86670] SUM test fails.

    Impact motherboard: All MBs.

    Affected functions:

    Validation :
        1. Run TC215 of SMSTC.

2.
    Category: Fix
    Description:
        [86764] The default alert mail sender name is incorrect.

    Impact motherboard: A2SDV.

    Affected functions:

    Validation :
        1. Send an alert mail without default sender name.
        2. Check the sender: BMCXXXXXXXXX@A2SDV.com.

-------------------------------------------------------------------------------------------
Filename: REDFISH_X10_363.bin  version: 3.63  Date: 12-04-2017
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r33
Redfish/iKVM version       : 1.0.1
Redfish API : Redfish_API_full_list_2017_07_11.xlsx

1.
    Category: Feature
    Description:
        Support NVIDIA V100.

    Impact motherboard:
        MBs used at GPU systems.
    Affected functions:

    Validation :
        1. Installed NVIDIA V100.
        2. Check the sensor page.

2.
    Category: Fix
    Description:
        [84605] [BIOS ECO] No UECC event log in BIOS and IPMI SEL with X10DRWN7.908 BIOS.

    Impact motherboard: X10DRW-NT
    Affected functions:
    Validation :
        1. Generate the UECC event log.
        2. Check the Webgui Event Log page.

3.
    Category: Fix (Workaround)
    Description:
        [86046] IPMI wont detect NVMe hot plugged if OS is up first without any NVMe installed.

    Impact motherboard: X10DRU
    Affected functions:
    Validation :
        1. AC power on the sytem.
        2. Check NVMeSSD web gui if exists.

4.
    Category: Fix
    Description:
        [86156] The help information does not match "LAN Mode Control" page in the IPMIWeb GUI.

    Impact motherboard: A2SDV
    Affected functions:
    Validation :
        1. Check the help page of LAN Mode Control.

5.
    Category: Enhancement
    Description:
        Improvement of multi-language content on the iKVM/HTML5 option menu and submenu.

    Impact motherboard: All MBs
    Affected functions:
    Validation :
        1. Log in web page.
        2. To launch an iKVM over HTML5.
        3. Check the option menu and submenu do not have missing contents.

6.
    Category: Enhancement
    Description:
        Disable MCTP support on Broadcom 3108 FW.
        Now it only supports I2C protocol.

    Impact motherboard: All MBs with 3108 storage controller
    Affected functions:
    Validation :
        1. Please use LSI card FW which supports I2C protocol(4.680.00-8290).
        2. Check if AOC SAS temp sensor exists.

---------------------------------------------------------------------------
Filename: REDFISH_X10_362.bin  version: 3.62  Date: 10-26-2017
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r33
Redfish/iKVM version       : 1.0.1
Redfish API : Redfish_API_full_list_2017_07_11.xlsx

1.
    Category: Fix
    Description:
        [83507] Change IPMI LAN mode fail by SMSTC.

    Impact motherboard: A2SDV
    Affected functions:
    Validation :
        1. Run SMSTC test.

2.
    Category: Fix
    Description:
        [83231] A2SDV-NE008 is not support IPMI Dedicate LAN and should be remove Dedicate LAN item in IPMI Network page.

    Impact motherboard: A2SDV
    Affected functions:
    Validation :
        1. Check Network page.
        2. It should only have share NIC.

3.
    Category: Fix
    Description:
        [70838][AOC-MHFI-i1C] No 100G Temperature Sensor Reading in IPMI Web.

    Impact motherboard: X10DRT-PS
    Affected functions:
    Validation :
        1. Insert AOC-MHFI-i1C into the system.
        2. Reboot the system and check the AOC_NIC_Temp.

4.
    Category: Fix
    Description:
        [84276] SUM "Test_case_215 Outband - ChangeBmcCfg and compare" fail.

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Run #215 by using the latest SUM version.

5.
    Category: Fix
    Description:
        [84774] P100 IPMI Temperature Threshold Incorrect  IPMI; GPU.

    Impact motherboard: X10DRG-O
    Affected functions:
    Validation :
        1. Please unselect the preserved SDRs during BMC FW is updated.

6.
    Category: Fix
    Description:
        [84935] IPMI - Cannot disable LDAP Authentication immediately after Enable it.

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Enable the LDAP in the LDAP page.
        2. Disable the LDAP in the LDAP page.
        3. It should not pop out warning message.

---------------------------------------------------------------------------
Filename: REDFISH_X10_361.bin  version: 3.61  Date: 08-21-2017
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r33
Redfish/iKVM version       : 1.0.1
Redfish API : Redfish_API_full_list_2017_07_11.xlsx

1.
    Category: Fix
    Description:
        [82590] FAN PWM check fail.

    Impact motherboard: A2SDV
    Affected functions:
    Validation :
        1. Check memory sensor reading.

2.
    Category: Fix
    Description:
        [Redfish] Incorrect product serial number

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Write product serial number into FRU with more that 15 characters through ipmicfg.
        2. Check the product serial number from web/redfish, it should be right.
3.
    Category: Fix
    Description:
        [83230] VLAN function is fail.

    Impact motherboard: A2SDV
    Affected functions:
    Validation :
        1. Set the VLAN function.

-------------------------------------------------------------------------------
Filename: REDFISH_X10_360.bin  version: 3.60  Date: 07-28-2017
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r33
Redfish/iKVM version       : 1.0.1
Redfish API : Redfish_API_full_list_2017_07_11.xlsx

1.
    Category: Enhancement
    Description:
        Support IERR event log.

    Impact motherboard: X10SRW-F
    Affected functions:
    Validation :
        1. Trigger Cat Error function.
        2. Check the event log.

2.
    Category: Fix (HW Workaround)
    Description:
        [81992] IPMI temperature check is failing.

    Impact motherboard: A2SDV
    Affected functions:
    Validation :
        1. Check the System Temp value.

3.
    Category: Fix
    Description:
        [80990] [SUM v1.7.0] Run Full Mode is FAIL

    Impact motherboard: X10SL7
    Affected functions:
    Validation :
        1. Run SUM test.

4.
    Category: Fix
    Description:
        [82533] There's no CPU Vcore and DIMM temperature sensor reading on IPMI Web.

    Impact motherboard: A2SDV
    Affected functions:
    Validation :
        1. It should have Vcpu sensor.

-------------------------------------------------------------------------------
Filename: REDFISH_X10_359.bin  version: 3.59  Date: 06-30-2017
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r33
Redfish/iKVM version       : 1.0.1
Redfish API : Redfish_API_full_list_2017_06_07.xlsx

1.
    Category: Fix
    Description:
        [81049] [BIOS A2SDICH7.518 ECO] LAN MAC address somtimes will be cleared during run SUM test

    Impact motherboard: A2SDI
    Affected functions:
    Validation :
        1. Run SUM test and check LAN MAC address.

2.
    Category: Fix
    Description:
        [80490] Change [BIOS ECO 1.2a] VBAT / PS status is displayed incorrectly in IPMI sensor readings

    Impact motherboard: A1SA2
    Affected functions:
    Validation :
        1. Check VBAT sensor reading.

-------------------------------------------------------------------------------
Filename: REDFISH_X10_358.bin  version: 3.58  Date: 06-09-2017
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r33
Redfish/iKVM version       : 1.0.1
Redfish API : Redfish_API_full_list_2017_06_07.xlsx

1.
    Category: Enhancement
    Description:
        Change the license requirement of web GUI syslog from DCMS to OOB

    Impact motherboard: All
    Affected functions:
    Validation :
        1. web --> Configuration --> Syslog, should not be available for use
        2. enable OOB license
        3. web --> Configuration --> Syslog, should be available for use
        4. diable OOB license and enable DCMS license
        5. web --> Configuration --> Syslog, should be available for use
-------------------------------------------------------------------------------
Filename: REDFISH_X10_357.bin  version: 3.57  Date: 06-07-2017
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r33
Redfish/iKVM version       : 1.0.1
Redfish API : Redfish_API_full_list_2017_06_07.xlsx

1.
    Category: Feature
    Description:
        [Redfish] Patch an empty json payload "{}" to those APIs support PATCH,
        a 204 http status code will be responded, while to those not support PATCH,
        a 405 http status code will be responded.

    Impact motherboard:
        All MBs
    Affected functions:
        Redfish PATCH for different APIs
    Validation :
        1. Please refer the file "Redfish_API_full_list_2017_06_07.xlsx" and patch
           an empty json payload, "{}", to each API to check http status code.

2.
    Category: Feature
    Description:
        [Redfish] Nest ICANN domain in "Oem" part if there is data to show

    Impact motherboard:
        All MBs
    Affected functions:
        Redfish "Oem" parts
    Validation :
        1. Check Redfish APIs response with "Oem" key, when there is data
           inside, a ICANN domain name (e.g. Supermicro) is nested as a middle
           json payload container

3.
    Category: Fixes
    Description:
        Secondary NTP server becomes empty after restore to default.

    Impact motherboard:
        All MBs
    Affected functions:
        NTP
    Validation :
        1. Restore BMC to default
        2. Both Primary and Secondary NTP server in Date and Time page should
           not be empty.

4.
    Category: Enhancement
    Description:
        Redfish API rename:
        /redfish/v1/UpdateService/SSL -> /redfish/v1/UpdateService/SSLCert
        /redfish/v1/UpdateService/SSL/Actions/SSL.Upload -> /redfish/v1/UpdateService/SSLCert/Actions/SSLCert.Upload

    Impact motherboard: All
    Affected functions:
    Validation :
        Check Redfish APIs' URI of SSL related

5.
    Category: Fixes
    Description:
        [80837] IPMI FW 3.56: Unable to handle SMTP Port Number correctly

    Impact motherboard:
        All MBs
    Affected functions:
        SMTP
    Validation :
        1. Go to SMTP tab in WEB
        2. Input floating number and string in "SMTP port"

6.
    Category: Fixes
    Description:
        [80838] IPMI FW 3.56: Unexpected alert when changing date and time settings

    Impact motherboard:
        All MBs
    Affected functions:
        NTP
    Validation :
        1. Go to Date and Time
        2. Disable NTP
        3. Change current month to a future month (i.e. from June change to July)
        4. Click Save

7.
    Category: Fixes
    Description:
        [80839] IPMI FW 3.56: Operator level access can reset iKVM

    Impact motherboard:
        All MBs
    Affected functions:
        Reset iKVM over WEB
    Validation :
        1. Login web page with operator privilege level
        2. Go to IKVM Reset Tab under Maintenance to check if "Reset" button is disabled

-------------------------------------------------------------------------------
Filename: REDFISH_X10_356.bin  version: 3.56  Date: 05-24-2017
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r33
Redfish/iKVM version       : 1.0.1
Redfish API : Redfish_API_full_list_2017_04_26.xlsx

1.
    Category: Enhancement
    Description:
        Reduce the action to reset OOB interface of Broadcom 3108 RAID controller

    Impact motherboard:
        All MBs with AOC-3108 or on board 3108 chip
    Affected functions:
        All RAID functions related to 3108
    Validation :
        1. Install a AOC-3108 on the MB(or a MB with on board 3108)
        2. Update 3108 ROM by this reposity:
               \\rdlab-fs\driver\LSI\SAS\3108\Current_Test\MR6.13_GCA_011717\FW
        3. Verify all the functions related to 3108 to check if there is error happens
        4. Finally run cburn AC ON/OFF test as long as you can to check if there is HDD lost in OS environment

2.
    Category: Fixes
    Description:
        System installed with 3108 AOC then run cburn ON/OFF test:
            1. Cause system hang at POST stage (and IERR happens)
            2. Some affiliated HDDs within 3108 will be lost(disk drop)

    Impact motherboard:
        All motherboard which support LSI 3108 card.
        MCTP protocol are needed to be supported by the bios.

    Affected functions:
    Validation :
        1. Insert LSI 3108 card
        2. Run cburn ON/OFF test, it will automatically check:
           2-1. System hang at POST stage (and IERR happens)
           2-2. The drives lost or not
           (If you don't know how to run this verification, please contact Joe Chung(in US))

3.
    Category: Enhancement
    Description:
        Fix security vulnerability (NTP mode 6 scanner)

    Impact motherboard: All
    Affected functions:
     Validation :
        1. Please do factory default.
        2. Enable NTP in Date and Time page.
        3. Run Nessus. NTP mode 6 scanner issue should not be in test report.

-------------------------------------------------------------------------------
Filename: REDFISH_X10_355.bin  version: 3.55  Date: 05-23-2017
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r33
Redfish/iKVM version :  1.0.1
Redfish API : Redfish_API_full_list_2017_04_26.xlsx

1.
    Category: Feature
    Description:
        Crash Dump: filter out false alarm CATERR.
    Impact motherboard: All
    Affected functions:
    Validation :
        1. Enter web GUI, Micellaneous --> Trouble Shooting
        2. Click 'Dump' button.
        3. Check SEL, there shouldn't display 'IERR' log
        4. ipmitool -H $YOUR_IP -U ADMIN -P ADMIN raw 0x3E 0x21
        5. Check SEL, there shouldn't display 'IERR' log

2.
    Category: Fixes
    Description:
        [79941] [ RedFish ] Not enough information for POST Storage.CreateVolume.
    Impact motherboard:
        All motherboards

    Affected functions:
     Validation :
        1. Check the content by https://$YOUR_IP/redfish/v1/Systems/1/Storage/HA-RAID/Actions/Oem/Storage.CreateVolume

3.
    Category: Fixes
    Description:
        [79710] IPMI unable to handle uppercase IPv6 Address

    Impact motherboard: All
    Affected functions:
     Validation :
       1. Go to Configuration -> Network, IPv6 Settings:
       2. Enter "0::FFFF:AC3F:2009/64" (be sure is in Uppercase) in IPv6 Address
       3. Click "Save"
       4. After saving, Click "Refresh" (inside IPMI, not the browser)
       5. Select "0:0:0:0:0:ffff:ac3f:2009/64" in the address list
       6. Select "Delete IP"
       7. Click "Save" and then "Refresh", the IP should not be in the address list.

4.
    Category: Fixes
    Description:
        [80231] POST action on /redfish/v1/UpdateService/SSL should not be allowed

    Impact motherboard: All
    Affected functions:
    Validation :
        1. POST a request on URI which doesn't support POST then check if BMC will reply error code to stop this illegal access

5.
    Category: Fixes
    Description:
        [80107] Duplicate MAC address shown in IPMI Web GUI.
    Impact motherboard:
        X10DRT-PS

    Affected functions:
     Validation :
        1. Login in the BMC web gui and check the system mac address.

6.
    Category: Fixes
    Description:
        [79983] IPMI SEL DIMM location is not meet MB silkscreen.
    Impact motherboard:
        X10SLM-F

    Affected functions:
     Validation :
        1. Lanuch the memory ecc err command.
        2. Check the wording on the sel log web gui.

7.
    Category: Fixes
    Description:
      [CRM SM1705014348]  Supermicro Case#SM1705014348

    Impact motherboard: SYS-6028UX-TR4
    Affected functions:
    Validation :
        1.Enter SMASH-CLP shell by operator privilege.
        2.Resst the host by "reset system1/pwrmgtsvc1".
        3.The action can be executed.

-------------------------------------------------------------------------------
Filename: REDFISH_X10_354.bin  version: 3.54  Date: 05-08-2017
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r33
Redfish/iKVM version :  1.0.1
Redfish API : Redfish_API_full_list_2017_04_26.xlsx

1.
    Category: Fixes
    Description:
        [79799] SUM Test failed
        [79797] SUM Test failed
        [79792] [Redfish v3.53 firmware ECO] Failed to run SUM ECO tests
    Impact motherboard: All
    Affected functions:
     Validation :
        1. Run SUM tests.

2.
    Category: Fixes
    Description:
        [79587] BIOS/IPMI SEL DIMM location is not meet MB silkscreen.
    Impact motherboard: All motherboards with one CPU is supported.
    Affected functions:
     Validation :
        1. Lanuch bios memory err command. (Failing DIMM: DIMM location).
        2. Check the wording.

-------------------------------------------------------------------------------
Filename: REDFISH_X10_353.bin  version: 3.53  Date: 05-03-2017
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r35
Redfish/iKVM version :  1.0.1
Redfish API : Redfish_API_full_list_2017_04_26.xlsx

1.
    Category: Feature
    Description:
        Redfish support new APIs

    Impact motherboard: all
    Affected functions:
    Validation :
        1. Valid on DCMS license only
        2. Check out the following APIs (including "actions"):
            /redfish/v1/Chassis/HA-RAID.[contoller_num].StorageEnclosure.[enclosure_num]/Drives/Disk.Bay.[disk_num]/Actions/Oem/Drive.Indicate (For 3108, Light on respective physical drive LED)

            /redfish/v1/Systems/1/Storage/HA-RAID/HA-RAID.[contoller_num].Volumes/[volume_num]/Actions/Oem/Volume.Indicate (For 3108, Light on respective logical drive LED)
            /redfish/v1/Systems/1/Storage/HA-RAID/HA-RAID.[contoller_num].Volumes/[volume_num]/Actions/Oem/Volume.Delete (For 3108, Delete specific logical drive)
            /redfish/v1/Systems/1/Storage/HA-RAID/Actions/Oem/Storage.CreateVolume (For 3108, Create logical drive against specific RAID controller)
            /redfish/v1/Systems/1/Storage/HA-RAID/Actions/Oem/Storage.ClearVolumes (For 3108, Clear all logical dirves against specific RAID controller)
            /redfish/v1/Systems/1/Storage/HA-RAID/Actions/Oem/HARAIDController.Save (For 3108, Save specific RAID controller's BIOS boot mode)

            /redfish/v1/Managers/1/VM1/CfgCD (Configure ISO image settings: host, path, username and password)
            /redfish/v1/Managers/1/VM1/CfgCD/Actions/IsoConfig.Mount (Do mount ISO image)
            /redfish/v1/Managers/1/VM1/CfgCD/Actions/IsoConfig.UnMount (Do unmount ISO image)

            /redfish/v1/Managers/1/IKVM (get a URL link to launch an iKVM over HTML5)

            /redfish/v1/UpdateService/SSL (view current SSL certification information)
            /redfish/v1/UpdateService/SSL/Actions/SSL.Upload (used to upload new SSL certification file)

2.
    Category: Fixes
    Description:
        [79065] Failed to eject NVMeSSD

    Impact motherboard: X10SRM-F
    Affected functions:
     Validation :
        1. Insert NVMe drives.
        2. Eject NVMe drive on NVMe web gui.
        3. Pull out the NVMe drive.
        4. Check the ejected event log on sel web gui.
        5. Plug in the drive.
        6. Insert the NVMe drive.
        7. Check the inserted event log on sel web gui.

3.
    Category: Fixes
    Description:
        [79016] VDIMM/PVNN/PVCC_REF sensor readings are in "NC" state.

    Impact motherboard: A2SDI-H-TP4F
    Affected functions:
     Validation :
        1. Update and remove old SDR.
        2. Check the threshold of VDIMM/PVNN/PVCC_REF sensor.

4.
   Category: Fixes
   Description:
       When you select French keyboard layout, there some digits keys don't work.

   Impact motherboard: all
   Affected functions:
   Validation :
       1. launch java remote console.
       2. select French keyboard layout in option menu
       3. test all keys

5.
   Category: Fixes
   Description:
       System hang during POST with IERR errors when using 3108 AOC

   Impact motherboard: all motherboard which support LSI 3108 card.
                       MCTP protocol are needed to be supported by the bios.
   Affected functions:
   Validation :
       1. Insert LSI 3108 card.
       2. Do system DC on/off test over 12 hours.
       3. Check if the system hang.

6.
   Category: New Feature
   Description:
       Download caterr dump data for TS team to analyza

   Impact motherboard: All

   Affected functions:
   Validation :
       1. Lanuch IERR function.
       2. Try to download caterr dump data by smcipmitool.
          SMCIPMITOOL.exe 10.133.176.184 ADMIN ADMIN ipmi oem gerneralfiledownload 19 c:\caterr.raw.
       3. Consult with TS team to process this raw data.

7.
   Category: Fixed
   Description:
       Work in with Broadcom's suggestion, 3108 controller will abandon the way on MCTP-over-PCIe

   Impact motherboard: All with 3108 controller

   Affected functions:
   Validation :
       1. Please contact with Chassis team's Farid or Manju to get respective
          I2C-versioned 3108's ROM and flash your testing 3108 with this ROM.
          Then check if it is workable.
       2. Please update 3108's ROM with the MCTP-over-PCIe version, basically,
          BMC will not recognize and of course won't managet it.

-------------------------------------------------------------------------------
Filename: REDFISH_X10_352.bin  version: 3.52  Date: 03-31-2017
Support Motherboard: All X10 MBs
U-Boot build time : 2008.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r33
Redfish/iKVM version :  1.0.1

1.
    Category: Fixes
    Description:
        [78034] [SUM 1.7.0(2017/02/02)] Test "UpdateRaidController" was failed.(ExitCode: 38)

    Impact motherboard: X10DRG-Q
    Affected functions:
     Validation :
        1. Run SUM UpdateRaidController command to update 3108 rom.
        2. Check the result.
2.
    Category: Enhancement
    Description:
        Upgrade NTP package to 4.2.8p9 for security issue CVE-2016-7434, Ref

    Impact motherboard: All
    Affected functions:
     Validation :
        1.Enable NTP in Date and Time page.

3.
    Category: Fixes
    Description:
        [72537] No CPU Throttle event in IPMI Event Log page
        [72531] No "CPU Overheat", "thermal Throttling" de-assertion event in
        IPMI Event Log page

    Impact motherboard: A2SDI
    Affected functions:
     Validation :
        1. Heat CPU until thermal trip.
        2. Check SEL, there should be thermal throttling event.

4.
    Category: Fixes
    Description:
        [78419] IPMI Web Session value didn't load default after IPMI Load Factory Default

    Impact motherboard: all
    Affected functions:
     Validation :
        1. Change Web session time and save.
        2. Do factory default commands.
        3. Re-login and check the value.

5.
    Category: Fixes
    Description:
        [77464] CPU Overheat LED function can't work

    Impact motherboard: A2SDI
    Affected functions:
     Validation :
        1. Heat CPU until throttling.
        2. Check overheat led

6.
    Category: Fixes
    Description:
        [78412] The fan RPM fluctuates for the NIC devices

    Impact motherboard: X10DRU-I+
    Affected functions:
     Validation :
        1. Install AOC ards.
        2. Try check the duty cycle of MB_NIC Temp and AOC_NIC Temp
           if they are the same.

7.
    Category: Enhancements
    Description:
        CVE-2003-0001

    Impact motherboard: all
    Affected functions:
     Validation :
        1. download etherleak.pl for issue verification and execute the perl
           script under linux.
        2. issue:
           sudo ./etherleak.pl -i eth1 -f host\ 10.138.160.118
        3. If no CVE-2003-0001 issue, the script will keep waiting and display
           nothing.

8.
    Category: New Feature
    Description:
        Redfish support storage APIs

    Impact motherboard: all
    Affected functions:
    Validation :
        1. Valid on DCMS license only
        2. Check out the following storage APIs:

           /redfish/v1/Systems/1/Storage
           /redfish/v1/Systems/1/Storage/HA-RAID (For Broadcom 3108)
           /redfish/v1/Systems/1/Storage/HA-RAID/HA-RAID.[contoller_num].Volumes (For Broadcom 3108)
           /redfish/v1/Systems/1/Storage/HA-RAID/HA-RAID.[contoller_num].Volumes/[volume_num] (For Broadcom 3108)
           /redfish/v1/Systems/1/Storage/RAIDIntegrated (For RSTe, Must have TAS running)
           /redfish/v1/Systems/1/Storage/RAIDIntegrated/Volumes (For RSTe, Must have TAS running)
           /redfish/v1/Systems/1/Storage/RAIDIntegrated/Volumes/[volume_num] (For RSTe, Must have TAS running)
           /redfish/v1/Systems/1/Storage/SATAEmbedded (For PCH SATA, Must have TAS running)
           /redfish/v1/Systems/1/Storage/SATAEmbedded/Volumes (For PCH SATA, Must have TAS running)
           /redfish/v1/Systems/1/Storage/SATAEmbedded/Volumes/[volume_num] (For PCH SATA, Must have TAS running)

           /redfish/v1/Chassis/HA-RAID.[contoller_num].StorageEnclosure.[enclosure_num] (For Broadcom 3108)
           /redfish/v1/Chassis/HA-RAID.[contoller_num].StorageEnclosure.[enclosure_num]/Drives/Disk.Bay.[disk_num] (For Broadcom 3108)
           /redfish/v1/Chassis/StorageBackplane (For PCH SATA or RSTe, Must have TAS running)
           /redfish/v1/Chassis/StorageBackplane/Drives/Disk.Bay.[disk_num] (For PCH SATA or RSTe, Must have TAS running)
           /redfish/v1/Chassis/NVMeSSD.[pcie_controller_num].Group.[group_num].StorageBackplane.[pcie_controller_num] (For NVMe)
           /redfish/v1/Chassis/NVMeSSD.[pcie_controller_num].Group.[group_num].StorageBackplane.[pcie_controller_num]/Drives/Disk.Bay.[disk_num] (For NVMe)

-------------------------------------------------------------------------------
Filename: REDFISH_X10_351.bin  version: 3.51  Date: 02-15-2017
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r33
Redfish/iKVM version :  1.0.1

1.
    Category: Fix
    Description:
        [74090] SUM test case 409 fail.

    Impact motherboard: X10DRH-CLN4
    Affected functions:
     Validation :
        1. Run SMSTC ECO test.
        2. Check the result.

2.
    Category: Fix
    Description:
        [77407] FAN3 and FANA header FAN fail function can't work
        [76836] IPMI function can't work

    Impact motherboard: A2SDI-H-LN4F
    Affected functions:
    Validation :
        1. Check Fan sensor in sensor page.

3.
    Category: Fix
    Description:
        [76902] eburn stress fail.
        [76854] IPMI FW will be "unknown" after serveral times reboot
		[76848] JD1 function can't work
		[76846] JWD1 jump can't work

    Impact motherboard: A2SDI-H-LN4F
    Affected functions:
    Validation :
        1. Check BMC status in BIOS


-------------------------------------------------------------------------------
Filename: REDFISH_X10_350.bin  version: 3.50  Date: 01-20-2017
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r33
Redfish/iKVM version :  1.0.1

1.
    Category: New Feature
    Description:
        Support new motherboard: A2SDI-H-LN4F

    Impact motherboard: A2SDI-H-LN4F
    Affected functions:
    Validation :
        1. Board ID: 0x0910.

2.
    Category: Fix
    Description:
        [75877] Missing "standard mode" in FSC

    Impact motherboard: X10DRC-LN4+
    Affected functions:
     Validation :
        1.Please do factory default and check default fan mode.

-------------------------------------------------------------------------------
Filename: REDFISH_X10_349.bin  version: 3.49  Date: 12-15-2016
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r33
Redfish/iKVM version :  1.0.1

1.
    Category: Fix
    Description:
        [75875] BIOS diag tool cannot save logs.

    Impact motherboard: All
    Affected functions:
     Validation :
        1. system boot into UEFI mode2. run BIOS diag tool.
        2. run BIOS diag tool.

2.
    Category: New feature
    Description:
        [75759] Micron 7100 NVMe) IPMI (fw: 03.48) is not displaying NVMe temperature correctly.
        [75564] Seagate XF1440 1.92TB NVMe doesn't display temperature in IPMI WebGUI.

    Impact motherboard: Motherboards which support NVMe functions.
    Affected functions:
    Validation :
        1. Install the Seagate/Seagate NVMe Drives.
        2. Check the temp on NVMe SSD page.

3.
    Category: New feature
    Description:
        [75460] IPv6: Sensor data can't be retrieved by iReasoning MIB Browser (SNMP).

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Lanuch iReasoning MIB Browser.
        2. Retrieve sensor data.

4.
    Category: Fix
    Description:
        [47976] [ SUM 1.7.0 ] SUM test fail.

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Run test case #215

5.
    Category: Fix
    Description:
        [MCTP] When using IPMI storage monitoring feature to crate Raid volume with "No Read
        Ahead" settting, MSM still showing Raid volume setting as "Always Read Aheard"

    Impact motherboard: Those installed with LSI3108 controller
    Affected functions:
        LSI3108 create RAID via WEB UI
    Validation :
        Create RAID drives via "Storage monitoring" on LSI3108 and open MSM to check

6.
    Category: New feature
    Description:
        NVMe event log when plugged in or pulled out

    Impact motherboard: All
    Affected functions:
    Validation :
        1.Plug NVMe drives and power on the machine.
        2.Press Eject/Insert function on NVMe web gui and wait for success message is received.
        3.Check event log.


-------------------------------------------------------------------------------
Filename: REDFISH_X10_348.bin  version: 3.48  Date: 11-xx-2016
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r31
Redfish/iKVM version :  1.0.1

1.
    Category: New feature
    Description:
        Support SEL Almost Full log (75%) and SEL Full log (99%).

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Generate a lot of logs.
        2. Check the "Event Logging Disabled" SELs are recorded.

2.
    Category: Fix
    Description:
        [75082] [BIOS ECO v2.0a]SUM test fail.
        [75025] [SUM 1.6.1]: Unable to change BMC configuration file by OutBand/InBand command.

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Run the SUM Test: TC_214, TC_215, and TC_313.
        2. They should be all pass.

3.
    Category: Fix
    Description:
        [75041] Redfish automation - 9 fails.

    Impact motherboard: X10QBi
    Affected functions:
    Validation :
        1. Run the Redfish automation test.
        2. They should be all pass.

4.
    Category: New feature
    Description:
        Support Pascal P4 GPU

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Install Pascal P4 GPU.
        2. Check the GPU temperature.

5.
    Category: New feature
    Description:
        Support save BIOS diag file into BMC by OOB command.

    Impact motherboard: All
    Affected functions:
    Validation :
        1. run BIOS diag tool.

6.
    Category: Fix
    Description:
        [74689] (Micron PCI9100 NVMe) IPMI (fw:03.47) is not displaying NVMe temperature correctly.

    Impact motherboard: X10DRU-i+
    Affected functions:
    Validation :
        1. Install the Micron PCI9100 NVMe.
        2. Check PCIe SSD page.

7.
    Category: Fix
    Description:
        Standard mode is missing on X10DRC

    Impact motherboard: X10DRC
    Affected functions:
    Validation :
        1. Check the fan mode

-------------------------------------------------------------------------------
Filename: REDFISH_X10_347.bin  version: 3.47  Date: 11-04-2016
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r31
Redfish/iKVM version :  1.0.1

1.
    Category: Fix
    Description:
        [73627] AOC-2UR68-m2TS No temperature sensor reading on X10DRU-i+

    Impact motherboard: X10DRU-I+
    Affected functions:
    Validation :
        1. Check NIC temp if exists
        2. Insert LSI3108, AOC card or GPU and check the related temps if exists

2.
    category: Fix
    Description:
        [74284][Red Fish] Powersupply status is absent but health condition show "ok"

    Impact motherboard: All
    Affected functions:
    Validation :
        1. connect to redfish/v1/Chassis/1/Power to check power supply status

3.
    category: Fix
    Description:
        Power consumptio reading is missing during with 'ipmitool' command.

    Impact motherboard: X10DRU-I+
    Affected functions:
    Validation :
        1.AC Power on the system
        2.Use 0x30 0xE2 commands to get power reading value if it not zero

-------------------------------------------------------------------------------
Filename: REDFISH_X10_346.bin  version: 3.46  Date: 10-14-2016
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r31
Redfish/iKVM version :  1.0.1

Note: This version is for X10SDV series motherboard

1.
    Category: Fix
    Description:
        [74203] [BIOS ECO 1.1c] NM function is not workable.
        [74192] [BIOS ECO 1.1c] NM function is not workable.

    Impact motherboard: X10SDV
    Affected functions:
    Validation :
        1. Use SMCIPMITool nm20 command.

-------------------------------------------------------------------------------
Filename: REDFISH_X10_345.bin  version: 3.45  Date: 09-19-2016
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r31
Redfish/iKVM version :  1.0.1

1.
    Category: Fix
    Description:
        [73219] Fans do not spin up when GPU temperature rises,
        causing GPU overheat when stressing only the GPU

    Impact motherboard: X10DRT-P
    Affected functions:
    Validation :
        1. Insert GPUs
        2. Heat GPU and check if fan speed rises accordingly

2.
    Category: Fix
    Description:
        [72782] SUM 1.6.1(2016/07/06) Test fail.
        [72493] SUM v1.6.1(2016/07/06) fail via smstc.

    Impact motherboard: X10QBi
    Affected functions:
    Validation :
        1. Run TC_212, 219, 229
        2. Check the result is pass.
3.
    Category: Fix
    Description:
        [72204] [IPMI] The console windows will jump from background to foreground when a character arrives on the screen.

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Lunch the iKVM viewer
        2. Check the behavior of iKVM viewer

4.
    Category: Fix
    Description:
        [72560] IPMI "BIOS Update" function is fail
        [72497] BIOS update fail by IPMI WebGUI

    Impact motherboard: A2SDI-H-TP4F, A2SDI-TP8F
    Affected functions:
    Validation :
        1. Update bios from bios update page.
        2. Check if bios update successful.

5.
    Category: Fix
    Description:
        [71429] Fan Pulse-Width-Modulation Measurement fail

    Impact motherboard: A2SDI-H-TP4F
    Affected functions:
    Validation :
        1. Check 10G LAN temp sensor should show up in sensor readings page.

6.
    Category: Fix
    Description:
        [72559] IPMI "iKVM Reset" function is fail

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Insert USB stick into USB port.
        2. Do iKVM reset.
        3. iKVM should be reset and iKVM function should work after reset.

-----------------------------------------------------------------
Filename: REDFISH_X10_344.bin  version: 3.44  Date: 08-18-2016
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r27
Redfish/iKVM version :  1.0.1

1.
    Category: Fix
    Description:
      Support on board NVMe

    Impact motherboard: X10DRD, X10DRD_L
    Affected functions:
    Validation :
        1. Insert NVMe drives.
        2. Check the NVMe web gui.

2.
    Category: Fix
    Description:
        [68370] No Thermal Trip event.

    Impact motherboard: X10SLA-F
    Affected functions:
    Validation :
        1. Heat the CPU to shutdown.
        2. Check the event log.

3.
    Category: Fix
    Description:
        Sensor will show "N/A" forever at cburn AC on/off test

    Impact motherboard: X10SRI
    Affected functions:
    Validation :
        1. Do curn AC On/Off test
        2. Check sensor reading web gui

-----------------------------------------------------------------
Filename: REDFISH_X10_343.bin  version: 3.43  Date: 08-xx-2016
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r27
Redfish/iKVM version :  1.0.1

1.
    Category: Fix
    Description:
      [72948] [1U TwinPro] FAN2 and FAN3 always in FAN FAIL state after updating BMC FW to 3.40+

    Impact motherboard: X10DRT-P (1U TwinPro)
    Affected functions:
    Validation :
        1. Check the sensor list page.

-----------------------------------------------------------------
Filename: REDFISH_X10_342.bin  version: 3.42  Date: 08-04-2016
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r27
Redfish/iKVM version :  1.0.1

1.
    Category: Fix
    Description:
      [72537] No CPU Throttle event in IPMI Event Log page

    Impact motherboard: A2SDI-LN4F, A2SDR-TP8F
    Affected functions:
    Validation :
        1. heat the CPU up

2.
    Category: Fix
    Description:
      [72720] VDIMM from E to H reporting upper non-recoverable

    Impact motherboard: X10DRG-O
    Affected functions:
    Validation :
        1. Check VDIMMEF, VDIMMGH senosr status when CPU2 is not inserted

3.
    Category: Enhancement
    Description:
      [72682] When Chassis Intru trigger, Chassis Intru will be reseted automatically after system AC off/on

    Impact motherboard: X10SDV
    Affected functions:
    Validation :
        1. Lanuch chassis intrusion
        2. AC off/on the system
        3. Check the chassis sensor if the state keeps at chassis intrusion

4.
    Category: Fix
    Description:
        [68570]  "VM mount ISO failed when enter ipv6 as sharehost"
        VM fail to mount ISO file in WebGUI when fill in ipv6 address instead of ipv4  address in the sharehost text box
    Impact Motherboard: X10 motherboards
    Affected functions:
    Validation :
        1. mount ISO file in WebGUI with ipv4 address as sharehost
        2. check and confirm ISO file mounted successfully
        3. unmounts ISO file and change ipv4 address to ipv6 address for the same file host
        4. the same ISO file mount will fail

5.
    Category: Fix
    Description:
      [72356] Should be remove "Share LAN" item in Network page

    Impact motherboard: X10SDV-4C-TLN2BF
    Affected functions:
    Validation :
        1. Please do 0x30 0x41 command aftre FW is updated
        2. Check the IPMI network setting web gui
        3. Check LAN Interface of network web gui. It should be "dedicate"

-----------------------------------------------------------------
Filename: REDFISH_X10_341.bin  version: 3.41  Date: 07-26-2016
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r27
Redfish/iKVM version :  1.0.1

1.
    Category: Fix
    Description:
      [70007] Jumper JL1 function test fail.
      [72495] Chassis Intru is not present in Sensor reading page

    Impact motherboard: A2SDI-LN4F, A2SDR-TP8F
    Affected functions:
    Validation :
        1. Power on the system and boot into the OS.
        2. Check the Sensor reading page.
        3. Chassis Intru should be present.

2.
    Category: HW Workaround
    Description:
      [70604] No CPU Throttle and Thermal Trip Event log in IPMI Web when Thermal trip event occur.

    Impact motherboard: X10QBL
    Affected functions:
    Validation :
        1. Triger thermal trip.
        2. Check the SEL.
        3. Power off the system.
        4. Make sure there is no Thermal trip SEL.

3.
    Category: Fix
    Description:
      [71206] [IPMI ECO] Nvidia M4 GPU sensor Missing in IPMI

    Impact motherboard: X10DRC-LN4+-P,X10DRC-T4+-P
    Affected functions:
    Validation :
        1. Check GPU sensors can be detected at slot 3 or slot 5

4.
    Category: HW Workaround
    Description:
      Disable PROC_HOT function

    Impact motherboard: X10SLA
    Affected functions:
    Validation :
        1. There should be no any Automatically throttled SEL.

6.
    Category: New Feature
    Description:
      AOC-2UR66-i4XTF no temperature reading

    Impact motherboard: X10DRU-I
    Affected functions:
    Validation :
        1. Check on board LAN sensor temperature

7.
    Category: Fix
    Description:
      [72512] CPU1 Temp and CPU2 will frequently show N/A while in OS with IPMI

    Impact motherboard: X10DRG-O with X10DRG-O-PCIE board
    Affected functions:
    Validation :
        1. Fully populated 10 GPU sensors
        2. Check sensor status frequently

-----------------------------------------------------------------
Filename: REDFISH_X10_340.bin  version: 3.40 Date: 07-15-2016
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r27
Redfish/iKVM version :  1.0.1

1.
    Category: Fix
    Description:
      [71982] The MAC quantity returned by IPMI
              OEM command are not match IPMI web site

    Impact motherboard: X10SDV-2C-TP8F
    Affected functions:
    Validation :
        1. Use 0x30 0x9f commands. It should return over 73 Bytes

2.
    Category: Fix
    Description:
      [72268] FAN mode default optimal mode on dual cooling zone motherboard

    Impact motherboard: X10SDV-8C-TLN4F+
    Affected functions:
    Validation :
        1. Do factory default acation and check Fan default mode

3.
    Category: New Feature
    Description:
      [72356] IPMI only sees 8 GPU instead of 10
      [72211] [X10DRG-O-PCIe] GPU Sensor readings are not in the correct order

    Impact motherboard: X10DRG-O with X10 PCIE board
    Affected functions:
    Validation :
        1. Install GPUs on PCIE board.
        2. Please check the mapping between GPU number and slot number
           Slot 1  -> GPU1
           Slot 2  -> GPU2
           Slot 3  -> GPU3
           Slot 4  -> GPU4
           Slot 5  -> GPU5
           Slot 8  -> GPU6
           Slot 9  -> GPU7
           Slot 10 -> GPU8
           Slot 11 -> GPU9
           Slot 12 -> GPU10

4.
    Category: New Feature
    Description:
      [72340] AOC-UR-i4XTF no temperature reading

    Impact motherboard: X10DRU-I
    Affected functions:
    Validation :
        1. Check on board LAN sensor temperature

-----------------------------------------------------------------
Filename: REDFISH_X10_339.bin  version: 3.39 Date: 07-06-2016
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r27
Redfish/iKVM version :  1.0.1

1.
    Category: HW workaround
    Description:
      [72239] 5V dual is lower critical
      [72238] 5V dual is lower critical
      [72115] FAN mode didn't show optimal mode
      [72058] No FAN-A reading


    Impact motherboard: X10SDV-xxC-TLN4F+, X10SDV-4C-TLN2BF
    Affected functions:
    Validation :
        1. Please confirm HW if GPIOH2 and GPIOH3 are reworked
        2. Check sensor reading web gui

2.
    Category: Fix
    Description:
      [70765] Fan PWM fail (The IPMI sensor show LAN 1G(I350) temperature, but
      when I350 temperature rises, the fan speed does not increase.)

    Impact motherboard: A2SDI
    Affected functions:
    Validation :
        1. No support temperature for I350, remove 1G temp from SDR.

3.
    Category: Hardware Workaround
    Description:
      Change the Thermal trip to low-level triggered.
      Remove the PROC_HOT and use Upper Ctritial to control the OH LED and Buzzer.

    Impact motherboard: X10QBL
    Affected functions:
    Validation :
        1. Make CPUs hot and check the OH LED, Buzzer.
        2. Make sure there are no Automatically Throttled SEL.
        3. Make the CPU hot enough and make system shutdown.
        4. Check the Thermal trip SEL.

-----------------------------------------------------------------
Filename: REDFISH_X10_338.bin  version: 3.38 Date: 06-27-2016
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r27
Redfish/iKVM version :  1.0.1

1.
    Category: Workaround solution
    Description:
      IPMI solution for M40 leakage on GPU systems

    Impact motherboard: X10DRG-Q, X10DRG-H, X10DRG-O, X10SRG
    Affected functions:
    Validation :
    1)
        1. MB Boot Feature  ¡§Restore on AC Power Loss¡¨ set to ¡§Stay Off¡¨
                2. AC and PS on/off
                3. Interrupt IPMI Initialization, press and hold PSON button to
                   force system shut down. Measure 3.3V.
    2)
        1. MB Boot Feature  ¡§Restore on AC Power Loss¡¨ set to ¡§Last State¡¨
                2. AC and PS on/off
                3. IInterrupt IPMI Initialization (tested @20s, 30s, 40s, 50s),
                   press and hold PSON button to force system shut down. Measure 3.3V.

    Measure B12 pin. On the left side 12th pin of PCIE connector.

2.
    Category: Fix
    Description:
      [71214] No UID control

    Impact motherboard: X10DRI Rev1.02B
    Affected functions:
    Validation :
        1. Check UID web gui if exists
-----------------------------------------------------------------
Filename: REDFISH_X10_337.bin  version: 3.37  Date: 06-20-2016
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r27
Redfish/iKVM version :  1.0.1

1.
    Category: Fix
    Description:
      [71214] PERR/SERR sensor name not consistant

    Impact motherboard: X10DSC-TP4S
    Affected functions:
    Validation :
        1. Launch SMCIPMIView and send PERR/SERR event
        2. Check trap content in SMCIPMIView
        3. Compare the format if the same as event log IPMI web page

2.
    Category: Hardware Work Around
    Description:
      Adjust the CPU VRM register 0xe8 value to 0x12

    Impact motherboard: X10DRI Rev1.02B
    Affected functions:
    Validation :
        1. Check the CPU VRM 0xe8 register value.

3.
    Category: Fix
    Description:
      [70604] No CPU Throttle and Thermal Trip Event log in IPMI Web when Thermal trip event occur.

    Impact motherboard: X10QBL
    Affected functions:
    Validation :
        1. Triger thermal trip.
        2. Check the SEL.
        3. Power off the system.
        4. Make sure there is no Thermal trip SEL.

4.
    Category: New motherboard support
    Description:
      [71725] NM function is fail and show not support Node Management
      [71716] Peripheral Temp, MB_10G Temp reading is "N/A" in IPMI Sensor Reading page
      [71715] No "FANA" sensor in IPMI Sensor Reading page

    Impact motherboard: X10SDV-12C-TLN4F+-
    Affected functions:
    Validation :
        1. Updating BMC FW and do 0x30 0x40 command
        2. Check sensor reading web gui
        3. Chekc NM function

5.
    Category: Fix
    Description:
      [71429] Fan Pulse-Width-Modulation Measurement fail for A2SDI

    Impact motherboard: A2SDI
    Affected functions:
    Validation :
        1. Optimal mode and heavy IO mode are available in fan mode page.

6.
    Category: Fix
    Description:
      [70765] Fan PWM fail (The IPMI LAN 10G temperature sensor display is not
      X557(10G), this is not correct.)

    Impact motherboard: A2SDI
    Affected functions:
    Validation :
        1. 10G and 1G LAN temp are switched in previous release. Corrected in
        this version.

-----------------------------------------------------------------
Filename: REDFISH_X10_336.bin  version: 3.36  Date: 05-27-2016
Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r27
Redfish/iKVM version :  1.0.1

1.
    Category: Enhancement
    Description:
      iKVM/HTML5 is hidden on 3.35

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Check this funciton is enable

2.
    Category: Fix
    Description:
      [70663] SD5 missing BPN2 temp

    Impact motherboard: X10DSC-TP4S
    Affected functions:
    Validation :
        1. Check BPN2 senosr number is unique

-----------------------------------------------------------------
Filename: REDFISH_X10_335.bin  version: 3.35  Date: 05-26-2016

Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r27
Redfish/iKVM version :  1.0.1

1.
    Category: New Feature
    Description:
      [70454] AOC-MHIBF-2QG] No IB Temperature Sensor Reading in

    Impact motherboard: X10DRT-PS
    Affected functions:
    Validation :
        1. Insert AOC IB card
        2. Power on the system and check sensors

2.
    Category: Fix
    Description:
      [71206] [IPMI ECO] Nvidia M4 GPU sensor Missing in IPMI.

    Impact motherboard: X10DRC
    Affected functions:
    Validation :
        1. Install an Nvidia M4 GPU onto the system.
        2. Check the sensor list.

3.
    Category: Fix
    Description:
      [71198] IPMI FW 3.33 not showing NVMe drive information after
        hot inserted. System reboot is required in order to show the information
    Impact motherboard: All X10 motherboards which support NVMe drives

    Affected functions:
    Validation :
        1. Eject NVMe drive and wait for action is done
        2. Insert drive again
        3. It should see NVMe VPD information on web gu

4.
    Category: Fix
    Description:
      [71291] (REDFISH_X10_334, IPMIWebTest) Some Information Lost From System Summary
      [71284] [IPMI ECO 3.34] BIOS, CPLD, redfish version gone in 3.34.
      [71392] Web GUI not showing BIOS information and MAC address
    Impact motherboard: all
    Affected functions:
    Validation :
        1.After FW is updated, reboot the system
        1.Login IPMI Web check firmware version

5.
    Category: Fix
    Description:
      [71336] [IPMI ECO 3.34]iKVM windows has noise with wrong resolution size.
      [71335] Remote console is broken.

    Impact motherboard: all
    Affected functions:
    Validation :
        1. Login IPMI Web
        2. Open iKVM function to check

6.
    Category: Fix
    Description:
      [71223] 4 SUM Test Case Fail
      [70334] [1.0 BIOS ECO] SUM test failed
      [71398] SUM test is fail

    Impact motherboard: all
    Affected functions:
    Validation :
        1. Please do ECO test
        2. Check if 215 test case is passed

7.
    Category: Fix
    Description:
      [70870] Fan PWM fail

    Impact motherboard: A2SDI
    Affected functions:
    Validation :
        1. Check memory sensor if appears
        2. Heat 10G sensor and check if duty raise

8.
    Category: Fix
    Description:
      [70859]  Enter Key Causes Session Logout under Web Session Feature

    Impact motherboard: all
    Affected functions:
    Validation :
        1. When user attempts to modify timeout value, hitting ENTE> key
           will force session to logout. It should not.
-----------------------------------------------------------------
Filename: REDFISH_X10_334.bin  version: 3.34  Date: 05-19-2016

Note: Do factory defualt after updating fw
      Please clear broswer cache

Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r27
Redfish/iKVM version :  1.0.1

1.
    Category: Fix
    Description:
      [70904] Invalid Offset for this SensorType - Assertion after IPMI upgrade.

    Impact motherboard: X10QBi
    Affected functions:
    Validation :
        1. Make a chassis intrusion.
        2. Check the SEL log.

2.
    Category: Fix
    Description:
      [71035] sensor name in IPMI& SD5 not match hardware monitoring sensor list.

    Impact motherboard: X10SDE-DF
    Affected functions:
    Validation :
        1. Restore to factory default to apply new SDR.
        2. Check in IPMI Web sensor page

3.
    Category: Enhancement
    Description:
      [70997] [NM] Can't get entire platform power statistics.

    Impact motherboard: X10SDE-DF
    Affected functions:
    Validation :
        1. Power on system
        2. issue nm20 statistics command

4.
    Category: Enhancement
    Description:
      iKVM connection use STUNNEL only for security manner.

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Reset to factory default by using the following command:
           ipmitool -I lanplus -H ${BMC_IPADDR} -U ADMIN -P ADMIN raw 0x30 0x40
        2. Connect the system with iKVM. It should be work.
        3. Change iKVM port and check whether iKVM works.

-----------------------------------------------------------------
Filename: REDFISH_X10_333.bin  version: 3.33  Date: 04-29-2016

Note: Do factory defualt after updating fw
      Please clear broswer cache

Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r27
Redfish/iKVM version :  1.0.1

1.
    Category: Fix
    Description:
      [70006] Header JPI2C1 function test fail

    Impact motherboard: A2SDI-LN4F A2SDI-TP8F
    Affected functions:
    Validation :
        1. Power on the system.
        2. Check the power status sensor.

2.
    Category: Fix
    Description:
      [70372] Cannot find CPU vcore sensor reading item.

    Impact motherboard: X10SDD
    Affected functions:
    Validation :
        1. Restore to factory default and power on the system.
        2. Check the Vcore sensor.

3.
    Category: Enhancement
    Description:
      Support GPU threshold in GPU thermal guide 1.09.

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Reset to factory default by using the following command:
           ipmitool -I lanplus -H ${BMC_IPADDR} -U ADMIN -P ADMIN raw 0x30 0x40
        2. power on the system with GPU card.
        3. Check the GPU sensor threshold, refer to GPU thermal guide 1.09
        (table 5-2) for detail threshold value.

4.
    Category: Fix
    Description:
      [70333] IPMI hardware monitor check fail

    Impact motherboard: A2SDI-LN4F A2SDI-TP8F
    Affected functions:
    Validation :
        1. Power on the system.
        2. Check Sensor Readings page.
5.
    Category: Fix
    Description:
      [70512] [Firmware RF v3.32] Lots of "PCH temp sensor" assert/de-assert events occurred within system is running stress.

    Impact motherboard: X10QBi.
    Affected functions:
    Validation :
        1. Power on the system.
        2. Check the Event Log page.

6.
    Category: Fix
    Description:
      [70429] The IPMI sensor readings test fail.

    Impact motherboard: X10SRM, X10DRT-L
    Affected functions:
    Validation :
        1. Install Broadwell R0 CPUs
        2. Check if memory sensors display correctly

7.
    Category: Enhancement
    Description:
      [70371] Share LAN status from AOC-STGS-i2T is 100M

    Impact motherboard: X10DRG-Q
    Affected functions:
    Validation :
        1. This validation only use 1G/10G share LAN functions. For multridrop
           function, this is OEM feature
        2. Please send 0x30 0x70 0x76 0x1 0x1 to enable multiple package support
        3. BMC do reboot
        4. Plug in 1G or 10G LAN cables and check network status on IPMI web gui
        5. Please send 0x30 0x70 0x76 0x1 0x0 ti disable multiple package id support

8.
    Category: Fix
    Description:
      [70601] Not allow to key in special character in SMTP password field.

    Impact motherboard: All
    Affected functions:
    Validation :
        1. type in the special characters in SMTP password.
        2. Check if any messages poped out.

9.
    Category: Fix
    Description:
      [70473] Can't get entire platform Power statistics.

    Impact motherboard: X10SDD-F
    Affected functions:
    Validation :
        1. use the nm command to get power statistics

10.
    Category: Fix
    Description:
      [70642] sum test fail with IPMI 3.32FW

    Impact motherboard: X10QBL
    Affected functions:
    Validation :
        1. run sum GetDMIInfo command to get dmi file.

11.
    Category: Fix
    Description:
      [70695] Four voltages sensor are not in the right order.

    Impact motherboard: X10QRH
    Affected functions:
    Validation :
        1. Restore to factory default to apply new SDR.
        2. Check Vcpu1/Vcpu2/Vcpu3/Vcpu4 sensor threshold values.

12.
    Category: New feature
    Description:
        10G/40G AOC Naming rule change.

    Impact motherboard: All X10 MB
    Affected functions:
    Validation :
        1. insert 10G/40G AOC, the name should show AOC_NIC_Temp.

13.
   Category: New Feature
   Description:
     Support NVIDIA M4 GPU

   Impact motherboard: All X10 MB
   Affected functions:
   Validation :
        1. Insert NVIDIA M4 GPU in MB.
        2. Check the sensor page

14.
   Category: Enhancement
   Description:
      [70096] PCIE SERR/PERR Alert mail "Sensor ID" is empty

   Impact motherboard: All X10 MB
   Affected functions:
   Validation :
        1. Register SMTP account
        2. Issue PCIE SERR/PERR event
        3. Get email alart
        4. Check "Sensor ID" item. It should have sensor number or sensor name

------------------------------------------------------------------------------------
Filename: REDFISH_X10_332.bin  version: 3.32  Date: 03-31-2016

Note: Do factory defualt after updating fw

Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r25
Redfish/iKVM version :  1.0.1

1.
    Category: Fix
    Description:
      [70147] failed on mounting/unmounting ISO using SUM
      [70072] Mount iso image function failed with out-of-band interface
      [70069] fix [SUM] v1.6.1 test failed
      [70068] v1.6.1 test failed
      [70137] The test failed and got one error message
          "IPMI execution exception occurred" when executed Test cases 414 and 415

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Do factory default action
        2. Run SUM test

2.
   Category: New Feature
   Description:
     Support new motherboard: X10SDE-DF

   Impact motherboard: X10SDE-DF
   Affected functions:
   Validation :
        1. Board ID: 0x092D.

3.
    Category: Fix
    Description:
      [70033] The temperature of 10G chipset didn't show in IPMI sensor reading.

    Impact motherboard: X10SDD-F
    Affected functions:
    Validation :
        1. plug in AOC-CTGS-i2T lan card
        2. check IPMI Web sensor reading

4.
    Category: Fix
    Description:
      [70007] Jumper JL1 function test fail

    Impact motherboard: A2SDI LN4F/TP8F
    Affected functions:
    Validation :
        1. Generature a Chassis Intru log.
        2. See the Chassis Intru function is good or not.

5.
    Category: Fix
    Description:
      [69996] FAN of HeavyIO mode test fail

    Impact motherboard: X10SRM
    Affected functions:
    Validation :
        1. heat 10G senosr, pwm at right side should increase.

6.
    Category: Fix
    Description:
      [69893] PCH temp issue shows in Event log.

    Impact motherboard: X10QRH.
    Affected functions:
    Validation :
        1. Power on the system.
        2. Check the Event Log page.

7.
    Category: Fix
    Description:
      [69394] Overheat LED can't work.

    Impact motherboard: A2SDI LN4F/TP8F
    Affected functions:
    Validation :
        1. Make the CPU overheat.
        2. See the Proc_hot SEL is generated or not.

8.
    Category: Fix
    Description:
      [69881] Front panel OH/PF LED will blinking once during system power off

    Impact motherboard: X10SDV-7TP4F
    Affected functions:
    Validation :
        1. Heat CPU to let overheat led blinking
        2. Power off the system
        3. Check

9.
    Category: Fix
    Description:
      [69993] LAN information is incorrect under IPMI WebGUI

    Impact motherboard: X10SDD-F
    Affected functions:
    Validation :
        1. check IPMI WebGUI

10.
    Category: Fix
    Description:
      [70101] [IPMICFG] Change gate way fail.

    Impact motherboard: All
    Affected functions:
    Validation :
        1. ipmicfg -dhcp off.
        2. ipmicfg -m <IP>.
        3. ipmicfg -k 255.255.255.0
        4. ipmicfg -g <GateWay IP>

-------------------------------------------------------------------------------------
Filename: REDFISH_X10_331.bin  version: 3.31  Date: 03-25-2016

Note: Do factory defualt after updating fw

Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r25
Redfish/iKVM version :  1.0.1

1.
    Category: Fix
    Description:
      [69083] Lower Critical going low.
      [69893] PCH temp issue shows in Event log.

    Impact motherboard: X10QBL, X10QRH.
    Affected functions:
    Validation :
        1. Power on the system.
        2. Check the Event Log page.

2.
    Category: Fix
    Description:
      [69691] Redfish 3.30 Fan Speed misbehvior after restoring factory setting.
      [69755] The fan PWM duty cycle work abnormally.
      [69579] The fan PWM duty cycle work abnormally.

    Impact motherboard: X10QBL, X10DRG-H
    Affected functions:
    Validation :
        1. Restore to factory default.
        2. Check the fan PWM duty cycle.

3.
    Category: Fix
    Description:
      [69689] Some voltage monitor items not displayed
      [69688] CPU Vcore sensor reading is not available

    Impact motherboard: X10SDV-T
    Affected functions:
    Validation :
        1. Do factory default.
        2. Check sensor readings

4.
    Category: Enhancement
    Description:
      [69482] Random CPU Thermal Trip Events
      [68904] CPU thermal trip no SEL logs

    Impact motherboard: X10SDV-T
    Affected functions:
    Validation :
        1. Heat CPU and until the system shutdown
        2. Check no thermal trip event log
5.
    Category: Fix
    Description:
      [69885] The overheat LED didn't blink when power fail.

    Impact motherboard: X10SDD-F
    Affected functions:
    Validation :
        1. Plug out PSU
        2. The power fail red LED will blink

-------------------------------------------------------------------------------------
Filename: REDFISH_X10_330.bin  version: 3.30  Date: 03-04-2016

Note: Do factory defualt after updating fw

Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r25
Redfish/iKVM version :  1.0.1


1.
    Category: Fix
    Description:
      [69472] PCH Temperature reporting asserted/deasserted.
      [69270] IPMI SEL keeps recording false PCH temper messages.
      [69263] IPMI SEL will log PCH Temperature Going Low events everytime system powers on.

    Impact motherboard: X10DRW-IT, X10DRT-PT, X10DRG-HT
    Affected functions:
    Validation :
        1. Power on the system.
        2. Check the Event Log page.
2.
    Category: Work around
    Description:
      [69147] Hardware monitor of RT1 is fail

    Impact motherboard: X10SDR-TP
    Affected functions:
    Validation :
        1. BMC add 2 degree offsest fro RT1
        2. Check the RT1 Temp sensor reading

3.
    Category: Work around
    Description:
      [69147] [1U TwinPro] PSU info randomly goes missing in DMI table when running on/off test

    Impact motherboard: X10DRT-P
    Affected functions:
    Validation :
        1. Do cburn on/off test
        2. Check if no power supply mismatch problem occurs

----------------------------------------------------------------------------------------
Filename: REDFISH_X10_329.bin  version: 3.29  Date: 02-26-2016

Note: Do factory defualt after updating fw

Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r25
Redfish/HTML5 iKVM version :  1.0.1

1.
    Category: Fix
    Description:
      [69011] PCH Sensor Reading Shows "N/A"

    Impact motherboard: All
    Affected functions:
    Validation :
        1. This is only enhance the error handling, if ME has no response.
        2. Check the PCH Temp sensor reading.

2.
    Category: Fix
    Description:
      [69270] IPMI SEL keeps recording false PCH temper messages.
      [69263] IPMI SEL will log PCH Temperature Going Low events everytime system powers on.

    Impact motherboard: X10DRW-IT, X10DRT-PT
    Affected functions:
    Validation :
        1. Power on the system.
        2. Check the Event Log page.

3.
    Category: Fix

    Description:
      [69294] [Redfish 3.28] Chassis intrusion status not correct

    Impact motherboard: All
    Affected functions:
    Validation :
        1. trigger chassis intrusion event and check the status in "IntrusionSensor".

4.
    Category: Fix
    Description:
      [69266] Redfish 3.28 mispelled Snooping

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Go to the redfish URI: /redfish/v1/Managers/1/Snooping

5.
    Category: Fix
    Description:
      [69348] [DVT] CPU2 Overheat Won't Trigger the Red Overheat LED on Front Panel.

    Impact motherboard: X10DRT-PS
    Affected functions:
    Validation :
        1. Heat the CPU2 to overheat.
        2. Check the Front Panel LED.

-----------------------------------------------------------------------
Filename: REDFISH_X10_328.bin  version: 3.28  Date: 02-19-2016

Note: Do factory defualt after updating fw

Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version    : v0.5.9
Java iKVM Viwer version    : v1.69 r25
Redfish/HTML5 iKVM version :  1.0.1

1.
    Category: New Feature
    Description:
        Support HTML5

    Impact motherboard: All X10
    Affected functions:
    Validation :

2.
    Category: New Feature
    Description:
        Support new motherboard: A2SDI-H-TP4F

    Impact motherboard: A2SDI-H-TP4F
    Affected functions:
    Validation :
        1. Board ID: 0x0910.

3.
    Category: New Feature
    Description:
        [Redfish] SNMP feature is added.

    Impact motherboard: All
    Affected functions:
    Validation :
        1. 'GET' all managers under the URN "redfish/v1/Managers/1" to check if there is "SNMP" in "oem" catagory.
        2. Then 'GET' its URN path: "redfish/v1/Managers/1/SNMP".
        3. 'GET' / 'PATCH' are acceptable operations.
        4. "SnmpEnabled" can be 'PATCH'
        5. After you set "SnmpEnabled" to 'true', check if there exist "SNMPv2" and "SNMPv3".
        6. Then 'GET' its URN path: "redfish/v1/Managers/1/SNMP/SNMPv2" or "redfish/v1/Managers/1/SNMP/SNMPv3".
        7. In SNMPv2 "ROCommunity" and "RWCommunity" can be 'PATCH'
        8. In SNMPv3 "Snmpv3Enabled", "UserName", "AuthProtocol", "PrivateProtocol", "AuthKey" and "PrivateKey" can be 'PATCH'

4.
    Category: New Feature
    Description:
        [Redfish] Syslog feature is added.

    Impact motherboard: All
    Affected functions:
    Validation :
        1. 'GET' all managers under the URN "redfish/v1/Managers/1" to check if there is "Syslog" in "oem" catagory.
        2. Then 'GET' its URN path: "redfish/v1/Managers/1/Syslog".
        3. 'GET' / 'PATCH' are acceptable operations.

5.
    Category: New Feature
    Description:
        [Redfish] Chassis Intrusion feature is added.

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Get command: https://IP/redfish/v1/Chassis/1/
        2. Clear Chassis Intrusion: 'PATCH' with data {"PhysicalSecurity":{"IntrusionSensor": "Normal"}}

6.
    Category: New Feature
    Description:
        [Redfish] SMCRAKP feature is added.

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Get https://x.x.x.x/redfish/v1/Managers/1/SMCRAKP
        2. PATCH
           Raw data :{"Mode": "Enabled"}

7.
    Category: New Feature
    Description:
        [Redfish] support IP Access Control

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Get https://x.x.x.x/redfish/v1/Managers/1/IPAccessControl
        2. Patch to enable/disable IPAceess with {"ServiceEnabled": true}
        3. Get https://x.x.x.x/redfish/v1/Managers/1/IPAcessControl/FilterRule
        4. 'GET'/'PATCH'/'POST' are acceptable operations.
        5. Post with {"Address": "10.136.176.0",  "PrefixLength": 24,  "Policy": "Accept"}

8.
    Category: New Feature
    Description:
        [Redfish] support VM (Virtual Media)

    Impact motherboard: All

    Affected functions:
    Validation :
        1. only 'GET' support, test it with Virtual media in Web
        2. Get https://x.x.x.x/redfish/v1/Managers/1/VM1

9.
    Category: New Feature
    Description:
        [Redfish] Snopping

    Impact motherboard: All
    Affected functions:
    Validation :
        1. only 'GET' support
        2. Get https://x.x.x.x/redfish/v1/Managers/1/Snopping

10.
    Category: Fix
    Description:
      [68709] [Redfish v3.27] Failed to PATCH UID via https://IP/redfish/v1/Chassis/1/ with {"IndicatorLED": "Blinking"}

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Get the command for https://IP/redfish/v1/Chassis/1/
        2. patch with  {"IndicatorLED": "Blinking"}

11.
    Category: Fix
    Description:
      [CRM SM1601107937]  Supermicro Case#SM1601107937:A1SRI-2758F
        IPv6 static adress lost after reboot on IPMI

    Impact motherboard: All
    Affected functions:
    Validation :
        Go to Configuration - Network
        Screen shoot: x10_ipv6_address_configured_before_reboot_ipmi_pub.png

        Reboot the IPMI

        Go to Configuration - Network
        Screen shoot: x10_ipv6_address_lost_after_reboot_ipmi_pub.png
        Reproduce   1. Go to Configuration - Network
        2. In IPv6 Setting:
        - untick Auto Configuration
        - Fill IPv6 address field with your IPv6 address/64.
        3. Save
        4. Go to Configuration - Network
        - You will see the static IPv6 address added previously in Address List of IPv6 setting
        - The static IPv6 address reply to ping.

        Reboot the IPMI

        1. Go to Configuration - Network
        - You will NOT see the static IPv6 address added before reboot in Address List of IPv6 setting.
        - The static IPv6 address didn't reply to ping.

12.
    Category: Fix
    Description:
        [68753] [IPMI ECO 3.27] FAN A,B,C,D can not set to Optimal by redfish API

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Go to the redfish URI: /redfish/v1/Chassis/1/ then set fanmode to check

13.
    Category: Fix
    Description:
        [68829] "Not Present" for 10G/40G AOC sensor reading after AC OFF/ON
        [68177] 10G and 40G LAN Card sensor reading miss

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Put on the 10G/40G card.
        2. Power on the system.
        3. Check 10G/40G sensors.

14.
    Category: Fix
    Description:
        [68976] IPMI sensor reading for fan RPM is incorrect

    Impact motherboard: X10QBi
    Affected functions:
    Validation :
        1. Check the RPM signal with the WebGUI reading.

15.
    Category: Workaround
    Description:
        [68946] After product release to enable BMC read LSI
                temperature from I2C cause system hung

    Impact motherboard: X10DRG-H, X10DRH, X10DRH-LN4, X10DRI, X10SRG
    Affected functions:
    Validation :
        1. When LSI 3108 card is plugged in, no LSI sensor appeared, and LSI web is hidden

16.
    Category: Workaround
    Description:
        Cannot read Nivida M60

    Impact motherboard: X10DRG-H
    Affected functions:
    Validation :
        1. Download this FW to verify

17.
    Category: Fix
    Description:
        [69226] Can not show System LAN MAC address completely in IPMI Summary web page
        [69148] Hardware monitor of RT2 is fail
        [69147] Hardware monitor of RT1 is fail
        [68904] CPU thermal trip no SEL logs
        [68853] No sensor readings

    Impact motherboard: X10SDV-7TP8F/X10SDV-7TP4F
    Affected functions:
    Validation :
        1. Check sensor reading web gui if all values are good
        2. Check thermal trip function


18.
    Category: Enhancement
    Description:
        VBat sensor reading cannot immediatedly reflect the battery's presence/absense

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Remove battery, then goto sensor reading page to press the button "Auto Refresh" to speed up for reflect the battery
        2. Install back battery, and then perform "stop auto refresh" and "auto refresh" button pressing in a row.

========================================================================================
Filename: REDFISH_X10_327.bin  version: 3.27  Date: 01-18-2016

Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r25

1.  Category: Fix
    Description:
        [68394] RedFish - The time zone format is incorrect.

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Change the time zone from the WebGUI and read it by using the redfish API.
        2. Check The time zone format

2.  Category: Fix
    Description:
        [68389] [Red_fish] Return Message is incorrect

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Post the command for https://IP/redfish/v1/Systems/1/Actions/ComputerSystem.Reset with {"ResetType":"????%#@"}
        2. Check http error code

3.  Category: Fix
    Description:
        [68390] [Redfish v3.26] Administrator/ReadOnlyUser confusion resulted in misbehavior

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Generated two accounts (different password) using the same username with one in Administrator group one in
           ReadOnlyUser group.
        2. To login using the ReadOnlyUser account and check privileges.

4.  Category: Fix
    Description:
        [68416] [Red_Fish]Return message not correct--{"IndicatorLED": "klkl"}

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Patch the command for https://IP/redfish/v1/Chassis/1/  with {"IndicatorLED": "klkl"}
        2. Check http error code

5.  Category: Fix
    Description:
        [68351] RedFish - No CPU model name and the max speed is always 4000MHz

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Get the command for https://IP/redfish/v1/Systems/1/Processors/1
        2. Check CPU Model name with WebGUI -> Hardware Information

6.
    Category: Fix
     Description:
       [67813] [EVT]FP LED - Overheat LED for CPU2 failed

     Impact motherboard: X10DSC-TP4S
     Affected functions:
       Validation :
           1. Stress CPU2 temp to observe.
           2. Check if red led turns on very quickly before it touch Tjamx degree

7.
    Category: Fix
     Description:
       [68010] AOC-STG-i2T 10G LAN cards is not supported.

     Impact motherboard: X10DRG-O
     Affected functions:
       Validation :
           1. Put the AOC-STG-i2T onto slot 5,6,7 of PCIe board.
           2. Check the 10G temp sensor.

8.
    Category: Fix
     Description:
       [68467] Wrong CPU sensor id
       [68464] Wrong sensor id Chassis

     Impact motherboard: All
     Affected functions:
       Validation :
           1. Set the SMTP and alert correctly.
           2. Generate CPU/Chassis related SEL.
           3. Check the email wording.

9.  Category: Fix
    Description:
        [68411] [Redfish v3.26]Radius Secret is hidden in IPMIGUI but API displays the entire string.

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Update(or do PATCH in redfish) RADIUS information and get it back to check

10. Category: Fix
    Description:
        [67259] Not easy to identify if there are multiple controllers installed

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Install 2 Avago 3108 devices then go to web to check the information subpage

11. Category: New Feature
     Description:
       Support new motherboard: X10SDD-F

     Impact motherboard: X10SDD-F
     Affected functions:
     Validation :
         1. Board ID: 0x0919.

12. Category: New Feature
     Description:
       Support new motherboard: A2SDI-TP8F

     Impact motherboard: A2SDI-TP8F
     Affected functions:
     Validation :
         1. Board ID: 0x090F.

13. Category: Fix
    Description:
        [67486] [SUM 1.6.0(2015/11/20)] Test fail.

    Impact motherboard: X10SLL
    Affected functions:
    Validation :
        1. Run the test 229.
        2. Check the result.

14.
    Category: Workaround
     Description:
       [65729] BIOS ECO:[SUM 1.4.2] SUM Test fail.

     Impact motherboard: A1SAM-2750F/A1ASM-2550F/A1SRM-2758F
     Affected functions:
     Validation :
         1. Run SUM test or try to BIOS upgrade

========================================================================================
Filename: REDFISH_X10_326.bin  version: 3.26  Date: 12-18-2015

Support Motherboard: All X10 MBs
U-Boot build time : 2009.01 (Nov 27 2013)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

1.  Category: New implementation
    Description:
        Add 10 MBs to support redfish service.
    Impact motherboard: A1SA2,    A1SA7,  A1SAI,  A1SAM, A2SCL, A1SAM_LN7F
                          X10DBT_T, X10QBI, X10QBL, C7X99, C7Z97, X10QRH_PLUS
                          X10SLM,   X10SRE, X10SLH_N6, X10SLM_LN4,

    Affected functions:
    Vagidation :

2.  Category: New Feature
    Description:
        Support 10G temperature reading on AOC-CTGS-i2T card

    Impact motherboard: X10SLD-F with  AOC-CTGS-i2T card
    Affected functions:
    Validation :
        1. Plug in AOC-CTGS-i2T card on X10SLD-F
        2. Power on and check the sensor reading

3.  Category: New Feature
    Description:
        [68016] [EVT] X10DSC-TP4S Rev1.00: Hardware Monitor Test Fail   Solved
        [67763] [EVT] BP (35R0-202142-10100F) FAN headers are not working properly
        [67759] [EVT] Onboard 10G-LAN Temp" Sensor not present in v2.24 firmware

    Impact motherboard: X10DSC-TP4S
    Affected functions:
    Validation :
        1. Check sensor reading

4.  Category: New implementaion
    Description:
        [67778] [SUM 1.6.0] Change LAN mode to supported mode will cause IPMI dead.

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Run the SUM command changebmccfg --file Template/dedicated.xml.

5.  Category: Fix
    Description:
        [67853] NVMe SSD tab in IPMI Web GUI shows traditional HD.

    Impact motherboard: X10QBi
    Affected functions:
    Validation :
        1. Check the WebGUI, if there are no NVMe devices, NVMe page should not present.

6.  Category: Enhancement
    Description:
        [64890] "[Redfish] System stop in "Factory Default" page and cannot back to Login page after press "Factory Default" button"

    Impact motherboard: X10QBi
    Affected functions:
    Validation :
        1. Check the WebGUI will back to Login page after press "Factory Default" button".

7.  Category: Fix
    Description:
        [67634] [1U-1028TP] No Backplane Nuvoton MCU Firmware Update Tool.

    Impact motherboard: X10DRT-P (1U TwinPro)
    Affected functions:
    Validation :
        1. Check the WebGUI will have page to update Nuvoton MCU FW.

8.  Category: Fix
    Description:
        [67642] [SUM v1.60] sum test fails.

    Impact motherboard: X10QBi
    Affected functions:
    Validation :
        1. Run the SMSTC test: TC226 and TC227.
        2. Check the result.


9.  Category: Enhancement
    Description:
        Support FANA on X10SDV 2.0
        Support 10G sensors on all motherboards

    Impact motherboard: X10SDV 1.0 and X10SDV 2.0
    Affected functions:
    Validation :
        1. All X10SDV motherboards should support MB_10G sensor.
        2. If motherboard is X10SDV 1.0, one zones are supported

10. Category: fix
    Description:
        [67919] [REDFISH_X10_325] "service received an authorization error authorized" while try to GET "https://BMC_IP/redfish/v1/...."

    Impact motherboard: All motherboards support Redfish
    Affected functions:
    Validation :
        1.GET "https://BMC_IP/redfish/v1/................" (AccountService, Managers, Systems, or Chassis .....)
          to check whether ok.

11. Category: fix
    Description:
        [67625] [Red Fish] The status reponse incorrect message, 200 OK

    Impact motherboard: All motherboards support Redfish
    Affected functions:
    Validation :
        1. Patch data to "redfish/v1/Managers/1/NTP".
        2. {"NTPEnable": true,"PrimaryNTPServer": "supermicro",
            "SecondaryNTPServer": "1.us.pool.ntp.org","DaylightSavingTime": true}
        3. check status code and error message.

12. Category: Fix
    Description:
    [68052] IERR Assertion in IPMI SEL during ONOFF test with M0 Stepping Broadwell CPU.
    [68012] lots of "Processor IERR Assertion" in IPMI event log when running PCH on/off with IPMI FW v3.25
    [68011] lots of "Processor IERR Assertion" in IPMI event log when running PCH on/off via BMC
    [67969] [firmware v2.24 / redfish v3.25] System generates "Processor - IERR -Assertion" event logs if run Cburn on/off stress.

    Impact motherboard: X10DDW-IN-P, X10DRH-CLN4-P, X10DRH-CT-P, X10DRFR-NT-P, X10DRT-P, X10DRU-I+
    Affected functions:
    Validation :
        1.run PCH on/off.
       PS: only Enable CPUERR feature on X10DRT-P, X10DRU-I+ only.

========================================================================================
Filename: REDFISH_X10_325.bin  version: 3.25  Date: 12-11-2015

Support Motherboard: X10SRH,    X10SLH,     X10SLE,    X10SRL,   X10SLX,      X10SRA,   X10SRD,
                     X10DRU-I+, X10DRT-P,   X10DRG-H,  X10DRW-I, X10DRI-T4+,  X10DDW-I, X10DRFR,
                     X10DRI-T,  X10DRFF,    X10DRFR-T, X10DRD,   X10DRD-L,    X10DRW-E, X10DRG-O+-CPU,
                     X10DRG-Q,  X10DRH-I,   X10DRC,    X10DRL_I, X10DRT_L,    X10DRU_X, X10DRH_LN4,
                     X10DRX,    X10DRU_XLL, X10SRG,    X10SRI,   X10SRW,      X10SDV,   X10SL7
                     X10SLA,    X10SLD,     X10SLE_D,  X10SLL,   X10SLL_PLUS

1.  Category: New implementation
    Description:
        Add 10 MBs to support redfish service.
    Impact motherboard: X10SRG, X10SRI,  X10SRW,   X10SDV, X10SL7
                          X10SLA, X10SLD,  X10SLE_D, X10SLL, X10SLL_PLUS
    Affected functions:
    Validation :

2.  Category: fix
    Description:
        [67625] [Red Fish] The status reponse incorrect message, 200 OK

    Impact motherboard: All motherboards support Redfish
    Affected functions:
    Validation :
        1. Patch data to "redfish/v1/Managers/1/NTP".
        2. {"NTPEnable": true,"PrimaryNTPServer": "supermicro",
            "SecondaryNTPServer": "1.us.pool.ntp.org","DaylightSavingTime": true}
        3. check status code.

3.  Category: fix
    Description:
        [67248] [Redfish] Cannot PATCH Active Directory Role Group Domain with PERIOD

    Impact motherboard: All motherboards support Redfish
    Affected functions:
    Validation :
        1. Connect to "redfish/v1/Managers/1/ActiveDirectory/RoleGroups/"
        2. POST data {"RoleGroupName":"test", "RoleGroupDomain":"bling.com","RoleGroupPrivilege":"Operator"}
        3. PATCH data {"RoleGroupName":"test", "RoleGroupDomain":"10.136.176.96","RoleGroupPrivilege":"Operator"}

========================================================================================
Filename: REDFISH_X10_324.bin  version: 3.24  Date: 11-20-2015

Support Motherboard: X10SRH,    X10SLH,   X10SLE,    X10SRL,   X10SLX,     X10SRA,   X10SRD,
                     X10DRU-I+, X10DRT-P, X10DRG-H,  X10DRW-I, X10DRI-T4+, X10DDW-I, X10DRFR,
                     X10DRI-T,  X10DRFF,  X10DRFR-T, X10DRD,   X10DRD-L,   X10DRW-E, X10DRG-O+-CPU,
                     X10DRG-Q,  X10DRH-I, X10DRC,    X10DRL_I, X10DRT_L,   X10DRU_X, X10DRH_LN4,
                     X10DRX,    X10DRU_XLL

1.  Category: New implementation
    Description:
        Add 10 MBs to support redfish service.
    Impact motherboard: X10DRC,     X10DRH_LN4, X10DRL_I, X10DRT_L, X10DRU_X,
                          X10DRU_XLL, X10DRX,     X10SLX,   X10SRA,   X10SRD
    Affected functions:
    Validation :

2.  Category: fix
    Description:
        [66840] The Syslog doesn't have the "help" translation on IPMI WebGUI.

    Impact motherboard: All motherboards support Redfish
    Affected functions:
    Validation :
        1. Connect to Syslog in simple chinese page and check "help".

3.  Category: fix
    Description:
        [66931] RedFish_3.23 The "RoleGroupPrivilege" can't be set as "Administrator" (ActiveDirectory)

    Impact motherboard: All motherboards support Redfish
    Affected functions:
    Validation :
        1. Connect to "redfish/v1/Managers/1/ActiveDirectory/RoleGroups"
        2. POST data to add rolegroup with "RoleGroupPrivilege":"Administrator"

4.  Category: fix
    Description:
        [66971] [Red_Fish] Status Return Incorrectly

    Impact motherboard: All motherboards support Redfish
    Affected functions:
    Validation :
        1. Connect to "/redfish/v1/Managers/1/SerialInterfaces/1"
        2. PATCH data with {"InterfaceEnabled": false}.
        3. check http code.

5.  Category: fix
    Description:
        [66905] [Red_fish] Return Message is incorrect

    Impact motherboard: All motherboards support Redfish
    Affected functions:
    Validation :
        1. Connect to "redfish/v1/EventService/Subscriptions/"
        2. POST data {"Destination":"http://www.dnsname.com/Destination1","Context":"user1_test","Events":["Alert","StatusChange"],"Protocol":"Redfish"}
        3. check http code and error message.

6.  Category: fix
    Description:
        [66843] RedFish_3.22 can use the same username to create accounts.

    Impact motherboard: All x10 motherboards
    Affected functions:
    Validation :
        1. create one Administrator and one ReadOnlyUser by using the same name (by Redfish).
        2. login to WebGUI, the user will be Administrator and link to Power Control page to make sure user can config

7.  Category: fix
    Description:
        [67248] [Redfish] Cannot PATCH Active Directory Role Group Domain with PERIOD

    Impact motherboard: All motherboards support Redfish
    Affected functions:
    Validation :
        1. Connect to "redfish/v1/Managers/1/ActiveDirectory/RoleGroups/"
        2. POST data {"RoleGroupName":"test", "RoleGroupDomain":"bling.server","RoleGroupPrivilege":"Operator"}
        3. PATCH data {"RoleGroupName":"test", "RoleGroupDomain":"bling.server","RoleGroupPrivilege":"Operator"}

8.  Category: fix
    Description:
        [67229] No 10G card sensor reading on IPMI web
        [67152] [Red_Fish] Can't detect AOC 10G and 40G Sensor Reading

    Impact motherboard: All motherboards in X10
    Affected functions:
    Validation :
        1. check sensor reading in web page.

========================================================================================
Filename: REDFISH_X10_323.bin  version: 3.23  Date: 11-06-2015

Support Motherboard: X10SRH,   X10SLH,    X10SLE,    X10SRL

                     X10DRU-I+, X10DRT-P, X10DRG-H,  X10DRW-I, X10DRI-T4+, X10DDW-I, X10DRFR,
                     X10DRI-T,  X10DRFF,  X10DRFR-T, X10DRD,   X10DRD-L,   X10DRW-E, X10DRG-O+-CPU,
                     X10DRG-Q,  X10DRH-I

1.  Category: New implementation
    Description:
        X10DRG-Q and X10SRL support redfish service.
    Impact motherboard: X10DRG-Q and X10SRL
    Affected functions:
    Validation :

2.  Category: Fix
    Description:
        [66810] RedFish_3.22 Vlan can't be enabled if Lan cable is not plug in Dedicate port.
    Impact motherboard: All X10 motherboards which support Redfish
    Affected functions:
    Validation :
        1. "PATCH" Vlan information on /redfish/v1/Managers/1/EthernetInterfaces/1 with data {"VLAN": {"VLANEnable":true,"VLANId": 12}}.

3.  Category: Fix
    Description:
        [66726] Redfoish v3.22] Failed to PATH "SecondaryNTPServer" under URN "https://BMC_IP/redfish/v1/Managers/1/NTP/"
        [66816] [Redfish] Cannot PATH NTP secondary server
    Impact motherboard: All X10 motherboards.
    Affected functions:
    Validation :
        1. Patch SecondaryNTPServer and check value.

4.  Category: fix
    Description:
        [66840] The Syslog doesn't have the "help" translation on IPMI WebGUI.

    Impact motherboard: All motherboards support NVMe
    Affected functions:
    Validation :
        1. Connect to Syslog in Japanese page and check "help"

5. Category: Fix
    Description:
        [66571 ] Redfish 3.21: redfish/v1/Managers/1/LDAP-> Patch operation allows invalid "LDAPPortNumber" value.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. Password will not show in response
        2. IPMI web do display SSL authentication field enabled when set enable.

6. Category: Fix
    Description:
        [66856] RedFish_3.22 "ReadOnlyUser" has the privilege to power control the system by API.
    Impact motherboard: All X10 motherboards which support Redfish
    Affected functions:
    Validation :
        1. Create an ReadOnlyUser account to test.

7. Category: Fix
    Description:
        [66812] Redfish 3.22 allows GET/POST/PATCH operations using HTTP service.
    Impact motherboard: All X10 motherboards which support Redfish
    Affected functions:
    Validation :
        1. Disable "ssl-redirect" in web then access Redfish APP via HTTP, the result should be returned as "Forbidden".

8. Category: Fix
    Description:
        [66809] Redfish API can't report correct DIMM installed with 64GB installed

    Impact motherboard: All X10 motherboards.
    Affected functions:
    Validation :
        1. Install memory which size larger than 32GB then access Redfish to check.


9. Category: Fix
    Description:
        [66464] Redfish_3.20: Boot order change for USB doesnot work it still boots to HDD.
        [66804] [Redfish] BootSourceOverride does not read paramter correctly.

    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. GET boot options in the redfish URI "/redfish/v1/Systems/1".
        2. Then PATCH different options in the same URI with the data:
           {
               "Boot": {
                   "BootSourceOverrideEnabled": ${RULE_YOU_CHOOSE},
                   "BootSourceOverrideTarget": ${OPTION_YOU_CHOOSE}
               }
           }
        3. Reboot to BIOS setup page to check boot order.

10. Category: Fix
     Description:
         [66841] [Redfish] /redfish/v1/Systems/1 is not showing correct total memory size with 64GB memory instal.
         [66809] Redfish API can't report correct DIMM installed with 64GB installed.

     Impact motherboard: All X10 motherboards in support list
     Affected functions:
     Validation :
          1. Install memory which size larger than 32GB then open web to check "Hardware Information" page.

========================================================================================
Filename: REDFISH_X10_322.bin  version: 3.22  Date: 10-30-2015

Support Motherboard: X10DRU-I+, X10DRT-P, X10DRG-H,      X10DRW-I, X10DRI-T4+, X10DDW-I, X10DRFR,
                     X10DRI-T,  X10DRFF,  X10DRFR-T,     X10DRD,   X10DRD-L,   X10SRH,   X10SLH,
                     X10SLE,    X10DRH-I, X10DRG-O+-CPU

1. Category: Fix
    Description:
        [66681] [IPMI FW 3.20] IPMI Hardware Info Page Shown Wrong Memory Size with 64GB Memory Installed.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. Installed memory which size over 32GB, then go to web to check "Hardware Information" page.

2. Category: Fix
    Description:
        [66674] RedFish is able to get token with http://.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. Access redfish URI via HTTP and HTTPs to check. If you use HTTP, it should reply with error message.
        2. Then go to web to check "http://${BMC_IP}", it should redirect to "https://${BMC_IP}" properly.

3. Category: Fix
    Description:
        [66464 ] Redfish_3.20: Boot order change for USB doesnot work it still boots to HDD.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. GET boot options in the redfish URI "/redfish/v1/Systems/1".
        2. Then PATCH different options in the same URI with the data:
           {
               "Boot": {
                   "BootSourceOverrideEnabled": ${RULE_YOU_CHOOSE},
                   "BootSourceOverrideTarget": ${OPTION_YOU_CHOOSE}
               }
           }
        3. Reboot to BIOS setup page to check boot order.

4. Category: Fix
    Description:
        [66566 ] Redfish:3.21- [Get] redfish/v1/Managers/1/RADIUS feature does not display "RadiusServerIP".
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. GET redfish URI "/redfish/v1/Managers/1/RADIUS" to check the field "RadiusServerIP".
        2. Or you can PATCH this field then GET it back again to see if it is modified or not.

5. Category: Fix
    Description:
        [66571 ] Redfish 3.21: redfish/v1/Managers/1/LDAP-> Patch operation allows invalid "LDAPPortNumber" value.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. Patch wrong IP will receive error message

6. Category: Fix
   Description:
        [66631] [IPMI v3.20] IPMI Event Log Report Wrong Error DIMM Location.
   Impact motherboard: All X10 motherboards.
   Affected functions:
   Validation :
        1.trigger Wrong Error DIMM Location.
        2.Open event log web to check.

7. Category: Fix
   Description:
       [66568] Processor Automatically Throttled Event does not de-assert until after FAN fail events have all been de-asserted
   Impact motherboard: All X10 motherboards.
   Affected functions:
   Validation :
       1. triggering fan fail and then CPU overheat event
       2. lowering the CPU back down to non-overheat range to check whether cause the "Processor Automatically Throttled" event to de-assert.

========================================================================================
Filename: REDFISH_X10_321.bin  version: 3.21  Date: 10-23-2015

Support Motherboard: X10DRU-I+, X10DRT-P, X10DRG-H,  X10DRW-I, X10DRI-T4+, X10DDW-I, X10DRFR,
                     X10DRI-T,  X10DRFF,  X10DRFR-T, X10DRD,   X10DRD-L,   X10SRH,   X10SLH,
                     X10SLE

1. Category: New implementation
    Description:
        NTP feature is added.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. 'GET' all managers under the URN "redfish/v1/Managers/1" to check if there is "NTP" in "oem" catagory.
        2. Then 'GET' its URN path: "redfish/v1/Managers/1/NTP".
        3. 'GET' / 'PATCH' are acceptable operations.
        4. "NTPEnable", "PrimaryNTPServer", "SecondaryNTPServer", "DaylightSavingTime" can be 'PATCH'

2. Category: New implementation
    Description:
        LDAP feature is added.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. 'GET' all managers under the URN "redfish/v1/Managers/1" to check if there is "LDAP" in "oem" catagory.
        2. Then 'GET' its URN path: "redfish/v1/Managers/1/LDAP".
        3. 'GET' / 'PATCH' are acceptable operations.
        4. "LDAPEnabled", "LDAPAuthOverSSL", "LDAPPortNumber", "LDAPServerIP", "LDAPPassword", "LDAPDN", "LDAPSearchbase" can be 'PATCH'

3. Category: New implementation
    Description:
        Radius feature is added.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. 'GET' all managers under the URN "redfish/v1/Managers/1" to check if there is "RADIUS" in "oem" catagory.
        2. Then 'GET' its URN path: "redfish/v1/Managers/1/RADIUS".
        3. 'GET' / 'PATCH' are acceptable operations.
        4. RadiusEnabled", "RadiusServerIP", "RadiusPortNumber", "RadiusSecret" can be 'PATCH'

========================================================================================
Filename: REDFISH_X10_320.bin  version: 3.20  Date: 10-16-2015

Support Motherboard: X10DRU-I+, X10DRT-P, X10DRG-H,  X10DRW-I, X10DRI-T4+, X10DDW-I, X10DRFR,
                     X10DRI-T,  X10DRFF,  X10DRFR-T, X10DRD,   X10DRD-L,   X10SRH,   X10SLH,
                     X10SLE

1. Category: Fix
   Description:
       [65106] [Redfish] System stop in "Factory Default" page and cannot back to Login page after press "Factory Default" button
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
       1. Try factory default and then wait for FW reboot.

2. Category: Fix
   Description:
        [66124] Redfish sensor name has extra characters
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
       1.GET the URI: redfish/v1/Chassis/1/Thermal to check.

3. Category: Fix
   Description:
        [66274] [RedFish] Redfish 3.19 responses "200 OK" when we PATCH Account password with empty string
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
       1. Clear user "Password" as empty string then PATCH it under the URL: "https://${BMC_IP}/redfish/v1/AccountService/Accounts/%d"

4. Category: Fix
   Description:
       [65858] Redfish threshold values are not in the right order
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
       1.connect to Chassis/1/Power to check max and min value in voltage.

5. Category: Fix
   Description:
        [66278] [RedFish] Redfish 3.19 /redfish/v1/Chassis/1/Power/ threshold values are in WRONG order
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
       1.GET the URI: redfish/v1/Chassis/1/Power to check.

6. Category: Fix
   Description:
        [66088] Redfish voltage sensor reading exceeds MaxReadingRange
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
       1.GET the URI: redfish/v1/Chassis/1/Power to check.

7. Category: Fix
   Description:
        [66270] [RedFish] /redfish/v1/Systems/1/Processors/ does not show any CPUs
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
       1.GET the URI: /redfish/v1/Systems/1/Processors/ to check.

========================================================================================
Filename: REDFISH_X10_319.bin  version: 3.19  Date: 10-02-2015

Support Motherboard: X10DRU-I+, X10DRT-P, X10DRG-H,  X10DRW-I, X10DRI-T4+, X10DDW-I, X10DRFR,
                     X10DRI-T,  X10DRFF,  X10DRFR-T, X10DRD,   X10DRD-L,   X10SRH,   X10SLH

1. Category: Fix
   Description:
       [65765] Redfish_3.17: Post SessionService/Sessions/ will have unexcept status over session number limit
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
       Continue POST SessionService/Sessions to session number limit is reached.

2. Category: Fix
   Description:
       [65950] Fixed MouseMode- shows "Unknown" mode as supported value issue.
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
       1. Connect to /redfish/v1/Managers/1/MouseMode and check "Unknown" mode does not show as supported value.

3. Category: Fix
   Description:
       [65898] Redfish_3.18: "redfish/v1/Managers/1/ActiveDirectory/RoleGroups/" type error
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
       1.connect to Managers/1/ActiveDirectory/RoleGroups/ to check odata.id

4. Category: Fix
   Description:
       [65627] Redfish_3.16: EventService action SubmitTestEvent EventType type error
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
       1.connect to action SubmitTestEvent with error type and check http status code.

5. Category: Fix
   Description:
       [65858] Redfish threshold values are not in the right order
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
       1.connect to Chassis/1/Power to check max and min value in voltage.

6. Category: Fix
   Description:
       [65798] Redfish_3.17 : System got 403 forbidden error on X10DDW-i.
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
       1.connect to /redfish/v1 to check whether can get data.

7. Category: Fix
   Description:
       The role - administrator can NOT change other users' password.
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
       1. Logon as administrator to change other users' password.

========================================================================================
Filename: REDFISH_X10_318.bin  version: 3.18  Date: 09-25-2015

Support Motherboard: X10DRU-I+, X10DRT-P, X10DRG-H, X10DRW-I, X10DRI-T4+, X10DDW-I,
                     X10DRFR, X10DRI-T, X10DRFF, X10DRFR-T, X10DRD,
                     X10DRD-L, X10SRH, X10SLH

1. Category: New implementation
    Description:
        Active Directory feature is added.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. 'GET' all managers under the URN "redfish/v1/Managers/1" to check if there is "ActiveDirectory" in "oem" catagory.
        2. Then 'GET' its URN path: "redfish/v1/Managers/1/ActiveDirectory".
        3. 'GET' / 'PATCH' are acceptable operations.
        4. Then 'GET' its URN path: "redfish/v1/Managers/1/ActiveDirectory/RoleGroups".
        5. 'GET' / 'POST'{"RoleGroupName":"xxx", "RoleGroupDomain":"xxx", "RoleGroupPrivilege":"Operator"} are acceptable operations.
        6. Then 'GET' its URN path: "redfish/v1/Managers/1/ActiveDirectory/RoleGroups/[no]".
        7. Then 'GET'/ 'PATCH'/ 'DELETE' are acceptable operations.

2. Category: New implementation
    Description:
        Get/Set iKVM mouse mode feature is added.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. 'GET' Mouse mode setting under "redfish/v1/Managers/1/MouseMode".
        2. Then 'PATCH' to path: "redfish/v1/Managers/1/MouseMode" using {"Mode": "Relative"} or one of the modes.
        3. 'GET' Mouse mode again, and mode is "Relative".
        4. 'GET' / 'PATCH' are acceptable operations.

3. Category: New implementation
    Description:
        Reset to Factory Default feature is added.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. 'POST' to path : "redfish/v1/Managers/1/Actions/Oem/ManagerConfig.Reset".
        2. 'POST' is the only acceptable operations.

4. Category: New implementation
    Description:
        Registries feature is added.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. 'GET' the main entry of Registries "redfish/v1/Registries".
        2. 'GET' the URN path "/redfish/v1/Registries/Base.1.0.0"

5. Category:Fix
   Description:
        [65776] Redfish_3.17: Patching operation does not work as expected for /redfish/v1/Managers/1/EthernetInterfaces/1/VLAN
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
        1. patch {"VLAN": {"VLANEnable": true, "VLANId": 2}}

6 Category:Fix
   Description:
        [65627] Redfish_3.16: EventService action SubmitTestEvent EventType type error
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
        1. 'POST' to path : redfish/v1/EventService/Actions/EventService.SendTestEvent with {"EventType":"Alert"}

========================================================================================
Filename: REDFISH_X10_317.bin  version: 3.17  Date: 09-22-2015

Support Motherboard: X10DRU-I+, X10DRT-P, X10DRG-H, X10DRW-I, X10DRI-T4+, X10DDW-I,
                     X10DRFR, X10DRI-T, X10DRFF, X10DRFR-T, X10DRD,
                     X10DRD-L, X10SRH

1. Category:Fix
   Description:
        [65306] Redfish_3.15: EventService subscriptions have typo.
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
        1. Goto EventService/Subscriptions/%d URI then check.

2. Category:
        Fix
   Description:
        [65118] Redfish_3.14: Patching operation does not work as expected for /redfish/v1/Managers/1/EthernetInterfaces/1
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
        1. patch {"AutoNeg": true, "FullDuplex": true} to see the result.
        2. patch {"VLAN": {"VLANEnable": true}} will get error message

3. Category: Fix
   Description:
        [65396] [Redfish 3.15]: redfish/v1/Managers/1/LogServices/Log1/Entries - shows incorrect format under "Message:"
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
        1. Read https://xxx.xxx.xxx.xxx/redfish/v1/Managers/1/LogServices/Log1/Entries/XX
        2. Check Message to see the sensor name in [], if there's no snesor name, "[]" will be removed.

4. Category: Fix
   Description:
        [65390] [redfish v3.15] "SenderAddress" string won't show in IPMIWeb GUI while PATCH "SMTP" server data thru API
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
        1. read https://xx.xx.xx.xx/redfish/v1/Managers/1/SMTP to PATCH and GET data
        2. check "SenderAddress" whether match with web gui.

5. Category: Fix
   Description
        [65557][MB: X10DRT-P] Redfish Fw-3.16: "redfish/v1/Chassis/1/Power" doesn't display any voltages if you update fw with factory default
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
        1.connect to redfish/v1/Chassis/1/Power to check voltages.

6.  Category: Fix
    Description:[65625] Redfish v3.16 : System processors have same Id.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1.get data from https://xx.xx.xx.xx/redfish/v1/Systems/1/Processors/[num]
        2.check [num] with Id whether it's match each.

7.  Category: Fix
    Description:[65565][redfish v3.16] SMTP Server is not working if PATCH server information thru /redfish/v1/Managers/SMTP/ . It won't accept email alert.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1.Do PATCH method on SMTP, then go to web and try sendtestmail or produce event to send email.

========================================================================================
Filename: REDFISH_X10_316.bin  version: 3.16  Date: 09-16-2015

Support Motherboard: X10DRU-I+, X10DRT-P, X10DRG-H, X10DRW-I, X10DRI-T4+, X10DDW-I,
                     X10DRFR, X10DRI-T, X10DRFF, X10DRFR-T, X10DRD,
                     X10DRD-L, X10SRH

1.  Category: New implementation
    Description:
        Privileged users ("ReadOnlyUser" is NOT included) can only modify theirselves password.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. Create 2 accounts with different privileges(one for "RoldId - Admin" and another is "RoleId - Operator"),
           For example, User 1 name: "supermicro" with "Admin" privilege
                        User 2 name: "dell" with "Operator" privilege
        2. Login with the users "supermicro" and "dell" respectively then modify the passwords of its own and others.
        3. The results should be - only "supermicro" can modify the paswword of itself and can not modify the password of "dell".
           On the other hand - only "dell" can modify itself password.
        4. Notice! Those users with privilege "ReadOnlyUser" can not modify its password, of course, even "Admin" still can NOT
           modify it.

2. Category: Fix
   Description:
        [65390] [redfish v3.15] "SenderAddress" string won't show in IPMIWeb GUI while PATCH "SMTP" server data thru API
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
        1. Do modification on SMTP sender address then GET it back to check.

3. Category: Fix
   Description:
        [65294] [redfish v3.15] SmtpServer won't accept "ip-address" when PATCH /redfish/v1/Managers/SMTP/.
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
        1. Modify the field, "SmtpServer", with IP-formated string then check its repsonse.

4. Category: Fix
   Description:
        [65306] Redfish_3.15: EventService subscriptions have typo.
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
        1. Goto EventService/Subscriptions/%d URI then check.

5. Category: Fix
   Description:
        [65262] [redfish v3.15] won't able change fanmode to "FullSpeed" mode via redfish API / Advanced Reset Client Application
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
        Set fan speed to "FullSpeed" fail
   Validation :
        1. Set fan speed to "FullSpeed" then check its RPM.

6. Category: Fix
   Description:
        [65468] POSTMAN got junk character
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
        1. Read https://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Power
        2. Check Powersupplies -> "Model", "FirmwareVersion", "SerialNumber"

7. Category: Fix
   Description:
        [65396] [Redfish 3.15]: redfish/v1/Managers/1/LogServices/Log1/Entries - shows incorrect format under "Message:"
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
        1. Read https://xxx.xxx.xxx.xxx/redfish/v1/Managers/1/LogServices/Log1/Entries/XX
        2. Check Message to see the sensor name in []

8. Category: Fix
   Description:
        [65118] Redfish_3.14: Patching operation does not work as expected for /redfish/v1/Managers/1/EthernetInterfaces/1
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
        1. patch "AutoNeg","FullDuplex","VLAN" to see the result.

9. Category: Fix
   Description:
        [65107] [Redfish] BIOS Update function descripe show "Undifined" when IPMI web language set to "Chinese"
   Impact motherboard: All X10 motherboards in support list
   Affected functions:
   Validation :
        1. De-activate the key.
        2. Check the BIOS update page.

========================================================================================
Filename: REDFISH_X10_315.bin  version: 3.15  Date: 09-02-2015

Support Motherboard: X10DRU-I+, X10DRT-P, X10DRG-H, X10DRW-I, X10DRI-T4+, X10DDW-I,
                     X10DRFR, X10DRI-T, X10DRFF, X10DRFR-T, X10DRD,
                     X10DRD-L, X10SRH
1. Category: New implementation
    Description:
        SMTP feature is added.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. 'GET' all managers under the URN "redfish/v1/Managers/1" to check if there is "SMTP" in "oem" catagory.
        2. Then 'GET' its URN path: "redfish/v1/Managers/1/SMTP".
        3. 'GET' / 'PATCH' are acceptable operations.

2.  Category: fix
    Description:
        [65118] Redfish_3.14: Patching operation does not work as expected for /redfish/v1/Managers/1/EthernetInterfaces/1
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. PATCH hostname under the URN path: "/redfish/v1/Managers/1/EthernetInterfaces/1".
        2. 'GET' the same URN for hostname's change.

3.  Category: fix
    Description:
        [65064] Incorrect PS sensor items in Redfish 3.14
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. Check status https://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Power

========================================================================================
Filename: REDFISH_X10_314.bin  version: 3.14  Date: 08-27-2015

Support Motherboard: X10DRU-I+, X10DRT-P, X10DRG-H, X10DRW-I, X10DRI-T4+, X10DDW-I,
                     X10DRFR, X10DRI-T, X10DRFF, X10DRFR-T, X10DRD,
                     X10DRD-L, X10SRH
1.  Category: fix
    Description:
       Remove debug message against Systems/1
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1.verify Systems/1 with LSI enabled.

2.  Category: enhancement
    Description:
       Present all EthernetInterface members against Systems/1/EthernetInterfaces
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1.verify Systems/1/EthernetInterfaces and its child path.

3.  Category: fix
    Description:
        [65010] Redfish API doens't push event to webserver
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1.Do factory default
        2.Create an event sbuscription with destination point to the webserver
        3.Remove platform FAN to generate an event.
        4.Check with your webserver's reaction.

========================================================================================
Filename: REDFISH_X10_313.bin  version: 3.13  Date: 08-26-2015

Support Motherboard: X10DRU-I+, X10DRT-P, X10DRG-H, X10DRW-I, X10DRI-T4+, X10DDW-I,
                     X10DRFR, X10DRI-T, X10DRFF, X10DRFR-T, X10DRD,
                     X10DRD-L, X10SRH

1.  Category: fix
    Description:
       [64881] [Redfish FW 3.12] Fail To Use Active Directory To Log In Redfish??        API.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1.use AD account to login redfish service.

2.  Category: New
    Description:
        X10SRH support redfish service.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :

3.  Category: Fix
    Description:
       [64832] Missing MB_10G Temp in IPMI Web GUI with REDFISH 3.12.

    Impact motherboard: X10DRU-i+, X10DRU-X(LL)
    Affected functions:
    Validation :
        1. After updating FW, power cycle the SUT.
        2. Check the MB_10G Temp1 and Temp2 value.

4.  Category: fix
    Description:
        [64840][IPMI_3.12]API Status report error
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. when pws fail, check status https://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Power
        2. also check overall status https://xxx.xxx.xxx.xxx/redfish/v1/Systems/1

5.  Category: fix
    Description:
        [64873][v3.12] will not allow save/mount virtual media drive
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1. Allow "\" character in path, \XXX\YYY.iso could be save and mount.

========================================================================================
Filename: REDFISH_X10_312.bin  version: 3.12  Date: 08-22-2015

Support Motherboard: X10DRU-I+, X10DRT-P, X10DRG-H, X10DRW-I, X10DRI-T4+, X10DDW-I,
                     X10DRFR, X10DRI-T, X10DRFF, X10DRT-HIBF, X10DRFR-T, X10DRD,
                     X10DRD-L
1.  Category: fix
    Description:
        [64571] Inconsistent Fan Fail Behavior between IPMI and Redfish
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1.Disconnecting a system fan while system is online triggers Fan Failure Alert in IPMI.
        2.https://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Thermal
        3.to see status and health of Fan sensor.

2.  Category: fix
    Description:
        Voltage sensor is absent but redfish show status OK.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1.https://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Power
        3.Check voltage sensor status.

3.  Category: fix
    Description:
        Session Audit and AC Power On event log can't show message in log service.
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1.Generate Session Audit and AC Power On event.
        2.https://xxx.xxx.xxx.xxx/redfish/v1/Managers/1/LogServices/Log1/Entries/
        3.Check event entries to see the message.

4.  Category: fix
    Description:
        [64644][IPMI_3.11] HTTPS always pops out the first time after flash
    Impact motherboard: All X10 motherboards in support list
    Affected functions:
    Validation :
        1.check if SSL redirection is enable on ipmi web.

========================================================================================
Filename: REDFISH_X10_311.bin  version: 3.11  Date: 08-14-2015

Support Motherboard: X10DRU-I+, X10DRT-P, X10DRG-H, X10DRW-I, X10DRI-T4+, X10DDW-I,
                     X10DRFR, X10DRI-T, X10DRFF, X10DRFR-T, X10DRD,
                     X10DRD-L

1.  Category: fix
    Description:
        [64504] Redfish IPMI FW 3.10: Redfish responses "200 OK" if we PATCH Accounts Password with empty string
    Impact motherboard:
    Affected functions:
    Validation :
        1. https://xxx.xxx.xxx.xxx/redfish/v1/AccountService/Accounts/3/
        2. [patch] {"UserName":"opera123", "Password":"","RoleId":"Admin"}
        3. Password length should be great than 8.

2.  Category: fix
    Description:
        [64324] Redfish 1.03: Event subscription doesnot display correct error message after creating max number of subscription

    Impact motherboard:
    Affected functions:
    Validation :
        Step1: try to create 16 subscriptions. status code should be 403.

3.  Category: fix
    Description:
        [64439] Redfish IPMI FW 3.10: After upgrading fw with factory default restored, previous event subscriptions remains present.

    Impact motherboard:
    Affected functions:
    Validation :
        1. do factory default
        2. check https://xxx.xxx.xxx.xxx/redfish/v1/EventService/Subscriptions/

4.  Category: fix
    Description:
        [64441]  Redfish IPMI FW 3.10: Redfish responses "200 OK" if we POST ComputerSystem reset operation without parsing payload.

    Impact motherboard:
    Affected functions:
    Validation :
        1.[POST] https://xxx.xxx.xxx.xxx/redfish/v1/Systems/1/Actions/ComputerSystem.Reset without payload data.
        2.will return status cod 400 and error message.

5.  Category: fix
    Description:
        [64505] Redfish 1.03: HTTP response 200 on PATCH Accounts RoleId with unknow type
    Impact motherboard:
    Affected functions:
    Validation :
        1. https://xxx.xxx.xxx.xxx/redfish/v1/AccountService/Accounts/3/
        2. [patch] {"UserName":"opera123","RoleId":"123"}
        3. will return error code and error message.

6.  Category: fix
    Description:
        [64506] Redfish 1.03: Account Collections miss Account after PATCH Account RoldId with unknow type
    Impact motherboard:
    Affected functions:
    Validation :
        1. https://xxx.xxx.xxx.xxx/redfish/v1/AccountService/Accounts/3/
        2. [patch] {"UserName":"opera123","RoleId":"123"}
        3. will return error code and error message.

7.  Category: fix
    Description:
        [64465] [Redfish] Sensor readings missing in IPMI3.10
    Impact Motherboard: MBD-X10DRU-I+-P
    Affected functions:
    Validation :
        1. https://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Power

8.  Category: fix
    Description:
        [64535] Redfish Managers/1/SerialInterface/1 InterfaceEnabled not available
    Impact motherboard:
    Affected functions:
    Validation :
        1. https://xxx.xxx.xxx.xxx/redfish/v1/Managers/1/SerialInterface/1

9.  Category: fix
    Description:
        [64556] Redfish /redfish/v1/Systems/1/Processors/2 and /redfish/v1/Systems/1/Processors/1 were swapped
    Impact motherboard:
    Affected functions:
    Validation :
        1. https://xxx.xxx.xxx.xxx/redfish/v1/Systems/1/Processors

10. Category: fix
    Description:
        SerialNumber and PartNumber of /redfish/v1/Systems/1 are from FRU0
    Impact motherboard:
    Affected functions:
    Validation :
        1. https://xxx.xxx.xxx.xxx/redfish/v1/Systems/1

========================================================================================
Filename: REDFISH_X10_310.bin  version: 3.10  Date: 08-07-2015

1. Category: fix
    Description:
    fix the mismtach for odata.type field
    Impact Motherboard: X10 motherboards
    Affected functions:
    Validation :
    1. please use PostMan to verify.

2.  Category: fix
    Description:
    fix the wrong for odata.context url
    Impact Motherboard: X10 motherboards
    Affected functions:
    Validation :
    1. please use PostMan to verify.

3.  Category: fix
    Description:
        [62000] PWS serial number does not match when run
        http://172.31.41.45/redfish/v1/Chassis/1/Power this command
    Impact Motherboard: X10 motherboards
    Affected functions:
    Validation :
        1. http://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Power
        2. Check PowerSupplies -> SerialNumber

4.  Category: fix
    Description:
        [62003] Some sensor readings are showing wrong when run
        http://172.31.41.45/redfish/v1/Chassis/1/Thermal command

    Impact motherboard: X10DRI
    Affected functions:
    Validation :
        1. http://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Thermal
        2. Check "PCH Temp" -> "Status" -> "Health"

5.  Category: fix
    Description:
        [62005] Fans sernsor reading show wrong readings when Fans are not
        plugged in with command http://172.31.41.45/redfish/v1/Chassis/1/Thermal

    Impact motherboard: X10DRI
    Affected functions:
    Validation :
        1. http://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Thermal
        2. Check "FAN" -> "Status" -> "Health"

6.  Category: fix
    Description:
        [62714] Log service entries have no detail & time stamp do not match with IPMI SEL
        when run "http://172.16.140.218/redfish/v1/Managers/1/LogServices/Log1/Entries/2" command

    Impact motherboard:
    Affected functions:
    Validation :
        1. check how many event log in BMC.
        2. Check event entries"http://xxx.xxx.xxx.xxx/redfish/v1/Managers/1/LogServices/Log1/Entries/

7.  Category: fix
    Description:
        [63641] Incorrect data type found on Redfish, using firmware version 1.0.2

    Impact motherboard:
    Affected functions:
    Validation :
        1. http://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Thermal to check "SensorNumber"  data type: Integer

8.  Category: fix
    Description:
        [63946]  redfish/v1/Chassis/1/Thermal: DIMM MIN/MAX Voltage values are not defined properly

    Impact motherboard:
    Affected functions:
    Validation :
        1. http://xxx.xxx.xxx.xxx/redfish/v1/Chassis/1/Thermal to check DIMM MIN/MAX values

8.  Category: fix
    Description:
        [64167] Redfish_FW 1.03: Event Subscription does not accept "ResourceRemoved" added inside ??Event Type??
    Impact motherboard:
    Affected functions:
    Validation :
        Step1: Posting subscription->got 201 created
            [Post]http://IP/redfish/v1/EventService/Subscriptions/
            {"Destination":"http://www.dnsname.com/Destination1","Context":"user1_test","EventTypes":["Alert","StatusChange", "ResourceRemoved"],"Protocol":"Redfish"}
        Step2: Validating Subscription:http://IP/redfish/v1/EventService/Subscriptions/

9.  Category: fix
    Description:
        [64324] Redfish 1.03: Event subscription doesnot display correct error message after creating max number of subscription

    Impact motherboard:
    Affected functions:
    Validation :
        Step1: try to create 16 subscriptions

========================================================================================
Filename: REDFISH_X10_103.bin  version: 1.03  Date: 07-27-2015

1. Category: New implementation
    Description:
        enable Https by default.
        Note:please do the reset-to-default
    Impact Motherboard: X10 motherboards
    Affected functions:
    Validation :
        1. please use PostMan to verify.

2.  Category: New implementation
    Description:
        Support NvME and LSI under Systems/1/SimpleStorage/
        Note:  LSI is restricted to LSI 3108 series
    Impact Motherboard: X10 motherboards
    Affected functions:
    Validation :
        1. MUST have NvME SSD or LSI storage card populated in the system.
        2. please use PostMan to verify.
3.  Category: Fix
    Description:
        fix the odata.context_url in some resources
    Impact Motherboard: X10 motherboards
    Affected functions:
    Validation : please use PostMan to verify.

4.  Category: New implementation
    Description:
        Support Fan Mode under /redfish/v1/Chassis/1
    Impact Motherboard: X10 motherboards
    Affected functions:
    Validation : please use PostMan to verify.

5.  Category: New implementation
    Description:
        Support EventService and send out alert through redfish.
    Impact Motherboard: X10 motherboards
    Affected functions:
    Validation : please use PostMan to verify.

========================================================================================
Filename: REDFISH_X10_102.bin  version: 1.02  Date: 06-018-2015

1.  Category: New implementation
    Description:
    Support to create, update and delete resource which is listed as below through redfish.
    It is supposed to be consistent with IPMI web.

    /redfish/v1/Systems/1
    update:
        Boot BootSourceOverrideEnabled BootSourceOverrideTarget IndicatorLED

    /redfish/v1/Managers/1
    update :
        DateTime (Note: value is changed when ntp is disabled)
        DateTimeLocalOffset (Note: value is changed when ntp is enabled)

    /redfish/v1/Managers/1/NetworkProtocol/
    update :
        HTTP
            Enabled
            Port
        HTTPS
            Enabled
            Port
        IPMI
            Enabled
            Port
        KVMIP
            Enabled
            Port
        SNMP
            Enabled
            Port
        SSH
            Enabled
            Port
        VirtualMedia (Note: When KVMIP is disabled, VirtualMedia will get disabled together)
            Enabled
            Port

    /Managers/1/SerialInterfaces/1/
    update :
        BitRate, FlowControl
    /Managers/1/EthernetInterfaces/1/
    update :
        AutoNeg, FullDuplex, SpeedMbps, HostName, VLAN{ VLANEnable, VLANId}, IPv4Addresses{ AddressOrigin, Address, SubnetMask, Gateway}, NameServers

    /AccountService/Account
        UserName Password and RoleId are required to create users.
    /AccountService/Account/[num]
        delete users and update user.
    /SesssionService/
        update :SessionTimeout

    Chassis/1/
        update: AssetTag

========================================================================================
Filename: REDFISH_X10_101.bin  version: 1.01  Date: 06-01-2015

    1.
    Category: New implementation
    Description:
        Support the below new RedFish APIs and redfish authentication following "Redfish Scalable Platforms Management API Specification"
        Be noted that please do reset-to-default and take new settings into effect.

    Impact Motherboard: X10 motherboards
    Affected functions:
    Validation : please use PostMan to verify.
        /redfish/v1/Managers/1/LogServices/
        /redfish/v1/Managers/1/LogServices/Log1/
        /redfish/v1/Managers/1/LogServices/Log1/Entries
        /redfish/v1/Managers/1/LogServices/Log1/Entries/[num]
        /redfish/v1/SessionService/
        /redfish/v1/SessionService/Sessions/
        /redfish/v1/SessionService/Sessions/[num]
        /redfish/v1/Systems
        /redfish/v1/Systems/1
        /redfish/v1/Systems/1/Processors/[num]
        /redfish/v1/Systems/1/EthernetInterfaces/[num]  (MUST install TAS)
        /redfish/v1/Managers/1/LogServices/Log1/Actions/LogService.Reset
        /redfish/v1/Managers/1/Actions/Manager.Reset
        /redfish/v1/Systems/1/Actions/ComputerSystem.Reset
    2.
    Category: Fix
    Description:
        fix the issues under the below urls.
        /redfish/v1/Chassis/1
        /redfish/v1/Chassis/1/Power/Voltages/1
        /redfish/v1/Managers/1/
        /redfish/v1/Managers/1/SerialInterfaces
        /redfish/v1/Managers/1/EthernetInterfaces

    Impact Motherboard: X10 motherboards
    Affected functions:
    Validation :
    3.
    Category: Fix
    Description:
        fix the typo on IPMI web.

    Impact Motherboard: X10 motherboards
    Affected functions:
    Validation :

========================================================================================
Filename: REDFISH_X10_100.bin  version: 1.00  Date: 04-29-2015
1.

    Category: New implementation
    Description:
        Support the below RedFish APIs.
        Be noted that please do reset-to-default and take new settings into effect.

    Impact Motherboard: X10 motherboards
    Affected functions:
    Validation :
        Please install JsonViewer and PostMan plugins in the browser, chrome or Firefox.

        /redfish/v1/
        /redfish/v1/$metadata
        /redfish/v1/Chassis
        /redfish/v1/Chassis/1
        /redfish/v1/Chassis/1/Thermal
        /redfish/v1/Chassis/1/Power
        /redfish/v1/Managers
        /redfish/v1/Managers/1
        /redfish/v1/Managers/1/NetworkProtocol
        /redfish/v1/Managers/1/EthernetInterfaces
        /redfish/v1/Managers/1/EthernetInterfaces/1
        /redfish/v1/Managers/1/SerialInterfaces
        /redfish/v1/Managers/1/SerialInterfaces/1
        /redfish/v1/AccountService
        /redfish/v1/AccountService/Accounts/
        /redfish/v1/AccountService/Accounts/[num]
        /redfish/v1/AccountService/Roles
        /redfish/v1/AccountService/Roles/Admin
        /redfish/v1/AccountService/Roles/Operator
        /redfish/v1/AccountService/Roles/ReadOnlyUser
