Filename: SMT_X11_147.bin version: 1.47 Date: 05-XX-2018
U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r35
Redfish version : 1.0.1
Redfish API : Redfish_API_full_list_2018_02_22.xlsx

1.
    Category: Fixes
    Description:
        [90273] DIMM temperature display is incorrect in IPMI Web GUI sensor reading page

    Impact motherboard:
        A2SD1

    Affected functions:
    Validation :
        1. Check DIMM temperature in sensor page.

2.
    Category: Fixes
    Description:
        [88905] SUM: Fail Test cases : 12

    Impact motherboard:
        A2SD1

    Affected functions:
    Validation :
        1. Run SUM TC219.

3.
    Category: Fixes
    Description:
        [90384] Redfish Automation: 12 critical test failed
        [90803] [IPMI ECO] Redfish Automation Test Failed
        [90804] [IPMI ECO] Redfish Automation Test Fails

    Impact motherboard:
        A2SD1, K1SPE, K1SPI

    Affected functions:
    Validation :
        1. Run Redfish Automation.

4.
    Category: Fixes
    Description:
        [90428] No SEL log entry and buzzer during overheat test

    Impact motherboard:
        K1SPE

    Affected functions:
    Validation :
        1. Heat up CPU and check event log.

5.
    Category: Fixes
    Description:
        [90427] No SEL log entry during overheat test

    Impact motherboard:
        K1SPI

    Affected functions:
    Validation :
        1. Heat up CPU and check event log.

-------------------------------------------------------------------------------
Filename: SMT_X11_146.bin version: 1.46 Date: 04-17-2018
U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r35
Redfish version : 1.0.1
Redfish API : Redfish_API_full_list_2018_02_22.xlsx

1.
    Category: Fixes
    Description:
        [88889] [ECO] PSU FAN RPM get difference value between SMCIPMITool and Web GUI.

    Impact motherboard:
        X11SSW-4TF.

    Affected functions:
    Validation :
        1. Compare the power supply fan values from both power source web gui
           and SMCIPMITOOL. it is the same.

2.
    Category: New feature
    Description: Add redfish memory information feature.
    Infected motherboard:
        All MBs
    Affected functions:
    Validation :
        1. check mothboard memory information from redfish(postman).

3.
    Category: Fixes
    Description:
        Add workaround for [88648] [BIOS ECO] SUM Test Failed

    Impact motherboard:
        K1SPI

    Affected functions:
    Validation :
        1. Run SUM.

4.
    Category: Fixes
    Description:
        [89176] No Cpu thottled ipmi event when the cpu is overheated

    Impact motherboard:
        A2SD1

    Affected functions:
    Validation :
        1. Heat CPU and check throttled event.

5.
    Category: Fixes
    Description:
        [89506] The user with "No Accres" privilege

    Impact motherboard:
        A2SD1

    Affected functions:
    Validation :
        1. Add an user with No Access privilege and check display in user page.

6.
    Category: Fixes
    Description:
        [89505] Email alert info is incorrect

    Impact motherboard:
        A2SD1

    Affected functions:
    Validation :
        1. Set alert mail and check description in mail.

7.
    Category: Fixes
    Description:
        [89500] IPMI undefined help information

    Impact motherboard:
        A2SD1

    Affected functions:
    Validation :
        1. Check help page in multinode page.

8.
    Category: Fixes
    Description:
        [89460] The VCPU drops to lower critical very often

    Impact motherboard:
        A2SD1

    Affected functions:
    Validation :
        1. Check VCPU in sensor page.


-------------------------------------------------------------------------------
Filename: SMT_X11_145.bin version: 1.45 Date: 02-06-2018
U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r35
Redfish version : 1.0.1
Redfish API : Redfish_API_full_list_2017_07_11.xlsx

1.
    Category: Fixes
    Description:
        [87561] [IPMI ECO] The Thermal Trip event log didn't follow TDG 4.06

    Impact motherboard:
        X11SSD-F

    Affected functions:
    Validation :
        1. Heat up CPU and check event log.

2.
    Category: Fixes
    Description:
        [87615] [1.43 IPMI ECO] Redfish automation tool check test fail
        [87616] [1.43 IPMI ECO] Redfish automation tool check test fail
        [88389] [IPMI ECO] Redfish automation test fail.

    Impact motherboard:
        All

    Affected functions:
    Validation :
        1. Run SATC redfish automation check tool.

3.
    Category: Fixes
    Description:
        [87831] IPMI X11 1.44 cannot trigger high fan speed during heavy IO mode

    Impact motherboard:
        A2SD1

    Affected functions:
    Validation :
        1. Heat up RT2 and check fan speed.

4.
    Category: Fixes
    Description:
        [87395][BIOS ECO 2.2] System will appear IPMI execution exception occurred while executing SUM test
        [88052] SUM – Receiving wrong completion code C0 after issued SUM GetBmcCfg/ChangeBmcCfg command
        [88407] [BIOS ECO]SUM bioseco mode test fail.

    Impact motherboard:
        All

    Affected functions:
    Validation :
        1. Run SUM.

5.
    Category: Fixes
    Description:
        [87984] IPMI unable to get IP with dedicate LAN plugged in

    Impact motherboard:
        A2SD1

    Affected functions:
    Validation :
        1. Check link status at dedicate mode.

6.
    Category: Fixes
    Description:
        [86447] A2SD1 IPMI sensor reading for PVCC_REF is incorrect
        [87644] [A2SD1-3750F] PVCC_REF is marked red at IPMI senor via WEB GUI

    Impact motherboard:
        A2SD1

    Affected functions:
    Validation :
        1. Check PVCC_REF in sensor page.

7.
    Category: Fixes
    Description:
        [87850] [IPMI V1.43 FW ECO] The help page of iKVM/HTML5 console didn't support multi-language and only support English

    Impact motherboard:
        All

    Affected functions:
    Validation :
        1. Check ikvm HTML page.


-------------------------------------------------------------------------------
Filename: SMT_X11_144.bin version: 1.44 Date: 01-05-2018
U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r35
Redfish version : 1.0.1
Redfish API : Redfish_API_full_list_2017_07_11.xlsx

1.
    Category: Fixes
    Description:
        [86676] [ECO] BMC doesn't get "Thermal Trip" event log when CPU over temp until system shutdown.

    Impact motherboard:
        X11SSV

    Affected functions:
    Validation :
        1. Heat up CPU to thermal trip and check event log.

2.
    Category: Enhancement
    Description:
        Add PUE2 mode into X11SSE-F

    Impact motherboard:
        X11SSE-F

    Affected functions:
    Validation :
        1. Check fan mode at Fan page.

3.
    Category: New Motherboard
    Description:
        New MB support A2SD1

    Impact motherboard:
        A2SD1

    Affected functions:
    Validation :
        1. New MB support A2SD1.

4.
    Category: Fixes
    Description:
        [87394] [BIOS ECO 2.2] System will appear IPMI sensor error "Non Recoverable" sensors while executing cburn stress test

    Impact motherboard:
        X11SAT-F

    Affected functions:
    Validation :
        1. Run SUM testing and check VCPUGT sensor.

-------------------------------------------------------------------------------
Filename: SMT_X11_143.bin version: 1.43 Date: 12-06-2017
U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r35
Redfish version : 1.0.1
Redfish API : Redfish_API_full_list_2017_07_11.xlsx

1.
    Category: Fixes
    Description:
        Fix web page logging problem

    Impact motherboard:
        All

    Affected functions:
    Validation :
        1. log in on web page

-------------------------------------------------------------------------------
Filename: SMT_X11_142.bin version: 1.42 Date: 12-01-2017
U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r35
Redfish version : 1.0.1
Redfish API : Redfish_API_full_list_2017_07_11.xlsx

1.
    Category: Workaround for SUM
    Description:
        [83589] [BIOS ECO 2.0c] SUM test is fail.

    Impact motherboard:
        X11SAT

    Affected functions:
    Validation :
        1. Run BIOS ECO testing.

2.
    Category: Workaround for PCH
    Description:
        [84363] PCH Temp Going Low

    Impact motherboard:
        K1SPI

    Affected functions:
    Validation :
        1. Run onoff test and check SEL page.

3.
    Category: Enhancement
    Description:
        Improvement of multi-language content on the iKVM/HTML5 option menu and submenu.

    Impact motherboard:
        All MBs

    Affected functions:
    Validation :
        1. Log in web page.
        2. To launch an iKVM over HTML5.
        3. Check the option menu and submenu do not have missing contents.

4.
    Category: Workaournd
    Description:
        VCPU voltage high alert during  AC on/off test

    Impact motherboard:
        X11SSW

    Affected functions:
    Validation :
        1. Run AC on/off and check SEL.


-------------------------------------------------------------------------------
Filename: SMT_X11_141.bin version: 1.41 Date: 08-21-2017

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r35
Redfish version : 1.0.1
Redfish API : Redfish_API_full_list_2017_07_11.xlsx

1.
    Category: Enhancement
    Description:
        Sensor readings do not update.

    Impact motherboard:
        X11SSZ

    Affected functions:
    Validation :
        1. Check sensor reading in sensor page and the value should be updated.

--------------------------------------------------------------------------------
Filename: SMT_X11_140.bin version: 1.40 Date: 08-18-2017

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r35
Redfish version : 1.0.1
Redfish API : Redfish_API_full_list_2017_07_11.xlsx

1.
    Category: Fixes
    Description:
        VcpuVRM has no sensor reading

    Impact motherboard:
        X11SSL-F

    Affected functions:
    Validation :
        1. Check VcpuVRM Temp in web page, it should have sensor reading.

---------------------------------------------------------------------------------
Filename: SMT_X11_139.bin version: 1.39 Date: 07-25-2017

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r35
Redfish version : 1.0.1
Redfish API : Redfish_API_full_list_2017_07_11.xlsx

1.
    Category: Feature
    Description:
        [Redfish] Patch an empty json payload "{}" to those APIs support PATCH,
        a 204 http status code will be responded, while to those not support PATCH,
        a 405 http status code will be responded.

    Impact motherboard:
        All MBs
    Affected functions:
        Redfish PATCH for different APIs
    Validation :
        1. Please refer the file "Redfish_API_full_list_2017_06_07.xlsx" and patch
           an empty json payload, "{}", to each API to check http status code.

2.
    Category: Feature
    Description:
        [Redfish] Nest ICANN domain in "Oem" part if there is data to show

    Impact motherboard:
        All MBs
    Affected functions:
        Redfish "Oem" parts
    Validation :
        1. Check Redfish APIs response with "Oem" key, when there is data
           inside, a ICANN domain name (e.g. Supermicro) is nested as a middle
           json payload container

3.
    Category: Enhancement
    Description:
        Redfish API rename:
        /redfish/v1/UpdateService/SSL -> /redfish/v1/UpdateService/SSLCert
        /redfish/v1/UpdateService/SSL/Actions/SSL.Upload -> /redfish/v1/UpdateService/SSLCert/Actions/SSLCert.Upload

    Impact motherboard: All
    Affected functions:
    Validation :
        Check Redfish APIs' URI of SSL related

4.
    Category: Fixes
    Description:
        [78746] [BIOS 2.0a ECO] System IPMI-SEL will happen VCPU Upper Non-recoverable going high log.
        (workaround for NCT6792)

    Impact motherboard: X11SAT

    Affected functions:
    Validation :
        1. Run in-band BIOS update.
        2. Check the PCH SEL.

5.
    Category: Enhancement
    Description:
        Change the license requirement of web GUI syslog from DCMS to OOB

    Impact motherboard: All
    Affected functions:
    Validation :
        1. web --> Configuration --> Syslog, should not be available for use
        2. enable OOB license
        3. web --> Configuration --> Syslog, should be available for use

6.
    Category: Fixes
    Description:
        [80046] [2.0b BIOS ECO] Failing DIMM location didn't match with MB silkscreen.
        [82319] [BIOS ECO 2.0b] Fail DIMM location didn't match with MB silkscreen issue.
        [82354] [BIOS ECO 2.0b] Fail DIMM location didn't match with MB silkscreen.

    Impact motherboard: X11SAT, X11SSH-F, X11SSH-CTF

    Affected functions:
    Validation :
        1. Trigger event and check the string.

7.
    Category: Fixes
    Description:
        [81013] [IPMI ECO 1.23]DCMS mods can't enabled syslog function
        [81105] [IPMI ECO 1.23]DCMS mods can't enabled syslog function  
        [81131] No OOB key is required to read syslog

    Impact motherboard: All

    Affected functions:
    Validation :
        1. Deactivate all licenses
        2. Activate DCMS license
        3. Check the web syslog page, it should be available to use
        4. Verify OOB license with the above steps as well

---------------------------------------------------------------------------------

Filename: SMT_X11_138.bin version: 1.38 Date: 06-01-2017

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r35
Redfish version : 1.0.1
Redfish API : Redfish_API_full_list_2017_04_26.xlsx

1.
    Category: Fixes
    Description:
        System installed with 3108 AOC then run cburn ON/OFF test:
            1. Cause system hang at POST stage (and IERR happens)
            2. Some affiliated HDDs within 3108 will be lost(disk drop)

    Impact motherboard:
        All motherboard which support LSI 3108 card.
        MCTP protocol are needed to be supported by the bios.

    Affected functions:
    Validation :
        1. Insert LSI 3108 card
        2. Run cburn ON/OFF test, it will automatically check:
           2-1. System hang at POST stage (and IERR happens)
           2-2. The drives lost or not
           (If you don't know how to run this verification, please contact Joe Chung(in US))

2.
    Category: Enhancement
    Description:
        Fix security vulnerability (NTP mode 6 scanner)

    Impact motherboard: All
    Affected functions:
     Validation :
        1. Please do factory default.
        2. Enable NTP in Date and Time page.
        3. Run Nessus. NTP mode 6 scanner issue should not be in test report.

3.
    Category: Fixes
    Description:
        [79700] dcmi power reading shows Instantaneous power reading 0 Watts
        (workaround for intel ME)

    Impact motherboard: X11SSH-F

    Affected functions:
    Validation :
        1. System on/off
        2. Read dcmi power reading

4.
    Category: Fixes
    Description:
        [78281] No Temperature Sensor Reading for AOM-C25G-M1SM

    Impact motherboard: X11SSE-F

    Affected functions:
    Validation :
        1. Check sensor reading in sensor page

---------------------------------------------------------------------------------
Filename: SMT_X11_137.bin version: 1.37 Date: 05-08-2017

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r35
Redfish version : 1.0.1
Redfish API : Redfish_API_full_list_2017_04_26.xlsx

01.
    Category: Fix
    Description:
        [75253] [IPMI V1.28 ECO] No Thermal Trip event in IPMI SEL

    Infected motherboard: X11SSL-CF
    Affected functions:
    Validation :
        1. heat up the CPU and trigger thermal trip

02.
    Category: Features
    Description:
        Redfish support new APIs

    Impact motherboard: all
    Affected functions:
    Validation :
        Check out the following storage APIs:
           /redfish/v1/Managers/1/VM1/CfgCD (license: OOB, SUM, DCMS, Configure ISO image settings: host, path, username and password)
           /redfish/v1/Managers/1/VM1/CfgCD/Actions/IsoConfig.Mount (license: OOB, SUM, DCMSDo mount ISO image)
           /redfish/v1/Managers/1/VM1/CfgCD/Actions/IsoConfig.UnMount (license: OOB, SUM, DCMSDo unmount ISO image)

           /redfish/v1/Managers/1/IKVM (license: DCMS, get a URL link to launch an iKVM over HTML5)

           /redfish/v1/UpdateService/SSL (license: OOB, SUM, DCMS, view current SSL certification information)
           /redfish/v1/UpdateService/SSL/Actions/SSL.Upload (license: OOB, SUM, DCMS, used to upload new SSL certification file)

           /redfish/v1/Systems/1/Storage (license: DCMS)
           /redfish/v1/Systems/1/Storage/HA-RAID (license: DCMS, For Broadcom 3108)
           /redfish/v1/Systems/1/Storage/HA-RAID/HA-RAID.[contoller_num].Volumes (license: DCMS, For Broadcom 3108)
           /redfish/v1/Systems/1/Storage/HA-RAID/HA-RAID.[contoller_num].Volumes/[volume_num] (license: DCMS, For Broadcom 3108)
           /redfish/v1/Systems/1/Storage/HA-RAID/HA-RAID.[contoller_num].Volumes/[volume_num]/Actions/Oem/Volume.Indicate (license: DCMS, For 3108, Light on respective logical drive LED)
           /redfish/v1/Systems/1/Storage/HA-RAID/HA-RAID.[contoller_num].Volumes/[volume_num]/Actions/Oem/Volume.Delete (license: DCMS, For 3108, Delete specific logical drive)
           /redfish/v1/Systems/1/Storage/HA-RAID/Actions/Oem/Storage.CreateVolume (license: DCMS, For 3108, Create logical drive against specific RAID controller)
           /redfish/v1/Systems/1/Storage/HA-RAID/Actions/Oem/Storage.ClearVolumes (license: DCMS, For 3108, Clear all logical dirves against specific RAID controller)
           /redfish/v1/Systems/1/Storage/HA-RAID/Actions/Oem/HARAIDController.Save (license: DCMS, For 3108, Save specific RAID controller's BIOS boot mode)
           /redfish/v1/Systems/1/Storage/RAIDIntegrated (license: DCMS, For RSTe, Must have TAS running)
           /redfish/v1/Systems/1/Storage/RAIDIntegrated/Volumes (license: DCMS, For RSTe, Must have TAS running)
           /redfish/v1/Systems/1/Storage/RAIDIntegrated/Volumes/[volume_num] (license: DCMS, For RSTe, Must have TAS running)
           /redfish/v1/Systems/1/Storage/SATAEmbedded (license: DCMS, For PCH SATA, Must have TAS running)
           /redfish/v1/Systems/1/Storage/SATAEmbedded/Volumes (license: DCMS, For PCH SATA, Must have TAS running)
           /redfish/v1/Systems/1/Storage/SATAEmbedded/Volumes/[volume_num] (license: DCMS, For PCH SATA, Must have TAS running)

           /redfish/v1/Chassis/HA-RAID.[contoller_num].StorageEnclosure.[enclosure_num] (license: DCMS, For Broadcom 3108)
           /redfish/v1/Chassis/HA-RAID.[contoller_num].StorageEnclosure.[enclosure_num]/Drives/Disk.Bay.[disk_num] (license: DCMS, For Broadcom 3108)
           /redfish/v1/Chassis/HA-RAID.[contoller_num].StorageEnclosure.[enclosure_num]/Drives/Disk.Bay.[disk_num]/Actions/Oem/Drive.Indicate (license: DCMS, For 3108, Light on respective physical drive LED)
           /redfish/v1/Chassis/StorageBackplane (license: DCMS, For PCH SATA or RSTe, Must have TAS running)
           /redfish/v1/Chassis/StorageBackplane/Drives/Disk.Bay.[disk_num] (license: DCMS, For PCH SATA or RSTe, Must have TAS running)
           /redfish/v1/Chassis/NVMeSSD.[pcie_controller_num].Group.[group_num].StorageBackplane.[pcie_controller_num] (license: DCMS, For NVMe)
           /redfish/v1/Chassis/NVMeSSD.[pcie_controller_num].Group.[group_num].StorageBackplane.[pcie_controller_num]/Drives/Disk.Bay.[disk_num] (license: DCMS, For NVMe)

03.
    Category: Fix
    Description:
        [78746] [BIOS 2.0a ECO] System IPMI-SELWill happen VCPU Upper Non-recoverable going high log (workaround for NCT6792)

    Infected motherboard: X11SAT-F
    Affected functions:
    Validation :
        1. check VCPU in sensor page

04.
    Category: Fix
    Description:
        [78843] IPMI Web Update BIOS Failed.

    Infected motherboard: K1SPE
    Affected functions:
    Validation :
        1. Update BIOS from WebGUI.

05.
    Category: Fix
    Description:
        [79284] K1SPi7.414 cannot update through SUM and Web GUI.
        [78566] [SUM] SUMv1.6.2 fail

    Infected motherboard: K1SPI
    Affected functions:
    Validation :
        1. Update BIOS from WebGUI.
        2. Use SUM to update BIOS.

06.
   Category: Fixes
    Description:
        When you select French keyboard layout, there some digits keys don't work.

    Impact motherboard: all
    Affected functions:
    Validation :
        1. launch java remote console.
        2. select French keyboard layout in option menu
        3. test all keys

---------------------------------------------------------------------------------
Filename: SMT_X11_136.bin version: 1.36 Date: 03-20-2017

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r33
Redfish version : 1.0.1

01.
    Category: Fix
    Description:
        [78037] FAN mode doesn't accuracy.

    Infected motherboard: X11SSW-TF
    Affected functions:
    Validation :
        1. Check FAN mode pages.

---------------------------------------------------------------------------------
Filename: SMT_X11_135.bin version: 1.35 Date: 03-16-2017

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r33
Redfish version : 1.0.1

01.
    Category: Fix
    Description:
        [78037] FAN mode doesn't accuracy.

    Infected motherboard: X11SSW-TF
    Affected functions:
    Validation :
        1. Check FAN mode pages.

02.
    Category: Fix
    Description:
        78188 No "Power Source" page in IPMI WebGUI

    Infected motherboard: K1SPI
    Affected functions:
    Validation :
        1. Check Power Source pages.

03.
    Category: Enhancement
    Description:
        [78261] [IPMI ECO v1.34] VCCSA sensor reading show Lower Critical 
        [77295] VCCSA messages in IPMI SEL during Windows rebooter test 

    Infected motherboard: X11SSH-GF, X11SSH-GTF
    Affected functions:
    Validation :
        1. check VCCSA in sensor page.

04.
    Category: Enhancement
    Description:
        [78291] [IPMI ECO] IPMI WebGUI no GPU card sensor reading

    Infected motherboard: X11SSL-F
    Affected functions:
    Validation :
        1. check GPU temperature in sensor page.

05.
    Category: Enhancement
    Description:
        [78292] [IPMI ECO] IPMI WebGUI "VcpuVRM Temp" status is N/A

    Infected motherboard: X11SSL-F
    Affected functions:
    Validation :
        1. check VRM temperature in sensor page.

---------------------------------------------------------------------------------
Filename: SMT_X11_134.bin version: 1.34 Date: 03-01-2017

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r33
Redfish version : 1.0.1

01.
    Category: Fix
    Description:
        [77378] CPU FSC doesn't go along with thermal guideline

    Infected motherboard: K1SPE
    Affected functions:
    Validation :
        1. Stress CPU and check CPU temperature.

02.
    Category: Fix
    Description:
        [77380] Fan duties fluctuates when PCI-e AOC temperatures decline from 90C

    Infected motherboard: K1SPE
    Affected functions:
    Validation :
        1. Stress AOC and check AOC temperature.

03.
    Category: Fix
    Description:
        [76240] cannot read NVMe HDD temperature in IPMI.

    Infected motherboard: X11SSH-GTF
    Affected functions:
    Validation :
        1. Power on the system.
        2. Wait the system booting to OS.
        3. Check NVMe sensor.

04.
    Category: Enhancement
    Description:
        [77916] The temperature of memory didn't show in IPMI.

    Infected motherboard: X11SSW-TF
    Affected functions:
    Validation :
        1. Power on the system.
        2. Wait the system booting to OS.
        3. Check Memory sensor temperature.
---------------------------------------------------------------------------------
Filename: SMT_X11_133.bin version: 1.33 Date: 01-05-2017

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r33
Redfish version : 1.0.1

01.
    Category: Fix
    Description:
        [74978] [ SUM 1.7.0 ] SUM test fail.

    Infected motherboard: X11SSH-F
    Affected functions:
    Validation :
        1. Download IPMI capability and check version.

02.
    Category: Fix
    Description:
        [75537] Dynamic DNS enable function is not workable.

    Infected motherboard: X11SSH-G(T)F
    Affected functions:
    Validation :
        1. Set the Time and Date NTP server first.
        2. Set DDNS config.
        3. Check the function is workable.

03.
    Category: Fix
    Description:
        [75217] [IPMI V1.28 ECO] No GPU card sensor reading

    Infected motherboard: X11SSH-F
    Affected functions:
    Validation :
        1. Check sensor reading in sensor page.

---------------------------------------------------------------------------------
Filename: SMT_X11_132.bin version: 1.32 Date: 12-16-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r33
Redfish version : 1.0.1

01.
    Category: Fix
    Description:
        [75389] No memory sensor for IPMI monitor.

    Infected motherboard: X11SSH-G(T)F
    Affected functions:
    Validation :
        1. Confirm all memory temperature sensors.

02.
    Category: New feature
    Description: Add SEL circular buffer support

    Infected motherboard: All
    Affected functions:
    Validation :
        1. enable/disable SEL circular buffer (default enable)
           When SEL logs is full (max=512), to add a new sel event log  to BMC
           Enable  -- new log will replace the oldest log.
           Disable -- new log wont’ be added to BMC.
           web and command support 
           NetFn Cmd   description                      Request Data                      Response Data
           0x30  0x73  SEL circular buffer ctrl Cmd     Data 1: 0 [Get]                   Get : Completion Code 
                                                                                            Data [ 0: disable ; 1:enable]
                                                        Data 1: 1 [Set]
                                                        Data 2: [ 0: disable ; 1:enable]  Set : Completion Code

03.
    Category: Fix
    Description:
        [75537] Dynamic DNS enable function is not workable.

    Infected motherboard: X11SSH-G(T)F
    Affected functions:
    Validation :
        1. Set the Time and Date NTP server first.
        2. Set DDNS config.
        3. Check the setting is saved.

04.
    Category: Fix
    Description:
        After HW reworking PECI path, the CPU Temperature cannot be read.

    Infected motherboard: X11SSH-G(T)F
    Affected functions:
    Validation :
        1. Check the CPU Temperature

---------------------------------------------------------------------------------
Filename: SMT_X11_131.bin version: 1.31 Date: 12-07-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r33
Redfish version : 1.0.1

01.
    Category: Hareware workaournd
    Description:
        Adjust every thresholds of Vcpu-core between 0.5v and 1.4v

    Infected motherboard: K1SPI & K1SPI
    Affected functions:
    Validation :
        1. Confirm all threholds of Vcpu-core sensor

---------------------------------------------------------------------------------
Filename: SMT_X11_130.bin version: 1.30 Date: 11-29-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r31
Redfish version : 1.0.1

01.
    Category: Fix
    Description:
        [75268] IPMI Voltage sensor fail.

    Infected motherboard: X11SSH-GTF
    Affected functions:
    Validation :
        1. Compare the IPMI reading value with DMM Reading value. (<5%)

02.
    Category: Enhancement
    Description:
        Adjust Vcpu-core Voltage and VCCU Voltage and thresholds

    Infected motherboard: K1SPI, K1SPE
    Affected functions:
    Validation :
        1. Check the thresholds of Vcpu-core sensor and VCCU sensor are different then
           the previous one
        2. Run cburn on/off test and check if no related event log occured

03.
    Category: Fix
    Description:
        [74000] Can not create raid on IPMI web.

    Infected motherboard: All X11UP MBs with our own brand LSI3108
    Affected functions:
    Validation :
        1. Loing web page and switch to the subpage - "Server Health - Storage
        Monitoring - Create Virtual Drive" to check the RAID selection and
        device selection fields.

04.
    Category: Fix
    Description:
        [75400] fan behavior weird.

    Infected motherboard: X11SSH-GF
    Affected functions:
    Validation :
        1. Make a power fail event.
        2. Check the fans don't up and down.

05.
    Category: Fix
    Description:
        [74943] NVME SSD doesn't show temperature in IPMI.

    Infected motherboard: X11SSW-TF
    Affected functions:
    Validation :
        1. Check sensor reading page

06.
    Category: Fix
    Description:
        [75018] vccsa vlotage isn't accuracy in IPMI.

    Infected motherboard: X11SSW-TF
    Affected functions:
    Validation :
        1. Check sensor reading page


---------------------------------------------------------------------------------
Filename: SMT_X11_129.bin version: 1.29 Date: 11-11-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r31
Redfish version : 1.0.1

01.
    Category: Fix
    Description: 
        [75052] When temperature increase, the fan speed of 10G unstable at standard mode
        [75053] Fan PWM measurement of 10G is fail at Heavy I/O mode

    Infected motherboard: X11SSW-TF
    Affected functions:
    Validation :
        1.switch fan mode to verify the PWM duty cycle

02.
    Category: Fix
    Description: 
        [74616] NM function can't work.

    Infected motherboard: X11SSW-TF
    Affected functions:
    Validation :
        1.issue the NM command to see the ME information

03.
    Category: Fix
    Description:
        [75079] LAN1 MAC address lost after BIOS updated through BMC on X11SSV-M4F
        [73967] Wrong Onboard LAN-1 MAC address was displayed on IPMI Web GUI

    Infected motherboard: X11SSV-M4F
    Affected functions:
    Validation :
        1.Lan-1 MAN will reserve after update BIOS.

04.
    Category: Fix
    Description:
        [73968] "VCPUGT" sensor shows "N/A" on IPMI Web GUI after firmware upgraded to v1.26

    Infected motherboard: X11SSV-M4F
    Affected functions:
    Validation :
        1. Remove VCPUGT in sensor page.

--------------------------------------------------------------------------------------
Filename: SMT_X11_128.bin version: 1.28 Date: 10-19-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r31
Redfish version : 1.0.1

01.
    Category: workaround
    Description:
        Apply MP2955 patch

    Infected motherboard: X11SSH_F, X11SAE_F, X11SSE_F, X11SSL_CF, X11SSM_F,
                          X11SSA_F, X11SSL_F, X11SSZ, X11SSD_F, X11SSH_CTF
    Affected functions:
    Validation :
        1. Apply this patch for s-line only

02.
    Category: workaround
    Description:
        Workaround for X11SSE 8211F lost IP when boot up.

    Infected motherboard: X11SSE_F
    Affected functions:
    Validation :
        1. X11SSE would not lost IP when boot up.

03.
    Category: Fix
    Description: 
        [73341] X11SSV-M4F_Rev1.01 Hardware Monitor Fail

    Infected motherboard: X11SSV-M4F
    Affected functions:
    Validation :
        1.check VCPU and 3.3VSB on sensor page.
--------------------------------------------------------------------------------------
Filename: SMT_X11_127.bin version: 1.27 Date: 10-11-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r31
Redfish version : 1.0.1

01.
    Category: workaround
    Description:
        Apply MP2955 patch

    Infected motherboard: X11SSH_F, X11SAE_F, X11SSE_F, X11SSL_CF, X11SSM_F,
                          X11SSA_F, X11SSL_F, X11SSZ, X11SSD_F, X11SSH_CTF
    Affected functions:
    Validation :
        1. After updating FW, shoule have seen similar log to the following one:
            ...
            It is MPS2955
            Check page0 value
            Match expected value
            Check page1 value
            Mis-Match, program new value: 0x 9 0x64
            Switch back to page0
            ...

02.
    Category: New Motherboard
    Description: 
             Support X11SSW-TF

    Infected motherboard: X11SSW-TF
    Affected functions:
    Validation :

03.
    Category: Fix
    Description: 
        74183 "UID Control" displayed since the platform did not support UID feature

    Infected motherboard: X11SSV-M4F
    Affected functions:
    Validation :
        1.check web gui.
--------------------------------------------------------------------------------------
Filename: SMT_X11_126.bin version: 1.26 Date: 09-19-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r31
Redfish version : 1.0.1

01.
    Category: Fix
    Description:
        73322 [ SUM 1.6.1 ] Get BMC config fail.
	73753 [KBL BIOS ECO] SUM can't test

    Infected motherboard: All
    Affected functions:
    Validation :
        1. Run sum GetBmcCfg

02.
    Category: Fix
    Description:
        73337 The 5VSB sensor reading is incorrect

    Infected motherboard: X11SSV-M4F
    Affected functions:
    Validation :
        1. Open sensor page and check 5VSB reading.

03.
    Category: Fix
    Description:
        72709 Run SMSTC is FAIL

    Infected motherboard: All
    Affected functions:
    Validation :
        1. Run sum GetBmcInfo

04.
    Category: New Motherboard
    Description:
        Support X11SSH-GF/GTF.

    Infected motherboard: X11SSH-GF/GTF
    Affected functions:
    Validation :

--------------------------------------------------------------------------------------
Filename: SMT_X11_125.bin version: 1.25 Date: 08-11-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r27
Redfish version : 1.0.1

01.
    Category: FW release
    Description: Add X11SSV-M4f board support

    Infected motherboard: X11SSV-M4F
    Affected functions:
    Validation :
        1. Add sensor list.

02.
    Category: New feature
    Description: Add NVME support
        [71116] [SMCIPMITOOL] Some NVME informations showed "unknown" on "Locate" amd "slot".

    Infected motherboard: X11SSL-nF
    Affected functions:
    Validation :
        1. connect on board nvme.
        2. check sensor page

03.		
    Category: Fix
    Description:
      Activated OOB License is missed when updating FW from ~1.22 to 1.23-1.24

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Use programmer to burn FW prior to 1.22. For example, 1.20.
        2. Activate OOB license by cburn "OOBB" and wait the action is finished.
        3. Update 1.25 FW. Then enter bios updating page, it should be activated.
        4. Downgrade to older FW between 1.23 and 1.24.
        5. Enter bios updating page, it should be activated.
        6. Use programmer to burn FW between 1.23 and 1.24.
        7. Activate OOB license by cburn "OOBB" and wait the action is finished.
        8. Update 1.25 FW. Then enter bios updating page, it should be activated.
        9. Downgrade to older FW prior to 1.22. For example, 1.20.
       10. Enter bios updating page, it should be activated.

--------------------------------------------------------------------------------------
Filename: SMT_X11_124.bin version: 1.24 Date: 06-24-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r27
Redfish version : 1.0.1

01.
    Category: Enhancement
    Description:
        change board ID, K1SPE: 0x09 0x42, K1SPE_IN001: 0x09 0x0E
    Impact motherboard: K1SPE
    Affected functions:
    Validation :
         1. Login webui.
         2. Check sensor reading in sensor page.

02.
    Category: Fix
    Description:
        [71364][IPMI] IPMI power consumption doesn't match up with Power meter reading.
    Impact motherboard: All multi-node platforms
    Affected functions:
    Validation :
         1. Refresh and login webui.
         2. See multi node web page.

--------------------------------------------------------------------------------------
Filename: SMT_X11_123.bin version: 1.23 Date: 06-07-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r27
Redfish version : 1.0.1

01.
    Category: Fix
    Description:
        71329 [IPMI] IPMI Web Session Timeout During IPMI and BIOS Flash
    Impact motherboard: X11SSE
    Affected functions:
    Validation :
         1. Login webui.

02.
    Category: Enhancement
    Description:
        Change copyright 2015 to 2016
    Impact motherboard: All
    Affected functions:
    Validation :
         1. Login webui.

03.
    Category: Fix
    Description:
        [70064] No AOC Temperature Sensors
    Impact motherboard: K1SPE
    Affected functions:
    Validation :
         1. Login webui.

04.
    Category: Enhancement
    Description:
        Add NVDIA K20 GPU support.
        [71181] NVDIA K20 GPU sensor reading issue
    Impact motherboard: X11SSZ
    Affected functions:
    Validation :
         1. check sensor page.

05.
    Category: Fix
    Description:
        [71580] [SUM 1.6.1] Get dmiinfo fail after 1000+ cycles.
    Impact motherboard: All
    Affected functions:
    Validation :
         1. Run the test case 502.
         2. It should pass 2000 times.

06.
    Category: Enhancement
    Description:
        [71561] FAN A keeps going "lower critical" with rev 1.01 mb
    Impact motherboard: K1SPE
    Affected functions:
    Validation :
		 1. reset to default
         2. check SEL page.

07.
    Category: Enhancement
    Description:
        [71327] [IPMI] Unexpected IPMI Events during RHEL 7.x installation.
    Impact motherboard: All
    Affected functions:
    Validation :
         1. check SEL page.

--------------------------------------------------------------------------------------
Filename: SMT_X11_122.bin version: 1.22 Date: 05-20-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r27
Redfish version : 1.0.1

01.
    Category: Fix
    Description:
        [70916] Set FRU1 Baseboard Version to R1.01 and FANB Sensor Missing.
    Impact motherboard: K1SPE K1SPE-IN001
    Affected functions:
    Validation :
         1. Use the same firmware to upgrade K1SPE and K1SPE-IN001 boards.
         2. Check the sensor web page.

02.
    Category: Fix
    Description:
        [69117] Multi Node Feature Shows Incorrect Values
    Impact motherboard: X11SSE
    Affected functions:
    Validation :
        1. View multi node webpage.

03.
    Category: Fix
    Description:
        [71042] [Red_Fish] Can't Support Red Fish Automation Test
    Impact motherboard: K1SPI
    Affected functions:
    Validation :
        1. Run redfish autotool.

--------------------------------------------------------------------------------------
Filename: SMT_X11_121.bin version: 1.21 Date: 05-09-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r27
Redfish version : 1.0.1

01.
    Category: New feature
    Description:
        Add redfish support in K1SPE
    Impact motherboard: K1SPE
    Affected functions:
    Validation :
         1. Need to reset to default after upgrade.
         2. Need oob licence to support redfish deature.
--------------------------------------------------------------------------------------
Filename: SMT_X11_120.bin version: 1.20 Date: 05-05-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r27
Redfish version : 1.0.1

01.
    Category: Fix
    Description:
        [70888] Multi Node shows incorrect power and current consumption.
    Impact motherboard: K1SPI
    Affected functions:
    Validation :
        1. View multi node webpage

02.
    Category: Fix
    Description:
        [70944] [IPMI] LCMC Firmware Information String Not Aligned
    Impact motherboard: K1SPI
    Affected functions:
    Validation :
        1. View multi node webpage.

03.
    Category: Fix
    Description:
        [70950] [IPMI] Multi Node: Remove CPU2 Temp
    Impact motherboard: K1SPI
    Affected functions:
    Validation :
        1. View multi node webpage.
--------------------------------------------------------------------------------------
Filename: SMT_X11_119.bin version: 1.19 Date: 04-XX-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r27
Redfish version : 1.0.1

01.
    Category: Fix
    Description:
        [70888] Multi Node shows incorrect power and current consumption.
    Impact motherboard: K1SPI
    Affected functions:
    Validation :
        1. View multi node webpage

02.
    Category: Enhancement
    Description:
        [70884] [IPMI] Memory Temperature Sensor String Does Not Match Motherboard Silkscreen
    Impact motherboard: K1SPI
    Affected functions:
    Validation :
        1. Open Sensor page and check string of DIMM temperature.
--------------------------------------------------------------------------------------
Filename: SMT_X11_118.bin version: 1.18 Date: 04-29-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r27
Redfish version : 1.0.1

01.
    Category: Fix
    Description:
        [70256] [IPMI] Multi node function doesn't work.
    Impact motherboard: K1SPI
    Affected functions:
    Validation :
        1. View multi node webpage

02.
    Category: Fix
    Description:
        [70742] There is no PWS readings under sensor page and no PWS failure LED as well, no SEL for failed Power Supply module as well.
    Impact motherboard: K1SPI
    Affected functions:
    Validation :
        1. PSU sensor will show in sensor page.

03.
    Category: New feature
    Description:
        Differentiate intel OEM and STD K1SPE from FRU1.
    Impact motherboard: K1SPE
    Affected functions:
    Validation :
        1. Use different fan curve by different board produce name in FRU1

04.
    Category: Fix
    Description:
        [70841] false SEL messages about AOC 3108 as "Drive Fault @ slot255" under IPMI webgui
    Impact motherboard: K1SPE
    Affected functions:
    Validation :
        1. Plug in a AOC3108 on MB then boot and login to web to check eventlog subpage.

05.
    Category: Enhancement
    Description:
        Change the sensor threshold of P1V0_VCCPIO for K1SPE to support FTU.
    Impact motherboard: K1SPE
    Affected functions:
    Validation :
        1. Run FTU tool
        2. See the FTU log file
--------------------------------------------------------------------------------------
Filename: SMT_X11_117.bin version: 1.17 Date: 04-19-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r27
Redfish version : 1.0.1

01.
    Category: New feature
    Description:
        10G/40G Naming rule change
    Impact motherboard: All X11 MB
    Affected functions:
    Validation :
        1. Change 10G/40G name to AOC_NIC_Temp

02.
    Category: Fix
    Description:
        [69484] [BIOS 1.0c ECO] SUM test fail
        [70158] [ SUM 1.6.1(2016/03/18) ] Test fail.
    Impact motherboard: All
    Affected functions:
    Validation :
        1. Do factory default action
        2. Run SUM test

03.
    Category: Enhancement
    Description:
        Support GPU threshold in GPU thermal guide 1.09.
    Impact motherboard: All
    Affected functions:
    Validation :
        1. Reset to factory default by using the following command:
           ipmitool -I lanplus -H ${BMC_IPADDR} -U ADMIN -P ADMIN raw 0x30 0x40
        2. power on the system with GPU card.
        3. Check the GPU sensor threshold, refer to GPU thermal guide 1.09
        (table 5-2) for detail threshold value.

04.
    Category: Fix
    Description:
      [70101] [IPMICFG] Change gate way fail.

    Impact motherboard: All
    Affected functions:
    Validation :
        1. ipmicfg -dhcp off.
        2. ipmicfg -m {IP}.
        3. ipmicfg -k 255.255.255.0
        4. ipmicfg -g {GateWay IP}

05.
    Category: Enhancement
    Description:
        [70122] [IPMI] IPMI shows PCH low criticial temperature events.

    Impact motherboard: K1SPI
    Affected functions:
    Validation :
        It will not show alert when PCH temperature unavailable in short time.

06.
    Category: Fix
    Description:
        [70058] [BIOS/IPMI] No temperature reading on AOC-S40G-i2Q.

    Impact motherboard: K1SPI
    Affected functions:
    Validation :
        1. View the sensor reading web page.

07.
    Category: Fix
    Description:
        [70520] Incorrect Fan Speed Control Mode in FW Rev1.16

    Impact motherboard: K1SPI
    Affected functions:
    Validation :
        Check K1SPI fan zone.

08.
    Category: Enhancement
    Description:
        [70142] [HW/IPMI] VBAT voltage is going criticial low for some reason.

    Impact motherboard: K1SPI
    Affected functions:
    Validation :
        Check sensor page and SEL.

09.
    Category: Fix
    Description:
        [70389] there is no Fan speed control

    Impact motherboard: K1SPI
    Affected functions:
    Validation :
        1. Change the fan mode
        2. See the fan speed in sensor reading web page

10.
    Category: Fix
    Description:
        [70315] There is no CPU OH LED in front panel when CPU goes to critical temperature

    Impact motherboard: K1SPI
    Affected functions:
    Validation :
        1. Trigger overheat event
        2. See the overheat LED

11.
    Category: Fix
    Description:
        [70345] IPMI SEL gets "P0V75_VCCCLR" upper critical high during PTU stress test

    Impact motherboard: K1SPI
    Affected functions:
    Validation :
        1. Run PTU stress
        2. See the SEL event

--------------------------------------------------------------------------------------
Filename: SMT_X11_116.bin version: 1.16 Date: 03-24-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24
Redfish version : 1.0.1

01.
    Category: Fix
    Description:
        [67570] Do we support power supply info "PS1 & PS2"uner IPMI sensor readings?
    Impact motherboard: K1SPI
    Affected functions:
    Validation :
        1. Power supply sensor woild show in sensor page.

02.
    Category: Fix
    Description:
        [67996] No Power fail LED in front panel when removed AC code from power supply & there is no SEL message about power failure either
    Impact motherboard: K1SPI
    Affected functions:
    Validation :
        1. Power fail LED will blinking when remove AC cord.

03.
    Category: Fix
    Description:
        [68921] WebGUI Help Menu Missing
    Impact motherboard: X11SSE-F
    Affected functions:
    Validation :
        1. Open LCMC update page and click help.

04.
    Category: Fix
    Description:
        [69138] [IPMI] 10G Temperature Sensor Shown on K1SPE SKU
    Impact motherboard: K1SPE
    Affected functions:
    Validation :
        1. Open sensor page to check.

05.
    Category: Fix
    Description:
        [68484] Fail HWM VBat, IPMI FW:0.59
    Impact motherboard: K1SPE
    Affected functions:
    Validation :
        1. Open sensor page to check.

06.
    Category: New feature
    Description:
        support html5
    Impact motherboard: All X11 MB
    Affected functions:
    Validation :
        1. Need to reset to default after upgrade.

07.
    Category: New feature
    Description:
        Web GUI improvements
    Impact motherboard: All X11 MB
    Affected functions:
    Validation :
        1. power control by upper-right corner new power button.

08.
    Category: Fix
    Description:
        [68568] No Temperature Sensor in IPMI for AOC-CTGS-i2T
    Impact motherboard: X11SSE-F
    Affected functions:
    Validation :
        1. 10G sensor will show in sensor page as static sensor.

09.
    Category: Fix
    Description:
        [69117] Multi Node Feature Shows Incorrect Values
    Impact motherboard: X11SSE-F
    Affected functions:
    Validation :
        1. Currect output current in multinode page.

--------------------------------------------------------------------------------------
Filename: SMT_X11_115.bin version: 1.15 Date: 02-19-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24
Redfish version : 1.0.1

01.
    Category: Fix
    Description:
        Cannot access GUI by IPv6 address when both "web port" and "web ssl port" are enabled.
    Impact motherboard: All
    Affected functions:
    Validation :
        1. Enable "web port" and "web ssl port" in port setting.
        2. Connect to the web ssl port by using IPv4 and IPv6 separately with browser.
        3. GUI should be accessable by both IPv4 and IPv6 address.

02.
    Category: Fix
    Description:
        [68467] Wrong CPU sensor id
        [68464] Wrong sensor id Chassis

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Set the SMTP and alert correctly.
        2. Generate CPU/Chassis related SEL.
        3. Check the email wording.

03.
    Category: Fix
    Description:
        [68879] No sensor reading of intel 3120A

    Impact motherboard: X11SAT
    Affected functions:
    Validation :
        1. Check this sensor in web page

04.
    Category: Fix
    Description:
        [68993] Sensor name of alert mail is not match Web Event log for
                CPU Overheat, Chassis Intru, Power Fail
        [68958] Sensor name of alert mail is not match Web Event log for
                CPU Overheat, Chassis Intru
        [68952] Sensor name of alert mail is not match Web Event log for
                CPU Overheat, Chassis Intru

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Set the SMTP and alert correctly.
        2. Generate CPU/Chassis related SEL.
        3. Check the email wording.

05.
    Category: Fix
    Description:
        [69135] Inconsistent GUI Content Descriptions, Help Message, and Titles

    Impact motherboard: All
    Affected functions:
    Validation :
        1. Please check IPMI Web GUI.

--------------------------------------------------------------------------------------
Filename: SMT_X11_114.bin version: 1.14 Date: 01-20-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24
Redfish version : 1.0.1

01.
     category: new feature
     description:
        Support redfish

     impact motherboard: All
     affected functions:
     validation :
         1. Need to reset to default after upgrade.
         2. Need oob licence to support redfish deature.

02.
     category: fix
     description:
        [67682] No CPU Overheat beep sound

     impact motherboard: X11SAT
     affected functions:
     validation :
         1. Trigger CPU oveheat and check this function.

03.
     category: Enhancement
     description:
        add IPMI FW recovery mechanism.
    
     impact motherboard: All
     affected functions:
     validation :
         1. do AC off while IPMI fw is updating
         2. FW will enter the recovery mode and update fw again by using
            inband update tool, like adupdate -f  fw filename.

04.
     category: fix
     description:
        [67900] USB drop and CPU sensor gone when system idle

     impact motherboard: X11SSH-TF
     affected functions:
     validation :
         1. VCPU will not disappear when system idle

05.
     category: fix
     description:
         [68114] X11SSL-CF 0x34 (Vcpu) voltage error

     impact motherboard: X11SSL-CF
     affected functions:
     validation :
         1. CPU temperature and ADC sensor will show normally.

06.
     category: fix
     description:
        [67484] IPMI Web didn't show add-on card sensor reading

     impact motherboard: All
     affected functions:
     validation :
         1. AOC sensor reading will show normally.

07.
     category: Enhancement
     description:
        Change SNMP WEB UI layout.

     impact motherboard: All
     affected functions:
     validation :
         1. SNMP V2 and V3 can enable at same time.

--------------------------------------------------------------------------------------
Filename: SMT_X11_113.bin version: 1.13 Date: 01-15-2016

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

01.
     category: fix
     description:
        [67407] [SUM] SUM test was fail.

     impact motherboard: X11SAT
     affected functions:
     validation :
         1. Reset to default will be share mode in X11SAT

02.
     category: fix
     description:
        [67748] Sometimes cannot open iKVM console after update IPMI V110 FW

     impact motherboard: All
     affected functions:
     validation :
         1. Clear java cache by java control panel
         2. Lunch iKVM console by web GUI 

03.
     category: fix
     description:
        [68216] [BIOS 1.0a ECO] SUM can not be verified in only one LAN board

     impact motherboard: X11SAE
     affected functions:
     validation :
         1. Reset to default will be share mode in X11SAE

04.
    category: fix
    description:
        [67743] X11SAT-F IPMI support share LAN only, so Network Status Link should be remove Dedicated LAN status

    impact motherboard: X11SAT-F
    affected functions:
    validation :
        1. check IPMI web network setting page

--------------------------------------------------------------------------------------
Filename: SMT_X11_112.bin version: 1.12 Date: 12-31-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

01.
     category: workaround
     description:
        [68084] VCPU sensor upper critical-going high idle in OS

     impact motherboard: All
     affected functions:
     validation :
         1. VCPU value greater than 1.7 will be filtered out.

02.
     category: fix
     description:
        [67922] No BIOS Version in IPMI Summary page

     impact motherboard: All X11 motherboards
     affected functions:
     validation :
         1. login to web to check BIOS version.

03.
     category: fix
     description:
        [67419] 40G and 10G has no temperature reading in IPMI

     impact motherboard: All X11 motherboards
     affected functions:
     validation :
         1. check web sensor reading page

04.
     category: fix
     description:
        [68216] [BIOS 1.0a ECO] SUM can not be verified in only one LAN board

     impact motherboard: All X11 one LAN motherboard.
     affected functions:
     validation :
         1. Run sum test.

05.
     category: workaround
     description:
        [68089] System Hang after Flashed BIOS in IPMI Web

     impact motherboard: X11SSA
     affected functions:
     validation :
         1. Add workaround for ME which command will time out after "force recovery
         mode" and "ME reset."


--------------------------------------------------------------------------------------
Filename: SMT_X11_111.bin version: 1.11 Date: 12-15-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

01.
     category: fix
     description:
        [67689] Cannot control Watchdog by ipmitool cmd

     infected motherboard: X11SAT-F
     affected functions:
     validation :
         1. Set wdt by ipmitool and will reset system in setting time.

02.
     category: fix
     description:
        [67587] Hardware sensor "VCPU" alarm threshold setting not correct

     infected motherboard: X11SAT-F
     affected functions:
     validation :
         1. VCPU voltage will not show low critical if voltage > 0V.

03.
     category: work around
     description:
     [67400] Normal Open lost CPU sensor during running ONOFF test

     infected motherboard: X11SSH-F
     affected functions:
     validation :
         1. View sensor reading web page and check the value.

--------------------------------------------------------------------------------------
Filename: SMT_X11_110.bin version: 1.10 Date: 12-04-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

01.
     category: fix
     description:
        [66505] MCU Info cannot Got 

     infected motherboard: X11SSE-F
     affected functions:
     validation :
         1.Write down board number and serial number by Ipmiview or Ipmicfg in advice
         2.Check these information on node1

02.
     category: fix
     description:
        [67317] Redirect IPMI web to the login page fail after factory default.

     infected motherboard: X11SBA
     affected functions:
     validation :
         1. Do factpry default and Web page will redirect after in 90s.

03.
     category: fix
     description:
        [67254] No power supply information in DMI table.
        [67178] SUM Test Fail
        [66945] Power fail status not follow design rule (add workaround)

     infected motherboard: X11SSE-F
     affected functions:
     validation :
         1. dmiinfo could show right ps number

04.
     category: fix
     description:
        [67501] IPMI BIOS Update page show "Undefined" when language set to "Simplified Chinese".

     infected motherboard: All X11 motherboards
     affected functions:
     validation :
         1. check BIOS Update page at website.

05.
     category: fix
     description:
        [67400] lost CPU sensor during running ONOFF test
        [66753] IPMI got some sensor reading lost after on/off test

     infected motherboard: X11SSH-F, X11SSE-F
     affected functions:
     validation :
         1. Do ac on/off, CPU temperature will not lost.

06.
     category: fix
     description:
        [67217] [IPMI] HDD status always is Drive Fault
        [67245] IPMI web sensor reading not consistent with IPMItool sensor reading.
        [67242] IPMI got CPU throttled and Vcpu lower critical.

     infected motherboard: X11SSE-F
     affected functions:
     validation :
         1. check HDD status in sensor page.
         2. check PS status and vcpu in sensor page.
         3. Remove power cords will not trigger PROCHOT. (for HW workaround)

07.
     category: fix
     description:
        [67244] Multi Node Monitoring is not working in IPMI web GUI.

     infected motherboard: X11SSE-F
     affected functions:
     validation :
         1. check multinode status in multinode page.

--------------------------------------------------------------------------------------
Filename: SMT_X11_055.bin version: 0.55 Date: 11-18-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

01.
     category: fix
     description:
        [67045] no PCH & DIMM temp in IPMI 

     infected motherboard: X11SAT-F
     affected functions:
     validation :
         1. View sensor reading web page and check the corresponding value.
02.
     category: fix
     description:
        [67007] 12Vcc & Vcpu IPMI reading fail

     infected motherboard: X11SAT-F
     affected functions:
     validation :
         1. View sensor reading web page and check the corresponding value.
03.
     category: fix
     description:
        [66918] Power fail LED frequency can not meet spec.

     infected motherboard: X11SAT-F
     affected functions:
     validation :
        1. Trigger power fail event and view the operation of LED.
04.
     category: fix
     description:
        [66456] Overheat LED can't work.

     infected motherboard: X11SAT-F
     affected functions:
     validation :
        1. Trigger CPU overheat event and view the operation of LED.
05.
     category: fix
     description:
        [67086] The IPMI hardware monitor test fail.

     infected motherboard: X11SSD-F
     affected functions:
     validation :
        1. View sensor reading web page and check the corresponding value.
06.
     category: fix
     description:
        [66826] No Thermal Trip event.

     infected motherboard: X11SSD-F
     affected functions:
     validation :
        1. Trigger CPU thermal trip.
07.
     category: fix
     description:
        [66825] CPU Overheat function still is not working.

     infected motherboard: X11SSD-F
     affected functions:
     validation :
        1. Trigger CPU overheat event and view the operation of LED.
08.
     category: fix
     description:
        [66794] Cannot set P/T state manually by smcipmitool.

     infected motherboard: X11SSD-F
     affected functions:
     validation :
        1. Setting P/T state value through nm command by smcipmitool.

--------------------------------------------------------------------------------------
Filename: SMT_X11_054.bin version: 0.54 Date: 11-04-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

01.
     category: fix
     description:
        Correct accuracy of sensor reading for 3.3VSB, VCCSA, and Vcpu.

     infected motherboard: All X11 motherboards.
     affected functions:
     validation :
        1.Open sensor reading page and check value.
02.
     category: FW release
     description: Add X11SSD-F

     infected motherboard: X11SSD-F
     affected functions:
     validation :
         1. Add sensor list.
03.
     category: fix
     description:
        [66406] IPMI Sensor Reading function can't data.

     infected motherboard: X11SAT
     affected functions:
     validation :
        1.View sensor reading page and check value.
04.
     category: fix
     description:
        [66407] IPMI FAN control function can't work

     infected motherboard: X11SAT 
     affected functions:
     validation :
         1. Change the fan mode.
         2. Check the fan behavior meet Thermal Guideline.

--------------------------------------------------------------------------------------
Filename: SMT_X11_053.bin version: 0.53 Date: 10-16-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

01.
     category: fix
     description:
        [66184] [SUM] Run SMSTC is FAIL
        [66134] [SUM] Run SMSTC is FAIL
        [66104] [BIOS ECO v1.00] SUM test fail
        [65960] [SUM] Run SMSTC test is FAIL
        [65941] [SUM] SUM Test case 215,305,306,307,313 failed.
        [65688] [SUM1.6.0] SUM test failed.
        [65614] [ SUM 1.6.0 ] SUM test fail.
        [64892] [SSM] Case311-002 "Change BMC Cfg" is fail.
        [64828] SUM test fail.
        [62270] SUM Test Failed


     infected motherboard: All X11 motherboards.
     affected functions:
     validation :
         1. Run SUM test case 211, 212, 215, 305, 306, 410, 412.

02.
     category: workaround
     description:
       [66054] No Thermal Trip event.

     infected motherboard: X11SAE-F
     affected functions:
     validation :
         1. Over heat CPU to trigger thermal trip event.

--------------------------------------------------------------------------------------
Filename: SMT_X11_052.bin version: 0.52 Date: 10-02-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

01.
     category: workaround
     description:
       [65807] VCPU sensor upper critical-going high during ONOFF test. 

     infected motherboard: X11SSH X11SSM X11SSL
     affected functions:
     validation :
         1. VCPU would ignore value over 1.6V for HW glitch.

02.
     category: fix
     description:
       Redirect IPMI WEB to the login page after executing factory default.

     infected motherboard: All X11 motherboards.
     affected functions:
     validation :
         1. Try factory default and then wait for FW reboot.

--------------------------------------------------------------------------------------
Filename: SMT_X11_051.bin version: 0.51 Date: 09-26-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

01.
     category: fix
     description:
       [65628] Check NM firmware version failed

     infected motherboard: X11 MB with SPS FW supported.
     affected functions:
     validation :
         1. It would not show "support node manager" when command nm detect.

02.
     category: fix
     description:
       [65270] E-burn stress test will generate Power Supply Event in ipmi-sel log.
       [65807] VCPU sensor upper critical-going high during ONOFF test. 

     infected motherboard: X11SSL-F, X11SSM-F.
     affected functions:
     validation :
         1. Run the on-off test.
         2. Check the SEL.

--------------------------------------------------------------------------------------
Filename: SMT_X11_050.bin version: 0.50 Date: 09-XX-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

01.
     category: fix
     description:
       [64713] Virtual Media cannot be saved

     infected motherboard: All X11 MB.
     affected functions:
     validation :
         1. The mount path include "\" could be save.

02.
     category: fix
     description:
       [64643]  VCPU sensor upper critical-going high during ONOFF test

     infected motherboard: X11SSH-F
     affected functions:
     validation :
         1. Vcpu reading over 1.77 will be filter 3 timesby this change.

--------------------------------------------------------------------------------------
Filename: SMT_X11_049.bin version: 0.49 Date: 08-26-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

01.
     category: fix
     description:
       [64370] There's 10G temperature reading item on IPMI Web
       [64444] [X11SSZ-QF] X11SSZ-QF not support 10G LAN, but still has "MB_10G Temp" item in IPMI Sensor Reading page

     infected motherboard: X11SSZ-QF
     affected functions:
     validation :
         1. 10G sensor would not show in X11SSZ-QF

02.
     category: fix
     description:
       [64371] Sometimes VCPUGT reading will show as 0
       [62657] IPMI Hardware Monitor Check fail

     infected motherboard: X11SSZ-QF X11SSZ-TLN4F
     affected functions:
     validation :
         1. Remove sensor VCPUGT

03.
     category: fix
     description:
       [64685] Somtimes cannot detect CPU Temp in IPMI Sensor Reading page

     infected motherboard: X11SSH-CTF, X11SSH-TF
     affected functions:
     validation :
         1. CPU Temp should detected on sensor page.

04.
     category: fix
     description:
       Enable thermal trip function.

     infected motherboard: X11SSH-CTF
     affected functions:
     validation :
         1. New thermal trip event log after thermail trip.

05.
     category: fix
     description:
       Enable thermal trip function.

     infected motherboard: X11SSE, X11SSA
     affected functions:
     validation :
         1. New thermal trip event log after thermail trip.

06.
     category: fix
     description:
       [64845] Function fail : X11SBA H/W monitor data can’t be read if IPMI can’t get IP.

     infected motherboard: x11sba-f/-ln4f
     affected functions:
     validation :
         1. Keep LAN unpluged.
         2. Boot to BIOS and use ipmicfg to get sensor reading ("ipmicfg -sdr").

--------------------------------------------------------------------------------------
Filename: SMT_X11_048.bin version: 0.48 Date: 08-10-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

01.
     category: fix
     description:
       [64159] word of activate license page will show "undefined" when language
       set to "simplified chinese"

     infected motherboard: x11sba-f/-ln4f
     affected functions:
     validation :
         1. open web page in simplified chinese language setting then switch
         to "activate license" sub item.

02.
     category: fix
     description:
       [63613] Power LED didn't blink when system enter S3 state
       [62805] LED frequency fail

     infected motherboard: x11sba-f/-ln4f
     affected functions:
     validation :
         1. Power on then wait for OS enter working state
         2. Set "Action performed when power button is pressed" to "Sleep" or
         "Hibernate" then save.
         3. Press power button to check power LED's blinking frequency.

03.
     Category: Fix
     Description:
       [64184 ] Functional fail : X11SBA-F/-LN4F R1.01 JL1 no function
       [64158 ] Jumper JL1 function could not be validated

     Infected motherboard: X11SSE-F
     Affected functions:
     Validation :
         1. Short JL1 jumper, then check IPMI web sensor reading page to see
            if chassis intrution is occurred.
         2. Press "Intrusion Reset" to clear.

--------------------------------------------------------------------------------------
Filename: SMT_X11_047.bin version: 0.47 Date: 07-31-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

01.
     Category: Fix
     Description:
       [64010] [EVT] Many IPMI Sensors Missing
       [64086] [EVT] NM No Working

     Infected motherboard: X11SSE-F
     Affected functions:
     Validation :
         1. Check IPMI sensor reading page.
         2. Check Node manager function by SMCIPMITOOL

02.
     Category: Fix
     Description:
       [63937] FAN5 no sensor reading

     Infected motherboard: X11SAE-F
     Affected functions:
     Validation :
         1. Check IPMI sensor reading page for FAN5 reading.

03.
     Category: Fix
     Description:
       [63861] IPMI didn't show add-on card sensor reading

     Infected motherboard: X11SSZ
     Affected functions:
     Validation :
         1. Check IPMI sensor reading page for AOC temperature.

04.
     Category: Fix
     Description:
       [63804] Hardware monitor of VPCH is fail.

     Infected motherboard: X11SAE-F
     Affected functions:
     Validation :
         1. Check IPMI sensor reading page for VPCH.

05.
     Category: Fix
     Description:
       [63919] LAN MAC Address Shows 00:00:00:00:00:00 in IPMI Web

     Infected motherboard: X11SSE-F
     Affected functions:
     Validation :
         1. Use latest bios FW
         2. heck IPMI web page

06.
     Category: Fix
     Description:
       [64184 ] Functional fail : X11SBA-F/-LN4F R1.01 JL1 no function
       [64158 ] Jumper JL1 function could not be validated

     Infected motherboard: X11SSE-F
     Affected functions:
     Validation :
         1. Short JL1 jumper, then check IPMI web sensor reading page to see
            if chassis intrution is occurred.

--------------------------------------------------------------------------------------
Filename: SMT_X11_046.bin version: 0.46 Date: 07-24-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

01.
     Category: Fix
     Description:
       [63882] IPMI Sensor Reading function is fail.

     Infected motherboard: X11SSL/M-F
     Affected functions:
     Validation :
         1. Check IPMI sensor reading page.

02.
     Category: Fix
     Description:
       [63804] Hardware monitor of VPCH is fail
       [63276] PCH temperature didn't show in IMPI sensor reading 

     Infected motherboard: X11SAE-F
     Affected functions:
     Validation :
         1. Check IPMI sensor reading page.

03.
     Category: Fix
     Description:
       [63744] SDHM test failed

     Infected motherboard: X11SBA-F
     Affected functions:
     Validation :
         1. Check IPMI sensor reading page or use ipmicfg to show sdr.

04.
     Category: Fix
     Description:
       [63881] Cannot use ipmicfg.exe.
       [63896] Cannot use ipmicfg.exe.
       [63883] BMC status is incorrect in BIOS IPMI page.
       [63897] BMC status is incorrect in BIOS IPMI page.

     Infected motherboard: All
     Affected functions:
     Validation :
         1. Power on the system.
         2. Check the KCS interface status with ipmicfg or BIOS IPMI page.

05.
     Category: Enhancement
     Description:
       Need to reset to default.

     Infected motherboard: All
     Affected functions:
     Validation :

06.
     Category: Fix
     Description:
       [63944] No PCH temp reading in IPMI sensor monitor page
       [62658] Fan Pulse-Width-Modulation Measurement fail
       [62657] IPMI Hardware Monitor Check fail
       [62347] Functional fail : X11SSZ seires hardware monitor some item test fail
       [62049] IPMI Sensor readings function can't work

     Infected motherboard: X11SSZ
     Affected functions:
     Validation :
         1. PCH Temp and PS1 can show on sensor page.

07.
     Category: Fix
     Description:
       [63903] System will logout automatically when into "Toggle SUM Licensed
       Checking" page

     Infected motherboard: X11SSZ
     Affected functions:
     Validation :
         1. Enter that "Toggle SUM Licensed Checking" page.

--------------------------------------------------------------------------------------
Filename: SMT_X11_045.bin version: 0.45 Date: 07-XX-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

01.
     Category: Fix
     Description:
       [62804] IPMI hardware monitor fail.

     Infected motherboard: X11SBA-LN4F
     Affected functions:
     Validation :
         1. Check Vcpu/RT1 reading and compare it with measure result.
02.
     Category: Fix
     Description:
       [63181] No "Chassis Intrusion" item in IPMI sensor reading page
       [63030] The project has 6 FAN, but IPMI sensor reading only has 5 FAN item

     Infected motherboard: X11SSH-CTF
     Affected functions:
     Validation :
         1. Check Chassis intrusion and the total numeber of Fan sesnor ar correct      
03.
     Category: Fix
     Description:
       [63028] NM is not working  

     Infected motherboard: X11SSH-CTF
     Affected functions:
     Validation :
         1. Use nm20 nmSDR command by smcipmitool to check if works

04.
     Category: Fix
     Description:

       [63327] The duty cycle of fan while power up is 100%, it should be 50%
       [63275] Hardware monitor of VBAT is fail
       [63274] Hardware monitor of VCPU is fail
       [63012] Fan Pulse-Width-Modulation measurement is fail
       [62948] Hardware monitor is fail
       [62744] The overheat LED didn't blink when FAN fail and power fail

     Infected motherboard: X11SAE-F
     Affected functions:
     Validation :
         1. Check fan mode function
         2. Check thermal trip function
         3. Check fan fail function

05.
     Category: Fix
     Description:
       [63081] IPMI "System Event Log" setting cannot be reloaded

     Infected motherboard: All
     Affected functions:
     Validation :
         1. "System Event Log" enabled.
         2. Save IPMI Configuration.
         3. Load Factory Default.
         4. Reload IPMI Configuration.
         5. Wait more than 60 seconds.
         6. Check the "System Event Log" status.

06.
     Category: New Feature
     Description:
       LSI 3108 management

     Infected motherboard: All motherboards which support LSI 3108 monitoring
     Affected functions:
         1. Activate OOB license (have a independent page: "Miscellaneous>Activate License")
     Validation :
         1. MUST enable OOB license
         2. Click "Storage Monitoring" page and start to manage RAID
            * RAID 0, 1, 5, 6, 10, 50 and 60 supported
            * Add/Delete VD
            * Start/Stop to locate LED
            * Get 3108 controller information
            * Import/Delete foreign configuration
            * Display progress/remaining time or elapsed time when RAID is rebuilding 
         3. Suggest to upgrade LSI firmware to MR6.7_GCA_051215 

07.
     Category: Fix
     Description:

       [63543] CLTM test failed.
       [62270] CLTM test failed

     Infected motherboard: X11SSM-F, X11SSL-F, X11SSL-CF
     Affected functions:
     Validation :
         1. Run the CLTM test.

08.
     Category: Fix
     Description:
       [63158] [NM] Cannot Change P/T-State Limits

     Infected motherboard: X11SSA
     Affected functions:
     Validation :
         1. IPMI firmware update to get CPU temperature from ME.

------------------------------------------------------------------------------
Filename: SMT_X11_044.bin version: 0.44 Date: 06-23-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24


03.
     Category: Enhancement
     Description: Removing special character set restriction
     Infected motherboard: All
     Affected functions:  All
     Validation : Could use special character in add user and modify user.

02.
     Category: Fix
     Description:
       C: [62502] Allow Factory Default to set iKVM language to default as well.

     Infected motherboard: All X11
     Affected functions:
     Validation :
         1. Change iKVM language to one that is not English.
         2. Do restore to Factory Default.
         3. Check iKVM language is back to English.

01.
     Category: Fix
     Description:
       [62473] Vcpu reading voltage is out of to tolerance in IPMI monitor.

     Infected motherboard: X11SSM-F
     Affected functions:
     Validation :
         1. Check the Vcpu reading and compare it with measure result.

------------------------------------------------------------------------------
Filename: SMT_X11_043.bin version: 0.43 Date: 06-05-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24


05.
     Category: Fix
     Description:
       [62473] Vcpu reading voltage is out of to tolerance in IPMI monitor.

     Infected motherboard: X11SSM-F
     Affected functions:
     Validation :
         1. Check the Vcpu reading and compare it with measure result.

04.
     Category: Fix
     Description:
       [62252] Change code to allow ADC sensor to work without ME. 

     Infected motherboard: X11SBA
     Affected functions:
     Validation :
         1. Able to see ADC sensor readings on Web.

03.
     Category: Fix
     Description:
       [61855][61918] Change Vcpu range based on CPU spec for X11SSL-CF and X11SSL-NF.

     Infected motherboard: X11SSL-CF/NF
     Affected functions:
     Validation :
         1. No lower CT/NR triggered for Vcpu.

02.
     Category: Fix
     Description:
       [61856] Add offset to RT1 temp.

     Infected motherboard: X11SSL-CF/NF
     Affected functions:
     Validation :
         1. Compare Web RT1 reading with infrared thermometer reading.

01.
     Category: Fix
     Description:
       Fixed the lock for Fru #1 not correctly locked at first time power on and after factory restore.

     Infected motherboard: All X11
     Affected functions:
     Validation :
         1. Do factory restore.
         2. Write to Fru #1 and check if the write fails.

------------------------------------------------------------------------------
Filename: SMT_X11_042.bin version: 0.42 Date: 05-22-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

09.
     Category: Fix
     Description:
     [61855] Incorrect VCPU voltage.
     [61858] Incorrect sensor naming and voltage value.

     Infected motherboard: X11SSL-CF
     Affected functions:
     Validation :
        1. Check VCPU and Vcpu1_VSA voltage.

08.
     Category: Fix
     Description:
     [61769] Short jumper JL1, the IPMI sensor reading "Chassis Intru" item's status not change.

     Infected motherboard: X11SSL-CF
     Affected functions:
     Validation :
        1. Short jumper JL1, see if chassis intrusion is triggered on IPMI sensor.

07.
     Category: Fix
     Description:
     [61582] Virtual storage cannot be removed when iKVM reset

     Infected motherboard: X11SSH
     Affected functions:
     Validation :
     	1.IKVM reset shold remove all virtual storage.

06.
     Category: Fix
     Description:
     1.	Add NM/ME support.
     2.	Issue #61700, Fix the naming of sensor.
     3.	Calibrate Vcpu and Vdimm reading.


     Infected motherboard: X11SSA-F/X11SSi-LN4F
     Affected functions:
     Validation :
     	1.Add NM/ME support.
     	2.Issue #61700, Fix the naming of sensor.
     	3.Calibrate Vcpu and Vdimm reading.

05.
     Category: Fix
     Description:
     [61585] IPMI cannot record Chassis Intrusion event when JL1 trigger

     Infected motherboard: X11SSH
     Affected functions:
     Validation :
	 1. Trigger chassis intrusion through JL1.

04.
     Category: Fix
     Description:
     [60963] IPMI hardware monitor fail

     Infected motherboard: X11SSH
     Affected functions:
     Validation :
	 1. VCPU should be around 1.29v in dos.

03.
     Category: Fix
     Description:
     [61625] CLTM test failed.

     Infected motherboard: X11SSH
     Affected functions:
     Validation :
	 1. Add throttling callback.

02.
     Category: Fix
     Description:
     [61579] Cannot upgrade BIOS by IPMI

     Infected motherboard: X11SSH
     Affected functions:
     Validation :
	 1. Update BIOS should not alwats show "Upgrade progress"
	 2. Should not show Board ID mismatch event the ID was same.

01.
     Category: Fix
     Description:
     [61581] Cannot enable IPMI "System Event Log" function

     Infected motherboard: X11SSH
     Affected functions:
     Validation :
	 1. System event log will clean and uncheck after factory default.

------------------------------------------------------------------------------
Filename: SMT_X11_041.bin version: 0.41 Date: 05-11-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

11.
     Category: Fix
     Description:
     [60963] IPMI hardware monitor fail

     Infected motherboard: X11SSH
     Affected functions:
     Validation :
	 1. PCH1.05 should be PCH1.00

10.
     Category: Fix
     Description:
     [61581] Cannot enable IPMI "System Event Log" function

     Infected motherboard: X11SSH
     Affected functions:
     Validation :
	 1. The enable checkbox will not disappear after clean system event log

9.
     Category: FW release
     Description: Add X11SSM board support

     Infected motherboard: X11SSM
     Affected functions:
     Validation :
         1. Add sensor list.

8.
     Category: Fix
     Description:
       [61630] Fan Pulse-Width-Modulation fail

     Infected motherboard: All X11
     Affected functions: Heavy IO mode.
     Validation :
         1. Change the fan mode to Heaby IO.
         2. Check the fan behavior meet Thermal Guideline.

7.
     Category: Fix
     Description:
       [61587] System will show "The IPMI Configuration file is damage"
        message when enter IPMI Configuration page.

     Infected motherboard: All X11
     Affected functions: IPMI Configuration save and reload.
     Validation :
         1. Close browser and open a new browser session.
         2. Go to IPMI Configuration web page, save the configuration to local.
         3. Reload using the configuration that was just saved in #1.
         4. After BMC reset completes, go to IPMI Configuration web page again, and there
            should not be any error message.

6.
     Category: Fix
     Description:
     [61579] Cannot upgrade BIOS by IPMI

     Infected motherboard: X11SSH
     Affected functions:
     Validation :
	 1. Page BIOS upload should not show "Upgrade in Progress" every time.

5.
     Category: Fix
     Description:
     [X11SSA-F/X11SSi-LN4] Fix the memory reading

     Infected motherboard: X11SSA, X11SSI
     Affected functions:
     Validation :
	 1. Memory temp could be read.

4.
     Category: Fix
     Description:
     [61562] Sometimes Vcpu status is N/A or Lower Critical in IPMI Sensor reading page

     Infected motherboard: X11SSH
     Affected functions:
     Validation :
	 1. Change vcpu range to 0~1.52

3.
     Category: Fix
     Description:
     [61555] IPMI Timestamp start from 1970/01/01 00:00:00

     Infected motherboard: X11SSH
     Affected functions:
     Validation :
	 1. Add ME support

2.
     Category: Fix
     Description:
     [61553] "Refresh Preview Image" function is not working

     Infected motherboard: X11SSH
     Affected functions:
     Validation :
	 1. Refresh button should update new image.

1.
     Category: Fix
     Description:
     [61495] NM/ME no Support

     Infected motherboard: X11SSH
     Affected functions:
     Validation :
	 1. nm20 nmSDR command should have response.

------------------------------------------------------------------------------
Filename: SMT_X11_040.bin version: 0.40 Date: 04-30-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

4.
     Category: FW release
     Description: Add X11SSL board support

     Infected motherboard: X11SSL
     Affected functions:
     Validation :
         1. Add sensor list.

3.
     Category: Fix
     Description:
     [60632] IPMI sensor readings test fail 

     Infected motherboard: X11SSH
     Affected functions:
     Validation :
	 1. VCPU will show correctly.
	 2. Remove VCPUGT

2.
     Category: Fix
     Description:
     [60963] IPMI hardware monitor fail

     Infected motherboard: X11SSH
     Affected functions:
     Validation :
	 1. VCPU will show correctly.
	 2. 3.3VSB will show correctly.
	 3. Remove VPCH1.5V

1.
     Category: Fix
     Description:
     [61141] Fan Pulse-Width-Modulation can't test

     Infected motherboard: X11SSH
     Affected functions:
     Validation :
	 1. Optimal mode should show on UI.

------------------------------------------------------------------------------
Filename: SMT_X11_030.bin version: 0.30 Date: 04-17-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

5.
     Category: Fix
     Description:
     [60476] Fan fail function didn't work 

     Infected motherboard: X11SSZ
     Affected functions:
     Validation :
	 1. Led should ligh on and fan spped up when fan fail.

4.
     Category: Fix
     Description:
     [60963] IPMI hardware monitor fail

     Infected motherboard: X11SSH
     Affected functions:
     Validation :
	 1. RT2 will show correctly.
	 2. VBAT will show correctly.

3.
     Category: Fix
     Description:
     [61141] Fan Pulse-Width-Modulation can't test

     Infected motherboard: X11SSH
     Affected functions:
     Validation :
	 1. RT2 will show correctly.

2.
     Category: Fix
     Description:
     [60438] Front Panel OH LED solid light when system AC on 

     Infected motherboard: X11SSZ
     Affected functions:
     Validation :
	 1. Led OH should not light solid when AC on.

1.
     Category: Fix
     Description:
     [60632] IPMI sensor readings test fail 

     Infected motherboard: X11SSH
     Affected functions:
     Validation :
	 1. Sensor list does not disappear by randomly ME command 3E.

------------------------------------------------------------------------------
Filename: SMT_X11_020.bin version: 0.20 Date: 03-27-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

1.
     Category: FW release
     Description: Add X11SSA, K1SPI

     Infected motherboard: X11SSA, K1SPI
     Affected functions:
     Validation :
	 1. Add sensor list.

------------------------------------------------------------------------------
Filename: SMT_X11_010.bin version: 0.10 Date: 03-19-2015

U-Boot build time : 2009.01 (03 12 2015)
Java SOL Viewer version : v0.5.9
Java iKVM Viwer version : v1.69 r24

1.
     Category: FW release
     Description:
      First release.

     Infected motherboard: X11SSZ, X11SSH-F
     Affected functions:
     Validation :
         1. Add sensor list.

------------------------------------------------------------------------------
