Firmware Version: 3.45
Firmware Name: SMT_B11IPMI_345_REDFISH.bin
Firmware CRC: B22CEBB0
Release date: 12/14/2017
Supported Platform: B11DPT, B11QPI, B11DPE, B11SP1, B11SPE
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     Y
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     Y
BIOS/IPMI Bug fixes      |     Y

1.   Category: Enhancements
     Description: 
         [ENGINEERING] Enhancements - Java KVM userlist show CMM instead of Unknow if java KVM is launched through CMM Remote Control
     Infected Motherboard: ALL
     Affected functions: Java KVM userlist
     Validation :
        1) Launch KVM through CMM Remote Control.
        2) Launch KVM through Blade BMC and check userlist. Check Java KVM userlist will show CMM for Launching KVM through CMM Remote Control.

2.   Category: fix
     Description: 
         [ENGINEERING]Enhancements - syslog port is read only in Configuration->Port
     Infected Motherboard: ALL
     Affected functions: Configuration->Port
     Validation :
        1) syslog port is read only in Configuration->Port
        2) syslog port and IP address can be configured in Configuration->syslog under OOB license.

3.   Category: fix
     Description: 
         [ENGINEERING] fix - LSI temperature to do fan control
     Infected Motherboard: B11DPE
     Affected functions: fan control
     Validation :
        1) heat AOC-LSI temperature to raise up fan speed. 

4.   Category: fix
     Description: 
         [ENGINEERING] fix - power consumption uncorrect because of using wrong Rload value.
     Infected Motherboard: B11DPE, B11QPI, B11SPE
     Affected functions: power consumption
     Validation :
        1) correct power consumption reading.

5.   Category: workaround
     Description: 
         [ENGINEERING] workaround - B11SPE IPMI LAN is not stable because of MAC1 MDIO/MDC, sometimes IP cannot be conneted.
     Infected Motherboard: B11SPE
     Affected functions: IPMI LAN
     Validation :
        1) check if B11SPE IPMI LAN is working well for a long time.

6.   Category: new
     Description: 
         [ENGINEERING] new - Add "Activate License" in Miscellaneous page
     Infected Motherboard: ALL
     Affected functions: Activate License
     Validation :
        1) check Miscellaneous->Activate License.

7.   Category: new
     Description: 
         [ENGINEERING] new - support new Intel NVME P4500 1TB
     Infected Motherboard: ALL
     Affected functions: NVME
     Validation :
        1) check Server Health-> NVMe SSD
-------------------------------------------------------------------------------------------

Firmware Version: 3.44
Firmware Name: SMT_B11IPMI_344_REDFISH.bin
Firmware CRC: 77F8373B
Release date: 12/8/2017
Supported Platform: B11DPT, B11QPI, B11DPE, B11SP1, B11SPE
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     Y
BIOS/IPMI Bug fixes      |     Y

1.   Category: Enhancements
     Description: 
         [ENGINEERING] Enhancements - remove LSI3108 MCTP
     Infected Motherboard: ALL
     Affected functions: LSI3108
     Validation :
        1) Install LSI3108 with FW rev 4.680.00.8290.
        2) AC cycle testing to check HDD presence and LSI3108 temperature.

2.   Category: fix
     Description: 
         [ENGINEERING]fix - bios cannot bootup after stress bios update via BMC.
     Infected Motherboard: ALL
     Affected functions: bios update
     Validation :
        1) Stress update BIOS
        2) BIOS boot up.

3.   Category: fix
     Description: 
         [ENGINEERING] fix - sometimes sensor readings are disabled and cannot show back after CPU overheat.
     Infected Motherboard: ALL
     Affected functions: sensor readings and sensor event
     Validation :
        1) Stress CPU overheat then cool down CPU
        2) Check sensor and event log.
-------------------------------------------------------------------------------------------

Firmware Version: 3.43
Firmware Name: SMT_B11IPMI_343_REDFISH.bin
Firmware CRC: A07AF091
Release date: 11/29/2017
Supported Platform: B11DPT, B11QPI, B11DPE, B11SP1, B11SPE
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     Y
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description: 
         [85490] fix - ipmicfg fail via SMSTC
     Infected Motherboard: ALL
     Affected functions: ipmicfg
     Validation :
        1) run SMTTC

2.   Category: new
     Description: 
         [ENGINEERING]new - support NVME P4500
                      fix - too much group list generated if click "locate" or "stop locate".
     Infected Motherboard: ALL
     Affected functions: PCIe_SSD webpage
     Validation :
        1) install NVME P4500 check PCIe_SSD webpage information.

3.   Category: improvement
     Description: 
         [ENGINEERING] NTP version update to 4.2.8p10
     Infected Motherboard: ALL
     Affected functions: NTP
     Validation :
        1) NTP verification

4.   Category: fix
     Description: 
         [ENGINEERING]fix - iKVM/HTML5 session id is negative
     Infected Motherboard: ALL
     Affected functions: iKVM
     Validation :
        1) open KVM/HTML5 and check session id in user list.

5.   Category: fix
     Description: 
         [ENGINEERING]fix - top menu upper right is still English after changing to Chinese language
     Infected Motherboard: ALL
     Affected functions: Chinese language
     Validation :
        1) verify top menu language change.
-------------------------------------------------------------------------------------------

Firmware Version: 3.42
Firmware Name: SMT_B11IPMI_342_REDFISH.bin
Firmware CRC: 9188A021
Release date: 11/16/2017
Supported Platform: B11DPT, B11QPI, B11DPE, B11SP1, B11SPE
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     Y
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description: 
         [85753]fix ipmiview cannot launch KVM.
     Infected Motherboard: ALL
     Affected functions: KVM
     Validation :
        1) launch KVM via ipmiview

2.   Category: fix
     Description: 
         [85653]fix - virtual media function failed.
     Infected Motherboard: ALL
     Affected functions: virtual media
     Validation :
        1) mount virtual media according issue description

3.   Category: fix
     Description: 
         [85490]fix - bios upgrade makes system MAC loss and bios crash
     Infected Motherboard: ALL
     Affected functions: bios update
     Validation :
        1) update bios

4.   Category: fix
     Description: 
         [ENGINEERING]fix - AC cycle stress testing makes BMC crash because of uncorrectable smbios file.
     Infected Motherboard: B11DPE
     Affected functions: AC on cycle
     Validation :
        1) stress test AC on cycle with LSI3108

5.   Category: new
     Description: 
         [ENGINEERING]new - support getsetbmcstatus command for TAS
     Infected Motherboard: ALL
     Affected functions: TAS
     Validation :
        1) TAS testing
-------------------------------------------------------------------------------------------

Firmware Version: 3.41
Firmware Name: SMT_B11IPMI_341_REDFISH.bin
Firmware CRC: 86EBED2D
Release date: 11/6/2017
Supported Platform: B11DPT, B11QPI, B11DPE, B11SP1, B11SPE
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     Y
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description: 
         [85307]fix GetRaidCfg - command does not detect the Raid controller on B11DPT
         [84325]fix Avago MegaRAID 3108 mezz RAID info is not shown in IPMI Web 
     Infected Motherboard: B11DPT
     Affected functions: GetRaidCfg
     Validation :
        1) GetRaidCfg.

2.   Category: fix
     Description: 
         [ENGINEERING] add sensor temperature on mezz2 slot device
         [ENGINEERING] CPU3VRM1 Temperature get very high value sometimes. need hardware rework
     Infected Motherboard: B11QPI
     Affected functions: sensor reading
     Validation :
        1) sensor temperature reading

3.   Category: fix
     Description: 
         [83701] [SUM v2.0.0] Run SUM is FAIL
         [84325] SUM Test Case 503 (Stress ME 200 cycles and make sure SUT is life) failed 
     Infected Motherboard: B11
     Affected functions: bios update
     Validation :
        1) bios update

4.   Category: fix
     Description: 
         [ENGINEERING] iKVM user list issue
     Infected Motherboard: ALL
     Affected functions: 
     Validation :
        1) N/A

5.   Category: fix
     Description: 
         [ENGINEERING] Redfish automated test failed 
     Infected Motherboard: ALL
     Affected functions: 
     Validation :
        1) Redfish automated test

6.   Category: improvement
     Description: 
         [ENGINEERING] update aspeed platform.S to V17
     Infected Motherboard: ALL
     Affected functions: 
     Validation :
        1) AC cycle stress testing.

7.   Category: enhancement
     Description: 
         [ENGINEERING] username and password can accept special characters
     Infected Motherboard: ALL
     Affected functions: 
     Validation :
        1) use special characters to set username and password

8.   Category: enhancement
     Description: 
         [ENGINEERING] improve SSL security
     Infected Motherboard: ALL
     Affected functions: 
     Validation :
        1) N/A
----------------------------------------------------------------------------------------

Firmware Version: 3.40
Firmware Name: SMT_B11IPMI_340_REDFISH.bin
Firmware CRC: 7781CBD0
Release date: 10/12/2017
Supported Platform: B11DPT, B11QPI, B11DPE, B11SP1, B11SPE
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: new
     Description: 
         VBAT new spec - below 2.5 for failed, 2.5-2.6V for low, 2.6 above for good
     Infected Motherboard: ALL
     Affected functions: VBAT
     Validation :
        1) Check VBAT spec.

2.   Category: fix
     Description: 
         fix 83829 - SAS card info does not show in IPMI webUI.
     Infected Motherboard: B11DPE
     Affected functions: storage page
     Validation :
        1) install LSI3108 and SAS HDD, check storage page in IPMI WEBUI
--------------------------------------------------------------------------------

Firmware Version: 3.39
Firmware Name: SMT_B11IPMI_339_REDFISH.bin
Firmware CRC: F4CE89A5
Release date: 10/06/2017
Supported Platform: B11DPT, B11QPI, B11DPE, B11SP1, B11SPE
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description: 
         [83364]fix  - B11QPI Hardware Monitor Fail. Vbat Reading failed
         [84293]fix  - VBAT sensor show error in 4U enclosure 
     Infected Motherboard: ALL
     Affected functions: VBAT
     Validation :
        1) Check VBAT spec.

2.   Category: fix
     Description: 
         [ENGINEERING]fix  - GPIOF1 current leakage when system power off.
     Infected Motherboard: B11
     Affected functions: current leakage
     Validation :
        1) hardware help check it.

3.   Category: fix
     Description: 
         [ENGINEERING]fix  - cannot log event log in IPMI 3.38
         [84729] fix - IPMI SEL no "Thermal Trip" event when system thermal trip. 
     Infected Motherboard: B11
     Affected functions: event log
     Validation :
        1) generate event log
-------------------------------------------------------------------------------------------------------------------------

Firmware Version: 3.38
Firmware Name: SMT_B11IPMI_338_REDFISH.bin
Firmware CRC: 0D313B92
Release date: 09/29/2017
Supported Platform: B11DPT, B11QPI, B11DPE, B11SP1, B11SPE
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description: 
         [83946]fix  - IPMI power/temperature record plots are not working.
     Infected Motherboard: ALL
     Affected functions: power/temperature history record chart
     Validation :
        1) Check power/temperature history record chart. all the history chart should have data there instead of zero.

2.   Category: fix
     Description: 
         [84354]fix  - Blade status shows error when system is on 
     Infected Motherboard: ALL
     Affected functions: system health status
     Validation :
        1) power off, health status should be normal.

3.   Category: fix
     Description: 
         [83829]fix  - SAS card info does not show in IPMI webGUI.  
     Infected Motherboard: B11DPE
     Affected functions: LSI3108
     Validation :
        1) Check SAS temperature and HDD Info

4.   Category: fix
     Description: 
         [83364]fix  - B11QPI Hardware Monitor Fail. Vbat Reading failed
         [84293]fix  - VBAT sensor show error in 4U enclosure 
     Infected Motherboard: ALL
     Affected functions: VBAT
     Validation :
        1) Check VBAT spec.

5.   Category: fix
     Description: 
         [ENGINEERING]fix  - SOL stress test failure
     Infected Motherboard: ALL
     Affected functions: SOL
     Validation :
        1) SOL stress test

6.   Category: fix
     Description: 
         [ENGINEERING]fix  - IPMI should show 3 HDD 
     Infected Motherboard: B11DPE
     Affected functions: LSI3108
     Validation :
        1) check WEB storage page.

7.   Category: fix
     Description: 
         [ENGINEERING]fix  - DIMMPQVRM tempeature is missing.
     Infected Motherboard: B11QPI
     Affected functions: NVME
     Validation :
        1) check WEB PCIeSSD page.

8.   Category: support
     Description: 
         [ENGINEERING]support - Support 6U superblade B11SPE
     Infected Motherboard: ALL
     Affected functions: blade status
     Validation :
        1) Monitor and configure B11SPE from CMM.

9.   Category: feature
     Description: 
         [ENGINEERING]new - Put syslog configuration under OOB license.
     Infected Motherboard: ALL
     Affected functions: configuration->syslog
     Validation :
        1) Go to configuration->syslog
	2) Enable oobkey then you can check syslog.
        3) Configure syslog.
        4) Do blade power control, you can receive maintenance system event log.
-------------------------------------------------------------------------------

Firmware Version: 3.37
Firmware Name: SMT_B11IPMI_337_REDFISH.bin
Firmware CRC: 249CC7B5
Release date: 09/08/2017
Supported Platform: B11DPT, B11QPI, B11DPE, B11SP1
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description: 
         [ENGINEERING]  - NTP mode cannot get datetime.
     Infected Motherboard: B11
     Affected functions: datetime
     Validation :
        1) set CMM datatime mode to NTP mode.
	2) AC cycle CMM, and wait for CMM ready
        3) check if CMM datetime is correct.

2.   Category: fix
     Description: 
         [ENGINEERING]  - Maintenance System Event Log datetime is not correct.
     Infected Motherboard: B11
     Affected functions: Maintenance System Event Log
     Validation :
	1) power on/off any blades
        2) event datetime should be the same in System Health Event Log and Maintenance System Event Log.

3.   Category: fix
     Description: 
         [83985]  - Only 2 NVME SSD are shown in web GUI.
         [83986]  - NVMe Slot#3 #4 Info Reading Error.
     Infected Motherboard: B11QPI
     Affected functions: PCIeSSD webpage
     Validation :
        1) installed 4 NVMe.
	2) check PCIeSSD webpage, should have 4 NVMe

4.   Category: fix
     Description: 
         [83364]  - B11QPI Hardware Monitor Fail. VBAT Reading failed .
     Infected Motherboard: B11
     Affected functions: VBAT sensor
     Validation :
	1) reset SDR
        2) check VBAT sensor reading.
--------------------------------------------------------------------------------------------------------


Firmware Version: 3.36
Firmware Name: SMT_B11IPMI_336_REDFISH.bin
Firmware CRC: E178B215
Release date: 08/28/2017
Supported Platform: B11DPT, B11QPI, B11DPE, B11SP1
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description:
         [B11] - in-band sum updatebmc successfully, but it takes too long time to upload fw.

     Infected Motherboard: B11
     Affected functions: sum updatebmc
     Validation :
        1) in-band sum -c updatebmc
-----------------------------------------------------------------------------------------------

Firmware Version: 3.35
Firmware Name: SMT_B11IPMI_335_REDFISH.bin
Firmware CRC: A28BCECD
Release date: 08/25/2017
Supported Platform: B11DPT, B11QPI, B11DPE, B11SP1
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description:
         [B11] - in-band sum updatebmc failed or hang.

     Infected Motherboard: B11
     Affected functions: sum updatebmc
     Validation :
        1) in-band sum -c updatebmc

2.   Category: fix
     Description:
         [B11] - in-band ipmitool hang after bmc reset cold

     Infected Motherboard: B11
     Affected functions: bmc reset
     Validation :
	1) in-band ipmitool bmc reset cold
        2) in-band ipmitool bmc info after bmc come back.

3.   Category: new
     Description:
         [B11] - user password can accept space

     Infected Motherboard: B11
     Affected functions: password
     Validation :
	1) use space as password
---------------------------------------------------------------------------------

Firmware Version: 3.34
Firmware Name: SMT_B11IPMI_334_REDFISH.bin
Firmware CRC: EBA13F59
Release date: 08/23/2017
Supported Platform: B11DPT, B11QPI, B11DPE, B11SP1
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: workaround
     Description:
         [B11DPE] - the front IO hardware wrongly design to reverse UID.

     Infected Motherboard: B11DPE
     Affected functions: UID
     Validation :
        1) UID on/off

2.   Category: new
     Description:
         [B11] - default enable system event log.
         [B11] - add more power control system event log to indicate source, date, user

     Infected Motherboard: B11
     Affected functions: system event log
     Validation :
	1) power control via CMM WEB/BMC WWEB/CMM ipmitool/BMC ipmitool
        2) check system evetn log in Maintenance->System Event Log

3.   Category: fix
     Description:
         [B11DPE] - fan control use new fan curve with CMM 3.16

     Infected Motherboard: B11DPE
     Affected functions: FAN control
     Validation :
        1) thermal testing
---------------------------------------------------------------------------------

Firmware Version: 3.33
Firmware Name: SMT_B11IPMI_333_REDFISH.bin
Firmware CRC: EA4C0A6D
Release date: 08/21/2017
Supported Platform: B11DPT, B11QPI, B11DPE, B11SP1
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description:
         [B11] fix - I2C read only method wrongly send write-bit.

     Infected Motherboard: B11
     Affected functions: I2C write/read
     Validation :
        1) none.
---------------------------------------------------------------------------------

Firmware Version: 3.32
Firmware Name: SMT_B11IPMI_332_REDFISH.bin
Firmware CRC: 06ED8DAE
Release date: 08/18/2017
Supported Platform: B11DPT, B11QPI, B11DPE, B11SP1
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description:
         [B11] fix - ipmiview failed to open kvm because raw 0x30 0x70 0x67 0x00 0x0f response stunnel service is there wrongly. root cause is that blade don't support stunnel service

     Infected Motherboard: B11
     Affected functions: open kvm using ipmiview
     Validation :
        1) open kvm using ipmiview

2.   Category: fix
     Description:
         [B11] fix - cburn on/off testing can show any BMC information sometimes

     Infected Motherboard: B11
     Affected functions: KCS
     Validation :
        1) burn on/off testing, BMC info should be always there.

3.   Category: fix
     Description:
         [B11DPE] new - support B11DPE

     Infected Motherboard: B11DPE
     Affected functions: ALL
     Validation :
        1) testing B11DPE everything
--------------------------------------------------------------------------

Firmware Version: 3.31
Firmware Name: SMT_B11IPMI_331_REDFISH.bin
Firmware CRC: BC4A8ED2
Release date: 08/3/2017
Supported Platform: B11DPT, B11QPI, B11DPE, B11SP1
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description:
         fix - Enable SMC RAKP

     Infected Motherboard: B11DPT
     Affected functions: sensor reading in CMM
     Validation :
        1) check sensor reading in CMM

2.   Category: new
     Description:
       new - launch HTML5 from CMM

     Infected Motherboard: ALL
     Affected functions: HTML5
     Validation :
         1) Login in CMM and go to blade system-> blade status
         2) Click on HTML5.

3.   Category: improvement
     Description:
       improvement - raw 0x30 0x70 0xf2 only clear oob key, do NOT clear DCMS key

     Infected Motherboard: ALL
     Affected functions: clear license key
     Validation :
         1) Login in CMM and go to blade system-> blade status
         2) Click on HTML5.

4.   Category: fix
     Description:
       fix #82918 - IPMIView failed to launch KVM console 

     Infected Motherboard: ALL
     Affected functions: launch KVM
     Validation :
         1) open IPMIView and connect BMC IP
         2) launch KVM
----------------------------------------------------------------------------------------------------------------

Firmware Version: 3.29
Firmware Name: SMT_B11IPMI_329_REDFISH.bin
Firmware CRC: 3D66C9E1
Release date: 07/18/2017
Supported Platform: B11DPT, B11QPI, B11DPE, B11SP1
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description:
         fix - CMM cannot show complete sensor reading on CMM blade node sensor reading page for B11DPT

     Infected Motherboard: B11DPT
     Affected functions: sensor reading in CMM
     Validation :
        1) check sensor reading in CMM

2.   Category: fix
     Description:
       fix - ipv6 cannot work.

     Infected Motherboard: ALL
     Affected functions: ALL
     Validation :
         1) open WEBUI through ipv6

3.   Category: fix
     Description:
       fix - BMC sometimes can't get OOB files from BIOS like fullsmbios

     Infected Motherboard: B11
     Affected functions: System->Hardware Information
     Validation :
         1) Check System->Hardware Information

4.   Category: new
     Description:
       new - B11DPE bring up

     Infected Motherboard: B11DPE
     Affected functions: ALL
     Validation :
         1) fully testing
----------------------------------------------------------------------------------------------------------------

Firmware Version: 3.28
Firmware Name: SMT_B11IPMI_328_REDFISH.bin
Firmware CRC: 7DC1A2E3
Release date: 07/07/2017
Supported Platform: B11DPT, B11QPI, B11SP1
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description:
         fix - sometimes LSI3108 temperature read is gone.

     Infected Motherboard: B11DPT
     Affected functions: LSI3108 sensor reading
     Validation :
        1) cburn on/off
        2) check LSI3108 sensor reading.

2.   Category: Vendor
     Description:
       upgrade platform2500.S to V16

     Infected Motherboard: ALL
     Affected functions: ALL
     Validation :
         1) fully testing.
----------------------------------------------------------------------------------------------------------------

Firmware Version: 3.27
Firmware Name: SMT_B11IPMI_327_REDFISH.bin
Firmware CRC: 40BF21EC
Release date: 07/01/2017
Supported Platform: B11DPT
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description:
         #79660: SMSTC test fail.  

     Infected Motherboard: B11DPT
     Affected functions: SMTSTC test
     Validation :
        1) setup SMSTC test
        3) TC211,T212 should be passed.

2.   Category: fix
     Description:
       #81609: AOM-B3108-H8-B11 temp does not show in IPMI sensor list. 

     Infected Motherboard: B11DPT
     Affected functions: power cycle
     Validation :
         1) Unmount ISO image by command "SMCIPMITool.exe Ipmi_ip ADMIN ADMIN wsiso umount".
         2) Mount ISO image by command "SMCIPMITool.exe Ipmi_ip ADMIN ADMIN wsiso mount iso_image".
         3) Do power cycle by command "SMCIPMITool.exe Ipmi_ip ADMIN ADMIN ipmi power cycle", tool not failure.
3.   Category: new
     Description:
         support B11QPI

     Infected Motherboard: B11QPI
     Affected functions: ALL
     Validation :
        1) all testing

4.   Category: new
     Description:
         support B11SP1

     Infected Motherboard: B11SP1
     Affected functions: ALL
     Validation :
        1) all testing

5.   Category: new
     Description:
         feature - trouble shooting

     Infected Motherboard: ALL
     Affected functions: none
     Validation :
        1) Maintenance->Trouble Shooting.
	2) generate and download.
----------------------------------------------------------------------------------------------------------------

Firmware Version: 3.26
Firmware Name: SMT_B11IPMI_326_REDFISH.bin
Firmware CRC: 043ECB01
Release date: 06/16/2017
Supported Platform: B11DPT
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description:
         
         #79660: SMSTC test fail.  

     Infected Motherboard: B11DPT
     Affected functions: SMTSTC test
     Validation :
        1) setup SMSTC test
        3) TC211,212 should be passed.

2.   Category: fix
     Description:
         BMC can grant that BIOS could use I2C to change M.2 riser card PCIe bandwidth.

     Infected Motherboard: B11DPT
     Affected functions: M.2 riser card configuration
     Validation :
        1) Install M.2 riser card AOM-B-4M
	2) Use latest BIOS with M.2 riser card config
        3) Check PCIe bandwidth.

3.   Category: fix
     Description:
         
       #79950: [SMCIPMITool] Tool return "failed" when executing power cycle command after unmount/mount iso image.  

     Infected Motherboard: B11DPT
     Affected functions: power cycle
     Validation :
         1) Unmount ISO image by command "SMCIPMITool.exe Ipmi_ip ADMIN ADMIN wsiso umount".
         2) Mount ISO image by command "SMCIPMITool.exe Ipmi_ip ADMIN ADMIN wsiso mount iso_image".
         3) Do power cycle by command "SMCIPMITool.exe Ipmi_ip ADMIN ADMIN ipmi power cycle", tool not failure.
----------------------------------------------------------------------------------------------------------------

Firmware Version: 3.25
Firmware Name: SMT_B11IPMI_325_REDFISH.bin
Firmware CRC: 0DC4B4E7
Release date: 06/13/2017
Supported Platform: B11DPT
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description:
         Add support of CPLD spec X11_CPLD_Register_Table_04242017.xlsx

     Infected Motherboard: B11DPT
     Affected functions: ThermalTrip
     Validation :
        1) Update BMC & Latest B11DPT CPLD,
        2) Do CPU ThermalTrip test,
        3) Shall see ThermalTrip event in BMC SEL after system shutdown.

2.   Category: fix
     Description:
         Support AOC-IBH, AOC-OPH, AOC-B-4M sensor

     Infected Motherboard: B11DPT
     Affected functions: AOC Temp
     Validation :
        1) Check BMC sensor,
        2) Shall see "AOC-IBH Temp"/"AOC-OPH Temp"/"AOM-B-4M Temp" sensors.

3.   Category: fix
     Description:
         Fix RedFish Processors info issue

     Infected Motherboard: B11DPT
     Affected functions: RedFish
     Validation :
        1) Open RedFish link with postman, https://.../redfish/v1/Systems/1/Processors
        2) Shall see CPU info.

----------------------------------------------------------------------------------------------------------------

Firmware Version: 3.24
Firmware Name: SMT_B11IPMI_324_REDFISH.bin
Firmware CRC: DA8EE719
Release date: 05/24/2017
Supported Platform: B11DPT
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description: 
         fix - sometimes SOL not working. (IssueID=80234)

     Infected Motherboard: B11DPT
     Affected functions: SOL
     Validation :
	1) AC Cycle all blades,
	2) Power on all blades after BMCs are ready,
	3) All blades SOL should work via Web/IPMITOOL/IPMIView.

2.   Category: Enhancements
     Description: 
         Enhancements - Enable REDFISH function

     Infected Motherboard: B11DPT
     Affected functions: REDFISH
     Validation :
	1) REDFISH function should work.

3.   Category: fix
     Description: 
         fix - Memory sensor names don't match the MB silkscreen.

     Infected Motherboard: B11DPT
     Affected functions: SENSOR
     Validation :
	1) Enter Linux OS and ipmitool sensor,
	2) All DIMM Temp sensor name should match the MB silkscreen.

4.   Category: fix
     Description: 
         fix - Some IPMI commands were fail on SSM web

     Infected Motherboard: B11DPT
     Affected functions: Remote Media
     Validation :
	1) Check deploy OS function of SSM.

5.   Category: fix
     Description: 
         fix - DDNS service not working when VLAN is enabled

     Infected Motherboard: B11DPT
     Affected functions: DDNS
     Validation :
	1) Use WebUI Set DDNS, load TSIG keys.
	2) Set NTP server as DDNS server
	3) Check test Domain not working
	4) IP direct to 192.168.2.1

6.   Category: Enhancements
     Description: 
         Enhancements - Add save button on Event Log webpage

     Infected Motherboard: B11DPT
     Affected functions: SEL, Web
     Validation :
	1) Open BMC web and navigate to Event Log webpage,
	2) Click the 'save' button which will allow to save the event log as a .csv file.

7.   Category: fix
     Description: 
         fix - No user privilege shown on Web when login with AD/LDAP/Radius user.

     Infected Motherboard: B11DPT
     Affected functions: Web
     Validation :
	1) Login BMC web with any AD/LDAP/Radius user,
	2) Check the Host Identification box at the top where should show user privilege after the user name.

----------------------------------------------------------------------------------------------------------------

Firmware Version: 3.22
Firmware Name: SMT_B11IPMI_322_REDFISH.bin
Firmware CRC: 71D4200C
Release date: 04/20/2017
Supported Platform: B11DPT
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description: 
         fix - sometimes CMM cannot power on/off blades, even retry power on/off cannot work, only button can work.

     Infected Motherboard: ALL
     Affected functions: CMM power on/off blades
     Validation :
	1) Set Blades AC Loss policy to power off
	2) AC Cycle all blades
	3) Power on all blades after BMCs are ready
	4) All blades should be power on.

2.   Category: fix
     Description: 
         fix - "Clear SNMP configure does not disable SNMP." (IssueID=79325)

     Infected Motherboard: ALL
     Affected functions: Clear SNMP configuration
     Validation :
	1)  Configuration -> SNMP, enable SNMP V2
	2)  Factory Default -> Clear SNMP configuration doesn't disable SNMP.
	3)  Configuration -> SNMP, the SNMP V2 should be disabled.

3.   Category: fix
     Description: 
         fix - inband(Linux OS) ipmitool cannot work after bmc reset.

     Infected Motherboard: B11DPT
     Affected functions: inband ipmitool
     Validation :
	1)  Enter Linux OS and ipmitool bmc info 
	2)  ipmitool bmc reset cold
	3)  ipmitool bmc info will fail before bmc boot ready.
	4)  ipmitool bmc info will work well after bmc boot ready.
----------------------------------------------------------------------------------------------------------------

Firmware Version: 3.21
Firmware Name: SMT_B11IPMI_321_REDFISH.bin
Firmware CRC: 6F6DC32D
Release date: 04/17/2017
Supported Platform: B11DPT
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description: 
         fix - diag tool don't work.

     Infected Motherboard: ALL
     Affected functions: diag tool
     Validation :
	1) diag tool

2.   Category: Enhancements
     Description: 
         Enhancements - new Platform init V15 on AST2500 from Aspeed company.

     Infected Motherboard: ALL
     Affected functions: Virtual Media, LPC
     Validation :
	1) Check Virtual Media function.
----------------------------------------------------------------------------------

Firmware Version: 3.20
Firmware Name: SMT_B11IPMI_320_REDFISH.bin
Firmware CRC: 34D0E3C9
Release date: 04/4/2017
Supported Platform: B11DPT
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description: 
         fix - use thermal spec 1.3

     Infected Motherboard: B11DPT HW1.01
     Affected functions: thermal
     Validation :
	1) Thermal test.

2.   Category: fix
     Description: 
         fix - blade cannot be powered on if updating bios during power off

     Infected Motherboard: B11DPT HW1.01
     Affected functions: BIOS update
     Validation :
	1) Power Off blade 
	2) Update BIOS
	3) Power On Blade
----------------------------------------------------------------------------------


Firmware Version: 3.19
Firmware Name: SMT_B11IPMI_319_REDFISH.bin
Firmware CRC: B43AFE8F
Release date: 03/29/2017
Supported Platform: B11DPT
Compatible CMM FW Version: 3.02 and above
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description: 
         fix - per thermal team request to change Mezz Card Temperature threshold as 95,100,105

     Infected Motherboard: B11DPT HW1.01
     Affected functions: sensor reading
     Validation :
	1) Check EDR card temperature threshold upper as 95,100,105

2.   Category: fix
     Description: 
         fix - Enable CPLD throttle capability if BBP module is installed.

     Infected Motherboard: B11DPT HW1.01
     Affected functions: BBP
     Validation :
	1) remove BBP to get CPLD setting value 8 by raw 0x06 0x52 0x03 0x70 0x01 0x00 
	2) installed BBP to get CPLD setting value 0 by raw 0x06 0x52 0x03 0x70 0x01 0x00
----------------------------------------------------------------------------------

Firmware Version: 3.18
Firmware Name: SMT_B11IPMI_318_REDFISH.bin
Firmware CRC: 280AFAE8
Release date: 03/28/2017
Supported Platform: B11DPT

SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description: 
         fix - IPMI 3.17 cannot power on/off/reset. no sensor reading

     Infected Motherboard: B11DPT HW1.01
     Affected functions: sensor reading/power on/off/reset
     Validation :
	1) Power on and check sensor reading
	2) Power off/reset/cycle

2.   Category: fix
     Description: 
         fix - IPMI 3.17 fan speed unstable.

     Infected Motherboard: B11DPT HW1.01
     Affected functions: fan control
     Validation :
	1) fan RPM reading stable
-----------------------------------------------------------------------------------

Firmware Version: 3.17
Firmware Name: SMT_B11IPMI_317_REDFISH.bin
Firmware CRC: F97AE017
Release date: 03/27/2017
Supported Platform: B11DPT

SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description: 
         fix - AC Cycle policy don't work well.

     Infected Motherboard: B11DPT HW1.01
     Affected functions: AC cycle 
     Validation :
	1) Set policy always OFF and AC cycle.
	2) Set policy always ON and AC cycle.
	3) Set policy last state and AC cycle.

2.   Category: fix
     Description: 
         fix - B11DPT bios update finished, but CMM always show flashing.

     Infected Motherboard: B11DPT HW1.01
     Affected functions: status showing of BIOS update
     Validation :
	1) Update bios 
	2) Check there is flashing status from CMM Web
	3) The status become normal after bios update finished.

3.   Category: fix
     Description: 
         fix - Node Product Key status show Not activated in CMM WebUI if SUM activate product key.

     Infected Motherboard: B11DPT HW1.01
     Affected functions: Node Product Key status
     Validation :
	1) Use SUM activate product key.
	2) Check Node Product Key status in CMM WebUI
--------------------------------------------------------------------------------

Firmware Version: 3.16
Firmware Name: SMT_B11IPMI_316_REDFISH.bin
Firmware CRC: C689EBCE
Release date: 03/24/2017
Supported Platform: B11DPT

SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: new
     Description: 
         new - apply new Fan Speed Control Algorithm Rev.1.1

     Infected Motherboard: B11DPT HW1.01
     Affected functions: Fan Control
     Validation :
	1) Have to Update CMM FW to SMT_CMMFW_301_REDFISH.zip
	2) Check Fan Speed control

2.   Category: fix
     Description: 
         fix - issue #78555 CMM WebUI does NOT show BIOS in flashing when flashing BIOS

     Infected Motherboard: B11DPT HW1.01
     Affected functions: status showing of BIOS update
     Validation :
	1) Update bios 
	2) Check there is flashing status from CMM Web

3.   Category: fix
     Description: 
         fix - issue #78522 Node Product Key status show Not activated in CMM WebUI if flashing 
			node’s BMC FW with Preserve Configuration unchecked 

     Infected Motherboard: B11DPT HW1.01
     Affected functions: Node Product Key status
     Validation :
	1) Check Node Product Key status in CMM WebUI

4.   Category: fix
     Description: 
         fix - issue #78309 CMM shows Upper Non-recoverable on PW Consumption sensor reading

     Infected Motherboard: B11DPT HW1.01
     Affected functions: Node Product Key status
     Validation :
	1) Check threshold status on PW Consumption sensor in CMM WebUI

5.   Category: fix
     Description: 
         fix - issue #77973 SUM BIOS OOB Check/Update not Available

     Infected Motherboard: B11DPT HW1.01
     Affected functions: OOB key
     Validation :
	1) As the replied messageID: 304020 in project, also need BIOS to fix the portion issue #2 as total solution.
		BMC already fix the portion #1 as we can do.

--------------------------------------------------------------------------------

Firmware Version: 3.15
Firmware Name: SMT_B11IPMI_315_REDFISH.bin
Firmware CRC: 9C893985
Release date: 03/09/2017
Supported Platform: B11DPT
*****importance: update 3.12 to 3.15 is MUST.

SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description: 
         fix - missing system MAC address after BMC update BIOS on B11DPT HW1.01

     Infected Motherboard: B11DPT HW1.01
     Affected functions: BIOS update
     Validation :
	1) Update bios 
	2) Check system MAC address still there.
--------------------------------------------------------------------------------

Firmware Version: 3.12
Firmware Name: SMT_B11IPMI_312_REDFISH.bin
Firmware CRC: 9C893985
Release date: 02/28/2017
Supported Platform: B11DPT
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: new
     Description: 
         new - BMC update BIOS on B11DPT HW1.01

     Infected Motherboard: B11DPT HW1.01
     Affected functions: BIOS update
     Validation :
	1) Enable OOB license
	2) Use BMC to update BIOS

2.   Category: fix
     Description: 
         fix SUM TC218 

     Infected Motherboard: ALL
     Affected functions: OOB function
     Validation :
	1. run test case TC218

3.   Category: fix
     Description: 
         fix SOL cannot launch when BMC web login with AD/LDAP/Radius account

     Infected Motherboard: ALL
     Affected functions: SOL launch
     Validation :
	1) web login with AD/LDAP/Radius account
	2) launch SOL.

4.   Category: new
     Description: 
         new - change the copyright to 2017

     Infected Motherboard: ALL
     Affected functions: WEBUI
     Validation :
	1. check WEBUI copyright 2017

5.   Category: new
     Description: 
         new - add sensor reading Power consumption 

     Infected Motherboard: ALL
     Affected functions: sensor
     Validation :
	1. read sensor reading of power consumption.
--------------------------------------------------------------------------------

Firmware Version: 3.11
Firmware Name: SMT_B11IPMI_311_REDFISH.bin
Firmware CRC: 10FA4F05
Release date: 02/10/2017
Supported Platform: B11DPT
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description: 
         fix 76610: IPMI Web GUI - No HW Information.  
         fix 76725: No Memory/CPU info in summary screen. 

     Infected Motherboard: B11DPT
     Affected functions: OOB function
     Validation :
	1. verify Hardware Info

2.   Category: fix
     Description: 
         customer issue - AD user cannot login if user is in the multiple AD groups.  

     Infected Motherboard: B11DPT
     Affected functions: AD configuration
     Validation :
	1. Create AD user and set this user to multiple AD groups in AD server
	2. In IPMI AD configuration, configure only one AD group, and try to login the user. 
	3. In IPMI AD configuration, configure another one AD group, and try to login the user. 

3.   Category: fix
     Description: 
         fix - redfish cannot send trap.  

     Infected Motherboard: B11DPT
     Affected functions: redfish subscribe
     Validation :
	1. check with REDFISH team to verify it.
---------------------------------------------------------------------------------------------

Firmware Version: 3.10
Firmware Name: SMT_B11IPMI_310_REDFISH.bin
Firmware CRC: CCA3A670
Release date: 02/06/2017
Supported Platform: B11DPT
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: fix
     Description: 
         fix 77063 - CPLD Version Shows 0 under NVME Tab on IPMI WebGUI   

     Infected Motherboard: B11DPT
     Affected functions: CPLD version
     Validation :
	1. check NVME CPLD FW revision	

2.   Category: fix
     Description: 
         fix - CPU2 voltage show error if CPU2 is not installed  

     Infected Motherboard: B11DPT
     Affected functions: sensor reading
     Validation :
	1. CPU2 voltage show not presence if CPU2 is not installed.

3.   Category: fix
     Description: 
         fix #76613 - CMM Power/Temperature Reading Incorrect.

     Infected Motherboard: ALL
     Affected functions: Power/Temperature Reading
     Validation :
	1) require IPMI FW 2.48 or 3.10 above.
	2) check Power/Temperature Reading record on CMM

4.   Category: new
     Description: 
         new - B11DPT to read EDR Mezzanine card temperature.   

     Infected Motherboard: B11DPT
     Affected functions: sensor reading
     Validation :
	1. Check Mezzanine Temperature.	

5.   Category: new
     Description: 
         new  - sync CMM date and time from the first available Blade system RTC.

     Infected Motherboard: ALL
     Affected functions: date and time
     Validation :
	1) require IPMI FW 2.48 or 3.09 above.
	2) select CMM date time option "Blade System".
	3) check the first available ME-Blade system time and CMM date and time. The both time should be the same.
	4) select all node BMC date and time option "CMM".
	5) check all the BMC and CMM time should be the same as the first availabe ME-Blade system time.
---------------------------------------------------------------------------------------

Firmware Version: 3.09
Firmware Name: SMT_B11IPMI_309_REDFISH.bin
Firmware CRC: 18CB2EB9
Release date: 1/19/2017
Supported Platform: B11DPT
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y

1.   Category: new
     Description: 
         use new FW Tag ATENs_FW_SuperBlade11   

     Infected Motherboard: B11DPT
     Affected functions: update 
     Validation :
	use programmer to update IPMI. online update can work after using this fw.	

2.   Category: fix
     Description: 
         fix - IPMI show wrong NVME speed.
         fix - IPMI show wrong CPLD Version
         fix - cannot throttle CPU if power is not enough.
         fix 76713- No VBAT low voltage alert    

     Infected Motherboard: B11DPT
     Affected functions: sensor reading, event log, webui
     Validation :

3.   Category: fix
     Description: 
         issue- IPMI heartbeat solid on.   

     Infected Motherboard: B11DPT
     Affected functions: heartbeat
     Validation :
	IPMI hearbeat flashing

4.   Category: fix
     Description: 
         issue- make VLAN work  

     Infected Motherboard: B11DPT
     Affected functions: VLAN
     Validation :
	update dummy switch fw to 2.0
---------------------------------------------------------------------------------------

Firmware Version: 3.08
Firmware Name: SMT_B11IPMI_308_REDFISH.bin
Firmware CRC: 4A11C2F0
Release date: 1/4/2017
Supported Platform: B11DPT
SW ECO Caused By         |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     N
BIOS/IPMI Enhancements   |     N
BIOS/IPMI Bug fixes      |     Y


1.   Category: fix
     Description: 
         fix 76319 -  [B11DPT] CMM Shows Initializing for B11DPT
         fix 76411 - IPMI WebGUI Crash
         fix 76320 - No Sensor Reading
         fix 76322 - Event Log No Reading 
         fix 76323 - Power/Temperature Record Abnormal       

     Infected Motherboard: B11DPT
     Affected functions: I2C, sensor reading, event log, webui
     Validation :
	SDR reset is MUST
--------------------------------------------------------------------------------
