Filename: SMT_H11AST2500_142.bin version: 1.42 Date: 12-19-2018
U-Boot build time : 2013.01 (Aug 09 2017)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37
Redfish API : Redfish_API_full_list_2018_11_15.xlsx

1.
    Category: Fixes
    Description:
        Fixed the issue where MI25 GPU could not be detected.

    Impact motherboard:
        All MBs

    Affected functions:
    Validation:
        1. Insert GPU cards.
        2. Check sensor reading web gui.

2.
    Category: Fixes
    Description:
        Fixed the issue [95751] [IPMI ECO 1.61]Change Time and Save it on IPMI Web and sometimes I will see "Save uncompleted" message

    Impact motherboard:
        All MBs.

    Affected functions:
    Validation :
        1. Enter page 'Date and Time'
        2. Try to set it with different time and try this multiple times
        3. Confirm that each time the configuration is saved successfully

3.
    Category: New feature
    Description:
        Support the featrue of riser with multi-chip

    Impact motherboard:
        All MBs.

    Affected functions:
    Validation:
        1. Ensure the behavior riser/PCIe_card with one chip should be backward compatible.
        2. Ensure Riser with multi chips should not affect other add on card.

4.
    Category: Enhancement
    Description:
        Update the threshold of the AMD GPU(MI8/MI25).

    Impact motherboard:
        All MBs

    Affected functions:
    Validation:
        1. Check the threshold of the GPU temperature.
        2. Check the fan speed of the cooling zone(it has reference to the GPU temperature).

5.
    Category: Fixes
    Description:
        Fixed the issue [87593] IPMI--SMT_X11AST2500_144--Multiple Web UI formatting issues

    Impact motherboard:
        All MBs.

    Affected functions:
    Validation :
        1. Please refer to PB issue id 87593

6.
    Category: Fixes
    Description:
        Fixed the issue #94031 "when does CPU throttle?"

    Impact motherboard:
        All MBs

    Affected functions:
    Validation:
        1. Heat the CPU until 95 degrees C.
        2. Web GUI CPU temperature sensor is red.
        3. Front panel red LED is on.
        4. Audio alarm is on.
        5. Add CPU throttling message in the event log.

7.
    Category: Fixes
    Description:
        Fixed the issue [94861][ECO]No deassert log after system recover from cpu overheat.

    Impact motherboard:
        All MBs.

    Affected functions:
    Validation:
        1. Heat up CPU or VRM until prochot happens.
        2. Check throttled event log(assert) from web gui.
        3. System recover from cpu overheat.
        4. Check throttled event log(de-assert) from web gui.

8.
    Category: New feature
    Description:
        Support the featrue of riser with multi-chip

    Impact motherboard:
        All MBs.

    Affected functions:
    Validation:
        1. Ensure the behavior riser/PCIe_card with one chip should be backward compatible.
        2. Ensure Riser with multi chips should not affect other add on card.

