X10DAL-i release note. 
-------------------------------------------------------------------------------------------------------------
 CPU Microcode                             | Option ROM/EFI driver                     | Intel RC/TXT/ME
-------------------------------------------------------------------------------------------------------------
 CPUID FAMILY                              | Intel SATA RAID        : 6.1.0.1017       | RC Package : 4.4.0
 306F2 Haswell-EP C-0, C-1, M-1   :00000043| Intel UEFI SATA RAID   : 6.1.0.1017       | SPS        : 3.1.3.72
 306F1 Haswell-EP B-0             :00000014| Intel Giga PXE         : 1.4.04           | BIOS ACM   : 20170206(3.1.1)
 306F0 Haswell-EP A-0             :FFFF0017| Intel iSCSI            : 2.7.128          | SINIT ACM  : 20170414(3.1.1)
 406F0 Broadwell-EP L0,A0,A1      :00000014| Intel Giga UEFI driver : 6.9.07           | 
 406F1 Broadwell-EP B0,M0,R0      :0B000036|
--------------------------------------------------------------------------------------------
 BIOS feature            |  Support
--------------------------------------------------------------------------------
OOB Flash BIOS           |     N
OOB Update Setting       |     N
OOB Change SMBIOS        |     N
InBand Flash BIOS        |     Y
InBand Update Setting    |     Y
InBand Change SMBIOS     |     Y
InBand SMI E7h supported |     Y
Firmware Authentication  |     N
--------------------------------------------------------------------------------
 SW ECO Caused By        |   Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     Y
BIOS/IPMI Enhancements   |     Y
BIOS/IPMI Bug fixes      |     Y
-------------------------------------------------------------------------------------------------------------------------------
BIOS          : X10DAL9.502      Release Date  : 05/02/2019
BIOS Revision : 3.1c             BIOS Engineer : Eason Lin
BIOS Checksum : 9E043CF7h        SVN Revision  : 6030

BIOS Change:

1. [Enhancements] Change BIOS revision to 3.1c.
    Description: Update BIOS revision
    Validation : Check BIOS revision is corrected in BIOS setup and bootable.
    
2. [Enhancements] Force a global reset if SPI descriptor is not write protected after BIOS flash
    Description: If using OOB to update BIOS, the value changed in ME flash won't be reflected in ME register
                 until an AC cycle
    Validation : Update BIOS from v3.0x or previous BIOS to v3.1x BIOS using OOB. Then check memory[0xfed1f850] bit8 is 0 or not

3. [Enhancements] Implement Anti-Roll Back for FDT Read-Only. 
                  Use an hidden item "Anti-Roll Back for FDT Read-Only" to control it, default setting is Disabled.
    Description: Implement Anti-Roll Back for FDT Read-Only.
                  Use an hidden item "Anti-Roll Back for FDT Read-Only" to control it, default setting is Disabled.
    Validation : 1. Use amibcp.exe to set item "Anti-Roll Back for FDT Read-Only"( in Boot Feature page ) to Enabled.
                 2. Update BIOS to FDT not read-only by flash package. For example, flash XXX.bin( ECO 3.0a BIOS ).
                 3. Make sure message "Anti-rollback!! The BIOS file includes improper security setting and is NOT allowed to update. 
                    Please contact TS for more information." is shown on screen.

4. [Fixes] Fix BIOS always retry boot when Re-Try Boot is Disabled.
    Description: Fix BIOS always retry boot when Re-Try Boot is Disabled.
    Validation : 1. Change Boot mode select to UEFI.
                 2. Disable UEFI Built-in EFI Shell.
                 3. Change Onboard LAN Option ROM Type to EFI.
                 4. Do not connect all LAN cables.
                 5. Confirm BIOS try to boot every UEFI PXE boot option one time only.
                 6. Confirm BIOS boot to Setup Menu after all boot options boot failed.

5. [Enhancements] Update EIP393007 & EIP411789 for TPM vulnerability during S3 resume.
    Description: AMISA50049 AMI_Aptio_5.x_TPM2.0_PCR_Reset
    Validation : Please verify TPM 1.2/2.0 related functions.

6. [Fixes] Fix METW may not work if we trigger a huge error events within a very short time.
    Description: The events time are incorrect because RTC is busying in progress . Need to wait for RTC time status flag bit before reading RTC time.
    Validation : 1. Set "Memory Corr. Error Threshold" as 1 by AMIBCP.
                  2. Turn on MCEON
                  3. Trigger Memory CECC error counts more than 500.
                  4. Only see one Memory CECC error event log within 60 min.                  

7. [Enhancements] Update Intel Server Platform Services 3.1.3.72 for Grantley Refresh Platforms
    Description: Update Post Launch Release 072 for Grantley Server for INTEL-SA-00213 Security Advisory to 
                 address CVE-2019-0089, CVE-2019-0090, CVE-2019-0086, CVE-2019-0091, CVE-2019-0092, CVE-2019-0093, 
				 CVE-2019-0094, CVE-2019-0096, CVE-2019-0097, CVE-2019-0098 and CVE-2019-0099 security issue.	
    Validation : a)Enter Setup menu to check the ME revision is 3.1.3.72 and current state is operational.
                 b)Check SPS functions like Node management.

8. [Enhancements] Update SATA/sSATA RAID OPROM/EFI driver to VROC PreOS v6.1.0.1017.
    Description: Update SATA/sSATA RAID OPROM/EFI driver to VROC PreOS v6.1.0.1017
    Validation : For legacy,
                 1. Connected two or more drive on the SATA/sSATA controller.
                 2. Change item "Configure SATA/sSATA as" to RAID, "SATA/sSATA RAID Option ROM/UEFI Driver" to legacy.
                 3. Check SATA/sSATA RAID option ROM version is 6.1.0.1017 during POST.
                 For uEFI,
                 1. Change item "Configure SATA/sSATA as" to RAID, "SATA/sSATA RAID Option ROM/UEFI Driver" to EFI.
                 2. Check Intel VROC SATA/sSATA Controller revision is 6.1.0.1017.

9.[Enhancements] Update VBIOS and Vga EFI Driver to 1.09.
    Description: Update VBIOS and Vga EFI Driver to 1.09 for fixing ASpeed CVE-2019-6260 secure issue.
    Validation : Check C000:0000 VBIOS shadowed address for VBIOS revision shows 1.09.00.
    Note       : Need BMC update BMC Firmware fix this problem together.

10.[Enhancements] Updated Haswell-EP/Broadwell-EP CPU microcode from SRV_P_273 for INTEL-SA-00233 Security Advisory 
                  to address CVE-2018-12126, CVE-2018-12127 and CVE-2018-12130 security issue.
    Description: Updated Haswell-EP C0,1/M0,1/R2 CPU microcode M6F306F2_00000043
                 Updated Broadwell-EP B0/M0/R0 CPU microcode MEF406F1_0B000036.
				 For INTEL-SA-00233 Security Advisory to address CVE-2018-12126, CVE-2018-12127 and CVE-2018-12130 security issue.
    Validation : Check Haswell-EP C0,1/M0,1/R2 CPU microcode version is 0x00000043.
                 Check Broadwell-EP B0/M0/R0 CPU microcode version is 0x0B000036.

11.[Fixes] Unhidden the driver health support pages to support LSI(Broadcom 9440-8i) driver health status.
    Description: Sync with Purley.
    Validation : a. Change Slot OPROM item to EFI depends on PCIE card install on which slot.  
                 b. Check whether the Driver Health pages present under Advanced pages if the uefi driver support driver health function.

--------------------------------------------------------------------------------
BIOS : X10DAL8.606                       Release Date  : 06/06/2018
BIOS revision: 3.1                       BIOS Engineer : Isaac Hsu
BIOS Checksum: 5702AA8Eh                 SVN Revision  : 5669
BIOS Change:            

1. [Enhancements] Change BIOS revision to 3.1
   Description: Update BIOS revision
   Validation : Check BIOS revision is corrected in BIOS Setup.

2. [Enhancements] Update CPU microcode to address 'Spectre' derivatives (CVE-2018-3639 & CVE-2018-3640) security issue.
   Description : Update Broadwell-EP B0/M0/R0 CPU uCode MEF406F1_0B00002E and Haswell-EP C0,1/M0,1/R2 CPU uCode M6F306F2_0000003D.
   Validation:  Check microcode version in Setup Menu.

3. [Fixes] Fix HD audio 7.1ch back panel function test fail.
   Description: Fix HD audio 7.1ch back panel function test fail.
   Validation:  Check HD audio 7.1ch back panel function test.

4. [Fixes] Fix SuperFlash hang during flashing BIOS.
   Description: SuperFlash hang during flashing BIOS.
   Validation:  Check if SuperFlash update BIOS works well.

5. [Fixes] SuperFlash show gargabe string.
   Description : Fix SuperFlash show gargabe string.
   Validation: 1. Enter Start SuperFlash Utility in Advanced with a USB storage installed
               2. Check if right sige has no garbage string.

6. [Enhancements] Add "SMBIOS Preservation" Enabled/Disabled item for flash recovery. (PB #85017 "The SMBIOS is not preserve after flash BIOS by recovery mode (super.rom).")
    Description: Add "SMBIOS Preservation" support for flash recovery.
    Validation : 1. Modify SMBIOS data e.g. type 1 serial no.
                 2. Recovery flash BIOS : Reboot and crash main block and plugged with super.rom USB key.
                 3. After enter setup. Check Recovery page, "SMBIOS Preservation" item is present.
                 4. Select "SMBIOS Preservation"=Enabled and enter to "Proceed with flash update"
                 5. After flash BIOS, boot to dos and check SMBIOS changes are preserved.

7. [Enhancements] Enhanced SMC Recovery Flash Boot Block Feature
    Description: 1. Enhanced SMC Recovery Flash Boot Block Feature for preserving SMBIOS during recovery process.
                 2. Modified prompt string that is suggested by technical writer for SMC Recovery Flash Boot Block Feature.
    Validation: a) Make sure on board BIOS is ECOed BIOS.
                b) Modify SMBIOS data e.g. type 1 serial number.
                c) Crash BIOS by command "RWBiosX64.efi -f" 
                d) Insert a USB device that contains SUPER.ROM (renamed from candidate ECO BIOS).
                e) Check if the system prompts "DXE--System Is Going To Reset And Enter Recovery Mode.." on POST screen.
                f) Check if the system stuck at POST screen and cannot boot into recovery page.
                g) After flashing BIOS, check SMBIOS changes are preserved.

8. [Enhancements] Update SATA RAID OPROM/EFI driver to RSTe PreOS v4.7.0.1014 (RSTe SATA 4.7.0.1069 and NVMe 4.7.0.2063).
   Description: Update SATA RAID OPROM/EFI driver to RSTe PreOS v4.7.0.1014
   Validation: For legacy,
               1. Connected two or more drive on the SATA controller.
               2. Change item "Configure SATA as" to RAID, "SATA RAID Option ROM/UEFI Driver" to legacy.
               3. Check SATA RAID option ROM version is 4.7.0.1014 during POST.
               For uEFI,
               1. Change item "Configure SATA as" to RAID, "SATA RAID Option ROM/UEFI Driver" to EFI.
               2. Boot to Shell.
               3. Run command drivers to check if the SATA RAID uEFi driver, VMD uEFi Driver version is 4.7.0.1014.

9. [Enhancements] Update Intel Server Platform Services 3.1.3.50 for Grantley Refresh Platforms
   Description: Post Launch Release 050 for Grantley Server
                CCG0100859893 Diagnostic interface crash after sending IPMI command SendRawPmBusReq with 
		              input: 0x2E 0x00 0xD9 0x57 0x01 0x00 0x50 0x00 0x7E 0x00 0x00 0x00 0x20 0x00 0x00.
                CCG0100859878 Adjusted diagnostic command filtering according to FAS.
		CCG0100859881
		CCG0100859887
		CCG0100201070 CUPS sensors don¡¦t get initialized and get updated if socket initialization 
		              information is not received during platform boot phase.
   Validation:  a)Enter Setup menu to check the ME revision is 3.1.3.50 and current state is operational.
                b)Check SPS functions like Node management.

10. [Enhancements] Remove out support Ctrl home for recovery 
    Description: Because system will automatically enter in recovery mode if the rom image checksum is invalid. So don't need this.
    Validation: a) Put SUPER.ROM in USB pen drive and plug it into SUT.
                b) Press Ctrl+home hot key and should not enter in recovery mode.

11. [Fixes] Updated FlashDriver module to Label 5 to fix system can't enter recovery mode when updated MAIN block 45% and then power off system.
    Description: Updated FlashDriver module to Label 5 to fix system can't enter recovery mode when updated MAIN block 45% and then power off system.( PB issue ID #85932 )
                 The issue only fixed by new ECO BIOS.
    Validation: 1. Update MB BIOS to new ECO BIOS and use new ECO BIOS as SUPER.ROM.
                2. Power off system when update MAIN block 45% and then power on system.
                3. Make sure system can enter recovery mode.

12. [Enhancements] Supported UEFI mode PXE boot of F12 hot key Net boot. (Refer to Groveport SVN Trunk revision #207 date: 2016/11/08 item #5. "F12 can support UEFI PXE.".)
    Description: Added F12 hot key to boot PXE net boot for UEFI network stack PXE boot.
    Validation : a) Enter to BIOS setup menu.
                 b) Change "Onboard LAN1 OPROM" to "PXE", change "Onboard LAN Option ROM Type" to "EFI" and change "Network Stack" to "Enabled" in under "Advanced -> PCIe/PCI/PnP Configuration" page.
                 c) Change "Boot Mode Select" to "DUAL" or "UEFI" in "Boot" page.
                 d) Change "UEFI AP:UEFI: Built-in EFI Shell" to first priority in fixed boot order in "Boot" page.
                 e) Save and restart the system.
                 f) Boot system to Supermicro logo screen in BDS phase.
                 g) Press hot key <F12> to boot from PXE/LAN.
                 h) Check if the system boots to UEFI PXE LAN.

13. [Enhancements] Update Broadwell-EP RC 4.4.0 release.
    Description: Update Grantley Refresh RC 4.4.0 for below issues.
                 5387096 Workaround issus of unexpected system behavior while reading the same 4Kbyte physical memory
    Validation:  a) Use PCI.exe to check Bus<0x7F,0xFF>/Device<0x10>/Function<0x07>/Reg<0x90>.
                    Please check Bus<0x7Fh> if two CPU attached and Bus<0xFFh> if only one CPU attached.
                    // [31:24] = Major revision number
                    // [23:16] = Minor revision number
                    // [15:8]  = Release Candidate number
	         b) Validate standard feature with Broadwell-EP/Haswell-EP CPU.
	         c) Validate CPU performance like LINPACK and others.

14. [Fixes] Per Intel recommended settings to set Descriptor Region of BIOS Region Write Access to "No".
    Description: Per Intel recommended settings to set Descriptor Region( Bit 0 ) of BIOS Region Write Access to "No"
    Validation:  Make sure bit 0 of memory 0xFED1F851(  0xFED1C000(RCBA) + 0x3800(SPI_BASE_ADDRESS) + 0x51 ) is 0.

--------------------------------------------------------------------------------
BIOS : X10DAL8.213                       Release Date  : 02/13/2018
BIOS revision: 3.0a                      BIOS Engineer : Isaac Hsu
BIOS Checksum: 272D1B33h                 SVN Revision  : 5463
BIOS Change:            

1. [Enhancements] Change BIOS revision to 3.0a
   Description: Update BIOS revision
   Validation : Check BIOS revision is corrected in BIOS Setup.

2. [Enhancements] Update CPU microcode SRV_B_204 for Haswell-EP C0,1/M0,1/R2 & Broadwell-EP B0/M0/R0.
   Description: Address Intel side-channel security fixed (INTEL-TA-201710-003) by updated Haswell-EP C0,1/M0,1/R2 CPU uCode M6F306F2_0000003C and Broadwell-EP B0/M0/R0 CPU uCode MEF406F1_0B00002A.
   Validation:  1) Check Haswell-EP C0,1/M0,1/R2 CPU microcode version is M6F306F2_0000003C.
                2) Check Broadwell-EP B0/M0/R0 CPU microcode version is 0x0B00002A.

3. [Enhancements] Change Memory correctable threshold to 100.
   Description: Change Memory correctable error threshold to 100.
   Validation:  Check "Memory Corr. Error Threshold" is 100 (Advance->EventLogs->Change SMIBOS EventLog Settings) by AMIBCP.

--------------------------------------------------------------------------------
BIOS : X10DAL7.A02                       Release Date  : 10/02/2017
BIOS revision: 2.0c                      BIOS Engineer : Isaac Hsu
BIOS Checksum: 77BB7C2Dh                 SVN Revision  : 5246
BIOS Change:            

1. [Enhancements] Update Grantley Refresh RC 4.3.0.
   Description: Update Grantley Refresh RC 4.3.0 version.
   Validation:  Validate standard feature with Broadwell-EP/Haswell-EP CPU.

2. [Enhancements] Update Broadwell-EP B0/M0/R0 CPU uCode MEF406F1_0B000021.
   Description: Update Broadwell-EP B0/M0/R0 CPU uCode MEF406F1_0B000021.
   Validation:  Check Broadwell-EP B0/M0/R0 CPU  microcode version is 0B000021.

3. [Enhancements] Update Haswell-EP C0,1/M0,1/R2 CPU uCode M6F306F2_0000003A.
   Description: Update Haswell-EP C0,1/M0,1/R2 CPU uCode M6F306F2_0000003A.
   Validation:  Check Haswell-EP C0,1/M0,1/R2 CPU microcode version is 0x3A.

4. [Enhancements] Update Intel Server Platform Services 3.1.3 38.0 PLR7 for Grantley Refresh Platforms
   Description: This is Post Launch Release 7 for Grantley Refresh Platforms for below issues.
                CCG0100857146 System unexpected shutdown with SPS FW exception error.
   Validation:  a)Enter Setup menu to check the ME revision is 3.1.3.38 and current state is operational.
                b)Check SPS functions like Node management.

5. [Fixes] Add a patch for the issue that screen doesn't light automatically after waked up from S3 by pressed Power Button in Windows 10.
   Description: Windows 10 cannot light screen when wake up from S3 by pressed Power Button.
   Validation:  Check if Windows 10 light screen after waked from S3 by pressed Power Button

6. [Fixes] Fix that display has no output when enables secure boot.
   Description: Display has no output when secure boot enabled.
   Validation:  Check if display has output when enable secure boot.

7. [Enhancements] Update SATA RAID OPROM/EFI driver to RSTe PreOS v4.6.0.1018 (RSTe package 4.6.0.1085).
    Description: Update SATA RAID OPROM/EFI driver to RSTe PreOS v4.6.0.1018
    Validation: 1. Change item "Configure SATA as" to RAID, "SATA RAID Option ROM/UEFI Driver" to EFI.
                2. Boot to Shell.
                3. Run command drivers to check if the SATA RAID OPROM/EFI version is 4.6.0.1018.

8. [Enhancements] Add tCCD_L Relaxation item under Memory Configuration menu.
   Description: For Micron certain memory, it need add setup item to increase the tCCD settings for memory stability.
   Validation: Enter setup menu and check there is "tCCD_L Relaxation" setup item is under Memory Configuration page.

9. [Enhancements] Update BIOS ACM 3.1.1 PW, SINIT ACM 3.1.1 PW.
   Description: Update BIOS ACM 3.1.1 PW, SINIT ACM 3.1.1 PW.
   Validation:  a) Run ServerTXTINFO.EFI in UEFI Shell and check the test result. Please provisioning TPM module.
                b) Run tBOOT OS and check OS boot up successfully, please use Skylake tBOOT image.

10. [Enhancements] Added Intel SPI vulnerability patch for Grantley.
    Description: Please refer to AMI BIOS Security Advisories "AMI SPI Flash Write Status Aptio 5.x SA50039 Document Revision 1.01 September 7, 2017", Section CRB UPDATE SOLUTION - SW SEQUENCING. Grantley case is "SPI_USE_HARDWARE_SEQUENCE == 0".
    Validation: Check BIOS flashing can be stressed overnight and the SPI Memory Mapped Configuration Registers (i.e. RCBA+0x3800+0x98=0xFED1F898) have no OPCODE 0xC7 and 0x01.

11. [Features] Implemented SMC Recovery Flash Boot Block Feature.
    Description: To resolve the issue of "Data Structure/PCD Data Base" inconsistent between PEI and DXE phase.
    Validation: Check if BIOS recovery feature works fine.

--------------------------------------------------------------------------------
BIOS : X10DAL6.910                       Release Date  : 09/10/2016
BIOS revision: 2.0b                      BIOS Engineer : Isaac Hsu
BIOS Checksum: FC9B9586h
BIOS Change:            

1. [Fixes] Fix that system report incorrect usable memory size.
   Description: Utility memtest and meminfo show incorrect usable memory size, ex. it only show 2GB memory with 16GB memory installed.
   Validation: See if utility memtest and meminfo show correct usable memory size.

--------------------------------------------------------------------------------
BIOS : X10DAL6.728                       Release Date  : 07/28/2016
BIOS revision: 2.0a                      BIOS Engineer : Isaac Hsu
BIOS Checksum: 6D3CC9D6h
BIOS Change:            

1. [Features] Update Grantley Refresh RC 3.6.0
   Description: Update Grantley Refresh RC 3.6.0  Maintenance Release (MR1) version.
   Validation: Validate standard feature with Broadwell-EP/Haswell-EP CPU.

2. [Features] Update Broadwell-EP B0/M0/R0 CPU uCode MEF406F1_0B00001B.
   Description: Update Broadwell-EP B0/M0/R0 CPU uCode MEF406F1_0B00001B.
   Validation: Check Broadwell-EP B0/M0/R0 CPU  microcode version is 0B00001B.

3. [Features] Update Haswell-EP C0,1/M0,1/R2 CPU uCode M6F306F2_00000038.
   Description: Update Haswell-EP C0,1/M0,1/R2 CPU uCode M6F306F2_00000038.
   Validation: Check Haswell-EP C0,1/M0,1/R2 CPU microcode version is 0x38

4. [Features] Update Intel Server Platform Services 3.1.3 36 PLR3 for Grantley Refresh Platforms
   Description: This is maintenance release for Grantley Refresh Platforms
                Fixed on some parts, NM PTU reported maximum power values for CPU domain are
                lower than power values measured on CPU domain running customer workloads.
   Validation:  a)Enter Setup menu to check the ME revision is 3.1.3.36 and current state is operational.
                b)Check SPS functions.

4. [Features] Updated Intel SATA/sSATA RAID Pre-OS option ROM and UEFI driver to v4.5.0.1012.
   Description: Intel released SATA/sSATA option ROM and UEFI driver v4.5.0.1012.
   Validation:  a)Enabled Intel SATA/sSATA RAID mode and connect two or more SATA HDDs, check the RAID
                  option ROM banner revision number during POST.
                b)Enabled Intel SATA/sSATA and change OpROM policy to "UEFI", check the driver
                  shows up under Advanced page.
                c)Follow UEFI/legacy OS installation SOP to install OS.

5. [Features] Update BIOS ACM 3.1.0 PW, SINIT ACM 3.1.0 PW.
   Description: BIOS & SINIT ACM 3.1.0 fixed following issues.
                1) Broadwell-EP 4P system may hang during IntelR Quick Path Interconnect (IntelR QPI) initialization, or report IERR on first boot
                   after CMOS battery removal.
                2) BIOS ACM reports TPM_MAXNVWRITES error (error code 0xC0480440) after multiple system boots.
                3) BIOS ACM reports ERR_POL_WRONG_VERSION (error code 0xC0062060) if the version field of the PS or PO policy with TPM 2.0 is not 3.0
                4) SINIT ACM fails trusted boot with TPM 2.0 when SHA-1 bank of PCRs is disabled.
   Validation:  a) Run ServerTXTINFO.EFI in UEFI Shell and check the test result. Please provisioning TPM module.
                b) Run tBOOT OS and check OS boot up successfully, please use Skylake tBOOT image.

--------------------------------------------------------------------------------
BIOS : X10DAL5.C18                       Release Date  : 12/18/2015
BIOS revision: 2.0                       BIOS Engineer : Isaac Hsu
BIOS Checksum: 5DDCCC73h
BIOS Change:            

1. [Features] Support Broadwell EP
   Description: Update Grantley Refresh RC 3.0.0
   Validation:  Validate standard feature with Broadwell CPU.

2. [Features] Update Intel Server Platform Services Grantley Refresh Pre-Production Candidate 3.1.3.21
   Description: This is Pre-Production Candidate 5 Release of the Intel Server Platform Services 
                Firmware for the Grantley Refresh Product Line
   Validation:  a)Enter Setup menu to check the ME revision is 3.1.3.21 and current state is operational.
                b)Check SPS functions like Node management.

3. [Features] Update BIOS ACM 3.0.2 PW.
   Description: Fixed Issuing a Clear CMOS operation may result in a system hang or shutdown on subsequent boot.
   Validation:  a) Run ServerTXTINFO.EFI in UEFI Shell and check the test result. Please provisioning TPM module.
                    b) Run tBOOT OS and check OS boot up successfully, please use Skylake tBOOT image.

4. [Features] Enable NVMe driver to support SAMSUNG NVMe device.
   Description: Fix SAMSUNG NVMe device can't boot to EFI OS.
   Validation: Install EFI OS into SAMSUNG NVMe and make sure boot to OS successfully.
   
5. [Fixes] Fixed issue that cannot pass check OA key test tool.
   Description: Fail to find "MSDM" table after flashing OA3.0 key.
   Validation: Check OA key function by ChkOaKeyX64.efi.

--------------------------------------------------------------------------------
BIOS : X10DALI5.814                       Release Date  : 08/14/2015
BIOS revision: 1.0a                       BIOS Engineer : Isaac Hsu
BIOS Checksum: 819822D5h
BIOS Change:

1. [Features] Updated Intel RC 1.17
   Description: Intel released Grantley reference code for Grantley platform.
   Validation : Please test PCIe, memory rank margin, SATA, USB and memory error log functions can work correctly.

2. [Features] Updated ME firmware to 3.0.7.173
   Description: Release for Grantley Platforms.
   Validation : 1) Follow SOP to flash ME and check the status.
                2) Boot to DOS , and check the ME version & status.

3. [Features] Updated Intel TXT ACM modules with BIOS ACM 2.2.
   Description: Intel released new PW version of ACM modules.
   Validation : Run ServerTXTINFO.EFI in UEFI Shell and check the test result. Please provisioning TPM
                module before the test and do not lock the TPM.

4. [Features] Added Intel Haswell-EP supported.
     - Rev 036 for Intel Haswell-EP C-0, C-1, M-1.
   Description: Intel released new microcode for Haswell-EP CPU.
   Validation : Check BIOS Setup menu with Haswell-EP CPU for microcode revision.

5. [Features] Updated Intel SATA/sSATA RAID Pre-OS option ROM and UEFI driver to v4.3.0.1018.
   Description: Intel released SATA/sSATA option ROM and UEFI driver v4.3.0.1018.
   Validation:  a)Enabled Intel SATA/sSATA RAID mode and connect two or more SATA HDDs, check the RAID
                  option ROM banner revision number during POST.
                b)Enabled Intel SATA/sSATA and change OpROM policy to "UEFI", check the driver
                  shows up under Advanced page.
                c)Follow UEFI/legacy OS installation SOP to install OS.

--------------------------------------------------------------------------------
BIOS : X10DALI5.306                       Release Date  : 03/06/2015
BIOS revision: 1.0                        BIOS Engineer : Isaac Hsu
BIOS Checksum: 15B5A27Ch
BIOS Change:

1. First release.
