BH12SSi release note.
-------------------------------------------------------------------------------------------------------------
 CPU Microcode                    | Option ROM/EFI driver                  | AMD AGESA
-------------------------------------------------------------------------------------------------------------
 CPUID FAMILY                     | Aspeed VBIOS             : 1.10.01     | AgesaPI : 1.0.0.7
 8300 SSP-A0           : 08300027 | Intel Giga PXE           : 1.5.84      | PL1PSP : FF.C.0.79
 8310 SSP-B0           : 08301038 | Intel Giga UEFI driver   : 5.3.00      | PL1SMU : 0.36.100.0
                                  | Intel 10G UEFI driver    : 5.8.06      | PL1ABL : 10072013
                                  | Intel 10G PXE            : 2.3.64      | PL2PSP : 0.C.0.79
                                  |                                        | PL2SMU : 0.36.100.0
                                  |                                        | PL2ABL : 10072013
-------------------------------------------------------------------------------------------------------------
 BIOS feature            |  Support
-------------------------------------------------------------------------------------------------------------
OOB Flash BIOS           |     Y
OOB Update Setting       |     Y
OOB Change SMBIOS        |     Y
InBand Flash BIOS        |     Y
InBand Update Setting    |     Y
InBand Change SMBIOS     |     Y
InBand SMI E7h supported |     N
InBand SMI D9h supported |     Y
Hii to BMC supported     |     Y
Firmware Authentication  |     Y
--------------------------------------------------------------------------------------------
 SW ECO Caused By        |  Status
--------------------------------------------------------------------------------
BIOS/IPMI Customization  |     N
HW Vendor Updates        |     N
BIOS/IPMI Workaround     |     N
BIOS/IPMI Vendor Updates |     Y
BIOS/IPMI Enhancements   |     Y
BIOS/IPMI Bug fixes      |     Y
-------------------------------------------------------------------------------------------------------------

BIOS : BH12SSi0.616     (CRC:  7439CBC3)  		Release Date : 06/16/2020     	BIOS revision: 1.0a

1. [Enhancements] Change BIOS revision to 1.0a.
Description : Update BIOS revision.
Validation : Check BIOS revision is correct in BIOS setup and bootable.

2. [Enhancements] Update AGESA RomePI to 1.0.0.7.
Description : Update AGESA RomePI to 1.0.0.7.
Validation : 1. Boot into BIOS setup.
2. Switch Setup page to Advanced->PSP Firmware Versions.
3. Make Sure ABL Version is "10072013".

3. [Enhancements] Update 8310 SSP-B2 microcode 8301038.
Description : Update 8310 SSP-B2 microcode 8301038.
Validation : 1. Use B2 stepping Rome CPU to boot into BIOS setup.
2. Make sure 8310 SSP-B2 Microcode Patch Level is 8301038.

4. [Enhancements] Fixed USB doesn't work on ipmi gui.
Description : Fixed USB doesn't work on ipmi gui.
Validation : 1. go to ipmi gui.
2. check mouses and key boards working properly.

5. [Enhancements] Auto update P1 slot bifurcation and sata mode.
Description : Auto update P1 slot bifurcation and sata mode.
Validation : 1. insert AOM-BPNIO-SCEA, and NVMes, check the NVMes are detectable
2. AOM-BPNIO-SNEA, and SATAs, check the SATAs are detectable

-------------------------------------------------------------------------------------------------------------

BIOS : BH12SSi0.504     (CRC:  D2EAE082)  		Release Date : 05/04/2020     	BIOS revision: 1.0

1. [Enhancements] First release.
   Description: N/A
   Validation : N/A
