***Notes to Release Notes Authors***

* *All fields must be completed; please indicate as “N/A” if not applicable.*
* *Release Notes should document functional changes, dependencies, bug fixes and added features.*
* *Release Notes must not mention the methods of implementation and/or internal processes.*
* *Release Notes must not mention of silicon errata and/or other external causations.*
* *Release Notes must not mention confidential/proprietary information and/or trade secrets of Supermicro or any third party.*
* *Please delete this page and the signature fields before submitting the document in PDF Format to Marketing for publication.*

**IPMI Firmware Release Notes Form**

*Supermicro disclaims all express and implied warranties, including without limitation, the implied warranties of merchantability, fitness for a particular purpose, and non-infringement, as well as any warranty arising from course of performance, course of dealing, or usage in trade. All products, computer systems, dates, and figures specified are preliminary based on current expectations, and are subject to change without notice. Supermicro and the Supermicro logo are trademarks of Super Micro Computer, Inc. in the U.S. and/or other countries. Copyright © 2018 Super Micro Computer, Inc. All rights reserved.*

|  |  |
| --- | --- |
| **Product Name** | **X11SCL-F** |
| **Release Version** | **1.23.06** |
| **Build Date** | **9/30/2020** |
| **Previous Version** | **1.23.04** |
| **Update Category** | **Recommended** |
| **Dependencies** | **None** |
| **Important Notes** | **None** |
| **Enhancements** | **1. Patched files for dropbear-2019.78 and updated the Dropbear SSH to the latest version (2019.78).** |
| **New features** | **N/A** |
| **Fixes** | **1. Corrected error message from 'User name must be 4~16 characters.' To 'User name must be 4~15 characters.'**  **2. Corrected typo in SSL Certification confirm window.**  **3. Fixed problem of user being permanently locked out after exceeding lockout times by SMCIPMITool.**  **4. Fixed problem of BMC issuing multiple alerts when hard drive fails.**  **5. Fixed problem of nonfunctional "Virtual Media" tab displaying on iKVM/HTML5.**  **6. Fixed failure of OOB flash of BIOS from ECO to OEM BIOS, failure of BIOS to pass the secure validation, and inability to apply "LC019\_X11DPFR\_2U\_20200804.v1.rom\_Signed".** |

***Release Notes from Previous Release(s)***

|  |
| --- |
| ***1.23.04 (11/15/2019)***  *1. Corrected verification of the concatenate string of unique password.*  *2. Fixed ability to clear unique password using raw command 0x30 0x74 0x2.*  *3. Fixed ability to remove unique password set bit by IPMITool raw command.*  *4. Corrected response 204 when posting factory default with invalid option value on Redfish and response 503 when posting factory default with empty body on Redfish.*  *5. Fixed failure of Java KVM to block Virtual Media section and show warning message when virtual media port is disabled.*  *6. Fixed missing new load factory default options for IPMICFG/SMCIPMITool/Redfish for IPMI firmware 1.71.7.*  *7. Fixed inconsistent behavior for factory function with firmware 1.71.7.*  *8. Corrected message for Delete User Without Selecting Slot.*  ***1.23.2 (8/30/2019)***  *1. Added support for third number (build version) of IPMI firmware version.*  *2. Added BMC Account Security.*  *3. Added modification for event severity.*  *4. Enabled sending all event logs (Health & Maintenance) to Syslog server.*  *5. Added UefiPxe to Redfish System boot order.*  *6. Fixed problem of IPMI WebGUI system status showing as critical after CPU overheat de-assertion.*  *7. Fixed problem of SEL showing error message after AOC-S3108 updates firmware.*  *8. Fixed multiple vulnerabilities with Supermicro BMC Virtual Media.*  *9. Fixed issue with IPMI web formatting for system.*  *10. Fixed failure of STAC Redfish automation test and inability to access Redfish with RADIUS session after factory default.*  *11. Fixed problem of IPMI RADIUS authentication client returning Localhost IP In NAS-IP-Address/, malfunction of IPMI RADIUS authentication if authentication is delayed for over 3 seconds, and problem of IPMI RADIUS authentication violating attribute 26 specification.*  *12. Fixed incorrect KEYPAD \* and + key maps via IPMI iKVM console and KEYPAD on physical keyboard.*  *13. Fixed incompatibility of IPMI after update.*  ***1.21 (3/21/2019)***  *1. Changed the naming for Health Event Log & Maintenance Event Log in Web UI.*  *2. Enabled clearing all system event logs without generating any log and dumping all the system event logs.*  *3. Added patch for CVE-2019-6260 pantsdown.*  *4. Fixed failure of IPMI SOL.*  *5. Fixed multiple Web UI formatting issues.*  *6. Fixed malfunction of IPMI Web Date & Time Configuration.*  *7. Fixed issue of the system status not referencing PSU state when AC is lost.*  *8. Corrected pop-up message when deleting a group in Active Directory.*  *9. Fixed problems of the sessions timing out after accessing system event log page and of BMC continuously rebooting.*  *10. Corrected grammar on the Alert page.*  *11. Fixed issue of COM1 and COM2 having UART1 output data when SOL is activated.*  *12. Fixed failure to updated BIOS in Web UI.*  *13. Corrected M.2 sensor name and listed it in the Hardware Monitoring document.*  *14. Fixed malfunction of KVM and remote control after using SSH in SMASH with AD account.* |

*\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_*

*Product Manager Date*