Supermicro Update Manager (SUM) UEFI Release Notes
==================================================
Software Release Version: V1.0.0-p1
Release Date: 2020/11/30


Introduction
============
The Supermicro Update Manager (SUM) UEFI can be used to manage the BIOS and BMC
firmware image update for select systems under EFI shell.


Requirements
============
@In-Band Usage
- Managed System
    * Operating system:
        EFI shell
    * Hardware:
        X12/H12 and later platforms except H12 non-RoT systems


Known Limitation
================
1. UpdateBios command does not support --preserve_setting option.
2. GetBiosInfo and GetBmcInfo commands only display information of the managed 
   system.
3. System has to be powered off to complete update BIOS process.
4. System will not be powered on automatically after BIOS is updated on non-RoT
   system.


Version History
===============
V1.0.0-p1 (2020/11/30)
======================
1. Fix         : Fix UpdateBMC hang problem.
2. Enhancement : Add 6 minutes wait in command BmcRotManage.
3. Enhancement : Improve messages of commands BiosRotManage and BmcRotManage.


V1.0.0 (2020/07/24)
======================
1. New Feature : Add GetBiosInfo, UpdateBios, BiosRotManage, GetBmcInfo, 
                 UpdateBmc and BmcRotManage commands to support system BIOS and
                 BMC management.


Technical Support
=================
Web Site:        www.supermicro.com
Headquarters:    support@supermicro.com
European Branch: support@supermicro.nl
Asian Branch:    support@supermicro.com.tw
