==============================================================================================================================
Filename: BMC_X12AST2500-ROT-F101MS_20220803_00.23.66_STDsp.bin version: 00.23.66
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_90_API_full_list_10042021
Supported MBs: X12QCH-NF, X12SPG-NF, X12SPA-TF

1. 
    Category: Fix
    Description:
        [144203] [DVT-final][BMC 00.23.65] M.2 SSD temp reading can't record in sensor page.
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Check M.2 SSD temp
		
2. 
    Category: Fix
    Description:
        [144021] ECO -- 16975 -- 00.23.64(20220624) -- sensor name not match with SPEC (M2_SSD1 Temp should not have underline & P1_PMemA~C Temp should be uppercase)
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Check Sensor reading

3. 
    Category: Fix
    Description:
        [144013] ECO -- 16975 -- 00.23.64(20220624) -- Change WEB setting and restore factory default by SMCIPMITool is not as expected
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Check Sensor reading

4. 
    Category: Fix
    Description:
        [144011] [ECO_BIOS 1.3 0606_IPMI 00.23.65] BMC SEL Log will show "SPI Channel attack is prevented - Assertion" during DC onoff cycles.	
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Check SEL

5. 
    Category: Fix
    Description:
        [144009] 	[ECO_BIOS 1.3 0606_IPMI 00.23.65] BMC SEL Log will show "PSU Status" during DC onoff cycles.
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Check SEL

6. 
    Category: Fix
    Description:
        [143993] 	ECO --16099 -- 00.23.64 -- Host IP address should not input decimal and it will occur error message.
    Impact motherboard:
        X12SPG
    
    Affected functions:
    Validation:
        1. Check Host IP
		
7. 
    Category: Fix
    Description:
        [143945] 		ECO--15662--00.23.64(06/24/2022)--Web GUI no responds when clicking "Save" by default value on syslog page.
    Impact motherboard:
        X12SPA
    
    Affected functions:
    Validation:
        1. Check UI

8. 
    Category: Fix
    Description:
        [143921] 		ECO--15662--00.23.64(06/24/2022)--Saving "RMCP" port to 65535 is success but set to default number 623.
    Impact motherboard:
        X12SPA
    
    Affected functions:
    Validation:
        1. Check UI

9. 
    Category: Fix
    Description:
        [143914] 		ECO --16099 -- 00.23.64 -- "Temperature" and "Controller Status" should be removed in Network AOC information.
    Impact motherboard:
        X12SPA
    
    Affected functions:
    Validation:
        1. Check UI

10. 
    Category: Fix
    Description:
        [143860] 			ECO --16099 -- 00.23.64 --[SMCIPMITool_2.27.0] ipmi lan vlan tag is not as expected
    Impact motherboard:
        X12SPG
    
    Affected functions:
    Validation:
        1. Check UI

11. 
    Category: Fix
    Description:
        [143841] 			ECO --16099 -- 00.23.64 --[SUM_2.9.0] SUM won't get PSU info but WEB UI can show PSU info normally. (TC 238, 325 and 425)
    Impact motherboard:
        X12SPG
    
    Affected functions:
    Validation:
        1. Check UI

12. 
    Category: Fix
    Description:
        [143707] 				[ IPMI ECO 00.23.64 ] Not detect the power module.	
    Impact motherboard:
        X12SPG
    
    Affected functions:
    Validation:
        1. Check UI

13. 
    Category: Fix
    Description:
        [143695] 				[ECO] Can't get PMinfo via SMCIPMITool	
    Impact motherboard:
        X12SPG
    
    Affected functions:
    Validation:
        1. Check UI
	
14. 
    Category: Fix
    Description:
        [143646] 					ECO -- 16975 -- 00.23.64(20220624) -- Dynamic DNS(DDNS) BMC host name "colon :" should be allowed
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Check UI
	
15. 
    Category: Fix
    Description:
        [143339] 					[ IPMI ECO 00.23.64 ] Drop PSU during AC on off stress.	
    Impact motherboard:
        X12SPG
    
    Affected functions:
    Validation:
        1. Check UI

16. 
    Category: Fix
    Description:
        [142209] 			ECO -- 16975 -- 00.23.62(20220519) -- [WEB Function] Restore to factory default is not well function	
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Check UI

17. 
    Category: Fix
    Description:
        [139231] 			ECO -- 16975 -- 00.23.57(20220303) -- Enable NTP server with invalid IP address, MEL miss "Configured to Disable successfully"
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Check UI
	
==============================================================================================================================
Filename: BMC_X12AST2500-ROT-F101MS_20220715_00.23.65_STDsp.bin version: 00.23.65
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_90_API_full_list_10042021
Supported MBs: X12QCH-NF

1. 
    Category: Fix
    Description:
        [142209] ECO -- 16975 -- 00.23.62(20220519) -- [WEB Function] Restore to factory default is not well function    
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Check configuration after factory default

2. 
    Category: Fix
    Description:
        [139231] ECO -- 16975 -- 00.23.57(20220303) -- Enable NTP server with invalid IP address, MEL miss "Configured to Disable successfully"
    
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Please check MEL

3
    Category: Fix
    Description:
        [142410] [ECO_BIOS 1.3_IPMI 00.23.62] BMC will show "Dedicated LAN Link Up and PSU Status" during DC onoff cycles.
    
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Check SEL

4
    Category: Fix
    Description:
        [141456] [DVT SKU-F][BMC 00.23.62] BMC webUI will automatic logout.
    
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Check logout issue

==============================================================================================================================
Filename: BMC_X12AST2500-ROT-F101MS_20220624_00.23.64_STDsp.bin version: 00.23.64
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_90_API_full_list_10042021
Supported MBs: X12QCH-NF X12SPG-TF

1. 
    Category: Fix
    Description:
        [139231] ECO -- 16975 -- 00.23.57(20220303) -- Enable NTP server with invalid IP address, MEL miss "Configured to Disable successfully"
    
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Check MEL when enable NTP service

2. 
    Category: Fix
    Description:
        [140192] STD -- 20151 -- 00.23.54 -- [Web Function] "Maintenance Event Log" not have MEL ID	IPMI
    
    Impact motherboard:
        X12SPG
    
    Affected functions:
    Validation:
        1. Check MEL

3. 
    Category: Fix
    Description:
        [141993] [DVT SKU-F][BIOS 1.3 20220606][BMC 00.23.62] BMC will record "Dedicated LAN Link Up - Assertion" during DC onoff cycles.
    
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Check MEL

4. 
    Category: Fix
    Description:
        [142072] ECO -- 16975 -- 00.23.62(20220519) -- Fail to restore default by SMCIPMITool command (raw 30 41 & fd 3)
    
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Using SMCIPMTool command raw 30 41

5. 
    Category: Fix
    Description:
        [142209] ECO -- 16975 -- 00.23.62(20220519) -- [WEB Function] Restore to factory default is not well function
    
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Using SMCIPMTool command raw 30 41

6. 
    Category: Fix
    Description:
        [142410] [ECO_BIOS 1.3_IPMI 00.23.62] BMC will show "Dedicated LAN Link Up and PSU Status" during DC onoff cycles.
    
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Do DC onoff cycles

7. 
    Category: Fix
    Description:
        [141042] BMC configuration mismatch after change LAN configuration via in-band in test case 373
    
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Run Test case 373

8. 
    Category: Fix
    Description:
        [142444] X12QCH+ 00.23.62 Redfish Automation Tool check	
    
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Run Redfish automatic tool

==============================================================================================================================
Filename: BMC_X12AST2500-ROT-F101MS_20220519_00.23.62_STDsp.bin version: 00.23.62
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_90_API_full_list_10042021
Supported MBs: X12QCH-NF X12SPG-TF

1. 
    Category: Fix
    Description:
        [141042] BMC configuration mismatch after change LAN configuration via in-band in test case 373	
    
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Run IPMIECO test and check report.

2. 
    Category: Fix
    Description:
        [141020] 	[DVT SKU-F][BMC 00.23.60] IPMI will go into slowly and webUI may logout during idle test.
    
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Check WebUI

3. 
    Category: Fix
    Description:
        [140999]	 [GPU-NVQRTX4000] IPMI GPU Sensor Name is not match with the spec.	
    
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Check Sensor list

4. 
    Category: Fix
    Description:
        [140313] 	[DVT] [SYS-440P-TNRT SKU F] BMC is unstable when read component data or read sensor page.
    
    Impact motherboard:
        X12QCH
    
    Affected functions:
    Validation:
        1. Check Sensor list
		
5. 
    Category: Fix
    Description:
        [140197] 	STD -- 20151 -- 00.23.54 -- [Web Function] Can't Launch SOL via JAVA	
    
    Impact motherboard:
        X12SPG
    
    Affected functions:
    Validation:
        1. Check SOL

6. 
    Category: Fix
    Description:
        [140196] 	STD -- 20151 -- 00.23.54 -- [Web Function] Can't launch ikvm via JAVA
    
    Impact motherboard:
        X12SPG
    
    Affected functions:
    Validation:
        1. Check IKVM
		
7. 
    Category: Fix
    Description:
        [140195] 	STD -- 20151 -- 00.23.54 -- [Web Function] Unable to mount "Virtual CD-ROM" while upload the *.img file.(Virtual Media)
    
    Impact motherboard:
        X12SPG
    
    Affected functions:
    Validation:
        1. Check Virtual CD-ROM
		
8. 
    Category: Fix
    Description:
        [140193] 	STD -- 20151 -- 00.23.54 -- [Web Function] Unable to mount "Floppy Disk" while upload the *.ima file.(Virtual Media)
    
    Impact motherboard:
        X12SPG
    
    Affected functions:
    Validation:
        1. Check Virtual CD-ROM

9. 
    Category: Fix
    Description:
        [140191] 	STD -- 20151 -- 00.23.54 -- [Web Function] Dynamic DNS server can be set to invalid IP address
    
    Impact motherboard:
        X12SPG
    
    Affected functions:
    Validation:
        1. Check Dynamic DNS

10. 
    Category: Fix
    Description:
        [140122] 	STD -- 20151 -- 00.23.54 -- [Web Function] set invalid NTP server IP, WEB disable NTP service and still restore invalid IP address
    
    Impact motherboard:
        X12SPG
    
    Affected functions:
    Validation:
        1. Check NTP service

==============================================================================================================================
Filename: BMC_X12AST2500-ROT-F101MS_20220517_00.23.61_STDsp.bin version: 00.23.61
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_90_API_full_list_10042021
Supported MBs: X12QCH-NF X12SPA-TF

1. 
    Category: Fix
    Description:
        [135968] [IPMI ECO 00.23.55] IPMI ECO automation test Failed.
    
    Impact motherboard:
        X12SPA-TF
    
    Affected functions:
    Validation:
        1. Run IPMIECO test and check report.

2.  
    Category: Fix
    Description:
        [140268] [ IPMI ECO 00.23.59 ] Redfish Automation Tool check Failed.
    
    Impact motherboard:
        X12SPA-TF
    
    Affected functions:
    Validation:
        1. Run Redfish Automation test and check report.

3.
    Category: Fix
    Description:
        C: Fix redfish login checking issue when input password shorter than real one but all correct

4. 
    Category: Fix
    Description:
       [139850] (X12STL2.408, sum) Test case 373 - In-Band - Test "Change LAN via BMC configuration" fail
       [139848] SUM test case 373 fail.
       [139847] [SUMECO] Test case 373 - In-Band - Test "Change LAN via BMC configuration" fail, due to BMC LAN cannot be modified.
    
    Impact motherboard:
       X12STL
       H12SSFR-AN6
       H12DST
    
    Affected functions:
    Validation:
      1.Run the latest SUMECO: TC373


==============================================================================================================================
Filename: BMC_X12AST2500-ROT-F101MS_20220414_00.23.59_STDsp.bin version: 00.23.59
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_90_API_full_list_10042021
Supported MBs: X12QCH-NF X12SPA-TF

1.
    Category: Fix
    Description:
        [139708] ECO -- 16099 -- 00.23.57 (2022/03/03) -- Add SNMP type user Not have * to inform Auth Key and Private Key are required items
        [137924] STD -- 16416 -- 01.01.22 (2022/02/15) -- Add SNMP type user Not have * to inform Auth Key and Private Key are required items
    
    Impact motherboard:
        X12SPA-TF
    
    Affected functions:
    Validation:
        1.Go to [Configuration] -> [Account Service]
        2.Create [Operator] and [User] account,
        3.Add an account, [Auth Key] and [Private Key] should be required

2. 
    Category: Fix
    Description:
        [139708] ECO -- 16099 -- 00.23.57(2022/03/03)-- Add SNMP type user Not have * to inform Auth Key and Private Key are required items
        [132850] ECO --20122 -- 00.13.17 (10/15/2021) -- Auth key and Private Key should be "Required" field and with star * mark. (SNMPv3)
        [132852] ECO --20122 -- 00.13.17 (10/15/2021) -- User name should not allow use special characters. (SNMPv3)
        [132895] ECO -- 20122 -- 00.13.17 -- WebUI -- SNMPv3 username should pop out error when type special characters are not allow.
        [132939] ECO --20122 -- 00.13.17 (10/15/2021) -- "Trap Community" should be "Required" field and with star * mark. (SNMPv1/Alerts)
        [133338] ECO --19453 -- 01.02.04 (10/29/2021) -- Fields name mismatch SPEC of Authentication/Encryption key and Protocol. (Alert/SNMPv3)
    
    Impact motherboard:
        X12SPA-TF
    
    Affected functions:
    Validation:
        1.Go to [Configuration] - [Notification] - [Alert] and [SNMP]
        2.Fill in [Auth/Private Key], [Trap Community] in [Alert] page and check the [each fields] specification in WIKI.

3. 
    Category: Fix
    Description:
        [139709] ECO--16099-- 00.23.57(2022/03/03) -- The tips still appear when uncheck SNMP check box when add user account
        [137358] ECO--17274-- 01.01.13(01/27/2022) -- The tips still appear when uncheck SNMP check box when add user account
        [137348] ECO--15340-- 01.01.13(01/27/2022) -- "Auth Key/Private Key" default value incorrect when enable "SNMP" on Modify User window.(ADMIN user)
        [137320] ECO--15340-- 01.01.13(01/27/2022) -- "Account Type" is not match on Add/Modify window and user list.
    
    Impact motherboard:
        X12SPA-TF
    
    Affected functions:
    Validation:
        1.Go to [Configuration] -> [Account Service]
        2.View tips were disappeared when uncheck the SNMP option
        3.View Auth Key/Private Key fields were all empty by default
        4.[Account Type] should be [Redfish/IPMI] instead of [Redfish]

4. 
    Category: Fix
    Description:
        [139710] ECO -- 16099 -- 00.23.57(2022/03/03)  -- Language Change title string not translated
        [138264] ECO -- 16774 -- 01.01.16 (2022/02/15) -- Language Change title string not translated
    
    Impact motherboard:
        X12SPA-TF
    
    Affected functions:
        Dashboard
    
    Validation:
        1. Login BMC GUI Web
        2. Change Language
        3. Check the title of the Language Change dialog

5. 
     Category: Fix
     Description:
         [139451] X12DHM Improvement 31, Able to add the user with password include \ but not able to modify the user with the same length password including \
    
     Impact motherboard:
         X12DHM-6-P
    
     Affected functions:
     Validation:
         1.Go to [Account Service] -> [User]
         2.Set password by [Super\1234512345678],[\Super1234512345678],[Super1234512345678\],[Qwerqwerqw12345678\]

6. 
    Category: Fix
    Description:
        [138110] ECO--15340-- 01.01.16 (02/15/2022) -- It should not present "Delete" icon while login "Operator" or "User" privileges account.
        [138112] ECO--15340-- 01.01.16 (02/15/2022) -- Modify password while login "Operator" or "User" privileges account will return Oops error!
    
    Impact motherboard:
        X12SPA-TF
    
    Affected functions:
    Validation:
        1.Go to [Configuration] -> [Account Service]
        2.Create [Operator] and [User] account,
        3.Modify password
        4.Check the [Delete] button

7. 
    Category: Fix
    Description:
        [139717] ECO -- 16099 -- 00.23.57(2022/03/03)-- Using an account with a <> symbol to log in will not work properly
        [139716] ECO -- 17274 -- 01.01.17(03/04/2022) -- Web will show timeout when login with new creating account ''
        [139499] STD -- 18605 -- X12DGO -- 01.01.04 -- Fail to log in with user accounts which are the combination of through GUI
        [139504] STD -- 18380 -- 1.01.09 - Fail to log in with new created user which contains special characters in username.
        Fixed UI cannot display user name with <>
    
    Impact motherboard:
        X12SPA-TF
    
    Affected functions:
    Validation:
        1. Go to Configuration - Account Services - Users page.
        2. Add a user with <test> username.
        3. Login in with <test> successfully.

==============================================================================================================================

Filename: BMC_X12AST2500-ROT-F101MS_20220303_00.23.57_STDsp.bin version: 00.23.57
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_90_API_full_list_10042021
Supported MBs: X12QCH-NF X12SPA-TF

1.
    Category: Fix
    Description:
        [137324] x12qch+ 00.23.55 automation test
    Impact motherboard:
        X12QCH+
    Affected functions:
    Validation:
        1. Run SATC
		
2.
    Category: Fix
    Description:
        [16494] [IPMI ECO 00.23.55] IPMI ECO automation test Failed.
    Impact motherboard:
        X12SPA
    Affected functions:
    Validation:
        1. Run IPMIECO

3.
    Category: Fix
    Description:
        [135852] [IPMI ECO 00.23.55] Redfish Automation Tool check Failed.
    Impact motherboard:
        X12SPA
    Affected functions:
    Validation:
        1. Run IPMIECO

4.
    Category: Fix
    Description:
        [135153] ECO -- 16975 -- 00.23.55(20211220) -- Function -- Can't launch more ikvm (html5) vai chrome after BMC reset
    Impact motherboard:
        X12QCH+
    Affected functions:
    Validation:
        1. Check iKVM

5.
    Category: Fix
    Description:
        [135151] ECO -- 16975 -- 00.23.55(20211220) -- Function -- Remote Console can't launch ikvm via JAVA plug-in
    Impact motherboard:
        X12QCH+
    Affected functions:
    Validation:
        1. Check iKVM by JAVA plug-in

==============================================================================================================================

Filename: BMC_X12AST2500-ROT-F101MS_20220127_00.23.56_STDsp.bin version: 00.23.56 Date: 1-27-2022
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_90_API_full_list_08282020
Supported MBs: X12QCH-NF X12SPA-TF

1.
    Category: Fix
    Description:
        [136336] [NVMe U.2 LCS - HDS-WUV1-0TS1930] U2_SSD Temp in IPMI Sensor Reading show "N/A" when insert HDS-WUV1-0TS1930
    Impact motherboard:
        X12QCH+
    Affected functions:
    Validation:
        1. Check temperature on sensor list

2.
    Category: Fix
    Description:
        [136081] STD --16099 -- Function-- 00.23.55 -- Can't Launch Console by JAVA
    Impact motherboard:
        X12SPA-TF
    Affected functions:
    Validation:
        1. Check iKVN

3.
    Category: Fix
    Description:
        [136076] [IPMI FW] IPMI FW 00.23.55 credential expired cause can't remote control by JAVA plug-in
    Impact motherboard:
        X12QCH
    Affected functions:
    Validation:
        1. Check iKVN

4.
    Category: Fix
    Description:
        [136022] STD --16099 -- Function -- 00.23.55 -- Can't receive Alert message via SMTP when IPV6 has DNS server.
    Impact motherboard:
        X12SPA
    Affected functions:
    Validation:
        1. Check DNS sever

5.
    Category: Fix
    Description:
        [136019] STD --16099 -- Function -- 00.23.55 -- Can't sync NTP server when BMC has IPv6 DNS.
    Impact motherboard:
        X12SPA
    Affected functions:
    Validation:
        1. Check DNS sever

6.
    Category: Fix
    Description:
        [136018] STD --16099 -- Function -- 00.23.55 -- Floppy Disk can't upload when file extension is .ima
    Impact motherboard:
        X12SPA
    Affected functions:
    Validation:
        1. Check Floppy mount

7.
    Category: Fix
    Description:
        [135968] [IPMI ECO 00.23.55] IPMI ECO automation test Failed.
    Impact motherboard:
        X12SPA
    Affected functions:
    Validation:
        1. Check DNS sever

8.
    Category: Fix
    Description:
        [135852] [IPMI ECO 00.23.55] Redfish Automation Tool check Failed.
    Impact motherboard:
        X12SPA
    Affected functions:
    Validation:
        1. Check DNS sever

==============================================================================================================================

Filename: BMC_X12AST2500-ROT-F101MS_2021220_00.23.55_STDsp.bin version: 00.23.55 Date: 12-23-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported MBs: X12QCH-NF X12SPA-TF

1.
    Category: Fix
    Description:
        [130722] [BIOS ECO 1.0c]SUM test fail
    Impact motherboard:
        X12QCH+
    Affected functions:
    Validation:
        1. Run BIOSECO

2.

    Category: Fix
    Description:
        [127463] [IPMI ECO] Redfish SATC automation test has 1 item failed.
    Impact motherboard:
        X12SPA-TF
    Affected functions:
    Validation:
        1. Run SATC

==============================================================================================================================

Filename: BMC_X12AST2500-ROT-F101MS_2021126_00.23.53_STDsp.bin version: 00.23.53 Date: 12-06-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported MBs: X12QCH-NF

1.
    Category: Fix
    Description:
        [132031] [AOC Compatibility] Disk Info is not match drive's name and Link Speed is 
	         empty in Storage Monitor's Physcial view when insert NVMe M.2 on AOC-SLG3-2H8M2
    Impact motherboard:
        X12QCH+
    Affected functions:
    Validation:
        1. Check UI

2.
    Category: Fix
    Description:
        [130722] [BIOS ECO 1.0c]SUM test fail
    Impact motherboard:
        X12QCH+
    Affected functions:
    Validation:
        1. Run BIOS ECO


==============================================================================================================================

Filename: BMC_X12AST2500-ROT-F101MS_2021126_00.23.52_STDsp.bin version: 00.23.52 Date: 10-26-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported MBs: X12SPG-NF

1.
    Category: Fix
    Description:
        [133676] ECO -- 16099 -- 00.23.51 -- Web -- Can't sync NTP server (Primary and Secondary)
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check UI

2.
    Category: Fix
    Description:
        [133546] ECO -- 16099 -- 00.23.51 -- SMCIPMItool -- NTP Server can be set localhost via smcipmitool
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check Help page

3.
    Category: Fix
    Description:
        [130975] 	ECO --16099 --00.23.48 (09/11/2021) -- Click on "Send Test Alert" web GUI will no responds and couldn't get message from email.
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check Multi Node


==============================================================================================================================

Filename: BMC_X12AST2500-ROT-F101MS_2021110_00.23.51_STDsp.bin version: 00.23.51 Date: 10-11-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported MBs: X12SPG-NF

1.
    Category: Fix
    Description:
        [132413] ECO --16099 --00.23.50 (10/13/2021) -- Enable auto stop after recording 2 minutes, couldn't stop the record when reach the time limit. (iKVM/HTML5)
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check UI

2.
    Category: Fix
    Description:
        [130977] ECO --16099 --00.23.48 (09/11/2021) -- No details information for "Multi Node" function on help content.
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check Help page

3.
    Category: Fix
    Description:
        [130976] ECO --16099 --00.23.48 (09/11/2021) -- Multi Node no related action on current node.
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check Multi Node
		
4.
    Category: Fix
    Description:
        [133237] [IPMI ECO 00.23.50] Redfish Automation Tool check Failed.
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Run Redfish Automation



==============================================================================================================================

Filename: BMC_X12AST2500-ROT-F101MS_20211013_00.23.50_STDsp.bin version: 00.23.50 Date: 13-10-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported MBs: X12SPG-NF

1.
    Category: Fix
    Description:
        [130153] [IPMI 00.23.45 ECO] IPMI automation test failed.
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. IPMIECO


==============================================================================================================================

Filename: BMC_X12AST2500-ROT-F101MS_20211006_00.23.49_STDsp.bin version: 00.23.49 Date: 06-10-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported MBs: X12SPG-NF

1.
    Category: Fix
    Description:
        [131350] [BETA]System Chassis Node A and Node B description mismatch with IPMI WEB GUI Multi-Node definition Copy Project Issue Link
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check UI and use the Mid-plane v1.0.3

2.
    Category: Fix
    Description:
        [130989] ECO --16099 --00.23.48 (09/11/2021) -- Recording file couldn't playback when recording on iKVM/HTML5.
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check UI

3.

    Category: Fix
    Description:
        [130979] ECO --16099 --00.23.48 (09/11/2021) -- Don't change any setting, then click on "Save" will return Oops! error(Date and Time).
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check UI

4.

    Category: Fix
    Description:
        [130976] ECO --16099 --00.23.48 (09/11/2021) -- Multi Node no related action on current node.	
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check UI

5.

    Category: Fix
    Description:
        [130153] [IPMI 00.23.45 ECO] IPMI automation test failed.
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. IPMIECO

==============================================================================================================================

Filename: BMC_X12AST2500-ROT-F101MS_20210911_00.23.48_STDsp.bin version: 00.23.48 Date: 11-09-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported MBs: X12SPG-NF

1.
    Category: Fix
    Description:
        [130153] [IPMI 00.23.45 ECO] IPMI automation test failed.
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Run IPMIECO

2.
    Category: Fix
    Description:
        [130062] [BIOS ECO 1.00] SUM test fail
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Run BIOSECO


3.
    Category: Fix
    Description:
        [130588] SYS-210GP-DNR (MBD-X12SPG-NF-P Rev.1.01) IPMI sensor reading definition is reverse from MB RT1/RT2 location.
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check sensor reading

==============================================================================================================================

Filename: BMC_X12AST2500-ROT-F101MS_20210906_00.23.47_STDsp.bin version: 00.23.47 Date: 06-09-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported MBs: X12DPI, X12QCH, X12SPA-TF, X12SPG-NF

1.
    Category: Fix
    Description:
        [130153] [IPMI 00.23.45 ECO] IPMI automation test failed.
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Run IPMIECO

2.
    Category: Fix
    Description:
        [130167] [DVT]Received "" IPMI message handler: BMC returned incorrect response, expected netfn 31 cmd 70, got netfn 31 cmd C4 "" when Cburn idle
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Run CBURN

3.
    Category: Fix
    Description:
        [130062] [BIOS ECO 1.00] SUM test fail
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Run BIOSECO

4.
    Category: Fix
    Description:
        [130062] [DVT]cburn AC on/off failed PSU info drop
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Run CBURN


==============================================================================================================================

Filename: BMC_X12AST2500-ROT-F101MS_20210818_00.23.46_STDsp.bin version: 00.23.45 Date: 30-08-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported MBs: X12DPI, X12QCH, X12SPA-TF, X12SPG-NF

1.
    Category: Fix
    Description:
        [130153] [IPMI 00.23.45 ECO] IPMI automation test failed.
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Run IPMIECO
	
2.
    Category: Fix
    Description:
        [130019] [IPMI 00.23.45 ECO] SATC automation test failed.
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Run SATC

3.
    Category: Fix
    Description:
        [129917] [DVT]cburn AC on/off failed PSU info drop
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Run CBurn

4.
    Category: Fix
    Description:
        [129872] There is a mis-leaded ghost “LAN” MAC address=00.00.00.00.00.00 from BMC Web GUI. (Remove AIOM card)
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check WebUI 


==============================================================================================================================

Filename: BMC_X12AST2500-ROT-F101MS_20210818_00.23.45_STDsp.bin version: 00.23.45 Date: 18-08-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported MBs: X12DPI, X12QCH, X12SPA-TF, X12SPG-NF

1.
    Category: Fix
    Description:
        [129776] [DVT]ON/OFF failed System reboots repeatedly during POST
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. DC ON/OFF



==============================================================================================================================

Filename: BMC_X12AST2500-ROT-F101MS_20210806_00.23.43_STDsp.bin version: 00.23.43 Date: 06-08-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported MBs: X12DPI, X12QCH, X12SPA-TF, X12SPG-NF

1.
    Category: Fix
    Description:
        [127907] Unable to read the power consumption of entire platform subsystem.	
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. webGUI update

2.
    Category: Fix
    Description:
        [129161] Missing Inlet Temp (RT0) sensor on SDR
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. webGUI update

3.
    Category: Fix
    Description:
        [129274] [DVT] WEB UI Power the Power Consumption show 0Watts
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. webGUI update
		
4.
    Category: Fix
    Description:
        [129460] System multi nodes AC onoff stress test fail
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. webGUI update

==============================================================================================================================

Filename: BMC_X12AST2500-ROT-F101MS_20210803_00.23.42_STDsp.bin version: 00.23.42 Date: 03-08-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported MBs: X12DPI, X12QCH, X12SPA-TF

1.
    Category: Fix
    Description:
        Cannot update BMC FW
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. webGUI update

==============================================================================================================================

Filename: BMC_X12AST2500-ROT-F101MS_20210730_00.23.41_STDsp.bin version: 00.23.41 Date: 30-07-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported MBs: X12DPI, X12QCH, X12SPA-TF

1.
    Category: Fix
    Description:
        [129080][DVT]System Chassis Node A and Node B description mismatch with IPMI WEB GUI Multi-Node definition
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. webGUI sensor page

2.
    Category: Fix
    Description:
        [129079][DVT]WEB UI Multi-Node Information empty
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. webGUI sensor page

3.
    Category: Fix
    Description:
        [129001]Fan RPM reading does not match fan module spec	
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. webGUI sensor page

4.
    Category: Fix
    Description:
        [128841][DVT]FAN failed does not trigger Front Panel fail LED and log
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. webGUI sensor page

5.
    Category: Fix
    Description:
        [128822][DVT]FAN mode function failed system always keep speed 20000 R.P.M
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. webGUI sensor page


==============================================================================================================================

Filename: BMC_X12AST2500-ROT-F101MS_20210720_00.23.40_STDsp.bin version: 00.23.40 Date: 20-07-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported MBs: X12DPI, X12QCH, X12SPA-TF

1.
    Category: Fix
    Description:
        [128841][DVT]FAN failed does not trigger Front Panel fail LED and log Copy Project Issue Link
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. webGUI sensor page

2.
    Category: Fix
    Description:
        [128827][DVT]No AOC-ATG-i2SM sensor reading on IPMI GUI	 Project Issue Link
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check sensor reading

3.
    Category: Fix
    Description:
        [128713][DVT]No AOC-A25G-m2SM sensor reading on IPMI GUI.
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check sensor reading

4.
    Category: Fix
    Description:
        [128650] Unable to detect the correct AIOM card information, when the AOC-AG-i2M card is installed on X12SPG-NF.
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check sensor reading

5. 
    Category: Fix
    Description:
        [128714] Cannot detect correct AOC-A25G-m2SM LAN1/2 MAC address.
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check sensor reading

6. 
    Category: Fix
    Description:
        [128516] No AIOM sensor reading on IPMI GUI.
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check sensor reading

7.
    Category: Fix
    Description:
        [128822] [DVT]FAN mode function failed system always keep speed 20000 R.P.M
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check sensor reading

8.
    Category: Fix
    Description:
        [127989] The naming of sensor readings does not follow Supermicro_X12 Temp Sensor Naming guideline.
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check sensor reading

9.
    Category: Fix
    Description:
        [127907] Unable to read the power consumption of entire platform subsystem.
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check sensor reading

10.
    Category: Fix
    Description:
        [127865] [EVT] Some IPMI sensor reading status failed.
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check sensor reading

11.
    Category: Fix
    Description:
        [127364] DFX: CM USI X12SPG-NF 1st sample run DFX report
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check sensor reading

12.
    Category: Fix
    Description:
        [125992] There is no smartpower option on WebGUI
    Impact motherboard:
        X12SPG
    Affected functions:
    Validation:
        1. Check sensor reading

Protection maps:
    X12SPG-NF 20210720.bin

==============================================================================================================================
Filename: BMC_X12AST2500-ROT-F101MS_20210714_00.23.39_STDsp.bin version: 00.23.39 Date: 14-07-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported MBs: X12DPI, X12QCH, X12SPA-TF

1.
    Category: Fix
    Description:
        Missing GPU card temperature reading
    Impact motherboard:
        All X12AST2500 MBs supporting GPU cards
    Affected functions:
    Validation:
        1. webGUI sensor page

Protection maps:
    X12DPI 20200606-151051.bin

==============================================================================================================================
Filename: BMC_X12AST2500-ROT-F101MS_20210707_00.23.38_STDsp.bin version: 00.23.38 Date: 07-07-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_08282020
Supported MBs: X12DPI, X12QCH, X12SPA-TF

Maintenance release.

Protection maps:
    X12DPI 20200606-151051.bin
==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002327.bin version: 0.23.27 Date: 03-09-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
Category: Fix
Description:
	[121244] [BIOS ECO 1.00]IPMI WEB Sensor Readings often fail to read MEM temperature Copy Project Issue Link

Impact motherboard:
	X12SPA

2.
Category: Fix
Description:
	[124020] CM USI Feedback ECO 24918 Update BIOS/IPMI FW, find run ipmicfg can’t detect U2_SSD1 temp issue

Impact motherboard:
	X12QCH


==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002325.bin version: 0.23.25 Date: 01-18-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
Category: Fix
Description:
	[121280] [IPMI 00.23.21 ECO] Power fail events are not match with SPEC.
	[120773] [Beta Test]Execute Power supply/Power cord hot-plug test check event log not meet spec
	[120383] Power fail events are not match with SPEC
	[119632] [MB 2.00] PSU plug in plug out event is not matched with SPEC, there is no event when insert/remove PSU module
	[119193] [DVT]Execute Power supply/Power cord hot-plug test check event log not meet spec

Impact motherboard:
	X12

2.
Category: Fix
Description:
	[121244][BIOS ECO 1.00]IPMI WEB Sensor Readings often fail to read MEM temperature

Impact motherboard:
	X12SPA



==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002324.bin version: 0.23.24 Date: 01-06-2021
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
Category: Fix
Description:
[121530]The DCPMM naming should be “PMEM” in IPMI sensor reading, not "DCPM"
Impact motherboard:
X12SPA
Affected functions:
Validation :
Plugin PMEM, login WebUI and check PMEM naming

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002323.bin version: 0.23.23 Date: 12-28-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
Category: Fix
Description:
[120713][IPMI 00.23.18 ECO] Redfish SATC automation test have 4 items failed.
Impact motherboard:
All X12 with AST2500 chips MB
Affected functions:
Validation :
Check Dump Service on Redfish

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002322.bin version: 0.23.22 Date: 12-15-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
Category: Fix
Description:
[121012] [Final run validation_for beta] When CPU3/4 overheat no appear any event log.
Impact motherboard:
*X12QCH+
Affected functions:
Validation :
Please check event log when processor hot

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002321.bin version: 0.23.21 Date: 12-15-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
Category: Fix
Description:
[120845] [IPMI 00.23.20 ECO] Can't flash BMC via IPMIView flash tool.
Impact motherboard:
*X12SPA-TF
Affected functions:
Validation :
Please use the IPMIView_2.18.0_build.201007

2.
Category: Fix
Description:
[11979] [RoT] CPLD JTag Port Lock function Failed
Impact motherboard:
*X12SPA-TF
Affected functions:
Validation :
Please check CPLD Jtag port

3.
Category: Fix
Description:
[121012] [Final run validation_for beta] When CPU3/4 overheat no appear any event log.
Impact motherboard:
*X12QCH
Affected functions:
Validation :
Please check Event log

4.
Category: Fix
Description:
[119746] The inband function will fail if customer change the IP or disable Host Interface device under OS
Impact motherboard:
*X12QCH
Affected functions:
Validation :
Try disable host interface


==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002320.bin version: 0.23.20 Date: 11-30-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
Category: Fix
Description:
[119363] 	[DVT] When power failure alert deassertion the front panel information led still blinking
Impact motherboard:
*X12QCH+
Affected functions:
Validation :
Check the information LED

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002319.bin version: 0.23.19 Date: 11-11-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
Category: Fix
Description:
[119689] [IPMIECO 00.23.18] Open iKVM via Remote Console monitor is not working in Dashboard page when pressing monitor in second time
Impact motherboard:
*X12QCH+
Affected functions:
Validation :
Check Remote Console monitor

2.
Category: Fix
Description:
[119604] [DVT] IPMI GUI event log can't switch to after two page.
Impact motherboard:
*X12QCH+
Affected functions:
Validation :
Check event log when they have over three pages


==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002318.bin version: 0.23.18 Date: 11-06-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
Category: Fix
Description:
[116049] [IPMI ECO] SUM automation test failed
Impact motherboard:
*X12QCH+
Affected functions:
Validation :
Run SUM automation test

2.
Category: Fix
Description:
[115402] SATC redfish automation standard mode test fail
Impact motherboard:
*X12QCH+
Affected functions:
Validation :
Run SATC redfish automation test

3.
Category: Fix
Description:
[119363][DVT] When power failure alert deassertion the front panel information led still blinking
Impact motherboard:
*X12QCH+
Affected functions:
Validation :
Check Information LED


==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002317.bin version: 0.23.17 Date: 10-27-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
Category: Fix
Description:
[116049] [IPMI ECO] SUM automation test failed
Impact motherboard:
*X12QCH+
Affected functions:
Validation :
Run SUM automation test

2.
Category: Fix
Description:
[115402] SATC redfish automation standard mode test fail
Impact motherboard:
*X12QCH+
Affected functions:
Validation :
Run SATC redfish automation test

3.
Category: Fix
Description:
[117382] IPMI can't sensor reading information when riser card RSC D2-668G4 insert Tesla T4 graphics card.
Impact motherboard:
*X12QCH+
Affected functions:
Validation :
Check "Sensor Listing" on web

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002316.bin version: 0.23.16 Date: 10-08-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
Category: Fix
Description:
[117320] [AOC/AIOM]AOC/AIOM card sensor reading will display wrong temp.
Impact motherboard:
*ALL
Affected functions:
Validation :
Check "Sensor Reading" on Web

Category: Fix
Description:
[117277] [DVT] Insert AOC-S100G-b2C no information in the IPMI GUI
Impact motherboard:
*ALL
Affected functions:
Validation :
Check "Sensor Reading" on Web

Category: Fix
Description:
[117276] [DVT] Insert AOC-S100G-b2C no information in the IPMI GUI
Impact motherboard:
*ALL
Affected functions:
Validation :
Check "Sensor Reading" on Web

Category: Fix
Description:
[117178] [DVT] DC on off test fail, the system will appear 5VSB "Upper Critical - going high - Assertion"
Impact motherboard:
*ALL
Affected functions:
Validation :
Check "Health Event Log" on Web

Category: Fix
Description:
[116965] [DVT] AC on/off test fail.
Impact motherboard:
*ALL
Affected functions:
Validation :

Category: Fix
Description:
[116930] [DVT] M2_SSD2 Temp will disappear when running HDD stress
Impact motherboard:
*ALL
Affected functions:
Validation :
==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002315.bin version: 0.23.15 Date: 09-18-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
Category: Fix
Description:
[116389] There is a label in front of Launch SOL function
Impact motherboard:
*ALL
Affected functions:
Validation :
Check "Launch SOL" on Web

2.
Category: Fix
Description:
[115461] RSC-D2R-668G4 multi sensor reading function test fail
Impact motherboard:
*ALL
Affected functions:
Validation :
Check Storage page on Web

3.
Category: Fix
Description:
[115398] The location of SERR/PERR event log is not matched
Impact motherboard:
*ALL
Affected functions:
Validation :
Check Log on Web


==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002314.bin version: 0.23.14 Date: 09-07-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : X12_Redfish_1_80_API_full_list_08282020

1.
Category: New
Description:
Support keyChange
Enable key check OEM cmd 0x30 0x68 0x28 0x0a
Impact motherboard:
*ALL
Affected functions:
Validation :
keyChange operation
 
==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002313.bin version: 0.23.13 Date: 09-04-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : TBD

1.
Category: Fix
Description:
[116112] [IPMI ECO] Sensor reading naming issue.	.
Impact motherboard:
*ALL
Affected functions:
Validation :
Check DCPM->PMem on Sensor Readings


2.
Category: Fix
Description:
[115866] SYS-240P-TNRT (MBD-X12QCH+ Rev.1.01) Fan Speed Control (FSC) profile deviation.
Impact motherboard:
*ALL
Affected functions:
Validation :
Check FAN control

3.
Category: Fix
Description:
[115829] [IPMIECO] No CPU3 and CPU4 throttle event log deviation.
Impact motherboard:
*ALL
Affected functions:
Validation :
Check Health event log




==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002312.bin version: 0.23.12 Date: 08-28-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : TBD

1.
Category: Fix
Description:
[115866] SYS-240P-TNRT (MBD-X12QCH+ Rev.1.01) Fan Speed Control (FSC) profile deviation.

Impact motherboard:
*ALL
Affected functions:
Validation :
Check FAN speed on FAN page

2.
Category: Fix
Description:
[115856] [IPMI ECO] Web GUI response too slow to check the system information

Impact motherboard:
*ALL
Affected functions:
Validation :
Login the web

3.
Category: Fix
Description:
[115818] [IPMI ECO] Launch SOL function will download Java SOL Viewer twice

Impact motherboard:
*ALL
Affected functions:
Validation :
Launch SOL

4.
Category: Fix
Description:
[115461] RSC-D2R-668G4 multi sensor reading function test fail

Impact motherboard:
*ALL
Affected functions:
Validation :
Check Sensor Reading

5.
Category: Fix
Description:
[115916] IPMI Hardware Monitor Check Fail

Impact motherboard:
*ALL
Affected functions:
Validation :
Check Sensor Reading

6.
Category: Fix
Description:
[115876] [DVT] IPMI storage page can't enable blinking NVMe LED port 12-23

Impact motherboard:
*ALL
Affected functions:
Validation :
Check Sensor Reading


==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002311.bin version: 0.23.11 Date: 08-18-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : TBD

1.
Category: Fix
Description:
[114839] Cannot switch remote console between JAVA and HTML5

Impact motherboard:
*ALL
Affected functions:
Validation :
Following lab's standard validation

2.
Category: Fix
Description:
[113939] Sensor naming and numbers are not mathced with SPEC
Impact motherboard:
*ALL
Affected functions:
Validation :
Following lab's standard validation

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002308.bin version: 0.23.08 Date: 07-13-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : TBD

1.
        Category: Fix
        Description:
                [113948] WebUI will not auto back to login page after do Factory Default

        Impact motherboard:
                *ALL
        Affected functions:
        Validation :
                Following lab's standard validation

2.
        Category: Fix
        Description:
                [113945] Get CPU/MEM/Disk/FRU/RAID Controller info from MIB is fail

        Impact motherboard:
                *ALL
        Affected functions:
        Validation :
                Following lab's standard validation

3.
        Category: Fix
        Description:
                [113939] Sensor naming and numbers are not mathced with SPEC

        Impact motherboard:
                X12QCH+
        Affected functions:
        Validation :
                Following lab's standard validation

4.
        Category: Fix
        Description:
                [113917] Chassis Intru sensor will disappear after do select a sensor type category, it will appear again after do refresh.

        Impact motherboard:
                X12QCH+
        Affected functions:
        Validation :
                Following lab's standard validation

5.
        Category: Fix
        Description:
                [113737] iKVM remote install OS fail

        Impact motherboard:
                X12QCH+
        Affected functions:
        Validation :
                Following lab's standard validation

6.
        Category: Fix
        Description:
                [113559] TDP Watts display "N/A" in Component Info - CPU page

        Impact motherboard:
                X12QCH+
        Affected functions:
        Validation :
                Following lab's standard validation
				
7.
        Category: Fix
        Description:
                [113512] Updated IPMI from 00.23.05 to 00.23.06 via UI page the IP will drop due to mac address dropped and change to random mac address

        Impact motherboard:
                X12QCH+
        Affected functions:
        Validation :
                Following lab's standard validation

8.
        Category: Fix
        Description:
                [113234] [RoT] No Download evidence event log on MEL	

        Impact motherboard:
                X12QCH+
        Affected functions:
        Validation :
                Following lab's standard validation

9.
        Category: Fix
        Description:
                [112849] Update BIOS failed when I tried to do the "preserver SMBIOS" on UI

        Impact motherboard:
                X12QCH+
        Affected functions:
        Validation :
                Following lab's standard validation

10.
        Category: Fix
        Description:
                [111786] [RoT] Please modify the manual update golden and download evidence function

        Impact motherboard:
                X12QCH+
        Affected functions:
        Validation :
                Following lab's standard validation

11.
        Category: Fix
        Description:
                [109672] IPMI SOL word display abnormal.

        Impact motherboard:
                X12QCH+
        Affected functions:
        Validation :
                Following lab's standard validation

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002307.bin version: 0.23.07 Date: 06-30-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : TBD

1.
	Category: Fix
	Description:
		[111531] [SUM]sum.2.5.0_042320 execute GetGpuInfo failed

	Impact motherboard:
		*ALL
	Affected functions:
	Validation :
		1. ignore read count , only return 4 byte data

2.
	Category: Fixes
	Description:
		[113555] icon always display green when warning event
	Impact motherboard:
		X12.
	Affected functions:
		Web health event page
	Validation:
		1. Check if icon still display green when warning event.

3.
	Category: Fixes
	Description:
		[113322] Only one temp sensor for AOC-NIC, if plug two
		same model AOC-NIC into AIOM1 and AIOM2
	Impact motherboard:
		X12DDW-A6.

	Affected functions:
	Validation:
		1. Plug two AIOM cards into AIOM slot, and check sensor reading.

4.
	Category: Fixes
	Description:
		[110288] Beta -- 16914 -- 00.10.11 – Web Storage and Redfish do not show correct info about NVMe

	Impact motherboard:
		All X12 and H12 boards

	Affected functions:
	Validation:
		1.Log in to WebUI -> System --> Storage Monitoring

5.
	Category: Fixes
	Description:
		[113366] Beta -- 16914 -- 00.10.23 – Web System Crash Dump does not refresh page until user changes page and revisit
	Impact motherboard:
		All X12 boards

	Affected functions:
	Validation:
		1. Log in to WebUI --> Troubleshooting --> System Crash Dump
		2. Click "Generate" button and wait until dump finish.
		3. "Download" button will be enable.

6.
	Category: Fixes
	Description:
		[113320] No temp sensor for AOC-A25G-b2SM
		[113322] Only one temp sensor for AOC-NIC, if plug two
		same model AOC-NIC into AIOM1 and AIOM2
	Impact motherboard:
		X12DDW-A6.

	Affected functions:
	Validation:
		1. Plug two AIOM cards into AIOM slot, and check sensor reading.

7.
	Category: Fixes
	Description:
		[113313] NO T4 GPU Sensor.
	Impact motherboard:
		All MBs.
	Affected functions:
	Validation:
		1. Install NVIDIA T4 GPU.
		2. Check the sensor reading.

8.
	Description:
		[113331] [DVT]VDimm error log records in BMC SEL

	Impact motherboard:
		MBD-X12SPO-F-P / SYS-510P-MR

	Affected functions:
	Validation:
		Following lab's standard validation

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002306.bin version: 0.23.06 Date: 06-18-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : TBD

1.
        Description:
            [110204] VDIMMP2 IPMI reading vs DMM reading fail to meet within +/- 2% spec

        Impact motherboard:
            X12DPU-6

        Affected functions:
            VDIMM2ABC VDIMM2DEF reading

        Validation:
            1. Login to Web.
            2. Check the sensor reading.

2.
        Description:
            [111540] Unable to detect AOC Temp readings in RSC slot 2

        Impact motherboard:
            All X12 board with SXB1

        Affected functions:
            AOC Card temperature reading

        Validation:
            1. Login to Web.
            2. Check the AOC card temperature reading.

3.
    Description:
        [109077] [TAS] The severity of the NIC down event should be critical not informational.

    Impact motherboard:
        X11/X12

    Affected functions:
    Validation:
        Following lab's standard validation

4.
    Description:
        [110299] Added BIOS signature check in slave task so web can block out invalid BIOS images.

    Impact motherboard:
        X12 CPLD ROT

    Affected functions:
    Validation:
         1. Upload a corrupted BIOS image.
         2. BMC will return an error message.

5.
    Category: Fix
    Description:
        [111764] no inlet temp sensor..

    Impact motherboard:
        X12DDW-A6

    Affected functions:
    Validation:
        1. Insert inlet sensor model: MCP-280-00033-0N.
        2. Check the inlet sensor status.

6.
    Category: Fix
    Description:
        [111816] BETA --16914 -- 00.10.18(06/01/2020) -- Crash Screen Dump image time stamp don't sync with BMC time zone

    Impact motherboard:
        All X12 MB

    Affected functions:
    Validation:
        1. Log in to web UI.
        2. Check TroubleShooting --> Console Capture --> Crash Screen Capture time stamp is local time.

7.
    Category: Fix
    Description:
        [104410] System can enter PC1 state (99%) only

    Impact motherboard:
        X12SCZ
    Affected functions:
    Validation :
        1.check if system can enter C10 state
        2.check if HID devices are still workable or not

8.
    Category: Fixes
    Description:
        [New Web UI] Web GUI still display update process when CPLDRoT already block the update process.

    Impact motherboard:
        All H12 ROT MBs.

    Affected functions:
    Validation:
        1. Upload a corrupted BIOS image.
        2. BMC will return an error message.

9.
	Category: Fixes
    Description:
        [111588] Sensor reading shows "MB_10G TEMP' which I have is -F MB and the SKU is I210

    Impact motherboard:
        X12SPL-(LN4)F

    Affected functions:
    Validation:
        1. Log in to web UI.
        2. Check there is no MB_10G TEMP in sensor reading.

10.
    Description:
        [109870] [EVT] Sensor reading fail.

    Impact motherboard:
        X12SPZ-LN4F/SPLN6F

    Affected functions:
    Validation:
        Following lab's standard validation

11.
    Description:
        [110405] [EVT] IPMI fan control no function on FANA

    Impact motherboard:
        X12SPM-LN4F/LN6TF/TF

    Affected functions:
    Validation:
        Following lab's standard validation

12.
    Description:
        [113025] [SNMP] SNMP has additional OIDs that are not supposed to be there.
Impact motherboard:
    All MBs.
    Affected functions:
    Validation:
        1. snmpwalk -v 2c -c public {sut_ip} .1.3.6.1.4.1.21317.1.3.1.1.4.x
        2. snmpwalk -v 2c -c public {sut_ip} .1.3.6.1.4.1.21317.1.7.3.1.13.x
        3. snmpwalk -v 2c -c public {sut_ip} .1.3.6.1.4.1.21317.1.7.3.1.14.x
        4. snmpwalk -v 2c -c public {sut_ip} .1.3.6.1.4.1.21317.1.7.2.1.16.x
        5. Return "End of MIB".


==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002305.bin version: 0.23.05 Date: 06-07-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : TBD

1.
    Category: fix
    Description:
        WK23 maintenance release.  Fix new UI issues and sensor issues.
    Impact motherboard:
        All X12AST2500 ROT
    Affected functions:
    Validation:

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002304.bin version: 0.23.04 Date: 05-23-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : TBD

1.
    Category: fix
    Description:
        WK21 maintenance release.  Fix new UI issues and sensor issues.
    Impact motherboard:
        All X12AST2500 ROT
    Affected functions:
    Validation:

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002303.bin version: 0.23.03 Date: 05-14-2020
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r39
Redfish API : TBD

1.
    Category: fix
    Description:
        fixed the following PB issues:
        [109240] [EVT]JL1 can't work
        [109659] [EVT] There is no Graceful Shutdown and Power Cycle option in Power Control"
        [109870] [EVT] Sensor reading fail
        [108563] Fixed the temperature sensor detection of onboard M.2 SSD drives.

    Impact motherboard:
        All X12AST2500 ROT
    Affected functions:
    Validation:
        Please verify the issues followed by the steps in PB.

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002302.bin version: 0.23.02 Date: 05-07-2020
+ RSA2K maintenance release of v0.23.01.

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002301.bin version: 0.23.01 Date: 05-06-2020

1.
    Category: fix
    Description:
        webgui_gen2 maintenance release
    Impact motherboard:
        All X12
    Affected functions:
    Validation:
        1. webGUI

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002300.bin version: 0.23.00 Date: 04-20-2020

1.
    Category: fix
    Description:
        webgui_gen2 first release
    Impact motherboard:
        All X12
    Affected functions:
    Validation:
        1. webGUI

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002205.bin version: 0.22.05 Date: 05-14-2020

1.
    Category: fix
    Description:
        [108563] DVT Chp.1] "M2_SDD1 Temp" sensor shows "not present" while platform has M.2 NVMe drive module inserted onboard.
    Impact motherboard:
        X12DAi
    Affected functions:
    Validation:
        1. Verify the sensor reading.

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002204.bin version: 0.22.04 Date: 05-07-2020
+ RSA2K maintenance release of v0.22.03.

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002203.bin version: 0.22.03 Date: 05-06-2020

1.
    Category: fix
    Description:
        Fix smbus arbitration problem.
    Impact motherboard:
        All X12
    Affected functions:
    Validation:
        1. bmc can access smbus after BIOS POST.

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002202.bin version: 0.22.02 Date: 04-28-2020

1.
    Category: new feature
    Description:
        Enable anti-RollBack ID for bmc fw
    Impact motherboard:
        All X12
    Affected functions:
    Validation:
        1. bmc image with smaller anti-RollBack ID will resutls upgrade failure

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002201.bin version: 0.22.01 Date: 04-24-2020

1.
    Category: fix
    Description:
        Fix Java iKVM feature broken
    Impact motherboard:
        All X12
    Affected functions:
    Validation:
        1. webGUI -> Java iKVM

2.
    Category: fix
    Description:
        Fix smbus arbitration feature broken
    Impact motherboard:
        All X12
    Affected functions:
    Validation:
        1. bios have smbus access during POST

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002200.bin version: 0.22.00 Date: 04-20-2020

1.
    Category: fix
    Description:
        [RoT][Provisioning] Fix provisioning with new nand.
    Impact motherboard:
        All X12
    Affected functions:
    Validation:
        1. Provisioning

2.
    Category: improvement
    Description:
        [RoT][Provisioning] Improve UID pattern during provisoning, scheme proposed by Steven Huang and reviewed by Jason Chen.
    Impact motherboard:
        All X12
    Affected functions:
    Validation:
        1. Provisioning

3.
    Category: improvement
    Description:
        [RoT][Provisioning] If system is power_on in the begining of provisioning, bmc will power_off it.
        [RoT][Provisioning] Remove the /nv/bios/* checking
    Impact motherboard:
        All X12
    Affected functions:
    Validation:
        1. Provisioning

4.
    Category: improvement
    Description:
        [RoT] Moved provision oem command from 0x30 0x70 0xb1 to 0x30 0x68 0x28.
        [RoT] Removed legacy 0xA0 0x19 and 0xA0 0x1a commands
    Impact motherboard:
        All X12
    Affected functions:
    Validation:
        1. Provisioning

5.
    Category: fix
    Description:
        Fix ipmi_kcs crash in cburn onoff test
    Impact motherboard:
        All X12
    Affected functions:
    Validation:
        1. Provisioning

6.
    Category: improvement
    Description:
        Improve video_drv
    Impact motherboard:
        All X12
    Affected functions:
    Validation:
        1. webGUI -> preview image

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002126.bin version: 0.21.26 Date: 04-01-2020

1.
    Category: fix
    Description:
        Fix router has been overwritten in dhcp.script
    Impact motherboard:
        All X12
    Affected functions:
    Validation:
        1. webGUI -> login

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002125.bin version: 0.21.25 Date: 03-30-2020

1.
    Category: enhancement
    Description:
        Improve the logic when cpld has no key.
    Impact motherboard:
        All X12
    Affected functions:
    Validation:
        1. Provisioning

2.
    Category: fix
    Description:
        Fix CPU thermal trip SEL
    Impact motherboard:
        All X12
    Affected functions:
    Validation:

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002124.bin version: 0.21.24 Date: 03-20-2020

1.
    Category: enhancement
    Description:
        For RSA4K fw, automatic write key to CPLD UFM if there is no key.
    Impact motherboard:
        All X12
    Affected functions:
    Validation:
        1. Provisioning

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002123.bin version: 0.21.23 Date: 03-18-2020

1.
    Category: Fix
    Description:
        [104295] sensor reading is abnormal.
        [104183] IPMI function can't work.
    Impact motherboard:
        X12SPW-F/TF
    Affected functions:
    Validation:
        1. Verify the sensor reading.

2.
    Category: Fix
    Description:
        [105584] GPU sensor reading failed.
    Impact motherboard:
        X12SPW-F/TF
    Affected functions:
    Validation:
        1. Verify the sensor reading.

3.
    Category: new
    Description:
        bmc does not access nor_bios outsideCOT, ready for future cpld fw integration.
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_RSA4K_002122.bin version: 0.21.22 Date: 03-06-2020
U-Boot build time : 2013.01(Oct 6 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37

1.
    Category: fix
    Description:
        bmc/bios fw upgrade results 500 Internal Server Error
    Impact motherboard:
        All X12
    Affected functions:
    Validation :
        1a. bmc fw upgrade by webGUI or tool.
        1b. bios fw upgrade by webGUI or tool.

1.
    Category: enhancement
    Description:
        bios firmware upgrade does not require system power_off
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_RSA4K_002121.bin version: 0.21.21 Date: 03-04-2020
U-Boot build time : 2013.01(Oct 6 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37

1.
    Category: new
    Description:
        Enable cpld fw upgrade with signed fw.
    Impact motherboard:
        All X12
    Affected functions:
    Validation : java -jar SMCIPMITool.jar 172.31.12.34 ADMIN ADMIN ipmi oem generalfileupload 13 signed.bin

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002120.bin version: 0.21.20 Date: 03-02-2020
U-Boot build time : 2013.01(Oct 6 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37

1.
    Category: fix
    Description:
        Reviewed PFR related SEL and MEL
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_RSA4K_002120.bin version: 0.21.20 Date: 02-29-2020
U-Boot build time : 2013.01(Oct 6 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37

1.
    Category: new
    Description:
        Initial release of PFR RSA4K bmc firmware with debug_key
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

2.
    Category: fix
    Description:
        Reviewed PFR related SEL and MEL
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002119.bin version: 0.21.19 Date: 02-27-2020
U-Boot build time : 2013.01(Oct 6 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37

1.
    Category: fix
    Description:
        Workaround to avoid ME hang when cpld reset bmc.
        Resume bios update systemReset dialogbox, for sum integration.
        Wordaround to "Clear Product Key"
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002117.bin version: 0.21.17 Date: 02-22-2020
U-Boot build time : 2013.01(Oct 6 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37

1.
    Category: fix
    Description:
        Work with SUM 2.5
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

2.
    Category: enhancement
    Description:
        PFR cmd migrates from 21/23/61/62/63 to 11/13/51/52/53
    Impact motherboard:
        All X12
    Affected functions:
    Validation :
        1. bmc/bios firmware upgrade/restore/backup

3.
    Category: Fix
    Description:
        [106999] IPMI web update BMC failed
        [106981] IPMI no "GPU" card sensor reading
        [105873] Motherboard sensors reading from IPMI Web occur missing
                 sensors & abnormal reading
        [105726] The Fan sensors (FANC and FAND) not display
        [105686] System power on got BMC event: Voltage(1.0V LAN) going low - Assertion
        [105684] Chassis Intrusion function fail
        [105031] AC on/off stress fail, it has some IPMI SEL log
        [104691] IPMI sensor reading failed
    Impact motherboard:
        X12DPG-QT
    Affected functions:
        SUM, SMCIPMITOOL, SSM SW tools.
    Validation:
        1. Verify the sensor reading.

4.
    Category: fix
    Description:
        Update the threshold of NVIDIA RTX6000/8000
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

5.
    Category: enhancement
    Description:
        Critical data covers unique password and license data
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002116.bin version: 0.21.16 Date: 02-15-2020
U-Boot build time : 2013.01(Oct 6 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37

1.
    Category: new feature
    Description:
        Enable usb0
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

2.
    Category: fix
    Description:
        fix cpld fw upgrade
    Impact motherboard:
        All X12
    Affected functions:
    Validation :
        1. Boot bmc to insideCOT mode
        2. java -jar SMCIPMITool.jar 172.31.xx.yy ADMIN ADMIN ipmi oem generalfileupload 13 signed_cpld_fw.bin
        3. Monitor the UID or the bmc debug console

3.
    Category: enhancement
    Description:
        bios update, bios backup, bios restore operations require system power off.
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_RSA4K_002115.bin version: 0.21.15 Date: 02-14-2020
U-Boot build time : 2013.01(Oct 6 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37

1.
    Category: new feature
    Description:
        Enable RSA4K
    Impact motherboard:
        All X12 MB with cpld supporting RSA4K
    Affected functions:
    Validation :

2.
    Category: new feature
    Description:
        cpld fw upgrade with signed cpld fw
    Impact motherboard:
        All X12 MB with cpld supporting RSA4K
    Affected functions:
    Validation :
        1. Boot bmc to insideCOT mode
        2. java -jar SMCIPMITool.jar 172.31.xx.yy ADMIN ADMIN ipmi oem generalfileupload 13 signed_cpld_fw.bin
        3. Monitor the UID or the bmc debug console

3.
    Category: new feature
    Description:
        Enable usb0
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002114.bin version: 0.21.14 Date: 02-13-2020
U-Boot build time : 2013.01(Oct 6 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37

1.
    Category: fix
    Description:
        Improved CPU thermal throttle behavior, if MB has procHot pin fixed
        Fixed CPU thermal trip behavior, if MB has procHot pin fixed
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

2.
    Category: fix
    Description:
        Fix i2c attack SEL.
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

3.
    Category: New Motherboards
    Description:
        Support X12DDW, X12DPFR-AN, X12DGO
    Impact motherboard: 
        X12DDW, X12DPFR-AN, X12DGO
    Affected functions:
    Validation :

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002113.bin version: 0.21.13 Date: 02-07-2020
U-Boot build time : 2013.01(Oct 6 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37

1.
    Category: fix
    Description:
        Fix DIMM temperature related feature - readings, SEL assertion, system critical icon 
    Impact motherboard:
        All X12
    Affected functions:
    Validation :
        1. Insert fewer DIMM
        2. Monitor webGUI -> Server Health -> Sensor Readings
        3. Monitor webGUI -> Server Health -> Health Event Log

2.
    Category: new feature
    Description:
        Support Unique Password (UPW) feature, tested with IPMICFG_1.31.0
    Impact motherboard:
        All X12
    Affected functions:
    Validation :
        1. ipmicfg -uniquepwd [password]   // Set password
        2. ipmicfg -verfiypwd [password]   // Verify password
        3. ipmicfg -lockuniquepwd          // Lock UPW

3.
    Category: fix
    Description:
        Fix IPv6 login web page will timeout.
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

4.
    Category: enhancement
    Description:
        fru1 BPN allows "X12DPI-NT" and "X12DPi-NT"
    Impact motherboard:
        X12DPI
    Affected functions:
    Validation :

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002112.bin version: 0.21.12 Date: 01-30-2020
U-Boot build time : 2013.01(Oct 6 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37

1.
    Category: fix
    Description:
        Disable usb0 
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

2.
    Category: fix
    Description:
        [PFR] SEL for backup image 
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002111.bin version: 0.21.11 Date: 01-25-2020
U-Boot build time : 2013.01(Oct 6 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37

1.
    Category: fix
    Description:
        Activate key via HSM 
    Impact motherboard:
        All X12
    Affected functions:
    Validation :
        http://10.135.15.108/activate/, SFT-OOB-LIC

2.
    Category: fix
    Description:
        Improvement of i2c arbitration with bios
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

3.
    Category: fix
    Description:
        BOOTID command remap from 0xA0 0x19 to 0x68 0x27, 
        GETCPLDVER command remap from 0xA0 0x1A to 0x68 0x29
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002110.bin version: 0.21.10 Date: 01-21-2020
U-Boot build time : 2013.01(Oct 6 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37

1.
    Category: fix
    Description:
        Update for memory group function
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002109.bin version: 0.21.09 Date: 01-20-2020
U-Boot build time : 2013.01(Oct 6 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37

1.
    Category: fix
    Description:
        BOOTID command remap from 0xA0 0x19 to 0x68 0x26, 0xA0 0x1A to 0x68 0x28
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002108.bin version: 0.21.08 Date: 01-17-2020
U-Boot build time : 2013.01(Oct 6 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37

1.
    Category: fix
    Description:
        Fix slow webGUI issues
    Impact motherboard:
        All X12
    Affected functions:
    Validation :
        1. Use webGUI

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_002107.bin version: 0.21.07 Date: 01-14-2020
U-Boot build time : 2013.01(Oct 28 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37

1.
    Category: fix
    Description:
        Enable i2c arbitration
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_02106.bin version: 0.21.06 Date: 01-10-2020
U-Boot build time : 2013.01(Oct 28 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37

1.
    Category: fix
    Description:
        Review X12 GUID
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

2.
    Category: new feature
    Description:
        Add usb0 interface, for potential usbnet application
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

3.
    Category: new feature
    Description:
        Backup ACTIVE image to Nand
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

4.
    Category: fix
    Description:
        Reviewed PFR related SEL
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

5.
    Category: fix
    Description:
        Add retry to set default gateway function
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

6.
    Category: fix
    Description:
        Apply new Memory Group API
    Impact motherboard:
        X12DPI
    Affected functions:
    Validation :
        1. webGUI -> Server Health -> Sensor Readings

7. 
    Category: fix
    Description:
        Fix Too_many_files_open burnIn test issue
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

8. 
    Category: fix
    Description:
        Fix auto_bmc_recovery_fail_to_restore_fru1|sdr
    Impact motherboard:
        All X12DPI
    Affected functions:
    Validation :

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_02105.bin version: 0.21.05 Date: 12-28-2019
U-Boot build time : 2013.01(Oct 28 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37

1.
    Category: fix
    Description:
        Enable SEL with auto recovery.
    Impact motherboard:
        All X12
    Affected functions:
    Validation :
        1. Make sure the MB is with good last known good image, and/or golden image.
        2. Erase the nor by programmer
        3. AC on, monitor the auto recovery process by cpld.
        4. When the recovery is done, webGUI -> Server Health -> Health Event Log

2.
    Category: fix
    Description:
        Enahce bmc reboot sequence
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

3. 
    Category: fix
    Description:
        Improve i2c protection map
    Impact motherboard: X12DPI
    Affected functions:
    Validation :

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_02104.bin version: 0.21.04 Date: 12-23-2019
U-Boot build time : 2013.01(Oct 28 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37

1.
    Category: fix
    Description:
        Fix bmc keep rebooting
    Impact motherboard:
        All X12
    Affected functions:
    Validation :
        1. Program nor_bmc with programmer
        2. AC on, assign macAddr, assign fru1 if required
        3. Monitor bmc will not keep rebooting

2.
    Category: fix
    Description:
        Redfish 1.8
    Impact motherboard:
        All X12
    Affected functions:
    Validation :

3. 
    Category: fix
    Description:
        Sensor review
    Impact motherboard: X12DPi-N, X12DPi-NT, X12DAI, X12DPU
    Affected functions:
    Validation :
        1. webGUI -> Server Health -> Sensor Readings

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_021_03.bin version: 0.21.03 Date: 12-16-2019
U-Boot build time : 2013.01(Oct 28 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37
Redfish API : Redfish_API_full_list_2019_07_10.xlsx

1.
    Category: fix
    Description:
        Integrate with new HSM oob license format
    Impact motherboard:
        X12SPA-TF, X12DPG-Q.
    Affected functions:
    Validation :

==============================================================================================================================
Filename: SMT_X12AST2500_ROT_02102.bin version: 0.21.02 Date: 12-07-2019
U-Boot build time : 2013.01(Oct 28 2019)
Java SOL Viewer version : v0.5.13
Java iKVM Viwer version : v1.69 r37
Redfish API : Redfish_API_full_list_2019_07_10.xlsx

1.
    Category: fix
    Description:
        Integrate with new HSM oob license format
    Impact motherboard:
        All X12
    Affected functions:
    Validation :
        1. curl the oob.json
        2. webGUI -> Miscellaneous -> Activate License

2.
    Category: fix
    Description:
        Improve X12DPI sensor naming
    Impact motherboard:
        X12DPI
    Affected functions:
    Validation :
        1. curl the oob.json
        2. webGUI -> Server Health -> Sensor Readings

3.
    Category: New Motherboards
    Description:
        Support X12DSU, X12DAI, X12SPI
    Impact motherboard: 
        X12DSU, X12DAI, X12SPI
    Affected functions:
    Validation :
