================================================================================
Filename: BMC_H13AST2600-F401MS_20250213_01.03.09_STDsp.bin
version: 01.03.09
Date: 2025-02-13
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.57
Redfish API: Redfish_1_21_API_full_list_20241227
RNDIS|CDC-ECM: RNDIS and CDC-ECM
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P, MBD-H13SRE-F

1.
    Category: Fix
    Description:
        [192396] [IPMIECO 01.03.07] SATC Redfish test failed

    Impact motherboard:
        All MBs.

    Affected functions:
        N/A.

    Validation:
        1. run SATC automation test.

2.
    Category: Fix
    Description:
        [192867] [IPMI ECO 01.03.07]Redfish automation test failure.

    Impact motherboard:
        All MBs.

    Affected functions:
        N/A.

    Validation:
        1. run SATC automation test.

3.
    Category: Fix
    Description:
        [193146] [IPMI ECO v01.03.07] [COMBINED ECO] Automation tests Failure.

    Impact motherboard:
        All MBs.

    Affected functions:
        N/A.

    Validation:
        1. run combined ECO failed test cases TC0035 & TC2038.

4.
    Category: Fix
    Description:
        [193833] ECO -- 22739 -- 01.03.08(20250110) -- Redfish -- Unable to Send test event with valid EventTimestamp format.

    Impact motherboard:
        All MBs.

    Affected functions:
        N/A.

    Validation:
        1. Send POST request /redfish/v1/EventService/Actions/EventService.SubmitTestEvent/ with body
            {"EventId": "TestEventId",
            "EventTimestamp": "2017-08-08T08:24:00Z",
            "Severity": "Warning",
            "Message": "TestMessage",
            "MessageId": "Required",
            "MessageArgs": ["args"],
            "OriginOfCondition": "/redfish/v1/"}

        2. Check return value

5.
    Category: Fix
    Description:
        [193912] ECO -- 22739 -- 01.03.08(20250110) -- WEB -- When updating CPLD, [MEL-0200] did not appear, and description of [MEL-0201] does not match the spec.

    Impact motherboard:
        All non-RoT MBs support motherboard CPLD update.

    Affected functions:
        N/A.

    Validation:
        1. Login BMC web with ADMIN privileges
        2. Go to Maintenance -> Firmware Management page
        3. Select Type : Motherboard CPLD1
        4. Select File : Upload "CPLD_H13SRE_F-4000EE07_20240826_07.XX.XX_STDsp.jed"
        5. File Version : Check new version displayed is correct -> Press Update button
        6. Wait CPLD update completely, check MELs

6.
    Category: Fix
    Description:
        [193921] ECO -- 22739 -- 01.03.08(20250110) -- -- WEB -- Will receive two [MEL-0072] when sending a Redfish alert.

    Impact motherboard:
        All MBs.

    Affected functions:
        N/A.

    Validation:
        1. Login with BMC web with ADMIN Network Privileges
        2. Go to Configuration -> Notifications -> Modify Alert
        3. Protocol select Redfish
        4. Event Type select Alert
        5. Destination Address : Input SATC service hosting address (ex. http://10.184.4.35:8080)
        6. Context input 1qaz2wsx
        7. Press Test Information Alert button
        8. Check redfish.log via SATC service hosting

7.
    Category: Fix
    Description:
        [194163] ECO -- 22739 -- 01.03.08(20250110) -- SAA -- Unable to GetPsuInfo via SAA tool.

    Impact motherboard:
        All MBs.

    Affected functions:
        N/A.

    Validation:
        1. SSH into RHEL OS
        2. ./saa -I Redfish_HI -u ADMIN -p 'ADMIN' -c GetPsuInfo
        3. Should be able to get psu info via SAA successfully.

8.
    Category: Fix
    Description:
        [194398] ECO — 22739 — 01.03.08 (2025/01/10) — [SUMECO] — Reboot BIOS will stuck at post code 10 over 20 mins.

    Impact motherboard:
        MBD-H13SRD-F-P

    Affected functions:
        N/A.

    Validation:
        1. Login SUT RHEL OS.
        2. Execute command with --reboot, i.g. : ./sum -c ChangeDmiInfo --file dmi_template.txt --reboot
        3. Host should be able to boot to OS without hanging at post code 10.

9.
    Category: Fix
    Description:
        [195022] [SSM] It got Error message: (Failed to get the system information. Cannot download the SMBIOS file.) on the Redfish system information on the H13SRD-F

    Impact motherboard:
        All MBs.

    Affected functions:
        N/A.

    Validation:
        1. POST /restapi/Actions/File.Generate. with body {"Name":"bios_fullsmbios"}

================================================================================
Filename: BMC_H13AST2600-F401MS_20250110_01.03.08_STDsp.bin
version: 01.03.08
Date: 2025-01-10
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.57
Redfish API: Redfish_1_14_API_full_list_20240726
RNDIS|CDC-ECM: RNDIS and CDC-ECM
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P, MBD-H13SRE-F

1.
    Category: Fix
    Description:
        [190161] [SCC_v3.7.0_b2411151445][AS -3015MR-H10TNR] LinkStatus should show "null" in Redfish EthernetInterfaces when AOC-CGP-i2 does not support PLDM.

    Impact motherboard:
        All MBs.

    Affected functions:
        N/A.

    Validation:
        1. Install AOC-CGP-i2.
        2. Check "LinkStatus" in redfish.

2.
    Category: Fix
    Description:
        [190173] [SCC_v3.7.0_b2411151445][AS -3015MR-H10TNR] BMC event log between SCC and BMC webUI do not match.(Memory error injection)

    Impact motherboard:
        All MBs.

    Affected functions:
        N/A.

    Validation:
        1. Add AS -3015MR-H10TNR to SCC.
        2. Trigger some errors to SUT.
        3. Compare with BMC webUI and SCC.

3.
    Category: Fix
    Description:
        [192396] [IPMIECO 01.03.07] SATC Redfish test failed

    Impact motherboard:
        All MBs.

    Affected functions:
        N/A.

    Validation:
        1. Run SATC redfish test failed item.

4.
    Category: Fix
    Description:
        [192867] [IPMI ECO 01.03.07]Redfish automation test failure.

    Impact motherboard:
        All MBs.

    Affected functions:
        N/A.

    Validation:
        1. Run SATC redfish test failed item.

5.
    Category: Fix
    Description:
        [192992] ECO -- 22739 -- 01.03.07(20241120) -- [IKVM] -- The popup message for IKVM reset does not align with the SPEC.

    Impact motherboard:
        All MBs.

    Affected functions:
        N/A.

    Validation:
        1. Login Web with ADMIN and switch to Remote Control> Launch Console-> Select HTML5 -> press 'Launch Console' button
        2. Open an IKVM session
        3. Press the Ikvm Help page on side bar
        4. Do Ikvm reset
        5. Check Ikvm return message

6.
    Category: Fix
    Description:
        [192994] ECO -- 22739 -- 01.03.07(20241120) -- [Redfish] -- Time difference of 1 hour in (UTC+10:30) Lord Howe Island with Auto Daylight Saving Time on or off.

    Impact motherboard:
        All MBs.

    Affected functions:
        N/A.

    Validation:
        1.Set the Time Zone to (UTC+10:30) Lord Howe Island and Auto Day light Saving Time.
        2.Set NTP enable.
        3.Check the setting on NTP is enabled and Auto Day light Saving Time is true
        4.Get the Date and Time
        5.Set Auto Day light Saving Time to false
        6.Get the Date and Time again.
        7.Compare the return Date and Time between step 4 and step 6.

7.
    Category: Fix
    Description:
        [189064] ECO -- 22739 -- 01.03.06(2024/09/25) -- Web -- Unable to receive Warning and Critical SMTP test alert mail

    Impact motherboard:
        All MBs.

    Affected functions:
        N/A.

    Validation:
        1. Setup SMTP environment on SMTP page
        2. Setup Warning severity SMTP alert on Alert page
        3. Setup Critical severity SMTP alert on Alert page
        4. Tap on Send Test Alert button, check if test alert mail has received in mailbox
        5. Setup Information severity SMTP alert on Alert page
        6. Tap on Send Test Alert button, check if test alert mail has received in mailbox

================================================================================
Filename: BMC_H13AST2600-F401MS_20241120_01.03.07_STDsp.bin
version: 01.03.07
Date: 2024-11-20
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.57
Redfish API: Redfish_1_14_API_full_list_20240726
RNDIS|CDC-ECM: RNDIS and CDC-ECM
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P, MBD-H13SRE-F

1.
    Category: Fix
    Description:
        [182623] ECO -- 22739 -- 01.03.02(2024/08/02)-- Web -- [MEL-0132] doesn't appear after closing all Java ikvm screens via ikvm reset

    Impact motherboard:
        All MBs.

    Affected functions:
        N/A.

    Validation:
        1. Login BMC web as ADMIN
        2. Launch ikvm via 'JAVA plug-in' and utilize openJDK to open jnlp file
        3. Check 'User list' on Java ikvm
        4. Do ikvm reset on BMC web
        5. Close ikvm warning alert
        6. Check MEL messages
        7. Launch ikvm ikvm, then repeat step 3-setp 6
        8. [MEL-0132] iKVM was closed successfully. (SessionID) should appear

2.
    Category: Fix
    Description:
        [184296] [Beta IPMI ECO v01.03.03] Some information displays N/A in Mutil Node Page.

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SRE-F

    Affected functions:
        N/A.

    Validation:
        Check if CPLD version on dashboard and multinode page are the same.

3.
    Category: Fix
    Description:
        [185248] [Beta IPMI ECO v01.03.05] COMBINEDECO Automation tests Failure.

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        N/A.

    Validation:
        Run Combined ECO TC0035.

4.
    Category: Fix
    Description:
        [182838] [IPMIECO 01.03.02] Chassis Intrusion Reset button will be missing after zoom in or out the web browser
    Impact motherboard:
        All MBs.
    Affected functions:
        WebUI
    Validation:
        1. Login to Web GUI
        2. Go to Sensor page
        3. Zoom-in/out page and check intrustion button

5.
    Category: Fix
    Description:
        [183453] Several sensor name reported by BMC are not match to the spec.
    Impact motherboard:
        H13SAE-MF
    Affected functions:
        Sensor name.
    Validation:
        It should be match as Supermicro_BMC_Sensor_Naming_Guildeline_2.8_Draft_06092024.

6.
    Category: Fix
    Description:
        [189004] ECO -- 22739 -- 01.03.06(2024/09/25)-- Web -- Air Cooling display area is unable to be expanded after expand and collapse couple of times
    Impact motherboard:
        All MBs.
    Affected functions:
        WebUI
    Validation:
        1. Login BMC web as ADMIN
        2. Enter to Cooling tab in Component Info page
        3. Constantly Expand and collapse Air Cooling display area
        4. Observe if it can be expanded
        5. Tap on Refresh button and check again

7.
    Category: Fix
    Description:
        [189006] ECO -- 22739 -- 01.03.06(2024/09/25)-- Web -- Unable to save network config when IPv6 is in static mode
    Impact motherboard:
        All MBs.
    Affected functions:
        WebUI
    Validation:
        1. Login BMC Web as ADMIN
        2. Enter to Network page on Configuration tab, IPv6 should be static mode and no address is set
        3. Input 2001::123, 64, 2001::FFFF:FFFF:FFFF:FFFF on IPv6 Address, Prefix Length and Gateway IP respectively
        4. Tap on Save button
        5. Only modify IPv6 Address and tap on Save button again
        6. Only modify Prefix Length and tap on Save button again
        7. Only tap Gateway IP textfield and tap on Save button again
        8. Only modify Gateway IP and tap on Save button again
8.
    Category: Fix
    Description:
        [189012] ECO -- 22739 -- 01.03.06(2024/09/25)-- Web -- Login BMC web display html source code after reload IPMI Configuration File
    Impact motherboard:
        All MBs.
    Affected functions:
        N/A
    Validation:
        1. Follow SATC Automation Web_Function Test step for BMC Setting > Test Reload IPMI Configuration File

================================================================================
Filename: BMC_H13AST2600-F401MS_20240925_01.03.06_STDsp.bin
version: 01.03.06
Date: 2024-09-25
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.55
Redfish API: Redfish_1_14_API_full_list_20240726
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P, MBD-H13SRE-F

1.
    Category: Fix
    Description:
        [180479] Onboard dedicated BMC LAN does not work when using standard IPMI FW:01.02.12(6/12/2024).

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        BMC dedicate LAN.

    Validation:
        Use below command to switch BMC dedicated LAN to onboard and check if it can work correctly.

        0x30 0x70 0x4 0x0 -> read mode, 0: Fiber(switchboard), 1: UTP(onboard)

        0x30 0x70 0x4 0x1 0x0 -> Fiber(default, switchboard)

        0x30 0x70 0x4 0x1 0x1 -> UTP(onboard)

 
2.
    Category: Fix
    Description:
        [182617] ECO -- 22739 -- 01.02.06(2024/07/12)-- Web -- IPv6 address can be nullable, which doesn't match 1.34 spec

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SAE-MF-P, MBD-H13SRE-F

    Affected functions:
        N/A

    Validation:
        check if the prompt text message match spec.

3.
    Category: Fix
    Description:
        [184154] Onboard dedicated BMC LAN settings cannot be retained after AC ON/OFF.

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        N/A

    Validation:
        1. Use below command to switch BMC dedicated LAN to onboard and check if it can work correctly.

            0x30 0x70 0x4 0x0 -> read mode, 0: Fiber(switchboard), 1: UTP(onboard)

            0x30 0x70 0x4 0x1 0x0 -> Fiber(default, switchboard)

            0x30 0x70 0x4 0x1 0x1 -> UTP(onboard)

        2. Do AC cycle.

        3. Check if BMC dedicate LAN setting is kept.

4.
    Category: Fix
    Description:
        [184296] [Beta IPMI ECO v01.03.03] Some information displays N/A in Mutil Node Page.

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SRE-F

    Affected functions:
        N/A

    Validation:
        check if information on multinode page displays correctly.

5.
    Category: Fix
    Description:
        [184866] [Beta IPMI ECO v01.03.03]BMC shared LAN cannot get BMC IP when used with AOC-CTGS-i2T.

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        N/A

    Validation:
        1.The "LAN SW" and "Micro_LP LAN1" ports are connected to the LAN cable respectively.
        2.Remove LAN cable on LAN SW
        3.BMC shared LAN should be able to get BMC IP.
 

================================================================================
Filename: BMC_H13AST2600-F401MS_20240913_01.03.05_STDsp.bin
version: 01.03.05
Date: 2024-09-13
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.55
Redfish API: Redfish_1_14_API_full_list_20240726
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P, MBD-H13SRE-F

1.
    Category: Fix
    Description:
        [184295] [Beta IPMI ECO v01.03.03] Through Node1, there is no MC(CPLD backplane) icon to update the backplane CPLD firmware.

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        Web

    Validation:
        1. Login to Web GUI
        2. Firmware Update
        3. Check MC icon

2.
    Category: Fix
    Description:
        [184292] [Beta IPMI ECO v01.03.03] The update page does not show the New CPLD version when updating CPLD.

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        N/A

    Validation:
        1. Login to Web GUI
        2. Firmware Update
        3. Check new CPLD version when updating CPLD.

3.
    Category: Fix
    Description:
        [184677] [Beta IPMI ECO v01.03.03] Redfish automation test fail.

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        N/A

    Validation:
        1. Run Redfish automation

4.
    Category: Fix
    Description:
        The OS hangs on POST code 99.

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        N/A

    Validation:
        1. Update BMC to V01.03.05
        2. Login to Web GUI
        3. Remote Control -> Launch Console
        4. Power Reset

5.
    Category: Fix
    Description:
        Fix system cannot get BMC version corrcetly on non-RoT platform issue.

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        N/A

    Validation:
        1. Check BMC version correctly.

================================================================================
Filename: BMC_H13AST2600-F401MS_20240830_01.03.04_STDsp.bin
version: 01.03.04
Date: 2024-08-30
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.55
Redfish API: Redfish_1_14_API_full_list_20240726
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P, MBD-H13SRE-F

1.
    Category: Fix
    Description:
        [183038] [DVT]The "Enable Smart Power" button on the WebGUI is gray and cannot be toggled.

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SAE-MF-P, MBD-H13SRE-F

    Affected functions:
        N/A

    Validation:
        1. Login to Web GUI
        2. System -> Component Info
        3. Check if smart power tab is displayed accordingly.

2.
    Category: Fix
    Description:
        [178590] [EVT] When the LAN cable is not connected, the IPMI Link LED is always on.
        [180479] Onboard dedicated BMC LAN does not work when using standard IPMI FW:01.02.12(6/12/2024).

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        N/A

    Validation:
        Desc:
            Get or Set the Dedicated LAN Mode cmd for the MBD-H13SRE-F.
         req: 0x30 0x70 0x04
            Data 1: [0: Get, 1: Set]
            Data 2: for Set data [0: Fiber, 1: UTP]
         rsp:
            Data 1: for Get data [0: Fiber, 1: UTP]

3.
    Category: Fix
    Description:
        [181762] [DVT] RADIUS service not works with IPv6.

    Impact motherboard:
        All motherboards.

    Affected functions:
        RADIUS

    Validation:
        1.Go to [Configuration] -> [Account Services] -> [Directory Service]
        2.Turn on [RADIUS]
        3.Set Radius server by IPv6 and try to login

4.
    Category: Fix
    Description:
        [182689] [DVT]The backplane CPLD firmware is updated through IPMI Web, but the update progress will stay at 96%.

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        Backplane CPLD update.

    Validation:
        1. Login web.
        2. Firmware update -> Choose MC (CPLD Backplane) to update.
        3. Check if web UI redirect to task list page and update progress is 100%.

5.
   Category: Fix
    Description:
        [184053] [AS-3015MR-H10TNR] IPMI web no show sensor NVMe_SSD2 Temp temperature.

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        NVMe_SSD Temp.

    Validation:
        1. Install HDS-MUN-MTFDKCC960TFR1BC5 NVME U.2 * 2.
        2. Boot cburn-88.
        3. Log in IPMI Web.
        4. Check IPMI Web show sensor NVMe_SSD2 Temp temperature.

================================================================================
Filename: BMC_H13AST2600-F401MS_20240813_01.03.03_STDsp.bin
version: 01.03.03
Date: 2024-08-13
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.55
Redfish API: Redfish_1_14_API_full_list_20240514
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P, MBD-H13SRE-F

1.
    Category: Enhancement
        Skip GPIOS5 checking of H13SRE.

    Description:

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        N/A

    Validation:
        Check if BMC dedicate LAN on switchboard works correctly.

2.
    Category: Fix
        [DVT] Unable to restore UID control after reloading saved ipmi configuration. 

    Description:

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SAE-MF-P, MBD-H13SRE-F
    Affected functions:
        N/A

    Validation:
        Check if UID is turned off after BMC reset.

3.
    Category: Fix
        [DVT] boot.avi size is 0B when setting 'Record until POST ends' at Console Capture Video.

    Description:

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SRE-F

    Affected functions:
        Console capture.

    Validation:
        1. Login Web GUI and change page to Maintenance -> Troubleshooting -> Console Capture -> Console Capture Video
        2. Switch 'Enable' to 'ON'
        3. Choose option to 'Record until POST ends'
        4. Press down button 'Apply'
        5. Reboot SUT
        6. Wait till POST end
        7. Check the boot.avi size

================================================================================
Filename: BMC_H13AST2600-F401MS_20240802_01.03.02_STDsp.bin
version: 01.03.02
Date: 2024-08-02
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.55
Redfish API: Redfish_1_14_API_full_list_20240514
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P, MBD-H13SRE-F

1.
    Category: Fix

    Description:
        [181216] [DVT] DMTF/Redfish-Reference Checker test is fail.

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        N/A

    Validation:
        Run Redfish automation.

2.
    Category: Fix

    Description:
        [181265] [DVT] Redfish automtion test fail.

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        N/A

    Validation:
        Run Redfish automation.

3.
    Category: Fix

    Description:
        [181581] [DVT] Unable to detect Node status on "Multi Node" page.

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        N/A

    Validation:
        Check the display of the web UI multinode page.

4.
    Category: Fix

    Description:
        Change the MB fan to a fan board through the BPN CPLD.

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        N/A

    Validation:
        Check fan read/write function works correctly.

===============================================================================
Filename: BMC_H13AST2600-F401MS_20240723_01.03.01_STDsp.bin
version: 01.03.01
Date: 2024-07-23
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.55
Redfish API: Redfish_1_11_API_full_list_20231218
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P, MBD-H13SRE-F

1.
    Category: Fix

    Description:
        [178964] [EVT] CPU overheat on BMC HEL during eburn stress test.
        [181142] [DVT] No GPU temperature sensor reading on IPMI Web when nvidia Tesla T4 GPU installed on RSC.
        [179224] [DVT] AOC sensor reading function test failed.
        [179697] Hardware Monitor - VBAT

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        Sensor

    Validation:
        1. Check CPU upper critical threshold to 100.
        2. Confirm VBAT thresholds for battery low and battery failed.
        3. Verify AOC and GPU slot mapping is correct.

2.
    Category: Fix

    Description:
        [179927] [SDO]It doesn't support the System (BIOS) Embedded Diagnostics function on H13SRE-F

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        N/A

    Validation:
        Check new feature in BMC 1.03.

3.
    Category: Fix

    Description:
        [179629] [SMCIPMITool] Test fail via smstc of H13SRE-F

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        IPv6

    Validation:
        Check TC0137 - IPMI Management - ipmi lan ipv6

4.
    Category: Fix

    Description:
        [180157] BMC Web UI cannot show current memory operating speed.

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        N/A

    Validation:
        Check current memory operating speed is displayed correctly on the Web UI.

================================================================================
Filename: BMC_H13AST2600-F401MS_20240612_01.02.12_STDsp.bin
version: 01.02.12
Date: 2024-06-12
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.55
Redfish API: Redfish_1_11_API_full_list_20231218
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P, MBD-H13SRE-F

1.
    Category: Fix
    Description:
        [176774] SMSTC automation test
        [177923] ECO -- 27739 -- 01.02.10(20240528) -- CombinedECO -- Failed due to DIMM info is not match with dmi_template.
        [178264] AS-2015A-TR SUM test fail #3006
        [178170] [SAA_1.0.0b20240516] SAA SMSTC test fail on H13SAE-MF.
    Impact motherboard:
        All MBs.
    Affected functions:
        N/A
    Validation:
        [176774] Run SMCTC CombinedECO TC1001, TC2012, TC2020.
        [177923] Run SMCTC CombinedECO TC2012, TC2020.
        [178264] Run SMCTC SUMECO TC3006.
        [178170] Run SMCTC SAAECO TC3006, TC4096, TC4101.

2.
    Category: Fix
    Description:
        [178407] ECO -- 22739 -- 01.02.11(20240531) -- GUI -- IP Access Control Help page is inconsistent with UI spec.
    Impact motherboard:
        All MBs.
    Affected functions:
        WebUI
    Validation:
        Check HELP page the IP Access Control help info description is consistent with UI SPEC.

3.
    Category: Fix
    Description:
        [176568] ECO -- 22739 -- 01.02.08(2024/05/08) -- Web -- VDD_MISC sensor name doesn't match with spec
    Impact motherboard:
        H13SAE-MF
    Affected functions:
        Sensor name.
    Validation:
        It should be match as Supermicro_BMC_Sensor_Naming_Guildeline_2.8_Draft_06092024.

================================================================================
Filename: BMC_H13AST2600-F401MS_20240531_01.02.11_STDsp.bin
version: 01.02.11
Date: 2024-05-31
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.55
Redfish API: Redfish_1_11_API_full_list_20231218
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P, MBD-H13SRE-F

1.
    Category: Fix

    Description:
        Adjust H13SRE sensor reading.

    Impact motherboard:
        MBD-H13SRE-F

    Affected functions:
        Sensor

    Validation:
        Check onboard U2 sensor reading and if system recognizes backplane.

================================================================================
Filename: BMC_H13AST2600-F401MS_20240528_01.02.10_STDsp.bin
version: 01.02.10
Date: 2024-05-28
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.55
Redfish API: Redfish_1_11_API_full_list_20231218
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P, MBD-H13SRE-F

1.
    Category: Fix
    Description:
        [176774] SMSTC automation test
    Impact motherboard:
        MBD-H13SAE-MF-P
    Affected functions:
        Sensor
    Validation:
        Run SMCTC CombinedECO TC0031.

================================================================================
Filename: BMC_H13AST2600-F401MS_20240521_01.02.09_STDsp.bin
version: 01.02.09
Date: 2024-05-21
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.55
Redfish API: Redfish_1_11_API_full_list_20231218
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P, MBD-H13SRE-F

1.
    Category: Fix
    Description:
        Fix CPU temperature reading from BPN CPLD.

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SRE-F

    Affected functions:
        N/A.

    Validation:
        1.  read CPU temperature from BPN CPLD by below raw commands:
            raw 0x06 0x52 0x07 0x82 0x01 0x00 0x38: Node 1, CPU1
            raw 0x06 0x52 0x07 0x82 0x01 0x00 0x78: Node 2, CPU1
            raw 0x06 0x52 0x07 0x82 0x01 0x00 0xB8: Node 3, CPU1
            raw 0x06 0x52 0x07 0x82 0x01 0x00 0xF8: Node 4, CPU1
            raw 0x06 0x52 0x07 0x82 0x01 0x01 0x38: Node 5, CPU1
            raw 0x06 0x52 0x07 0x82 0x01 0x01 0x78: Node 6, CPU1
            raw 0x06 0x52 0x07 0x82 0x01 0x01 0xB8: Node 7, CPU1
            raw 0x06 0x52 0x07 0x82 0x01 0x01 0xF8: Node 8, CPU1

2.
    Category: Fix
    Description:
        [176564] ECO -- 22739 -- 01.02.06(2024/04/22) -- Web -- Error message was unexpected when uploading 1 byte TSIG file
    Impact motherboard:
        All MBs.
    Affected functions:
        Web
    Validation:
        1. Login BMC web GUI -> Go Configuration ->BMC Settings
        2. Date and Time -> Enable NTP
        3. Go DDNS page -> Enable Dynamic Update and Enable TSIG Authentication
        4. Upload "TSIG .key" and "TSIG.private" with 0kb file (reference attach file)

3.
    Category: Fix
    Description:
        [176571] ECO -- 22739 -- 01.02.08(2024/05/08) -- Web -- Error message was unexpected when trying to disable logined user
    Impact motherboard:
        All MBs.
    Affected functions:
        Web
    Validation:
        1. Open browser 1 and Login web with ADMIN.
        2. Create KC123 account.
        3. Open browser 2 to login with KC123 user.
        4. Return to browser 1 and login with ADMIN to disable KC123 user.

4.
    Category: Fix
    Description:
        [176582] ECO -- 22739 -- 01.02.08(2024/05/08) -- SMCIPMITool(2.28.0_240411) -- NTP timezone unexpectedly changed after setting up ntp address
    Impact motherboard:
        All MBs.
    Affected functions:
        NTP
    Validation:
        1. SMCIPMITool <BMC IP> <user id> <password> shell
            step-1 ipmi oem x10cfg ntp state enable
            step-2 ipmi oem x10cfg ntp timezone 16
            step-3 ipmi oem x10cfg ntp daylight yes
            step-4 ipmi oem x10cfg ntp primary <ntp ip>
        2. Check if the time zone is correct

5.
    Category: Fix
    Description:
        [176698] ECO -- 22739 -- 01.02.08(2024/05/08) -- Web -- Sensor severity filter is malfunction when thresholds is enabled
    Impact motherboard:
        All MBs.
    Affected functions:
        Web
    Validation:
        1. Enter to Sensor tab in Component info page
        2. Turn severity filter on and off and check sensors in sensor reading
        3. Enable Show Thresholds
        4. Turn severity filter on and off and check sensors in sensor reading

================================================================================
Filename: BMC_H13AST2600-F401MS_20240508_01.02.08_STDsp.bin
version: 01.02.08
Date: 2024-05-08
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.54
Redfish API: Redfish_1_11_API_full_list_20231218
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P, MBD-H13SRE-F

1.
    Category: Initial
    Description:
        Initial
    Impact motherboard:
        MBD-H13SRE-F
    Affected functions:
        N/A
    Validation:
        Initial board bring up bmc FW.

================================================================================
Filename: BMC_H13AST2600-F401MS_20240423_01.02.07_STDsp.bin
version: 01.02.07
Date: 2024-04-23
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.54
Redfish API: Redfish_1_11_API_full_list_20231218
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P

1.
    Category: Fix
    Description:
        [174837] ECO – 22739 – 01.02.06 (2024/04/15) –BMC– Fail to cancel BMC/BIOS update after enter update stage.
    Impact motherboard:
        All MBs.
    Affected functions:
        Web update.
    Validation:
        Cancel update firmware is now available.

2.
    Category: Fix
    Description:
        [163486] ECO -- 22739 -- 01.01.09 (2023/09/14) -- Incorrect ikvm reset error code when opening more than 2-3 sessions. (code: 12592, reason: 01)

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SAE-MF-P

    Affected functions:
        IKVM.

    Validation:
        1. Login web with ADMIN.
         
        # Launch 1 session 
        2. Remote Control → Launch Console → Current Interface → Choose "HTML 5" → Press "Lanuch Console" (Press 1 time) → Check is launch 1 session → Waiting few seconds to see OS
        3. IKVM Reset → Press "Reset"
        4. Check IKVM is reset and check reset error code = 1006.
         
        # Launch 2 session
        5. Remote Control → Launch Console → Current Interface → Choose "HTML 5" → Press "Lanuch Console" (Press 2 times) → Check is launch 2 session → Waiting few seconds to see OS
        6. IKVM Reset → Press "Reset" 
        7. Check both 2 IKVM is reset and check reset error code = 1006. 
         
        8. Repeat step 2~4 to launch more than 2 session.

3.
    Category: Fix
    Description:
        [171065] ECO -- 22739 -- 01.01.12(2024/01/19) -- Web -- MEL will record extra launch ikvm success msg when doing ikvm reset.

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SAE-MF-P

    Affected functions:
        IKVM.

    Validation:
        1. Login web with ADMIN.
        2. Remote Control → Launch Console → Current Interface : HTML5 → Press "Launch Console"
        3. Maintenance → Maintenance Event Log
        4. Repeat Step 2~3 for 4 times and check MEL has 4 ikvm lanuched success msg.
        5. Remote Control → IKVM Reset → Press "Reset"
        6. Maintenance → Maintenance Event Log check has 4 ikvm closed success msg.

4.
    Category: Fix
    Description:
        [171570] STD -- 22739 -- 01.02.01 (2024/02/02) -- WEB -- MEL will record extra launch ikvm success msg when do ikvm reset.

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SAE-MF-P

    Affected functions:
        IKVM.

    Validation:
        1. Login web with ADMIN.
        2. Remote Control → Launch Console → Current Interface : HTML5 → Press "Launch Console"
        3. Maintenance → Maintenance Event Log
        4. Repeat Step 2~3 for 4 times and check MEL has 4 lanuch ikvm success msg.
        5. Remote Control → IKVM Reset → Press "Reset"
        6. Maintenance → Maintenance Event Log check only has 4 ikvm closed success msg.

5.
    Category: Fix
    Description:
        [173680] [IPMI ECO 01.02.05] Redfish automation tool check is fail.

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SAE-MF-P

    Affected functions:
        IKVM.

    Validation:
        Run SATC test case:
            Test URIs Reachable When DCMS Activated

6.
    Category: Fix
    Description:
        [174678] [IPMIECO 01.02.06] There is no DIMM sensor reading.
    Impact motherboard:
        MBD-H13SAE-MF-P
    Affected functions:
        Sensor reading.
    Validation:
        DIMM sensor read is working now.

================================================================================
Filename: BMC_H13AST2600-F401MS_20240415_01.02.06_STDsp.bin
version: 01.02.06
Date: 2024-04-15
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.54
Redfish API: Redfish_1_11_API_full_list_20231218
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P

1.
    Category: Fix
    Description:
        [171534] [IPMI ECO 01.01.02] redfish automation tool check is fail

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SAE-MF-P

    Affected functions:
        Redfish url.

    Validation:
        1. Run below SATC tests.
            "Redfish.Permission.Permission.Check Operator Privilege".
            "Redfish.Permission.Permission.Check User Privilege".

2.
    Category: Fix
    Description:
        [172274] ECO -- 22739 -- 01.02.03(2024/03/05) -- GUI -- SMTP description is inconsistent with WEB page at Help page.

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SAE-MF-P

    Affected functions:
        N/A

    Validation:
        1. Login web with ADMIN.
        2. Configuration → Notifications → SMTP
        3. Click right bar : "Help" icon → Search "SMTP"
        4. Compare SMTP's field string between web page and help page.

3.
    Category: Fix
    Description:
        [172566] ECO -- 22739 -- 01.02.03(2024/03/05) -- Web -- Virtual media 'Path to Image' error tips didn't fully display.

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SAE-MF-P

    Affected functions:
        N/A

    Validation:
        1. Login Web
        2. Enter to Virtual Media page and tap on edit button
        3. Input incorrect Path and check the prompt tip

4.
    Category: Fix
    Description:
        [172708] ECO -- 22739 -- 01.02.03(2024/03/05) -- Web -- Fail to upload Valid File For TSIG Authentication

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SAE-MF-P

    Affected functions:
        N/A

    Validation:
        1. Login to the Web UI
        2. Switch on NTP in "Date and Time" Tab (Configuration >BMC Settings)
        3. Switch on Dynamic DNS in "Dynamic DNS" Tab (Configuration >BMC Settings)
        4. Input Server Address or BMC Hostname
        5. Switch on TSIG Authentication
        6. Select TSIG .key File & TSIG .private File

5.
    Category: Fix
    Description:
        [174125] ECO -- 22739 -- 01.02.05(2024/03/25) -- Web -- IPv6 gateway address isn't displayed when configuring to DHCPv6 stateful

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SAE-MF-P

    Affected functions:
        N/A

    Validation:
        1. Login web with ADMIN.
        2. Enter to Network page
        3. Select DHCPv6 stateful
        4. Wait for 1 minute then tap on refreash button
        5. Check if all IPv6 information are correctly displayed

6.
    Category: Fix
    Description:
        [170563] ECO -- 22739 -- 01.01.12 (2024/01/19) -- CombinedECO -- IPMI configuration should be preserved after flash IPMI.
    Impact motherboard:
        MBD-H13SAE-MF-P
    Affected functions:
        N/A
    Validation:
        Run SMCTC CombinedECO TC0002.

7.
    Category: Fix
    Description:
        [171101] IPMI 01.02.01(2024/02/02) Redfish test failed
    Impact motherboard:
        MBD-H13SAE-MF-P
    Affected functions:
        N/A
    Validation:
        Run SATC item "Redfish.License Key.License Permission.Test URIs Reachable When DCMS Activated".

8.
    Category: Fix
    Description:
        [171391] automation test failed
    Impact motherboard:
        MBD-H13SAE-MF-P
    Affected functions:
        N/A
    Validation:
        Run SMCTC CombinedECO TC5002.

9.
    Category: Fix
    Description:
        [171656] STD -- 22739 -- 01.02.01 (2024/02/02) -- SUMECO -- Fail to set secure boot key. (TC 3111/ TC4129)
    Impact motherboard:
        MBD-H13SAE-MF-P
    Affected functions:
        N/A
    Validation:
        Run SMCTC SUMECO TC3111.

================================================================================
Filename: BMC_H13AST2600-F401MS_20240314_01.02.04_STDsp.bin
version: 01.02.04
Date: 2024-03-14
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.54
Redfish API: Redfish_1_11_API_full_list_20231218
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P

1.
    Category: Fix
    Description:
        [171534] [IPMI ECO 01.01.02] redfish automation tool check is fail
        [171101] IPMI 01.02.01(2024/02/02) Redfish test failed

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SAE-MF-P

    Affected functions:
        Redfish url.

    Validation:
        1. Run below SATC tests.
            "Redfish.Permission.Permission.Check Operator Privilege".
            "Redfish.Permission.Permission.Check User Privilege".

2.
    Category: Fix
    Description:
        [172258] ECO -- 22739 -- 01.02.03(2024/03/05) -- Web -- IPv6 gateway MEL display twice when changing network settings other than IPv6 gateway itself

    Impact motherboard:
        ALL

    Affected functions:
        Corresponding MEL display timing.

    Validation:
        1. Enter to Network page
        2. Change IPv6 setting to Static Configuration and fill in IPv6 address, Prefix and Gateway IP then save it
           IPv6 address: 2001::123:1:aaaa
           Prefix: 64
           Gateway IP: 2001::123:1:bbbb
        3. Clear MEL
        4. Go back to Network page, change IPv4 network setting from DHCP to Static
        5. Check MEL messages

3.
    Category: Fix
    Description:
        [172297] ECO -- 21603 -- 01.02.01(2024/03/01) -- Web -- RADIUS web elements are disabled without license
        [172290] ECO -- 22739 -- 01.02.03(2024/03/05) -- Web -- RADIUS web elements are disabled without license activation
        [171972] ECO -- 16914 -- 01.04.03 -- At clear / No License, Directory Service RADIUS switch is enabled, but RADIUS elements are disabled

    Impact motherboard:
        H13SSL
        H13SRD
        X12DAI-N-P
        X12DDW-A6-P
        X12DHM-6-P
        X12SPI-TF-P
        X12SPM-LN6TF-P
        X12SPW-TF-001-P

    Affected functions:
        N/A

    Validation:
        1.Clear license. Can be done through SMSTC.
        2.UI > Configuration > Account Services > Directory Service
        3.RADIUS: ON
        4.Check RADIUS section


================================================================================
Filename: BMC_H13AST2600-F401MS_20240305_01.02.03_STDsp.bin
version: 01.02.03
Date: 2024-03-05
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.53
Redfish API: Redfish_1_11_API_full_list_20231218
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P

1.
    Category: Fix
    Description:
        [171350] STD -- 22739 -- 01.02.01(02/02/2024) -- AutoDST should be disable when timezone is (UTC+02:00) Damascus from 2023

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SAE-MF-P

    Affected functions:
        NTP setting.
    Validation:
        1. Login WEB GUI and change page to Configuration -> BMC Settings -> Date and Time
        2. Choice 'Time Zone' to '(UTC+02:00) Damascus'
        3. Press down button 'Save'
        4. Check the 'Auto Daylight Savings Time' status

2.
    Category: Fix
    Description:
        [171564] ECO -- 22739 -- 01.02.02(2024/02/20) -- Web -- Multi Node page keeps loading

    Impact motherboard:
        MBD-H13SRD-F-P

    Affected functions:
        N/A
    Validation:
        1. Login Web
        2. Enter to Multi Node page
        3. Check if web loads multinode page correctly.

3.
    Category: Fix
    Description:
        [171626] ECO -- 22739 -- 01.02.02(2024/02/20) -- Web -- AC Power on and FIFO event logs are disabled on operator privilege

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SAE-MF-P

    Affected functions:
        N/A
    Validation:
        1. Create an operator account
        2. Login Web as Operator account
        3. Enter to Health event log page
        4. Check AC Power on and FIFO event switch toggle buttons


================================================================================
Filename: BMC_H13AST2600-F401MS_20240220_01.02.02_STDsp.bin
version: 01.02.02
Date: 2024-02-20
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.53
Redfish API: Redfish_1_11_API_full_list_20231218
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P

1.
    Category: Fix
    Description:
        [167551] After applying ECO 29091, MB boot up but no display and cannot get the BMC IP

    Impact motherboard:
        MBD-H13SRD-F-P

    Affected functions:
        Host and BMC boot up.

    Validation:
        1. Update BMC firmware.
        2. AC off and AC on.
        3. Check if host and BMC can boot up successfully.
        
================================================================================
Filename: BMC_H13AST2600-F401MS_20240202_01.02.01_STDsp.bin
version: 01.02.01
Date: 2024-02-02
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.53
Redfish API: Redfish_1_11_API_full_list_20231218
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P

1.
    Category: Fix
    Description:
        Fix CVE-2023-4879 Terrapin Attack.

    Impact motherboard:
        All

    Affected functions:
        ssh service

    Validation:
        1. Perform vulnerability scan using nmap for ssh2-enum-algos
2.
    Category: Fix
    Description:
        (CVE-2023-48795) SMC-2024010013 Terrapin Attack vulnerability
        SMC-2024010010 Command Injection attack
        SMC-2024010011 XSS attack

    Impact motherboard:
        All

    Affected functions: N/A
    Validation:
        Please contact Glen's team to do the validation.
3.
    Category: Fix
    Description:
        (CVE-2023-33413) SMC-2024010012 Command Injection attack

    Impact motherboard:
        All

    Affected functions: N/A
    Validation:
        Please contact Glen's team to do the validation.

4.
    Category: Fix
    Description:
        [169578] ECO -- 22739 -- 01.01.11(2023/11/28) -- GUI -- SNMP in Help page is inconsistent with Actual WEB page.
    Impact motherboard:
        All MBs.
    Affected functions:
        WebUI
    Validation:
        1. Login WEB GUI
        2. Check Notification of SNMPv3: Configuration-> Notifications-> SNMP-> SNMPv3
        3. Check Notification in Help page
5.
    Category: Fix
    Description:
        [169679] ECO -- 22739 -- 01.01.11(2023/11/28) -- Web -- Both DNS Lookup and Static address can be modified at the same time
    Impact motherboard:
        All MBs.
    Affected functions:
        WebUI
    Validation:
        1. Enter to Directory Services page and toggle on Active Directory
        2. Add 1 address on DNS Lookup then submit it
        3. Turn off DNS Lookup
        4. Add 1 static address, observe if edit and delete icons appear on DNS Lookup field
        5. Delete all address then submit it

6.
    Category: Fix
    Description:
        [169690] ECO -- 22739 -- 01.01.11(2023/11/28) -- Web -- Network page can save Class D and Class E ipv4 addresses
    Impact motherboard:
        All MBs.
    Affected functions:
        WebUI
    Validation:
        1. Enter to Network and switch to static ip address
        2. Input Class D or Class E ipv4 address
        3. Tap on save button

================================================================================
Filename: BMC_H13AST2600-F401MS_20240119_01.01.12_STDsp.bin
version: 01.01.12
Date: 2024-01-19
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.53
Redfish API: Redfish_1_11_API_full_list_20231218
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P

1.
    Category: Fix
    Description:
        Change CPU upper critical thereshold to 100.

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SAE-MF-P

    Affected functions:
        Sensor reading.

    Validation:
        1. Check if CPU upper critical thereshold is set to 100.

2.
    Category: Fix
    Description:
        [161622] ECO -- 22739 -- 01.01.08(08/04/2023) -- GUI -- Sensor naming is not match as spec defined
    Impact motherboard:
        H13SAE-MF
    Affected functions:
        Sensor name.
    Validation:
        1. Login BMC web and switch to sensor Readings at dashboard.
        2. Check Sensor naming with naming spec 2.7_Draft_12282023.
        3. It should be match as spec.

3.
    Category: Fix
    Description:
        [169485] ECO -- 22739 -- 01.01.11 (2023/12/04) -- WEB -- DNS pop-up message description does not match SPEC
    Impact motherboard:
        All MBs.
    Affected functions:
        WebUI
    Validation:
        1. Login WEB GUI
        2. Configuration -> Network -> IPv4
        3. Switch Advanced Settings to "Manually obtain DNS server IP"
        4. Enter DNS Server IP as 0.0.0.0 and press SAVE.
        5. Confirm the pop-up message.

4.
    Category: Fix
    Description:
        [169486] ECO -- 22739 -- 01.01.11 (2023/12/04) -- WEB -- Could notnable to save the Gateway IP for IPv6 static configuration settings.
    Impact motherboard:
        All MBs.
    Affected functions:
        WebUI
    Validation:
        1. Login web with ADMIN.
        2. Configuration → Network → IPv6 → Turn on IPv6
        3. Choose Auto Configuration → Static Configuration →
        4. Fill in Static Configuration as below
            Pv6 Address : 2001:db8::7ec2:55ff:fe51:20FF
            Prefix Length : 64
            Gateway IP : 2001::1234:0001:aaaa
            → Press "Save" to save network settings
        5. Check the IPv6 Static Configuration

5.
    Category: Fix
    Description:
        [169577] ECO -- 22739 -- 01.01.11 (2023/12/04) -- WEB -- [GUI] Help page not match with WEB GUI (SNMPv3/License Management)
    Impact motherboard:
        All MBs.
    Affected functions:
        WebUI
    Validation:
        1. Login WEB GUI
        2. Choice side bar icon 'Help'
        3. Choice menu 'Maintenance'
        4. Check the number about 'Maintenance Event Log' and 'License Activation'

================================================================================
Filename: BMC_H13AST2600-F401MS_20231204_01.01.11_STDsp.bin
version: 01.01.11
Date: 12-04-2023
Java SOL Viewer version: v0.5.16
Java iKVM Viwer version: v1.69.53
Redfish API: Redfish_1_11_API_full_list_20231003
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P

1.
    Category: Fix
    Description:
        Update redfish API list version.
        [165343] ECO -- 22739 -- 01.01.10(10/19/2023) -- Could not get URI '/redfish/v1/Managers/1/Oem/Supermicro/Syslog' without License

2.
    Category: Fix
    Description:
        [160993] ECO -- 22739 -- 01.01.08 -- [GUI] Help page not list related info of SSDP & LLDP

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SAE-MF-P

    Affected functions:
    Validation:
        1. Check help page info of SSDP and LLDP.

3.
    Category: Fix
    Description:
        [163489] ECO -- 22739 -- 01.01.09 (2023/09/14) -- WEB -- No related MEL when disable TSIG Authentication.

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SAE-MF-P

    Affected functions:
    Validation:
        1. Check if TSIG MEL shows up after executing corresponding actions.

4.
    Category: Fix
    Description:
        [165339] ECO -- 22739 -- 01.01.10(10/19/2023) -- Virtual Media is able to set expected image path with Redfish URI
                 '/redfish/v1/Managers/1/VirtualMedia/VirtualMedia1/Actions/VirtualMedia.InsertMedia', but Web GUI could not

    Impact motherboard:
        MBD-H13SRD-F-P, MBD-H13SAE-MF-P

    Affected functions:
    Validation:
        1. Check if the invalid path is blocked when setting virtual media.

================================================================================
Filename: BMC_H13AST2600-F401MS_20231019_01.01.10_STDsd.bin
version: 01.01.10
Date: 10-19-2023
Java SOL Viewer version: v0.5.14
Java iKVM Viwer version: v1.69.45
Redfish API: Redfish_1_11_API_full_list_20230613
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P

1.
    Category: Fix
    Description:
        [160904] ECO -- 22739 -- 01.01.08 -- [GUI] — Deditcated Link speed has 10M speed
        [163149] ECO -- 22739 -- 01.01.09 (2023/09/14) -- WEB -- No Link speed after enabled LAN Interface in Dedicated mode.

    Impact motherboard:
        MBD-H13SRD-F-P

    Affected functions:
    Validation:
        Check if 10M link speed is removed and other options are correct.

2.
    Category: Fix
    Description:
        [163404] ECO -- 22739 -- 01.01.09 (2023/09/14) -- WEB -- MEL is incorrect after do ikvm reset.

    Impact motherboard:
        MBD-H13SRD-F-P

    Affected functions:
    Validation:

3.
    Category: Fix
    Description:
        [163483] ECO -- 22739 -- 01.01.09 (2023/09/14) -- WEB -- MEL incorrect when configure Account Lockout Duration.

    Impact motherboard:
        MBD-H13SRD-F-P

    Affected functions:
    Validation:

4.
    Category: Fix
    Description:
        [163489] ECO -- 22739 -- 01.01.09 (2023/09/14) -- WEB -- No related MEL when disable TSIG Authentication.

    Impact motherboard:
        MBD-H13SRD-F-P

    Affected functions:
    Validation:

5.
    Category: Fix
    Description:
        Host interface cannot get IP.

    Impact motherboard:
        MBD-H13SRD-F-P

    Affected functions:
    Validation:
        Check if host interface has IP.

================================================================================
Filename: BMC_H13AST2600-F401MS_20230914_01.01.09_STDsd.bin
version: 01.01.09
Date: 09-14-2023
Java SOL Viewer version: v0.5.14
Java iKVM Viwer version: v1.69.45
Redfish API: Redfish_1_11_API_full_list_20230613
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P

1.
    Category: Fix
    Description:
        [160904] ECO -- 22739 -- 01.01.08 -- [GUI] — Deditcated Link speed has 10M speed

    Impact motherboard:
        MBD-H13SRD-F-P

    Affected functions:
    Validation:
        Check if 10M link speed is removed.

================================================================================
Filename: BMC_H13AST2600-F401MS_20230803_01.01.08_STDsd.bin
version: 01.01.08
Date: 08-03-2023
Java SOL Viewer version: v0.5.14
Java iKVM Viwer version: v1.69.45
Redfish API: Redfish_1_11_API_full_list_20230613
Supported MBs: MBD-H13SRD-F-P, MBD-H13SAE-MF-P

1.
    Category: Fix
    Description:
        [159112] ECO -- 22739 -- 01.01.05 -- Sensor naming is not match as spec define.

    Impact motherboard:
        MBD-H13SRD-F-P

    Affected functions:
    Validation:
        Check if "CPU_VDDCR0" sensor name matches spec.

2.
    Category: Fix
    Description:
        [158897] [Barebone][IPMI 01.01.05][BIOS 1.0 20230630] System will show black screen during AC onoff cycle randomly.
    Impact motherboard:
        All MBs.
    Affected functions:
    Validation:
        Added workaround command for BIOS to avoid stuck boot.
        BIOS needs to add an extra call.
        Host reset watchdog raw command.
        
                 cmd,      en bit, time(min), entry
        enable:  0x30 0x97 0x01    0x01       0x01
        disable: 0x30 0x97 0x00    0x01       0x01
        
                 cmd,      entry
        reset:   0x30 0x98 0x01

================================================================================
Filename: BMC_H13AST2600-F401MS_20230705_01.01.07_STDsp.bin
version: 01.01.07
Date: 07-05-2023
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : Redfish_1_11_API_full_list_20230613

1.
    Category: Fix
    Description:
        [158645] [BIOS ECO 1.0]SUM ATT Test fail
    Impact motherboard:
        MBD-H13SAE-MF-P
    Affected functions:
    Validation:
        RUN SMCTC TC1001.

================================================================================
Filename: BMC_H13AST2600-F401MS_20230630_01.01.06_STDsp.bin
version: 01.01.06
Date: 06-30-2023
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : Redfish_1_11_API_full_list_20230613

1.
    Category: Fix
    Description:
        [158555] [CombinedECO BIOS 1.0 & IPMI 01.01.05] Automation test failure.
    Impact motherboard:
        MBD-H13SRD-F-P
    Affected functions:
    Validation:
        Run Redfish SATC test.

2.
    Category: Fix
    Description:
        [156483] One node will not be able to poweroff use multi nodes to perform ac onoff stress test
        [156341] [IPMI 01.01.02][BIOS 1.0 20230503] System will show black screen during AC onoff cycle randomly.

        Add AC on/off workaround function.
    Impact motherboard:
        MBD-H13SRD-F-P
    Affected functions:
    Validation:
        1. Run AC on/off stress test.
        2. Check if host stuck at S5 state.

Supported MBs: MBD-H13SAE-MF-P
1.
    Category: Fix
    Description:
        [158775] [IPMIECO 01.01.05] Redfish SATC automation test failed.
    Impact motherboard:
        H13SAE-MF
    Affected functions:
    Validation:
        1. RUN Redfish SATC automation test.
2.
    Category: Fix
    Description:
        [158724]ECO -- 22739 -- 01.01.05 -- Add buton is clickable when SUT has 16 users
    Impact motherboard:
        H13SAE-MF
    Affected functions:
    Validation:
        1. Enter to Account Services page
        2. Add user to number 16
        3. Check if Add button is disabled
        4. Delete 1 user
        5. Check if Add button is disabled
        6. Add button should be disabled if SUT has 16 users
        7. Add button should be enabled if SUT has less than 16 users

3.
    Category: Fix
    Description:
        [158645] [BIOS ECO 1.0]SUM ATT Test fail
    Impact motherboard:
        H13SAE-MF
    Affected functions:
        1. RUN SMCTC TC1001, TC4011-4013, TC2009, TC2022, TC2039, TC2088

4.
    Category: Fix
    Description:
        [157922] [IPMIECO v01.01.04] FAN speed control don't work when RT2 overheat.
    Impact motherboard:
        H13SAE-MF
    Affected functions:
        When RT2 overheats, FANA/B will speed up.

================================================================================
Filename: BMC_H13AST2600-F401MS_20230619_01.01.05_STDsp.bin
version: 01.01.05
Date: 06-19-2023
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : Redfish_1_11_API_full_list_20230518

1.
    Category: Fix
    Description:
        [157570] [IPMI 01.01.04] Redfish SATC automation test has failed.
    Impact motherboard:
        MBD-H13SRD-F-P
    Affected functions:
    Validation:
        Run Redfish SATC test.

Supported MBs: MBD-H13SAE-MF-P
1.
    Category: Fix
    Description:
        [157808] ECO -- 22739 -- 01.01.04(05/25/2023) -- GUI -- Sensor naming is not match as spec define
    Impact motherboard:
        MBD-H13SAE-MF-P
    Affected functions:
    Validation:
        1. Login BMC web and switch to sensor Readings at dashboard
        2. Check Sensor naming with naming spec 2.5_06082023
        3. It should be match as spec

2.
    Category: Fix
    Description:
        [157922] [IPMIECO v01.01.04] FAN speed control don't work when RT2 overheat.
    Impact motherboard:
        MBD-H13SAE-MF-P
    Affected functions:
    Validation:
        When RT2 overheats, FANA/B will speed up.

3.
    Category: Fix
    Description:
        [157886] ECO -- 22739 -- 01.01.04(05/25/2023) -- KVM -- Can't launch ikvm after redirect from the port off warning window.
    Impact motherboard:
        MBD-H13SAE-MF-P
    Affected functions:
        Port
    Validation:
        1.Click Configuration > Network > Port
        2.Turn off Ikvm Server port and save
        3.Click "Remote Control" and click the pop out window to redirect back to "port" page.
        4.After redirected to port page and ready, turn on the ikvm server port and save
        5.Check can launch ikvm(HTML 5) successfully.

4.
    Category: Fix
    Description:
        [157958] ECO -- 22739 -- 01.01.04(05/25/2023) -- MEL -- SNMPv3 alert descriptions are not follow spec
    Impact motherboard:
        MBD-H13SAE-MF-P
    Affected functions:
    Validation:
        1.Click Configuration > Notifications >Edit a empty Alert
        2.Select SNMPv3 protocol and set Address to 1.2.3.4
        3.Set user name to Henry2 ; Auth key to Henry2345 Encry key to Henry6789
        4.Click save
        5.Check MEL at Maintenance page

5.
    Category: Fix
    Description:
        [157959] ECO -- 22739 -- 01.01.04(05/25/2023) -- MEL -- Wrong MEL state description when turn off directory service
    Impact motherboard:
        MBD-H13SAE-MF-P
    Affected functions:
    Validation:
        1.Click Configuration > Account Service > Directory Service
        2.Switch on LDAP and switch off LDAP
        3.Check MEL at Maintenance page

================================================================================
Filename: BMC_H13AST2600-F401MS_20230525_01.01.04_STDsp.bin
version: 01.01.04
Date: 05-25-2023
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : Redfish_1_11_API_full_list_20230518

1.
    Category: Fix
    Description:
        [156071] Network AOC in WebUI will show incorrect information.
    Impact motherboard:
        MBD-H13SRD-F-P
    Affected functions:
    Validation:
        Chekc if there are "undefined" blocks under network AOC card page.

2.
    Category: Fix
    Description:
        [152382] Redfish SATC automation test has failed.
        [153278] SATC Redfish automation test failed
    Impact motherboard:
        All MBs.
    Affected functions:
    Validation:
        Run Redfish SATC test.

Supported MBs: MBD-H13SAE-MF-P
1.
    Category: Fix
    Description:
        [153600] Hardware Monitor Voltage test fail
    Impact motherboard:
        MBD-H13SAE-MF-P
    Affected functions:
    Validation:
        Check sensor readings.

2.
    Category: Fix
    Description:
        [155381] Digital Battery Reading Check Fail
    Impact motherboard:
        MBD-H13SAE-MF-P
    Affected functions:
    Validation:
        On the sensor readings webpage.
        When inputting 2.55v it should show "Battery low (predictive failure) " but BMC Web shows "Battery Presence Detected".
        When inputting 2.4v it should show "Battery Failed " but BMC Web shows "Battery Presence Detected".

================================================================================
Filename: BMC_H13AST2600-F401MS_20230516_01.01.03_STDsp.bin
version: 01.01.03
Date: 05-16-2023
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : Redfish_1_11_API_full_list_20230410

1.
    Category: Fix
    Description:
        [156071] Update BIOS will have additional alert update backup / golden image pop-up windows.
    Impact motherboard:
        All MBs.
    Affected functions:
    Validation:
        Update BIOS will have no additional alert update backup / golden image pop-up windows.

Supported MBs: MBD-H13SAE-MF-P
    Sensor reading table changes for HW Rev 1.01.(some errors when used on Rev 1.00)

Supported MBs: MBD-H13SRD-F-P
1.
    Category: Fix
    Description:
        [150021][SSM_5.3.0_b1209] The System Information test fail on the M13SRD-F

    Impact motherboard:
        MBD-H13SRD-F-P
    Affected functions:
    Validation:
        Check if contents are correct on SSM.

2.
    Category: Fix
    Description:
        [150218][SUM_2.10.0_20221209] SUM test fail on the M13SRD-F
    Impact motherboard:
        MBD-H13SRD-F-P
    Affected functions:
    Validation:
        Run SUM ECO.

3.
    Category: Fix
    Description:
        [152382]Redfish SATC automation test has failed.
    Impact motherboard:
        MBD-H13SRD-F-P
    Affected functions:
    Validation:
        Run SATC.
 
4.
    Category: Fix
    Description:
        [155123][IPMI 01.00.07] Sensor reading not match with SPEC.
    Impact motherboard:
        MBD-H13SRD-F-P
    Affected functions:
    Validation:
       Check if sensor names are correct. 

5.
    Category: Fix
    Description:
        [155332][IPMI 01.00.07] NVMe eject and insert function not work in WebUI storage monitor.
    Impact motherboard:
        MBD-H13SRD-F-P
    Affected functions:
    Validation:
        Chekc if eject and insert sign are removed.

6.
    Category: Fix
    Description:
        [155984][BIOS ECO1.0] An error message will appear in the flash BIOS
    Impact motherboard:
        MBD-H13SRD-F-P
    Affected functions:
    Validation:
        Run BIOS ECO.
 
7.
    Category: Fix
    Description:
        [156155][CombinedECO BIOS 1.0 & IPMI 01.01.01] Automation test failure.
    Impact motherboard:
        MBD-H13SRD-F-P
    Affected functions:
    Validation:
        Run Combined ECO.
 
8.
    Category: Fix
        [156193][IPMI 01.01.02] CPU information can't show speed and TDP in WebUI.
    Description:
    Impact motherboard:
        MBD-H13SRD-F-P
    Affected functions:
    Validation:
        Check speed and TPD values on CPU page.



================================================================================
Filename: BMC_H13AST2600-F401MS_20230428_01.01.02_STDsp.bin
version: 01.01.02
Date: 04-28-2023
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : Redfish_1_11_API_full_list_20230320

1.
    Category: Fix
    Description:
        [155532] No CPU voltage on IPMI web
        [155123] [IPMI 01.00.07] Sensor reading not match with SPEC.

        Add CPU voltage sensor "CPU_VDDCR".
        Correct "M2_SSD1 Temp" sensor name.
    Impact motherboard:
        MBD-H13SRD-F-P
    Affected functions:
    Validation:
        1. Check if "CPU_VDDCR" and "M2_SSD1 Temp" are correct on sensor
    page.

2.
    Add support CDC-ECM feature.
    Please use a supported BIOS to avoid unexpected errors.

Supported MBs: MBD-H13SAE-MF-P
1.
    Category: Fix
    Description:
        [153999] [DVT] Fan thermal control test fail.
    Impact motherboard:
        MBD-H13SAE-MF-P
    Affected functions:
    Validation:
        View the relationship between GPU temperature and fan speed.

================================================================================
Filename: BMC_H13AST2600-F401MS_20230421_01.01.01_STDsp.bin
version: 01.01.01
Date: 04-21-2023
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : Redfish_1_11_API_full_list_20230320

1.
    Category: Fix
    Description:
        [153624] Hardware Monitor Voltage test fail.
        Sensor reading of 1.2V BMC test fail.
    Impact motherboard:
        MBD-H13SRD-F-P
    Affected functions:
    Validation:
        1. Check if error of reading value of 1.2V BMC is withing
            criterion.

2.
    Category: Fix
    Description:
        [153123] [DVT] CPU TDP Watts display error on BMC WebGUi
    Impact motherboard:
        All MBs.
    Affected functions:
    Validation:
        CPU TDP Watts display "N/A" on BMC WebGUi.

3.
    Category: Fix
    Description:
        [152270] The power failure event log missed an info event - "Info |Power Supply Installed - Assertion"
        [154853] [IPMI 01.00.07] When unplug one of PSU cable , WebUI will take a long time to record PSU events.
    Impact motherboard:
        All MBs.
    Affected functions:
    Validation:
        Check if BMC assert log as "bmc_psu_lan_plug_in_out_behavior_v1.3" within 15 to 20 seconds.

4.
    Category: Fix
    Description:
        [152382] Redfish SATC automation test has failed.
    Impact motherboard:
        MBD-H13SRD-F-P
    Affected functions:
    Validation:
        Run redfish automation test.

5.
    Category: Fix
    Description:
        [152594] It allows 64 characters input and show saved successfully.
    Impact motherboard:
        MBD-H13SRD-F-P
    Affected functions:
    Validation:
        1.Into Network page -> General - Hostname.
        2.Input 64 characters.
        3.Press "Save".
        4.It should be blocked by the system.

6.
    Category: Fix
    Description:
        [152396] DMTF/Redfish-Protocol Validator test is fail.
        [152397] DMTF/Redfish-Service Validator test is fail.
        [152398] DMTF/Redfish-Reference Checker test is fail.
    Impact motherboard:
        MBD-H13SRD-F-P
    Affected functions:
    Validation:
        Run redfish automation test.

7.
    Category: Fix
    Description:
        [154906] [SD5_5.17.0_b1061] Redfish credential bootstrapping test fail (return code is C1) on the H13SRD-F
    Impact motherboard:
        MBD-H13SRD-F-P
    Affected functions:
    Validation:
        Check if ipmi raw command "ipmi raw 2c 05 52 a5" works correctly.

8.
    Category: Fix
    Description:
        [155134] AS-3015MR-H8TNR (MBD-H13SRD-F-P Rev 1.01) IPMI sensor reading definition is reverse from MB RT1/RT2 location.
    Impact motherboard:
        MBD-H13SRD-F-P
    Affected functions:
    Validation:
        Check if the RT1/RT2 sensor reading are correct.

9.
    Changed BIOS flash "MX25U25643G" SPI speed from 50MHz to 16MHz.

Supported MBs: H13SAE-MF
1.
    Category: Fix
    Description:
        [153602] IPMI Web does not display CPU voltage.
        [153600] Hardware Monitor Voltage test fail.
        [153416] [DVT] Cannot find the related memory voltages in Supermicro_BMC_Sensor_Naming_Guildeline.
        [153166] [DVT] CPU Voltage test failed.
    Impact motherboard:
        MBD-H13SAE-MF-P
    Affected functions:
    Validation:
        Check sensor readings.

2.
    Category: Fix
    Description:
        [153482] There is System Crash Dump and Crash Screen Capture function on the BMC WebGUI
    Impact motherboard:
        MBD-H13SAE-MF-P
    Affected functions:
    Validation:
        Check Troubleshooting web page.

3.
    Category: Fix
    Description:
        [153999] [DVT] Fan thermal control test fail.
    Impact motherboard:
        MBD-H13SAE-MF-P
    Affected functions:
    Validation:
        FANA/B speed change when heat up GPU card.

4.
    Changed FAN LowCT from 280RPM to 420RPM.

================================================================================
Filename: BMC_M13AST2600-F401MS_20230221_01.00.07_STDsp.bin
version: 01.00.07
Date: 02-21-2023
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_90_API_full_list_11032021

1.
    R: [150026] [SSM_5.3.0_b1209] Call home trigger item
        Category: Fix
        Description:
            [150026] [SSM_5.3.0_b1209] Call home trigger item (temp:Local Administrator Setting)
            no match SSM design on the M13SRD-F Copy Project Issue Link

        Impact motherboard:
            MBD-M13SRD-F-P

        Affected functions:
        Validation :
            1. Login BMC web and check if only AOC_NIC critical values are viable.

2.
    R: [150678] There is no "System Crash Dump" in Troubleshooting page.
       Category: Fix
       Description:
            [150678] There is no "System Crash Dump" in Troubleshooting page.

       Impact motherboard:
           MBD-M13SRD-F-P

       Affected functions:
       Validation:
            1. Login WEB and go to troubleshooting page.
            2. Check if there's system crash dump tab.

3.
    Fix the problem that the system fan will slow down when the CPU exceeds 100C.

4.
    R: [152620] Please define support FAN speed mode in IPMI page.

        Category: Fix
        Description:
            [152620] Please define support FAN speed mode in IPMI page.
            Remove optimal fan mode.

        Impact motherboard:
            MBD-M13SRD-F-P

        Affected functions:
        Validation:
            1. Login web and check if optimal fan mode is removed.

Supported MBs: M13SAE-MF
    1. Fix no console capture on WEB issue. (Ref b31fab50)
    2. Fix ipmb reading error. (Ref 4297edf7)
    3. There is no "System Crash Dump" in Troubleshooting page. (Ref ef67e34f)
    4. Fix can't read dcmi power status.
    5. Modify VRM address 0x21 to 0x2F to accommodate hardware changes.
    6. Modify CPU temperature HighCT 98 to 100.
    7. Added M.2 temperature sensor read.
    8. Added PCIE functionality and GPU temperature sensor reading.
    9. Added Chassis Intru functionality.
    10. Added reading CPU Vout(8Bh) from VRM I2C bus.

================================================================================
Filename: BMC_M13AST2600-F401MS_20230207_01.00.06_STDsp.bin
version: 01.00.06
Date: 02-07-2023
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_90_API_full_list_11032021

1.
    Category: Fix
    Description:
        [150026] [SSM_5.3.0_b1209] Call home trigger item (temp:Local Administrator Setting)
        no match SSM design on the M13SRD-F Copy Project Issue Link

    Impact motherboard:
        MBD-M13SRD-F-P

    Affected functions:
    Validation :
        1. Login BMC web and check if only sensor critical values are viable.

2.
    Category: Fix
    Description:
        [149936] [SD5_5.16.0_build.1047] SD5 validation fail 
        (sensor:P1V05_PCH_AUX sensor detect fail and lack the FAN2 and VRMCpu Temp,DIMMAB Temp,M2NVMeSSD Temp1 sensor on the M13SRD-F

    Impact motherboard:
        MBD-M13SRD-F-P

    Affected functions:
    Validation :
        1. Execute SD5 validation.
        2. Check if sensor reaings are correct.

3.
    Category: Fix
    Description:
        [150021] [SSM_5.3.0_b1209] The System Information test fail on the M13SRD-F Copy Project Issue Link

    Impact motherboard:
        MBD-M13SRD-F-P

    Affected functions:
    Validation :
        1. Execute SSM and check if system information is correct.
 
4.
    Category: Fix
    Description:
        [151134] The BMC sensor readout only detects "DIMMA2" and "DIMMB2"
        when inserted into DDR5 memory slot full of DIMMs (DIMMA1, DIMMA2, DIMMB1, DIMMB2).

    Impact motherboard:
        MBD-M13SRD-F-P

    Affected functions:
    Validation :
        1. Login BMC WEB.
        2. Check if DIMM are displayed correctly in sensor reading page.

5.
    Category: Fix
    Description:
        [150019] [EVT] IPMI sensor reading failed, many items show N/A or error.

    Impact motherboard:
        MBD-M13SRD-F-P

    Affected functions:
    Validation :
        1. Login BMC WEB.
        2. Check if sensor readings are correct.

6.
    Modify gpio mapping.

7.
    Fix duplicate processor hot event log.

Supported MBs: M13SAE-MF
    1. Modify SDR thresholds to meet Thermal Design Guide 4.07. (Ref a7d51996)
    2. Add thermal trip trigger function.

================================================================================
Filename: BMC_M13AST2600-F401MS_20230112_01.00.05_STDsp.bin
version: 01.00.05
Date: 01-12-2023
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_90_API_full_list_11032021

Release the wrong branch, update 01.00.05 and fix it.

================================================================================
Filename: BMC_M13AST2600-F401MS_20230109_01.00.04_STDsp.bin
version: 01.00.04
Date: 01-09-2023
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_90_API_full_list_11032021

1.
    Category: Fix
    Description:
        [149914] [IPMICFG] Test fail via SMSTC with IPMICFG on the M13SRD-F.

    Impact motherboard:
        MBD-M13SRD-F-P

    Affected functions:
    Validation :
        1. Execute IPMICFG ECO test case 120.

2.
    Category: Fix
    Description:
        [150679] There is no "Console Capture" in Troubleshooting page.

    Impact motherboard:
        MBD-M13SRD-F-P

    Affected functions:
    Validation :
        1. Login to BMC WEB and check if there's console capture tab in maintenance/troubleshooting.

3.
    Category: Fix
    Description:
        [150727] IPMI WEB storage monitor function can't work.

    Impact motherboard:
        MBD-M13SRD-F-P

    Affected functions:
    Validation :
        1. Install storage card on MB.
        2. Check if the "storage monitor" block is displayed on BMC WEB.

4.
    Category: Fix
    Description:
        [151045] BMC network link status shows "No Connected" in the setup page when connected to Shared LAN (AOC-CTG-i2S).

    Impact motherboard:
        MBD-M13SRD-F-P

    Affected functions:
    Validation :
        1. Install LAN card on MB.
        2. Check if the network related information is displayed on BIOS setup menu.

5.
    Category: Fix
    Description:
        [151046] IPMI Web - NetworkAOC page does not display AOC card (AOC-C25G-m1S) and Temperature.

    Impact motherboard:
        MBD-M13SRD-F-P

    Affected functions:
    Validation :
        1. Install LAN card on MB.
        2. Check if the AOC card name and temperature are displayed on BMC WEB.
6.
    Category: Fix
    Description:
        [150015] [M13][EVT] When the CPU overheat is triggered, the test
        board/onboard LED overheat LED does not blink and no CPU reports
        overheat messages in the IPMI event log.
    Impact motherboard:
        MBD-M13SRD-F-P

    Affected functions:
    Validation:
         1. Check if the processor hot event log is recorded when CPU
            overheat.

Supported MBs: M13SAE-MF
    1. Apply DIMM Sensor Readings. (Ref 3daa4c5d)
    2. Fix ipmicfg return C3 when get NM device id. (Ref e4a9692d)
    3. Apply Fan Sensor Readings.
    4. Fix temperature reading error.

================================================================================
Filename: BMC_M13AST2600-F401MS_20221227_01.00.03_STDsp.bin
version: 01.00.03
Date: 01-04-2023
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_90_API_full_list_11032021
Supported MBs: M13SRD-F

    1. Fix DIMM sensor reading.
    2. Fix ADC sensor reading.
    3. Modify ADC sensor names.
        1. PVCCIN_PCH_AUX to P1V8.
        2. P1V05_PCH_AUX to 1.2V BMC.
        3. P1V2_VDDQ to VDDIO_MEM_S3.
        4. PVCC_CPU to P5V_DDR_S3.

Supported MBs: M13SAE-MF
    1. Initial board bring up bmc FW.

================================================================================
Filename: BMC_M13AST2600-F401MS_20221227_01.00.02_STDsp.bin
version: 01.00.02
Date: 12-27-2022
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_12172020
Supported MBs: M13SRD-F

    1. Fix VRM sensor reading.

================================================================================
Filename: BMC_M13AST2600-F401MS_20221205_01.00.01_STDsp.bin
version: 01.00.01
Date: 12-05-2022
U-Boot build time :
Java SOL Viewer version : v0.5.14
Java iKVM Viwer version : v1.69 r43
Redfish API : X12_Redfish_1_80_API_full_list_12172020
Supported MBs: M13SRD-F

    1. M13 first release.
