Product Name: X11DPT-PS
Revision: 1.0b		Previous Revision: 1.0a
Release Date: 9/23/2017
Update Category: Critical
Dependencies:
None
Important Notes:
None
Enhancements:
1. Changed BIOS revision to 1.0b.
2. Updated Purley RC 142.R08, SPS 4.0.03.235, ACM files, and CPU microcode.
3. Hid "TXT Support" in BIOS Setup menu dynamically when CPU doesn't support it.
4. Enabled display of EarlyVideo message by onboard video when VGA Priority is set to Offboard.
5. Removed the "System Firmware Error (POST ERROR)" error log from BMC and "EFI 01030006" in BIOS event log.
6. Added Setup item "Core Disable Bitmap(Hex)" to BIOS CPU Configuration setup page.
7. Corrected help string of setup item "Enforce POR".
New Features:
1. Set to show recovery error message when no BIOS image is in USB pen drive.
2. Set display of setup option for always turbo mode function as default.
Fixes:
1. Fixed problem of the Runtime UCE memory causing DIMM mapout to not show on screen.
2. Set GPP_J0, GPP_J2, GPP_J4, and GPP_J6 as input as a workaround for hardware issue of front panel LAN activity LED always staying on.
3. Fixed failure of SMBIOS Type 20 to fill Interleave Position and Interleaved Data Depth correctly.
4. Fixed inability of Intel P3100 M.2 to boot to OS.
5. Updated BMC LAN configuration for saving settings of BIOS setup menu.
6. Fixed failure of Password Preservation Test due to password not being preserved.
7. Fixed system hanging when running SUM Test_case_220 and Test_case_308.